RADLAN-DNSCL-MIB DEFINITIONS ::= BEGIN

-- Title:                DNSCL Private Extension
--                       This Private MIB supports the DNS Client
-- Version:              7.30
-- Date:                 24 Oct 2003



IMPORTS
    rlDnsCl                                 FROM RADLAN-MIB
    dnsResConfigSbeltEntry                  FROM DNS-RESOLVER-MIB
    DnsName                                 FROM DNS-SERVER-MIB
    OBJECT-TYPE, IpAddress,
    Unsigned32, Integer32                   FROM SNMPv2-SMI
    DisplayString                           FROM SNMPv2-TC
    TEXTUAL-CONVENTION,
    TruthValue, RowStatus                   FROM SNMPv2-TC;

rlDnsClMibVersion OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MIB's version, the current version is 1."
::= { rlDnsCl 1 }

rlDnsClEnable OBJECT-TYPE
    SYNTAX INTEGER{
       enable(1),
       disable(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
       "Enable or Disable the use of the DNS client feature."
    ::=  { rlDnsCl 2 }

rlDnsClDomainNameTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlDnsClDomainNameEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
    "The domain names table."
     ::= { rlDnsCl 3}

rlDnsClDomainNameEntry  OBJECT-TYPE
   SYNTAX RlDnsClDomainNameEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
     " The row definition for this table."
   INDEX { rlDnsClDomainNameName }
   ::= { rlDnsClDomainNameTable  1 }

RlDnsClDomainNameEntry  ::= SEQUENCE {
    rlDnsClDomainNameName           DnsName,
    rlDnsClDomainNameOwner          INTEGER,
    rlDnsClDomainNameRowStatus      RowStatus
}

rlDnsClDomainNameName OBJECT-TYPE
   SYNTAX DnsName
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
     "The domain name for this ifIndex."
     ::= { rlDnsClDomainNameEntry 1 }

rlDnsClDomainNameOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The Domain Name owner. Static if Domain Name defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { rlDnsClDomainNameEntry 2 }

rlDnsClDomainNameRowStatus  OBJECT-TYPE
    SYNTAX   RowStatus
    MAX-ACCESS   read-write
    STATUS   current
    DESCRIPTION
      "The row status variable, used according to
      row installation and removal conventions."
    ::= { rlDnsClDomainNameEntry 3 }

rlDnsClMaxNumOfRetransmissions OBJECT-TYPE
    SYNTAX      INTEGER (0..10)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The maximum number of retransmissions for each query."
    DEFVAL      { 3 }
::= { rlDnsCl 4 }

rlDnsClMinRetransmissionInterval OBJECT-TYPE
    SYNTAX      INTEGER (1..15)
    MAX-ACCESS      read-write
    STATUS      current
    DESCRIPTION
        "The minimum number of seconds that must elapsed before
         retransmission for each query."
    DEFVAL      { 5 }
::= { rlDnsCl 5 }

rlDnsClNamesTable OBJECT-TYPE
   SYNTAX SEQUENCE OF RlDnsClNamesEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
    "The Names table."
     ::= { rlDnsCl 6}

rlDnsClNamesEntry  OBJECT-TYPE
   SYNTAX RlDnsClNamesEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       " The row definition for this table."
   INDEX { rlDnsClNamesName,
           rlDnsClNamesOwner,
           rlDnsClNamesIndex }
   ::= { rlDnsClNamesTable 1 }

RlDnsClNamesEntry  ::= SEQUENCE {
  rlDnsClNamesName          DnsName,
  rlDnsClNamesOwner         INTEGER,
  rlDnsClNamesIndex         Integer32,
  rlDnsClNamesAddr          IpAddress,
  rlDnsClNamesRowStatus     RowStatus
}

rlDnsClNamesName OBJECT-TYPE
   SYNTAX     DnsName
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
       "The host name."
     ::= { rlDnsClNamesEntry 1 }

rlDnsClNamesOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The Host Name Entry owner. Static if  Host Name Entry defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { rlDnsClNamesEntry 2 }

rlDnsClNamesIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A value which makes entries in the table unique when the
            other index values (rlDnsClNamesName) do not
            provide a unique index."
    ::= { rlDnsClNamesEntry 3 }

rlDnsClNamesAddr OBJECT-TYPE
   SYNTAX     IpAddress
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
       "The host IP address"
     ::=  { rlDnsClNamesEntry 4 }

rlDnsClNamesRowStatus  OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The row status variable, used according to
       row installation and removal conventions."
    ::= { rlDnsClNamesEntry 5 }

dnsResConfigSbeltExtTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF DnsResConfigSbeltExtEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Augmenting dnsResConfigSbeltTable (dns resolver safety belt table)
         for added info"
    ::= {rlDnsCl 7 }

dnsResConfigSbeltExtEntry OBJECT-TYPE
    SYNTAX     DnsResConfigSbeltExtEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A row of the table dnsResConfigSbeltTable Extended
         by this definition."
    AUGMENTS { dnsResConfigSbeltEntry }
    ::= {dnsResConfigSbeltExtTable  1 }

DnsResConfigSbeltExtEntry  ::= SEQUENCE {
  dnsResConfigSbeltOwner         INTEGER
}


dnsResConfigSbeltOwner OBJECT-TYPE
    SYNTAX  INTEGER{
           static(1),
           dhcp(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "The DNS server Entry owner. Static if DNS server Entry defined by user, dhcp
        if received by boot protocol like DHCP."
    DEFVAL  { static }
    ::=   { dnsResConfigSbeltExtEntry 1 }


END

