
--
-- Juniper Enterprise Specifics MIB
-- 
-- Copyright (c) 2010 Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--

JNX-PPPOE-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Unsigned32 ,Counter64
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, DisplayString, RowStatus, TruthValue, MacAddress
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndex, InterfaceIndexOrZero
        FROM IF-MIB
    jnxPppoeMibRoot
        FROM JUNIPER-SMI;

jnxPPPoEMIB  MODULE-IDENTITY
    LAST-UPDATED "201007220942Z"  -- 22-Jul-10 03:12 PM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  support@Juniper.net"
    DESCRIPTION
        "The Point-to-Point Protocol over Ethernet (PPPoE) MIB for the Junos
        product family.  This MIB contains managed objects for each of
        two interface layers: PPPoE interfaces, and PPPoE subinterfaces.  For
        each of these layers, management objects are provided to query for an
        available interface index, and to create/delete interfaces of that type."
    -- Revision History
    REVISION    "201007220942Z"  -- 22-Jul-10 03:12 PM EST  - JUNOS 11.0
    DESCRIPTION
        "Initial version."
    ::= { jnxPppoeMibRoot 1 }




JnxPPPoEServiceNameAction  ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The set of Service-name action types.
            drop        no PADO packet will be sent.
            terminate   a PADO packet will be sent."
    SYNTAX      INTEGER {
                    drop(0),
                    terminate(1) }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
jnxPPPoEObjects        OBJECT IDENTIFIER ::= { jnxPPPoEMIB 1 }
jnxPPPoEIfLayer        OBJECT IDENTIFIER ::= { jnxPPPoEObjects 1 }
jnxPPPoESubIfLayer     OBJECT IDENTIFIER ::= { jnxPPPoEObjects 2 }
jnxPPPoESummary        OBJECT IDENTIFIER ::= { jnxPPPoEObjects 3 }
jnxPPPoEServices       OBJECT IDENTIFIER ::= { jnxPPPoEObjects 4 }


-- /////////////////////////////////////////////////////////////////////////////

--
-- This layer is managed with the following elements:
--  o NextIfIndex (generator for PPPoEIfIndex selection)
--  o Interface Table (creation/configuration/deletion of PPPoEinterfaces)
--  o Statistics Table (PPPoEinterface statistics)
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- IfIndex selection for creating new PPPoEinterfaces
--
jnxPPPoENextIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in jnxPPPoEIfTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { jnxPPPoEIfLayer 1 }

--
-- The PPPoEInterface Table
--
jnxPPPoEIfTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPPPoEIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The parameters for the PPPoEservice on this interface."
    REFERENCE
        "RFC 2156 A method for transmitting PPP over Ethernet"
    ::= { jnxPPPoEIfLayer 2 }

jnxPPPoEIfEntry OBJECT-TYPE
    SYNTAX      JnxPPPoEIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Parameters for a particular PPPoEinterface.

        Creating/deleting entries in this table causes corresponding entries for
        be created/deleted in ifTable/ifXTable/jnxIfTable, and
        jnxPPPoEIfStatsTable."
    INDEX     { jnxPPPoEIfIfIndex }
    ::= { jnxPPPoEIfTable 1 }

JnxPPPoEIfEntry ::= SEQUENCE {
    jnxPPPoEIfIfIndex           InterfaceIndex,
    jnxPPPoEIfMaxNumSessions    INTEGER,
    jnxPPPoEIfRowStatus         RowStatus,
    jnxPPPoEIfLowerIfIndex      InterfaceIndexOrZero,
    jnxPPPoEIfAcName            DisplayString,
    jnxPPPoEIfDupProtect        INTEGER,
    jnxPPPoEIfPADIFlag          INTEGER,
    jnxPPPoEIfAutoconfig        INTEGER,
    jnxPPPoEIfServiceNameTable  DisplayString,
    jnxPPPoEIfPadrRemoteCircuitIdCapture INTEGER,
    jnxPPPoEIfMtu               Integer32,
    jnxPPPoEIfLockoutMin        Integer32,
    jnxPPPoEIfLockoutMax        Integer32 ,
    jnxPPPoEIfDynamicProfile   DisplayString}

jnxPPPoEIfIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex value of the corresponding ifEntry."
    ::= { jnxPPPoEIfEntry 1 }

jnxPPPoEIfMaxNumSessions OBJECT-TYPE
    SYNTAX      INTEGER (0..65335)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of sessions allowed on the PPPoEinterface, zero indicates
        unlimited."
    DEFVAL    { 0 }
    ::= { jnxPPPoEIfEntry 2 }

jnxPPPoEIfRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with READ-CREATE
         maximum access, according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            jnxPPPoEIfRowStatus
            jnxPPPoEIfLowerIfIndex

        In addition, when creating an entry the following conditions must hold:
            A value for jnxPPPoEIfIndex must have been determined previously,
            by reading jnxPPPoENextIfIndex.

            The interface identified by jnxPPPoEIfLowerIfIndex must exist, and
            must be an interface type that permits layering of PPPoEabove it.

        A corresponding entry in ifTable/ifXTable/jnxIfTable is created or
        destroyed as a result of creating or destroying an entry in this table.

         The following values can be read from this object:
             active(1)"
    ::= { jnxPPPoEIfEntry 3 }

jnxPPPoEIfLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of an interface over which this PPPoEinterface is to be
        layered.  A value of zero indicates no layering.  An implementation may
        choose to require that a nonzero value be configured at entry creation."
    ::= { jnxPPPoEIfEntry 4 }

jnxPPPoEIfAcName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name to use for the AC-NAME tag that is sent in any PADO that is
        sent on this interface."
    ::= { jnxPPPoEIfEntry 5 }

jnxPPPoEIfDupProtect OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Flag to allow duplicate MAC addresses."
    DEFVAL    { disable }
    ::= { jnxPPPoEIfEntry 6 }

jnxPPPoEIfPADIFlag OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }  
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This flag controls whether we always respond to a PADI with a PADO
        regardless of the ability to create the session and allows the session
        establish phase to resolve it."
    DEFVAL    { disable }
    ::= { jnxPPPoEIfEntry 7 }

jnxPPPoEIfAutoconfig OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This flags determines whether the upper PPPoEinterface is created
        dynamically or statically.  When enable(1) the interface is created
        dynamically."
    DEFVAL    {disable  }
    ::= { jnxPPPoEIfEntry 8 }

jnxPPPoEIfServiceNameTable OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Associate a PPPoEService Name Table with this interface for PADI
        processing."
    ::= { jnxPPPoEIfEntry 9 }

jnxPPPoEIfPadrRemoteCircuitIdCapture OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This flags determines whether the remote circuit id string will
        be captured and subsequently used as the NAS-PORT-ID radius
        attribute when it arrives as a tag in the PADR packet."
    DEFVAL    { disable }
    ::= { jnxPPPoEIfEntry 10 }

jnxPPPoEIfMtu OBJECT-TYPE
    SYNTAX      Integer32 (1|2|66..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The initial Maximum Transmit Unit (MTU) that the PPPoEmajor interface
        entity will advertise to the remote entity.

        If the value of this variable is 1 then the local PPPoEentity will
        use an MTU value determined by its underlying media interface.

        If the value of this variable is 2 then the local PPPoEentity will
        use a value determined by the PPPoEMax-Mtu-Tag transmitted from the
        client in the PADR packet.  If no Max-Mtu-Tag is received, the value
        defaults to a maximum of 1494.

		The operational MTU is limited by the MTU of the underlying media
        interface minus the PPPoEframe overhead."
    DEFVAL    { 1494 }
    ::= { jnxPPPoEIfEntry 11 }

jnxPPPoEIfLockoutMin OBJECT-TYPE
    SYNTAX      Integer32 (0..86400)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The lower bound, in seconds, of the time range used to specify 
        the duration of the lockout of the client from recognition for
        the specified interface.  This only takes effect if
        jnxPPPoEIfAutoconfig is set for this interface.

        The ability to lockout the client in the event of an error in
        creating a PPP interface is enabled by default.  The initial lockout
        duration is this object's value and increases exponentially for
        each failure that occurs for the client creating a PPP interface
        for the PPPoEinterface within the greater of 15 minutes
        and jnxPPPoEIfLockoutMax.

        The lockout duration for the client will not exceed jnxPPPoEIfLockoutMax.
        If the time between creation errors for the PPP interface for this
        interface is greater than the greater of 15 minutes and
        jnxPPPoEIfLockoutMax, then the lockout duration reverts to this
        object's value.


        To disable the ability to lockout the client from recognition in the
        event of an error in creating a PPP interface for the specified interface,
        the value of this object and jnxPPPoEIfLockoutMin must be set to 0.
        It is not recommended that this lockout feature be disabled except for 
        debugging purposes or when this interface supports more than one session."
    DEFVAL    { 0 }
    ::= { jnxPPPoEIfEntry 12 }

jnxPPPoEIfLockoutMax OBJECT-TYPE
    SYNTAX      Integer32 (0..86400)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The upper bound, in seconds, of the time range used to specify 
        the duration of the lockout of the client from recognition for
        the specified interface.  This only takes effect if
        jnxPPPoEIfAutoconfig is set for this interface.

        The ability to lockout the client from recognition in the event
        of an error in creating a PPP interface is enabled by default.
        The initial lockout duration is jnxPPPoEIfLockoutMin and
        increases exponentially for each failure that occurs for the client
        interface within the greater of 15 minutes and this object's value.

        The lockout duration for the client will not exceed jnxPPPoEIfLockoutMax.
        If the time between creation errors for the PPP interface for this
        interface is greater than the greater of 15 minutes and
        jnxPPPoEIfLockoutMax, then the lockout duration reverts to
        jnxPPPoEIfLockoutMin.

        To disable the ability to lockout the client from recognition in the
        event of an error in creating a PPP interface for the specified interface,
        the value of this object and jnxPPPoEIfLockoutMin must be set to 0.
        It is not recommended that this lockout feature be disabled except for 
        debugging purposes or when this interface supports more than one session."
    DEFVAL    { 0 }
	::= { jnxPPPoEIfEntry 13 }

jnxPPPoEIfDynamicProfile OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Attach dynamic-profile to this interface"
    DEFVAL    { " " }
    ::= { jnxPPPoEIfEntry 14 }

--
-- The PPPoEInterface Statistics Table
--
jnxPPPoEIfStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPPPoEIfStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The statistics for the PPP over Ethernet Interface for the PPPoE
        service on this interface."
    ::= { jnxPPPoEIfLayer 3 }

jnxPPPoEIfStatsEntry OBJECT-TYPE
    SYNTAX      JnxPPPoEIfStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The statistics for a particular PPPoEInterface."
    INDEX     { jnxPPPoEIfIfIndex }
    ::= { jnxPPPoEIfStatsTable 1 }

JnxPPPoEIfStatsEntry ::= SEQUENCE {
    jnxPPPoEIfStatsRxPADI                   Counter32,
    jnxPPPoEIfStatsTxPADO                   Counter32,
    jnxPPPoEIfStatsRxPADR                   Counter32,
    jnxPPPoEIfStatsTxPADS                   Counter32,
    jnxPPPoEIfStatsRxPADT                   Counter32,
    jnxPPPoEIfStatsTxPADT                   Counter32,
    jnxPPPoEIfStatsRxInvVersion             Counter32,
    jnxPPPoEIfStatsRxInvCode                Counter32,
    jnxPPPoEIfStatsRxInvTags                Counter32,
    jnxPPPoEIfStatsRxInvSession             Counter32,
    jnxPPPoEIfStatsRxInvTypes               Counter32,
    jnxPPPoEIfStatsRxInvPackets             Counter32,
    jnxPPPoEIfStatsRxInsufficientResources  Counter32,
    jnxPPPoEIfStatsTxPADM                   Counter32,
    jnxPPPoEIfStatsTxPADN                   Counter32,
    jnxPPPoEIfStatsRxInvTagLength           Counter32,
    jnxPPPoEIfStatsRxInvLength              Counter32,
    jnxPPPoEIfStatsRxInvPadISession         Counter32,
    jnxPPPoEIfStatsRxInvPadRSession         Counter32 }

jnxPPPoEIfStatsRxPADI OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADI packets received."
    ::= { jnxPPPoEIfStatsEntry 1 }

jnxPPPoEIfStatsTxPADO OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADO packets transmitted."
    ::= { jnxPPPoEIfStatsEntry 2 }

jnxPPPoEIfStatsRxPADR OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADR packets received."
    ::= { jnxPPPoEIfStatsEntry 3 }

jnxPPPoEIfStatsTxPADS OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADS packets transmitted."
    ::= { jnxPPPoEIfStatsEntry 4 }

jnxPPPoEIfStatsRxPADT OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADT packets received."
    ::= { jnxPPPoEIfStatsEntry 5 }

jnxPPPoEIfStatsTxPADT OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADT packets transmitted."
    ::= { jnxPPPoEIfStatsEntry 6 }

jnxPPPoEIfStatsRxInvVersion OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received with invalid version."
    ::= { jnxPPPoEIfStatsEntry 7 }

jnxPPPoEIfStatsRxInvCode OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received with invalid code."
    ::= { jnxPPPoEIfStatsEntry 8 }

jnxPPPoEIfStatsRxInvTags OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received with invalid tags."
    ::= { jnxPPPoEIfStatsEntry 9 }

jnxPPPoEIfStatsRxInvSession OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "Number of packets received with invalid session identifiers.

        This object became obsolete when separate counters were added for PADI
        and PADR packets."
    ::= { jnxPPPoEIfStatsEntry 10 }

jnxPPPoEIfStatsRxInvTypes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received with invalid types."
    ::= { jnxPPPoEIfStatsEntry 11 }

jnxPPPoEIfStatsRxInvPackets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of invalid packets received."
    ::= { jnxPPPoEIfStatsEntry 12 }

jnxPPPoEIfStatsRxInsufficientResources OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of session requests that could not be honored due to invalid
        resources."
    ::= { jnxPPPoEIfStatsEntry 13 }

jnxPPPoEIfStatsTxPADM OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADM packets transmitted."
    ::= { jnxPPPoEIfStatsEntry 14 }

jnxPPPoEIfStatsTxPADN OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADN packets transmitted."
    ::= { jnxPPPoEIfStatsEntry 15 }

jnxPPPoEIfStatsRxInvTagLength OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received with invalid tag length."
    ::= { jnxPPPoEIfStatsEntry 16 }

jnxPPPoEIfStatsRxInvLength OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received with invalid length."
    ::= { jnxPPPoEIfStatsEntry 17 }

jnxPPPoEIfStatsRxInvPadISession OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADI packets received with invalid session identifiers."
    ::= { jnxPPPoEIfStatsEntry 18 }

jnxPPPoEIfStatsRxInvPadRSession OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PADR packets received with invalid session identifiers."
    ::= { jnxPPPoEIfStatsEntry 19 }

--
-- The PPPoEInterface Client Lockout Table
--
jnxPPPoEIfLockoutTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPPPoEIfLockoutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "The lockout configuration and state of a PPPoEclient on this interface."
    ::= { jnxPPPoEIfLayer 4 }

jnxPPPoEIfLockoutEntry OBJECT-TYPE
    SYNTAX      JnxPPPoEIfLockoutEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains the configuration and state of a particular
         PPPoEinterface client lockout."
    INDEX     { jnxPPPoEIfIfIndex, jnxPPPoEIfLockoutClientAddress }
    ::= { jnxPPPoEIfLockoutTable 1 }

JnxPPPoEIfLockoutEntry ::= SEQUENCE {
	jnxPPPoEIfLockoutClientAddress     MacAddress,
	jnxPPPoEIfLockoutTime              Integer32,
	jnxPPPoEIfLockoutElapsedTime       Integer32,
	jnxPPPoEIfLockoutNextTime          Integer32 }

jnxPPPoEIfLockoutClientAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The source MAC address if the client."
    ::= { jnxPPPoEIfLockoutEntry 1 }

jnxPPPoEIfLockoutTime OBJECT-TYPE
    SYNTAX      Integer32 (0..86400)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time duration, in seconds, currently used to lockout the
        specified encapsulation type from recognition for the specified
        interface.  The reported value is within the range specified by
        jnxPPPoEIfLockoutMin and jnxPPPoEIfLockoutMax.  A value of 0 
        indicates that no lockout is occurring for the encapsulation type
        for the specified interface."
    ::= { jnxPPPoEIfLockoutEntry 2 }

jnxPPPoEIfLockoutElapsedTime OBJECT-TYPE
    SYNTAX      Integer32 (0..86400)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The elapsed time, in seconds, that the specified encapsulation type
        has been locked-out from recognition for the specified interface. 
        Its value will not exceed that of jnxPPPoEIfLockoutTime.  A value of 
        0 indicates that no lockout is occurring for the encapsulation type
        for the specified interface."
    ::= { jnxPPPoEIfLockoutEntry 3 }

jnxPPPoEIfLockoutNextTime OBJECT-TYPE
    SYNTAX      Integer32 (0..86400)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time duration, in seconds, that will be used to lockout the 
        specified encapsulation type from recognition for the specified
        interface for the next event that results in a lockout condition.
        The reported value is within the range specified by
        jnxPPPoEIfLockoutMin and jnxPPPoEIfLockoutMax.  When
        jnxPPPoEIfEnable is set to enable, a value of 0 indicates that
        lockout is prevented from occurring for the encapsulation type
        for the specified interface (i.e., jnxPPPoEIfLockoutMin and
        jnxPPPoEIfLockoutMax are both set to 0)."
    ::= { jnxPPPoEIfLockoutEntry 4 }


-- /////////////////////////////////////////////////////////////////////////////
--
-- PPPoESubinterface Layer
--
-- This layer is managed with the following elements:
--  o NextIfIndex (generator for PPPoEsubinterface IfIndex selection)
--  o SubIf Table (creation/configuration/deletion of PPPoEsubinterfaces)
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- IfIndex selection for creating new PPPoESubinterfaces
--
jnxPPPoESubIfNextIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in jnxPPPoESubIfTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { jnxPPPoESubIfLayer 1 }


--
-- The PPPoESubinterface Table
--
jnxPPPoESubIfTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPPPoESubIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for PPPoESubinterfaces present in the
        system."
    ::= { jnxPPPoESubIfLayer 2 }

jnxPPPoESubIfEntry OBJECT-TYPE
    SYNTAX      JnxPPPoESubIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a PPPoESubinterface.
        With READ-CREATE maximum access ,creating/deleting entries in this 
        table causes corresponding entries for
        be created /deleted in ifTable/ifXTable/jnxIfTable."
    INDEX     { jnxPPPoESubIfIndex }
    ::= { jnxPPPoESubIfTable 1 }

JnxPPPoESubIfEntry ::= SEQUENCE {
    jnxPPPoESubIfIndex          InterfaceIndex,
    jnxPPPoESubIfRowStatus      RowStatus,
    jnxPPPoESubIfLowerIfIndex   InterfaceIndexOrZero,
    jnxPPPoESubIfId             Integer32,
    jnxPPPoESubIfSessionId      Integer32,
    jnxPPPoESubIfMotm           DisplayString,
    jnxPPPoESubIfUrl            DisplayString }

jnxPPPoESubIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the PPPoESubinterface.  When creating entries in this
        table, suitable values for this object are determined by reading
        jnxPPPoESubNextIfIndex."
    ::= { jnxPPPoESubIfEntry 1 }

jnxPPPoESubIfRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with READ-CREATE
         maximum access ,according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            jnxPPPoESubIfRowStatus
            jnxPPPoESubIfLowerIfIndex

        In addition, when creating an entry the following conditions must hold:
            A value for jnxPPPoESubIfIndex must have been determined
            previously, by reading jnxPPPoESubIfNextIfIndex.

            The interface identified by jnxPPPoESubIfLowerIfIndex must exist,
            and must be a PPPoEinterface.

            A positive value configured for jnxPPPoESubIfId must not already be
            assigned to another subinterface layered onto the same underlying
            PPPoEinterface.

        A corresponding entry in ifTable/ifXTable/jnxIfTable is created or
        destroyed as a result of creating or destroying an entry in this table.

        The following values can be read from this object:
             active(1) "
    ::= { jnxPPPoESubIfEntry 2 }

jnxPPPoESubIfLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of a PPPoEinterface over which this PPPoESubinterface is
        to be layered.  A value of zero indicates no layering.  An
        implementation may choose to require that a nonzero value be configured
        at entry creation."
    ::= { jnxPPPoESubIfEntry 3 }

jnxPPPoESubIfId OBJECT-TYPE
    SYNTAX      Integer32 (-1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An integer identifier for the PPPoEsubinterface, used in conjunction
        with the command-line interface.  It is provided here for
        cross-reference purposes only.

        The value must be unique among subinterfaces configured on the same
        underlying PPPoEinterface.

        If this object is not configured, or is configured with a value of -1, a
        nonzero value will be allocated internally and can be retrieved from
        this object after table entry creation has succeeded.

        A value of zero for this object is reserved for future use."
    DEFVAL    { -1 }
    ::= { jnxPPPoESubIfEntry 4 }

jnxPPPoESubIfSessionId OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current sessionId associated with this sub-interface."
    ::= { jnxPPPoESubIfEntry 5 }

jnxPPPoESubIfMotm OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..127))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A message to send via a PADM on the sub-interface when the
        sub-interface transitions to the ifOperStatusUp state.  The client may
        choose to display this message to the user."
    ::= { jnxPPPoESubIfEntry 6 }

jnxPPPoESubIfUrl OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..127))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A URL to be sent via a PADM on the sub-interface when the sub-interface
        transitions to the ifOperStatusUp state.  The client may use this URL as
        the initial web-page for the user."
    ::= { jnxPPPoESubIfEntry 7 }

-- /////////////////////////////////////////////////////////////////////////////
--
-- PPPoEInterface per queue stats table.
-- This is a new table added in addition to existing 
-- JUNOSe PPPoEMIB.
-- /////////////////////////////////////////////////////////////////////////////

jnxPppoeSubIfQueueStatsTable OBJECT-TYPE
   SYNTAX	                    SEQUENCE OF JnxPppoeSubIfPerQueueStatsEntry
   MAX-ACCESS                       not-accessible
   STATUS                                  current
   DESCRIPTION
    "Table containing the Queue parameters for the PPPoEsessions."
::=  { jnxPPPoESubIfLayer 3 }   

jnxPppoeSubIfPerQueueStatsEntry OBJECT-TYPE
    SYNTAX      JnxPppoeSubIfPerQueueStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
               "The statistics for a particular trrafic class queue for 
                PPPoEsub Interface(i.e. session). ). Forwarding class to
                 queue number mapping is not always one-to-one. Forwarding
                  classes and queues are the same only when default 
                  forwarding-class-to-queue mapping is in effect "
    INDEX     { jnxPPPoESubIfIndex,
                jnxPppoeSubIfQueueIndex }
    ::= { jnxPppoeSubIfQueueStatsTable 1 }

JnxPppoeSubIfPerQueueStatsEntry ::= SEQUENCE {
jnxPppoeSubIfQueueIndex                                 INTEGER(0..7),
jnxPppoeSubIfQueueStatsPacketSent                       Counter64,
jnxPppoeSubIfQueueStatsBytesSent                        Counter64,
jnxPppoeSubIfQueueStatsPacketDropped                    Counter64,
jnxPppoeSubIfQueueStatsBytesDropped                     Counter64,
jnxPppoeSubIfQueueStatsActualBitRate                    Counter32,
jnxPppoeSubIfQueueStatsActualDroppedBitRate             Counter32 }

jnxPppoeSubIfQueueIndex                OBJECT-TYPE
      SYNTAX               INTEGER(0..7)
      MAX-ACCESS           not-accessible
      STATUS               current
      DESCRIPTION
      "This attribute returns the queue index ranging from 0 to 7 of the
      queue configure on the PPPoEsubinterface to support the traffic class for 
      PPPoEsession configured on that subinterface. Forwarding class to queue
      number mapping is not always one-to-one. Forwarding classes and queues are
       the same only when default forwarding-class-to-queue mapping is in effect."
::= { jnxPppoeSubIfPerQueueStatsEntry 1}

jnxPppoeSubIfQueueStatsPacketSent  OBJECT-TYPE
       SYNTAX            Counter64
       MAX-ACCESS   read-only
       STATUS             current
       DESCRIPTION   
                  "This attribute returns the counts of number of packet sent
                   per PPPoEsession and per queue."
       ::= { jnxPppoeSubIfPerQueueStatsEntry 2} 

jnxPppoeSubIfQueueStatsBytesSent   OBJECT-TYPE
       SYNTAX            Counter64
       MAX-ACCESS   read-only
       STATUS             current
       DESCRIPTION   
                  "This attribute returns the counts of number of bytes sent 
                  per PPPoEsession and per queue." 
       ::= { jnxPppoeSubIfPerQueueStatsEntry 3 }

jnxPppoeSubIfQueueStatsPacketDropped   OBJECT-TYPE
       SYNTAX            Counter64
       MAX-ACCESS   read-only
       STATUS             current
       DESCRIPTION   
                  "This attribute returns the number of packet dropped per 
                  PPPoEsession and per queue."
       ::= { jnxPppoeSubIfPerQueueStatsEntry 4}

 jnxPppoeSubIfQueueStatsBytesDropped   OBJECT-TYPE
       SYNTAX            Counter64
       MAX-ACCESS   read-only
       STATUS             current
       DESCRIPTION   
                  "This attribute returns the number of bytes dropped per 
                  PPPoEsession and per queue."
        ::= { jnxPppoeSubIfPerQueueStatsEntry 5 }

jnxPppoeSubIfQueueStatsActualBitRate   OBJECT-TYPE
       SYNTAX            Counter32
       MAX-ACCESS   read-only
       STATUS             current
       DESCRIPTION   
                  "This attribute returns the actual bit rate for per
                   PPPoEsession and per queue."
       ::= { jnxPppoeSubIfPerQueueStatsEntry  6 }
             
jnxPppoeSubIfQueueStatsActualDroppedBitRate    OBJECT-TYPE
       SYNTAX            Counter32
       MAX-ACCESS   read-only
       STATUS             current
       DESCRIPTION   
                  "This attribute returns the actual dropped bit rate for per 
                  PPPoEsession and per queue."
      ::= { jnxPppoeSubIfPerQueueStatsEntry 7 }

-- /////////////////////////////////////////////////////////////////////////////
-- /////////////////////////////////////////////////////////////////////////////
--
-- PPPoEService-name tables
--
--  The service-name tables are non interface based objects
-- This layer is managed with the following elements:
--
--  o Service-name table table (table if service-name tables)
--  o Service-name table (service-name table entries) indexed by Service-name
--    table name and service-name string value.
--  o Service-name AciAri table (service-name AciAri table entries) indexed by 
--    Service-name table name,service-name string value, Agent circuit
-- Id( Aci string value)
--    and Agent Remote Id (ari string value)
--
-- ///////////////////////////////////////////////////////////////

-- /////////////////////////////////////////////////////////////////////////////
--
-- Service-name table table
--
-- /////////////////////////////////////////////////////////////////////////////
jnxPPPoEServiceNameTableTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPPPoEServiceNameTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for the PPPoEService-name tables."
    ::= { jnxPPPoEServices 1 }

jnxPPPoEServiceNameTableEntry OBJECT-TYPE
    SYNTAX      JnxPPPoEServiceNameTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The parameters for the PPPoEservice-name table."
    INDEX     { jnxPPPoEServiceNameTableName }
    ::= { jnxPPPoEServiceNameTableTable 1 }

JnxPPPoEServiceNameTableEntry ::= SEQUENCE {
    jnxPPPoEServiceNameTableName        DisplayString,
    jnxPPPoEServiceNameTableRowStatus   RowStatus }

jnxPPPoEServiceNameTableName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Service-name table name."
    ::= { jnxPPPoEServiceNameTableEntry 1 }


jnxPPPoEServiceNameTableRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with READ-CREATE
         maximum access,according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            jnxPPPoEServiceNameTableRowStatus
            jnxPPPoEServiceNameTableName
           

        The Empty Service and  Any  service will be automatically configured 
       for each Service Name Table created. On creating or deleting an entry in 
        this table will create/destroy an entry for <Empty >Service and <Any> 
        service in jnxServiceNameTable.

        A corresponding entry in jnxServiceNameTable gets created or destroyed
        as a result of creating or destroying an entry in this table.
         The following values can be read from this object:
             active(1) "
    ::= { jnxPPPoEServiceNameTableEntry 2 }

-- ==========================================================================

-- Service-name Table

-- ========================================================================
jnxPPPoEServiceNameTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPPPoEServiceNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for the PPPoEService-names."
    ::= { jnxPPPoEServices 2 }

jnxPPPoEServiceNameEntry OBJECT-TYPE
    SYNTAX      JnxPPPoEServiceNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The parameters for the PPPoEservice-name table entry."
    INDEX     { jnxPPPoEServiceNameTableName,
                jnxPPPoEServiceName }
    ::= { jnxPPPoEServiceNameTable 1 }

JnxPPPoEServiceNameEntry ::= SEQUENCE {
    jnxPPPoEServiceName                DisplayString,
    jnxPPPoEServiceNameAction          JnxPPPoEServiceNameAction,
    jnxPPPoEServiceNameDynamicProfile  DisplayString,
    jnxPPPoEServiceNameRoutingInstance DisplayString,
    jnxPPPoEServiceNameMaxSessions     Unsigned32,
    jnxPPPoEServiceNameRowStatus       RowStatus }

jnxPPPoEServiceName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..64))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Service-name tag value."
    ::= { jnxPPPoEServiceNameEntry 1 }

jnxPPPoEServiceNameAction OBJECT-TYPE
    SYNTAX      JnxPPPoEServiceNameAction
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Identifies the behavior when the the Service-name tag is received in a
        PADI frame."
    ::= { jnxPPPoEServiceNameEntry 2 }

jnxPPPoEServiceNameDynamicProfile OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Dynamic Profile associated with a Service-name."
    ::= { jnxPPPoEServiceNameEntry 3 }

jnxPPPoEServiceNameRoutingInstance OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Routing Instance associated with a Service-name."
    ::= { jnxPPPoEServiceNameEntry 4 }

jnxPPPoEServiceNameMaxSessions OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Max Sessions value used to cap the number of active PPPoEssessions 
        that may be established with the specified Service entry."
    ::= { jnxPPPoEServiceNameEntry 5 }


jnxPPPoEServiceNameRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with READ-CREATE 
        maximum access  ,according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            jnxPPPoEServiceNameRowStatus

        The Service name is configured via the INDEX specified.

        A corresponding entry in jnxPPPoEServiceNameAciAriTable is destroyed
        as a result of destroying an entry in this table.

        The following values can be read from this object:
             active(1)"
    ::= { jnxPPPoEServiceNameEntry 6 }

-- ===========================================================================


--Service-name ACI ARI Table

-- ==============================================
jnxPPPoEServiceNameAciAriTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPPPoEServiceNameAciAriEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for the PPPoEServicename AciAri entries."
    ::= { jnxPPPoEServices 3 }

jnxPPPoEServiceNameAciAriEntry OBJECT-TYPE
    SYNTAX      JnxPPPoEServiceNameAciAriEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The parameters for the PPPoEservice-name AciAri table entry."
    INDEX     { jnxPPPoEServiceNameTableName,
                jnxPPPoEServiceName, 
                jnxPPPoEServiceNameAgentCircuitId,
                jnxPPPoEServiceNameAgentRemoteId
                }
    ::= { jnxPPPoEServiceNameAciAriTable 1 }

JnxPPPoEServiceNameAciAriEntry ::= SEQUENCE {
    jnxPPPoEServiceNameAgentCircuitId                DisplayString,
    jnxPPPoEServiceNameAgentRemoteId                 DisplayString,
    jnxPPPoEServiceNameAciAriAction                  JnxPPPoEServiceNameAction,
    jnxPPPoEServiceNameAciAriDynamicProfile          DisplayString,
    jnxPPPoEServiceNameAciAriRoutingInstance         DisplayString,
    jnxPPPoEServiceNameAciAriStaticInterface         DisplayString,
    jnxPPPoEServiceNameAciAriRowStatus               RowStatus }

jnxPPPoEServiceNameAgentCircuitId OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..64))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "ACI tag values that the PPPoEclient would send in the PADI/PADR 
        control packet."
    ::= { jnxPPPoEServiceNameAciAriEntry 1 }

jnxPPPoEServiceNameAgentRemoteId OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..64))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "ACI tag values that the PPPoEclient would send in the PADI/PADR 
        control packet."
    ::= { jnxPPPoEServiceNameAciAriEntry 2 }


jnxPPPoEServiceNameAciAriAction OBJECT-TYPE
    SYNTAX      JnxPPPoEServiceNameAction
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Identifies the behavior when the the Service-name with ACI/ARI pairs 
        is received in a PADI frame."
    ::= { jnxPPPoEServiceNameAciAriEntry 3 }

jnxPPPoEServiceNameAciAriDynamicProfile OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Dynamic Profile associated with a Service-name and ACI/ARI pairs"
    ::= { jnxPPPoEServiceNameAciAriEntry 4 }

jnxPPPoEServiceNameAciAriRoutingInstance OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..31))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Routing-Instance associated with a Service-name and ACI/ARI pairs"
    ::= { jnxPPPoEServiceNameAciAriEntry 5 }

jnxPPPoEServiceNameAciAriStaticInterface OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Static Interface associated with each ACI/ARI Entry."
    ::= { jnxPPPoEServiceNameAciAriEntry 6 }


jnxPPPoEServiceNameAciAriRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with READ-CREATE
         maximum access, according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            jnxPPPoEServiceNameAciAriRowStatus

        The ACIARI Entry is configured via the INDEX specified.

        The following values can be read from this object:
             active(1)"
    ::= { jnxPPPoEServiceNameAciAriEntry 7 }

-- 
-- ////////////////////////////////////////////////////////////////////////////
--
-- PPP Interface Summary Counts
--
-- /////////////////////////////////////////////////////////////////////////////
jnxPPPoEMajorInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEmajor interfaces configured and created in
        the system."
    ::= { jnxPPPoESummary 1 }

jnxPPPoESummaryMajorIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEmajor interfaces in the system that are
        administratively configured to up(1)."
    REFERENCE
        "ifAdminStatus from IF-MIB"
    ::= { jnxPPPoESummary 2 }

jnxPPPoESummaryMajorIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEmajor interfaces in the system that are
        administrateively configued to down(2)."
    REFERENCE
        "ifAdminStatus from IF-MIB"
    ::= { jnxPPPoESummary 3 }

jnxPPPoESummaryMajorIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEmajor interfaces in the system with an
        operational state of up(1)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 4 }

jnxPPPoESummaryMajorIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEmajor interfaces in the system with an
        operational state of down(2)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 5 }

jnxPPPoESummaryMajorIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEmajor interfaces in the system with an
        operational state of lowerLayerDown(7)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 6 }

jnxPPPoESummaryMajorIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEmajor interfaces in the system with an
        operational state of notPresent(6)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 7 }

jnxPPPoESummarySubInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEsubinterfaces configured in the system."
    ::= { jnxPPPoESummary 8 }

jnxPPPoESummarySubIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEsubinterfaces in the system that are
        administratively configured to up(1)."
    REFERENCE
        "ifAdminStatus from IF-MIB"
    ::= { jnxPPPoESummary 9 }

jnxPPPoESummarySubIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEsubinterfaces in the system that are
        administrateively configued to down(2)."
    REFERENCE
        "ifAdminStatus from IF-MIB"
    ::= { jnxPPPoESummary 10 }

jnxPPPoESummarySubIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEsubinterfaces in the system with an
        operational state of up(1)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 11 }

jnxPPPoESummarySubIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEsubinterfaces in the system with an
        operational state of down(2)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 12 }

jnxPPPoESummarySubIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEsubinterfaces in the system with an
        operational state of lowerLayerDown(7)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 13 }

jnxPPPoESummarySubIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPPoEsubinterfaces in the system with an
        operational state of notPresent(6)."
    REFERENCE
        "ifOperStatus from IF-MIB"
    ::= { jnxPPPoESummary 14 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- jnxPPPoETrapControl      OBJECT IDENTIFIER ::= { jnxPPPoEMIB 2 }
-- jnxPPPoETraps            OBJECT IDENTIFIER ::= { jnxPPPoEMIB 3 }
-- jnxPPPoETrapPrefix       OBJECT IDENTIFIER ::= { jnxPPPoETraps 0 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
jnxPPPoEConformance OBJECT IDENTIFIER ::= { jnxPPPoEMIB 4 }
jnxPPPoECompliances OBJECT IDENTIFIER ::= { jnxPPPoEConformance 1 }
jnxPPPoEGroups      OBJECT IDENTIFIER ::= { jnxPPPoEConformance 2 }


END


