ENTERASYS-IEEE802DOT11EXT-MIB DEFINITIONS ::= BEGIN

IMPORTS
 
    MODULE-IDENTITY, OBJECT-TYPE                FROM SNMPv2-SMI
    TEXTUAL-CONVENTION,
    TruthValue, MacAddress,
    AutonomousType                              FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP             FROM SNMPv2-CONF 
    SnmpAdminString                             FROM SNMP-FRAMEWORK-MIB 
    ifIndex                                     FROM IF-MIB           
    EnabledStatus                               FROM P-BRIDGE-MIB     
    dot11WEPDefaultKeyIndex                     FROM IEEE802dot11-MIB 
    etsysModules                                FROM ENTERASYS-MIB-NAMES;
                         
etsysDot11ExtMIB MODULE-IDENTITY
    LAST-UPDATED "200203071945Z"  -- Thu Mar  7 19:45 GMT 2002
    ORGANIZATION "Enterasys Networks, Inc"
    CONTACT-INFO
    "Postal: Enterasys Networks
             35 Industrial Way, P.O. Box 5005
             Rochester, NH 03867-0505

     Phone:  +1 603 332 9400
     E-mail: support@enterasys.com
     WWW:    http://www.enterasys.com"
   
     DESCRIPTION
        "This mib module defines a portion of the SNMP enterprise
         MIBs under Enterasys Networks enterprise OID as an extension 
         to the IEEE802Dot11 MIB.
         
         This Enterasys Networks Proprietary MIB was designed to be 
         used for read-write access to configuration objects not provided
         by IEEE802.11 MIB, or any other standard MIB."
            
    REVISION "200203071945Z"  -- Thu Mar  7 19:45 GMT 2002
    DESCRIPTION
       "Removed some comments so that it would compile."

    REVISION "200105081800Z"
    DESCRIPTION
       "The initial version of this MIB module"

    ::= { etsysModules 9 }
       
-- ----------------------------------------------------------------------------
-- MIB Objects
-- ----------------------------------------------------------------------------

etsysDot11ExtObjects        OBJECT IDENTIFIER ::= { etsysDot11ExtMIB 1 }
     
etsysDot11ExtLinkTest       OBJECT IDENTIFIER ::= { etsysDot11ExtObjects 1 }           
etsysDot11ExtGeneral        OBJECT IDENTIFIER ::= { etsysDot11ExtObjects 2 }
etsysDot11ExtBldg           OBJECT IDENTIFIER ::= { etsysDot11ExtObjects 3 }
etsysDot11ExtWEP            OBJECT IDENTIFIER ::= { etsysDot11ExtObjects 4 }
etsysDot11ExtEffect         OBJECT IDENTIFIER ::= { etsysDot11ExtObjects 5 }
                    
-- ----------------------------------------------------------------------------
  
etsysDot11ExtLinkTestTable OBJECT-TYPE
        SYNTAX SEQUENCE OF EtsysDot11ExtLinkTestEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This table contains objects to test the link between a 
             requester (entity which sends out the management request 
             message) and a responder (entity which responds with 
             the appropriate management response message). An entity
             could be either an Access Point(AP) or a station (STA)."
                 
        ::= {  etsysDot11ExtLinkTest 1 }

etsysDot11ExtLinkTestEntry OBJECT-TYPE
        SYNTAX EtsysDot11ExtLinkTestEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the LinkTest Table.  
             By means of message transmission between requester
             and responder, the communication quality between the 
             two stations can be determined. The requester and 
             responder can be any combination of AP and STA except
             STA to STA in an Infrastructure Network (network which 
             has at least one AP present."
             
        INDEX {ifIndex}
    
        ::= {  etsysDot11ExtLinkTestTable 1 }

EtsysDot11ExtLinkTestEntry ::=
        SEQUENCE {
                    etsysDot11ExtLTRemoteStationMAC            MacAddress,
                    etsysDot11ExtLTRemoteStationName           SnmpAdminString,              
                    etsysDot11ExtLTTrigger                     INTEGER,
                    etsysDot11ExtLTRemoteContents              OCTET STRING           
         }  
  
 
    etsysDot11ExtLTRemoteStationMAC OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "The MAC address for the remote station to participate
                 in the Link Test.

                 To initiate a search for a participating station, write the
                 broadcast address (FF-FF-FF-FF-FF-FF) to this variable."

        ::= { etsysDot11ExtLinkTestEntry 1 }

    etsysDot11ExtLTRemoteStationName OBJECT-TYPE
        SYNTAX  SnmpAdminString (SIZE (0..20))
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "The wireless station name of the remote station
                 participating in the Link Test."

        ::= { etsysDot11ExtLinkTestEntry 2 }

    etsysDot11ExtLTTrigger OBJECT-TYPE
        SYNTAX  INTEGER (1..1)
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "Writing a 1 to this variable causes a single Link Test 
                 request message to be sent to the remote station."

        ::= { etsysDot11ExtLinkTestEntry 3 }

    
    etsysDot11ExtLTRemoteContents OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE  (84))
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "The exact byte-by-byte contents of the Link Test packet returned by
                 the remote station."

        ::= { etsysDot11ExtLinkTestEntry 4 }

etsysDot11ExtGeneralTable OBJECT-TYPE
        SYNTAX SEQUENCE OF EtsysDot11ExtGeneralEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This table contains all the objects that must be 
            configured on every radio card installed in the 
            Access Point regardless of the operating mode in use."
    
        ::= {  etsysDot11ExtGeneral 1 }

etsysDot11ExtGeneralEntry OBJECT-TYPE
        SYNTAX EtsysDot11ExtGeneralEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the Dot11General Table.  
             This allows for multiple instances of radio cards 
             in the Access Point."

        INDEX {ifIndex}
    
        ::= {  etsysDot11ExtGeneralTable 1 }

EtsysDot11ExtGeneralEntry ::=
        SEQUENCE {   
                    etsysDot11ExtPCCardType                INTEGER,
                    etsysDot11ExtPCCardVersions            SnmpAdminString, 
                    etsysDot11ExtBridgeMode                INTEGER,
                    etsysDot11ExtResetOptions              INTEGER,
                    etsysDot11ExtSystemScale               INTEGER,
                    etsysDot11ExtSecureAccess              EnabledStatus,
                    etsysDot11ExtMulticastTxRate           INTEGER,
                    etsysDot11ExtIntraBSSRelay             EnabledStatus,
                    etsysDot11ExtStationName               SnmpAdminString
         }  
                     
                  
    etsysDot11ExtPCCardType OBJECT-TYPE
        SYNTAX  INTEGER  {                              
                        none(1), 
                        deprecatedValue1(2),
                        deprecatedValue2(3),
                        deprecatedValue3(4),
                        ds80211b(5),    -- IEEE 802.11 2.4Ghz DS 11Mb card 
                        ds80211a(6),    -- IEEE 802.11 2.4Ghz DS 54Mb card   
                        unknown(15)
                }
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "The type of PC card inserted in the Access Point."
        
        ::= { etsysDot11ExtGeneralEntry 1 }


    etsysDot11ExtPCCardVersions OBJECT-TYPE
        SYNTAX  SnmpAdminString (SIZE (1..80))
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Specifies the version identifiers for the PC card.
                 This will indicate both the Hardware and the Firmware
                 versions."

        ::= { etsysDot11ExtGeneralEntry 2 }

    etsysDot11ExtBridgeMode OBJECT-TYPE
        SYNTAX  INTEGER  {                                 
                        workgroup(1),
                        lanToLanEndpoint(2),            
                        lanToLanMultipoint(3)      
                }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "CURRENT Access Point bridge mode state.  
                 
                 In workgroup mode all communications between clients 
                 passes through the Access Point.
                 
                 LAN-to-LAN mode is the improved name for 802.11.  
                 LAN-to-LAN used to be called full-bridge pre-802.11.
                 This mode is a method of connecting two wired LAN's 
                 via a wireless link, also referred to as Point-to-Point 
                 mode.
                             
                 LAN-to-LAN-HUB mode allows the interconnection of multiple 
                 (ie. more than two) wired LAN's via wireless links, also 
                 referred to as Point-to-MultiPoint mode. 
                 
                 When operating in multimode the Access Point can simultaneously 
                 operate in both workgroup mode and either Point-to-Point or
                 Point-to-MultiPoint modes.
                 
                 This object must be saved across a system reset and/or a 
                 power cycle."
                                          
                                                     
        ::= { etsysDot11ExtGeneralEntry 3 }
       
    etsysDot11ExtResetOptions   OBJECT-TYPE
        SYNTAX  INTEGER {
                        noReset (0),
                        resetRadioCardIfNecessary (1),
                        resetRadioCardRegardless (2)
                }       
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                 "noReset (0)
                  No reset is performed. A 'get' on this object always returns 
                  this value.
                 
                  resetRadioCardIfNecessary (1)
                  Some parameters can only be given to the card at initialization
                  time, and if any of these are changed, a card reset will be 
                  necessary for them to go into place. The card will be reset at 
                  this time if any of those parameters have indeed been changed.
                  
                  resetRadioCardRegardless (2)                  
                  Forces the radio card to reset, even if no radio card 
                  parameters have been changed."

            ::= { etsysDot11ExtGeneralEntry 4 }

    
    etsysDot11ExtSystemScale OBJECT-TYPE
        SYNTAX  INTEGER  {
                        low(1),
                        medium(2),
                        high(3)
                }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "Specifies the CURRENT Access Point density in the 
                 Extended Service Set (ESS).
                 
                 This object must be saved across a system reset and/or a 
                 power cycle."
                 

        ::= { etsysDot11ExtGeneralEntry 5 }

    etsysDot11ExtSecureAccess OBJECT-TYPE
        SYNTAX  EnabledStatus
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "When this mode is set to enabled, the AP will only associate
                 with stations that have the same network name as the AP.
                 When this mode is set to disabled, a station with the
                 network name of ANY is allowed to associate.
                 
                 This object must be saved across a system reset and/or a 
                 power cycle."
                
        ::= { etsysDot11ExtGeneralEntry 6 }
        
    etsysDot11ExtMulticastTxRate OBJECT-TYPE
        SYNTAX  INTEGER  {
                            fixed1Mbit(1),
                            fixed2Mbit(2),
                            fixedMediumRate(3),
                            fixedHighRate(4)
                }           
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "This value specifies the Multicast data transmission 
                 rate of the AP. It is implemented when cards that operate
                 faster than the 2Mbit 802.11 standard are inserted.
                 
                 This object must be saved across a system reset and/or a 
                 power cycle."

        ::= { etsysDot11ExtGeneralEntry 7 }

    etsysDot11ExtIntraBSSRelay OBJECT-TYPE
        SYNTAX  EnabledStatus     
        MAX-ACCESS  read-write
        STATUS  current        
        DESCRIPTION
                "When this mode is enabled the AP entity within the PC Card will
                 relay frames to destined for stations associated with it and will NOT
                 forward them to the bridging entity within the AP.
                 When this mode is set to disabled, the AP entity within the PC Card 
                 will not relay frames from wireless client(s) to station(s) associated with it, 
                 instead forwards frames to the bridging entity within the AP.
                 
                 This object must be saved across a system reset and/or a 
                 power cycle."

        ::= { etsysDot11ExtGeneralEntry 8 }   
 
    etsysDot11ExtStationName OBJECT-TYPE
        SYNTAX  SnmpAdminString (SIZE (0..20))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "DURABLE:
                The wireless station name sent out as part of
                the beacon messages.  Valid only when a DS card
                is inserted in the Access Point."

        ::= { etsysDot11ExtGeneralEntry 9 }


-- ----------------------------------------------------------------------------
-- 802.11 Building-to-Building section.
-- ---------------------------------------------------------------------------- 

etsysDot11ExtBldgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF EtsysDot11ExtBldgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This table contains the objects required to enable
             the Access Point to operate in Point-to-MultiPoint mode."
    
        ::= {  etsysDot11ExtBldg 1 }

etsysDot11ExtBldgEntry OBJECT-TYPE
        SYNTAX EtsysDot11ExtBldgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "An Entry (conceptual row) in the Dot11Bldg Table.
             A collection of objects containing information for activating 
             and using the Access Point in Point-to-MultiPoint mode."

        INDEX {ifIndex}
    
        ::= {  etsysDot11ExtBldgTable 1 }

EtsysDot11ExtBldgEntry ::=
        SEQUENCE {       
                    etsysDot11ExtBldgRemoteMAC1        MacAddress,                    
                    etsysDot11ExtBldgRemoteMAC2        MacAddress,
                    etsysDot11ExtBldgRemoteMAC3        MacAddress,
                    etsysDot11ExtBldgRemoteMAC4        MacAddress,
                    etsysDot11ExtBldgRemoteMAC5        MacAddress,
                    etsysDot11ExtBldgRemoteMAC6        MacAddress,
                    etsysDot11ExtBldgMPActivationKey   OCTET STRING                                          
         }  

    etsysDot11ExtBldgRemoteMAC1 OBJECT-TYPE          
        SYNTAX  MacAddress
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "The MAC address for the remote station participating
             in a 802.11 Building-to-Building link.
             
             This object must be saved across a system reset and/or a 
             power cycle."     
             
        ::= { etsysDot11ExtBldgEntry 1 }
         

    etsysDot11ExtBldgRemoteMAC2 OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "The MAC address for the remote station participating
             in a 802.11 Building-to-Building link.
             
             This object must be saved across a system reset and/or a 
             power cycle."

        ::= { etsysDot11ExtBldgEntry 2 }

    etsysDot11ExtBldgRemoteMAC3 OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "The MAC address for the remote station participating
             in a 802.11 Building-to-Building link.
             
             This object must be saved across a system reset and/or a 
             power cycle."


        ::= { etsysDot11ExtBldgEntry 3 }

    etsysDot11ExtBldgRemoteMAC4 OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "The MAC address for the remote station participating
             in a 802.11 Building-to-Building link.
             
             This object must be saved across a system reset and/or a 
             power cycle."

        ::= { etsysDot11ExtBldgEntry 4 }

    etsysDot11ExtBldgRemoteMAC5 OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "The MAC address for the remote station participating
             in a 802.11 Building-to-Building link.
             
             This object must be saved across a system reset and/or a 
             power cycle."

        ::= { etsysDot11ExtBldgEntry 5 }

    etsysDot11ExtBldgRemoteMAC6 OBJECT-TYPE
        SYNTAX  MacAddress
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
            "The MAC address for the remote station participating
             in a 802.11 Building-to-Building link.
             
             This object must be saved across a system reset and/or a 
             power cycle."

        ::= { etsysDot11ExtBldgEntry 6 }
 
    etsysDot11ExtBldgMPActivationKey OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(16))
        MAX-ACCESS  read-write
        STATUS  current        
        DESCRIPTION
               "Point-to-multipoint bridge mode requires an activation 
                key to enable. A valid multipoint activation key must
                be entered as a string of ACSCII characters translating
                to the binary HEX value of the key before the Access Point 
                will accept the point-to-multipoint bridge mode setting.
              
                Returns SNMP_BAD_VALUE if validation fails.
                
                This object must be saved across a system reset and/or a 
                power cycle."

        ::= { etsysDot11ExtBldgEntry 7 }

       
etsysDot11ExtWEPDefaultKeysTable OBJECT-TYPE
        SYNTAX SEQUENCE OF EtsysDot11ExtWEPDefaultKeysEntry       
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Conceptual table for WEP default keys.  This table shall
            contain the four WEP default secret key values
            corresponding to the four possible KeyID values.  The WEP
            default secret keys are logically WRITE-ONLY.  Attempts to
            read the entries in this table shall return unsuccessful
            status and a value of null. The default value of each WEP 
            default key shall be null."

        REFERENCE "IEEE Std 802.11-1997, 8.3.2"
    
        ::= {   etsysDot11ExtWEP 1 }
 
etsysDot11ExtWEPDefaultKeysEntry OBJECT-TYPE 
        SYNTAX EtsysDot11ExtWEPDefaultKeysEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the WEP Default Keys Table.
             A collection of objects containing information used to
             determine if a WEPkey as been defined and if so, the 
             value of the WEPkey."

        INDEX {ifIndex, dot11WEPDefaultKeyIndex }           
        
        ::= {  etsysDot11ExtWEPDefaultKeysTable  1 }

EtsysDot11ExtWEPDefaultKeysEntry ::= 
        SEQUENCE  {
                    etsysDot11ExtWEPKeyDefined            TruthValue,
                    etsysDot11ExtWEPKeyValue              OCTET STRING
                         }

    etsysDot11ExtWEPKeyDefined OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The state column used for determining if an
             encryption key is set (true) or not (false), 
             false is the default value."
                    
        ::= {  etsysDot11ExtWEPDefaultKeysEntry 1 }

    etsysDot11ExtWEPKeyValue OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(5|13))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "A WEP default secret key value. For 40-bit encryption
                 use 5 printable characters or 10 HEX digits. For 128-bit 
                 encryption use 13 printable characters or 26 HEX digits.
                 
                 This object must be saved across a system reset and/or a 
                 power cycle."
          
        ::= {  etsysDot11ExtWEPDefaultKeysEntry 2 }  
 
 
etsysDot11ExtWEPEnhancedTable OBJECT-TYPE
        SYNTAX SEQUENCE OF EtsysDot11ExtWEPEnhancedEntry       
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Conceptual table for WEP default keys.  This table shall
            contain the four WEP default secret key values
            corresponding to the four possible KeyID values.  The WEP
            default secret keys are logically WRITE-ONLY.  Attempts to
            read the entries in this table shall return unsuccessful
            status and a value of null. The default value of each WEP 
            default key shall be null."

        REFERENCE "IEEE Std 802.11-1997, 8.3.2"
    
        ::= {   etsysDot11ExtWEP 2 }
 
etsysDot11ExtWEPEnhancedEntry OBJECT-TYPE 
        SYNTAX EtsysDot11ExtWEPEnhancedEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the WEP Default Keys Table.
             A collection of objects containing information used to
             determine if a WEPkey as been defined and if so, the 
             value of the WEPkey."

        INDEX {ifIndex }           
        
        ::= {  etsysDot11ExtWEPEnhancedTable  1 }

EtsysDot11ExtWEPEnhancedEntry ::= 
        SEQUENCE  {
                  etsysDot11ExtWEPEnhancedImplemented   TruthValue
        }

    etsysDot11ExtWEPEnhancedImplemented OBJECT-TYPE
        SYNTAX  TruthValue
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "This value indicates whether the AP is capable of Enhanced
                 Wireless Equivalent Privacy (WEP), using 128-bit keys."

        ::= { etsysDot11ExtWEPEnhancedEntry 1 }


etsysDot11ExtOIDNotInEffectTable OBJECT-TYPE
        SYNTAX SEQUENCE OF EtsysDot11ExtOIDNotInEffectEntry       
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            " This table will be used to determine which wireless
              parameters have been modified but are not yet in effect.
              These parameters will not take effect until a reset has been 
              performed."
                
        ::= { etsysDot11ExtEffect 1 }                 
 
etsysDot11ExtOIDNotInEffectEntry OBJECT-TYPE 
        SYNTAX EtsysDot11ExtOIDNotInEffectEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "
            "

        INDEX { ifIndex, etsysDot11ExtOIDIndex }           
        
        ::= {  etsysDot11ExtOIDNotInEffectTable  1 }

EtsysDot11ExtOIDNotInEffectEntry ::= 
        SEQUENCE  {  
                    etsysDot11ExtOIDIndex          AutonomousType,
                    etsysDot11ExtOIDNotInEffect    TruthValue        
        }
     
            
     etsysDot11ExtOIDIndex OBJECT-TYPE
        SYNTAX AutonomousType
        MAX-ACCESS not-accessible         
        STATUS current
        DESCRIPTION
            " This object will keep a list of OIDS"
               -- Fix this descriptions later     
        ::= {  etsysDot11ExtOIDNotInEffectEntry 1 }
     
     etsysDot11ExtOIDNotInEffect  OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            " This object specifies if the OID being accesed currently
            has been changed but is not in effect."
            -- Fix this descriptions later 
        ::= {  etsysDot11ExtOIDNotInEffectEntry 2 }


      
-- -------------------------------------------------------------
-- Conformance Information
-- -------------------------------------------------------------

etsysDot11ExtConformance OBJECT IDENTIFIER ::= { etsysDot11ExtMIB 2 }
etsysDot11ExtGroups      OBJECT IDENTIFIER ::= { etsysDot11ExtConformance 1 }
etsysDot11ExtCompliances OBJECT IDENTIFIER ::= { etsysDot11ExtConformance 2 }

-- -------------------------------------------------------------
-- Units of conformance
-- -------------------------------------------------------------

etsysDot11ExtBaseGroup OBJECT-GROUP
    OBJECTS {   
                etsysDot11ExtLTRemoteStationMAC,
                etsysDot11ExtLTRemoteStationName,
                etsysDot11ExtLTTrigger,
                etsysDot11ExtLTRemoteContents,
                etsysDot11ExtSystemScale,
                etsysDot11ExtSecureAccess,
                etsysDot11ExtMulticastTxRate,
                etsysDot11ExtIntraBSSRelay,
                etsysDot11ExtPCCardType,    
                etsysDot11ExtPCCardVersions,               
                etsysDot11ExtBridgeMode, 
                etsysDot11ExtResetOptions,
                etsysDot11ExtStationName, 
                etsysDot11ExtBldgRemoteMAC1,               
                etsysDot11ExtBldgRemoteMAC2,
                etsysDot11ExtBldgRemoteMAC3,
                etsysDot11ExtBldgRemoteMAC4,
                etsysDot11ExtBldgRemoteMAC5,
                etsysDot11ExtBldgRemoteMAC6,
                etsysDot11ExtBldgMPActivationKey, 
                etsysDot11ExtWEPKeyDefined,
                etsysDot11ExtWEPKeyValue, 
                etsysDot11ExtWEPEnhancedImplemented,
                etsysDot11ExtOIDNotInEffect                                
            }
    STATUS      current
    DESCRIPTION
        "The basic etsysDot11Ext stuff."
    
    ::= { etsysDot11ExtGroups 1 }

-- -------------------------------------------------------------
-- Compliance statements
-- -------------------------------------------------------------

etsysDot11ExtCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for devices that support 
         802Dot11 extensions."

    MODULE
        MANDATORY-GROUPS { etsysDot11ExtBaseGroup }

    ::= { etsysDot11ExtCompliances 1 }

END 
