
-- *****************************************************************************
-- Juniper-QoS-MIB
--
-- Juniper Networks Enterprise MIB
--   Quality of Service (QoS) MIB
--
-- Copyright (c) 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002 - 2005 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************


Juniper-QoS-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Gauge32, Counter64, Unsigned32, Integer32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, RowStatus, TruthValue, DisplayString
        FROM SNMPv2-TC
    ifIndex
        FROM IF-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    juniMibs
        FROM Juniper-MIBs;

juniQosMIB  MODULE-IDENTITY
    LAST-UPDATED "200507061418Z"  -- 06-Jul-05 10:18 AM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The Quality of Service (QoS) MIB for the Juniper Networks enterprise."
    -- Revision History
    REVISION    "200507061418Z"  -- 06-Jul-05 10:18 AM EDT  - JUNOSe 7.0
    DESCRIPTION
        "Added support for QoS SVlans."
    REVISION    "200504011900Z"  -- 1-Apr-05 03:00 PM EDT  - JUNOSe 7.0
    DESCRIPTION
        "Added support for QoS Parameters."
    REVISION    "200412101916Z"  -- 10-Dec-04 03:16 PM EDT  - JUNOSe 6.1
    DESCRIPTION
        "o Added support for compound shared shaping.  Scheduler-profile
           list reved.
         o Added/Corrected DEFVALs for QosProfileElementEntry."
    REVISION    "200401261419Z"  -- 26-Jan-04 09:19 AM EST  - JUNOSe 6.0
    DESCRIPTION
        "Added support for multiple traffic class groups."
    REVISION    "200311042010Z"  -- 04-Nov-03 03:10 PM EST  - JUNOSe 5.3
    DESCRIPTION
        "Added support for Hierarchical Assured Rate."
    REVISION    "200305081705Z"  -- 08-May-03 01:05 PM EDT  - JUNOSe 5.1
    DESCRIPTION
        "Added support for ATM VP UID, statistics profile list, scheduler
        profile assured rate, and QoS mode port."
    REVISION    "200303131817Z"  -- 13-Mar-03 01:17 PM EST  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         Added drop profile list support."
    REVISION    "200303121830Z"  -- 12-Mar-03 01:30 PM EST  - JUNOSe 4.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 57 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

JuniQosLogicalInterfaceType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A logical interface type supported by QoS."
    SYNTAX      BITS {
                    atmInterface(0),
                    hdlcInterface(1),
                    ethernetInterface(2),
                    atm1483Interface(3),
                    atmVirtualPath(4),
                    ipInterface(5),
                    ipv6Interface(6),
                    vlanSubInterface(7),
                    frameRelaySubInterface(8),
                    cbfInterface(9),
                    serverPortInterface(10),
                    l2tpFromTunnelQueue(11),
                    ipTunnelFromTunnelQueue(12),
                    mplsMinorInterface(13),
                    bridgeInterface(14),
                    l2tpSessionInterface(15),
                    stackedVlan(16),
                    lagInterface(17) }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosObjects                           OBJECT IDENTIFIER ::= { juniQosMIB 1 }
juniQosCapability                        OBJECT IDENTIFIER ::= { juniQosObjects 1 }
juniQos                                  OBJECT IDENTIFIER ::= { juniQosObjects 2 }
juniQosTrafficClassList                  OBJECT IDENTIFIER ::= { juniQosObjects 3 }
juniQosTrafficClassGroupList             OBJECT IDENTIFIER ::= { juniQosObjects 4 }
juniQosTrafficClassGroupEntryList        OBJECT IDENTIFIER ::= { juniQosObjects 5 }
juniQosSchedulerProfileList              OBJECT IDENTIFIER ::= { juniQosObjects 6 }
juniQosQueueProfileList                  OBJECT IDENTIFIER ::= { juniQosObjects 7 }
juniQosProfile                           OBJECT IDENTIFIER ::= { juniQosObjects 8 }
juniQosProfileElement                    OBJECT IDENTIFIER ::= { juniQosObjects 9 }
juniQosIfAttach                          OBJECT IDENTIFIER ::= { juniQosObjects 10 }
juniQosQosPortTypeProfile                OBJECT IDENTIFIER ::= { juniQosObjects 11 }
juniQosQueueStatistics                   OBJECT IDENTIFIER ::= { juniQosObjects 12 }
juniQosDropProfileList                   OBJECT IDENTIFIER ::= { juniQosObjects 13 }
juniQosAtmVpUidSupport                   OBJECT IDENTIFIER ::= { juniQosObjects 14 }
juniQosStatisticsProfileList             OBJECT IDENTIFIER ::= { juniQosObjects 15 }
juniQosQosModePortList                   OBJECT IDENTIFIER ::= { juniQosObjects 16 }
juniQosQosShapingModeList                OBJECT IDENTIFIER ::= { juniQosObjects 17 }
juniQosSVlanUidSupport                   OBJECT IDENTIFIER ::= { juniQosObjects 18 }
juniQosSVlanIdSupport                    OBJECT IDENTIFIER ::= { juniQosObjects 19 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Capability Attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosMaxTrafficClass OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the maximum number of traffic classes supported."
    ::= { juniQosCapability 1 }

juniQosMaxQueueLength OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the maximum supported queue length in bytes."
    ::= { juniQosCapability 2 }

juniQosMinSchedulerBurst OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the minimum supported scheduler burst size in
        bytes."
    ::= { juniQosCapability 3 }

juniQosMaxSchedulerBurst OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the maximum supported scheduler burst size in
        bytes."
    ::= { juniQosCapability 4 }

juniQosMaxQosProfileRules OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the maximum number of rules per qos-profile
        supported."
    ::= { juniQosCapability 5 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Scalar Attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosTrafficClassCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured traffic classes."
    ::= { juniQos 1 }

juniQosQueueProfileCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured queue profiles."
    ::= { juniQos 2 }

juniQosSchedulerProfileCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured scheduler profiles."
    ::= { juniQos 3 }

juniQosProfileCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured QoS profiles."
    ::= { juniQos 4 }

juniQosInterfaceCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured interface QoS
        attachments."
    ::= { juniQos 5 }

juniQosQosPortTypeProfileCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured default port profiles."
    ::= { juniQos 6 }

juniQosDropProfileCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured drop profiles."
    ::= { juniQos 7 }

juniQosStatisticsProfileCount OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the number of configured statistics profiles."
    ::= { juniQos 8 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Traffic Class List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosTrafficClassNextIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar object returns the index of the next available row in the
        juniQosTrafficClassTable."
    ::= { juniQosTrafficClassList 1 }

juniQosTrafficClassTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosTrafficClassEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of Traffic Class definitions."
    ::= { juniQosTrafficClassList 2 }

juniQosTrafficClassEntry OBJECT-TYPE
    SYNTAX      JuniQosTrafficClassEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a traffic class element."
    INDEX     { juniQosTrafficClassIndex }
    ::= { juniQosTrafficClassTable 1 }

JuniQosTrafficClassEntry ::= SEQUENCE {
    juniQosTrafficClassIndex                     Unsigned32,
    juniQosTrafficClassRowStatus                 RowStatus,
    juniQosTrafficClassName                      DisplayString,
    juniQosTrafficClassWeight                    Unsigned32,
    juniQosTrafficClassStrictPriority            TruthValue,
    juniQosTrafficClassUpdatePending             TruthValue,
    juniQosTrafficClassUpdateNow                 TruthValue,
    juniQosTrafficClassIsReferencedByGroup       TruthValue,
    juniQosTrafficClassIsReferencedByQosProfile  TruthValue }

juniQosTrafficClassIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number of the traffic class entry which is defined by this row."
    ::= { juniQosTrafficClassEntry 1 }

juniQosTrafficClassRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosTrafficClassRowStatus
             juniQosTrafficClassName "
    ::= { juniQosTrafficClassEntry 2 }

juniQosTrafficClassName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the name of the traffic class defined by this row."
    ::= { juniQosTrafficClassEntry 3 }

juniQosTrafficClassWeight OBJECT-TYPE
    SYNTAX      Unsigned32 (1..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The relative weight for queues in this traffic class."
    DEFVAL    { 8 }
    ::= { juniQosTrafficClassEntry 4 }

juniQosTrafficClassStrictPriority OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The traffic to be dequeued before all other classes."
    DEFVAL    { false }
    ::= { juniQosTrafficClassEntry 5 }

juniQosTrafficClassUpdatePending OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if modifications have been made to the traffic class object which
        have not been committed to the line cards."
    ::= { juniQosTrafficClassEntry 6  }

juniQosTrafficClassUpdateNow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When set to true, modifications made to the traffic class object will
        be committed to the line cards."
    DEFVAL    { false }
    ::= { juniQosTrafficClassEntry 7 }

juniQosTrafficClassIsReferencedByGroup OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, the traffic class is referenced by a traffic class group."
    ::= { juniQosTrafficClassEntry 8 }

juniQosTrafficClassIsReferencedByQosProfile OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, the traffic class is referenced by a QoS profile."
    ::= { juniQosTrafficClassEntry 9 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Traffic Class Group List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosTrafficClassGroupNextIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar object returns the index of the next available row in the
        juniQosTrafficClassGroupTable."
    ::= { juniQosTrafficClassGroupList 1 }

juniQosTrafficClassGroupTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosTrafficClassGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of Traffic Class group
        definitions."
    ::= { juniQosTrafficClassGroupList 2 }

juniQosTrafficClassGroupEntry OBJECT-TYPE
    SYNTAX      JuniQosTrafficClassGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a traffic class group
        element."
    INDEX     { juniQosTrafficClassGroupIndex }
    ::= { juniQosTrafficClassGroupTable 1 }

JuniQosTrafficClassGroupEntry ::= SEQUENCE {
    juniQosTrafficClassGroupIndex                    Unsigned32,
    juniQosTrafficClassGroupRowStatus                RowStatus,
    juniQosTrafficClassGroupName                     DisplayString,
    juniQosTrafficClassGroupUpdatePending            TruthValue,
    juniQosTrafficClassGroupUpdateNow                TruthValue,
    juniQosTrafficClassGroupIsReferencedByQosProfile TruthValue,
    juniQosTrafficClassGroupSlotNumber               Integer32,
    juniQosTrafficClassGroupExtendedGroup            TruthValue }

juniQosTrafficClassGroupIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number of the traffic class entry which is defined by this row."
    ::= { juniQosTrafficClassGroupEntry 1 }

juniQosTrafficClassGroupRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosTrafficClassGroupRowStatus
             juniQosTrafficClassGroupName "
    ::= { juniQosTrafficClassGroupEntry 2 }

juniQosTrafficClassGroupName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the name of the traffic class group defined by this row."
    ::= { juniQosTrafficClassGroupEntry 3 }

juniQosTrafficClassGroupUpdatePending OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if modifications have been made to the traffic class group object
        which have not been committed to the line cards."
    ::= { juniQosTrafficClassGroupEntry 4  }

juniQosTrafficClassGroupUpdateNow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When set to true, modifications made to the traffic class group object
        will be committed to the line cards."
    DEFVAL    { false }
    ::= { juniQosTrafficClassGroupEntry 5 }

juniQosTrafficClassGroupIsReferencedByQosProfile OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, the traffic class group is referenced by a QoS profile."
    ::= { juniQosTrafficClassGroupEntry 6 }

juniQosTrafficClassGroupSlotNumber OBJECT-TYPE
    SYNTAX      Integer32 (-1..2147483647)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The number of the slot on which this traffic class group is applied.
        Traffic class groups may be global or local.  Global groups indicate
        that the traffic class group is to be applied to each line card in the
        chassis.  The value of this object is -1 for global traffic class
        groups.  Local traffic class groups override global traffic class groups
        and are applied to the slot indicated by the value of this object."
    DEFVAL    { -1 }
    ::= { juniQosTrafficClassGroupEntry 7 }

juniQosTrafficClassGroupExtendedGroup OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When true, the traffic class group is an extended group.  False
        indicates the traffic class group is an auto-strict-priority group."
    DEFVAL    { false }
    ::= { juniQosTrafficClassGroupEntry 8 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Traffic Class Group Entry List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosTrafficClassGroupEntryTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosTrafficClassGroupEntryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table identifies which traffic classes are in each traffic class
        group."
    ::= { juniQosTrafficClassGroupEntryList 1 }

juniQosTrafficClassGroupEntryEntry OBJECT-TYPE
    SYNTAX      JuniQosTrafficClassGroupEntryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry ties a traffic class table entry to a traffic class group."
    INDEX     { juniQosTrafficClassGroupIndex,
                juniQosTrafficClassIndex }
    ::= { juniQosTrafficClassGroupEntryTable 1 }

JuniQosTrafficClassGroupEntryEntry ::= SEQUENCE {
    juniQosTrafficClassGroupEntryRowStatus   RowStatus }

juniQosTrafficClassGroupEntryRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry object MUST be
        explicitly configured:
             juniQosTrafficClassGroupEntryRowStatus "
    ::= { juniQosTrafficClassGroupEntryEntry 1 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Queue Profile List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosQueueProfileNextIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar object returns the index of the next available row in the
        juniQosQueueProfileTable."
    ::= { juniQosQueueProfileList 1 }

juniQosQueueProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosQueueProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of queue profile definitions."
    ::= { juniQosQueueProfileList 2 }

juniQosQueueProfileEntry OBJECT-TYPE
    SYNTAX      JuniQosQueueProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a queue profile element."
    INDEX     { juniQosQueueProfileIndex }
    ::= { juniQosQueueProfileTable 1 }

JuniQosQueueProfileEntry ::= SEQUENCE {
    juniQosQueueProfileIndex                     Unsigned32,
    juniQosQueueProfileRowStatus                 RowStatus,
    juniQosQueueProfileName                      DisplayString,
    juniQosQueueProfileCommittedMinLength        Unsigned32,
    juniQosQueueProfileCommittedMaxLength        Unsigned32,
    juniQosQueueProfileConformedMinLength        Unsigned32,
    juniQosQueueProfileConformedMaxLength        Unsigned32,
    juniQosQueueProfileExceededMinLength         Unsigned32,
    juniQosQueueProfileExceededMaxLength         Unsigned32,
    juniQosQueueProfileConformedFraction         Unsigned32,
    juniQosQueueProfileExceededFraction          Unsigned32,
    juniQosQueueProfileCommittedDropThreshold    Unsigned32,
    juniQosQueueProfileCommittedDropRate         Unsigned32,
    juniQosQueueProfileConformedDropThreshold    Unsigned32,
    juniQosQueueProfileConformedDropRate         Unsigned32,
    juniQosQueueProfileExceededDropThreshold     Unsigned32,
    juniQosQueueProfileExceededDropRate          Unsigned32,
    juniQosQueueProfileBufferWeight              Unsigned32,
    juniQosQueueProfileUpdatePending             TruthValue,
    juniQosQueueProfileUpdateNow                 TruthValue,
    juniQosQueueProfileIsReferencedByQosProfile  TruthValue }

juniQosQueueProfileIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number of the queue profile entry which is defined by this row."
    ::= { juniQosQueueProfileEntry 1 }

juniQosQueueProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosQueueProfileRowStatus
             juniQosQueueProfileName "
    ::= { juniQosQueueProfileEntry 2 }

juniQosQueueProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the name of the queue profile defined by this row."
    ::= { juniQosQueueProfileEntry 3 }

juniQosQueueProfileCommittedMinLength OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the minimum queue length in bytes for committed traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 4 }

juniQosQueueProfileCommittedMaxLength OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum queue length in bytes for committed traffic."
    DEFVAL    { 1073741824 }
    ::= { juniQosQueueProfileEntry 5 }

juniQosQueueProfileConformedMinLength OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the minimum queue length in bytes for conformed traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 6 }

juniQosQueueProfileConformedMaxLength OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum queue length in bytes for conformed traffic."
    DEFVAL    { 1073741824 }
    ::= { juniQosQueueProfileEntry 7 }

juniQosQueueProfileExceededMinLength OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the minimum queue length in bytes for exceeded traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 8 }

juniQosQueueProfileExceededMaxLength OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum queue length in bytes for exceeded traffic."
    DEFVAL    { 1073741824 }
    ::= { juniQosQueueProfileEntry 9 }

juniQosQueueProfileConformedFraction OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum percentage of queue occupied by conformed
        traffic."
    DEFVAL    { 50 }
    ::= { juniQosQueueProfileEntry 10 }

juniQosQueueProfileExceededFraction OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum percentage of queue occupied by exceeded
        traffic."
    DEFVAL    { 25 }
    ::= { juniQosQueueProfileEntry 11 }

juniQosQueueProfileCommittedDropThreshold OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the drop threshold (percent of queue) for committed traffic."
    DEFVAL    { 100 }
    ::= { juniQosQueueProfileEntry 12 }

juniQosQueueProfileCommittedDropRate OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the drop rate (percent of traffic) for committed traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 13 }

juniQosQueueProfileConformedDropThreshold OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the drop threshold (percent of queue) for comformed traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 14 }

juniQosQueueProfileConformedDropRate OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the drop rate (percent of traffic) for comformed traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 15 }

juniQosQueueProfileExceededDropThreshold OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the drop threshold (percent of queue) for exceeded traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 16 }

juniQosQueueProfileExceededDropRate OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the drop rate (percent of traffic) for exceeded traffic."
    DEFVAL    { 0 }
    ::= { juniQosQueueProfileEntry 17 }

juniQosQueueProfileBufferWeight OBJECT-TYPE
    SYNTAX      Unsigned32 (1..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The relative weight for queues in this traffic class."
    DEFVAL    { 8 }
    ::= { juniQosQueueProfileEntry 18 }

juniQosQueueProfileUpdatePending OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if modifications have been made to the queue profile object which
        have not been committed to the line cards."
    ::= { juniQosQueueProfileEntry 19  }

juniQosQueueProfileUpdateNow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When set to true, modifications made to the queue profile object will
        be committed to the line cards."
    DEFVAL    { false }
    ::= { juniQosQueueProfileEntry 20 }

juniQosQueueProfileIsReferencedByQosProfile OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, the queue profile is referenced by a QoS profile."
    ::= { juniQosQueueProfileEntry 21 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Scheduler Profile List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosSchedulerProfileNextIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar object returns the index of the next available row in the
        juniQosSchedulerProfileTable."
    ::= { juniQosSchedulerProfileList 1 }

juniQosSchedulerProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosSchedulerProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of Scheduler Profile
        definitions."
    ::= { juniQosSchedulerProfileList 2 }

juniQosSchedulerProfileEntry OBJECT-TYPE
    SYNTAX      JuniQosSchedulerProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a scheduler profile
        element."
    INDEX     { juniQosSchedulerProfileIndex }
    ::= { juniQosSchedulerProfileTable 1 }

JuniQosSchedulerProfileEntry ::= SEQUENCE {
    juniQosSchedulerProfileIndex                     Unsigned32,
    juniQosSchedulerProfileRowStatus                 RowStatus,
    juniQosSchedulerProfileName                      DisplayString,
    juniQosSchedulerProfileShapingRate               Unsigned32,
    juniQosSchedulerProfileBurst                     Unsigned32,
    juniQosSchedulerProfileWeight                    Unsigned32,
    juniQosSchedulerProfileStrictPriority            TruthValue,
    juniQosSchedulerProfileUpdatePending             TruthValue,
    juniQosSchedulerProfileUpdateNow                 TruthValue,
    juniQosSchedulerProfileIsReferencedByQosProfile  TruthValue,
    juniQosSchedulerProfileAssuredRate               Unsigned32,
    juniQosSchedulerProfileSharedShapingRate         Unsigned32,
    juniQosSchedulerProfileSharedShapingBurstSize    Unsigned32,
    juniQosSchedulerProfileSharedShapingType         INTEGER,
    juniQosSchedulerProfileSharedShapingExplicitConstituents TruthValue,
    juniQosSchedulerProfileSharedShapingPriority     Integer32,
    juniQosSchedulerProfileSharedShapingWeight       Integer32 }

juniQosSchedulerProfileIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number of the scheduler profile entry which is defined by this
        row."
    ::= { juniQosSchedulerProfileEntry 1 }

juniQosSchedulerProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosSchedulerProfileRowStatus
             juniQosSchedulerProfileName "
    ::= { juniQosSchedulerProfileEntry 2 }

juniQosSchedulerProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the name of the scheduler profile defined by this row."
    ::= { juniQosSchedulerProfileEntry 3 }

juniQosSchedulerProfileShapingRate OBJECT-TYPE
    SYNTAX      Unsigned32 (0..1000000000)
    UNITS       "bps"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the shaping rate in bits per second (bps).
         Values between 1 and 63999 are not supported."
    DEFVAL    { 0 }
    ::= { juniQosSchedulerProfileEntry 4 }

juniQosSchedulerProfileBurst OBJECT-TYPE
    SYNTAX      Unsigned32 (0..522240)
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the catch-up burst size in bytes.
         Burst value of 0 indicates the largest burst size the
         system will allow without losing accuracy."
    DEFVAL    { 0 }
    ::= { juniQosSchedulerProfileEntry 5 }

juniQosSchedulerProfileWeight OBJECT-TYPE
    SYNTAX      Unsigned32 (0..4080)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The relative weight of the scheduler.  When an assured rate is
        specified, this object is ignored."
    DEFVAL    { 8 }
    ::= { juniQosSchedulerProfileEntry 6 }

juniQosSchedulerProfileStrictPriority OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the traffic to be dequeued before all other scheduler nodes."
    DEFVAL    { false }
    ::= { juniQosSchedulerProfileEntry 7 }

juniQosSchedulerProfileUpdatePending OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if modifications have been made to the scheduler profile object
        which have not been committed to the line cards."
    ::= { juniQosSchedulerProfileEntry 8  }

juniQosSchedulerProfileUpdateNow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When set to true, modifications made to the scheduler profile object
        will be committed to the line cards."
    DEFVAL    { false }
    ::= { juniQosSchedulerProfileEntry 9 }

juniQosSchedulerProfileIsReferencedByQosProfile OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, the scheduler profile is referenced by a QoS profile."
    ::= { juniQosSchedulerProfileEntry 10 }

juniQosSchedulerProfileAssuredRate OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 25000..1000000000 | 4294967295)
    UNITS       "bps"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the assured rate in bits per second (bps).
        When this object has a non-default value, the scheduler 
        weight (juniQosSchedulerProfileWeight) is ignored.

        A value of '4294967295' configures Hierarchical Assured Rate."
    DEFVAL    { 0 }
    ::= { juniQosSchedulerProfileEntry 11 }

juniQosSchedulerProfileSharedShapingRate OBJECT-TYPE
    SYNTAX      Unsigned32 (0..1000000000)
    UNITS       "bps"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the shared shaping rate in bits per second (bps).
        The range of 1 to 63999 is not supported."
    DEFVAL    { 0 }
    ::= { juniQosSchedulerProfileEntry 12 }

juniQosSchedulerProfileSharedShapingBurstSize OBJECT-TYPE
    SYNTAX      Unsigned32 (0..522240)
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the catch-up burst size for a shared shaping,
        in bytes.

        A value of zero indicates that the system should choose
        an appropriate default value."
    DEFVAL    { 0 }
    ::= { juniQosSchedulerProfileEntry 13 }

juniQosSchedulerProfileSharedShapingType OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    simple(1),
                    compound(2),
                    auto(3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the type
        of shared shaping that is to be performed when
        shared shaping is enabled.  Shared shaper types 
        are defined as follows:

        'simple' indicates that Simple Shared Shaping is 
        performed regardless of the line cards capabilities.

        'compound' indicates that Compound Shared Shaping is 
        to be performed.  When compound is specified for a line 
        card that does not support Compound Shared Shaping, a 
        warning message is logged, and Simple Shared Shaping 
        is configured instead.

        'auto' indicates that selection of the shared shaper 
        should be automatic such that compound shared shaping 
        is performed on line cards which support it and simple 
        shared shaping is performed on line cards that do not
        support it."
    DEFVAL    { auto }
    ::= { juniQosSchedulerProfileEntry 14 }

juniQosSchedulerProfileSharedShapingExplicitConstituents OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This option allows automatic shared shaper constituent 
        selecting and bandwidth allocation to be overridden.  
        By default, constituents are configured implicitly."
    DEFVAL    { false }
    ::= { juniQosSchedulerProfileEntry 15 }

juniQosSchedulerProfileSharedShapingPriority OBJECT-TYPE
    SYNTAX      Integer32 (-1..8)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The priority of a strict shared shaper constituent.

        When the value of juniQosSchedulerProfileSharedShaper-
        ConstituentType is 'strict' the value of this object
        determines the order in which the strict constituent
        can claim bandwidth.  Priority values range from 1 to 8, 
        with priority 1 getting first claim amongst strict 
        constituents on available shared bandwidth, and 
        priority 8 getting final claim amongst strict 
        constituents on available bandwidth.  When two or 
        more strict constituents have the same priority 
        value, the rules used for implicit bandwidth 
        allocation are applied to determine their order.

        A value of zero indicates 'not a constituent' 
        of a shared shaper.

        A value of -1 indicates 'is a constituent' of a shared 
        shaper, but the system is free to choose whether the 
        constituent is 'strict-priority' of 'weighted'

        This object takes precedence over the
        juniQosSchedulerProfileSharedShapingWeight object.
        When set to a value from 1 to 8 the system sets
        the value of juniQosSchedulerProfileSharedShaping-
        Weight to zero."
    DEFVAL    { 0 }
    ::= { juniQosSchedulerProfileEntry 16 }

juniQosSchedulerProfileSharedShapingWeight OBJECT-TYPE
    SYNTAX      Integer32 (-1..31)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The weight of a weighted shared shaper constituent.

        When the value of juniQosSchedulerProfileSharedShaper-
        ConstituentType is 'weighted' the value of this object
        determines the proportion of the weighted constituent's
        bandwidth

        Non-zero values specify the weight of a weighted 
        shared shaping constituent.  A value of zero 
        indicates 'not a constituent' of a shared shaper.

        A value of -1 indicates 'is a constituent' of a 
        shared shaper, but the system is free to choose 
        whether the constituent is 'strict-priority' of 
        'weighted'

        The juniQosSchedulerProfileSharedShapingPriority
        has precedence over the this object."
    DEFVAL    { 0 }
    ::= { juniQosSchedulerProfileEntry 17 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Profile Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosProfileNextIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar object returns the index of the next available row in the
        juniQosProfileTable."
    ::= { juniQosProfile 1 }

juniQosProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of QoS Profile definitions."
    ::= { juniQosProfile 2 }

juniQosProfileEntry OBJECT-TYPE
    SYNTAX      JuniQosProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a QoS profile element."
    INDEX     { juniQosProfileIndex }
    ::= { juniQosProfileTable 1 }

JuniQosProfileEntry ::= SEQUENCE {
    juniQosProfileIndex                                  Unsigned32,
    juniQosProfileRowStatus                              RowStatus,
    juniQosProfileName                                   DisplayString,
    juniQosProfileUpdatePending                          TruthValue,
    juniQosProfileUpdateNow                              TruthValue,
    juniQosProfileIsReferencedByInterfaceQosAttachment   TruthValue,
    juniQosProfileIsReferencedByQosPortTypeProfile       TruthValue }

juniQosProfileIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number identifies this QoS profile."
    ::= { juniQosProfileEntry 1 }

juniQosProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create a QoS profile in this table, the following entry objects MUST
        be explicitly configured:
             juniQosProfileRowStatus
             juniQosProfileName "
    ::= { juniQosProfileEntry 2 }

juniQosProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the name of the QoS profile defined by this row."
    ::= { juniQosProfileEntry 3 }

juniQosProfileUpdatePending OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if modifications have been made to the QoS profile object which
        have not been committed to the line cards."
    ::= { juniQosProfileEntry 4  }

juniQosProfileUpdateNow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When set to true, modifications made to the QoS profile object will be
        committed to the line cards."
    DEFVAL    { false }
    ::= { juniQosProfileEntry 5 }

juniQosProfileIsReferencedByInterfaceQosAttachment OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, the QoS profile is referenced by an interface QoS
        attachment."
    ::= { juniQosProfileEntry 6 }

juniQosProfileIsReferencedByQosPortTypeProfile OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, the QoS profile is referenced by a QoS port type profile."
    ::= { juniQosProfileEntry 7 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Profile Element Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosProfileElementTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosProfileElementEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of QoS profile definitions."
    ::= { juniQosProfileElement 1 }

juniQosProfileElementEntry OBJECT-TYPE
    SYNTAX      JuniQosProfileElementEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a QoS profile element."
    INDEX     { juniQosProfileIndex,
                juniQosInterfaceType,
                juniQosProfileEntryType,
                juniQosTrafficClassIndex,
                juniQosTrafficClassGroupIndex }
    ::= { juniQosProfileElementTable 1 }

JuniQosProfileElementEntry ::= SEQUENCE {
    juniQosProfileElementEntryRowStatus          RowStatus,
    juniQosProfileElementEntryQueueProfile       Unsigned32,
    juniQosProfileElementEntrySchedulerProfile   Unsigned32,
    juniQosInterfaceType                         INTEGER,
    juniQosProfileEntryType                      INTEGER,
    juniQosProfileElementEntryDropProfile        Unsigned32,
    juniQosProfileElementEntryStatisticsProfile  Unsigned32 }

juniQosProfileElementEntryRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry object MUST be
        explicitly configured:
             juniQosProfileRowStatus "
    ::= { juniQosProfileElementEntry 1 }

juniQosProfileElementEntryQueueProfile OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the queue profile assigned to the QoS entry."
    DEFVAL    { 1 }
    ::= { juniQosProfileElementEntry 2 }

juniQosProfileElementEntrySchedulerProfile OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the scheduler profile assigned to the QoS entry."
    DEFVAL    { 1 }
    ::= { juniQosProfileElementEntry 3 }

juniQosInterfaceType OBJECT-TYPE
    SYNTAX      INTEGER {
                    ip(0),
                    ethernet(6),
                    atm(9),
                    atmVc(11),
                    serial(13),
                    frVc(16),
                    l2tpSession(21),
                    serverPort(31),
                    vlan(35),
                    cbf(36),
                    ipv6(50),
                    l2tpTunnel(150),
                    ipTunnel(151),
                    atmVp(163),
                    svlan(174) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The QoS interface type ID, part of the index for
        juniQosProfileElementTable.

        Please note that if the juniQpsProfileEntryType is trafficClassGroup,
        then only ethernet, atm, serial, and serverPort are valid interface
        types."
    ::= { juniQosProfileElementEntry 4 }

juniQosProfileEntryType OBJECT-TYPE
    SYNTAX      INTEGER {
                    trafficClass(1),
                    schedulerProfile(2),
                    trafficClassGroup(3),
                    shadowNode(4) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The QoS profile type, part of the index for
        juniQosProfileElementTable."
    ::= { juniQosProfileElementEntry 5 }

juniQosProfileElementEntryDropProfile OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the drop profile assigned to the QoS entry."
    DEFVAL    { 1 }
    ::= { juniQosProfileElementEntry 6 }

juniQosProfileElementEntryStatisticsProfile OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the statistics profile assigned to the QoS entry."
    DEFVAL    { 1 }
    ::= { juniQosProfileElementEntry 7 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Interface Attached Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosIfAttachTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosIfAttachEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries which represent attachment of QoS to
        interfaces."
    ::= { juniQosIfAttach 1 }

juniQosIfAttachEntry OBJECT-TYPE
    SYNTAX      JuniQosIfAttachEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains the attachment of QoS to an interface."
    INDEX     { juniQosIfAttachIndex }
    ::= { juniQosIfAttachTable 1 }

JuniQosIfAttachEntry ::= SEQUENCE {
    juniQosIfAttachIndex             Unsigned32,
    juniQosIfAttachRowStatus         RowStatus,
    juniQosIfAttachQosProfileIndex   Unsigned32 }

juniQosIfAttachIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface number representing the interface to which QoS has been
        attached."
    ::= { juniQosIfAttachEntry 1 }

juniQosIfAttachRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        juniQosIfAttachQosProfileIndex must be specified when creating the row.

        *** LIMITED ACCESS LIST CONFIGURATION LEVEL ***
        RowStatus createAndGo/destroy operations have the following
        special-purpose semantics:
            createAndGo     Create an entry having the specified configuration
                            and append it to the target list.
            destroy         Destroy the specified list and all of its
                            constituent elements. "
    ::= { juniQosIfAttachEntry 2 }

juniQosIfAttachQosProfileIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The QoS profile attached to this interface."
    ::= { juniQosIfAttachEntry 3 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Port Type Profile Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosQosPortTypeProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosQosPortTypeProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries which represent attachment of QoS to
        interface types with which they are associated."
    ::= { juniQosQosPortTypeProfile 1 }

juniQosQosPortTypeProfileEntry OBJECT-TYPE
    SYNTAX      JuniQosQosPortTypeProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains the attachment of QoS to an interface."
    INDEX     { juniQosQosPortTypeProfileIndex }
    ::= { juniQosQosPortTypeProfileTable 1 }

JuniQosQosPortTypeProfileEntry ::= SEQUENCE {
    juniQosQosPortTypeProfileIndex           INTEGER,
    juniQosQosPortTypeProfileRowStatus       RowStatus,
    juniQosQosPortTypeProfileQosProfileIndex Unsigned32 }

juniQosQosPortTypeProfileIndex OBJECT-TYPE
    SYNTAX      INTEGER {
                    ethernet(6),
                    atm(9),
                    serial(13),
                    serverPort(31),
                    lag(54) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface number representing the types of interface to which QoS
        has been attached."
    ::= { juniQosQosPortTypeProfileEntry 1 }

juniQosQosPortTypeProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        juniQosQosPortTypeProfileQosProfileIndex must be specified when creating
        the row.

        *** LIMITED ACCESS LIST CONFIGURATION LEVEL ***
        RowStatus createAndGo/destroy operations have the following
        special-purpose semantics:
            createAndGo     Create an entry having the specified configuration
                            and append it to the target list.

            destroy         Destroy the specified list and all of its
                            constituent elements. "
     ::= { juniQosQosPortTypeProfileEntry 2 }

juniQosQosPortTypeProfileQosProfileIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The QoS profile assigned to this port type."
    ::= { juniQosQosPortTypeProfileEntry 3 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Queue Statistics
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosQueueStatisticsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosQueueStatisticsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry within this table contains queue statistics for an
        interface/traffic class combination."
    ::= { juniQosQueueStatistics 1 }

juniQosQueueStatisticsEntry OBJECT-TYPE
    SYNTAX      JuniQosQueueStatisticsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry defines a single queue statistics entry."
    INDEX     { ifIndex,
                juniQosTrafficClassIndex }
    ::= { juniQosQueueStatisticsTable 1 }

JuniQosQueueStatisticsEntry ::= SEQUENCE {
    juniQosOutPacketForwarded                Counter64,
    juniQosOutBytesForwarded                 Counter64,
    juniQosOutGreenPacketsSchedulerDrops     Counter64,
    juniQosOutYellowPacketsSchedulerDrops    Counter64,
    juniQosOutRedPacketsSchedulerDrops       Counter64,
    juniQosOutGreenBytesSchedulerDrops       Counter64,
    juniQosOutYellowBytesSchedulerDrops      Counter64,
    juniQosOutRedBytesSchedulerDrops         Counter64 }

juniQosOutPacketForwarded OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets queued on this interface."
    ::= { juniQosQueueStatisticsEntry 1 }

juniQosOutBytesForwarded OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of bytes queued on this interface."
    ::= { juniQosQueueStatisticsEntry 2 }

juniQosOutGreenPacketsSchedulerDrops OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of green packets dropped on this interface."
    ::= { juniQosQueueStatisticsEntry 3 }

juniQosOutYellowPacketsSchedulerDrops OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of yellow packets dropped on this interface."
    ::= { juniQosQueueStatisticsEntry 4 }

juniQosOutRedPacketsSchedulerDrops OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of red packets dropped on this interface."
    ::= { juniQosQueueStatisticsEntry 5 }

juniQosOutGreenBytesSchedulerDrops OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of green bytes dropped on this interface."
    ::= { juniQosQueueStatisticsEntry 6 }

juniQosOutYellowBytesSchedulerDrops OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of yellow bytes dropped on this interface."
    ::= { juniQosQueueStatisticsEntry 7 }

juniQosOutRedBytesSchedulerDrops OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of red bytes dropped on this interface."
    ::= { juniQosQueueStatisticsEntry 8 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS ATM VP UID support Scalar Attributes
--
-- To translate an ATM port interface and VP into an ATM VP UID, write the port
-- interface and path objects, and read the VP UID object.
--
-- To translate an ATM VP UID into an ATM port interface and path, write the
-- ATM VP UID object and read the ATM port interface and path objects.
--
-- The validity of the objects is represented by the ATM VP UID valid object.
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

juniQosAtmVpUidValid OBJECT-TYPE
    SYNTAX      INTEGER {
                    valid(0),
                    badPortInterfaceUid(1),
                    badPath(2),
                    badAtmVpUid(3) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reflects the status of the ATM VP UID translation objects."
    ::= { juniQosAtmVpUidSupport 1 }

juniQosAtmVpAtmPortInterfaceUid OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object is the ATM port interface UID which correlates to the ATM
        VP UID object."
    ::= { juniQosAtmVpUidSupport 2 }

juniQosAtmVpAtmPath OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object is the ATM VP which correlates to the ATM VP UID object."
    ::= { juniQosAtmVpUidSupport 3 }

juniQosAtmVpUid OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object is the ATM VP UID which correlates to the ATM port
        interface and path objects."
    ::= { juniQosAtmVpUidSupport 4 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Drop Profile List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosDropProfileNextIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar object returns the index of the next available row in the
        juniQosDropProfileTable."
    ::= { juniQosDropProfileList 1 }

juniQosDropProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosDropProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of drop profile definitions."
    ::= { juniQosDropProfileList 2 }

juniQosDropProfileEntry OBJECT-TYPE
    SYNTAX      JuniQosDropProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a drop profile element."
    INDEX     { juniQosDropProfileIndex }
    ::= { juniQosDropProfileTable 1 }

JuniQosDropProfileEntry ::= SEQUENCE {
    juniQosDropProfileIndex                                 Unsigned32,
    juniQosDropProfileRowStatus                             RowStatus,
    juniQosDropProfileName                                  DisplayString,
    juniQosDropProfileAverageLengthExponent                 Unsigned32,
    juniQosDropProfileCommittedThresholdUnits               INTEGER,
    juniQosDropProfileCommittedThresholdMinThreshold        Unsigned32,
    juniQosDropProfileCommittedThresholdMaxThreshold        Unsigned32,
    juniQosDropProfileCommittedThresholdMaxDropProbability  Unsigned32,
    juniQosDropProfileConformedThresholdUnits               INTEGER,
    juniQosDropProfileConformedThresholdMinThreshold        Unsigned32,
    juniQosDropProfileConformedThresholdMaxThreshold        Unsigned32,
    juniQosDropProfileConformedThresholdMaxDropProbability  Unsigned32,
    juniQosDropProfileExceededThresholdUnits                INTEGER,
    juniQosDropProfileExceededThresholdMinThreshold         Unsigned32,
    juniQosDropProfileExceededThresholdMaxThreshold         Unsigned32,
    juniQosDropProfileExceededThresholdMaxDropProbability   Unsigned32,
    juniQosDropProfileUpdatePending                         TruthValue,
    juniQosDropProfileUpdateNow                             TruthValue,
    juniQosDropProfileIsReferencedByQosProfile              TruthValue }

juniQosDropProfileIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number of the drop profile entry which is defined by this row."
    ::= { juniQosDropProfileEntry 1 }

juniQosDropProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosDropProfileRowStatus
             juniQosDropProfileName "
    ::= { juniQosDropProfileEntry 2 }

juniQosDropProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the name of the drop profile defined by this row."
    ::= { juniQosDropProfileEntry 3 }

juniQosDropProfileAverageLengthExponent OBJECT-TYPE
    SYNTAX      Unsigned32 (0..20)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the exponent used to weight the average queue length over
        time, controlling RED responsiveness.  A non-default value enables
        the average queue length calculation."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 4 }

juniQosDropProfileCommittedThresholdUnits OBJECT-TYPE
    SYNTAX      INTEGER {
                    bytes(1),
                    percent(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the units for the committed minimum and maximum thresholds."
    DEFVAL    { bytes }
    ::= { juniQosDropProfileEntry 5 }

juniQosDropProfileCommittedThresholdMinThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the minimum drop threshold for committed traffic.  The units
        are defined by juniQosDropProfileCommittedThresholdUnits.

        If units are bytes, the value must be in the range of 0..1073741824.
        If units are percent, the value must be in the range of 1..100."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 6 }

juniQosDropProfileCommittedThresholdMaxThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum drop threshold for committed traffic.  The units
        are defined by juniQosDropProfileCommittedThresholdUnits.

        If units are bytes, the value must be in the range of 0..1073741824.
        If units are percent, the value must be in the range of 1..100.
        Setting the minimum and maximum thresholds to 0 disables the threshold."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 7 }

juniQosDropProfileCommittedThresholdMaxDropProbability OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum drop probability for committed traffic."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 8 }

juniQosDropProfileConformedThresholdUnits OBJECT-TYPE
    SYNTAX      INTEGER {
                    bytes(1),
                    percent(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the units for the conformed minimum and maximum thresholds."
    DEFVAL    { bytes }
    ::= { juniQosDropProfileEntry 9 }

juniQosDropProfileConformedThresholdMinThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the minimum drop threshold for conformed traffic.  The units
        are defined by juniQosDropProfileConformedThresholdUnits.

        If units are bytes, the value must be in the range of 0..1073741824.
        If units are percent, the value must be in the range of 1..100."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 10 }

juniQosDropProfileConformedThresholdMaxThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum drop threshold for conformed traffic.  The units
        are defined by juniQosDropProfileConformedThresholdUnits.

        If units are bytes, the value must be in the range of 0..1073741824.
        If units are percent, the value must be in the range of 1..100.
        Setting the minimum and maximum thresholds to 0 disables the threshold."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 11 }

juniQosDropProfileConformedThresholdMaxDropProbability OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum drop probability for conformed traffic."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 12 }

juniQosDropProfileExceededThresholdUnits OBJECT-TYPE
    SYNTAX      INTEGER {
                    bytes(1),
                    percent(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the units for the exceeded minimum and maximum thresholds."
    DEFVAL    { bytes }
    ::= { juniQosDropProfileEntry 13 }

juniQosDropProfileExceededThresholdMinThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the minimum drop threshold for exceeded traffic.  The units
        are defined by juniQosDropProfileExceededThresholdUnits.

        If units are bytes, the value must be in the range of 0..1073741824.
        If units are percent, the value must be in the range of 1..100."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 14 }

juniQosDropProfileExceededThresholdMaxThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum drop threshold for exceeded traffic.  The units
        are defined by juniQosDropProfileExceededThresholdUnits.

        If units are bytes, the value must be in the range of 0..1073741824.
        If units are percent, the value must be in the range of 1..100.
        Setting the minimum and maximum thresholds to 0 disables the threshold."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 15 }

juniQosDropProfileExceededThresholdMaxDropProbability OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum drop probability for exceeded traffic."
    DEFVAL    { 0 }
    ::= { juniQosDropProfileEntry 16 }

juniQosDropProfileUpdatePending OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if modifications have been made to the drop profile object which
        have not been committed to the line cards."
    ::= { juniQosDropProfileEntry 17 }

juniQosDropProfileUpdateNow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When set to true, modifications made to the drop profile object will be
        committed to the line cards."
    DEFVAL    { false }
    ::= { juniQosDropProfileEntry 18 }

juniQosDropProfileIsReferencedByQosProfile OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if the drop profile is referenced by QoS profile(s)."
    ::= { juniQosDropProfileEntry 19 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Statistics Profile List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosStatisticsProfileNextIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar object returns the index of the next available row in the
        juniQosStatsProfileTable."
    ::= { juniQosStatisticsProfileList 1 }

juniQosStatisticsProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosStatisticsProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of Statistics Profile
        definitions."
    ::= { juniQosStatisticsProfileList 2 }

juniQosStatisticsProfileEntry OBJECT-TYPE
    SYNTAX      JuniQosStatisticsProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a statstics profile
        element."
    INDEX     { juniQosStatisticsProfileIndex }
    ::= { juniQosStatisticsProfileTable 1 }

JuniQosStatisticsProfileEntry ::= SEQUENCE {
    juniQosStatisticsProfileIndex                       Unsigned32,
    juniQosStatisticsProfileName                        DisplayString,
    juniQosStatisticsProfileRowStatus                   RowStatus,
    juniQosStatisticsProfileForwardingRateThreshold     Unsigned32,
    juniQosStatisticsProfileCommittedDropThreshold      Unsigned32,
    juniQosStatisticsProfileConformedDropThreshold      Unsigned32,
    juniQosStatisticsProfileExceededDropThreshold       Unsigned32,
    juniQosStatisticsProfileRatePeriod                  Unsigned32,
    juniQosStatisticsProfileUpdatePending               TruthValue,
    juniQosStatisticsProfileUpdateNow                   TruthValue,
    juniQosStatisticsProfileIsReferencedByQosProfile    TruthValue }

juniQosStatisticsProfileIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number of the statistics profile entry which is defined by this
        row."
    ::= { juniQosStatisticsProfileEntry 1 }

juniQosStatisticsProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosStatisticsProfileRowStatus
             juniQosStatisticsProfileName "
    ::= { juniQosStatisticsProfileEntry 2 }

juniQosStatisticsProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the name of the statistics profile defined by this row."
    ::= { juniQosStatisticsProfileEntry 3 }

juniQosStatisticsProfileForwardingRateThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the forwarding rate threshold."
    DEFVAL    { 0 }
    ::= { juniQosStatisticsProfileEntry 4 }

juniQosStatisticsProfileCommittedDropThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the committed drop threshold."
    DEFVAL    { 0 }
    ::= { juniQosStatisticsProfileEntry 5 }

juniQosStatisticsProfileConformedDropThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the conformed drop threshold."
    DEFVAL    { 0 }
    ::= { juniQosStatisticsProfileEntry 6 }

juniQosStatisticsProfileExceededDropThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the exceeded drop threshold."
    DEFVAL    { 0 }
    ::= { juniQosStatisticsProfileEntry 7 }

juniQosStatisticsProfileRatePeriod OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the rate period over which forwarding and drop thresholds are
        calculated "
    DEFVAL    { 0 }
    ::= { juniQosStatisticsProfileEntry 8 }

juniQosStatisticsProfileUpdatePending OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if modifications have been made to the statistics profile object
        which have not been committed to the line cards."
    ::= { juniQosStatisticsProfileEntry 9 }

juniQosStatisticsProfileUpdateNow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When set to true, modifications made to the statistics profile object
        will be committed to the line cards."
    DEFVAL    { false }
    ::= { juniQosStatisticsProfileEntry 10 }

juniQosStatisticsProfileIsReferencedByQosProfile OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "True if the statistics profile is referenced by QoS profile(s)."
    ::= { juniQosStatisticsProfileEntry 11 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Mode Port List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosQosModePortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosQosModePortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of QoS mode port definitions."
    ::= { juniQosQosModePortList 1 }

juniQosQosModePortEntry OBJECT-TYPE
    SYNTAX      JuniQosQosModePortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a QoS mode port element."
    INDEX     { juniQosQosModePortIndex }
    ::= { juniQosQosModePortTable 1 }

JuniQosQosModePortEntry ::= SEQUENCE {
    juniQosQosModePortIndex         Unsigned32,
    juniQosQosModePortRowStatus     RowStatus,
    juniQosQosModePortFrameMode     INTEGER }

juniQosQosModePortIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ATM port interface for which this row defines QoS mode port
        settings."
    ::= { juniQosQosModePortEntry 1 }

juniQosQosModePortRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosQosModePortRowStatus
             juniQosQosModePortFrameMode "
    ::= { juniQosQosModePortEntry 2 }

juniQosQosModePortFrameMode OBJECT-TYPE
    SYNTAX      INTEGER {
                    lowCdv(0),
                    lowLatency(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the frame mode for this ATM port interface.

        lowCdv mode can not be configured unless
        juniQosQosShapingModeShapingMode for the ATM port interface is
        configured as 'cell'."
    ::= { juniQosQosModePortEntry 3 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Shaping Mode List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosQosShapingModeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosQosShapingModeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of QoS shaping mode
        definitions."
    ::= { juniQosQosShapingModeList 1 }

juniQosQosShapingModeEntry OBJECT-TYPE
    SYNTAX      JuniQosQosShapingModeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a QoS shaping mode
        element."
    INDEX     { juniQosQosShapingModeIndex }
    ::= { juniQosQosShapingModeTable 1 }

JuniQosQosShapingModeEntry ::= SEQUENCE {
    juniQosQosShapingModeIndex         Unsigned32,
    juniQosQosShapingModeRowStatus     RowStatus,
    juniQosQosShapingModeShapingMode   INTEGER }

juniQosQosShapingModeIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ATM port interface for which this row defines QoS shaping mode port
        settings."
    ::= { juniQosQosShapingModeEntry 1 }

juniQosQosShapingModeRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of conceptual rows within this table.

        All rowStatus modes are supported.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
             juniQosQosShapingModeRowStatus
             juniQosQosShapingModeShapingMode "
    ::= { juniQosQosShapingModeEntry 2 }

juniQosQosShapingModeShapingMode OBJECT-TYPE
    SYNTAX      INTEGER {
                    frame(0),
                    cell(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the QoS shaping mode for this ATM port interface.  'frame'
        indicates shaping is to be based on frames, not including cell
        encapsulation and padding.  'cell' indicates shaping is to be based on
        cells, with cell encapsulation and padding included.

        'frame' mode can not be configured unless juniQosQosModePortFrameMode
        for the ATM port interface is configured as 'lowLatency'."
    DEFVAL    { frame }
    ::= { juniQosQosShapingModeEntry 3 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Stacked Vlan Uid Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosSVlanUidTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosSVlanUidTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains an entry for each possible stacked vlan UID."
    ::= { juniQosSVlanUidSupport 1 }

juniQosSVlanUidTableEntry OBJECT-TYPE
    SYNTAX      JuniQosSVlanUidTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "Each entry is a stacked vlan UID."
    INDEX       { juniQosSVlanUidTablePortUid,
                  juniQosSVlanUidTableSVlanId }
    ::= { juniQosSVlanUidTable 1 }

JuniQosSVlanUidTableEntry ::= SEQUENCE {
    juniQosSVlanUidTablePortUid   Unsigned32,
    juniQosSVlanUidTableSVlanId   Unsigned32,
    juniQosSVlanUidTableSVlanUid  Unsigned32 }

juniQosSVlanUidTablePortUid OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The UID of the Ethernet port on which the stacked vlan 
         is defined"
     ::= { juniQosSVlanUidTableEntry 1 }

juniQosSVlanUidTableSVlanId OBJECT-TYPE
    SYNTAX      Unsigned32 (0..4095)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The stacked vlan ID"
     ::= { juniQosSVlanUidTableEntry 2 }

juniQosSVlanUidTableSVlanUid OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The stacked vlan UID"
     ::= { juniQosSVlanUidTableEntry 3 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- QoS Stacked Vlan Id Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosSVlanIdTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniQosSVlanIdTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains an entry for each possible Ethernet port/stacked vlan id."
    ::= { juniQosSVlanIdSupport 1 }

juniQosSVlanIdTableEntry OBJECT-TYPE
    SYNTAX      JuniQosSVlanIdTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "Each entry is a stacked vlan Ethernet port/stacked vlan ID."
    INDEX       { juniQosSVlanIdTableSVlanUid }
    ::= { juniQosSVlanIdTable 1 }

JuniQosSVlanIdTableEntry ::= SEQUENCE {
    juniQosSVlanIdTableSVlanUid  Unsigned32,
    juniQosSVlanIdTablePortUid   Unsigned32,
    juniQosSVlanIdTableSVlanId   Unsigned32 }

juniQosSVlanIdTableSVlanUid OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The stacked vlan UID"
     ::= { juniQosSVlanIdTableEntry 1 }

juniQosSVlanIdTablePortUid OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The UID of the Ethernet port on which the stacked vlan 
         is defined"
     ::= { juniQosSVlanIdTableEntry 2 }

juniQosSVlanIdTableSVlanId OBJECT-TYPE
    SYNTAX      Unsigned32 (0..4095)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The stacked vlan ID"
     ::= { juniQosSVlanIdTableEntry 3 }



-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniQosConformance OBJECT IDENTIFIER ::= { juniQosMIB 2 }
juniQosCompliances OBJECT IDENTIFIER ::= { juniQosConformance 1 }
juniQosGroups      OBJECT IDENTIFIER ::= { juniQosConformance 2 }

--
-- Compliance statements.
--
juniQosCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        QoS management MIB.  This statement became obsolete when drop profile
        list support was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniQosCapabilityGroup,
            juniQosScalarGroup,
            juniQosTrafficClassListGroup,
            juniQosTrafficClassGroupListGroup,
            juniQosQueueProfileListGroup,
            juniQosSchedulerProfileListGroup,
            juniQosProfileListGroup,
            juniQosProfileElementGroup,
            juniQosIfAttachGroup,
            juniQosQosPortTypeProfileGroup,
            juniQosQueueStatisticsGroup }
    ::= { juniQosCompliances 1 }                                   -- JUNOSe 4.0

juniQosCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        QoS management MIB.  This statement became obsolete when ATM VP UID,
        statistics profile list and QoS mode port support was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniQosCapabilityGroup,
            juniQosScalarGroup2,
            juniQosTrafficClassListGroup,
            juniQosTrafficClassGroupListGroup,
            juniQosQueueProfileListGroup,
            juniQosSchedulerProfileListGroup,
            juniQosProfileListGroup,
            juniQosProfileElementGroup2,
            juniQosIfAttachGroup,
            juniQosQosPortTypeProfileGroup,
            juniQosQueueStatisticsGroup,
            juniQosDropProfileListGroup }
    ::= { juniQosCompliances 2 }                                   -- JUNOSe 5.0

juniQosCompliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        QoS management MIB.  This statement became obsolete when multiple
        traffic class group support was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniQosCapabilityGroup,
            juniQosScalarGroup3,
            juniQosTrafficClassListGroup,
            juniQosTrafficClassGroupListGroup,
            juniQosQueueProfileListGroup,
            juniQosSchedulerProfileListGroup2,
            juniQosProfileListGroup,
            juniQosProfileElementGroup3,
            juniQosIfAttachGroup,
            juniQosQosPortTypeProfileGroup,
            juniQosQueueStatisticsGroup,
            juniQosDropProfileListGroup,
            juniQosAtmVpUidSupportGroup,
            juniQosStatisticsProfileListGroup,
            juniQosQosModePortGroup,
            juniQosQosShapingModeGroup }
    ::= { juniQosCompliances 3 }                                   -- JUNOSe 5.1

juniQosCompliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper QoS
        management MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniQosCapabilityGroup,
            juniQosScalarGroup3,
            juniQosTrafficClassListGroup,
            juniQosTrafficClassGroupListGroup2,
            juniQosQueueProfileListGroup,
            juniQosSchedulerProfileListGroup2,
            juniQosProfileListGroup,
            juniQosProfileElementGroup3,
            juniQosIfAttachGroup,
            juniQosQosPortTypeProfileGroup,
            juniQosQueueStatisticsGroup,
            juniQosDropProfileListGroup,
            juniQosAtmVpUidSupportGroup,
            juniQosStatisticsProfileListGroup,
            juniQosQosModePortGroup,
            juniQosQosShapingModeGroup }
    ::= { juniQosCompliances 4 }                                   -- JUNOSe 6.0

juniQosCompliance5  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper QoS
        management MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniQosCapabilityGroup,
            juniQosScalarGroup3,
            juniQosTrafficClassListGroup,
            juniQosTrafficClassGroupListGroup2,
            juniQosQueueProfileListGroup,
            juniQosSchedulerProfileListGroup3,
            juniQosProfileListGroup,
            juniQosProfileElementGroup3,
            juniQosIfAttachGroup,
            juniQosQosPortTypeProfileGroup,
            juniQosQueueStatisticsGroup,
            juniQosDropProfileListGroup,
            juniQosAtmVpUidSupportGroup,
            juniQosStatisticsProfileListGroup,
            juniQosQosModePortGroup,
            juniQosQosShapingModeGroup }
    ::= { juniQosCompliances 5 }                                   -- JUNOSe 7.0

juniQosCompliance6  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper QoS
        management MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniQosCapabilityGroup,
            juniQosScalarGroup3,
            juniQosTrafficClassListGroup,
            juniQosTrafficClassGroupListGroup2,
            juniQosQueueProfileListGroup,
            juniQosSchedulerProfileListGroup4,
            juniQosProfileListGroup,
            juniQosProfileElementGroup3,
            juniQosIfAttachGroup,
            juniQosQosPortTypeProfileGroup,
            juniQosQueueStatisticsGroup,
            juniQosDropProfileListGroup,
            juniQosAtmVpUidSupportGroup,
            juniQosStatisticsProfileListGroup,
            juniQosQosModePortGroup,
            juniQosQosShapingModeGroup,
            juniQosSVlanUidSupportGroup,
            juniQosSVlanIdSupportGroup }
    ::= { juniQosCompliances 6 }                                   -- Kyoto FIXME:smg  Change to a number.

--
-- Units of conformance.
--
juniQosCapabilityGroup  OBJECT-GROUP
    OBJECTS {
        juniQosMaxTrafficClass,
        juniQosMaxQueueLength,
        juniQosMinSchedulerBurst,
        juniQosMaxSchedulerBurst,
        juniQosMaxQosProfileRules }
    STATUS      current
    DESCRIPTION
        "This group defines QoS application-wide capabilities management."
    ::= { juniQosGroups 1 }                                        -- JUNOSe 4.0

juniQosScalarGroup  OBJECT-GROUP
    OBJECTS {
        juniQosTrafficClassCount,
        juniQosQueueProfileCount,
        juniQosSchedulerProfileCount,
        juniQosProfileCount,
        juniQosInterfaceCount,
        juniQosQosPortTypeProfileCount }
    STATUS      obsolete
    DESCRIPTION
        "This obsolete group defines QoS application-wide counters.  This group
        became obsolete when drop profile list support was added."
    ::= { juniQosGroups 2 }                                        -- JUNOSe 4.0

juniQosTrafficClassListGroup  OBJECT-GROUP
    OBJECTS {
        juniQosTrafficClassNextIndex,

        juniQosTrafficClassRowStatus,
        juniQosTrafficClassName,
        juniQosTrafficClassWeight,
        juniQosTrafficClassStrictPriority,
        juniQosTrafficClassUpdatePending,
        juniQosTrafficClassUpdateNow,
        juniQosTrafficClassIsReferencedByGroup,
        juniQosTrafficClassIsReferencedByQosProfile }
    STATUS      current
    DESCRIPTION
        "This group defines QoS traffic class management."
    ::= { juniQosGroups 3 }                                        -- JUNOSe 4.0

juniQosTrafficClassGroupListGroup  OBJECT-GROUP
    OBJECTS {
        juniQosTrafficClassGroupNextIndex,

        juniQosTrafficClassGroupRowStatus,
        juniQosTrafficClassGroupName,
        juniQosTrafficClassGroupUpdatePending,
        juniQosTrafficClassGroupUpdateNow,
        juniQosTrafficClassGroupIsReferencedByQosProfile,

        juniQosTrafficClassGroupEntryRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "This obsolete group defines QoS traffic class group management.  This
        group became obsolete when multiple traffic class group support was
        added."
    ::= { juniQosGroups 4 }                                        -- JUNOSe 4.0

juniQosQueueProfileListGroup  OBJECT-GROUP
    OBJECTS {
        juniQosQueueProfileNextIndex,

        juniQosQueueProfileRowStatus,
        juniQosQueueProfileName,
        juniQosQueueProfileCommittedMinLength,
        juniQosQueueProfileCommittedMaxLength,
        juniQosQueueProfileConformedMinLength,
        juniQosQueueProfileConformedMaxLength,
        juniQosQueueProfileExceededMinLength,
        juniQosQueueProfileExceededMaxLength,
        juniQosQueueProfileConformedFraction,
        juniQosQueueProfileExceededFraction,
        juniQosQueueProfileCommittedDropThreshold,
        juniQosQueueProfileCommittedDropRate,
        juniQosQueueProfileConformedDropThreshold,
        juniQosQueueProfileConformedDropRate,
        juniQosQueueProfileExceededDropThreshold,
        juniQosQueueProfileExceededDropRate,
        juniQosQueueProfileBufferWeight,
        juniQosQueueProfileUpdatePending,
        juniQosQueueProfileUpdateNow,
        juniQosQueueProfileIsReferencedByQosProfile }
    STATUS      current
    DESCRIPTION
        "This group defines QoS queue profile management."
    ::= { juniQosGroups 5 }                                        -- JUNOSe 4.0

juniQosSchedulerProfileListGroup  OBJECT-GROUP
    OBJECTS {
        juniQosSchedulerProfileNextIndex,

        juniQosSchedulerProfileRowStatus,
        juniQosSchedulerProfileName,
        juniQosSchedulerProfileShapingRate,
        juniQosSchedulerProfileBurst,
        juniQosSchedulerProfileWeight,
        juniQosSchedulerProfileStrictPriority,
        juniQosSchedulerProfileUpdatePending,
        juniQosSchedulerProfileUpdateNow,
        juniQosSchedulerProfileIsReferencedByQosProfile }
    STATUS      obsolete
    DESCRIPTION
        "This obsolete group defines QoS scheduler profile management.  This
        group became obsolete when assured rate support was added."
    ::= { juniQosGroups 6 }                                        -- JUNOSe 4.0

juniQosProfileListGroup  OBJECT-GROUP
    OBJECTS {
        juniQosProfileNextIndex,

        juniQosProfileRowStatus,
        juniQosProfileName,
        juniQosProfileUpdatePending,
        juniQosProfileUpdateNow,
        juniQosProfileIsReferencedByInterfaceQosAttachment,
        juniQosProfileIsReferencedByQosPortTypeProfile }
    STATUS      current
    DESCRIPTION
        "This group defines QoS profile management."
    ::= { juniQosGroups 7 }                                        -- JUNOSe 4.0

juniQosProfileElementGroup  OBJECT-GROUP
    OBJECTS {
        juniQosProfileElementEntryRowStatus,
        juniQosProfileElementEntryQueueProfile,
        juniQosProfileElementEntrySchedulerProfile }
    STATUS      obsolete
    DESCRIPTION
        "This obsolete group defines QoS profile element entry management.  This
        group became obsolete when drop profile list support was added."
    ::= { juniQosGroups 8 }                                        -- JUNOSe 4.0

juniQosIfAttachGroup  OBJECT-GROUP
    OBJECTS {
        juniQosIfAttachRowStatus,
        juniQosIfAttachQosProfileIndex }
    STATUS      current
    DESCRIPTION
        "This group defines QoS interface attachment management."
    ::= { juniQosGroups 9 }                                        -- JUNOSe 4.0

juniQosQosPortTypeProfileGroup  OBJECT-GROUP
    OBJECTS {
        juniQosQosPortTypeProfileRowStatus,
        juniQosQosPortTypeProfileQosProfileIndex }
    STATUS      current
    DESCRIPTION
        "This group defines QoS default port profile management."
    ::= { juniQosGroups 10 }                                       -- JUNOSe 4.0

juniQosQueueStatisticsGroup  OBJECT-GROUP
    OBJECTS {
        juniQosOutPacketForwarded,
        juniQosOutBytesForwarded,
        juniQosOutGreenPacketsSchedulerDrops,
        juniQosOutYellowPacketsSchedulerDrops,
        juniQosOutRedPacketsSchedulerDrops,
        juniQosOutGreenBytesSchedulerDrops,
        juniQosOutYellowBytesSchedulerDrops,
        juniQosOutRedBytesSchedulerDrops }
    STATUS      current
    DESCRIPTION
        "This group defines QoS queue statistics reporting."
    ::= { juniQosGroups 11 }                                       -- JUNOSe 4.0

juniQosScalarGroup2  OBJECT-GROUP
    OBJECTS {
        juniQosTrafficClassCount,
        juniQosQueueProfileCount,
        juniQosSchedulerProfileCount,
        juniQosProfileCount,
        juniQosInterfaceCount,
        juniQosQosPortTypeProfileCount,
        juniQosDropProfileCount }
    STATUS      obsolete
    DESCRIPTION
        "This obsolete group defines QoS application-wide counters.  This group
        became obsolete when statistics profile list support was added."
    ::= { juniQosGroups 12 }                                       -- JUNOSe 5.0

juniQosProfileElementGroup2  OBJECT-GROUP
    OBJECTS {
        juniQosProfileElementEntryRowStatus,
        juniQosProfileElementEntryQueueProfile,
        juniQosProfileElementEntrySchedulerProfile,
        juniQosProfileElementEntryDropProfile }
    STATUS      obsolete
    DESCRIPTION
        "This obsolete group defines QoS profile element entry management.  This
        group became obsolete when statistics profile list support was added."
    ::= { juniQosGroups 13 }                                       -- JUNOSe 5.0

juniQosDropProfileListGroup  OBJECT-GROUP
    OBJECTS {
        juniQosDropProfileNextIndex,

        juniQosDropProfileRowStatus,
        juniQosDropProfileName,
        juniQosDropProfileAverageLengthExponent,
        juniQosDropProfileCommittedThresholdUnits,
        juniQosDropProfileCommittedThresholdMinThreshold,
        juniQosDropProfileCommittedThresholdMaxThreshold,
        juniQosDropProfileCommittedThresholdMaxDropProbability,
        juniQosDropProfileConformedThresholdUnits,
        juniQosDropProfileConformedThresholdMinThreshold,
        juniQosDropProfileConformedThresholdMaxThreshold,
        juniQosDropProfileConformedThresholdMaxDropProbability,
        juniQosDropProfileExceededThresholdUnits,
        juniQosDropProfileExceededThresholdMinThreshold,
        juniQosDropProfileExceededThresholdMaxThreshold,
        juniQosDropProfileExceededThresholdMaxDropProbability,
        juniQosDropProfileUpdatePending,
        juniQosDropProfileUpdateNow,
        juniQosDropProfileIsReferencedByQosProfile }
    STATUS      current
    DESCRIPTION
        "This group defines QoS drop profile management."
    ::= { juniQosGroups 14 }                                       -- JUNOSe 5.0

juniQosAtmVpUidSupportGroup  OBJECT-GROUP
    OBJECTS {
        juniQosAtmVpUidValid,
        juniQosAtmVpAtmPortInterfaceUid,
        juniQosAtmVpAtmPath,
        juniQosAtmVpUid }
    STATUS      current
    DESCRIPTION
        "This group defines QoS ATM VP UID support."
    ::= { juniQosGroups 15 }                                       -- JUNOSe 5.1

juniQosScalarGroup3  OBJECT-GROUP
    OBJECTS {
        juniQosTrafficClassCount,
        juniQosQueueProfileCount,
        juniQosSchedulerProfileCount,
        juniQosProfileCount,
        juniQosInterfaceCount,
        juniQosQosPortTypeProfileCount,
        juniQosDropProfileCount,
        juniQosStatisticsProfileCount }
    STATUS      current
    DESCRIPTION
        "This group defines QoS application-wide counters."
    ::= { juniQosGroups 16 }                                       -- JUNOSe 5.1

juniQosProfileElementGroup3  OBJECT-GROUP
    OBJECTS {
        juniQosProfileElementEntryRowStatus,
        juniQosProfileElementEntryQueueProfile,
        juniQosProfileElementEntrySchedulerProfile,
        juniQosProfileElementEntryDropProfile,
        juniQosProfileElementEntryStatisticsProfile }
    STATUS      current
    DESCRIPTION
        "This group defines QoS profile element entry management."
    ::= { juniQosGroups 17 }                                       -- JUNOSe 5.1

juniQosStatisticsProfileListGroup  OBJECT-GROUP
    OBJECTS {
        juniQosStatisticsProfileNextIndex,

        juniQosStatisticsProfileRowStatus,
        juniQosStatisticsProfileName,
        juniQosStatisticsProfileForwardingRateThreshold,
        juniQosStatisticsProfileCommittedDropThreshold,
        juniQosStatisticsProfileConformedDropThreshold,
        juniQosStatisticsProfileExceededDropThreshold,
        juniQosStatisticsProfileRatePeriod,
        juniQosStatisticsProfileUpdatePending,
        juniQosStatisticsProfileUpdateNow,
        juniQosStatisticsProfileIsReferencedByQosProfile }
    STATUS      current
    DESCRIPTION
        "This group defines QoS statistics profile management."
    ::= { juniQosGroups 18 }                                       -- JUNOSe 5.1

juniQosSchedulerProfileListGroup2  OBJECT-GROUP
    OBJECTS {
        juniQosSchedulerProfileNextIndex,

        juniQosSchedulerProfileRowStatus,
        juniQosSchedulerProfileName,
        juniQosSchedulerProfileShapingRate,
        juniQosSchedulerProfileBurst,
        juniQosSchedulerProfileWeight,
        juniQosSchedulerProfileStrictPriority,
        juniQosSchedulerProfileUpdatePending,
        juniQosSchedulerProfileUpdateNow,
        juniQosSchedulerProfileIsReferencedByQosProfile,
        juniQosSchedulerProfileAssuredRate,
        juniQosSchedulerProfileSharedShapingRate,
        juniQosSchedulerProfileSharedShapingBurstSize }
    STATUS      current
    DESCRIPTION
        "This group defines QoS scheduler profile management."
    ::= { juniQosGroups 19 }                                       -- JUNOSe 5.1

juniQosQosModePortGroup  OBJECT-GROUP
    OBJECTS {
        juniQosQosModePortRowStatus,
        juniQosQosModePortFrameMode }
    STATUS      current
    DESCRIPTION
        "This group defines QoS mode port management."
    ::= { juniQosGroups 20 }                                       -- JUNOSe 5.1

juniQosQosShapingModeGroup  OBJECT-GROUP
    OBJECTS {
        juniQosQosShapingModeRowStatus,
        juniQosQosShapingModeShapingMode }
    STATUS      current
    DESCRIPTION
        "This group defines QoS shaping mode management."
    ::= { juniQosGroups 21 }                                       -- JUNOSe 5.1

juniQosTrafficClassGroupListGroup2  OBJECT-GROUP
    OBJECTS {
        juniQosTrafficClassGroupNextIndex,

        juniQosTrafficClassGroupRowStatus,
        juniQosTrafficClassGroupName,
        juniQosTrafficClassGroupUpdatePending,
        juniQosTrafficClassGroupUpdateNow,
        juniQosTrafficClassGroupIsReferencedByQosProfile,
        juniQosTrafficClassGroupSlotNumber,
        juniQosTrafficClassGroupExtendedGroup,

        juniQosTrafficClassGroupEntryRowStatus }
    STATUS      current
    DESCRIPTION
        "This group defines QoS traffic class group management."
    ::= { juniQosGroups 22 }                                       -- JUNOSe 6.0

juniQosSchedulerProfileListGroup3  OBJECT-GROUP
    OBJECTS {
        juniQosSchedulerProfileNextIndex,

        juniQosSchedulerProfileRowStatus,
        juniQosSchedulerProfileName,
        juniQosSchedulerProfileShapingRate,
        juniQosSchedulerProfileBurst,
        juniQosSchedulerProfileWeight,
        juniQosSchedulerProfileStrictPriority,
        juniQosSchedulerProfileUpdatePending,
        juniQosSchedulerProfileUpdateNow,
        juniQosSchedulerProfileIsReferencedByQosProfile,
        juniQosSchedulerProfileAssuredRate,
        juniQosSchedulerProfileSharedShapingRate,
        juniQosSchedulerProfileSharedShapingBurstSize,
        juniQosSchedulerProfileSharedShapingType,
        juniQosSchedulerProfileSharedShapingExplicitConstituents,
        juniQosSchedulerProfileSharedShapingPriority,
        juniQosSchedulerProfileSharedShapingWeight }
    STATUS      current
    DESCRIPTION
        "This group defines QoS scheduler profile management."
    ::= { juniQosGroups 23 }                                       -- JUNOS/e 7.0

juniQosSchedulerProfileListGroup4  OBJECT-GROUP
    OBJECTS {
        juniQosSchedulerProfileNextIndex,

        juniQosSchedulerProfileRowStatus,
        juniQosSchedulerProfileName,
        juniQosSchedulerProfileShapingRate,
        juniQosSchedulerProfileBurst,
        juniQosSchedulerProfileWeight,
        juniQosSchedulerProfileStrictPriority,
        juniQosSchedulerProfileUpdatePending,
        juniQosSchedulerProfileUpdateNow,
        juniQosSchedulerProfileIsReferencedByQosProfile,
        juniQosSchedulerProfileAssuredRate,
        juniQosSchedulerProfileSharedShapingRate,
        juniQosSchedulerProfileSharedShapingBurstSize,
        juniQosSchedulerProfileSharedShapingType,
        juniQosSchedulerProfileSharedShapingExplicitConstituents,
        juniQosSchedulerProfileSharedShapingPriority,
        juniQosSchedulerProfileSharedShapingWeight }
    STATUS      current
    DESCRIPTION
        "This group defines QoS scheduler profile management."
    ::= { juniQosGroups 24 }                                       -- JUNOS/e Kyoto FIXME:smg

juniQosSVlanUidSupportGroup OBJECT-GROUP
    OBJECTS {
        juniQosSVlanUidTableSVlanUid }
    STATUS  current
    DESCRIPTION
        "This group defines QoS stacked vlan UID listing support."
    ::= { juniQosGroups 25 }

juniQosSVlanIdSupportGroup OBJECT-GROUP
    OBJECTS {
        juniQosSVlanIdTablePortUid,
        juniQosSVlanIdTableSVlanId }
    STATUS  current
    DESCRIPTION
        "This group defines QoS stacked vlan port/id listing support."
    ::= { juniQosGroups 26 }

END

