--
-- Juniper Enterprise specific MIB: SRX5000 SPU monitoring MIB
--
-- Copyright (c) 2008-2010, Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--

JUNIPER-SRX5000-SPU-MONITORING-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Gauge32, Unsigned32
        FROM SNMPv2-SMI
    CounterBasedGauge64
        FROM HCNUM-TC
    DisplayString 
        FROM SNMPv2-TC
    jnxJsSPUMonitoringRoot
        FROM JUNIPER-JS-SMI;

jnxJsSPUMonitoringMIB MODULE-IDENTITY
    LAST-UPDATED "201003250000Z" -- Mar 25 00:00:00 2010 UTC
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
            "        Juniper Technical Assistance Center
                     Juniper Networks, Inc.
                     1194 N. Mathilda Avenue
                     Sunnyvale, CA 94089
                     E-mail: support@juniper.net"
    DESCRIPTION
        "This is Juniper Networks' implementation of enterprise
                 specific MIB for SRX5000 SPU monitoring."
    REVISION
        "201003250000Z" -- Mar 25 00:00:00 2010 UTC
    DESCRIPTION
        "add MIB for session creation per second."

    ::= { jnxJsSPUMonitoringRoot 1 }

    jnxJsSPUMonitoringObjectsTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF JnxJsSPUMonitoringObjectsEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
            "This table exposes SPUs utilization statistics." 
        ::= { jnxJsSPUMonitoringMIB 1 }

    jnxJsSPUMonitoringObjectsEntry OBJECT-TYPE
        SYNTAX        JnxJsSPUMonitoringObjectsEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
            "Each entry collects CPU/Memory utilization for a SPU."
        INDEX   { jnxJsSPUMonitoringIndex }
        ::= { jnxJsSPUMonitoringObjectsTable 1 }

    JnxJsSPUMonitoringObjectsEntry ::= SEQUENCE
    {
        jnxJsSPUMonitoringIndex         Unsigned32,
        jnxJsSPUMonitoringFPCIndex      Unsigned32,
        jnxJsSPUMonitoringSPUIndex      Unsigned32,
        jnxJsSPUMonitoringCPUUsage      Unsigned32,
        jnxJsSPUMonitoringMemoryUsage   Unsigned32,
        jnxJsSPUMonitoringCurrentFlowSession	Unsigned32,
        jnxJsSPUMonitoringMaxFlowSession	Unsigned32,
        jnxJsSPUMonitoringCurrentCPSession	Unsigned32,
        jnxJsSPUMonitoringMaxCPSession	Unsigned32,
        jnxJsSPUMonitoringNodeIndex     Unsigned32,
        jnxJsSPUMonitoringNodeDescr     DisplayString
    }

    jnxJsSPUMonitoringIndex OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
                "SPU's overall index in platform."
        ::= { jnxJsSPUMonitoringObjectsEntry 1 }

    jnxJsSPUMonitoringFPCIndex OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Which FPC SPU is on."
        ::= { jnxJsSPUMonitoringObjectsEntry 2 }

    jnxJsSPUMonitoringSPUIndex OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "SPU'Index inside the FPC."
        ::= { jnxJsSPUMonitoringObjectsEntry 3 }

    jnxJsSPUMonitoringCPUUsage OBJECT-TYPE
        SYNTAX  Unsigned32
        UNITS   "percent"
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Current SPU(CPU) Utilization in percentage."
        ::= { jnxJsSPUMonitoringObjectsEntry 4 }

    jnxJsSPUMonitoringMemoryUsage OBJECT-TYPE
        SYNTAX  Unsigned32
        UNITS   "percent"
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Current memory usage of SPU(CPU) in percentage."
        ::= { jnxJsSPUMonitoringObjectsEntry 5 }
	
    jnxJsSPUMonitoringCurrentFlowSession OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Current flow session number of SPU."
        ::= { jnxJsSPUMonitoringObjectsEntry 6 }

    jnxJsSPUMonitoringMaxFlowSession OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Max flow session number of SPU."
        ::= { jnxJsSPUMonitoringObjectsEntry 7 }

    jnxJsSPUMonitoringCurrentCPSession OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Current CP session number of SPU."
        ::= { jnxJsSPUMonitoringObjectsEntry 8 }

    jnxJsSPUMonitoringMaxCPSession OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Max CP session number of SPU."
        ::= { jnxJsSPUMonitoringObjectsEntry 9 }

    jnxJsSPUMonitoringNodeIndex OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "This attribute is used to identify a chassis. A chassis can 
                 be configured in a single or cluster mode.  When it is in a 
                 cluster mode, the chassis can be denote as a cluster node."
        ::= { jnxJsSPUMonitoringObjectsEntry 10 }

    jnxJsSPUMonitoringNodeDescr OBJECT-TYPE
        SYNTAX        DisplayString (SIZE(1..255))
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION
            "This attribute is used to describe the chassis/cluster 
             node information.  Chassis can be configured as a single, or 
             cluster node.  When it is cluster mode, the chassis can be 
             denoted as a cluster node."
        ::= { jnxJsSPUMonitoringObjectsEntry 11 }

    jnxJsSPUMonitoringCurrentTotalSession OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "System level total session in use."
        ::= { jnxJsSPUMonitoringMIB 2 }

    jnxJsSPUMonitoringMaxTotalSession OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "System level max session possible."
        ::= { jnxJsSPUMonitoringMIB 3 }

    jnxSPUClusterObjectsTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF JnxSPUClusterObjectsEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
            "This table exposes SPU monitoring objects in HA cluster."
        ::= { jnxJsSPUMonitoringMIB 4 }


    jnxSPUClusterObjectsEntry OBJECT-TYPE
        SYNTAX        JnxSPUClusterObjectsEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
            "Each entry collects SPU monitoring contents in HA cluster."
        INDEX   { jnxJsClusterMonitoringNodeIndex }
        ::= { jnxSPUClusterObjectsTable 1 }

    JnxSPUClusterObjectsEntry ::= SEQUENCE
    {
        jnxJsClusterMonitoringNodeIndex     Unsigned32,
        jnxJsClusterMonitoringNodeDescr     DisplayString,
        jnxJsNodeCurrentTotalSession 	Unsigned32,
        jnxJsNodeMaxTotalSession	Unsigned32,
        jnxJsNodeSessionCreationPerSecond	CounterBasedGauge64
    }

    jnxJsClusterMonitoringNodeIndex OBJECT-TYPE
        SYNTAX  Unsigned32
        MAX-ACCESS not-accessible
        STATUS  current
        DESCRIPTION
                "This attribute is used to identify a chassis. A chassis can 
                 be configured in a single or cluster mode.  When it is in a 
                 cluster mode, the chassis can be denote as a cluster node."
        ::= { jnxSPUClusterObjectsEntry 1 }

    jnxJsClusterMonitoringNodeDescr OBJECT-TYPE
        SYNTAX        DisplayString (SIZE(1..255))
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION
            "This attribute is used to describe the chassis/cluster 
             node information.  Chassis can be configured as a single, or 
             cluster node.  When it is cluster mode, the chassis can be 
             denoted as a cluster node."
        ::= { jnxSPUClusterObjectsEntry 2 }
	
    jnxJsNodeCurrentTotalSession OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Node total session in use."
        ::= { jnxSPUClusterObjectsEntry 3 }

    jnxJsNodeMaxTotalSession OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "Node max session possible."
        ::= { jnxSPUClusterObjectsEntry 4 }
	
    jnxJsNodeSessionCreationPerSecond OBJECT-TYPE
	SYNTAX CounterBasedGauge64
	MAX-ACCESS  read-only
	STATUS  current
	DESCRIPTION
		"Node average session created in last 96 seconds."
	::= { jnxSPUClusterObjectsEntry 5 }

END

