 NEMO-MIB DEFINITIONS ::= BEGIN
  IMPORTS
    MODULE-IDENTITY,  mib-2, Unsigned32, Counter32,
    Gauge32,
    OBJECT-TYPE, NOTIFICATION-TYPE
               FROM SNMPv2-SMI
    TEXTUAL-CONVENTION,
    TruthValue, DateAndTime, TimeStamp
               FROM SNMPv2-TC
    SnmpAdminString
               FROM SNMP-FRAMEWORK-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
               FROM SNMPv2-CONF
    InetAddressType, InetAddress, InetAddressPrefixLength
               FROM INET-ADDRESS-MIB
    InterfaceIndex
               FROM IF-MIB
    mip6BindingHomeAddressType, mip6BindingHomeAddress,
    mip6MnBLEntry, mip6BindingCacheEntry,
    mip6MnBLCOAType, mip6MnBLCOA
               FROM MOBILEIPV6-MIB
    ;

 nemoMIB MODULE-IDENTITY
     LAST-UPDATED "200903100000Z"      -- 10 March 2009
     ORGANIZATION "IETF MEXT Working Group"

     CONTACT-INFO
        "           Sri Gundavelli
            Postal: Cisco
                    170 W.Tasman Drive,
                    San Jose, CA 95134
                    USA
               Tel: +1-408-527-6109
             Email: sgundave@cisco.com

                    Glenn Mansfield Keeni
            Postal: Cyber Solutions Inc.
                    6-6-3, Minami Yoshinari
                    Aoba-ku, Sendai, Japan 989-3204.
               Tel: +81-22-303-4012
               Fax: +81-22-303-4015
            E-mail: glenn@cysols.com

                    Kenichi Nagami
            Postal: INTEC NetCore Inc.
                    1-3-3, Shin-suna
                    Koto-ku, Tokyo, 135-0075
                    Japan
               Tel: +81-3-5665-5069
            E-mail: nagami@inetcore.com

                    Kazuhide Koide
            Postal: KDDI CORPORATION
                    GARDEN AIR TOWER 3-10-10, Iidabashi
                    Chiyoda-ku, Tokyo, 102-8460 Japan
               Tel: +81-3-6678-3378
            E-mail: ka-koide@kddi.com

        Support Group E-mail: mext@ietf.org
        "
        DESCRIPTION
         "Copyright (c) 2009 IETF Trust and the persons identified
          as authors of the code.  All rights reserved.

          Redistribution and use in source and binary forms, with
          or without modification, are permitted provided that the
          following conditions are met:

          - Redistributions of source code must retain the above
            copyright notice, this list of conditions and the
            following disclaimer.

          - Redistributions in binary form must reproduce the
            above copyright notice, this list of conditions and
            the following disclaimer in the documentation and/or
            other materials provided with the distribution.

          - Neither the name of Internet Society, IETF or IETF
            Trust, nor the names of specific contributors, may be
            used to endorse or promote products derived from this
            software without specific prior written permission.

         THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
         CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED
         WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
         WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A
         PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE
         COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT,
         INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
         CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
         PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
         DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
         CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
         CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE
         OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
         SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH
         DAMAGE.

         This version of this MIB module is part of RFC 5488;
         see the RFC itself for full legal notices."

         REVISION    "200903100000Z"      -- 10 March 2009
         DESCRIPTION "Initial version, published as RFC 5488."
              ::= { mib-2  184 }

  -- The NEMO MIB has the following primary groups

  nemoNotifications        OBJECT IDENTIFIER ::= { nemoMIB 0 }
  nemoObjects              OBJECT IDENTIFIER ::= { nemoMIB 1 }
  nemoConformance          OBJECT IDENTIFIER ::= { nemoMIB 2 }
  nemoCore                 OBJECT IDENTIFIER ::= { nemoObjects 1 }
  nemoMr                   OBJECT IDENTIFIER ::= { nemoObjects 2 }
  nemoCn                   OBJECT IDENTIFIER ::= { nemoObjects 3 }
  nemoHa                   OBJECT IDENTIFIER ::= { nemoObjects 4 }

   -- The sub groups

  nemoSystem               OBJECT IDENTIFIER ::= { nemoCore 1 }
  nemoBindings             OBJECT IDENTIFIER ::= { nemoCore 2 }

  nemoConfiguration        OBJECT IDENTIFIER ::= { nemoCore 3 }
  nemoStats                OBJECT IDENTIFIER ::= { nemoCore 4 }

  nemoMrSystem             OBJECT IDENTIFIER ::= { nemoMr 1 }
  nemoMrConf               OBJECT IDENTIFIER ::= { nemoMr 2 }
  nemoMrRegistration       OBJECT IDENTIFIER ::= { nemoMr 3 }
  nemoMrGlobalStats        OBJECT IDENTIFIER ::= { nemoMr 4 }

  nemoHaAdvertisement      OBJECT IDENTIFIER ::= { nemoHa 1 }
  nemoHaStats              OBJECT IDENTIFIER ::= { nemoHa 2 }
  nemoHaRegistration       OBJECT IDENTIFIER ::= { nemoHa 3 }
  nemoHaGlobalStats        OBJECT IDENTIFIER ::= { nemoHaStats 1 }

  -- Textual Conventions
NemoBURequestRejectionCode ::= TEXTUAL-CONVENTION
       STATUS        current
       DESCRIPTION
               "The value of the status field in the Binding
                Acknowledgment message when the Binding Update
                was rejected for NEMO-specific reasons.
               "
       REFERENCE
               "RFC 3963: Section 4.2"
       SYNTAX  INTEGER {
               mobileRouterOperationNotPermitted (140),
               invalidPrefix                     (141),
               notAuthorizedForPrefix            (142),
               forwardingSetupFailed             (143)
              }

  --
  --
  -- nemoSystem group
  --
  --

  nemoCapabilities OBJECT-TYPE
      SYNTAX      BITS {
                       mobileRouter       (0),
                       homeAgentSupport   (1)
                  }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
              "This object indicates the NEMO functions that
               are supported by this managed entity.  Multiple
               NEMO functions may be supported by a single
               entity.
              "
      REFERENCE
              "RFC 3963: Section 3"
      ::= { nemoSystem 1 }

  nemoStatus OBJECT-TYPE
      SYNTAX      INTEGER { enabled(1), disabled(2) }
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
              "This object indicates whether the NEMO
               function is enabled for the managed entity.  If it
               is enabled, the agent discovery and registration
               functions will be operational.

               Changing the status from enabled(1) to disabled(2)
               will terminate the agent discovery and registration
               functions.  On the other hand, changing the status
               from disabled(2) to enabled(1) will start the agent
               discovery and registration functions.

               The value of this object MUST remain unchanged
               across reboots of the managed entity.
              "
      ::= { nemoSystem 2 }

 nemoCounterDiscontinuityTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The value of sysUpTime on the most recent occasion at
             which any one or more of this NEMO entity's counters,
             viz., counters with OID prefix 'nemoMrConf',
             'nemoMrRegnCounters', 'nemoMrGlobalStats', or
             'nemoHaGlobalStats', suffered a discontinuity.  If
             no such discontinuities have occurred since the last
             re-initialization of the local management subsystem,
             then this object will have a zero value.
            "
    ::= { nemoStats 1 }
 --
 --

 --   nemoConfiguration group
 --
 --

nemoMrBLTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF NemoMrBLEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table corresponds to the Binding Update List
             (BL) that includes NEMO-related information and that
             is maintained by the mobile router.  The table
             holds a row for every binding that the mobile
             router has established or is trying to establish.
             Entries from the table are deleted as the lifetime
             of the binding expires.
            "
    REFERENCE
            "RFC 3775: Sections 4.5, 11.1
             RFC 3963: Section 5.2"
    ::= { nemoMrRegistration 1 }

nemoMrBLEntry  OBJECT-TYPE
    SYNTAX      NemoMrBLEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry pertaining to NEMO-related information
             contained in a Binding Update sent by a NEMO-enabled
             mobile router to its home agent.
            "
    AUGMENTS {mip6MnBLEntry}
::= { nemoMrBLTable 1 }

NemoMrBLEntry ::= SEQUENCE {
    nemoMrBLMode     INTEGER,
    nemoMrBLMrFlag   TruthValue,
    nemoMrBLHomeAddressPrefixLength   InetAddressPrefixLength,
    nemoMrBLCareofAddressPrefixLength InetAddressPrefixLength,
    nemoMrBLActiveEgressIfIndex       InterfaceIndex,
    nemoMrBLEstablishedHomeTunnelIfIndex InterfaceIndex
    }
nemoMrBLMode OBJECT-TYPE
    SYNTAX      INTEGER {
      implicitMode (1),
      explicitMode (2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "implicitMode(1): the Mobile Network Prefix Option
             is not included in the Binding Update by the mobile
             router.

             explicitMode(2): the mobile router included one or
             more Mobile Network Prefix Options in the Binding
             Update.
            "
    REFERENCE
            "RFC 3963: Section 5.2"
    ::= { nemoMrBLEntry 1 }

nemoMrBLMrFlag OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "true(1): the mobile router sent the Binding Update
             with Mobile Router Flag set.

             false(2): the mobile router did not send the Binding
             Update with Mobile Router Flag set.  This implies that
             the mobile router is acting as a mobile node.
            "
    REFERENCE
            "RFC 3963: Sections 4.1, 5.1"
    ::= { nemoMrBLEntry 2 }

nemoMrBLHomeAddressPrefixLength  OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The prefix length of the mobile router's home network.
            "
    REFERENCE
        "RFC 3963: Section 3"
    ::= { nemoMrBLEntry 3 }

nemoMrBLCareofAddressPrefixLength  OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The prefix length of the care-of address of the
             mobile router.
            "
    REFERENCE
        "RFC 3963: Section 3"
    ::= { nemoMrBLEntry 4 }

nemoMrBLActiveEgressIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The interface index of the currently active
             egress interface.
            "
    REFERENCE
        "RFC 3963: Section 5.5"
    ::= { nemoMrBLEntry 5 }

nemoMrBLEstablishedHomeTunnelIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The interface index of the tunnel established
             between the mobile router and the home agent
             for NEMO traffic.
            "
    REFERENCE
        "RFC 3963: Section 5.5"
    ::= { nemoMrBLEntry 6 }

-- Mobile Router Registration Group Counters

nemoMrRegnCounters OBJECT IDENTIFIER ::= { nemoMrRegistration 2 }

nemoMrMobilityMessagesSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of mobility messages, i.e., IPv6
             datagrams with Mobility Header, sent by the mobile
             node.  This will include Binding Updates sent by a
             mobile router with the Mobile Router Flag set.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3775: Sections 4.2, 6.1
             RFC 3963: Section 4.1"
    ::= {  nemoMrRegnCounters 1 }

nemoMrMobilityMessagesRecd OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of mobility messages, i.e., IPv6
             datagrams with Mobility Header, received by the
             mobile node.  This will include Binding
             Acknowledgements with Mobile Router Flag set that
             are sent to a mobile router.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3775: Sections 4.2, 6.1
             RFC 3963: Sections 4.1, 4.2"
    ::= {  nemoMrRegnCounters 2 }

nemoMrPrefixRegMode OBJECT-TYPE
    SYNTAX INTEGER {
              implicitMode       (1),
              explicitMode       (2)
           }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "This object indicates the mode in which the mobile
             network prefixes will be registered with the home
             agent.

             implicitMode(1): the Mobile Network Prefix Option will
             not be included in the Binding Update by the mobile
             router.

             explicitMode(2): the mobile router will include one or
             more Mobile Network Prefix Options in the Binding
             Update.

             The value of this object MUST remain unchanged
             across reboots of the managed entity.
            "
    REFERENCE
            "RFC 3963: Section 5.2"
    ::= { nemoMrRegistration 3 }

nemoHaMobileNetworkPrefixTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF NemoHaMobileNetworkPrefixEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains the mobile network prefixes
             that the home agent maintains for the mobile router.
             The mobile network prefixes in this table are
             registered by Binding Updates or are manually
             pre-configured.
            "
    REFERENCE
            "RFC 3963: Section 6.1.2"
    ::= { nemoHaRegistration 1 }

nemoHaMobileNetworkPrefixEntry OBJECT-TYPE
    SYNTAX      NemoHaMobileNetworkPrefixEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry for a mobile network prefix.

             The instances of the columnar objects in this entry
             pertain to an interface for a particular value of
             mip6BindingHomeAddressType, mip6BindingHomeAddress,
             and nemoHaMobileNetworkPrefixSeqNo.

             The nemoHaMobileNetworkPrefixSeqNo object is used to
             distinguish between multiple instances of
             the mobile network prefix in the same Binding Update
             for the same set of mip6BindingHomeAddressType and
             mip6BindingHomeAddress.

             There is no upper-bound on the maximum number of
             mobile network prefixes in a Binding Update but, for
             practical purposes, the upper bound of the value

             nemoHaMobileNetworkPrefixSeqNo is set to 1024.

             Implementers need to be aware that if the total
             number of octets in mip6BindingHomeAddress
             exceeds 112, then OIDs of column
             instances in this row will have more than 128
             sub-identifiers and cannot be accessed using
             SNMPv1, SNMPv2c, or SNMPv3.
            "
    INDEX  { mip6BindingHomeAddressType,
             mip6BindingHomeAddress,
             nemoHaMobileNetworkPrefixSeqNo
}
::= { nemoHaMobileNetworkPrefixTable 1 }

NemoHaMobileNetworkPrefixEntry ::= SEQUENCE {
    nemoHaMobileNetworkPrefixSeqNo       Unsigned32,
    nemoHaMobileNetworkPrefixType        InetAddressType,
    nemoHaMobileNetworkPrefix            InetAddress,
    nemoHaMobileNetworkPrefixLength      Unsigned32,
    nemoHaMobileNetworkPrefixSource      INTEGER
}

nemoHaMobileNetworkPrefixSeqNo OBJECT-TYPE
    SYNTAX      Unsigned32 (1..1024)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A Binding Update may have multiple mobile network
             prefixes.

             This object, along with mip6BindingHomeAddressType
             and mip6BindingHomeAddress, uniquely identifies a
             row containing a single mobile network prefix for
             a mobile router in this table.
            "
    REFERENCE
            "RFC 3963: Sections 2, 6.1, 6.2"
    ::= { nemoHaMobileNetworkPrefixEntry 1 }

nemoHaMobileNetworkPrefixType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The address type for the mobile network prefix
             that follows.
            "
    ::= { nemoHaMobileNetworkPrefixEntry 2 }

nemoHaMobileNetworkPrefix OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "A mobile network prefix related to the
             corresponding Binding Update.

             The type of the address represented by this object
             is specified by the corresponding
             nemoHaMobileNetworkPrefixType object.
            "
    REFERENCE
            "RFC 3963: Sections 2, 6.1, 6.2"
    ::= { nemoHaMobileNetworkPrefixEntry 3 }

nemoHaMobileNetworkPrefixLength OBJECT-TYPE
    SYNTAX      Unsigned32 (0..128)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The length of the prefix specified by the corresponding
             nemoHaMobileNetworkPrefix object.
            "
    REFERENCE
            "RFC 3963: Sections 4.3, 6.1, 6.2"
    ::= { nemoHaMobileNetworkPrefixEntry 4 }

nemoHaMobileNetworkPrefixSource OBJECT-TYPE
    SYNTAX      INTEGER {
             configured    (1),
             bindingUpdate (2)
             }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The information source of the mobile network prefix
             configured with the Binding Update.

             configured(1): indicates that the mobile network prefix
             has been manually pre-configured.

             bindingUpdate(2): indicates that the information is
             introduced to the home agent by the Mobile Network

             Prefix Option in the Binding Updates received by the
             home agent.
            "
    REFERENCE
            "RFC 3963: Sections 4.3, 6.1, 6.2"
    ::= { nemoHaMobileNetworkPrefixEntry 5 }

nemoBindingCacheTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF NemoBindingCacheEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "This table models the Binding Cache that includes
            NEMO-related information and that is maintained by the
            home agent.  Entries in this table are not required
            to survive a reboot of the home agent.
           "
    REFERENCE
            "RFC 3775: Sections 4.5, 9.1, 10.1,
             RFC 3963: Section 6.1"
    ::= { nemoBindings 1 }

nemoBindingCacheEntry  OBJECT-TYPE
    SYNTAX      NemoBindingCacheEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry containing additional information related
             to NEMO-enabled entries in the Binding Cache table
             of the home agent.
            "
    AUGMENTS {mip6BindingCacheEntry}
::= { nemoBindingCacheTable 1 }

NemoBindingCacheEntry ::= SEQUENCE {
     nemoBindingMrFlag     TruthValue,
     nemoBindingMrMode     INTEGER
    }

nemoBindingMrFlag OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "true(1): indicates that the Binding Cache entry is from
             an entity acting as a mobile router.

             false(2): implies that the Binding Cache entry is from
             an entity acting as a mobile node.
            "
    REFERENCE
            "RFC 3963: Sections 6.1.1, 6.2"
    ::= { nemoBindingCacheEntry 1 }

nemoBindingMrMode OBJECT-TYPE
    SYNTAX      INTEGER {
      implicitMode(1),
      explicitMode(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "implicitMode(1): the Mobile Network Prefix Option is
             not included in the Binding Update by the mobile
             router.

             explicitMode(2): the mobile router included one or
             more Mobile Network Prefix Options in the Binding
             Update.
            "
    REFERENCE
            "RFC 3963: Sections 5.2, 6.1.1, 6.2"
    ::= { nemoBindingCacheEntry 2 }

--
-- nemoMrEgressIfTable
--
nemoMrEgressIfTable        OBJECT-TYPE
     SYNTAX      SEQUENCE OF NemoMrEgressIfEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
             "A table representing the egress interfaces that
              will be used by the mobile router for roaming to
              foreign networks.  Each entry in this table
              represents a configured egress interface.
             "
     ::= { nemoMrSystem 1 }

nemoMrEgressIfEntry OBJECT-TYPE
     SYNTAX      NemoMrEgressIfEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
             "An entry in the egress interface table.  It

              represents a single egress interface entry.
             "
     INDEX  { nemoMrEgressIfIndex }
     ::= { nemoMrEgressIfTable 1 }

NemoMrEgressIfEntry ::=
     SEQUENCE {
      nemoMrEgressIfIndex             InterfaceIndex,
      nemoMrEgressIfPriority          Unsigned32,
      nemoMrEgressIfDescription       SnmpAdminString,
      nemoMrEgressIfRoamHoldDownTime  Gauge32
     }

nemoMrEgressIfIndex  OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
             "The index of the interface on the mobile router.
             "
     ::= { nemoMrEgressIfEntry 1 }

nemoMrEgressIfPriority   OBJECT-TYPE
     SYNTAX      Unsigned32 (0..255)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
             "The priority configured to the egress interface.
              This value will be configured to a value between 0
              and 255.
             "
     ::= { nemoMrEgressIfEntry 2 }

nemoMrEgressIfDescription   OBJECT-TYPE
     SYNTAX      SnmpAdminString
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
             "A human-readable textual description of the egress
              interface on the mobile router.
             "
     ::= { nemoMrEgressIfEntry 3 }

nemoMrEgressIfRoamHoldDownTime  OBJECT-TYPE
     SYNTAX      Gauge32
     UNITS       "seconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
             "This object indicates the time for which the
              egress interface will be held down during roaming
              to avoid interface flapping.
             "
     ::= { nemoMrEgressIfEntry 4 }

nemoMrDiscoveryRequests OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of Modified Dynamic Home Agent Address
             Discovery Requests, with Mobile Router Support Flag
             set, sent by the mobile router.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3775: Sections 10.5, 11.4.1
             RFC 3963: Section 7.1"
       ::= { nemoMrConf 1 }

nemoMrDiscoveryReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of Modified Dynamic Home Agent Address
             Discovery Replies, with Mobile Router Support Flag
             set, received by the mobile router.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3775: Sections 10.5, 11.4.1
             RFC 3963: Section 7.2"
       ::= { nemoMrConf 2 }

nemoMrDiscoveryRepliesRouterFlagZero OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of Modified Dynamic Home Agent Address
             Discovery Replies, with Mobile Router Support Flag set
             to 0 although the flag in the corresponding request
             is set to 1.  It implies that there is no home agent
             that supports mobile router functionality in the home
             network.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3775: Sections 10.5, 11.4.1
             RFC 3963: Section 7.2"
       ::= { nemoMrConf 3 }

nemoMrMovedHome OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of times the mobile router has detected
             movement from a foreign network to its home
             network.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
        "RFC 3963: Section 3"
        ::= { nemoMrConf 4 }

nemoMrMovedOutofHome OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of times the mobile router has detected
             movement to a foreign network from the home
             network, has acquired a care-of address, and
             has initiated the care-of address registration
             process.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
        "RFC 3963: Section 3"
        ::= { nemoMrConf 5 }

nemoMrMovedFNtoFN OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of times the mobile router has detected
             movement to/from a foreign network from/to another
             foreign network.  Note that 'movement' implies
             movement in layer 3, i.e., the mobile router's care-of
             address changed, and it initiated the care-of address
             registration process.

             If there are multiple egress interfaces, this counter
             counts the total number of movements.  The movement
             as a mobile node of the mobile entity is not counted.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 3"
        ::= { nemoMrConf 6 }

nemoMrBetterIfDetected OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Number of times the NEMO entity has found an egress
             interface with better priority.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
        ::= { nemoMrConf 7 }

--
-- nemoStats:nemoMrGlobalStats
--

nemoMrBindingAcksWONemoSupport  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements without
             NEMO support received by the mobile router.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 5.3"
        ::= { nemoMrGlobalStats 1 }

nemoMrBindingAcksRegTypeChangeDisallowed  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements
             received by the mobile router with status code
             indicating 'Registration type change disallowed'
             (Code 139).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3775: Section 9.5.1
             RFC 3963: Section 6.2"
        ::= { nemoMrGlobalStats 2 }

nemoMrBindingAcksOperationNotPermitted  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements
             received by the mobile router with status code

             indicating 'Mobile Router Operation not permitted'
             (Code 140).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoMrGlobalStats 3 }

nemoMrBindingAcksInvalidPrefix  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements
             received by the mobile router with status code
             indicating 'Invalid Prefix' (Code 141).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoMrGlobalStats 4 }

nemoMrBindingAcksNotAuthorizedForPrefix OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements
             received by the mobile router with status code
             indicating 'Not Authorized for Prefix' (Code 142).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963 : Section 6.6"
        ::= { nemoMrGlobalStats 5 }

nemoMrBindingAcksForwardingSetupFailed OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements
             received by the mobile router with status code
             indicating 'Forwarding Setup failed' (Code 143).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoMrGlobalStats 6 }

nemoMrBindingAcksOtherError OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements
             received by the mobile router (Mobile Router Flag is
             set) with status code other than:

             successfully processed                  --(Code 0  )
             mobileRouterOperationNotPermitted (140) --(Code 140)
             invalidPrefix                     (141) --(Code 141)
             notAuthorizedForPrefix            (142) --(Code 142)
             forwardingSetupFailed             (143) --(Code 143)

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963 : Section 6.6"
        ::= { nemoMrGlobalStats 7 }

--
-- nemoStats:nemoHaGlobalStats
--

nemoHaBUAcksWONemoSupport  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Acknowledgements
             without NEMO support sent by the home agent.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 5.3"
        ::= { nemoHaGlobalStats 1 }

nemoHaBUAcksRegTypeChangeDisallowed  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Update requests
             rejected by the home agent with status code
             in the Binding Acknowledgement indicating
             'Registration type change disallowed' (Code 139).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3775: Section 9.5.1
             RFC 3963: Section 6.2"
        ::= { nemoHaGlobalStats 2 }

nemoHaBUAcksOperationNotPermitted  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Update requests
             rejected by the home agent with status code in
             the Binding Acknowledgement indicating 'Mobile
             Router Operation not permitted' (Code 140).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of

             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoHaGlobalStats 3 }

nemoHaBUAcksInvalidPrefix  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Update requests
             rejected by the home agent with status code in
             the Binding Acknowledgement indicating 'Invalid
             Prefix' (Code 141).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoHaGlobalStats 4 }

nemoHaBUAcksNotAuthorizedForPrefix OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Update requests
             rejected by the home agent with status code in
             the Binding Acknowledgement indicating 'Not
             Authorized for Prefix' (Code 142).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoHaGlobalStats 5 }

nemoHaBUAcksForwardingSetupFailed OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Update requests
             rejected by the home agent with status code in
             the Binding Acknowledgement indicating 'Forwarding
             Setup failed' (Code 143).

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoHaGlobalStats 6 }

nemoHaBUAcksOtherError OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of Binding Update requests
             from mobile routers (Mobile Router Flag is set)
             rejected by the home agent with status code
             other than:

             mobileRouterOperationNotPermitted (140)
             invalidPrefix                     (141)
             notAuthorizedForPrefix            (142)
             forwardingSetupFailed             (143)

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoCounterDiscontinuityTime.
            "
    REFERENCE
            "RFC 3963: Section 6.6"
        ::= { nemoHaGlobalStats 7 }

nemoHaCounterTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF NemoHaCounterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A table containing registration statistics for all
             mobile routers registered with the home agent.
            "
    ::= { nemoHaStats 2 }

nemoHaCounterEntry  OBJECT-TYPE
    SYNTAX      NemoHaCounterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Home agent registration statistics for a mobile
             router.

             Implementers need to be aware that if the total
             number of octets in mip6BindingHomeAddress
             exceeds 113, then OIDs of column instances in
             this row will have more than 128 sub-identifiers and
             cannot be accessed using SNMPv1, SNMPv2c, or SNMPv3.
            "
    INDEX   { mip6BindingHomeAddressType,
              mip6BindingHomeAddress
            }
    ::= { nemoHaCounterTable 1 }

NemoHaCounterEntry      ::= SEQUENCE {
    nemoHaBURequestsAccepted       Counter32,
    nemoHaBURequestsDenied         Counter32,
    nemoHaBCEntryCreationTime      DateAndTime,
    nemoHaBUAcceptedTime           DateAndTime,
    nemoHaBURejectionTime          DateAndTime,
    nemoHaRecentBURejectionCode    NemoBURequestRejectionCode,
    nemoHaCtrDiscontinuityTime     TimeStamp
    }

nemoHaBURequestsAccepted OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of Binding Update requests from the
             mobile router accepted by the home agent.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoHaCtrDiscontinuityTime.
            "
    ::= { nemoHaCounterEntry 1 }

nemoHaBURequestsDenied   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Total number of Binding Update requests from the
             mobile router rejected by the home agent.

             Discontinuities in the value of this counter can
             occur at re-initialization of the management system,
             and at other times as indicated by the value of
             nemoHaCtrDiscontinuityTime.
            "
    ::= { nemoHaCounterEntry 2 }

nemoHaBCEntryCreationTime   OBJECT-TYPE
    SYNTAX      DateAndTime (SIZE (11))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The time when the current Binding Cache entry was
             created for the mobile router.  An implementation
             MUST return all 11 bytes of the DateAndTime
             textual-convention so that a manager may retrieve
             the offset from GMT time.
            "
    ::= { nemoHaCounterEntry 3 }

nemoHaBUAcceptedTime  OBJECT-TYPE
    SYNTAX      DateAndTime (SIZE (11))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The time at which the last Binding Update was
             accepted by the home agent for this mobile router.
             An implementation MUST return all 11 bytes of the
             DateAndTime textual-convention so that a manager
             may retrieve the offset from GMT time.
            "
    ::= { nemoHaCounterEntry 4 }

nemoHaBURejectionTime  OBJECT-TYPE
    SYNTAX      DateAndTime (SIZE (11))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The time at which the last Binding Update was
             rejected by the home agent for this mobile router.
             If there have been no rejections, then this object
             will be inaccessible.  An implementation MUST return
             all 11 bytes of the DateAndTime textual-convention
             so that a manager may retrieve the offset from GMT

             time.
            "
    ::= { nemoHaCounterEntry 5 }

nemoHaRecentBURejectionCode  OBJECT-TYPE
    SYNTAX      NemoBURequestRejectionCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The Status code (>= 128) in the latest Binding
             Acknowledgment indicating a rejection, sent to this
             mobile router.

             If a Binding Update request is rejected and a Binding
             Acknowledgment is not sent to this mobile router,
             then this will be the value of the Status code that
             corresponds to the reason of the rejection.  If there
             have been no Binding Update request rejections, then
             this object will be inaccessible.
            "
    ::= { nemoHaCounterEntry 6 }

nemoHaCtrDiscontinuityTime OBJECT-TYPE
   SYNTAX      TimeStamp
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
           "The value of sysUpTime on the most recent occasion
            at which any one or more of the counters in this row,
            viz., instances of 'nemoHaBURequestsAccepted' and
            'nemoHaBURequestsDenied', suffered a discontinuity.
            If no such discontinuity has occurred since the
            last re-initialization of the local management
            subsystem, then this object will have a zero value.
           "
   ::= { nemoHaCounterEntry 7 }

--
--
-- nemoNotifications
--
--

nemoHomeTunnelEstablished NOTIFICATION-TYPE
    OBJECTS   {
                nemoMrBLActiveEgressIfIndex,
                nemoMrBLEstablishedHomeTunnelIfIndex,
                mip6MnBLCOAType,
                mip6MnBLCOA,
                nemoMrBLHomeAddressPrefixLength,
                nemoMrBLCareofAddressPrefixLength
              }
    STATUS    current
    DESCRIPTION
            "This notification is sent by the mobile router
             every time the tunnel is established between the
             home agent and the mobile router.
            "
    REFERENCE
            "RFC 3963: Section 5.5"
        ::= { nemoNotifications 1 }

nemoHomeTunnelReleased NOTIFICATION-TYPE
    OBJECTS {
                nemoMrBLActiveEgressIfIndex,
                nemoMrBLEstablishedHomeTunnelIfIndex,
                mip6MnBLCOAType,
                mip6MnBLCOA,
                nemoMrBLHomeAddressPrefixLength,
                nemoMrBLCareofAddressPrefixLength
            }
    STATUS    current
    DESCRIPTION
            "This notification is sent by the mobile router
             every time the tunnel is deleted between the home
             agent and the mobile router.
            "
    REFERENCE
            "RFC 3963: Section 5.5"
        ::= { nemoNotifications 2}

-- Conformance information
nemoGroups      OBJECT IDENTIFIER ::= { nemoConformance 1 }
nemoCompliances OBJECT IDENTIFIER ::= { nemoConformance 2 }

-- Units of conformance
nemoSystemGroup    OBJECT-GROUP
     OBJECTS {
               nemoCapabilities,
               nemoStatus
    }
     STATUS  current
     DESCRIPTION
             "A collection of objects for basic NEMO
              monitoring.
             "
     ::= { nemoGroups 1 }

nemoBindingCacheGroup    OBJECT-GROUP
     OBJECTS {
               nemoBindingMrFlag,
               nemoBindingMrMode
    }
     STATUS  current
     DESCRIPTION
             "A collection of objects for monitoring the
              NEMO extensions of the Binding Cache.
             "
     ::= { nemoGroups 2 }

nemoStatsGroup    OBJECT-GROUP
     OBJECTS {
               nemoCounterDiscontinuityTime
    }
     STATUS  current
     DESCRIPTION
             "A collection of objects for
              monitoring NEMO statistics.
             "
     ::= { nemoGroups 3 }

nemoMrConfGroup   OBJECT-GROUP
     OBJECTS {
               nemoMrEgressIfPriority,
               nemoMrEgressIfDescription,
               nemoMrEgressIfRoamHoldDownTime,
               nemoMrDiscoveryRequests,
               nemoMrDiscoveryReplies,
               nemoMrDiscoveryRepliesRouterFlagZero,
               nemoMrMovedHome,
               nemoMrMovedOutofHome,
               nemoMrMovedFNtoFN,
               nemoMrBetterIfDetected
    }
     STATUS  current
     DESCRIPTION
             "A collection of objects for monitoring
              the configuration-related information on
              the mobile router.
             "
     ::= { nemoGroups 4 }

nemoMrRegistrationGroup  OBJECT-GROUP

     OBJECTS {
               nemoMrBLMode,
               nemoMrBLMrFlag,
               nemoMrBLHomeAddressPrefixLength,
               nemoMrBLCareofAddressPrefixLength,
               nemoMrBLActiveEgressIfIndex,
               nemoMrBLEstablishedHomeTunnelIfIndex,
               nemoMrMobilityMessagesSent,
               nemoMrMobilityMessagesRecd,
               nemoMrPrefixRegMode,
               nemoMrBindingAcksWONemoSupport,
               nemoMrBindingAcksRegTypeChangeDisallowed,
               nemoMrBindingAcksOperationNotPermitted,
               nemoMrBindingAcksInvalidPrefix,
               nemoMrBindingAcksNotAuthorizedForPrefix,
               nemoMrBindingAcksForwardingSetupFailed,
               nemoMrBindingAcksOtherError
    }
     STATUS  current
     DESCRIPTION
             "A collection of objects for monitoring
              the registration details and statistics for
              the mobile router.
             "
     ::= { nemoGroups 5 }

nemoHaSystemGroup    OBJECT-GROUP
    OBJECTS {
              nemoHaMobileNetworkPrefixType,
              nemoHaMobileNetworkPrefix,
              nemoHaMobileNetworkPrefixLength,
              nemoHaMobileNetworkPrefixSource
   }
    STATUS  current
    DESCRIPTION
            "A collection of objects for basic NEMO
             configuration monitoring at the home agent.
            "
    ::= { nemoGroups 6 }

nemoHaStatsGroup   OBJECT-GROUP
    OBJECTS {
              nemoHaBURequestsAccepted,
              nemoHaBURequestsDenied,
              nemoHaBCEntryCreationTime,
              nemoHaBUAcceptedTime,
              nemoHaBURejectionTime,
              nemoHaRecentBURejectionCode,
              nemoHaCtrDiscontinuityTime
   }
    STATUS  current
    DESCRIPTION
            "A collection of objects for monitoring NEMO
             registration-related statistics pertaining to
             the mobile routers registered with the home agent.
            "
    ::= { nemoGroups 7 }

nemoHaGlobalStatsGroup   OBJECT-GROUP
    OBJECTS {
              nemoHaBUAcksWONemoSupport,
              nemoHaBUAcksRegTypeChangeDisallowed,
              nemoHaBUAcksOperationNotPermitted,
              nemoHaBUAcksInvalidPrefix,
              nemoHaBUAcksNotAuthorizedForPrefix,
              nemoHaBUAcksForwardingSetupFailed,
              nemoHaBUAcksOtherError
   }
    STATUS  current
    DESCRIPTION
            "A collection of objects for monitoring basic
             NEMO advertisement and registration statistics
             on a home agent.
            "
    ::= { nemoGroups 8 }

nemoNotificationGroup   NOTIFICATION-GROUP
    NOTIFICATIONS {
             nemoHomeTunnelEstablished,
             nemoHomeTunnelReleased
   }
    STATUS  current
    DESCRIPTION
            "A collection of notifications from a home agent
             or correspondent node to the manager about the
             tunnel status of the mobile router.
            "
    ::= { nemoGroups 9 }

-- Compliance statements
nemoCoreCompliance MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities
             that implement the NEMO-MIB.
             "

     MODULE  -- this module
         MANDATORY-GROUPS { nemoSystemGroup
                          }
     ::= { nemoCompliances 1 }

nemoCompliance2 MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities that
             implement the NEMO-MIB and support monitoring of
             the Binding Cache.

             There are a number of INDEX objects that cannot be
             represented in the form of OBJECT clauses in SMIv2,
             but for which there are compliance requirements,
             expressed in OBJECT-clause form in this description:

             -- OBJECT      mip6BindingHomeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             -- OBJECT      mip6BindingHomeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoSystemGroup,
                            nemoBindingCacheGroup
                          }
     ::= { nemoCompliances 2 }

nemoCoreReadOnlyCompliance MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities
             that implement the NEMO-MIB without support
             for read-write (i.e., in read-only mode).
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoSystemGroup
                          }

     OBJECT      nemoStatus
     MIN-ACCESS  read-only
     DESCRIPTION
            "Write access is not required."
     ::= { nemoCompliances 3 }

nemoReadOnlyCompliance2 MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities that
             implement the NEMO-MIB without support for read-write
             (i.e., in read-only mode) and with support for
             monitoring of the Binding Cache.

             There are a number of INDEX objects that cannot be
             represented in the form of OBJECT clauses in SMIv2,
             but for which there are compliance requirements,
             expressed in OBJECT-clause form in this description:

             -- OBJECT      mip6BindingHomeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             -- OBJECT      mip6BindingHomeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoSystemGroup,
                            nemoBindingCacheGroup
                          }
     OBJECT      nemoStatus
     MIN-ACCESS  read-only
     DESCRIPTION
            "Write access is not required."
     ::= { nemoCompliances 4 }

nemoMrCompliance MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities that

             implement the NEMO-MIB for monitoring configuration-
             related information, registration details, and
             statistics on a mobile router.

             There are a number of INDEX objects that cannot be
             represented in the form of OBJECT clauses in SMIv2,
             but for which there are compliance requirements,
             expressed in OBJECT-clause form in this description:

             -- OBJECT      mip6MnHomeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnHomeAddress
             --     object.
             --
             -- OBJECT      mip6MnHomeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnHomeAddress
             --     object.
             --
             -- OBJECT      mip6MnBLNodeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnBLNodeAddress
             --     object.
             --
             -- OBJECT      mip6MnBLNodeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnBLNodeAddress
             --     object.
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoStatsGroup,
                            nemoMrConfGroup,
                            nemoMrRegistrationGroup
                          }
     ::= { nemoCompliances 5 }

nemoMrReadOnlyCompliance2 MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities that

             implement the NEMO-MIB without support for read-
             write (i.e., in read-only mode) and with support for
             monitoring of configuration-related information,
             registration details, and statistics on a mobile
             router.

             There are a number of INDEX objects that cannot be
             represented in the form of OBJECT clauses in SMIv2,
             but for which there are compliance requirements,
             expressed in OBJECT-clause form in this description:

             -- OBJECT      mip6MnHomeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnHomeAddress
             --     object.
             --
             -- OBJECT      mip6MnHomeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnHomeAddress
             --     object.
             --
             -- OBJECT      mip6MnBLNodeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnBLNodeAddress
             --     object.
             --
             -- OBJECT      mip6MnBLNodeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6MnBLNodeAddress
             --     object.
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoStatsGroup,
                            nemoMrConfGroup,
                            nemoMrRegistrationGroup
                          }

     OBJECT      nemoMrPrefixRegMode
     MIN-ACCESS  read-only
     DESCRIPTION
            "Write access is not required."
     ::= { nemoCompliances 6 }

nemoHaCoreCompliance MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities that
             implement the NEMO-MIB for configuration monitoring
             at the home agent.

             There are a number of INDEX objects that cannot be
             represented in the form of OBJECT clauses in SMIv2,
             but for which there are compliance requirements,
             expressed in OBJECT-clause form in this description:

             -- OBJECT      mip6BindingHomeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             -- OBJECT      mip6BindingHomeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoHaSystemGroup
                          }
     ::= { nemoCompliances 7 }

nemoHaCompliance2 MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities that
             implement the NEMO-MIB with support for monitoring
             of the home agent functionality, specifically the
             home-agent-registration-related statistics.

             There are a number of INDEX objects that cannot be
             represented in the form of OBJECT clauses in SMIv2,
             but for which there are compliance requirements,
             expressed in OBJECT-clause form in this description:

             -- OBJECT      mip6BindingHomeAddressType
             -- SYNTAX      InetAddressType { ipv6(2) }
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             -- OBJECT      mip6BindingHomeAddress
             -- SYNTAX      InetAddress (SIZE(16))
             -- DESCRIPTION
             --     This MIB module requires support for global
             --     IPv6 addresses for the mip6BindingHomeAddress
             --     object.
             --
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoHaSystemGroup,
                            nemoHaStatsGroup,
                            nemoHaGlobalStatsGroup
                          }
     ::= { nemoCompliances 8 }

nemoNotificationCompliance MODULE-COMPLIANCE
     STATUS  current
     DESCRIPTION
            "The compliance statement for SNMP entities that
             implement the NEMO-MIB and support Notification
             from the home agent.
             "
     MODULE  -- this module
         MANDATORY-GROUPS { nemoNotificationGroup
                          }
     ::= { nemoCompliances 9 }

END
