   RIPv2-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, Counter32,
       TimeTicks, IpAddress                     FROM SNMPv2-SMI
       TEXTUAL-CONVENTION, RowStatus            FROM SNMPv2-TC
       MODULE-COMPLIANCE, OBJECT-GROUP          FROM SNMPv2-CONF
       mib-2                                    FROM RFC1213-MIB;

   --  This MIB module uses the extended OBJECT-TYPE macro as
   --  defined in [9].

   rip2  MODULE-IDENTITY
           LAST-UPDATED "9407272253Z"      -- Wed Jul 27 22:53:04 PDT 1994
           ORGANIZATION "IETF RIP-II Working Group"
           CONTACT-INFO
          "       Fred Baker
          Postal: Cisco Systems
                  519 Lado Drive
                  Santa Barbara, California 93111
          Tel:    +1 805 681 0115
          E-Mail: fbaker@cisco.com

          Postal: Gary Malkin
                  Xylogics, Inc.
                  53 Third Avenue
                  Burlington, MA  01803

          Phone:  (617) 272-8140
          EMail:  gmalkin@Xylogics.COM"
      DESCRIPTION
         "The MIB module to describe the RIP2 Version 2 Protocol"
     ::= { mib-2 23 }

 --  RIP-2 Management Information Base

 -- the RouteTag type represents the contents of the
 -- Route Domain field in the packet header or route entry.
 -- The use of the Route Domain is deprecated.

 RouteTag ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "the RouteTag type represents the contents of the Route Domain
        field in the packet header or route entry"
    SYNTAX      OCTET STRING (SIZE (2))

--4.1 Global Counters

--      The RIP-2 Globals Group.
--      Implementation of this group is mandatory for systems
--      which implement RIP-2.

-- These counters are intended to facilitate debugging quickly
-- changing routes or failing neighbors

rip2Globals OBJECT IDENTIFIER ::= { rip2 1 }

    rip2GlobalRouteChanges OBJECT-TYPE
        SYNTAX   Counter32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The number of route changes made to the IP Route
           Database by RIP.  This does not include the refresh
           of a route's age."
       ::= { rip2Globals 1 }

    rip2GlobalQueries OBJECT-TYPE
        SYNTAX   Counter32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The number of responses sent to RIP queries
           from other systems."
       ::= { rip2Globals 2 }

--4.2 RIP Interface Tables

--  RIP Interfaces Groups
--  Implementation of these Groups is mandatory for systems
--  which implement RIP-2.

-- The RIP Interface Status Table.

    rip2IfStatTable OBJECT-TYPE
        SYNTAX   SEQUENCE OF Rip2IfStatEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
           "A list of subnets which require separate
           status monitoring in RIP."
       ::= { rip2 2 }

   rip2IfStatEntry OBJECT-TYPE
       SYNTAX   Rip2IfStatEntry
       MAX-ACCESS   not-accessible
       STATUS   current
       DESCRIPTION
          "A Single Routing Domain in a single Subnet."
      INDEX { rip2IfStatAddress }
      ::= { rip2IfStatTable 1 }

    Rip2IfStatEntry ::=
        SEQUENCE {
            rip2IfStatAddress
                IpAddress,
            rip2IfStatRcvBadPackets
                Counter32,
            rip2IfStatRcvBadRoutes
                Counter32,
            rip2IfStatSentUpdates
                Counter32,
            rip2IfStatStatus
                RowStatus
    }

    rip2IfStatAddress OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The IP Address of this system on the indicated
           subnet. For unnumbered interfaces, the value 0.0.0.N,
           where the least significant 24 bits (N) is the ifIndex
           for the IP Interface in network byte order."
       ::= { rip2IfStatEntry 1 }

    rip2IfStatRcvBadPackets OBJECT-TYPE
        SYNTAX   Counter32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The number of RIP response packets received by
           the RIP process which were subsequently discarded
           for any reason (e.g. a version 0 packet, or an
           unknown command type)."
       ::= { rip2IfStatEntry 2 }

    rip2IfStatRcvBadRoutes OBJECT-TYPE
        SYNTAX   Counter32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The number of routes, in valid RIP packets,
           which were ignored for any reason (e.g. unknown
           address family, or invalid metric)."
       ::= { rip2IfStatEntry 3 }

    rip2IfStatSentUpdates OBJECT-TYPE
        SYNTAX   Counter32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The number of triggered RIP updates actually
           sent on this interface.  This explicitly does
           NOT include full updates sent containing new
           information."
       ::= { rip2IfStatEntry 4 }

    rip2IfStatStatus OBJECT-TYPE
        SYNTAX   RowStatus
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "Writing invalid has the effect of deleting
           this interface."
       ::= { rip2IfStatEntry 5 }

-- The RIP Interface Configuration Table.

    rip2IfConfTable OBJECT-TYPE
        SYNTAX   SEQUENCE OF Rip2IfConfEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
           "A list of subnets which require separate
           configuration in RIP."
       ::= { rip2 3 }

   rip2IfConfEntry OBJECT-TYPE
       SYNTAX   Rip2IfConfEntry
       MAX-ACCESS   not-accessible
       STATUS   current
       DESCRIPTION
          "A Single Routing Domain in a single Subnet."
      INDEX { rip2IfConfAddress }
      ::= { rip2IfConfTable 1 }

    Rip2IfConfEntry ::=
        SEQUENCE {

            rip2IfConfAddress
                IpAddress,
            rip2IfConfDomain
                RouteTag,
            rip2IfConfAuthType
                INTEGER,
            rip2IfConfAuthKey
                OCTET STRING (SIZE(0..16)),
            rip2IfConfSend
                INTEGER,
            rip2IfConfReceive
                INTEGER,
            rip2IfConfDefaultMetric
                INTEGER,
            rip2IfConfStatus
                RowStatus,
            rip2IfConfSrcAddress
                IpAddress
    }

    rip2IfConfAddress OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The IP Address of this system on the indicated
           subnet.  For unnumbered interfaces, the value 0.0.0.N,
           where the least significant 24 bits (N) is the ifIndex
           for the IP Interface in network byte order."
       ::= { rip2IfConfEntry 1 }

    rip2IfConfDomain OBJECT-TYPE
        SYNTAX   RouteTag
        MAX-ACCESS   read-create
        STATUS   obsolete
        DESCRIPTION
           "Value inserted into the Routing Domain field
           of all RIP packets sent on this interface."
       DEFVAL { '0000'h }
       ::= { rip2IfConfEntry 2 }

    rip2IfConfAuthType OBJECT-TYPE
        SYNTAX   INTEGER {
                    noAuthentication (1),
                    simplePassword (2),
                    md5 (3)
                 }
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "The type of Authentication used on this
           interface."
       DEFVAL { noAuthentication }
       ::= { rip2IfConfEntry 3 }

    rip2IfConfAuthKey OBJECT-TYPE
        SYNTAX   OCTET STRING (SIZE(0..16))
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "The value to be used as the Authentication Key
           whenever the corresponding instance of
           rip2IfConfAuthType has a value other than
           noAuthentication.  A modification of the corresponding
           instance of rip2IfConfAuthType does not modify
           the rip2IfConfAuthKey value.  If a string shorter
           than 16 octets is supplied, it will be left-
           justified and padded to 16 octets, on the right,
           with nulls (0x00).

           Reading this object always results in an  OCTET
           STRING of length zero; authentication may not
           be bypassed by reading the MIB object."
       DEFVAL { ''h }
       ::= { rip2IfConfEntry 4 }

    rip2IfConfSend OBJECT-TYPE
        SYNTAX   INTEGER {
                    doNotSend (1),
                    ripVersion1 (2),
                    rip1Compatible (3),
                    ripVersion2 (4),
                    ripV1Demand (5),
                    ripV2Demand (6)
                 }
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "What the router sends on this interface.
           ripVersion1 implies sending RIP updates compliant
           with  RFC  1058.   rip1Compatible implies
           broadcasting RIP-2 updates using RFC 1058 route
           subsumption rules.  ripVersion2 implies
           multicasting RIP-2 updates.  ripV1Demand indicates
           the use of Demand RIP on a WAN interface under RIP
           Version 1 rules.  ripV2Demand indicates the use of

           Demand RIP on a WAN interface under Version 2 rules."
       DEFVAL { rip1Compatible }
       ::= { rip2IfConfEntry 5 }

    rip2IfConfReceive OBJECT-TYPE
        SYNTAX   INTEGER {
                    rip1 (1),
                    rip2 (2),
                    rip1OrRip2 (3),
                    doNotRecieve (4)
                 }
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "This indicates which version of RIP updates
           are to be accepted.  Note that rip2 and
           rip1OrRip2 implies reception of multicast
           packets."
       DEFVAL { rip1OrRip2 }
       ::= { rip2IfConfEntry 6 }

    rip2IfConfDefaultMetric OBJECT-TYPE
        SYNTAX   INTEGER ( 0..15 )
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "This variable indicates the metric that is to
           be used for the default route entry in RIP updates
           originated on this interface.  A value of zero
           indicates that no default route should be
           originated; in this case, a default route via
           another router may be propagated."
       ::= { rip2IfConfEntry 7 }

    rip2IfConfStatus OBJECT-TYPE
        SYNTAX   RowStatus
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "Writing invalid has  the  effect  of  deleting
           this interface."
       ::= { rip2IfConfEntry 8 }

    rip2IfConfSrcAddress OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-create
        STATUS   current
        DESCRIPTION
           "The IP Address this system will use as a source
            address on this interface.  If it is a numbered
            interface, this MUST be the same value as
            rip2IfConfAddress.  On unnumbered interfaces,
            it must be the value of rip2IfConfAddress for
            some interface on the system."
       ::= { rip2IfConfEntry 9 }

--4.3 Peer Table

--  Peer Table

--      The RIP Peer Group
--      Implementation of this Group is Optional

--      This group provides information about active peer
--      relationships intended to assist in debugging.  An
--      active peer is a router from which a valid RIP
--      updated has been heard in the last 180 seconds.

    rip2PeerTable OBJECT-TYPE
        SYNTAX   SEQUENCE OF Rip2PeerEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
           "A list of RIP Peers."
       ::= { rip2 4 }

   rip2PeerEntry OBJECT-TYPE
       SYNTAX   Rip2PeerEntry
       MAX-ACCESS   not-accessible
       STATUS   current
       DESCRIPTION
          "Information regarding a single routing peer."
      INDEX { rip2PeerAddress, rip2PeerDomain }
      ::= { rip2PeerTable 1 }

    Rip2PeerEntry ::=
        SEQUENCE {
            rip2PeerAddress
                IpAddress,
            rip2PeerDomain
                RouteTag,
            rip2PeerLastUpdate
                TimeTicks,
            rip2PeerVersion
                INTEGER,
            rip2PeerRcvBadPackets

                Counter32,
            rip2PeerRcvBadRoutes
                Counter32
            }

    rip2PeerAddress OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The IP Address that the peer is using as its source
            address.  Note that on an unnumbered link, this may
            not be a member of any subnet on the system."
       ::= { rip2PeerEntry 1 }

    rip2PeerDomain OBJECT-TYPE
        SYNTAX   RouteTag
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The value in the Routing Domain field  in  RIP
           packets received from the peer.  As domain suuport
           is deprecated, this must be zero."
       ::= { rip2PeerEntry 2 }

    rip2PeerLastUpdate OBJECT-TYPE
        SYNTAX   TimeTicks
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The value of sysUpTime when the most recent
           RIP update was received from this system."
       ::= { rip2PeerEntry 3 }

    rip2PeerVersion OBJECT-TYPE
        SYNTAX   INTEGER ( 0..255 )
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The RIP version number in the header of the
           last RIP packet received."
       ::= { rip2PeerEntry 4 }

    rip2PeerRcvBadPackets OBJECT-TYPE
        SYNTAX   Counter32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The number of RIP response packets from this
           peer discarded as invalid."
       ::= { rip2PeerEntry 5 }

    rip2PeerRcvBadRoutes OBJECT-TYPE
        SYNTAX   Counter32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The number of routes from this peer that were
           ignored because the entry format was invalid."
       ::= { rip2PeerEntry 6 }

-- conformance information

rip2Conformance OBJECT IDENTIFIER ::= { rip2 5 }

rip2Groups      OBJECT IDENTIFIER ::= { rip2Conformance 1 }
rip2Compliances OBJECT IDENTIFIER ::= { rip2Conformance 2 }

-- compliance statements
rip2Compliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
       "The compliance statement "
    MODULE  -- this module
    MANDATORY-GROUPS {
                 rip2GlobalGroup,
                 rip2IfStatGroup,
                 rip2IfConfGroup,
                 rip2PeerGroup
        }
    GROUP       rip2GlobalGroup
    DESCRIPTION
       "This group defines global controls for RIP-II systems."
    GROUP       rip2IfStatGroup
    DESCRIPTION
       "This group defines interface statistics for RIP-II systems."
    GROUP       rip2IfConfGroup
    DESCRIPTION
       "This group defines interface configuration for RIP-II systems."
    GROUP       rip2PeerGroup
    DESCRIPTION
       "This group defines peer information for RIP-II systems."
    ::= { rip2Compliances 1 }

-- units of conformance

rip2GlobalGroup    OBJECT-GROUP
    OBJECTS {
                rip2GlobalRouteChanges,
                rip2GlobalQueries
    }
    STATUS  current
    DESCRIPTION
       "This group defines global controls for RIP-II systems."
    ::= { rip2Groups 1 }
rip2IfStatGroup    OBJECT-GROUP
    OBJECTS {
            rip2IfStatAddress,
            rip2IfStatRcvBadPackets,
            rip2IfStatRcvBadRoutes,
            rip2IfStatSentUpdates,
            rip2IfStatStatus
    }
    STATUS  current
    DESCRIPTION
       "This group defines interface statistics for RIP-II systems."
    ::= { rip2Groups 2 }
rip2IfConfGroup    OBJECT-GROUP
    OBJECTS {
            rip2IfConfAddress,
            rip2IfConfAuthType,
            rip2IfConfAuthKey,
            rip2IfConfSend,
            rip2IfConfReceive,
            rip2IfConfDefaultMetric,
            rip2IfConfStatus,
            rip2IfConfSrcAddress
    }
    STATUS  current
    DESCRIPTION
       "This group defines interface configuration for RIP-II systems."
    ::= { rip2Groups 3 }
rip2PeerGroup    OBJECT-GROUP
    OBJECTS {
            rip2PeerAddress,
            rip2PeerDomain,
            rip2PeerLastUpdate,
            rip2PeerVersion,
            rip2PeerRcvBadPackets,
            rip2PeerRcvBadRoutes
    }
    STATUS  current
    DESCRIPTION
       "This group defines peer information for RIP-II systems."
    ::= { rip2Groups 4 }
END
