--
-- Juniper Enterprise Specific MIB: Vlan
--
-- Copyright (c) 2007-2008, Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--

JUNIPER-VLAN-MIB DEFINITIONS ::= BEGIN
    
IMPORTS
    Integer32, IpAddress, OBJECT-TYPE, MODULE-IDENTITY    
	FROM SNMPv2-SMI
    MacAddress, TruthValue, DisplayString             	
	FROM SNMPv2-TC
    InterfaceIndex 
	FROM IF-MIB
    InetAddress, InetAddressType, InetAddressPrefixLength
	FROM INET-ADDRESS-MIB
     Unsigned32
         FROM SNMPv2-SMI
    jnxExVlan                                       	
	FROM JUNIPER-EX-SMI;

jnxVlanMIBObjects  MODULE-IDENTITY
    LAST-UPDATED "200901090000Z" -- Fri Jan 09 00:00:00 2009 UTC
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "Juniper Technical Assistance Center
         Juniper Networks, Inc.
         1194 N. Mathilda Avenue
         Sunnyvale, CA 94089
         E-mail: support@juniper.net"
    DESCRIPTION
        "This module contains definitions for management information for 
	pre-standards IEEE 802.1Q VLANs and their association with a Lan 
	Emulation Client (lec). Devices implementing these pre-standards 
	maintain port groupings and associated filters used to form a 
	'virtual bridge'."
    REVISION   
        "200901090000Z" -- Fri Jan 09 00:00:00 2009 UTC
    DESCRIPTION
        "Marked the deprecated Objects of jnxVlanTable, 
         jnxVlanInterfaceTable and jnxVlanPortGroupTable 
         as Obsolete."
    REVISION
        "200901200000Z" -- Mon Jan 20 00:00:00 2009 UTC
    DESCRIPTION
        "Added new Object jnxExVlanTag to represent Vlan Tag information
         for each Vlan."
    REVISION
        "201009070000Z" -- Tue Sep 7 00:00:00 2010 UTC
    DESCRIPTION
        "Added new Objects jnxExVlanPortTagness and jnxExVlanPortAccessMode as
        part of jnxExVlanPortGroupTable."

    ::= { jnxExVlan 1 }

--------------------------------------------------------------------------------
-- VLAN Configuration
--------------------------------------------------------------------------------

jnxVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table of VLAN names and characteristics."
    ::= { jnxVlanMIBObjects 1 }

jnxVlanEntry OBJECT-TYPE
    SYNTAX      JnxVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table entry containing VLAN names and characteristics."
    INDEX   { IMPLIED jnxVlanName }
    ::= { jnxVlanTable 1 }

JnxVlanEntry ::=
    SEQUENCE {
        jnxVlanName               DisplayString,
	jnxVlanID                 Integer32,
        jnxVlanType               INTEGER,
        jnxVlanPortGroupInstance  Integer32,
        jnxVlanMacListInstance    Integer32
    }
     
jnxVlanName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..255)) 
    MAX-ACCESS  not-accessible 
    STATUS      obsolete
    DESCRIPTION
        "Vlan name is the textual name and this is the identifier
        that the user of a configuration utility will use."
    ::= {  jnxVlanEntry 1 }

jnxVlanID OBJECT-TYPE
    SYNTAX      Integer32(1..4094)
    MAX-ACCESS  read-only 
    STATUS      obsolete
    DESCRIPTION
        "This is the locally significant ID that is used internally by this 
	device to reference this VLAN."
    ::= { jnxVlanEntry 2 }

jnxVlanType OBJECT-TYPE
    SYNTAX 	INTEGER {
        static (1),
        dynamic(2)
    }
    MAX-ACCESS 	read-only
    STATUS      obsolete
    DESCRIPTION
        "The valn type can be
        static (1)
        Dynamic(2)"
    DEFVAL { 1 }
    ::= { jnxVlanEntry 3 }

jnxVlanPortGroupInstance OBJECT-TYPE
    SYNTAX 	Integer32
    MAX-ACCESS 	read-only
    STATUS      obsolete
    DESCRIPTION
        "jnxVlanPortGroupInstance is the index that identifies that the sub 
	tree in the jnxVlanPortGroupTable helps to retrieve the group of 
	ports in this VLAN."
    ::= { jnxVlanEntry 4 }

jnxVlanMacListInstance OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "jnxVlanMacListInstance is the index , if this is a MAC-based VLAN 
	which identifies the sub tree to retrieve the list of MAC address to 
	allow into this VLAN. If this is not a MAC-based VLAN then the 
	value is 0"
    DEFVAL { 0 }
    ::= { jnxVlanEntry 5 }

jnxVlanInterfaceTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF JnxVlanInterfaceEntry
     MAX-ACCESS  not-accessible
     STATUS      obsolete
     DESCRIPTION
         "A table of VLAN names and characteristics in layer 3."
     ::= { jnxVlanMIBObjects 2 }

jnxVlanInterfaceEntry OBJECT-TYPE
    SYNTAX      JnxVlanInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table entry containing VLAN names and characteristics in layer 3."
    INDEX   { IMPLIED jnxVlanName }
    ::= { jnxVlanInterfaceTable 1 }

JnxVlanInterfaceEntry ::=
    SEQUENCE {
        jnxVlanInterfaceIpAddress            InetAddress,
        jnxVlanInterfaceProtocol             InetAddressType,
        jnxVlanInterfaceSubNetMask           IpAddress,
        jnxVlanInterfaceBroadcastAddress     IpAddress,
        jnxVlanInterfaceDescription          DisplayString,
        jnxVlanInterfaceAdminStatus          TruthValue,
        jnxVlanInterfaceOperStatus           DisplayString,
        jnxVlanSnmpIfIndex		     InterfaceIndex 
    }

jnxVlanInterfaceIpAddress OBJECT-TYPE
     SYNTAX      InetAddress 
     MAX-ACCESS  read-only
     STATUS      obsolete
     DESCRIPTION
         "This specifies the IPAddress of this interface. "
     ::= { jnxVlanInterfaceEntry 1 }

jnxVlanInterfaceProtocol OBJECT-TYPE
    SYNTAX	InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
         "This specifies the protocol for ipv4."
    ::= { jnxVlanInterfaceEntry 2 }

jnxVlanInterfaceSubNetMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "This specifies the subnet mask address of the vlan ."
    ::= { jnxVlanInterfaceEntry 3 }

jnxVlanInterfaceBroadcastAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "This specifies the broadcast address of the vlan."
    ::= { jnxVlanInterfaceEntry 4 }

jnxVlanInterfaceDescription OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..255))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "jnxvlanInterfaceDescription provides the description for the vlan."
    ::= { jnxVlanInterfaceEntry 5 }

jnxVlanInterfaceAdminStatus OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "This takes care of administration status of the vlan"
    ::= { jnxVlanInterfaceEntry 6 }

jnxVlanInterfaceOperStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "This specifies the operational status of the vlan"
    ::= { jnxVlanInterfaceEntry 7 }

jnxVlanSnmpIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "This specifies the SNMP IF Index ."
    ::= { jnxVlanInterfaceEntry 8 }

-------------------------------------------------------------------------------
-- Port Group Table
--------------------------------------------------------------------------------

jnxVlanPortGroupTable OBJECT-TYPE
    SYNTAX  	SEQUENCE OF JnxVlanPortGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table of port groupings."
    ::= { jnxVlanMIBObjects 3 }

jnxVlanPortGroupEntry OBJECT-TYPE
    SYNTAX      JnxVlanPortGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table entry containing a port number"
    INDEX   { jnxVlanPortGroupIndex, jnxVlanPort }
    ::= { jnxVlanPortGroupTable 1 }

JnxVlanPortGroupEntry ::=
    SEQUENCE {
        jnxVlanPortGroupIndex      Integer32,
        jnxVlanPort                Integer32,
        jnxVlanPortStatus          INTEGER
    }

jnxVlanPortGroupIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Index used so that there can be many different
        port groups"
    ::= { jnxVlanPortGroupEntry 1 }

jnxVlanPort OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The vlanPort specifies the port in the vlan.By adding a port here,
        that port will now be part of any VLAN(s) that this port group is 
	associated with."
    ::= { jnxVlanPortGroupEntry 2 }

jnxVlanPortStatus OBJECT-TYPE
    SYNTAX      INTEGER {
        autoActive      (1),
        allowed         (2),
        allowedActive   (3),
        allowedNotAvail (4),
        notAssociated   (5)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The status of this port relative to the VLAN that points
        at this port group.[1.autoactive , 2.allowed, 3.allowedActive
        4.allowedNotAvail, 5.notAssociated]

        autoActive     : Means that the port is part of this VLAN
        	    	 because the switch automatically added it.
        allowed        : Means that the port has been configured so that
                    	 if all other criteria (if any) are met, this port
                    	 is allowed to be in this VLAN.
        allowedActive  : Means the same as allowed plus the fact
                       	 that there is a device attached to this port and
                       	 participating in the VLAN.
        allowedNotAvail: This value is only needed for devices
                         that don't allow a port to be in more than one
                         VLAN at a time.  This value means that this port
                         also exists in some other VLAN(s) and is active
                         in another VLAN.  Therefore this port is not
                         available to be used in this VLAN.
        notAssociated :  Means that the Port Group is not currently
                         associated with any VLAN."
    DEFVAL { allowed }
    ::= { jnxVlanPortGroupEntry 3 }

--------------------------------------------------------------------------------
-- MAC List Table
--------------------------------------------------------------------------------

jnxVlanMacListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxVlanMacListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "jnxVlanMacListTable is the table of MAC Lists. "
    ::= { jnxVlanMIBObjects 4 }

jnxVlanMacListEntry OBJECT-TYPE
    SYNTAX      JnxVlanMacListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table entry containing MAC Addresses"
    INDEX   { jnxVlanMacListIndex }
    ::= { jnxVlanMacListTable 1 }

JnxVlanMacListEntry ::=
    SEQUENCE {
        jnxVlanMacListIndex        Integer32,
        jnxVlanMacAddress          MacAddress
    }

jnxVlanMacListIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "jnxVlanMacListIndex can be used beacuse there can  be many different
        MAC Lists"
    ::= { jnxVlanMacListEntry 1 }

jnxVlanMacAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "jnxVlanMacAddress is the MAC Address that belongs to this group."
    ::= { jnxVlanMacListEntry 2 }

--------------------------------------------------------------------------------
-- Ex VLAN Configuration
--------------------------------------------------------------------------------

jnxExVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxExVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of VLAN names and characteristics."
    ::= { jnxVlanMIBObjects 5 }

jnxExVlanEntry OBJECT-TYPE
    SYNTAX      JnxExVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table entry containing VLAN names and characteristics."
    INDEX   { jnxExVlanID }
    ::= { jnxExVlanTable 1 }

JnxExVlanEntry ::=
    SEQUENCE {
        jnxExVlanID                 Integer32,
        jnxExVlanName               DisplayString,
        jnxExVlanType               INTEGER,
        jnxExVlanPortGroupInstance  Integer32,
        jnxExVlanTag                Unsigned32
    }

jnxExVlanID OBJECT-TYPE
    SYNTAX      Integer32(1..4094)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the locally significant ID that is used internally by this
        device to reference this VLAN."
    ::= { jnxExVlanEntry 1 }

jnxExVlanName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Vlan name is the textual name."
    ::= {  jnxExVlanEntry 2 }

jnxExVlanType OBJECT-TYPE
    SYNTAX      INTEGER {
        static (1),
        dynamic(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The vlan type can be
        static (1)
        Dynamic(2)"
    DEFVAL { 1 }
    ::= { jnxExVlanEntry 3 }

jnxExVlanPortGroupInstance OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "jnxExVlanPortGroupInstance is the index that identifies that the sub
        tree in the jnxVlanPortGroupTable helps to retrieve the group of
        ports in this VLAN."
    ::= { jnxExVlanEntry 4 }

jnxExVlanTag OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "jnxExVlanTag gives the Vlan Tag details for each Vlan."
    ::= { jnxExVlanEntry 5 }

--------------------------------------------------------------------------------
-- Ex VLAN Interface Table 
--------------------------------------------------------------------------------

jnxExVlanInterfaceTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF JnxExVlanInterfaceEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "A table of VLAN names and characteristics in layer 3."
     ::= { jnxVlanMIBObjects 6 }

jnxExVlanInterfaceEntry OBJECT-TYPE
    SYNTAX      JnxExVlanInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table entry containing VLAN names and characteristics in layer 3."
    INDEX   { jnxExVlanID }
    ::= { jnxExVlanInterfaceTable 1 }

JnxExVlanInterfaceEntry ::=
    SEQUENCE {
        jnxExVlanInterfaceProtocol             InetAddressType,
        jnxExVlanInterfaceIpAddress            InetAddress,
        jnxExVlanInterfacePrefixLength         InetAddressPrefixLength,
        jnxExVlanInterfaceBroadcastAddress     InetAddress,
        jnxExVlanInterfaceDescription          DisplayString,
        jnxExVlanInterfaceAdminStatus          INTEGER,
        jnxExVlanInterfaceOperStatus           INTEGER,
        jnxExVlanSnmpIfIndex                   InterfaceIndex
    }

jnxExVlanInterfaceProtocol OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "This specifies the protocol for ipv4."
    ::= { jnxExVlanInterfaceEntry 1 }

jnxExVlanInterfaceIpAddress OBJECT-TYPE
     SYNTAX      InetAddress
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
         "This specifies the IPAddress of this interface. "
     ::= { jnxExVlanInterfaceEntry 2 }

jnxExVlanInterfacePrefixLength OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This specifies the length of subnet mask address of the vlan ."
    ::= { jnxExVlanInterfaceEntry 3 }

jnxExVlanInterfaceBroadcastAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This specifies the broadcast address of the vlan."
    ::= { jnxExVlanInterfaceEntry 4 }

jnxExVlanInterfaceDescription OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "jnxExvlanInterfaceDescription provides the description for the vlan."
    ::= { jnxExVlanInterfaceEntry 5 }

jnxExVlanInterfaceAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    up(1),        -- ready to pass packets
                    down(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This takes care of administration status of the vlan"
    ::= { jnxExVlanInterfaceEntry 6 }

jnxExVlanInterfaceOperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    up(1),        -- ready to pass packets
                    down(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This specifies the operational status of the vlan"
    ::= { jnxExVlanInterfaceEntry 7 }

jnxExVlanSnmpIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This specifies the SNMP IF Index ."
    ::= { jnxExVlanInterfaceEntry 8 }

-------------------------------------------------------------------------------
-- Ex Port Group Table
--------------------------------------------------------------------------------

jnxExVlanPortGroupTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxExVlanPortGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of port groupings."
    ::= { jnxVlanMIBObjects 7 }

jnxExVlanPortGroupEntry OBJECT-TYPE
    SYNTAX      JnxExVlanPortGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table entry containing a port number"
    INDEX   { jnxExVlanPortGroupIndex, jnxExVlanPort }
    ::= { jnxExVlanPortGroupTable 1 }

JnxExVlanPortGroupEntry ::=
    SEQUENCE {
        jnxExVlanPortGroupIndex      Integer32,
        jnxExVlanPort                Integer32,
        jnxExVlanPortStatus          INTEGER,
        jnxExVlanPortTagness         INTEGER,
        jnxExVlanPortAccessMode      INTEGER
    }

jnxExVlanPortGroupIndex OBJECT-TYPE
    SYNTAX      Integer32(1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Index used so that there can be many different
        port groups"
    ::= { jnxExVlanPortGroupEntry 1 }

jnxExVlanPort OBJECT-TYPE
    SYNTAX      Integer32(1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vlanPort specifies the port in the vlan.By adding a port here,
        that port will now be part of any VLAN(s) that this port group is
        associated with."
    ::= { jnxExVlanPortGroupEntry 2 }

jnxExVlanPortStatus OBJECT-TYPE
    SYNTAX      INTEGER {
        autoActive      (1),
        allowed         (2),
        allowedActive   (3),
        allowedNotAvail (4),
        notAssociated   (5)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The status of this port relative to the VLAN that points
        at this port group.[1.autoactive , 2.allowed, 3.allowedActive
        4.allowedNotAvail, 5.notAssociated]

        autoActive     : Means that the port is part of this VLAN
                         because the switch automatically added it.
        allowed        : Means that the port has been configured so that
                         if all other criteria (if any) are met, this port
                         is allowed to be in this VLAN.
        allowedActive  : Means the same as allowed plus the fact
                         that there is a device attached to this port and
                         participating in the VLAN.
        allowedNotAvail: This value is only needed for devices
                         that don't allow a port to be in more than one
                         VLAN at a time.  This value means that this port
                         also exists in some other VLAN(s) and is active
                         in another VLAN.  Therefore this port is not
                         available to be used in this VLAN.
        notAssociated :  Means that the Port Group is not currently
                         associated with any VLAN."
    DEFVAL { allowed }
    ::= { jnxExVlanPortGroupEntry 3 }

jnxExVlanPortTagness  OBJECT-TYPE
    SYNTAX      INTEGER {
        tagged   (1),
        untagged (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VlanPortTaqness gives whether the Port is tagged or untagged."
    ::= { jnxExVlanPortGroupEntry 4 }

jnxExVlanPortAccessMode  OBJECT-TYPE
    SYNTAX      INTEGER {
        acces   (1),
        trunk   (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VlanPortAccessMode gives whether the Port is Access or Trunk."
    ::= { jnxExVlanPortGroupEntry 5 }

END

