-- ==================================================================
-- Copyright (C) 2009 by H3C Technologies.  All rights reserved.
--
-- Description: Lan Switch trap MIB
-- Reference:
-- Version: V1.1
-- History:
-- V1.0 Created by Zhangshilin, 2001.06.29
-- V1.1 Modified by lifengguang 2008.11.10, add trap node hh3cBootImageUpdated
-- ==================================================================

-- ==================================================================
--
-- Variables and types be imported
--
-- ==================================================================
HH3C-LswTRAP-MIB DEFINITIONS ::= BEGIN
IMPORTS
    MODULE-IDENTITY,NOTIFICATION-TYPE
        FROM SNMPv2-SMI

    hh3clswCommon
        FROM HH3C-OID-MIB

    hh3cDevMPowerNum, hh3cDevMFanNum
        FROM HH3C-LswDEVM-MIB

    hh3cLswFrameIndex, hh3cLswSlotIndex, hh3cLswSubslotIndex
        FROM HH3C-LSW-DEV-ADM-MIB;

-- ==================================================================
--
-- ======================= definition begin =========================
--
-- ==================================================================

     hh3cLswTrapMib MODULE-IDENTITY
            LAST-UPDATED "200106290000Z"
            ORGANIZATION
                "Hangzhou H3C Tech. Co., Ltd."
            CONTACT-INFO
                "Platform Team Hangzhou H3C Tech. Co., Ltd.
                Hai-Dian District Beijing P.R. China
                http://www.h3c.com
                Zip:100085
                "
            DESCRIPTION
            ""
            REVISION "200106290000Z"
            DESCRIPTION
            ""
            ::= { hh3clswCommon 12 }

    hh3csLswTRAPMibObject OBJECT IDENTIFIER ::= { hh3cLswTrapMib 1 }

    hh3cpowerfailure NOTIFICATION-TYPE
      OBJECTS { hh3cDevMPowerNum }
      STATUS  current
      DESCRIPTION
              "Power supply failure"
      ::= { hh3csLswTRAPMibObject 1 }

    hh3cPowerNormal NOTIFICATION-TYPE
      OBJECTS { hh3cDevMPowerNum }
      STATUS  current
      DESCRIPTION
              "Power supply normal"
      ::= { hh3csLswTRAPMibObject 2 }

    hh3cMasterPowerNormal NOTIFICATION-TYPE
      OBJECTS { hh3cDevMPowerNum }
      STATUS  current
      DESCRIPTION
              "Master power supply normal"
      ::= { hh3csLswTRAPMibObject 3 }

    hh3cSlavePowerNormal NOTIFICATION-TYPE
      OBJECTS { hh3cDevMPowerNum }
      STATUS  current
      DESCRIPTION
              "Slave power supply normal"
      ::= { hh3csLswTRAPMibObject 4 }

    hh3cPowerRemoved NOTIFICATION-TYPE
      OBJECTS { hh3cDevMPowerNum }
      STATUS  current
      DESCRIPTION
              "Power removed"
      ::= { hh3csLswTRAPMibObject 5 }

    hh3cfanfailure NOTIFICATION-TYPE
      OBJECTS { hh3cDevMFanNum }
      STATUS  current
      DESCRIPTION
              "Fan failure"
      ::= { hh3csLswTRAPMibObject 6 }

    hh3cFanNormal NOTIFICATION-TYPE
      OBJECTS { hh3cDevMFanNum }
      STATUS  current
      DESCRIPTION
              "Fan normal"
      ::= { hh3csLswTRAPMibObject 7 }

    hh3cBoardRemoved NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board removed"
      ::= { hh3csLswTRAPMibObject 8 }

    hh3cBoardInserted NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex,hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board inserted"
      ::= { hh3csLswTRAPMibObject 9 }

    hh3cBoardFailure NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board failed"
      ::= { hh3csLswTRAPMibObject 10 }

    hh3cBoardNormal NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board normal"
      ::= { hh3csLswTRAPMibObject 11 }

    hh3cSubcardRemove NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex, hh3cLswSubslotIndex }
      STATUS  current
      DESCRIPTION
              "Sub card removeed"
      ::= { hh3csLswTRAPMibObject 12 }

    hh3cSubcardInsert NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex, hh3cLswSubslotIndex }
      STATUS  current
      DESCRIPTION
              "Sub card inserted"
      ::= { hh3csLswTRAPMibObject 13 }

    hh3cBoardTemperatureLower NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board temperature low"
      ::= { hh3csLswTRAPMibObject 14 }

    hh3cBoardTemperatureFromLowerToNormal NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board temperature form lower to normal"
      ::= { hh3csLswTRAPMibObject 15 }

    hh3cBoardTemperatureHigher NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board temperature high"
      ::= { hh3csLswTRAPMibObject 16 }

    hh3cBoardTemperatureFormHigherToNormal NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board temperature from higher to normal"
      ::= { hh3csLswTRAPMibObject 17 }

    hh3cRequestLoading NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board request load"
      ::= { hh3csLswTRAPMibObject 18 }

    hh3cLoadFailure NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board load failure"
      ::= { hh3csLswTRAPMibObject 19 }

    hh3cLoadFinished NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "Board load finished"
      ::= { hh3csLswTRAPMibObject 20 }

    hh3cBackBoardModeSetFuilure NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex }
      STATUS  current
      DESCRIPTION
              "Back board mode set failure"
      ::= { hh3csLswTRAPMibObject 21 }

    hh3cBackBoardModeSetOK NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex }
      STATUS  current
      DESCRIPTION
              "Back board mode set OK"
      ::= { hh3csLswTRAPMibObject 22 }

    hh3cPowerInserted NOTIFICATION-TYPE
      OBJECTS { hh3cDevMPowerNum }
      STATUS  current
      DESCRIPTION
              "Power inserted"
      ::= { hh3csLswTRAPMibObject 23 }

    hh3cBootImageUpdated NOTIFICATION-TYPE
      OBJECTS { hh3cLswFrameIndex, hh3cLswSlotIndex }
      STATUS  current
      DESCRIPTION
              "This trap node indicates that the boot image of specified board
              is updated."
      ::= { hh3csLswTRAPMibObject 24 }

END
