RADLAN-UDP DEFINITIONS ::= BEGIN

-- Title:      UDP Private Extension
-- Version:    7.37.00.00
-- Date:       17 May 2004

IMPORTS
    rnd                                                     FROM RADLAN-MIB
    ipAddrEntry                                             FROM IP-MIB
    rip2IfConfEntry                                         FROM RFC1389-MIB
    ipCidrRouteEntry,ipCidrRouteDest,
    ipCidrRouteMask, ipCidrRouteTos, ipCidrRouteNextHop     FROM IP-FORWARD-MIB
    DisplayString                                           FROM SNMPv2-TC
    Unsigned32, Integer32, Counter32, IpAddress,
    MODULE-IDENTITY, OBJECT-TYPE                            FROM SNMPv2-SMI
    RowStatus, TruthValue, TEXTUAL-CONVENTION               FROM SNMPv2-TC;

rsUDP MODULE-IDENTITY
      LAST-UPDATED "200406010000Z"
      ORGANIZATION ""
      CONTACT-INFO
           ""
      DESCRIPTION
           "The private MIB module definition for UDP MIB."
      REVISION "200406010000Z"
      DESCRIPTION
           "Initial version of this MIB."
      ::= { rnd 42 }



rsUdpRelayTable  OBJECT-TYPE
   SYNTAX  SEQUENCE OF RsUdpRelayEntry
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       "This table contains the udp relay configuration per port."
   ::= {rsUDP 1}

rsUdpRelayEntry  OBJECT-TYPE
   SYNTAX     RsUdpRelayEntry
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       " The row definition for this table."

   INDEX {rsUdpRelayDstPort,
          rsUdpRelaySrcIpInf,
          rsUdpRelayDstIpAddr }
   ::= {rsUdpRelayTable 1}

RsUdpRelayEntry  ::= SEQUENCE {
    rsUdpRelayDstPort   INTEGER,
    rsUdpRelaySrcIpInf  IpAddress,
    rsUdpRelayDstIpAddr IpAddress,
    rsUdpRelayStatus    RowStatus,
    rsUdpRelayUserInfo  INTEGER
}

rsUdpRelayDstPort OBJECT-TYPE
   SYNTAX     INTEGER
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
       "The UDP port number in the UDP message header."
   ::= {rsUdpRelayEntry 1}

rsUdpRelaySrcIpInf OBJECT-TYPE
   SYNTAX      IpAddress
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
        "The source interface IP that receives UDP message.
         255.255.255.255 from all IP interface.
         0.0.0.0 - 0.255.255.255 and 127.0.0.0 - 127.255.255.255
         not relevant addresses."
--    DEFVAL  { 255.255.255.255 }
   ::= {rsUdpRelayEntry 2}

rsUdpRelayDstIpAddr OBJECT-TYPE
   SYNTAX      IpAddress
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
        "The destination IP address the UDP message will be forward.
         0.0.0.0 does not forward, 255.255.255.255 broadcasts to all
         addresses."
--    DEFVAL  { 255.255.255.255 }
   ::= {rsUdpRelayEntry 3}

rsUdpRelayStatus OBJECT-TYPE
   SYNTAX       RowStatus
   MAX-ACCESS  read-write
   STATUS       current
   DESCRIPTION
       "The status of a table entry.
        It is used to delete an entry from this table."
  ::= { rsUdpRelayEntry 4 }

rsUdpRelayUserInfo  OBJECT-TYPE
   SYNTAX      INTEGER
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
        "The information used for implementation purposes"
  DEFVAL  { 0 }
  ::= { rsUdpRelayEntry 5 }

rsUdpRelayMibVersion  OBJECT-TYPE
   SYNTAX      INTEGER
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
        "Mib version. The current version is 1."
   ::= {rsUDP 2}

END

