-- *******************************************************************
-- Juniper enterprise specific DHCP MIB.
--
-- Copyright (c) 2010-2011, Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
-- *******************************************************************

JUNIPER-JDHCP-MIB DEFINITIONS ::= BEGIN
IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, IpAddress, 
    Counter32, NOTIFICATION-TYPE, Unsigned32
        FROM SNMPv2-SMI
    ifIndex,InterfaceIndex
        FROM IF-MIB
    TEXTUAL-CONVENTION, DisplayString, DateAndTime, MacAddress
        FROM SNMPv2-TC 
    jnxJdhcpMibRoot
        FROM JUNIPER-SMI;

jnxJdhcpMIB  MODULE-IDENTITY
    LAST-UPDATED "201107090000Z" --  July 9, 2011
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
            "        Juniper Technical Assistance Center
                     Juniper Networks, Inc.
                     1194 N. Mathilda Avenue
                     Sunnyvale, CA 94089
                     E-mail: support@juniper.net"
    DESCRIPTION
        "The JUNOS DHCP MIB for the Juniper Networks enterprise."

    -- revision history
    REVISION      "201107090000Z"
    DESCRIPTION   "Add scalar for pkts dropped due to recovery in progress"
    REVISION      "201103150000Z"
    DESCRIPTION   "Add OIDs to the Interface Statistics Table"
    REVISION      "201101250000Z"
    DESCRIPTION   "Add Interface Statistics Table"
    REVISION      "201004190000Z"
    DESCRIPTION   "Creation Date"
    ::= { jnxJdhcpMibRoot 61 }
    

-- Managed object groups
jnxJdhcpLocalServerObjects   OBJECT IDENTIFIER ::= { jnxJdhcpMIB 1 }
jnxJdhcpRelayObjects         OBJECT IDENTIFIER ::= { jnxJdhcpMIB 2 }

-- Managed objects for DHCP Local Server
jnxJdhcpLocalServerStatistics OBJECT IDENTIFIER
    ::= { jnxJdhcpLocalServerObjects 1 }
jnxJdhcpLocalServerBindings   OBJECT IDENTIFIER
    ::= { jnxJdhcpLocalServerObjects 2 }
jnxJdhcpLocalServerTraps    OBJECT IDENTIFIER
    ::= { jnxJdhcpLocalServerObjects 3 }
jnxJdhcpLocalServerTrapVars   OBJECT IDENTIFIER 
    ::= { jnxJdhcpLocalServerObjects 4 }
jnxJdhcpLocalServerIfcStats   OBJECT IDENTIFIER
    ::= { jnxJdhcpLocalServerObjects 5 }

-- DHCP Local Server Statistics
jnxJdhcpLocalServerTotalDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped."
    ::= { jnxJdhcpLocalServerStatistics 1}

jnxJdhcpLocalServerBadHardwareDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped due to bad hardware address."
    ::= { jnxJdhcpLocalServerStatistics 2}

jnxJdhcpLocalServerBadBootpOpcodeDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to not BOOTP message."
    ::= { jnxJdhcpLocalServerStatistics 3}

jnxJdhcpLocalServerBadOptionsDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to bad options in the packet."
    ::= { jnxJdhcpLocalServerStatistics 4}

jnxJdhcpLocalServerBadAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to invalid server address."
    ::= { jnxJdhcpLocalServerStatistics 5}

jnxJdhcpLocalServerNoAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no available addresses."
    ::= { jnxJdhcpLocalServerStatistics 6}

jnxJdhcpLocalServerNoInterfaceDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no interface match."
    ::= { jnxJdhcpLocalServerStatistics 7}

jnxJdhcpLocalServerNoRoutingInstanceDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no routing instance match."
    ::= { jnxJdhcpLocalServerStatistics 8}

jnxJdhcpLocalServerNoLocalAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no valid local address."
    ::= {  jnxJdhcpLocalServerStatistics 9}

jnxJdhcpLocalServerShortPacketDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to packet too short."
    ::= { jnxJdhcpLocalServerStatistics 10}

jnxJdhcpLocalServerBadReadDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to send error."
    ::= { jnxJdhcpLocalServerStatistics 11}

jnxJdhcpLocalServerBadSendDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to send error."
    ::= { jnxJdhcpLocalServerStatistics 12}

jnxJdhcpLocalServerAuthenticationDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to authentication failure."
    ::= { jnxJdhcpLocalServerStatistics 13}

jnxJdhcpLocalServerDynamicProfileDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to dynamic profile error."
    ::= { jnxJdhcpLocalServerStatistics 14}

jnxJdhcpLocalServerLicenseDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to license error."
    ::= { jnxJdhcpLocalServerStatistics 15}

jnxJdhcpLocalServerBootRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Boot Request packets received."
    ::= { jnxJdhcpLocalServerStatistics 16}

jnxJdhcpLocalServerDhcpDeclineReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Decline packets received."
    ::= { jnxJdhcpLocalServerStatistics 17}

jnxJdhcpLocalServerDhcpDiscoverReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Discover packets received."
    ::= { jnxJdhcpLocalServerStatistics 18}

jnxJdhcpLocalServerDhcpInformReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP inform packets received."
    ::= { jnxJdhcpLocalServerStatistics 19}

jnxJdhcpLocalServerDhcpReleaseReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP release packets received."
    ::= { jnxJdhcpLocalServerStatistics 20}

jnxJdhcpLocalServerDhcpRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP request packets received."
    ::= { jnxJdhcpLocalServerStatistics 21}

jnxJdhcpLocalServerDhcpBootReplySent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Boot Reply packets sent."
    ::= { jnxJdhcpLocalServerStatistics 22}

jnxJdhcpLocalServerDhcpOfferSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Offer packets sent."
    ::= { jnxJdhcpLocalServerStatistics 23}

jnxJdhcpLocalServerDhcpAckSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Ack packets sent."
    ::= { jnxJdhcpLocalServerStatistics 24}

jnxJdhcpLocalServerDhcpNakSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Nak packets sent."
    ::= { jnxJdhcpLocalServerStatistics 25}

jnxJdhcpLocalServerForceRenewSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Force Renew packets sent."
    ::= { jnxJdhcpLocalServerStatistics 26}

jnxJdhcpLocalServerTotalLeaseCount OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Bound DHCP Clients."
    ::= { jnxJdhcpLocalServerStatistics 27}

jnxJdhcpLocalServerSwitchDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to switchover recovery in progress."
    ::= { jnxJdhcpLocalServerStatistics 28}


-- DHCP Local Server Bindings Table

jnxJdhcpLocalServerBindingsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxJdhcpLocalServerBindingsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of address bindings maintained by this JUNOS DHCP Local Server."
    ::= { jnxJdhcpLocalServerBindings 1 }

jnxJdhcpLocalServerBindingsEntry OBJECT-TYPE
    SYNTAX      JnxJdhcpLocalServerBindingsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) representing an address binding (client) maintained by
        this JUNOS DHCP Local Server."
    INDEX     { jnxJdhcpLocalServerBindingsIpAddress }
    ::= { jnxJdhcpLocalServerBindingsTable 1 }

JnxJdhcpLocalServerBindingsEntry ::= SEQUENCE {
    jnxJdhcpLocalServerBindingsIpAddress                    IpAddress,
    jnxJdhcpLocalServerBindingsMacAddress                   MacAddress,
    jnxJdhcpLocalServerBindingsState                        INTEGER,
    jnxJdhcpLocalServerBindingsLeaseEndTime                 DateAndTime,
    jnxJdhcpLocalServerBindingsLeaseExpireTime              Unsigned32,
    jnxJdhcpLocalServerBindingsLeaseStartTime               DateAndTime,
    jnxJdhcpLocalServerBindingsIncomingClientInterface      DisplayString,
    jnxJdhcpLocalServerBindingsClientInterfaceVlanId        Unsigned32,
    jnxJdhcpLocalServerBindingsDemuxInterfaceName           DisplayString,
    jnxJdhcpLocalServerBindingsServerIpAddress              IpAddress,
    jnxJdhcpLocalServerBindingsBootpRelayAddress            IpAddress,
    jnxJdhcpLocalServerBindingsPreviousBootpRelayAddress    IpAddress,
    jnxJdhcpLocalServerBindingsClientPoolName               DisplayString,
    jnxJdhcpLocalServerBindingsClientProfileName            DisplayString
    }

jnxJdhcpLocalServerBindingsIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address associated with this entry in the bindings table."
    ::= { jnxJdhcpLocalServerBindingsEntry 1 }

jnxJdhcpLocalServerBindingsMacAddress OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC Address associated with this entry in the bindings
        table and corresponding to the IP Address denoted by the table index."
    ::= { jnxJdhcpLocalServerBindingsEntry 2 }

jnxJdhcpLocalServerBindingsState OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    init(1),
                    selecting(2),
                    requesting(3),
                    release(4),
                    bound(5),
                    renewing(6),
                    rebinding(7)  }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The state associated with this entry in the bindings table."
    ::= { jnxJdhcpLocalServerBindingsEntry 3 }

jnxJdhcpLocalServerBindingsLeaseEndTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time the lease expires on this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 4 }

jnxJdhcpLocalServerBindingsLeaseExpireTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time remaining until the lease expires for this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 5 }

jnxJdhcpLocalServerBindingsLeaseStartTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time the lease was started for this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 6 }

jnxJdhcpLocalServerBindingsIncomingClientInterface OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The incoming interface for this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 7 }

jnxJdhcpLocalServerBindingsClientInterfaceVlanId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VLAN ID for this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 8 }

jnxJdhcpLocalServerBindingsDemuxInterfaceName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The demux interface for this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 9 }

jnxJdhcpLocalServerBindingsServerIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP Address associated with the server for this entry in the bindings table."
    ::= { jnxJdhcpLocalServerBindingsEntry 10 }

jnxJdhcpLocalServerBindingsBootpRelayAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The BOOTP relay Address associated with the server for this entry in the bindings table."
    ::= { jnxJdhcpLocalServerBindingsEntry 11 }

jnxJdhcpLocalServerBindingsPreviousBootpRelayAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Previous BOOTP relay Address associated with the server for this entry in the bindings table."
    ::= { jnxJdhcpLocalServerBindingsEntry 12 }

jnxJdhcpLocalServerBindingsClientPoolName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The client pool name for this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 13 }

jnxJdhcpLocalServerBindingsClientProfileName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The client pool name for this binding."
    ::= { jnxJdhcpLocalServerBindingsEntry 14 }

-- DHCP Local Server Interface Statistics Table

jnxJdhcpLocalServerIfcStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxJdhcpLocalServerIfcStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of interface statistics maintained by this JUNOS DHCP Local Server."
    ::= { jnxJdhcpLocalServerIfcStats 1 }

jnxJdhcpLocalServerIfcStatsEntry OBJECT-TYPE
    SYNTAX      JnxJdhcpLocalServerIfcStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) representing an address binding (client) maintained by
        this JUNOS DHCP Local Server."
    INDEX     { jnxJdhcpLocalServerIfcStatsIfIndex }
    ::= { jnxJdhcpLocalServerIfcStatsTable 1 }

JnxJdhcpLocalServerIfcStatsEntry ::= SEQUENCE {
    jnxJdhcpLocalServerIfcStatsIfIndex                     InterfaceIndex,
    jnxJdhcpLocalServerIfcStatsTotalDropped                Counter32,
    jnxJdhcpLocalServerIfcStatsBadHardwareDropped          Counter32,
    jnxJdhcpLocalServerIfcStatsBadBootpOpcodeDropped       Counter32,
    jnxJdhcpLocalServerIfcStatsBadOptionsDropped           Counter32,
    jnxJdhcpLocalServerIfcStatsBadAddressDropped           Counter32,
    jnxJdhcpLocalServerIfcStatsNoAddressDropped            Counter32,
    jnxJdhcpLocalServerIfcStatsNoInterfaceCfgDropped       Counter32,
    jnxJdhcpLocalServerIfcStatsNoLocalAddressDropped       Counter32,
    jnxJdhcpLocalServerIfcStatsShortPacketDropped          Counter32,
    jnxJdhcpLocalServerIfcStatsBadSendDropped              Counter32,
    jnxJdhcpLocalServerIfcStatsAuthenticationDropped       Counter32,
    jnxJdhcpLocalServerIfcStatsDynamicProfileDropped       Counter32,
    jnxJdhcpLocalServerIfcStatsLicenseDropped              Counter32,
    jnxJdhcpLocalServerIfcStatsBootRequestReceived         Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpDeclineReceived         Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpDiscoverReceived        Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpInformReceived          Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpReleaseReceived         Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpRequestReceived         Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpBootReplySent           Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpOfferSent               Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpAckSent                 Counter32,
    jnxJdhcpLocalServerIfcStatsDhcpNakSent                 Counter32,
    jnxJdhcpLocalServerIfcStatsForceRenewSent              Counter32,
    jnxJdhcpLocalServerIfcStatsTotalLeaseCount             Counter32,
    jnxJdhcpLocalServerIfcStatsBadDhcpOpcodeDropped        Counter32,
    jnxJdhcpLocalServerIfcStatsNoOptionsDropped            Counter32,
    jnxJdhcpLocalServerIfcStatsHopLimitDropped             Counter32,
    jnxJdhcpLocalServerIfcStatsTtlExpiredDropped           Counter32,
    jnxJdhcpLocalServerIfcStatsBadUdpCksumDropped          Counter32,
    jnxJdhcpLocalServerIfcStatsOption60Dropped             Counter32
    }

-- According to IF-MIB.txt and interface index is an Integer 32 (1 - 2147483647) 
-- This will correlate with an IFL in DHCP

jnxJdhcpLocalServerIfcStatsIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The ifIndex value of the interface for which this entry
            contains information."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 1}

jnxJdhcpLocalServerIfcStatsTotalDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 2}

jnxJdhcpLocalServerIfcStatsBadHardwareDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped due to bad hardware address."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 3}

jnxJdhcpLocalServerIfcStatsBadBootpOpcodeDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to not BOOTP message."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 4}

jnxJdhcpLocalServerIfcStatsBadOptionsDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to bad options in the packet."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 5}

jnxJdhcpLocalServerIfcStatsBadAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to invalid server address."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 6}

jnxJdhcpLocalServerIfcStatsNoAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no available addresses."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 7}

jnxJdhcpLocalServerIfcStatsNoInterfaceCfgDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no interface match."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 8}

jnxJdhcpLocalServerIfcStatsNoLocalAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no valid local address."
    ::= {  jnxJdhcpLocalServerIfcStatsEntry 9}

jnxJdhcpLocalServerIfcStatsShortPacketDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to packet too short."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 10}

jnxJdhcpLocalServerIfcStatsBadSendDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to send error."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 11}

jnxJdhcpLocalServerIfcStatsAuthenticationDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to authentication failure."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 12}

jnxJdhcpLocalServerIfcStatsDynamicProfileDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to dynamic profile error."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 13}

jnxJdhcpLocalServerIfcStatsLicenseDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to license error."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 14}

jnxJdhcpLocalServerIfcStatsBootRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Boot Request packets received."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 15}

jnxJdhcpLocalServerIfcStatsDhcpDeclineReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Decline packets received."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 16}

jnxJdhcpLocalServerIfcStatsDhcpDiscoverReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Discover packets received."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 17}

jnxJdhcpLocalServerIfcStatsDhcpInformReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP inform packets received."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 18}

jnxJdhcpLocalServerIfcStatsDhcpReleaseReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP release packets received."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 19}

jnxJdhcpLocalServerIfcStatsDhcpRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP request packets received."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 20}

jnxJdhcpLocalServerIfcStatsDhcpBootReplySent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Boot Reply packets sent."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 21}

jnxJdhcpLocalServerIfcStatsDhcpOfferSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Offer packets sent."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 22}

jnxJdhcpLocalServerIfcStatsDhcpAckSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Ack packets sent."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 23}

jnxJdhcpLocalServerIfcStatsDhcpNakSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Nak packets sent."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 24}

jnxJdhcpLocalServerIfcStatsForceRenewSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Force Renew packets sent."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 25}

jnxJdhcpLocalServerIfcStatsTotalLeaseCount OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Bound DHCP Clients."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 26}

jnxJdhcpLocalServerIfcStatsBadDhcpOpcodeDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped with bad DHCP opcode."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 27}

jnxJdhcpLocalServerIfcStatsNoOptionsDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped with no options."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 28}

jnxJdhcpLocalServerIfcStatsHopLimitDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to hop limit violation."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 29}

jnxJdhcpLocalServerIfcStatsTtlExpiredDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to ttl expiration."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 30}

jnxJdhcpLocalServerIfcStatsBadUdpCksumDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to bad UDP checksum."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 31}

jnxJdhcpLocalServerIfcStatsOption60Dropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to bad option 60."
    ::= { jnxJdhcpLocalServerIfcStatsEntry 32}


-- Managed objects for DHCP Relay
jnxJdhcpRelayStatistics OBJECT IDENTIFIER
    ::= { jnxJdhcpRelayObjects 1 }
jnxJdhcpRelayBindings   OBJECT IDENTIFIER
    ::= { jnxJdhcpRelayObjects 2 }
jnxJdhcpRelayTraps    OBJECT IDENTIFIER
    ::= { jnxJdhcpRelayObjects 3 }
jnxJdhcpRelayTrapVars   OBJECT IDENTIFIER 
    ::= { jnxJdhcpRelayObjects 4 }
jnxJdhcpRelayIfcStats   OBJECT IDENTIFIER
    ::= { jnxJdhcpRelayObjects 5 }

-- DHCP RelayStatistics
jnxJdhcpRelayTotalDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped."
    ::= { jnxJdhcpRelayStatistics 1}

jnxJdhcpRelayBadHardwareDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped due to bad hardware address."
    ::= { jnxJdhcpRelayStatistics 2}

jnxJdhcpRelayBadBootpOpcodeDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to not BOOTP message."
    ::= { jnxJdhcpRelayStatistics 3}

jnxJdhcpRelayBadOptionsDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to bad options in the packet."
    ::= { jnxJdhcpRelayStatistics 4}

jnxJdhcpRelayBadAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to invalid server address."
    ::= { jnxJdhcpRelayStatistics 5}

jnxJdhcpRelayNoAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no available addresses."
    ::= { jnxJdhcpRelayStatistics 6}

jnxJdhcpRelayNoInterfaceDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no interface match."
    ::= { jnxJdhcpRelayStatistics 7}

jnxJdhcpRelayNoRoutingInstanceDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no routing instance match."
    ::= { jnxJdhcpRelayStatistics 8}

jnxJdhcpRelayNoLocalAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no valid local address."
    ::= {  jnxJdhcpRelayStatistics 9}

jnxJdhcpRelayShortPacketDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to packet too short."
    ::= { jnxJdhcpRelayStatistics 10}

jnxJdhcpRelayBadReadDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to read error."
    ::= { jnxJdhcpRelayStatistics 11}

jnxJdhcpRelayBadSendDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to send error."
    ::= { jnxJdhcpRelayStatistics 12}

jnxJdhcpRelayOption82Dropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to failure to add Option 82."
    ::= { jnxJdhcpRelayStatistics 13}

jnxJdhcpRelayOption60Dropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to configure to drop."
    ::= { jnxJdhcpRelayStatistics 14}

jnxJdhcpRelayAuthenticationDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to authentication failure."
    ::= { jnxJdhcpRelayStatistics 15}

jnxJdhcpRelayDynamicProfileDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to dynamic profile error."
    ::= { jnxJdhcpRelayStatistics 16}

jnxJdhcpRelayLicenseDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to license error."
    ::= { jnxJdhcpRelayStatistics 17}

jnxJdhcpRelayBootRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Boot Request packets received."
    ::= { jnxJdhcpRelayStatistics 18}

jnxJdhcpRelayDhcpDeclineReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Decline packets received."
    ::= { jnxJdhcpRelayStatistics 19}

jnxJdhcpRelayDhcpDiscoverReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Discover packets received."
    ::= { jnxJdhcpRelayStatistics 20}

jnxJdhcpRelayDhcpInformReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP inform packets received."
    ::= { jnxJdhcpRelayStatistics 21}

jnxJdhcpRelayDhcpReleaseReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP release packets received."
    ::= { jnxJdhcpRelayStatistics 22}

jnxJdhcpRelayDhcpRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP request packets received."
    ::= { jnxJdhcpRelayStatistics 23}

jnxJdhcpRelayDhcpBootReplySent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Boot Reply packets sent."
    ::= { jnxJdhcpRelayStatistics 24}

jnxJdhcpRelayDhcpOfferSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Offer packets sent."
    ::= { jnxJdhcpRelayStatistics 25}

jnxJdhcpRelayDhcpAckSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Ack packets sent."
    ::= { jnxJdhcpRelayStatistics 26}

jnxJdhcpRelayDhcpNakSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Nak packets sent."
    ::= { jnxJdhcpRelayStatistics 27}

jnxJdhcpRelayForceRenewSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Force Renew packets sent."
    ::= { jnxJdhcpRelayStatistics 28}

jnxJdhcpRelayTotalLeaseCount OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Bound DHCP Clients."
    ::= { jnxJdhcpRelayStatistics 29}

jnxJdhcpRelaySwitchDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to switchover recovery in progress."
    ::= { jnxJdhcpRelayStatistics 30}

-- DHCP Relay Bindings Table

jnxJdhcpRelayBindingsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxJdhcpRelayBindingsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of address bindings maintained by this JUNOS DHCP Relay."
    ::= { jnxJdhcpRelayBindings 1 }

jnxJdhcpRelayBindingsEntry OBJECT-TYPE
    SYNTAX      JnxJdhcpRelayBindingsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) representing an address binding (client) maintained by
        this JUNOS DHCP Relay."
    INDEX     { jnxJdhcpRelayBindingsIpAddress }
    ::= { jnxJdhcpRelayBindingsTable 1 }

JnxJdhcpRelayBindingsEntry ::= SEQUENCE {
    jnxJdhcpRelayBindingsIpAddress                    IpAddress,
    jnxJdhcpRelayBindingsLeaseState                   INTEGER,
    jnxJdhcpRelayBindingsLeaseEndTime                 DateAndTime,
    jnxJdhcpRelayBindingsLeaseExpireTime              Unsigned32,
    jnxJdhcpRelayBindingsLeaseStartTime               DateAndTime,
    jnxJdhcpRelayBindingsIncomingClientInterface      DisplayString,
    jnxJdhcpRelayBindingsClientInterfaceVlanId        Unsigned32,
    jnxJdhcpRelayBindingsDemuxInterfaceName           DisplayString,
    jnxJdhcpRelayBindingsServerIpAddress              IpAddress,
    jnxJdhcpRelayBindingsServerInterface              DisplayString,
    jnxJdhcpRelayBindingsBootpRelayAddress            IpAddress,
    jnxJdhcpRelayBindingsPreviousBootpRelayAddress    IpAddress,
    jnxJdhcpRelayBindingsClientProfileName            DisplayString
    }

jnxJdhcpRelayBindingsIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address associated with this entry in the bindings table."
    ::= { jnxJdhcpRelayBindingsEntry 1 }

jnxJdhcpRelayBindingsLeaseState OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    init(1),
                    selecting(2),
                    requesting(3),
                    release(4),
                    bound(5),
                    renewing(6),
                    rebinding(7)  }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The state associated with this entry in the bindings table."
    ::= { jnxJdhcpRelayBindingsEntry 2 }

jnxJdhcpRelayBindingsLeaseEndTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time the lease expires on this binding."
    ::= { jnxJdhcpRelayBindingsEntry 3 }

jnxJdhcpRelayBindingsLeaseExpireTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time remaining until the lease expires for this binding."
    ::= { jnxJdhcpRelayBindingsEntry 4 }

jnxJdhcpRelayBindingsLeaseStartTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time the lease was started for this binding."
    ::= { jnxJdhcpRelayBindingsEntry 5 }

jnxJdhcpRelayBindingsIncomingClientInterface OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The incoming interface or this binding."
    ::= { jnxJdhcpRelayBindingsEntry 6 }

jnxJdhcpRelayBindingsClientInterfaceVlanId  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VLAN ID for this binding."
    ::= { jnxJdhcpRelayBindingsEntry 7 }

jnxJdhcpRelayBindingsDemuxInterfaceName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The demux interface for this binding."
    ::= { jnxJdhcpRelayBindingsEntry 8 }

jnxJdhcpRelayBindingsServerIpAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address associated with the server for this entry in the bindings table."
    ::= { jnxJdhcpRelayBindingsEntry 9 }

jnxJdhcpRelayBindingsServerInterface  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The demux interface for this binding."
    ::= { jnxJdhcpRelayBindingsEntry 10 }

jnxJdhcpRelayBindingsBootpRelayAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address associated with the Bootp Relay for this entry in the bindings table."
    ::= { jnxJdhcpRelayBindingsEntry 11 }

jnxJdhcpRelayBindingsPreviousBootpRelayAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address associated with the Previous Bootp Relay for this entry in the bindings table."
    ::= { jnxJdhcpRelayBindingsEntry 12 }

jnxJdhcpRelayBindingsClientProfileName  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The display client profile name."
    ::= { jnxJdhcpRelayBindingsEntry 13 }

-- DHCP Relay Interface Statistics Table

jnxJdhcpRelayIfcStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxJdhcpRelayIfcStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of interface statistics maintained by this JUNOS DHCP Relay."
    ::= { jnxJdhcpRelayIfcStats 1 }

jnxJdhcpRelayIfcStatsEntry OBJECT-TYPE
    SYNTAX      JnxJdhcpRelayIfcStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) representing an address binding (client) maintained by
        this JUNOS DHCP Relay."
    INDEX     { jnxJdhcpRelayIfcStatsIfIndex }
    ::= { jnxJdhcpRelayIfcStatsTable 1 }

JnxJdhcpRelayIfcStatsEntry ::= SEQUENCE {
    jnxJdhcpRelayIfcStatsIfIndex                     InterfaceIndex,
    jnxJdhcpRelayIfcStatsTotalDropped                Counter32,
    jnxJdhcpRelayIfcStatsBadHardwareDropped          Counter32,
    jnxJdhcpRelayIfcStatsBadBootpOpcodeDropped       Counter32,
    jnxJdhcpRelayIfcStatsBadOptionsDropped           Counter32,
    jnxJdhcpRelayIfcStatsBadAddressDropped           Counter32,
    jnxJdhcpRelayIfcStatsNoAddressDropped            Counter32,
    jnxJdhcpRelayIfcStatsNoInterfaceCfgDropped       Counter32,
    jnxJdhcpRelayIfcStatsNoLocalAddressDropped       Counter32,
    jnxJdhcpRelayIfcStatsShortPacketDropped          Counter32,
    jnxJdhcpRelayIfcStatsBadSendDropped              Counter32,
    jnxJdhcpRelayIfcStatsAuthenticationDropped       Counter32,
    jnxJdhcpRelayIfcStatsDynamicProfileDropped       Counter32,
    jnxJdhcpRelayIfcStatsLicenseDropped              Counter32,
    jnxJdhcpRelayIfcStatsBootRequestReceived         Counter32,
    jnxJdhcpRelayIfcStatsDhcpDeclineReceived         Counter32,
    jnxJdhcpRelayIfcStatsDhcpDiscoverReceived        Counter32,
    jnxJdhcpRelayIfcStatsDhcpInformReceived          Counter32,
    jnxJdhcpRelayIfcStatsDhcpReleaseReceived         Counter32,
    jnxJdhcpRelayIfcStatsDhcpRequestReceived         Counter32,
    jnxJdhcpRelayIfcStatsDhcpBootReplySent           Counter32,
    jnxJdhcpRelayIfcStatsDhcpOfferSent               Counter32,
    jnxJdhcpRelayIfcStatsDhcpAckSent                 Counter32,
    jnxJdhcpRelayIfcStatsDhcpNakSent                 Counter32,
    jnxJdhcpRelayIfcStatsForceRenewSent              Counter32,
    jnxJdhcpRelayIfcStatsTotalLeaseCount             Counter32,
    jnxJdhcpRelayIfcStatsBadDhcpOpcodeDropped        Counter32,
    jnxJdhcpRelayIfcStatsNoOptionsDropped            Counter32,
    jnxJdhcpRelayIfcStatsHopLimitDropped             Counter32,
    jnxJdhcpRelayIfcStatsTtlExpiredDropped           Counter32,
    jnxJdhcpRelayIfcStatsBadUdpCksumDropped          Counter32,
    jnxJdhcpRelayIfcStatsOption82Dropped             Counter32
    }

jnxJdhcpRelayIfcStatsIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The ifIndex value of the interface for which this entry
            contains information."
    ::= { jnxJdhcpRelayIfcStatsEntry 1}

jnxJdhcpRelayIfcStatsTotalDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped."
    ::= { jnxJdhcpRelayIfcStatsEntry 2}

jnxJdhcpRelayIfcStatsBadHardwareDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets dropped due to bad hardware address."
    ::= { jnxJdhcpRelayIfcStatsEntry 3}

jnxJdhcpRelayIfcStatsBadBootpOpcodeDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to not BOOTP message."
    ::= { jnxJdhcpRelayIfcStatsEntry 4}

jnxJdhcpRelayIfcStatsBadOptionsDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to bad options in the packet."
    ::= { jnxJdhcpRelayIfcStatsEntry 5}

jnxJdhcpRelayIfcStatsBadAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to invalid server address."
    ::= { jnxJdhcpRelayIfcStatsEntry 6}

jnxJdhcpRelayIfcStatsNoAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no available addresses."
    ::= { jnxJdhcpRelayIfcStatsEntry 7}

jnxJdhcpRelayIfcStatsNoInterfaceCfgDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no interface match."
    ::= { jnxJdhcpRelayIfcStatsEntry 8}

jnxJdhcpRelayIfcStatsNoLocalAddressDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to no valid local address."
    ::= {  jnxJdhcpRelayIfcStatsEntry 9}

jnxJdhcpRelayIfcStatsShortPacketDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to packet too short."
    ::= { jnxJdhcpRelayIfcStatsEntry 10}

jnxJdhcpRelayIfcStatsBadSendDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to send error."
    ::= { jnxJdhcpRelayIfcStatsEntry 11}

jnxJdhcpRelayIfcStatsAuthenticationDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to authentication failure."
    ::= { jnxJdhcpRelayIfcStatsEntry 12}

jnxJdhcpRelayIfcStatsDynamicProfileDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to dynamic profile error."
    ::= { jnxJdhcpRelayIfcStatsEntry 13}

jnxJdhcpRelayIfcStatsLicenseDropped OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to license error."
    ::= { jnxJdhcpRelayIfcStatsEntry 14}

jnxJdhcpRelayIfcStatsBootRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Boot Request packets received."
    ::= { jnxJdhcpRelayIfcStatsEntry 15}

jnxJdhcpRelayIfcStatsDhcpDeclineReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Decline packets received."
    ::= { jnxJdhcpRelayIfcStatsEntry 16}

jnxJdhcpRelayIfcStatsDhcpDiscoverReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Discover packets received."
    ::= { jnxJdhcpRelayIfcStatsEntry 17}

jnxJdhcpRelayIfcStatsDhcpInformReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP inform packets received."
    ::= { jnxJdhcpRelayIfcStatsEntry 18}

jnxJdhcpRelayIfcStatsDhcpReleaseReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP release packets received."
    ::= { jnxJdhcpRelayIfcStatsEntry 19}

jnxJdhcpRelayIfcStatsDhcpRequestReceived OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP request packets received."
    ::= { jnxJdhcpRelayIfcStatsEntry 20}

jnxJdhcpRelayIfcStatsDhcpBootReplySent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Boot Reply packets sent."
    ::= { jnxJdhcpRelayIfcStatsEntry 21}

jnxJdhcpRelayIfcStatsDhcpOfferSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Offer packets sent."
    ::= { jnxJdhcpRelayIfcStatsEntry 22}

jnxJdhcpRelayIfcStatsDhcpAckSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Ack packets sent."
    ::= { jnxJdhcpRelayIfcStatsEntry 23}

jnxJdhcpRelayIfcStatsDhcpNakSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Nak packets sent."
    ::= { jnxJdhcpRelayIfcStatsEntry 24}

jnxJdhcpRelayIfcStatsForceRenewSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of DHCP Force Renew packets sent."
    ::= { jnxJdhcpRelayIfcStatsEntry 25}

jnxJdhcpRelayIfcStatsTotalLeaseCount OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of Bound DHCP Clients."
    ::= { jnxJdhcpRelayIfcStatsEntry 26}

jnxJdhcpRelayIfcStatsBadDhcpOpcodeDropped  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped with bad DHCP opcode."
    ::= { jnxJdhcpRelayIfcStatsEntry 27}

jnxJdhcpRelayIfcStatsNoOptionsDropped  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped with no options."
    ::= { jnxJdhcpRelayIfcStatsEntry 28}

jnxJdhcpRelayIfcStatsHopLimitDropped  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to hop limit violation."
    ::= { jnxJdhcpRelayIfcStatsEntry 29}

jnxJdhcpRelayIfcStatsTtlExpiredDropped  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to ttl expiration."
    ::= { jnxJdhcpRelayIfcStatsEntry 30}

jnxJdhcpRelayIfcStatsBadUdpCksumDropped  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to bad UDP checksum."
    ::= { jnxJdhcpRelayIfcStatsEntry 31}

jnxJdhcpRelayIfcStatsOption82Dropped  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to failure to add Option 82."
    ::= { jnxJdhcpRelayIfcStatsEntry 32}

-- Objects used for traps
jnxJdhcpLocalServerLastDetected  OBJECT-TYPE
    SYNTAX       DateAndTime
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "The time the duplicate client was last detected"
    ::= { jnxJdhcpLocalServerTrapVars 1 }

jnxJdhcpRouterName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..257))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The VRF ID in JUNOS. Represented as the Logical Router (LR)
         Name followed by the Router Instance (RI) Name."
    ::= { jnxJdhcpLocalServerTrapVars 2 }

jnxJdhcpLocalServerMacAddress  OBJECT-TYPE
    SYNTAX       MacAddress
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "The MAC address of the client that changed interfaces."
    ::= { jnxJdhcpLocalServerTrapVars 3 }

jnxJdhcpLocalServerInterfaceName  OBJECT-TYPE
    SYNTAX       DisplayString
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "The interface where the DHCP client was detected"
    ::= { jnxJdhcpLocalServerTrapVars 4 }

jnxJdhcpLocalServerInterfaceLimit  OBJECT-TYPE
    SYNTAX       Unsigned32
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "The number of clients supported on this interface."
    ::= { jnxJdhcpLocalServerTrapVars 5 }

jnxJdhcpLocalServerEventSeverity OBJECT-TYPE
    SYNTAX      INTEGER {
                    debug(0),
                    warning(1),
                    critical(2)
                }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The level of error. "
    ::= { jnxJdhcpLocalServerTrapVars 6 }

jnxJdhcpLocalServerEventString  OBJECT-TYPE
    SYNTAX       DisplayString
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "The text of the event string associated with the health event."
    ::= { jnxJdhcpLocalServerTrapVars 7 }

jnxJdhcpRelayRouterName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..257))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The VRF ID in JUNOS. Represented as the Logical Router (LR)
         Name followed by the Router Instance (RI) Name."
    ::= { jnxJdhcpRelayTrapVars 1 }

jnxJdhcpRelayInterfaceName  OBJECT-TYPE
    SYNTAX       DisplayString
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "The interface where the DHCP client was detected"
    ::= { jnxJdhcpRelayTrapVars 2 }

jnxJdhcpRelayInterfaceLimit  OBJECT-TYPE
    SYNTAX       Unsigned32
    MAX-ACCESS   accessible-for-notify
    STATUS       current
    DESCRIPTION
        "The number of clients supported on this interface."
    ::= { jnxJdhcpRelayTrapVars 3 }


-- Notifications

jnxJdhcpLocalServerDuplicateClient  NOTIFICATION-TYPE
    OBJECTS {
        jnxJdhcpRouterName,
        jnxJdhcpLocalServerMacAddress,
        jnxJdhcpLocalServerInterfaceName,
        jnxJdhcpLocalServerLastDetected }
    STATUS      current
    DESCRIPTION
        "Reports the first occurance of detection of a DHCP client that
         changed interfaces."
    ::= { jnxJdhcpLocalServerTraps 1 }

jnxJdhcpLocalServerInterfaceLimitExceeded  NOTIFICATION-TYPE
    OBJECTS {
        jnxJdhcpRouterName,
        jnxJdhcpLocalServerInterfaceName,
        jnxJdhcpLocalServerInterfaceLimit }
    STATUS      current
    DESCRIPTION
        "Reports when the limit of clients has been exceeded on an interface."
    ::= { jnxJdhcpLocalServerTraps 2 }

jnxJdhcpLocalServerInterfaceLimitAbated  NOTIFICATION-TYPE
    OBJECTS {
        jnxJdhcpRouterName,
        jnxJdhcpLocalServerInterfaceName,
        jnxJdhcpLocalServerInterfaceLimit }
    STATUS      current
    DESCRIPTION
        "Reports when the number of clients on an interface has fallen
        below the limit allowed on that interface."
    ::= { jnxJdhcpLocalServerTraps 3 }

jnxJdhcpLocalServerHealth NOTIFICATION-TYPE
    OBJECTS {
        jnxJdhcpRouterName,
        jnxJdhcpLocalServerEventSeverity,
        jnxJdhcpLocalServerEventString }
    STATUS      current
    DESCRIPTION
        "Reports when a health event occurs in the Local Server 
         application."
    ::= { jnxJdhcpLocalServerTraps 4 }

-- Relay Notifications

jnxJdhcpRelayInterfaceLimitExceeded  NOTIFICATION-TYPE
    OBJECTS {
        jnxJdhcpRelayRouterName,
        jnxJdhcpRelayInterfaceName,
        jnxJdhcpRelayInterfaceLimit }
    STATUS      current
    DESCRIPTION
        "Reports when the limit of clients has been exceeded on an interface."
    ::= { jnxJdhcpRelayTraps 1 }

jnxJdhcpRelayInterfaceLimitAbated  NOTIFICATION-TYPE
    OBJECTS {
        jnxJdhcpRelayRouterName,
        jnxJdhcpRelayInterfaceName,
        jnxJdhcpRelayInterfaceLimit }
    STATUS      current
    DESCRIPTION
        "Reports when the number of clients on an interface has fallen
        below the limit allowed on that interface."
    ::= { jnxJdhcpRelayTraps 2 }


END


