JNX-IPSEC-MONITOR-MIB DEFINITIONS ::= BEGIN

      IMPORTS
         MODULE-IDENTITY, OBJECT-TYPE, Counter32, Counter64, Integer32, Unsigned32
           FROM SNMPv2-SMI
         InetAddress, InetAddressType
           FROM INET-ADDRESS-MIB
         TEXTUAL-CONVENTION, DisplayString, TimeInterval
           FROM SNMPv2-TC
         jnxMibs
           FROM JUNIPER-SMI
        jnxSpSvcSetName 
           FROM JUNIPER-SP-MIB;
      jnxIpSecMonitorMIB MODULE-IDENTITY
         LAST-UPDATED "201202102100Z" --  2012 UTC      
         ORGANIZATION "Juniper Networks, Inc."
         CONTACT-INFO
                "Juniper Technical Assistance Center
                      Juniper Networks, Inc.
                      1194 N. Mathilda Avenue
                      Sunnyvale, CA 94089
                      E-mail: support@juniper.net"
	     DESCRIPTION " "
         REVISION "201202102100Z"
         DESCRIPTION
                   "Initial version implements only the following
                    tables:
                    - IKE tunnel table
                    - IPSec tunnel table
                    - IPSec security associations table
                    "

         ::= { jnxMibs 22 } 


   -- +++++++++++++++++++++++++++++++++++++++++++++++++++
   -- Local Textual Conventions
   -- +++++++++++++++++++++++++++++++++++++++++++++++++++


      JnxIkePeerType  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of IPsec Phase-1 IKE peer identity.
            The IKE peer may be identified by one of the
            ID types defined in IPSEC DOI."
         SYNTAX INTEGER {
                   unknown(0),
                   idIpv4Addr(1),
                   idFqdn(2),
                   idDn(3)
         }

      JnxIkeNegoMode  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The IPsec Phase-1 IKE negotiation mode."
         SYNTAX INTEGER {
                   main(1),
                   aggressive(2),
                   ikev2(3)
         }

      JnxIkeHashAlgo   ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The hash algorithm used in IPsec Phase-1
            IKE negotiations."
         SYNTAX INTEGER {
                   md5(1),
                   sha(2),
                   sha256(3)
         }

      JnxIkeAuthMethod ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The authentication method used in IPsec Phase-1 IKE
             negotiations."
         SYNTAX INTEGER {
                   preSharedKey(1),
                   dssSignature(2),
                   rsaSignature(3),
                   rsaEncryption(4),
                   revRsaEncryption(5)
         }

      JnxIkePeerRole ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "Role of the local endpoint in negotiating the IPsec Phase-1 IKE
             security association. It can be either Initiator or Responder."
         SYNTAX INTEGER {
                   initiator(1),
                   responder(2)
         }

      JnxIkeNegState ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "State of the Phase-1 IKE negotiation."
         SYNTAX INTEGER {
                   matured(1),
                   notmatured(2)
         }


      JnxDiffHellmanGrp ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The Diffie Hellman Group used in negotiations.
                   modp768        -- 768-bit MODP
                   modp1024       -- 1024-bit MODP
                   modp1536       -- 1536-bit MODP
                   modp2048       -- 2048-bit MODP
            "
         SYNTAX INTEGER {
                   unknown(0),
                   modp768(1),
                   modp1024(2),
                   modp1536(5),
                   modp2048(14)
         }

      JnxKeyType    ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of key used by an IPsec Phase-2 Tunnel."
         SYNTAX INTEGER{
                  unknown(0),
                  keyIke(1),
                  keyManual(2)
         }

      JnxEncapMode  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The encapsulation mode used by an IPsec Phase-2
            Tunnel."
         SYNTAX INTEGER{
                  unknown(0),
                  tunnel(1),
                  transport(2)
         }

      JnxEncryptAlgo   ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The encryption algorithm used in negotiations."
         SYNTAX INTEGER {
                   espDes(1),
                   esp3des(2),
                   espNull(3),
                   espAes128 (4),  
                   espAes192 (5),
                   espAes256 (6)
         }

      JnxSpi  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of the SPI associated with IPsec Phase-2 security
            associations."
         SYNTAX Unsigned32 (256..4294967295)
      -- Umesh  SYNTAX INTEGER (256..4294967295)

      JnxAuthAlgo      ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The authentication algorithm used by a
             security association of an IPsec Phase-2 Tunnel."
         SYNTAX INTEGER{
                   unknown(0),
                   hmacMd5(2),
                   hmacSha(3),
                   hmacSha256(4)
         }

      JnxRemotePeerType  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of the remote peer gateway (endpoint). It can be one
             of the following two types:
               - static (Remote peer whose IP address is known beforehand)
               - dynamic (Remote peer whose IP address is not known
                          beforehand)"
         SYNTAX INTEGER {
                   unknown(0),
                   static(1),
                   dynamic(2)
         }

      JnxSAType   ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "SA Type manual or dynamic"
         SYNTAX INTEGER {
                   unknown(0),
                   manual(1),
                   dynamic(2)
         }
      


   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- IPsec MIB Object Groups
   --
   -- This MIB module contains the following groups:
   -- 1) IPsec Levels Group
   -- 2) IPsec Phase-1 Group
   -- 3) IPsec Phase-2 Group
   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++

      jnxIpSecMIBObjects OBJECT IDENTIFIER  
	                 ::= {jnxIpSecMonitorMIB 1}
      jnxIpSecLevels OBJECT IDENTIFIER
                     ::= { jnxIpSecMIBObjects 1 }
      jnxIpSecPhaseOne OBJECT IDENTIFIER
                     ::= { jnxIpSecMIBObjects 2 }
      jnxIpSecPhaseTwo OBJECT IDENTIFIER
                     ::= { jnxIpSecMIBObjects 3 }

   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- IPsec Levels Group
   --
   -- This group consists of a:
   -- 1) IPsec MIB Level
   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++

      jnxIpSecMibLevel OBJECT-TYPE
         SYNTAX Integer32 (1..4096)
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The version of the IPsec MIB."
         ::= { jnxIpSecLevels 1 }

   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- The IPsec Phase-1 Internet Key Exchange Tunnel Table
   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
   
      jnxIkeTunnelTable OBJECT-TYPE
         SYNTAX SEQUENCE OF JnxIkeTunnelEntry
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "The IPsec Phase-1 Internet Key Exchange Tunnel Table.
             There is one entry in this table for each active IPsec
             Phase-1 IKE Tunnel."
        ::= { jnxIpSecPhaseOne 1 }

      jnxIkeTunnelEntry OBJECT-TYPE
         SYNTAX JnxIkeTunnelEntry
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
               "Each entry contains the attributes associated with
                an active IPsec Phase-1 IKE Tunnel."
         INDEX { jnxSpSvcSetName, -- From the jnxSpSvcSetTable
                 jnxIkeTunRemoteGwAddrType,
                 jnxIkeTunRemoteGwAddr,
                 jnxIkeTunIndex }
         ::= { jnxIkeTunnelTable 1}

      JnxIkeTunnelEntry ::= SEQUENCE {
         jnxIkeTunIndex                 Integer32,
         jnxIkeTunLocalRole             JnxIkePeerRole,    
         jnxIkeTunNegState              JnxIkeNegState,    
         jnxIkeTunInitiatorCookie       DisplayString,
         jnxIkeTunResponderCookie       DisplayString,

         jnxIkeTunLocalIdType           JnxIkePeerType,
         jnxIkeTunLocalIdValue          DisplayString,
         jnxIkeTunLocalGwAddrType       InetAddressType,
         jnxIkeTunLocalGwAddr           InetAddress,
         jnxIkeTunLocalCertName         DisplayString,
         jnxIkeTunRemoteIdType          JnxIkePeerType,
         jnxIkeTunRemoteIdValue         DisplayString,
         jnxIkeTunRemoteGwAddrType      InetAddressType,
         jnxIkeTunRemoteGwAddr          InetAddress,
         jnxIkeTunNegoMode              JnxIkeNegoMode,
         jnxIkeTunDiffHellmanGrp        JnxDiffHellmanGrp,
         jnxIkeTunEncryptAlgo           JnxEncryptAlgo,
         jnxIkeTunHashAlgo              JnxIkeHashAlgo,
         jnxIkeTunAuthMethod            JnxIkeAuthMethod,
         jnxIkeTunLifeTime              Integer32,
         jnxIkeTunActiveTime            TimeInterval,

         jnxIkeTunInOctets              Counter64,
         jnxIkeTunInPkts                Counter32,
         jnxIkeTunOutOctets             Counter64,
         jnxIkeTunOutPkts               Counter32
      }

      jnxIkeTunIndex OBJECT-TYPE
         SYNTAX Integer32 (1..2147483647)
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "The index of the IPsec Phase-1 IKE Tunnel Table.
             The value of the index is a number which begins
             at one and is incremented with each tunnel that
             is created. The value of this object will
             wrap at 2,147,483,647."
         ::= { jnxIkeTunnelEntry 1 }

      jnxIkeTunLocalRole OBJECT-TYPE
         SYNTAX JnxIkePeerRole
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The role of local peer identity.  The Role of 
			the local peer can be:
             1. initiator.
             2. or responder."
         ::= { jnxIkeTunnelEntry 2 }

      jnxIkeTunNegState OBJECT-TYPE
         SYNTAX JnxIkeNegState
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The state of the current negotiation , It can be 
			1. matured
			2. not matured "
         ::= { jnxIkeTunnelEntry 3 }
		 
      jnxIkeTunInitiatorCookie OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Cookie as generated by the peer that initiated the IKE Phase-1
             negotiation. This cookie is carried in the ISAKMP header."
         ::= { jnxIkeTunnelEntry 4 }

      jnxIkeTunResponderCookie OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Cookie as generated by the peer responding to the IKE Phase-1
             negotiation initiated by the remote peer. This cookie is carried
             in the ISAKMP header."
         ::= { jnxIkeTunnelEntry 5 }
		 
      jnxIkeTunLocalIdType OBJECT-TYPE
         SYNTAX JnxIkePeerType
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The type of local peer identity.  The local
            peer may be identified by:
             1. an IP address, or
             2. or a fully qualified domain name string.
             3. or a distinguished name string."
         ::= { jnxIkeTunnelEntry 6 }

      jnxIkeTunLocalIdValue OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The value of the local peer identity.

             If the local peer type is an IP Address, then this
             is the IP Address used to identify the local peer.

             If the local peer type is id_fqdn, then this is
             the FQDN of the remote peer.

             If the local peer type is a id_dn, then this is
             the distinguished name string of the local peer."
         ::= { jnxIkeTunnelEntry 7 }

      jnxIkeTunLocalGwAddrType OBJECT-TYPE
         SYNTAX InetAddressType
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address type of the local endpoint (gateway) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelEntry 8 }

      jnxIkeTunLocalGwAddr OBJECT-TYPE
         SYNTAX InetAddress
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address of the local endpoint (gateway) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelEntry 9 }

      jnxIkeTunLocalCertName OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "Name of the certificate used for authentication of the local
             tunnel endpoint. This object will have some valid value only
             if negotiated IKE authentication method is other than pre-saherd
             key. If the IKE negotiation do not use certificate based
             authentication method, then the value of this object will be a
             NULL string."  
         ::= { jnxIkeTunnelEntry 10 }

      jnxIkeTunRemoteIdType OBJECT-TYPE
         SYNTAX JnxIkePeerType
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The type of remote peer identity.
            The remote peer may be identified by:
             1. an IP address, or
             2. or a fully qualified domain name string.
             3. or a distinguished name string."
         ::= { jnxIkeTunnelEntry 11 }

      jnxIkeTunRemoteIdValue OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The value of the remote peer identity.

             If the remote peer type is an IP Address, then this
             is the IP Address used to identify the remote peer.

             If the remote peer type is id_fqdn, then this is
             the FQDN of the remote peer.

             If the remote peer type is a id_dn, then this is
             the distinguished named string of the remote peer."
         ::= { jnxIkeTunnelEntry 12 }

      jnxIkeTunRemoteGwAddrType OBJECT-TYPE
         SYNTAX InetAddressType
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address type of the remote gateway (endpoint) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelEntry 13 }

      jnxIkeTunRemoteGwAddr OBJECT-TYPE
         SYNTAX InetAddress
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address of the remote gateway (endpoint) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelEntry 14 }

      jnxIkeTunNegoMode OBJECT-TYPE
         SYNTAX JnxIkeNegoMode
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The negotiation mode of the IPsec Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelEntry 15 }

      jnxIkeTunDiffHellmanGrp OBJECT-TYPE
         SYNTAX JnxDiffHellmanGrp
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The Diffie Hellman Group used in IPsec Phase-1 IKE
             negotiations."
         ::= { jnxIkeTunnelEntry 16 }

      jnxIkeTunEncryptAlgo OBJECT-TYPE
         SYNTAX JnxEncryptAlgo
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The encryption algorithm used in IPsec Phase-1 IKE
             negotiations."
         ::= { jnxIkeTunnelEntry 17 }

      jnxIkeTunHashAlgo OBJECT-TYPE
         SYNTAX JnxIkeHashAlgo
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The hash algorithm used in IPsec Phase-1 IKE
             negotiations."
         ::= { jnxIkeTunnelEntry 18 }

      jnxIkeTunAuthMethod OBJECT-TYPE
         SYNTAX JnxIkeAuthMethod
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The authentication method used in IPsec Phase-1 IKE
             negotiations."
         ::= { jnxIkeTunnelEntry 19 }

      jnxIkeTunLifeTime OBJECT-TYPE
         SYNTAX Integer32 (1..2147483647)
         UNITS "seconds"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The negotiated LifeTime of the IPsec Phase-1 IKE Tunnel
             in seconds."
         ::= { jnxIkeTunnelEntry 20 }

      jnxIkeTunActiveTime OBJECT-TYPE
         SYNTAX TimeInterval
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The length of time the IPsec Phase-1 IKE tunnel has been
             active in hundredths of seconds."
         ::= { jnxIkeTunnelEntry 21 }

      jnxIkeTunInOctets OBJECT-TYPE
         SYNTAX Counter64
         UNITS "Octets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The total number of octets received by
            this IPsec Phase-1 IKE security association."
         ::= { jnxIkeTunnelEntry 22 }

      jnxIkeTunInPkts OBJECT-TYPE
         SYNTAX Counter32
         UNITS "Packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The total number of packets received by
            this IPsec Phase-1 IKE security association."
         ::= { jnxIkeTunnelEntry 23 }

      jnxIkeTunOutOctets OBJECT-TYPE
         SYNTAX Counter64
         UNITS "Octets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The total number of octets sent by this IPsec Phase-1
             IKE security association."
         ::= { jnxIkeTunnelEntry 24 }

      jnxIkeTunOutPkts OBJECT-TYPE
         SYNTAX Counter32
         UNITS "Packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The total number of packets sent by this IPsec Phase-1
             IKE security association."
         ::= { jnxIkeTunnelEntry 25 }





   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- The IPsec Phase-2 Tunnel Table
   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
      jnxIpSecTunnelTable OBJECT-TYPE
         SYNTAX SEQUENCE OF JnxIpSecTunnelEntry
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "The IPsec Phase-2 Tunnel Table.
            There is one entry in this table for
            each active IPsec Phase-2 Tunnel."
         ::= { jnxIpSecPhaseTwo 1 }

      jnxIpSecTunnelEntry OBJECT-TYPE
         SYNTAX JnxIpSecTunnelEntry
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "Each entry contains the attributes
            associated with an active IPsec Phase-2 Tunnel."
         INDEX {jnxSpSvcSetName, -- From the jnxSpSvcSetTable
                jnxIpSecTunRemoteGwAddrType,
                jnxIpSecTunRemoteGwAddr,
                jnxIpSecTunIndex }
         ::= { jnxIpSecTunnelTable 1 }

      JnxIpSecTunnelEntry ::= SEQUENCE {
         jnxIpSecTunIndex                Integer32,
         jnxIpSecRuleName                DisplayString,
         jnxIpSecTermName                DisplayString,
         jnxIpSecTunLocalGwAddrType      InetAddressType,
         jnxIpSecTunLocalGwAddr          InetAddress,
         jnxIpSecTunRemoteGwAddrType     InetAddressType,
         jnxIpSecTunRemoteGwAddr         InetAddress,
         jnxIpSecTunLocalProxyId         DisplayString,
         jnxIpSecTunRemoteProxyId        DisplayString,
         jnxIpSecTunKeyType              JnxKeyType,
         jnxIpSecRemotePeerType          JnxRemotePeerType,   
         jnxIpSecTunMtu                  Integer32,

         jnxIpSecTunOutEncryptedBytes    Counter64,
         jnxIpSecTunOutEncryptedPkts     Counter64,
         jnxIpSecTunInDecryptedBytes     Counter64,
         jnxIpSecTunInDecryptedPkts      Counter64,

         jnxIpsSecTunAHInBytes           Counter64,
         jnxIpsSecTunAHInPkts            Counter64,
         jnxIpsSecTunAHOutBytes          Counter64,
         jnxIpsSecTunAHOutPkts           Counter64,

         jnxIpSecTunReplayDropPkts       Counter64,
         jnxIpSecTunAhAuthFails          Counter64,
         jnxIpSecTunEspAuthFails         Counter64,
         jnxIpSecTunDecryptFails         Counter64,
         jnxIpSecTunBadHeaders           Counter64,
         jnxIpSecTunBadTrailers          Counter64,
         jnxIpSecTunDroppedPkts          Counter64	
      }											

       jnxIpSecTunIndex OBJECT-TYPE
         SYNTAX Integer32 (1..2147483647)
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "The index of the IPsec Phase-2 Tunnel Table.
             The value of the index is a number which begins
             at one and is incremented with each tunnel that
             is created. The value of this object will wrap
             at 2,147,483,647."
         ::= { jnxIpSecTunnelEntry 1 }

       jnxIpSecRuleName OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Name of the rule configured in IPSec configuration."
         ::= { jnxIpSecTunnelEntry 2 }

       jnxIpSecTermName OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Name of the term configured under IPSec rule."
         ::= { jnxIpSecTunnelEntry 3 }
		 
       jnxIpSecTunLocalGwAddrType OBJECT-TYPE
         SYNTAX InetAddressType
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address type of the local gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelEntry 4 }

       jnxIpSecTunLocalGwAddr OBJECT-TYPE
         SYNTAX InetAddress
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address of the local gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelEntry 5 }

      jnxIpSecTunRemoteGwAddrType OBJECT-TYPE
         SYNTAX InetAddressType
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address type of the remote gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelEntry 6 }

      jnxIpSecTunRemoteGwAddr OBJECT-TYPE
         SYNTAX InetAddress
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The IP address of the remote gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelEntry 7 }

      jnxIpSecTunLocalProxyId OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Identifier for the local end."
         ::= { jnxIpSecTunnelEntry 8 }

      jnxIpSecTunRemoteProxyId OBJECT-TYPE
         SYNTAX DisplayString
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Identifier for the remote end."
         ::= { jnxIpSecTunnelEntry 9 }
		 
      jnxIpSecTunKeyType OBJECT-TYPE
         SYNTAX JnxKeyType
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "The type of key used by the IPsec Phase-2 Tunnel. It can be
             one of the following two types:
               - IKE negotiated
               - Manually installed"
         ::= { jnxIpSecTunnelEntry 10 }

      jnxIpSecRemotePeerType OBJECT-TYPE
         SYNTAX JnxRemotePeerType
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The type of the remote peer gateway (endpoint). It can be one
             of the following two types:
               - static (Remote peer whose IP address is known beforehand)
               - dynamic (Remote peer whose IP address is not known
                          beforehand)"
         ::= { jnxIpSecTunnelEntry 11 }
		 

      jnxIpSecTunMtu OBJECT-TYPE
         SYNTAX Integer32
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "MTU value of this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 12 }
		 

      jnxIpSecTunOutEncryptedBytes OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of bytes encrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 13 }
		 

      jnxIpSecTunOutEncryptedPkts OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets encrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 14 }
		 

      jnxIpSecTunInDecryptedBytes OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of bytes decrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 15 }
		 

      jnxIpSecTunInDecryptedPkts OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets decrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 16 }
		 

      jnxIpsSecTunAHInBytes OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of incoming bytes authenticated using AH by this Phase-2
             tunnel."
         ::= { jnxIpSecTunnelEntry 17 }
		 

      jnxIpsSecTunAHInPkts OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of incoming packets authenticated using AH by this Phase-2
             tunnel."
         ::= { jnxIpSecTunnelEntry 18 }
		 

      jnxIpsSecTunAHOutBytes OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of outgoing bytes applied AH by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 19 }
		 

      jnxIpsSecTunAHOutPkts OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of outgoing packets applied AH by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 20 }
		 
      jnxIpSecTunReplayDropPkts OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets dropped by this Phase-2 tunnel due to
             anti replay check failure."
         ::= { jnxIpSecTunnelEntry 21 }
		 

      jnxIpSecTunAhAuthFails OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed AH authentication."
         ::= { jnxIpSecTunnelEntry 22 }
		 

      jnxIpSecTunEspAuthFails OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed ESP authentication."
         ::= { jnxIpSecTunnelEntry 23 }
		 

      jnxIpSecTunDecryptFails OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed decryption."
         ::= { jnxIpSecTunnelEntry 24 }
		 

      jnxIpSecTunBadHeaders OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed due to bad headers."
         ::= { jnxIpSecTunnelEntry 25 }
		 
      jnxIpSecTunBadTrailers OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed due to bad ESP trailers."
         ::= { jnxIpSecTunnelEntry 26 }
		 
      jnxIpSecTunDroppedPkts  OBJECT-TYPE
         SYNTAX Counter64
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "Total number of dropped packets for this Phase-2 tunnel."
         ::= { jnxIpSecTunnelEntry 27 }
		 




   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- The IPsec Phase-2 Security Association Table
   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++

      jnxIpSecSaTable OBJECT-TYPE
         SYNTAX SEQUENCE OF JnxIpSecSaEntry
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "The IPsec Phase-2 Security Association Table.
            This table identifies the structure (in terms of
            component SAs) of each active Phase-2 IPsec tunnel.
            This table contains an entry for each active and
            expiring security association and maps each entry
            in the active Phase-2 tunnel table (ipSecTunTable)
            into a number of entries in this table. The index of this
            table reflects the

                <destination-address, protocol, spi>

            rule for identifying Security Associations."
         ::= { jnxIpSecPhaseTwo 2 }

      jnxIpSecSaEntry OBJECT-TYPE
         SYNTAX JnxIpSecSaEntry
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "Each entry contains the attributes associated with
             active and expiring IPsec Phase-2
             security associations."
         INDEX { jnxSpSvcSetName,          -- From jnxSpSvcSetTable
                 jnxIpSecTunRemoteGwAddrType, -- From ipSecTunnelTable
                 jnxIpSecTunRemoteGwAddr,     -- From ipSecTunnelTable
                 jnxIpSecTunIndex,            -- From ipSecTunnelTable
                 jnxIpSecSaIndex  }
         ::= { jnxIpSecSaTable 1 }

      JnxIpSecSaEntry ::= SEQUENCE {
         jnxIpSecSaProtocol              INTEGER,	  
         jnxIpSecSaIndex                 Integer32,
         jnxIpSecSaInSpi                 JnxSpi,		  
         jnxIpSecSaOutSpi                JnxSpi,		  
         jnxIpSecSaInAuxSpi              JnxSpi,
         jnxIpSecSaOutAuxSpi             JnxSpi,
         jnxIpSecSaType                  JnxSAType,
         jnxIpSecSaEncapMode             JnxEncapMode,
         jnxIpSecSaLifeSize              Integer32,
         jnxIpSecSaLifeTime              Integer32,
         jnxIpSecSaActiveTime            TimeInterval,
         jnxIpSecSaLifeSizeThreshold     Integer32,  
         jnxIpSecSaLifeTimeThreshold     Integer32, 
         jnxIpSecSaEncryptAlgo           JnxEncryptAlgo,
         jnxIpSecSaAuthAlgo              JnxAuthAlgo,	  
         jnxIpSecSaState                 INTEGER
      }
      jnxIpSecSaProtocol OBJECT-TYPE
         SYNTAX INTEGER{
                   ah(1),
                   esp(2)
                }
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "The index, represents the security protocol (AH, ESP or
             IPComp) for which this security association was setup."
         ::= { jnxIpSecSaEntry 1 }

      jnxIpSecSaIndex OBJECT-TYPE
         SYNTAX Integer32 (1..2147483647)
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
            "The index, in the context of the IPsec tunnel ipSecTunIndex,
            of the security association represented by this table entry.
            The value of this index is a number which begins at one and
            is incremented with each SPI associated with an IPsec Phase-2
            Tunnel.  The value of this object will wrap at 2,147,483,647."
         ::= { jnxIpSecSaEntry 2 }

      jnxIpSecSaInSpi OBJECT-TYPE
         SYNTAX JnxSpi
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
             "The value of the incoming SPI."
         ::= { jnxIpSecSaEntry 3 }

      jnxIpSecSaOutSpi OBJECT-TYPE
         SYNTAX JnxSpi
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
             "The value of the outgoing SPI."
         ::= { jnxIpSecSaEntry 4 }

      jnxIpSecSaInAuxSpi OBJECT-TYPE
         SYNTAX JnxSpi
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
             "The value of the incoming auxiliary SPI. This is valid for AH
              and ESP bundles."
         ::= { jnxIpSecSaEntry 5 }

      jnxIpSecSaOutAuxSpi OBJECT-TYPE
         SYNTAX JnxSpi
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
             "The value of the outgoing auxiliary SPI. This is valid for AH
              and ESP bundles."
         ::= { jnxIpSecSaEntry 6 }

      jnxIpSecSaType OBJECT-TYPE
         SYNTAX JnxSAType
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
             "This field represents the type of security associations 
			 which can be either manual or dynamic"
         ::= { jnxIpSecSaEntry 7 }

      jnxIpSecSaEncapMode OBJECT-TYPE
         SYNTAX JnxEncapMode
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The encapsulation mode used by an IPsec Phase-2 Tunnel. "
         ::= { jnxIpSecSaEntry 8 }

      jnxIpSecSaLifeSize OBJECT-TYPE
         SYNTAX Integer32
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The negotiated LifeSize of the IPsec Phase-2 Tunnel in kilobytes. "
         ::= { jnxIpSecSaEntry 9 }

      jnxIpSecSaLifeTime OBJECT-TYPE
         SYNTAX Integer32
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The negotiated LifeTime of the IPsec Phase-2 Tunnel in seconds. "
         ::= { jnxIpSecSaEntry 10 }

      jnxIpSecSaActiveTime OBJECT-TYPE
         SYNTAX TimeInterval
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The length of time the IPsec Phase-2 Tunnel has been active in seconds. "
         ::= { jnxIpSecSaEntry 11 }

      jnxIpSecSaLifeSizeThreshold OBJECT-TYPE
         SYNTAX Integer32
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The security association LifeSize refresh threshold in kilobytes. "
         ::= { jnxIpSecSaEntry 12 }

      jnxIpSecSaLifeTimeThreshold OBJECT-TYPE
         SYNTAX Integer32
         MAX-ACCESS read-only 
         STATUS current 
         DESCRIPTION
            "The security association LifeTime refresh threshold in seconds. "
         ::= { jnxIpSecSaEntry 13 }

      jnxIpSecSaEncryptAlgo OBJECT-TYPE
         SYNTAX JnxEncryptAlgo
         MAX-ACCESS read-only 
         STATUS current
         DESCRIPTION
            "The Encryption algorithm used to encrypt 
			 the packets which can be either es-cbc or 3des-cbc. "
         ::= { jnxIpSecSaEntry 14 }

      jnxIpSecSaAuthAlgo OBJECT-TYPE
         SYNTAX JnxAuthAlgo
         MAX-ACCESS read-only 
         STATUS current
         DESCRIPTION
            "The algorithm used for authentication of packets which
			 can be hmac-md5-96 or hmac-sha1-96"
         ::= { jnxIpSecSaEntry 15 }

      jnxIpSecSaState OBJECT-TYPE
         SYNTAX INTEGER{
                   unknown(0),
                   active(1),
                   expiring(2)
                }
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
            "This column represents the status of the security association
            represented by this table entry. If the status of the SA is
            'active', the SA is ready for active use. The status
            'expiring' represents any of the various states that the
            security association transitions through before being purged."
         ::= { jnxIpSecSaEntry 16 }
   END

