
F5-BIGIP-LOCAL-MIB DEFINITIONS ::= BEGIN
--================================================================
-- F5-BIGIP-LOCAL-MIB 
--     A private enterprise MIB for F5 local traffic management 
--     systems.
--     VERSION: 10.2.0
--================================================================

IMPORTS
    OBJECT-TYPE, NOTIFICATION-TYPE, MODULE-IDENTITY,
    Integer32, Opaque, enterprises, Counter32, Counter64, TimeTicks
        FROM SNMPv2-SMI

    TEXTUAL-CONVENTION, MacAddress 
        FROM SNMPv2-TC 

    OBJECT-GROUP, MODULE-COMPLIANCE
        FROM SNMPv2-CONF

    InetAddress, InetAddressType
      FROM INET-ADDRESS-MIB

    bigipTrafficMgmt, bigipCompliances, bigipGroups, LongDisplayString
      FROM F5-BIGIP-COMMON-MIB;

--================================================================
bigipLocalTM MODULE-IDENTITY
    LAST-UPDATED "201001291708Z" -- Fri Jan 29 17:08:32 UTC 2010 
    ORGANIZATION "F5 Networks, Inc."
    CONTACT-INFO
         "postal: F5 Networks, Inc. 
	 	  401 Elliott Ave. West 
                  Seattle, WA 98119
          phone:  (206) 272-5555
          email:  support@f5.com"

    DESCRIPTION
        "Top-level infrastructure of the F5 enterprise MIB tree." 
    ::= { bigipTrafficMgmt 2 }

--================================================================

-- bigipLocalTM
ltmGlobals             OBJECT IDENTIFIER ::= { bigipLocalTM 1 }
ltmMirrors             OBJECT IDENTIFIER ::= { bigipLocalTM 2 }
ltmNATs                OBJECT IDENTIFIER ::= { bigipLocalTM 3 }
ltmNodes               OBJECT IDENTIFIER ::= { bigipLocalTM 4 }
ltmPools               OBJECT IDENTIFIER ::= { bigipLocalTM 5 }
ltmProfiles            OBJECT IDENTIFIER ::= { bigipLocalTM 6 }
ltmRateFilters         OBJECT IDENTIFIER ::= { bigipLocalTM 7 }
ltmRules               OBJECT IDENTIFIER ::= { bigipLocalTM 8 }
ltmSNATs               OBJECT IDENTIFIER ::= { bigipLocalTM 9 }
ltmVirtualServers      OBJECT IDENTIFIER ::= { bigipLocalTM 10 }

--ltmGlobals
ltmGlobalAttr           OBJECT IDENTIFIER ::= { ltmGlobals 1 }

--ltmMirrors     
ltmMirrorPort           OBJECT IDENTIFIER ::= { ltmMirrors 1 }
ltmMirrorPortMember     OBJECT IDENTIFIER ::= { ltmMirrors 2 }

--ltmNATs
ltmNat                  OBJECT IDENTIFIER ::= { ltmNATs 1 }
ltmNatStat              OBJECT IDENTIFIER ::= { ltmNATs 2 }
ltmNatVlan              OBJECT IDENTIFIER ::= { ltmNATs 3 }

--ltmNodes
ltmNodeAddr             OBJECT IDENTIFIER ::= { ltmNodes 1 }
ltmNodeAddrStat         OBJECT IDENTIFIER ::= { ltmNodes 2 }
ltmNodeAddrStatus       OBJECT IDENTIFIER ::= { ltmNodes 3 }

--ltmPools
ltmPool                 OBJECT IDENTIFIER ::= { ltmPools 1 }
ltmPoolStat             OBJECT IDENTIFIER ::= { ltmPools 2 }
ltmPoolMember           OBJECT IDENTIFIER ::= { ltmPools 3 }
ltmPoolMemberStat       OBJECT IDENTIFIER ::= { ltmPools 4 }
ltmPoolStatus           OBJECT IDENTIFIER ::= { ltmPools 5 }
ltmPoolMemberStatus     OBJECT IDENTIFIER ::= { ltmPools 6 }

--ltmProfiles
ltmAuth                 OBJECT IDENTIFIER ::= { ltmProfiles 1 }
ltmClientSsl            OBJECT IDENTIFIER ::= { ltmProfiles 2 }
ltmServerSsl            OBJECT IDENTIFIER ::= { ltmProfiles 3 }
ltmConnPool             OBJECT IDENTIFIER ::= { ltmProfiles 4 }
ltmFastL4               OBJECT IDENTIFIER ::= { ltmProfiles 5 }
ltmFtp                  OBJECT IDENTIFIER ::= { ltmProfiles 6 }
ltmHttp                 OBJECT IDENTIFIER ::= { ltmProfiles 7 }
ltmPersist              OBJECT IDENTIFIER ::= { ltmProfiles 8 }
ltmStream               OBJECT IDENTIFIER ::= { ltmProfiles 9 }
ltmTcp                  OBJECT IDENTIFIER ::= { ltmProfiles 10 }
ltmUdp                  OBJECT IDENTIFIER ::= { ltmProfiles 11 }
ltmFastHttp             OBJECT IDENTIFIER ::= { ltmProfiles 12 }
ltmXml                  OBJECT IDENTIFIER ::= { ltmProfiles 13 }
ltmDns                  OBJECT IDENTIFIER ::= { ltmProfiles 14 }
ltmHttpClass            OBJECT IDENTIFIER ::= { ltmProfiles 15 }
ltmIiop                 OBJECT IDENTIFIER ::= { ltmProfiles 16 }
ltmRtsp                 OBJECT IDENTIFIER ::= { ltmProfiles 17 }
ltmSctp                 OBJECT IDENTIFIER ::= { ltmProfiles 18 }
ltmUserStat             OBJECT IDENTIFIER ::= { ltmProfiles 19 }
ltmSip                  OBJECT IDENTIFIER ::= { ltmProfiles 20 }
ltmIsession             OBJECT IDENTIFIER ::= { ltmProfiles 21 }

--ltmAuth
ltmAuthProfile          OBJECT IDENTIFIER ::= { ltmAuth 1 }
ltmAuthProfileStat      OBJECT IDENTIFIER ::= { ltmAuth 2 }

--ltmClientSsl
ltmClientSslProfile     OBJECT IDENTIFIER ::= { ltmClientSsl 1 }
ltmClientSslProfileStat OBJECT IDENTIFIER ::= { ltmClientSsl 2 }

--ltmServerSsl
ltmServerSslProfile     OBJECT IDENTIFIER ::= { ltmServerSsl 1 }
ltmServerSslProfileStat OBJECT IDENTIFIER ::= { ltmServerSsl 2 }

--ltmConnPool
ltmConnPoolProfile      OBJECT IDENTIFIER ::= { ltmConnPool 1 }
ltmConnPoolProfileStat  OBJECT IDENTIFIER ::= { ltmConnPool 2 }

--ltmFastL4
ltmFastL4Profile        OBJECT IDENTIFIER ::= { ltmFastL4 1 }
ltmFastL4ProfileStat    OBJECT IDENTIFIER ::= { ltmFastL4 2 }

--ltmFtp
ltmFtpProfile           OBJECT IDENTIFIER ::= { ltmFtp 1 }

--ltmHttp
ltmHttpProfile                    OBJECT IDENTIFIER ::= { ltmHttp 1 }
ltmHttpProfileCompUriIncl         OBJECT IDENTIFIER ::= { ltmHttp 2 }
ltmHttpProfileCompUriExcl         OBJECT IDENTIFIER ::= { ltmHttp 3 }
ltmHttpProfileCompContTypeIncl    OBJECT IDENTIFIER ::= { ltmHttp 4 }
ltmHttpProfileCompContTypeExcl    OBJECT IDENTIFIER ::= { ltmHttp 5 }
ltmHttpProfileStat                OBJECT IDENTIFIER ::= { ltmHttp 6 }
ltmHttpProfileRamUriExcl          OBJECT IDENTIFIER ::= { ltmHttp 7 }
ltmHttpProfileRamUriIncl          OBJECT IDENTIFIER ::= { ltmHttp 8 }
ltmHttpProfileRamUriPin           OBJECT IDENTIFIER ::= { ltmHttp 9 }
ltmHttpProfileFallbackStatus      OBJECT IDENTIFIER ::= { ltmHttp 10 }
ltmHttpProfileRespHeadersPerm     OBJECT IDENTIFIER ::= { ltmHttp 11 }
ltmHttpProfileEncCookies          OBJECT IDENTIFIER ::= { ltmHttp 12 }

--ltmPersist
ltmPersistProfile       OBJECT IDENTIFIER ::= { ltmPersist 1 }

--ltmStream
ltmStreamProfile        OBJECT IDENTIFIER ::= { ltmStream 1 }
ltmStreamProfileStat    OBJECT IDENTIFIER ::= { ltmStream 2 }

--ltmTcp
ltmTcpProfile           OBJECT IDENTIFIER ::= { ltmTcp 1 }
ltmTcpProfileStat       OBJECT IDENTIFIER ::= { ltmTcp 2 }

--ltmUdp
ltmUdpProfile           OBJECT IDENTIFIER ::= { ltmUdp 1 }
ltmUdpProfileStat       OBJECT IDENTIFIER ::= { ltmUdp 2 }

--ltmFastHttp
ltmFastHttpProfile      OBJECT IDENTIFIER ::= { ltmFastHttp 1 }
ltmFastHttpProfileStat  OBJECT IDENTIFIER ::= { ltmFastHttp 2 }


--ltmXml
ltmXmlProfile           OBJECT IDENTIFIER ::= { ltmXml 1 }
ltmXmlProfileStat       OBJECT IDENTIFIER ::= { ltmXml 2 }
ltmXmlProfileXpathQueries      OBJECT IDENTIFIER ::= { ltmXml 3 }
ltmXmlProfileNamespaceMappings      OBJECT IDENTIFIER ::= { ltmXml 4 }


--ltmHttpClass
ltmHttpClassProfile     OBJECT IDENTIFIER ::= { ltmHttpClass 1 }
ltmHttpClassProfileHost OBJECT IDENTIFIER ::= { ltmHttpClass 2 }
ltmHttpClassProfileUri  OBJECT IDENTIFIER ::= { ltmHttpClass 3 }
ltmHttpClassProfileHead OBJECT IDENTIFIER ::= { ltmHttpClass 4 }
ltmHttpClassProfileCook OBJECT IDENTIFIER ::= { ltmHttpClass 5 }
ltmHttpClassProfileStat OBJECT IDENTIFIER ::= { ltmHttpClass 6 }

--ltmIiop
ltmIiopProfile          OBJECT IDENTIFIER ::= { ltmIiop 1 }
ltmIiopProfileStat      OBJECT IDENTIFIER ::= { ltmIiop 2 }

--ltmRtsp
ltmRtspProfile          OBJECT IDENTIFIER ::= { ltmRtsp 1 }
ltmRtspProfileStat      OBJECT IDENTIFIER ::= { ltmRtsp 2 }

--ltmSctp
ltmSctpProfile          OBJECT IDENTIFIER ::= { ltmSctp 1 }
ltmSctpProfileStat      OBJECT IDENTIFIER ::= { ltmSctp 2 }

--ltmUserStat
ltmUserStatProfile      OBJECT IDENTIFIER ::= { ltmUserStat 1 }
ltmUserStatProfileStat  OBJECT IDENTIFIER ::= { ltmUserStat 2 }

--ltmSip
ltmSipProfile           OBJECT IDENTIFIER ::= { ltmSip 1 }
ltmSipProfileStat       OBJECT IDENTIFIER ::= { ltmSip 2 }

--ltmIsession
ltmIsessionProfile      OBJECT IDENTIFIER ::= { ltmIsession 1 }
ltmIsessionProfileStat  OBJECT IDENTIFIER ::= { ltmIsession 2 }

--ltmDns
ltmDnsProfile           OBJECT IDENTIFIER ::= { ltmDns 1 }

--ltmRateFilters     
--ltmRateFilters     
ltmRateFilter           OBJECT IDENTIFIER ::= { ltmRateFilters 1 }
ltmRateFilterStat       OBJECT IDENTIFIER ::= { ltmRateFilters 2 }

--ltmRules     
ltmRule                 OBJECT IDENTIFIER ::= { ltmRules 1 }
ltmRuleEvent            OBJECT IDENTIFIER ::= { ltmRules 2 }
ltmRuleEventStat        OBJECT IDENTIFIER ::= { ltmRules 3 }

--ltmSNATs
ltmSnat                 OBJECT IDENTIFIER ::= { ltmSNATs 1 }
ltmSnatStat             OBJECT IDENTIFIER ::= { ltmSNATs 2 }
ltmSnatVlan             OBJECT IDENTIFIER ::= { ltmSNATs 3 }
ltmSnatOrigAddr         OBJECT IDENTIFIER ::= { ltmSNATs 4 }
ltmTransAddr            OBJECT IDENTIFIER ::= { ltmSNATs 5 }
ltmTransAddrStat        OBJECT IDENTIFIER ::= { ltmSNATs 6 }
ltmSnatPool             OBJECT IDENTIFIER ::= { ltmSNATs 7 }
ltmSnatPoolStat         OBJECT IDENTIFIER ::= { ltmSNATs 8 }
ltmSnatpoolTransAddr    OBJECT IDENTIFIER ::= { ltmSNATs 9 }



--ltmVirtualServers
ltmVirtualServ          OBJECT IDENTIFIER ::= { ltmVirtualServers 1 }
ltmVirtualServStat      OBJECT IDENTIFIER ::= { ltmVirtualServers 2 }
ltmVirtualServAuth      OBJECT IDENTIFIER ::= { ltmVirtualServers 3 }
ltmVirtualServPersist   OBJECT IDENTIFIER ::= { ltmVirtualServers 4 }
ltmVirtualServProfile   OBJECT IDENTIFIER ::= { ltmVirtualServers 5 }
ltmVirtualServPool      OBJECT IDENTIFIER ::= { ltmVirtualServers 6 }
ltmVirtualServClonePool OBJECT IDENTIFIER ::= { ltmVirtualServers 7 }
ltmVirtualServRule      OBJECT IDENTIFIER ::= { ltmVirtualServers 8 }
ltmVirtualServVlan      OBJECT IDENTIFIER ::= { ltmVirtualServers 9 }
ltmVirtualAddr          OBJECT IDENTIFIER ::= { ltmVirtualServers 10 }
ltmVirtualAddrStat      OBJECT IDENTIFIER ::= { ltmVirtualServers 11 }
ltmVirtualServHttpClass OBJECT IDENTIFIER ::= { ltmVirtualServers 12 }
ltmVirtualServStatus    OBJECT IDENTIFIER ::= { ltmVirtualServers 13 }
ltmVirtualAddrStatus    OBJECT IDENTIFIER ::= { ltmVirtualServers 14 }
ltmVirtualModuleScore   OBJECT IDENTIFIER ::= { ltmVirtualServers 15 }




--==================================================================
-- Global
--==================================================================
ltmAttrLbmodeFastestMaxIdleTime OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum idle time (in seconds) used for load balancing
		 to the fastest node."
	::= { ltmGlobalAttr 1 } 

ltmAttrMirrorState OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state of mirroring in redundant systems."
	::= { ltmGlobalAttr 2 } 

ltmAttrPersistDestAddrLimitMode OBJECT-TYPE 
	SYNTAX INTEGER {
		timeout(0),
		maxcount(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The method of limiting destination address entries."
	::= { ltmGlobalAttr 3 } 

ltmAttrPersistDestAddrMaxCount OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of entries allowed for the destination address entries."
	::= { ltmGlobalAttr 4 } 

ltmAttrSnatAnyIpProtocol OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The status of the feature that allows any IP traffic 
		 through SNATs."
	::= { ltmGlobalAttr 5 } 

ltmAttrMirrorPeerIpAddr OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of the mirroring peer in redundant systems"
	::= { ltmGlobalAttr 6 } 

--==================================================================
-- Rate_filter_class
--==================================================================
ltmRateFilterNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmRateFilter entries in the table."
	::= { ltmRateFilter 1 } 

ltmRateFilterTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRateFilterEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of rate filters for shaping."
	::= { ltmRateFilter 2 } 

ltmRateFilterEntry OBJECT-TYPE
	SYNTAX  LtmRateFilterEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRateFilter Table"
	INDEX {
		ltmRateFilterCname
	}
	::= { ltmRateFilterTable 1 } 

LtmRateFilterEntry ::= 
	SEQUENCE {
        	ltmRateFilterCname                                     LongDisplayString,
        	ltmRateFilterRate                                      Integer32,
        	ltmRateFilterCeil                                      Integer32,
        	ltmRateFilterBurst                                     Integer32,
        	ltmRateFilterPname                                     LongDisplayString,
        	ltmRateFilterQtype                                     INTEGER,
        	ltmRateFilterDirection                                 INTEGER
	}

ltmRateFilterCname OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The rate class name specified by the user according to the  
		 same syntax allowed for rules or pool names"
	::= { ltmRateFilterEntry 1 } 

ltmRateFilterRate OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The base rate. It is a number which may be postfixed with a 
		 metric of either bps, Kbps or Mbps, to indicate bits per 
		 second, Kilobits per second, or Megabits per second, 
		 respectively. 
		 Note: these numbers are powers of 10, not powers of 2. 
		 If no postfix is specified, the number is interpreted as bps. 
		 The rate specifies the maximum throughput to allot to traffic 
		 handled by the Rate Class. Packets in excess of the posted 
		 rate will be dropped."
	::= { ltmRateFilterEntry 2 } 

ltmRateFilterCeil OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The ceiling rate. It is defined like the base rate, but specifies 
		 how far beyond the base rate the traffic is allowed to flow 
		 when bursting (details on bursting below). The ceiling rate is 
		 an absolute limit - it is impossible for traffic to flow at a 
		 higher rate than the ceiling rate, even when bursting. If the 
		 ceiling rate is omitted or is equal to the base rate, the 
		 traffic may not exceed the base rate. It is illegal for the 
		 ceiling rate to be less than the base rate."
	::= { ltmRateFilterEntry 3 } 

ltmRateFilterBurst OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The burst size. It specifies the maximum number of bytes the 
		 traffic is allowed to burst when exceeding the base rate. The 
		 burst size is measured in bytes. If omitted, a default burst 
		size is 0."
	::= { ltmRateFilterEntry 4 } 

ltmRateFilterPname OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The parent rate class name. It indicates that the rate class 
		 is a child of the named parent. Any child rate class has the 
		 ability to borrow bandwidth from its parent. (Borrowing is a 
		 feature which allows a child to burst even beyond the burst 
		 size by borrowing from the burst size of a parent.) If omitted, 
		 the rate class is not a child, but may be a parent if another 
		 rate class refers to it as such."
	::= { ltmRateFilterEntry 5 } 

ltmRateFilterQtype OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		sfq(1),
		pfifo(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The queue discipline type.
		 none  - invalid state;
		 sfq   - stochastic fair queue;
		 pfifo - priority FIFO."
	::= { ltmRateFilterEntry 6 } 

ltmRateFilterDirection OBJECT-TYPE 
	SYNTAX INTEGER {
		any(0),
		client(1),
		server(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state of the direction which the filter shapes traffic to.
		any    - shape to the client and server;
		client - only shape traffic to the client;
		server - only shape traffic to the server."
	::= { ltmRateFilterEntry 7 } 

--==================================================================
-- Rate_filter_class_stat
--==================================================================
ltmRateFilterStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmRateFilterStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmRateFilterStat 1 } 

ltmRateFilterStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmRateFilterStat entries in the table."
	::= { ltmRateFilterStat 2 } 

ltmRateFilterStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRateFilterStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of rate filters for shaping."
	::= { ltmRateFilterStat 3 } 

ltmRateFilterStatEntry OBJECT-TYPE
	SYNTAX  LtmRateFilterStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRateFilterStat Table"
	INDEX {
		ltmRateFilterStatCname
	}
	::= { ltmRateFilterStatTable 1 } 

LtmRateFilterStatEntry ::= 
	SEQUENCE {
        	ltmRateFilterStatCname                                 LongDisplayString,
        	ltmRateFilterStatRateBytes                             Counter64,
        	ltmRateFilterStatBurstBytes                            Counter64,
        	ltmRateFilterStatDroppedBytes                          Counter64,
        	ltmRateFilterStatBytesQueued                           Counter64,
        	ltmRateFilterStatBytesPerSec                           Counter64,
        	ltmRateFilterStatDropTailPkts                          Counter64,
        	ltmRateFilterStatDropTailBytes                         Counter64,
        	ltmRateFilterStatDropRandPkts                          Counter64,
        	ltmRateFilterStatDropRandBytes                         Counter64,
        	ltmRateFilterStatDropTotPkts                           Counter64,
        	ltmRateFilterStatDropTotBytes                          Counter64
	}

ltmRateFilterStatCname OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The rate class name specified by the user according to the  
		 same syntax allowed for rules or pool names"
	::= { ltmRateFilterStatEntry 1 } 

ltmRateFilterStatRateBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes at or below base rate - increments by 1 for 
		 every byte of every packet handled at or below the base rate."
	::= { ltmRateFilterStatEntry 2 } 

ltmRateFilterStatBurstBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes bursted (above base rate) - increments by 
		 1 for every byte of every packet handled above the base rate 
		 (i.e. bursted traffic)"
	::= { ltmRateFilterStatEntry 3 } 

ltmRateFilterStatDroppedBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		 Replaced by ltmRateFilterStatDropTotBytes: 
		 the number of bytes dropped - increments by 1 for every byte  
		 of every packet dropped by the rate class."
	::= { ltmRateFilterStatEntry 4 } 

ltmRateFilterStatBytesQueued OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes queued."
	::= { ltmRateFilterStatEntry 5 } 

ltmRateFilterStatBytesPerSec OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The average bytes/sec over last 4 sec."
	::= { ltmRateFilterStatEntry 6 } 

ltmRateFilterStatDropTailPkts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets dropped - increments by 1 for
	         every packet dropped by the rate class as queue overflow."
	::= { ltmRateFilterStatEntry 7 } 

ltmRateFilterStatDropTailBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes dropped - increments by 1 for every byte
	         of every packet dropped by the rate class as queue overflow."
	::= { ltmRateFilterStatEntry 8 } 

ltmRateFilterStatDropRandPkts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets dropped - increments by 1 for
	         every packet dropped by the rate class as RED or FRED policy."
	::= { ltmRateFilterStatEntry 9 } 

ltmRateFilterStatDropRandBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The  number of bytes dropped - increments by 1 for every byte
	         of every packet dropped by the rate class as RED or FRED policy."
	::= { ltmRateFilterStatEntry 10 } 

ltmRateFilterStatDropTotPkts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of packets dropped - increments by 1 for
	         every packet dropped by the rate class."
	::= { ltmRateFilterStatEntry 11 } 

ltmRateFilterStatDropTotBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of bytes dropped - increments by 1 for every byte
	         of every packet dropped by the rate class."
	::= { ltmRateFilterStatEntry 12 } 

--==================================================================
-- Mirror_port
--==================================================================
ltmMirrorPortNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmMirrorPort entries in the table."
	::= { ltmMirrorPort 1 } 

ltmMirrorPortTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmMirrorPortEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of mirrored ports."
	::= { ltmMirrorPort 2 } 

ltmMirrorPortEntry OBJECT-TYPE
	SYNTAX  LtmMirrorPortEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmMirrorPort Table"
	INDEX {
		ltmMirrorPortName
	}
	::= { ltmMirrorPortTable 1 } 

LtmMirrorPortEntry ::= 
	SEQUENCE {
        	ltmMirrorPortName                                      LongDisplayString
	}

ltmMirrorPortName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a port to which is mirrored."
	::= { ltmMirrorPortEntry 1 } 

--==================================================================
-- Mirror_port_mbr
--==================================================================
ltmMirrorPortMemberNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmMirrorPortMember entries in the table."
	::= { ltmMirrorPortMember 1 } 

ltmMirrorPortMemberTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmMirrorPortMemberEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of mirrored port members."
	::= { ltmMirrorPortMember 2 } 

ltmMirrorPortMemberEntry OBJECT-TYPE
	SYNTAX  LtmMirrorPortMemberEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmMirrorPortMember Table"
	INDEX {
		ltmMirrorPortMemberToName,
		ltmMirrorPortMemberName
	}
	::= { ltmMirrorPortMemberTable 1 } 

LtmMirrorPortMemberEntry ::= 
	SEQUENCE {
        	ltmMirrorPortMemberToName                              LongDisplayString,
        	ltmMirrorPortMemberName                                LongDisplayString,
        	ltmMirrorPortMemberConduitName                         LongDisplayString
	}

ltmMirrorPortMemberToName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a port which it is mirrored to."
	::= { ltmMirrorPortMemberEntry 1 } 

ltmMirrorPortMemberName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a mirrored port."
	::= { ltmMirrorPortMemberEntry 2 } 

ltmMirrorPortMemberConduitName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This attribute is used to represent a local edge port 
		when a conduit between switch devices is necessary."
	::= { ltmMirrorPortMemberEntry 3 } 

--==================================================================
-- Nat
--==================================================================
ltmNatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmNat entries in the table."
	::= { ltmNat 1 } 

ltmNatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmNatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of NAT."
	::= { ltmNat 2 } 

ltmNatEntry OBJECT-TYPE
	SYNTAX  LtmNatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmNat Table"
	INDEX {
		ltmNatTransAddrType,
		ltmNatTransAddr
	}
	::= { ltmNatTable 1 } 

LtmNatEntry ::= 
	SEQUENCE {
        	ltmNatTransAddrType                                    InetAddressType,
        	ltmNatTransAddr                                        InetAddress,
        	ltmNatOrigAddrType                                     InetAddressType,
        	ltmNatOrigAddr                                         InetAddress,
        	ltmNatEnabled                                          INTEGER,
        	ltmNatArpEnabled                                       INTEGER,
        	ltmNatUnitId                                           Integer32,
        	ltmNatListedEnabledVlans                               INTEGER
	}

ltmNatTransAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmNatTransAddr"
	::= { ltmNatEntry 1 } 

ltmNatTransAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The NAT translation address. It is 
		interpreted within the context of a ltmNatTransAddrType value."
	::= { ltmNatEntry 2 } 

ltmNatOrigAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmNatOrigAddr."
	::= { ltmNatEntry 3 } 

ltmNatOrigAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The NAT original address associated with the specified NAT translation address. 
		It is interpreted within the context of a ltmNatOrigAddrType value."
	::= { ltmNatEntry 4 } 

ltmNatEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether the specified NAT address is enabled or not."
	::= { ltmNatEntry 5 } 

ltmNatArpEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The ARP state for the specified NAT, whether it is enabled or not."
	::= { ltmNatEntry 6 } 

ltmNatUnitId OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The unit number associated with the specified NAT translation address."
	::= { ltmNatEntry 7 } 

ltmNatListedEnabledVlans OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether associated VLANs are NAT enabled or not.
		The associated VLANs are listed in ltmNatVlanTable."
	::= { ltmNatEntry 8 } 

--==================================================================
-- Nat_stat
--==================================================================
ltmNatStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmNatStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmNatStat 1 } 

ltmNatStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmNatStat entries in the table."
	::= { ltmNatStat 2 } 

ltmNatStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmNatStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of NAT."
	::= { ltmNatStat 3 } 

ltmNatStatEntry OBJECT-TYPE
	SYNTAX  LtmNatStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmNatStat Table"
	INDEX {
		ltmNatStatTransAddrType,
		ltmNatStatTransAddr
	}
	::= { ltmNatStatTable 1 } 

LtmNatStatEntry ::= 
	SEQUENCE {
        	ltmNatStatTransAddrType                                InetAddressType,
        	ltmNatStatTransAddr                                    InetAddress,
        	ltmNatStatServerPktsIn                                 Counter64,
        	ltmNatStatServerBytesIn                                Counter64,
        	ltmNatStatServerPktsOut                                Counter64,
        	ltmNatStatServerBytesOut                               Counter64,
        	ltmNatStatServerMaxConns                               Counter64,
        	ltmNatStatServerTotConns                               Counter64,
        	ltmNatStatServerCurConns                               Counter64
	}

ltmNatStatTransAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmNatStatTransAddr"
	::= { ltmNatStatEntry 1 } 

ltmNatStatTransAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The NAT translation address. It is 
		interpreted within the context of a ltmNatStatTransAddrType value."
	::= { ltmNatStatEntry 2 } 

ltmNatStatServerPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received from server-side."
	::= { ltmNatStatEntry 3 } 

ltmNatStatServerBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received from server-side."
	::= { ltmNatStatEntry 4 } 

ltmNatStatServerPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to server-side."
	::= { ltmNatStatEntry 5 } 

ltmNatStatServerBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to server-side."
	::= { ltmNatStatEntry 6 } 

ltmNatStatServerMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from server-side."
	::= { ltmNatStatEntry 7 } 

ltmNatStatServerTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from server-side."
	::= { ltmNatStatEntry 8 } 

ltmNatStatServerCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from server-side."
	::= { ltmNatStatEntry 9 } 

--==================================================================
-- Nat_vlan
--==================================================================
ltmNatVlanNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmNatVlan entries in the table."
	::= { ltmNatVlan 1 } 

ltmNatVlanTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmNatVlanEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing VLAN information associated with NAT."
	::= { ltmNatVlan 2 } 

ltmNatVlanEntry OBJECT-TYPE
	SYNTAX  LtmNatVlanEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmNatVlan Table"
	INDEX {
		ltmNatVlanTransAddrType,
		ltmNatVlanTransAddr,
		ltmNatVlanVlanName
	}
	::= { ltmNatVlanTable 1 } 

LtmNatVlanEntry ::= 
	SEQUENCE {
        	ltmNatVlanTransAddrType                                InetAddressType,
        	ltmNatVlanTransAddr                                    InetAddress,
        	ltmNatVlanVlanName                                     LongDisplayString
	}

ltmNatVlanTransAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmNatVlanTransAddr"
	::= { ltmNatVlanEntry 1 } 

ltmNatVlanTransAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The NAT translation address. It is interpreted within 
		the context of a ltmNatVlanTransAddrType value."
	::= { ltmNatVlanEntry 2 } 

ltmNatVlanVlanName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a VLAN associated with the specified NAT.
		Only when ltmNatListedEnabledVlans is set to enable, 
		NAT is enabled on the VLAN. "
	::= { ltmNatVlanEntry 3 } 

--==================================================================
-- Node_address
--==================================================================
ltmNodeAddrNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmNodeAddr entries in the table."
	::= { ltmNodeAddr 1 } 

ltmNodeAddrTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmNodeAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of node addresses."
	::= { ltmNodeAddr 2 } 

ltmNodeAddrEntry OBJECT-TYPE
	SYNTAX  LtmNodeAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmNodeAddr Table"
	INDEX {
		ltmNodeAddrAddrType,
		ltmNodeAddrAddr
	}
	::= { ltmNodeAddrTable 1 } 

LtmNodeAddrEntry ::= 
	SEQUENCE {
        	ltmNodeAddrAddrType                                    InetAddressType,
        	ltmNodeAddrAddr                                        InetAddress,
        	ltmNodeAddrConnLimit                                   Integer32,
        	ltmNodeAddrRatio                                       Integer32,
        	ltmNodeAddrDynamicRatio                                INTEGER,
        	ltmNodeAddrMonitorState                                INTEGER,
        	ltmNodeAddrMonitorStatus                               INTEGER,
        	ltmNodeAddrMonitorRule                                 LongDisplayString,
        	ltmNodeAddrNewSessionEnable                            INTEGER,
        	ltmNodeAddrSessionStatus                               INTEGER,
        	ltmNodeAddrPoolMemberRefCount                          Integer32,
        	ltmNodeAddrScreenName                                  LongDisplayString,
        	ltmNodeAddrAvailabilityState                           INTEGER,
        	ltmNodeAddrEnabledState                                INTEGER,
        	ltmNodeAddrDisabledParentType                          Integer32,
        	ltmNodeAddrStatusReason                                LongDisplayString
	}

ltmNodeAddrAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmNodeAddrAddr."
	::= { ltmNodeAddrEntry 1 } 

ltmNodeAddrAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a node. It is interpreted within 
		 the context of a ltmNodeAddrAddrType value."
	::= { ltmNodeAddrEntry 2 } 

ltmNodeAddrConnLimit OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of connections the specified node address is 
		 allowed to have open at one time."
	::= { ltmNodeAddrEntry 3 } 

ltmNodeAddrRatio OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The ratio of the specified node address, used in load balance algorithm."
	::= { ltmNodeAddrEntry 4 } 

ltmNodeAddrDynamicRatio OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The dynamic ratio of the specified node address, used in load balance algorithm."
	::= { ltmNodeAddrEntry 5 } 

ltmNodeAddrMonitorState OBJECT-TYPE 
	SYNTAX INTEGER {
		unchecked(0),
		checking(1),
		inband(2),
		forced-up(3),
		up(4),
		down(19),
		forced-down(20),
		irule-down(22),
		inband-down(23),
		down-manual-resume(24),
		disabled(25)
	}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The internal tmm monitor state for the specified node address."
	::= { ltmNodeAddrEntry 6 } 

ltmNodeAddrMonitorStatus OBJECT-TYPE 
	SYNTAX INTEGER {
		unchecked(0),
		checking(1),
		inband(2),
		forced-up(3),
		up(4),
		addr-down(18),
		down(19),
		forced-down(20),
		maint(21),
		irule-down(22),
		inband-down(23),
		down-manual-resume(24)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The hierarchical load balance state for the specified node address, including parent status. 
		 unchecked - enabled node that is not monitored;
		 checking  - initial state until monitor reports;
	         inband    - the tmm has marked the node up;
	     forced-up - forced up manually
		 up        - enabled node when its monitors succeed;
		 addr-down   - node address monitor fails or forced down;
		 down        - enabled node when its monitors fail;
		 forced-down - node forced down manually;
		 maint       - in maintenance mode;
	         irule-down  - an iRule has marked the node down;
	         inband-down - the tmm has marked the node down;
	         down-manual-resume - the node is down and must be manually enabled; 
		 "
	::= { ltmNodeAddrEntry 7 } 

ltmNodeAddrMonitorRule OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The monitor rule used for load balance the specified node address."
	::= { ltmNodeAddrEntry 8 } 

ltmNodeAddrNewSessionEnable OBJECT-TYPE 
	SYNTAX INTEGER {
		user-disabled(1),
		user-enabled(2),
		monitor-enabled(3),
		monitor-disabled(4)
	}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The state indicating whether a new session can be enabled or not for the specified node address."
	::= { ltmNodeAddrEntry 9 } 

ltmNodeAddrSessionStatus OBJECT-TYPE 
	SYNTAX INTEGER {
		enabled(1),
		addrdisabled(2),
		servdisabled(3),
		disabled(4),
		forceddisabled(5)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The hierarchical status of the session, including parent status, for 
		the specified node address.
		enabled       - new sessions enabled;
		addrdisabled - new sessions disabled on node address;
		servdisabled - new sessions disabled on node server;
		disabled      - new sessions disabled;
		forceddisabled - new sessions forced to be disabled."
	::= { ltmNodeAddrEntry 10 } 

ltmNodeAddrPoolMemberRefCount OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pool members referencing the specified node."
	::= { ltmNodeAddrEntry 11 } 

ltmNodeAddrScreenName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The screen names for the specified node address."
	::= { ltmNodeAddrEntry 12 } 

ltmNodeAddrAvailabilityState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmNodeAddrStatusAvailState under ltmNodeAddrStatus.
		The state of the specified node address availability indicated in color."
	::= { ltmNodeAddrEntry 13 } 

ltmNodeAddrEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! 
		Replaced by ltmNodeAddrStatusEnabledState under ltmNodeAddrStatus.
		The state of the specified node address activity status, as specified 
		by the user."
	::= { ltmNodeAddrEntry 14 } 

ltmNodeAddrDisabledParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! 
		Replaced by ltmNodeAddrStatusParentType under ltmNodeAddrStatus.
		The type of parent object which disabled the specified node address."
	::= { ltmNodeAddrEntry 15 } 

ltmNodeAddrStatusReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! 
		Replaced by ltmNodeAddrStatusDetailReason under ltmNodeAddrStatus.
		The detail description of the node's status of parent object 
		which disabled the specified node address."
	::= { ltmNodeAddrEntry 16 } 

--==================================================================
-- Node_address_stat
--==================================================================
ltmNodeAddrStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmNodeAddrStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmNodeAddrStat 1 } 

ltmNodeAddrStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmNodeAddrStat entries in the table."
	::= { ltmNodeAddrStat 2 } 

ltmNodeAddrStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmNodeAddrStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of node addresses."
	::= { ltmNodeAddrStat 3 } 

ltmNodeAddrStatEntry OBJECT-TYPE
	SYNTAX  LtmNodeAddrStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmNodeAddrStat Table"
	INDEX {
		ltmNodeAddrStatAddrType,
		ltmNodeAddrStatAddr
	}
	::= { ltmNodeAddrStatTable 1 } 

LtmNodeAddrStatEntry ::= 
	SEQUENCE {
        	ltmNodeAddrStatAddrType                                InetAddressType,
        	ltmNodeAddrStatAddr                                    InetAddress,
        	ltmNodeAddrStatServerPktsIn                            Counter64,
        	ltmNodeAddrStatServerBytesIn                           Counter64,
        	ltmNodeAddrStatServerPktsOut                           Counter64,
        	ltmNodeAddrStatServerBytesOut                          Counter64,
        	ltmNodeAddrStatServerMaxConns                          Counter64,
        	ltmNodeAddrStatServerTotConns                          Counter64,
        	ltmNodeAddrStatServerCurConns                          Counter64,
        	ltmNodeAddrStatPvaPktsIn                               Counter64,
        	ltmNodeAddrStatPvaBytesIn                              Counter64,
        	ltmNodeAddrStatPvaPktsOut                              Counter64,
        	ltmNodeAddrStatPvaBytesOut                             Counter64,
        	ltmNodeAddrStatPvaMaxConns                             Counter64,
        	ltmNodeAddrStatPvaTotConns                             Counter64,
        	ltmNodeAddrStatPvaCurConns                             Counter64,
        	ltmNodeAddrStatTotRequests                             Counter64,
        	ltmNodeAddrStatTotPvaAssistConn                        Counter64,
        	ltmNodeAddrStatCurrPvaAssistConn                       Counter64
	}

ltmNodeAddrStatAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmNodeAddrStatAddr"
	::= { ltmNodeAddrStatEntry 1 } 

ltmNodeAddrStatAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a node. It is interpreted within 
		 the context of an ltmNodeAddrStatAddrType value."
	::= { ltmNodeAddrStatEntry 2 } 

ltmNodeAddrStatServerPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received by the specified node address from server-side."
	::= { ltmNodeAddrStatEntry 3 } 

ltmNodeAddrStatServerBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received by the specified node address from server-side."
	::= { ltmNodeAddrStatEntry 4 } 

ltmNodeAddrStatServerPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to server-side from the specified node address."
	::= { ltmNodeAddrStatEntry 5 } 

ltmNodeAddrStatServerBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to server-side from the specified node address."
	::= { ltmNodeAddrStatEntry 6 } 

ltmNodeAddrStatServerMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from server-side to the specified node address."
	::= { ltmNodeAddrStatEntry 7 } 

ltmNodeAddrStatServerTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from server-side to the specified node address."
	::= { ltmNodeAddrStatEntry 8 } 

ltmNodeAddrStatServerCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from server-side to the specified node address."
	::= { ltmNodeAddrStatEntry 9 } 

ltmNodeAddrStatPvaPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated packets received by the specified node address."
	::= { ltmNodeAddrStatEntry 10 } 

ltmNodeAddrStatPvaBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated bytes received by the specified node address."
	::= { ltmNodeAddrStatEntry 11 } 

ltmNodeAddrStatPvaPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated packets sent out from the specified node address."
	::= { ltmNodeAddrStatEntry 12 } 

ltmNodeAddrStatPvaBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated bytes sent out from the specified node address."
	::= { ltmNodeAddrStatEntry 13 } 

ltmNodeAddrStatPvaMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum hardware accelerated connections to the specified node address."
	::= { ltmNodeAddrStatEntry 14 } 

ltmNodeAddrStatPvaTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total hardware accelerated connections to the specified node address."
	::= { ltmNodeAddrStatEntry 15 } 

ltmNodeAddrStatPvaCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current hardware accelerated connections to the specified node address."
	::= { ltmNodeAddrStatEntry 16 } 

ltmNodeAddrStatTotRequests OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of requests going through the specified node address."
	::= { ltmNodeAddrStatEntry 17 } 

ltmNodeAddrStatTotPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections to the specified node address, 
		which are partially hardware accelerated."
	::= { ltmNodeAddrStatEntry 18 } 

ltmNodeAddrStatCurrPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of connections to the specified node address,
		 which are partially hardware accelerated."
	::= { ltmNodeAddrStatEntry 19 } 

--==================================================================
-- Pool
--==================================================================
ltmPoolNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmPool entries in the table."
	::= { ltmPool 1 } 

ltmPoolTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmPoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of pools."
	::= { ltmPool 2 } 

ltmPoolEntry OBJECT-TYPE
	SYNTAX  LtmPoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmPool Table"
	INDEX {
		ltmPoolName
	}
	::= { ltmPoolTable 1 } 

LtmPoolEntry ::= 
	SEQUENCE {
        	ltmPoolName                                            LongDisplayString,
        	ltmPoolLbMode                                          INTEGER,
        	ltmPoolActionOnServiceDown                             INTEGER,
        	ltmPoolMinUpMembers                                    INTEGER,
        	ltmPoolMinUpMembersEnable                              INTEGER,
        	ltmPoolMinUpMemberAction                               INTEGER,
        	ltmPoolMinActiveMembers                                INTEGER,
        	ltmPoolActiveMemberCnt                                 INTEGER,
        	ltmPoolDisallowSnat                                    INTEGER,
        	ltmPoolDisallowNat                                     INTEGER,
        	ltmPoolSimpleTimeout                                   Integer32,
        	ltmPoolIpTosToClient                                   INTEGER,
        	ltmPoolIpTosToServer                                   INTEGER,
        	ltmPoolLinkQosToClient                                 INTEGER,
        	ltmPoolLinkQosToServer                                 INTEGER,
        	ltmPoolDynamicRatioSum                                 Integer32,
        	ltmPoolMonitorRule                                     LongDisplayString,
        	ltmPoolAvailabilityState                               INTEGER,
        	ltmPoolEnabledState                                    INTEGER,
        	ltmPoolDisabledParentType                              Integer32,
        	ltmPoolStatusReason                                    LongDisplayString,
        	ltmPoolSlowRampTime                                    Integer32,
        	ltmPoolMemberCnt                                       Integer32
	}

ltmPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a pool."
	::= { ltmPoolEntry 1 } 

ltmPoolLbMode OBJECT-TYPE 
	SYNTAX INTEGER {
		roundRobin(0),
		ratioMember(1),
		leastConnMember(2),
		observedMember(3),
		predictiveMember(4),
		ratioNodeAddress(5),
		leastConnNodeAddress(6),
		fastestNodeAddress(7),
		observedNodeAddress(8),
		predictiveNodeAddress(9),
		dynamicRatio(10),
		fastestAppResponse(11),
		leastSessions(12),
		dynamicRatioMember(13),
		l3Addr(14)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The load balance method for this pool"
	::= { ltmPoolEntry 2 } 

ltmPoolActionOnServiceDown OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		reset(1),
		drop(2),
		reselect(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The action to be taken if the service for the specified pool is down."
	::= { ltmPoolEntry 3 } 

ltmPoolMinUpMembers OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The minimum number of UP members required for the specified pool 
		before a high availability action to be taken. 
		This is used when ltmPoolMinUpMembersEnable is true."
	::= { ltmPoolEntry 4 } 

ltmPoolMinUpMembersEnable OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not an action will be taken when the 
		minimum number of UP members requirement is not met for the specified pool."
	::= { ltmPoolEntry 5 } 

ltmPoolMinUpMemberAction OBJECT-TYPE 
	SYNTAX INTEGER {
		unusedhaaction(0),
		reboot(1),
		restart(2),
		failover(3),
		goactive(4),
		noaction(5),
		restartall(6),
		failoveraborttm(7),
		gooffline(8),
		goofflinerestart(9),
		goofflineaborttm(10),
		goofflinedownlinks(11),
		goofflinedownlinksrestart(12)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The action to be taken if the minimum number of UP members requirement 
		is not met for the specified pool. This is used when 
		ltmPoolMinUpMembersEnable is true."
	::= { ltmPoolEntry 6 } 

ltmPoolMinActiveMembers OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The minimum number of active members required for traffic to be sent to 
		the specified pool. This feature is used for priority pools. The minimum 
		active members take into account both the status of the pool member (up/down) 
		as well as the number of connections present on the pool member.  
		If the number of active members falls below this given threshold, 
		traffic is sent to the next priority pool."
	::= { ltmPoolEntry 7 } 

ltmPoolActiveMemberCnt OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of the current active members in the specified pool."
	::= { ltmPoolEntry 8 } 

ltmPoolDisallowSnat OBJECT-TYPE 
	SYNTAX INTEGER {
		allowed(0),
		disallowed(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state whether SNAT is disallowed or not for the specified pool."
	::= { ltmPoolEntry 9 } 

ltmPoolDisallowNat OBJECT-TYPE 
	SYNTAX INTEGER {
		allowed(0),
		disallowed(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state whether NAT is disallowed or not for the specified pool."
	::= { ltmPoolEntry 10 } 

ltmPoolSimpleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The timeout (in seconds) in simple persistence for the specified pool."
	::= { ltmPoolEntry 11 } 

ltmPoolIpTosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP ToS value for client traffic for the specified pool."
	::= { ltmPoolEntry 12 } 

ltmPoolIpTosToServer OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP ToS value for server traffic for the specified pool."
	::= { ltmPoolEntry 13 } 

ltmPoolLinkQosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The link QoS value for client traffic for the specified pool."
	::= { ltmPoolEntry 14 } 

ltmPoolLinkQosToServer OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The link QoS value for server traffic for the specified pool."
	::= { ltmPoolEntry 15 } 

ltmPoolDynamicRatioSum OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The sum of the dynamic ratio from all the members of the specified pool."
	::= { ltmPoolEntry 16 } 

ltmPoolMonitorRule OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of monitor rule used by the specified pool."
	::= { ltmPoolEntry 17 } 

ltmPoolAvailabilityState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPooltatusAvailState under ltmPoolStatus.
		The state of the specified pool availability indicated in color."
	::= { ltmPoolEntry 18 } 

ltmPoolEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPoolStatusEnabledState under ltmPoolStatus.
		The state of the specified pool activity status, as specified by the user."
	::= { ltmPoolEntry 19 } 

ltmPoolDisabledParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPoolStatusParentType under ltmPoolStatus.
		The type of parent object which disabled the specified pool."
	::= { ltmPoolEntry 20 } 

ltmPoolStatusReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPoolStatusDetailReason under ltmPoolStatus.
		The detail description of the pool's status of parent object 
		which disabled the specified pool."
	::= { ltmPoolEntry 21 } 

ltmPoolSlowRampTime OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The ramp-up time (in seconds) to gradually ramp up the load 
		on newly added or freshly detected UP pool members."
	::= { ltmPoolEntry 22 } 

ltmPoolMemberCnt OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of members in the specified pool."
	::= { ltmPoolEntry 23 } 

--==================================================================
-- Pool_stat
--==================================================================
ltmPoolStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmPoolStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmPoolStat 1 } 

ltmPoolStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmPoolStat entries in the table."
	::= { ltmPoolStat 2 } 

ltmPoolStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmPoolStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of pools."
	::= { ltmPoolStat 3 } 

ltmPoolStatEntry OBJECT-TYPE
	SYNTAX  LtmPoolStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmPoolStat Table"
	INDEX {
		ltmPoolStatName
	}
	::= { ltmPoolStatTable 1 } 

LtmPoolStatEntry ::= 
	SEQUENCE {
        	ltmPoolStatName                                        LongDisplayString,
        	ltmPoolStatServerPktsIn                                Counter64,
        	ltmPoolStatServerBytesIn                               Counter64,
        	ltmPoolStatServerPktsOut                               Counter64,
        	ltmPoolStatServerBytesOut                              Counter64,
        	ltmPoolStatServerMaxConns                              Counter64,
        	ltmPoolStatServerTotConns                              Counter64,
        	ltmPoolStatServerCurConns                              Counter64,
        	ltmPoolStatPvaPktsIn                                   Counter64,
        	ltmPoolStatPvaBytesIn                                  Counter64,
        	ltmPoolStatPvaPktsOut                                  Counter64,
        	ltmPoolStatPvaBytesOut                                 Counter64,
        	ltmPoolStatPvaMaxConns                                 Counter64,
        	ltmPoolStatPvaTotConns                                 Counter64,
        	ltmPoolStatPvaCurConns                                 Counter64,
        	ltmPoolStatTotPvaAssistConn                            Counter64,
        	ltmPoolStatCurrPvaAssistConn                           Counter64
	}

ltmPoolStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of this pool."
	::= { ltmPoolStatEntry 1 } 

ltmPoolStatServerPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received by the specified pool from server-side."
	::= { ltmPoolStatEntry 2 } 

ltmPoolStatServerBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received by the specified pool from server-side."
	::= { ltmPoolStatEntry 3 } 

ltmPoolStatServerPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to server-side from the specified pool."
	::= { ltmPoolStatEntry 4 } 

ltmPoolStatServerBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to server-side from the specified pool."
	::= { ltmPoolStatEntry 5 } 

ltmPoolStatServerMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from server-side to the specified pool."
	::= { ltmPoolStatEntry 6 } 

ltmPoolStatServerTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from server-side to the specified pool."
	::= { ltmPoolStatEntry 7 } 

ltmPoolStatServerCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from server-side to the specified pool."
	::= { ltmPoolStatEntry 8 } 

ltmPoolStatPvaPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated packets received by the specified pool."
	::= { ltmPoolStatEntry 9 } 

ltmPoolStatPvaBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated bytes received by the specified pool."
	::= { ltmPoolStatEntry 10 } 

ltmPoolStatPvaPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated packets sent out from the specified pool."
	::= { ltmPoolStatEntry 11 } 

ltmPoolStatPvaBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated bytes sent out from the specified pool."
	::= { ltmPoolStatEntry 12 } 

ltmPoolStatPvaMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum hardware accelerated connections to the specified pool."
	::= { ltmPoolStatEntry 13 } 

ltmPoolStatPvaTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total hardware accelerated connections to the specified pool."
	::= { ltmPoolStatEntry 14 } 

ltmPoolStatPvaCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current hardware accelerated connections to the specified pool."
	::= { ltmPoolStatEntry 15 } 

ltmPoolStatTotPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections to the specified pool, 
		which are partially hardware accelerated."
	::= { ltmPoolStatEntry 16 } 

ltmPoolStatCurrPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of connections to the specified pool, 
		which are partially hardware accelerated."
	::= { ltmPoolStatEntry 17 } 

--==================================================================
-- Pool_member
--==================================================================
ltmPoolMemberNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmPoolMember entries in the table."
	::= { ltmPoolMember 1 } 

ltmPoolMemberTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmPoolMemberEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of pool members."
	::= { ltmPoolMember 2 } 

ltmPoolMemberEntry OBJECT-TYPE
	SYNTAX  LtmPoolMemberEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmPoolMember Table"
	INDEX {
		ltmPoolMemberPoolName,
		ltmPoolMemberAddrType,
		ltmPoolMemberAddr,
		ltmPoolMemberPort
	}
	::= { ltmPoolMemberTable 1 } 

LtmPoolMemberEntry ::= 
	SEQUENCE {
        	ltmPoolMemberPoolName                                  LongDisplayString,
        	ltmPoolMemberAddrType                                  InetAddressType,
        	ltmPoolMemberAddr                                      InetAddress,
        	ltmPoolMemberPort                                      INTEGER,
        	ltmPoolMemberConnLimit                                 Integer32,
        	ltmPoolMemberRatio                                     Integer32,
        	ltmPoolMemberWeight                                    INTEGER,
        	ltmPoolMemberPriority                                  INTEGER,
        	ltmPoolMemberDynamicRatio                              INTEGER,
        	ltmPoolMemberMonitorState                              INTEGER,
        	ltmPoolMemberMonitorStatus                             INTEGER,
        	ltmPoolMemberNewSessionEnable                          INTEGER,
        	ltmPoolMemberSessionStatus                             INTEGER,
        	ltmPoolMemberMonitorRule                               LongDisplayString,
        	ltmPoolMemberAvailabilityState                         INTEGER,
        	ltmPoolMemberEnabledState                              INTEGER,
        	ltmPoolMemberDisabledParentType                        Integer32,
        	ltmPoolMemberStatusReason                              LongDisplayString
	}

ltmPoolMemberPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a pool."
	::= { ltmPoolMemberEntry 1 } 

ltmPoolMemberAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmPoolMemberAddr."
	::= { ltmPoolMemberEntry 2 } 

ltmPoolMemberAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a pool member in the specified pool.  
		It is interpreted within the context of an ltmPoolMemberAddrType value."
	::= { ltmPoolMemberEntry 3 } 

ltmPoolMemberPort OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The port number of the specified pool member."
	::= { ltmPoolMemberEntry 4 } 

ltmPoolMemberConnLimit OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections allowed to the specified pool member."
	::= { ltmPoolMemberEntry 5 } 

ltmPoolMemberRatio OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The load balancing ratio of the specified pool member, 
		used in pool member ratio load balancing mode."
	::= { ltmPoolMemberEntry 6 } 

ltmPoolMemberWeight OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The weight of the specified pool member, used in dynamic load balancing mode."
	::= { ltmPoolMemberEntry 7 } 

ltmPoolMemberPriority OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The priority level of the specified pool member, 
		used in priority pool member load balancing mode."
	::= { ltmPoolMemberEntry 8 } 

ltmPoolMemberDynamicRatio OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The dynamic ratio for the specified pool member, used in load balance 
		 algorithm."
	::= { ltmPoolMemberEntry 9 } 

ltmPoolMemberMonitorState OBJECT-TYPE 
	SYNTAX INTEGER {
		unchecked(0),
		checking(1),
		inband(2),
		forced-up(3),
		up(4),
		down(19),
		forced-down(20),
		irule-down(22),
		inband-down(23),
		down-manual-resume(24),
		disabled(25)
	}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The internal tmm monitor state for the specified node address."
	::= { ltmPoolMemberEntry 10 } 

ltmPoolMemberMonitorStatus OBJECT-TYPE 
	SYNTAX INTEGER {
		unchecked(0),
		checking(1),
		inband(2),
		forced-up(3),
		up(4),
		addr-down(18),
		down(19),
		forced-down(20),
		maint(21),
		irule-down(22),
		inband-down(23),
		down-manual-resume(24)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The hierarchical load balance state for the specified node address, including parent status. 
		 unchecked - enabled node that is not monitored;
		 checking  - initial state until monitor reports;
	         inband    - the tmm has marked the node up;
	     forced-up - forced up manually;
		 up        - enabled node when its monitors succeed;
		 addr-down   - node address monitor fails or forced down;
		 down        - enabled node when its monitors fail;
		 forced-down - node forced down manually;
		 maint       - in maintenance mode;
	         irule-down  - an iRule has marked the node down;
	         inband-down - the tmm has marked the node down;
	         down-manual-resume - the node is down and must be manually enabled; 
		 "
	::= { ltmPoolMemberEntry 11 } 

ltmPoolMemberNewSessionEnable OBJECT-TYPE 
	SYNTAX INTEGER {
		user-disabled(1),
		user-enabled(2),
		monitor-enabled(3),
		monitor-disabled(4)
	}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"Whether a new session can be enabled or not for the specified pool member."
	::= { ltmPoolMemberEntry 12 } 

ltmPoolMemberSessionStatus OBJECT-TYPE 
	SYNTAX INTEGER {
		enabled(1),
		addrdisabled(2),
		servdisabled(3),
		disabled(4),
		forceddisabled(5)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The hierarchical status of the session, including parent status,
		for the specified pool member.
		enabled        - new sessions enabled;
		addrdisabled   - new sessions disabled on node address;
		servdisabled   - new sessions disabled on node server;
		disabled       - new sessions disabled;
		forceddisabled - new sessions forced to be disabled."
	::= { ltmPoolMemberEntry 13 } 

ltmPoolMemberMonitorRule OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The monitor rule used by the specified pool member. 
		If this value is empty, ltmPoolMonitorRule will be used."
	::= { ltmPoolMemberEntry 14 } 

ltmPoolMemberAvailabilityState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPoolMbrStatusAvailState under ltmPoolMemberStatus.
		The state of the specified pool member availability indicated in color."
	::= { ltmPoolMemberEntry 15 } 

ltmPoolMemberEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPoolMbrStatusEnabledState under ltmPoolMemberStatus.
		The state of the specified pool member activity status, as specified 
		by the user."
	::= { ltmPoolMemberEntry 16 } 

ltmPoolMemberDisabledParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPoolMbrStatusParentType under ltmPoolMemberStatus.
		The type of parent object which disabled the specified pool member."
	::= { ltmPoolMemberEntry 17 } 

ltmPoolMemberStatusReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmPoolMbrStatusDetailReason under ltmPoolMemberStatus.
		The detail description of the pool member's status of parent object 
		which disabled the specified pool member."
	::= { ltmPoolMemberEntry 18 } 

--==================================================================
-- Pool_member_stat
--==================================================================
ltmPoolMemberStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmPoolMemberStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmPoolMemberStat 1 } 

ltmPoolMemberStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmPoolMemberStat entries in the table."
	::= { ltmPoolMemberStat 2 } 

ltmPoolMemberStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmPoolMemberStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of pool members."
	::= { ltmPoolMemberStat 3 } 

ltmPoolMemberStatEntry OBJECT-TYPE
	SYNTAX  LtmPoolMemberStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmPoolMemberStat Table"
	INDEX {
		ltmPoolMemberStatPoolName,
		ltmPoolMemberStatAddrType,
		ltmPoolMemberStatAddr,
		ltmPoolMemberStatPort
	}
	::= { ltmPoolMemberStatTable 1 } 

LtmPoolMemberStatEntry ::= 
	SEQUENCE {
        	ltmPoolMemberStatPoolName                              LongDisplayString,
        	ltmPoolMemberStatAddrType                              InetAddressType,
        	ltmPoolMemberStatAddr                                  InetAddress,
        	ltmPoolMemberStatPort                                  INTEGER,
        	ltmPoolMemberStatServerPktsIn                          Counter64,
        	ltmPoolMemberStatServerBytesIn                         Counter64,
        	ltmPoolMemberStatServerPktsOut                         Counter64,
        	ltmPoolMemberStatServerBytesOut                        Counter64,
        	ltmPoolMemberStatServerMaxConns                        Counter64,
        	ltmPoolMemberStatServerTotConns                        Counter64,
        	ltmPoolMemberStatServerCurConns                        Counter64,
        	ltmPoolMemberStatPvaPktsIn                             Counter64,
        	ltmPoolMemberStatPvaBytesIn                            Counter64,
        	ltmPoolMemberStatPvaPktsOut                            Counter64,
        	ltmPoolMemberStatPvaBytesOut                           Counter64,
        	ltmPoolMemberStatPvaMaxConns                           Counter64,
        	ltmPoolMemberStatPvaTotConns                           Counter64,
        	ltmPoolMemberStatPvaCurConns                           Counter64,
        	ltmPoolMemberStatTotRequests                           Counter64,
        	ltmPoolMemberStatTotPvaAssistConn                      Counter64,
        	ltmPoolMemberStatCurrPvaAssistConn                     Counter64
	}

ltmPoolMemberStatPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a pool."
	::= { ltmPoolMemberStatEntry 1 } 

ltmPoolMemberStatAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmPoolMemberStatAddr."
	::= { ltmPoolMemberStatEntry 2 } 

ltmPoolMemberStatAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a pool member in the specified pool.  
		It is interpreted within the context of an ltmPoolMemberStatAddrType value."
	::= { ltmPoolMemberStatEntry 3 } 

ltmPoolMemberStatPort OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The port number of the specified pool member."
	::= { ltmPoolMemberStatEntry 4 } 

ltmPoolMemberStatServerPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received by the specified pool member from server-side."
	::= { ltmPoolMemberStatEntry 5 } 

ltmPoolMemberStatServerBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received by the specified pool member from server-side."
	::= { ltmPoolMemberStatEntry 6 } 

ltmPoolMemberStatServerPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to server-side from the specified pool member."
	::= { ltmPoolMemberStatEntry 7 } 

ltmPoolMemberStatServerBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to server-side from the specified pool member."
	::= { ltmPoolMemberStatEntry 8 } 

ltmPoolMemberStatServerMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from server-side to the specified pool member."
	::= { ltmPoolMemberStatEntry 9 } 

ltmPoolMemberStatServerTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from server-side to the specified pool member."
	::= { ltmPoolMemberStatEntry 10 } 

ltmPoolMemberStatServerCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from server-side to the pool member."
	::= { ltmPoolMemberStatEntry 11 } 

ltmPoolMemberStatPvaPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated packets received by the specified pool member."
	::= { ltmPoolMemberStatEntry 12 } 

ltmPoolMemberStatPvaBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated bytes received by the specified pool member."
	::= { ltmPoolMemberStatEntry 13 } 

ltmPoolMemberStatPvaPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated packets sent out from the specified pool member."
	::= { ltmPoolMemberStatEntry 14 } 

ltmPoolMemberStatPvaBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated bytes sent out from the specified pool member."
	::= { ltmPoolMemberStatEntry 15 } 

ltmPoolMemberStatPvaMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum hardware accelerated connections to the specified pool member."
	::= { ltmPoolMemberStatEntry 16 } 

ltmPoolMemberStatPvaTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total hardware accelerated connections to the specified pool member."
	::= { ltmPoolMemberStatEntry 17 } 

ltmPoolMemberStatPvaCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current hardware accelerated connections to the specified pool member."
	::= { ltmPoolMemberStatEntry 18 } 

ltmPoolMemberStatTotRequests OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of requests going through the specified pool member."
	::= { ltmPoolMemberStatEntry 19 } 

ltmPoolMemberStatTotPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections to the specified pool member, 
		which are partially hardware accelerated."
	::= { ltmPoolMemberStatEntry 20 } 

ltmPoolMemberStatCurrPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of connections to the specified pool member, 
		which are partially hardware accelerated."
	::= { ltmPoolMemberStatEntry 21 } 

--==================================================================
-- Profile_auth
--==================================================================
ltmAuthProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmAuthProfile entries in the table."
	::= { ltmAuthProfile 1 } 

ltmAuthProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmAuthProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of BIGIP authentication profiles."
	::= { ltmAuthProfile 2 } 

ltmAuthProfileEntry OBJECT-TYPE
	SYNTAX  LtmAuthProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmAuthProfile Table"
	INDEX {
		ltmAuthProfileName
	}
	::= { ltmAuthProfileTable 1 } 

LtmAuthProfileEntry ::= 
	SEQUENCE {
        	ltmAuthProfileName                                     LongDisplayString,
        	ltmAuthProfileConfigSource                             INTEGER,
        	ltmAuthProfileDefaultName                              LongDisplayString,
        	ltmAuthProfileConfigName                               LongDisplayString,
        	ltmAuthProfileType                                     INTEGER,
        	ltmAuthProfileMode                                     INTEGER,
        	ltmAuthProfileCredentialSource                         INTEGER,
        	ltmAuthProfileRuleName                                 LongDisplayString,
        	ltmAuthProfileIdleTimeout                              Integer32
	}

ltmAuthProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of an authentication profile."
	::= { ltmAuthProfileEntry 1 } 

ltmAuthProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmAuthProfileEntry 2 } 

ltmAuthProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmAuthProfileEntry 3 } 

ltmAuthProfileConfigName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the authentication configuration that the specified 
		profile will be using."
	::= { ltmAuthProfileEntry 4 } 

ltmAuthProfileType OBJECT-TYPE 
	SYNTAX INTEGER {
		ldap(0),
		radius(1),
		sslccldap(2),
		sslocsp(3),
		tacacs(4),
		generic(5),
		sslcrldp(6),
		krbdelegate(7)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The authentication type that the specified profile will be using."
	::= { ltmAuthProfileEntry 5 } 

ltmAuthProfileMode OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The mode for the specified auth profile."
	::= { ltmAuthProfileEntry 6 } 

ltmAuthProfileCredentialSource OBJECT-TYPE 
	SYNTAX INTEGER {
		httpbasicauth(0)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The source of the credentials that the specified profile will be using."
	::= { ltmAuthProfileEntry 7 } 

ltmAuthProfileRuleName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the rule that the specified profile will be using."
	::= { ltmAuthProfileEntry 8 } 

ltmAuthProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The idle timeout in seconds for the authentication session."
	::= { ltmAuthProfileEntry 9 } 

--==================================================================
-- Profile_auth_stat
--==================================================================
ltmAuthProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmAuthProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmAuthProfileStat 1 } 

ltmAuthProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmAuthProfileStat entries in the table."
	::= { ltmAuthProfileStat 2 } 

ltmAuthProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmAuthProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of BIGIP authentication profiles."
	::= { ltmAuthProfileStat 3 } 

ltmAuthProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmAuthProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmAuthProfileStat Table"
	INDEX {
		ltmAuthProfileStatName
	}
	::= { ltmAuthProfileStatTable 1 } 

LtmAuthProfileStatEntry ::= 
	SEQUENCE {
        	ltmAuthProfileStatName                                 LongDisplayString,
        	ltmAuthProfileStatTotSessions                          Counter64,
        	ltmAuthProfileStatCurSessions                          Counter64,
        	ltmAuthProfileStatMaxSessions                          Counter64,
        	ltmAuthProfileStatSuccessResults                       Counter64,
        	ltmAuthProfileStatFailureResults                       Counter64,
        	ltmAuthProfileStatWantcredentialResults                Counter64,
        	ltmAuthProfileStatErrorResults                         Counter64
	}

ltmAuthProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of an authentication profile."
	::= { ltmAuthProfileStatEntry 1 } 

ltmAuthProfileStatTotSessions OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of concurrent auth sessions for the specified profile."
	::= { ltmAuthProfileStatEntry 2 } 

ltmAuthProfileStatCurSessions OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of concurrent auth sessions for the specified profile."
	::= { ltmAuthProfileStatEntry 3 } 

ltmAuthProfileStatMaxSessions OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of concurrent auth sessions for the specified profile"
	::= { ltmAuthProfileStatEntry 4 } 

ltmAuthProfileStatSuccessResults OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of auth success results (That is when a 
		successful authorization has completed all of the required 
		auth services.) for the specified profile."
	::= { ltmAuthProfileStatEntry 5 } 

ltmAuthProfileStatFailureResults OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of auth failure results (That is when an 
		unsuccessful authorization operation has completed.) for the associated 
		virtual server for the specified profile."
	::= { ltmAuthProfileStatEntry 6 } 

ltmAuthProfileStatWantcredentialResults OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of auth wantcredential results (That is when 
		an authorization operation needs an additional credential.) 
		for the specified profile."
	::= { ltmAuthProfileStatEntry 7 } 

ltmAuthProfileStatErrorResults OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of auth error results (That is when an error 
		occurred during authorization has occurred.) for the specified profile."
	::= { ltmAuthProfileStatEntry 8 } 

--==================================================================
-- Profile_clientssl
--==================================================================
ltmClientSslNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmClientSslProfile entries in the table."
	::= { ltmClientSslProfile 1 } 

ltmClientSslTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmClientSslEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of the client-side SSL profiles.(BIG-IP acts as an SSL server)"
	::= { ltmClientSslProfile 2 } 

ltmClientSslEntry OBJECT-TYPE
	SYNTAX  LtmClientSslEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmClientSsl Table"
	INDEX {
		ltmClientSslName
	}
	::= { ltmClientSslTable 1 } 

LtmClientSslEntry ::= 
	SEQUENCE {
        	ltmClientSslName                                       LongDisplayString,
        	ltmClientSslConfigSource                               INTEGER,
        	ltmClientSslDefaultName                                LongDisplayString,
        	ltmClientSslMode                                       INTEGER,
        	ltmClientSslKey                                        LongDisplayString,
        	ltmClientSslCert                                       LongDisplayString,
        	ltmClientSslChain                                      LongDisplayString,
        	ltmClientSslCafile                                     LongDisplayString,
        	ltmClientSslCrlfile                                    LongDisplayString,
        	ltmClientSslClientcertca                               LongDisplayString,
        	ltmClientSslCiphers                                    LongDisplayString,
        	ltmClientSslPassphrase                                 LongDisplayString,
        	ltmClientSslOptions                                    Integer32,
        	ltmClientSslModsslmethods                              INTEGER,
        	ltmClientSslCacheSize                                  Integer32,
        	ltmClientSslCacheTimeout                               Integer32,
        	ltmClientSslRenegotiatePeriod                          Integer32,
        	ltmClientSslRenegotiateSize                            Integer32,
        	ltmClientSslRenegotiateMaxRecordDelay                  Integer32,
        	ltmClientSslHandshakeTimeout                           Integer32,
        	ltmClientSslAlertTimeout                               Integer32,
        	ltmClientSslPeerCertMode                               INTEGER,
        	ltmClientSslAuthenticateOnce                           INTEGER,
        	ltmClientSslAuthenticateDepth                          Integer32,
        	ltmClientSslUncleanShutdown                            INTEGER,
        	ltmClientSslStrictResume                               INTEGER,
        	ltmClientSslAllowNonssl                                INTEGER
	}

ltmClientSslName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a client-side SSL profile."
	::= { ltmClientSslEntry 1 } 

ltmClientSslConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmClientSslEntry 2 } 

ltmClientSslDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmClientSslEntry 3 } 

ltmClientSslMode OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The mode of this profile."
	::= { ltmClientSslEntry 4 } 

ltmClientSslKey OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The key file name."
	::= { ltmClientSslEntry 5 } 

ltmClientSslCert OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The certificate file name."
	::= { ltmClientSslEntry 6 } 

ltmClientSslChain OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The certificate chain file name."
	::= { ltmClientSslEntry 7 } 

ltmClientSslCafile OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The CA certificate file name."
	::= { ltmClientSslEntry 8 } 

ltmClientSslCrlfile OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The CRL file name."
	::= { ltmClientSslEntry 9 } 

ltmClientSslClientcertca OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The CA certificate file name."
	::= { ltmClientSslEntry 10 } 

ltmClientSslCiphers OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The set of ciphers available for client-side SSL negotiation."
	::= { ltmClientSslEntry 11 } 

ltmClientSslPassphrase OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The key passphrase (if any)."
	::= { ltmClientSslEntry 12 } 

ltmClientSslOptions OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SSL options. 
		SSLOPT_MICROSOFT_SESS_ID_BUG              = 1
		SSLOPT_NETSCAPE_CHALLENGE_BUG             = 2
		SSLOPT_NETSCAPE_REUSE_CIPHER_CHANGE_BUG   = 8
		SSLOPT_SSLREF2_REUSE_CERT_TYPE_BUG        = 16
		SSLOPT_MICROSOFT_BIG_SSLV3_BUFFER         = 32
		SSLOPT_MSIE_SSLV2_RSA_PADDING             = 64
		SSLOPT_SSLEAY_080_CLIENT_DH_BUG           = 128
		SSLOPT_TLS_D5_BUG                         = 256
		SSLOPT_TLS_BLOCK_PADDING_BUG              = 512
		SSLOPT_DONT_INSERT_EMPTY_FRAGMENTS        = 2048
		SSLOPT_ALL_BUGFIXES                       = 4095
		SSLOPT_PASSIVE_CLOSE                      = 4096
		SSLOPT_NO_SESSION_RESUMPTION_ON_RENEGOTIATION = 65536
		SSLOPT_SINGLE_DH_USE                      = 1048576
		SSLOPT_EPHEMERAL_RSA                      = 2097152
		SSLOPT_CIPHER_SERVER_PREFERENCE           = 4194304
		SSLOPT_TLS_ROLLBACK_BUG                   = 8388608
		SSLOPT_NO_SSLv2                           = 16777216
		SSLOPT_NO_SSLv3                           = 33554432
		SSLOPT_NO_TLSv1                           = 67108864
		SSLOPT_PKCS1_CHECK_1                      = 134217728
		SSLOPT_PKCS1_CHECK_2                      = 268435456
		SSLOPT_NETSCAPE_CA_DN_BUG                 = 536870912
		SSLOPT_NETSCAPE_DEMO_CIPHER_CHANGE_BUG    = 1073741824"
	::= { ltmClientSslEntry 13 } 

ltmClientSslModsslmethods OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The ModSSL method emulation."
	::= { ltmClientSslEntry 14 } 

ltmClientSslCacheSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SSL session cache size."
	::= { ltmClientSslEntry 15 } 

ltmClientSslCacheTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SSL session cache timeout."
	::= { ltmClientSslEntry 16 } 

ltmClientSslRenegotiatePeriod OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Time-based trigger."
	::= { ltmClientSslEntry 17 } 

ltmClientSslRenegotiateSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Throughput-based trigger MB."
	::= { ltmClientSslEntry 18 } 

ltmClientSslRenegotiateMaxRecordDelay OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The timeout of renegotiation."
	::= { ltmClientSslEntry 19 } 

ltmClientSslHandshakeTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The handshake timeout in seconds."
	::= { ltmClientSslEntry 20 } 

ltmClientSslAlertTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The alert timeout in seconds."
	::= { ltmClientSslEntry 21 } 

ltmClientSslPeerCertMode OBJECT-TYPE 
	SYNTAX INTEGER {
		ignore(0),
		require(1),
		request(2),
		auto(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The mode of peer certification."
	::= { ltmClientSslEntry 22 } 

ltmClientSslAuthenticateOnce OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The feature to request client cert once or with each SSL
		session renegotiation."
	::= { ltmClientSslEntry 23 } 

ltmClientSslAuthenticateDepth OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum traversal depth for client certificate chain."
	::= { ltmClientSslEntry 24 } 

ltmClientSslUncleanShutdown OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state of shutdown for this SSL, whether it is unclean 
		 shutdown (not sending a close notification alert when closing 
		 connection.)."
	::= { ltmClientSslEntry 25 } 

ltmClientSslStrictResume OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Whether to enforce strict SSL session resumption 
		 per RFC2246"
	::= { ltmClientSslEntry 26 } 

ltmClientSslAllowNonssl OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Whether to allow non-SSL connections to pass through as 
		cleartext."
	::= { ltmClientSslEntry 27 } 

--==================================================================
-- Profile_clientssl_stat
--==================================================================
ltmClientSslStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmClientSslProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmClientSslProfileStat 1 } 

ltmClientSslStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmClientSslProfileStat entries in the table."
	::= { ltmClientSslProfileStat 2 } 

ltmClientSslStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmClientSslStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of the client-side SSL profiles.(BIG-IP acts as an SSL server)"
	::= { ltmClientSslProfileStat 3 } 

ltmClientSslStatEntry OBJECT-TYPE
	SYNTAX  LtmClientSslStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmClientSslStat Table"
	INDEX {
		ltmClientSslStatName
	}
	::= { ltmClientSslStatTable 1 } 

LtmClientSslStatEntry ::= 
	SEQUENCE {
        	ltmClientSslStatName                                   LongDisplayString,
        	ltmClientSslStatCurConns                               Counter64,
        	ltmClientSslStatMaxConns                               Counter64,
        	ltmClientSslStatCurNativeConns                         Counter64,
        	ltmClientSslStatMaxNativeConns                         Counter64,
        	ltmClientSslStatTotNativeConns                         Counter64,
        	ltmClientSslStatCurCompatConns                         Counter64,
        	ltmClientSslStatMaxCompatConns                         Counter64,
        	ltmClientSslStatTotCompatConns                         Counter64,
        	ltmClientSslStatEncryptedBytesIn                       Counter64,
        	ltmClientSslStatEncryptedBytesOut                      Counter64,
        	ltmClientSslStatDecryptedBytesIn                       Counter64,
        	ltmClientSslStatDecryptedBytesOut                      Counter64,
        	ltmClientSslStatRecordsIn                              Counter64,
        	ltmClientSslStatRecordsOut                             Counter64,
        	ltmClientSslStatFullyHwAcceleratedConns                Counter64,
        	ltmClientSslStatPartiallyHwAcceleratedConns            Counter64,
        	ltmClientSslStatNonHwAcceleratedConns                  Counter64,
        	ltmClientSslStatPrematureDisconnects                   Counter64,
        	ltmClientSslStatMidstreamRenegotiations                Counter64,
        	ltmClientSslStatSessCacheCurEntries                    Counter64,
        	ltmClientSslStatSessCacheHits                          Counter64,
        	ltmClientSslStatSessCacheLookups                       Counter64,
        	ltmClientSslStatSessCacheOverflows                     Counter64,
        	ltmClientSslStatSessCacheInvalidations                 Counter64,
        	ltmClientSslStatPeercertValid                          Counter64,
        	ltmClientSslStatPeercertInvalid                        Counter64,
        	ltmClientSslStatPeercertNone                           Counter64,
        	ltmClientSslStatHandshakeFailures                      Counter64,
        	ltmClientSslStatBadRecords                             Counter64,
        	ltmClientSslStatFatalAlerts                            Counter64,
        	ltmClientSslStatSslv2                                  Counter64,
        	ltmClientSslStatSslv3                                  Counter64,
        	ltmClientSslStatTlsv1                                  Counter64,
        	ltmClientSslStatAdhKeyxchg                             Counter64,
        	ltmClientSslStatDhDssKeyxchg                           Counter64,
        	ltmClientSslStatDhRsaKeyxchg                           Counter64,
        	ltmClientSslStatDssKeyxchg                             Counter64,
        	ltmClientSslStatEdhDssKeyxchg                          Counter64,
        	ltmClientSslStatRsaKeyxchg                             Counter64,
        	ltmClientSslStatNullBulk                               Counter64,
        	ltmClientSslStatAesBulk                                Counter64,
        	ltmClientSslStatDesBulk                                Counter64,
        	ltmClientSslStatIdeaBulk                               Counter64,
        	ltmClientSslStatRc2Bulk                                Counter64,
        	ltmClientSslStatRc4Bulk                                Counter64,
        	ltmClientSslStatNullDigest                             Counter64,
        	ltmClientSslStatMd5Digest                              Counter64,
        	ltmClientSslStatShaDigest                              Counter64,
        	ltmClientSslStatNotssl                                 Counter64,
        	ltmClientSslStatEdhRsaKeyxchg                          Counter64
	}

ltmClientSslStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a client-side SSL  profile."
	::= { ltmClientSslStatEntry 1 } 

ltmClientSslStatCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of concurrent connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 2 } 

ltmClientSslStatMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of concurrent connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 3 } 

ltmClientSslStatCurNativeConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of concurrent native connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 4 } 

ltmClientSslStatMaxNativeConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of concurrent native connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 5 } 

ltmClientSslStatTotNativeConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of concurrent native connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 6 } 

ltmClientSslStatCurCompatConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of concurrent compat connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 7 } 

ltmClientSslStatMaxCompatConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of concurrent compat connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 8 } 

ltmClientSslStatTotCompatConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of concurrent compat connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmClientSslStatEntry 9 } 

ltmClientSslStatEncryptedBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total encrypted bytes received."
	::= { ltmClientSslStatEntry 10 } 

ltmClientSslStatEncryptedBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total encrypted bytes sent."
	::= { ltmClientSslStatEntry 11 } 

ltmClientSslStatDecryptedBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total decrypted bytes received."
	::= { ltmClientSslStatEntry 12 } 

ltmClientSslStatDecryptedBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total decrypted bytes sent."
	::= { ltmClientSslStatEntry 13 } 

ltmClientSslStatRecordsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total records received."
	::= { ltmClientSslStatEntry 14 } 

ltmClientSslStatRecordsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total records sent."
	::= { ltmClientSslStatEntry 15 } 

ltmClientSslStatFullyHwAcceleratedConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Fully hardware-accelerated implies usage of the Cavium 
		 Nitrox or similar hardware accelerator such that all 
		 significant cryptographic operations are offloaded, 
		 including but not limited to the SSL handshake (at least 
		 the RSA/DSA/DH operations) and record processing (at least 
		 the bulk cipher plus MAC)."
	::= { ltmClientSslStatEntry 16 } 

ltmClientSslStatPartiallyHwAcceleratedConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Partially hardware-accelerated indicates that at least the 
		 RSA decryptions are offloaded."
	::= { ltmClientSslStatEntry 17 } 

ltmClientSslStatNonHwAcceleratedConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Non-accelerated connections are those for which no 
		 steady-state hardware acceleration is available (either 
		 because no hardware accelerators are available or because 
		 the necessary cryptographic operations are unsupported).  
		 Because the extent of hardware acceleration may not be known 
		 until a connection has closed (mid-stream SSL handshakes 
		 might renegotiate an SSL session not supported by hardware 
		 acceleration), this statistic will not be updated for a  
		 given connection until it has closed."
	::= { ltmClientSslStatEntry 18 } 

ltmClientSslStatPrematureDisconnects OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections disconnected before SSL session 
		 establishment: the total number of connections that were 
		 prematurely closed before an SSL session was established, 
		 not including connections in passthrough mode."
	::= { ltmClientSslStatEntry 19 } 

ltmClientSslStatMidstreamRenegotiations OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of mid-stream SSL re-negotiations, not including 
		 initial SSL session establishment."
	::= { ltmClientSslStatEntry 20 } 

ltmClientSslStatSessCacheCurEntries OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of the current entries in this cache."
	::= { ltmClientSslStatEntry 21 } 

ltmClientSslStatSessCacheHits OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the cache hits."
	::= { ltmClientSslStatEntry 22 } 

ltmClientSslStatSessCacheLookups OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the cache lookups."
	::= { ltmClientSslStatEntry 23 } 

ltmClientSslStatSessCacheOverflows OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the cache overflows."
	::= { ltmClientSslStatEntry 24 } 

ltmClientSslStatSessCacheInvalidations OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the session invalidations."
	::= { ltmClientSslStatEntry 25 } 

ltmClientSslStatPeercertValid OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the valid certificates."
	::= { ltmClientSslStatEntry 26 } 

ltmClientSslStatPeercertInvalid OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the invalid certificates."
	::= { ltmClientSslStatEntry 27 } 

ltmClientSslStatPeercertNone OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections without certificates."
	::= { ltmClientSslStatEntry 28 } 

ltmClientSslStatHandshakeFailures OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of handshake failures."
	::= { ltmClientSslStatEntry 29 } 

ltmClientSslStatBadRecords OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the bad records."
	::= { ltmClientSslStatEntry 30 } 

ltmClientSslStatFatalAlerts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the fatal alerts."
	::= { ltmClientSslStatEntry 31 } 

ltmClientSslStatSslv2 OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections for SSL protocol version 2."
	::= { ltmClientSslStatEntry 32 } 

ltmClientSslStatSslv3 OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections for SSL protocol version 3."
	::= { ltmClientSslStatEntry 33 } 

ltmClientSslStatTlsv1 OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections for SSL TLS protocol version 1."
	::= { ltmClientSslStatEntry 34 } 

ltmClientSslStatAdhKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The anonymous Diffie-Hellman."
	::= { ltmClientSslStatEntry 35 } 

ltmClientSslStatDhDssKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! DSS certificate is obsolete in BIGIP.
		The diffie-Hellman w/ DSS certificate."
	::= { ltmClientSslStatEntry 36 } 

ltmClientSslStatDhRsaKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The diffie-Hellman w/ RSA certificate."
	::= { ltmClientSslStatEntry 37 } 

ltmClientSslStatDssKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! DSS certificate is obsolete in BIGIP.
		The DSS certificate."
	::= { ltmClientSslStatEntry 38 } 

ltmClientSslStatEdhDssKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! DSS certificate is obsolete in BIGIP.
		The ephemeral Diffie-Hellman w/ DSS cert."
	::= { ltmClientSslStatEntry 39 } 

ltmClientSslStatRsaKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The RSA certificate."
	::= { ltmClientSslStatEntry 40 } 

ltmClientSslStatNullBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"No encryption."
	::= { ltmClientSslStatEntry 41 } 

ltmClientSslStatAesBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Advances Encryption Standard (CBC)."
	::= { ltmClientSslStatEntry 42 } 

ltmClientSslStatDesBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Digital Encryption Standard (CBC)."
	::= { ltmClientSslStatEntry 43 } 

ltmClientSslStatIdeaBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"IDEA (old SSLv2 cipher)."
	::= { ltmClientSslStatEntry 44 } 

ltmClientSslStatRc2Bulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Rivest Cipher 2 (CBC)."
	::= { ltmClientSslStatEntry 45 } 

ltmClientSslStatRc4Bulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Rivest Cipher 4 (CBC)."
	::= { ltmClientSslStatEntry 46 } 

ltmClientSslStatNullDigest OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"No message authentication."
	::= { ltmClientSslStatEntry 47 } 

ltmClientSslStatMd5Digest OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Message Digest 5."
	::= { ltmClientSslStatEntry 48 } 

ltmClientSslStatShaDigest OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Secure Hash Algorithm."
	::= { ltmClientSslStatEntry 49 } 

ltmClientSslStatNotssl OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the bad client greetings."
	::= { ltmClientSslStatEntry 50 } 

ltmClientSslStatEdhRsaKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Ephemeral Diffie-Hellman w/ RSA cert."
	::= { ltmClientSslStatEntry 51 } 

--==================================================================
-- Profile_serverssl
--==================================================================
ltmServerSslNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmServerSslProfile entries in the table."
	::= { ltmServerSslProfile 1 } 

ltmServerSslTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmServerSslEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of the server-side SSL profiles.(BIG-IP acts as an SSL client)"
	::= { ltmServerSslProfile 2 } 

ltmServerSslEntry OBJECT-TYPE
	SYNTAX  LtmServerSslEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmServerSsl Table"
	INDEX {
		ltmServerSslName
	}
	::= { ltmServerSslTable 1 } 

LtmServerSslEntry ::= 
	SEQUENCE {
        	ltmServerSslName                                       LongDisplayString,
        	ltmServerSslConfigSource                               INTEGER,
        	ltmServerSslDefaultName                                LongDisplayString,
        	ltmServerSslMode                                       INTEGER,
        	ltmServerSslKey                                        LongDisplayString,
        	ltmServerSslCert                                       LongDisplayString,
        	ltmServerSslChain                                      LongDisplayString,
        	ltmServerSslCafile                                     LongDisplayString,
        	ltmServerSslCrlfile                                    LongDisplayString,
        	ltmServerSslCiphers                                    LongDisplayString,
        	ltmServerSslPassphrase                                 LongDisplayString,
        	ltmServerSslOptions                                    Integer32,
        	ltmServerSslModsslmethods                              INTEGER,
        	ltmServerSslRenegotiatePeriod                          Integer32,
        	ltmServerSslRenegotiateSize                            Integer32,
        	ltmServerSslPeerCertMode                               INTEGER,
        	ltmServerSslAuthenticateOnce                           INTEGER,
        	ltmServerSslAuthenticateDepth                          Integer32,
        	ltmServerSslAuthenticateName                           LongDisplayString,
        	ltmServerSslUncleanShutdown                            INTEGER,
        	ltmServerSslStrictResume                               INTEGER,
        	ltmServerSslHandshakeTimeout                           Integer32,
        	ltmServerSslAlertTimeout                               Integer32,
        	ltmServerSslCacheSize                                  Integer32,
        	ltmServerSslCacheTimeout                               Integer32
	}

ltmServerSslName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a server-side SSL  profile."
	::= { ltmServerSslEntry 1 } 

ltmServerSslConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmServerSslEntry 2 } 

ltmServerSslDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmServerSslEntry 3 } 

ltmServerSslMode OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The status of this profile."
	::= { ltmServerSslEntry 4 } 

ltmServerSslKey OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The key file name."
	::= { ltmServerSslEntry 5 } 

ltmServerSslCert OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The certificate file name."
	::= { ltmServerSslEntry 6 } 

ltmServerSslChain OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The certificate chain file name."
	::= { ltmServerSslEntry 7 } 

ltmServerSslCafile OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The CA certificate file name."
	::= { ltmServerSslEntry 8 } 

ltmServerSslCrlfile OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The CRL file name."
	::= { ltmServerSslEntry 9 } 

ltmServerSslCiphers OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The set of ciphers available for server-side SSL negotiation."
	::= { ltmServerSslEntry 10 } 

ltmServerSslPassphrase OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The key passphrase (if any)."
	::= { ltmServerSslEntry 11 } 

ltmServerSslOptions OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SSL options. 
		SSLOPT_MICROSOFT_SESS_ID_BUG              = 1
		SSLOPT_NETSCAPE_CHALLENGE_BUG             = 2
		SSLOPT_NETSCAPE_REUSE_CIPHER_CHANGE_BUG   = 8
		SSLOPT_SSLREF2_REUSE_CERT_TYPE_BUG        = 16
		SSLOPT_MICROSOFT_BIG_SSLV3_BUFFER         = 32
		SSLOPT_MSIE_SSLV2_RSA_PADDING             = 64
		SSLOPT_SSLEAY_080_CLIENT_DH_BUG           = 128
		SSLOPT_TLS_D5_BUG                         = 256
		SSLOPT_TLS_BLOCK_PADDING_BUG              = 512
		SSLOPT_DONT_INSERT_EMPTY_FRAGMENTS        = 2048
		SSLOPT_ALL_BUGFIXES                       = 4095
		SSLOPT_PASSIVE_CLOSE                      = 4096
		SSLOPT_NO_SESSION_RESUMPTION_ON_RENEGOTIATION = 65536
		SSLOPT_SINGLE_DH_USE                      = 1048576
		SSLOPT_EPHEMERAL_RSA                      = 2097152
		SSLOPT_CIPHER_SERVER_PREFERENCE           = 4194304
		SSLOPT_TLS_ROLLBACK_BUG                   = 8388608
		SSLOPT_NO_SSLv2                           = 16777216
		SSLOPT_NO_SSLv3                           = 33554432
		SSLOPT_NO_TLSv1                           = 67108864
		SSLOPT_PKCS1_CHECK_1                      = 134217728
		SSLOPT_PKCS1_CHECK_2                      = 268435456
		SSLOPT_NETSCAPE_CA_DN_BUG                 = 536870912
		SSLOPT_NETSCAPE_DEMO_CIPHER_CHANGE_BUG    = 1073741824"
	::= { ltmServerSslEntry 12 } 

ltmServerSslModsslmethods OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The status of using ModSSL method emulation."
	::= { ltmServerSslEntry 13 } 

ltmServerSslRenegotiatePeriod OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Time-based trigger."
	::= { ltmServerSslEntry 14 } 

ltmServerSslRenegotiateSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Throughput-based trigger MB."
	::= { ltmServerSslEntry 15 } 

ltmServerSslPeerCertMode OBJECT-TYPE 
	SYNTAX INTEGER {
		ignore(0),
		require(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The mode of peer certification."
	::= { ltmServerSslEntry 16 } 

ltmServerSslAuthenticateOnce OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The feature to request server cert with each SSL session 
		renegotiation."
	::= { ltmServerSslEntry 17 } 

ltmServerSslAuthenticateDepth OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The max traversal depth for client certificate chain."
	::= { ltmServerSslEntry 18 } 

ltmServerSslAuthenticateName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The expected server certificate DN(Domain Name)."
	::= { ltmServerSslEntry 19 } 

ltmServerSslUncleanShutdown OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state of shutdown for this SSL, whether it is unclean 
		 shutdown (not sending a close notification alert when closing 
		 connection.)."
	::= { ltmServerSslEntry 20 } 

ltmServerSslStrictResume OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The feature whether to enforce strict SSL session resumption 
		 per RFC2246"
	::= { ltmServerSslEntry 21 } 

ltmServerSslHandshakeTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The handshake timeout in seconds."
	::= { ltmServerSslEntry 22 } 

ltmServerSslAlertTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The alert timeout in seconds."
	::= { ltmServerSslEntry 23 } 

ltmServerSslCacheSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SSL session cache size."
	::= { ltmServerSslEntry 24 } 

ltmServerSslCacheTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SSL session cache timeout."
	::= { ltmServerSslEntry 25 } 

--==================================================================
-- Profile_serverssl_stat
--==================================================================
ltmServerSslStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmServerSslProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmServerSslProfileStat 1 } 

ltmServerSslStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmServerSslProfileStat entries in the table."
	::= { ltmServerSslProfileStat 2 } 

ltmServerSslStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmServerSslStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of the server-side SSL profiles.(BIG-IP acts as an SSL client)"
	::= { ltmServerSslProfileStat 3 } 

ltmServerSslStatEntry OBJECT-TYPE
	SYNTAX  LtmServerSslStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmServerSslStat Table"
	INDEX {
		ltmServerSslStatName
	}
	::= { ltmServerSslStatTable 1 } 

LtmServerSslStatEntry ::= 
	SEQUENCE {
        	ltmServerSslStatName                                   LongDisplayString,
        	ltmServerSslStatCurConns                               Counter64,
        	ltmServerSslStatMaxConns                               Counter64,
        	ltmServerSslStatCurNativeConns                         Counter64,
        	ltmServerSslStatMaxNativeConns                         Counter64,
        	ltmServerSslStatTotNativeConns                         Counter64,
        	ltmServerSslStatCurCompatConns                         Counter64,
        	ltmServerSslStatMaxCompatConns                         Counter64,
        	ltmServerSslStatTotCompatConns                         Counter64,
        	ltmServerSslStatEncryptedBytesIn                       Counter64,
        	ltmServerSslStatEncryptedBytesOut                      Counter64,
        	ltmServerSslStatDecryptedBytesIn                       Counter64,
        	ltmServerSslStatDecryptedBytesOut                      Counter64,
        	ltmServerSslStatRecordsIn                              Counter64,
        	ltmServerSslStatRecordsOut                             Counter64,
        	ltmServerSslStatFullyHwAcceleratedConns                Counter64,
        	ltmServerSslStatPartiallyHwAcceleratedConns            Counter64,
        	ltmServerSslStatNonHwAcceleratedConns                  Counter64,
        	ltmServerSslStatPrematureDisconnects                   Counter64,
        	ltmServerSslStatMidstreamRenegotiations                Counter64,
        	ltmServerSslStatSessCacheCurEntries                    Counter64,
        	ltmServerSslStatSessCacheHits                          Counter64,
        	ltmServerSslStatSessCacheLookups                       Counter64,
        	ltmServerSslStatSessCacheOverflows                     Counter64,
        	ltmServerSslStatSessCacheInvalidations                 Counter64,
        	ltmServerSslStatPeercertValid                          Counter64,
        	ltmServerSslStatPeercertInvalid                        Counter64,
        	ltmServerSslStatPeercertNone                           Counter64,
        	ltmServerSslStatHandshakeFailures                      Counter64,
        	ltmServerSslStatBadRecords                             Counter64,
        	ltmServerSslStatFatalAlerts                            Counter64,
        	ltmServerSslStatSslv2                                  Counter64,
        	ltmServerSslStatSslv3                                  Counter64,
        	ltmServerSslStatTlsv1                                  Counter64,
        	ltmServerSslStatAdhKeyxchg                             Counter64,
        	ltmServerSslStatDhDssKeyxchg                           Counter64,
        	ltmServerSslStatDhRsaKeyxchg                           Counter64,
        	ltmServerSslStatDssKeyxchg                             Counter64,
        	ltmServerSslStatEdhDssKeyxchg                          Counter64,
        	ltmServerSslStatRsaKeyxchg                             Counter64,
        	ltmServerSslStatNullBulk                               Counter64,
        	ltmServerSslStatAesBulk                                Counter64,
        	ltmServerSslStatDesBulk                                Counter64,
        	ltmServerSslStatIdeaBulk                               Counter64,
        	ltmServerSslStatRc2Bulk                                Counter64,
        	ltmServerSslStatRc4Bulk                                Counter64,
        	ltmServerSslStatNullDigest                             Counter64,
        	ltmServerSslStatMd5Digest                              Counter64,
        	ltmServerSslStatShaDigest                              Counter64,
        	ltmServerSslStatNotssl                                 Counter64,
        	ltmServerSslStatEdhRsaKeyxchg                          Counter64
	}

ltmServerSslStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a server-side SSL profile."
	::= { ltmServerSslStatEntry 1 } 

ltmServerSslStatCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of concurrent connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 2 } 

ltmServerSslStatMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of concurrent connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 3 } 

ltmServerSslStatCurNativeConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of concurrent native connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 4 } 

ltmServerSslStatMaxNativeConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of concurrent native connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 5 } 

ltmServerSslStatTotNativeConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of concurrent native connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 6 } 

ltmServerSslStatCurCompatConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of concurrent compat connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 7 } 

ltmServerSslStatMaxCompatConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of concurrent compat connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 8 } 

ltmServerSslStatTotCompatConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of concurrent compat connections with 
		 established SSL sessions being maintained by the filter."
	::= { ltmServerSslStatEntry 9 } 

ltmServerSslStatEncryptedBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total encrypted bytes received."
	::= { ltmServerSslStatEntry 10 } 

ltmServerSslStatEncryptedBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total encrypted bytes sent."
	::= { ltmServerSslStatEntry 11 } 

ltmServerSslStatDecryptedBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total decrypted bytes received."
	::= { ltmServerSslStatEntry 12 } 

ltmServerSslStatDecryptedBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total decrypted bytes sent."
	::= { ltmServerSslStatEntry 13 } 

ltmServerSslStatRecordsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total records received."
	::= { ltmServerSslStatEntry 14 } 

ltmServerSslStatRecordsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total records sent."
	::= { ltmServerSslStatEntry 15 } 

ltmServerSslStatFullyHwAcceleratedConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Fully hardware-accelerated implies usage of the Cavium 
		 Nitrox or similar hardware accelerator such that all 
		 significant cryptographic operations are offloaded, 
		 including but not limited to the SSL handshake (at least 
		 the RSA/DSA/DH operations) and record processing (at least 
		 the bulk cipher plus MAC)."
	::= { ltmServerSslStatEntry 16 } 

ltmServerSslStatPartiallyHwAcceleratedConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Partially hardware-accelerated indicates that at least the 
		 RSA decryptions are offloaded."
	::= { ltmServerSslStatEntry 17 } 

ltmServerSslStatNonHwAcceleratedConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Non-accelerated connections are those for which no 
		 steady-state hardware acceleration is available (either 
		 because no hardware accelerators are available or because 
		 the necessary cryptographic operations are unsupported).  
		 Because the extent of hardware acceleration may not be known 
		 until a connection has closed (mid-stream SSL handshakes 
		 might renegotiate an SSL session not supported by hardware 
		 acceleration), this statistic will not be updated for a  
		 given connection until it has closed."
	::= { ltmServerSslStatEntry 18 } 

ltmServerSslStatPrematureDisconnects OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections disconnected before SSL session 
		 establishment: the total number of connections that were 
		 prematurely closed before an SSL session was established, 
		 not including connections in pass-through mode."
	::= { ltmServerSslStatEntry 19 } 

ltmServerSslStatMidstreamRenegotiations OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of mid-stream SSL re-negotiations, not including 
		 initial SSL session establishment."
	::= { ltmServerSslStatEntry 20 } 

ltmServerSslStatSessCacheCurEntries OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of the current entries in this cache."
	::= { ltmServerSslStatEntry 21 } 

ltmServerSslStatSessCacheHits OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the cache hits."
	::= { ltmServerSslStatEntry 22 } 

ltmServerSslStatSessCacheLookups OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the cache lookups."
	::= { ltmServerSslStatEntry 23 } 

ltmServerSslStatSessCacheOverflows OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the cache overflows."
	::= { ltmServerSslStatEntry 24 } 

ltmServerSslStatSessCacheInvalidations OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the session invalidations."
	::= { ltmServerSslStatEntry 25 } 

ltmServerSslStatPeercertValid OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the valid certificates."
	::= { ltmServerSslStatEntry 26 } 

ltmServerSslStatPeercertInvalid OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the invalid certificates."
	::= { ltmServerSslStatEntry 27 } 

ltmServerSslStatPeercertNone OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections without certificates."
	::= { ltmServerSslStatEntry 28 } 

ltmServerSslStatHandshakeFailures OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of handshake failures."
	::= { ltmServerSslStatEntry 29 } 

ltmServerSslStatBadRecords OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the bad records."
	::= { ltmServerSslStatEntry 30 } 

ltmServerSslStatFatalAlerts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the fatal alerts."
	::= { ltmServerSslStatEntry 31 } 

ltmServerSslStatSslv2 OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections for SSL protocol version 2."
	::= { ltmServerSslStatEntry 32 } 

ltmServerSslStatSslv3 OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections for SSL protocol version 3."
	::= { ltmServerSslStatEntry 33 } 

ltmServerSslStatTlsv1 OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections for SSL TLS protocol version 1."
	::= { ltmServerSslStatEntry 34 } 

ltmServerSslStatAdhKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The anonymous Diffie-Hellman."
	::= { ltmServerSslStatEntry 35 } 

ltmServerSslStatDhDssKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! DSS certificate is obsolete in BIGIP.
		The diffie-Hellman w/ DSS certificate."
	::= { ltmServerSslStatEntry 36 } 

ltmServerSslStatDhRsaKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The diffie-Hellman w/ RSA certificate."
	::= { ltmServerSslStatEntry 37 } 

ltmServerSslStatDssKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! DSS certificate is obsolete in BIGIP.
		The DSS certificate."
	::= { ltmServerSslStatEntry 38 } 

ltmServerSslStatEdhDssKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! DSS certificate is obsolete in BIGIP.
		The ephemeral Diffie-Hellman w/ DSS cert."
	::= { ltmServerSslStatEntry 39 } 

ltmServerSslStatRsaKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The RSA certificate."
	::= { ltmServerSslStatEntry 40 } 

ltmServerSslStatNullBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"No encryption."
	::= { ltmServerSslStatEntry 41 } 

ltmServerSslStatAesBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Advances Encryption Standard (CBC)."
	::= { ltmServerSslStatEntry 42 } 

ltmServerSslStatDesBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Digital Encryption Standard (CBC)."
	::= { ltmServerSslStatEntry 43 } 

ltmServerSslStatIdeaBulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"IDEA (old SSLv2 cipher)."
	::= { ltmServerSslStatEntry 44 } 

ltmServerSslStatRc2Bulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Rivest Cipher 2 (CBC)."
	::= { ltmServerSslStatEntry 45 } 

ltmServerSslStatRc4Bulk OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Rivest Cipher 4 (CBC)."
	::= { ltmServerSslStatEntry 46 } 

ltmServerSslStatNullDigest OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"No message authentication."
	::= { ltmServerSslStatEntry 47 } 

ltmServerSslStatMd5Digest OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Message Digest 5."
	::= { ltmServerSslStatEntry 48 } 

ltmServerSslStatShaDigest OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Secure Hash Algorithm."
	::= { ltmServerSslStatEntry 49 } 

ltmServerSslStatNotssl OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of the bad client greetings."
	::= { ltmServerSslStatEntry 50 } 

ltmServerSslStatEdhRsaKeyxchg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Ephemeral Diffie-Hellman w/ RSA cert."
	::= { ltmServerSslStatEntry 51 } 

--==================================================================
-- Profile_connpool
--==================================================================
ltmConnPoolProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmConnPoolProfile entries in the table."
	::= { ltmConnPoolProfile 1 } 

ltmConnPoolProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmConnPoolProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of connection pool profiles."
	::= { ltmConnPoolProfile 2 } 

ltmConnPoolProfileEntry OBJECT-TYPE
	SYNTAX  LtmConnPoolProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmConnPoolProfile Table"
	INDEX {
		ltmConnPoolProfileName
	}
	::= { ltmConnPoolProfileTable 1 } 

LtmConnPoolProfileEntry ::= 
	SEQUENCE {
        	ltmConnPoolProfileName                                 LongDisplayString,
        	ltmConnPoolProfileConfigSource                         INTEGER,
        	ltmConnPoolProfileDefaultName                          LongDisplayString,
        	ltmConnPoolProfileSrcMaskType                          InetAddressType,
        	ltmConnPoolProfileSrcMask                              InetAddress,
        	ltmConnPoolProfileMaxSize                              Integer32,
        	ltmConnPoolProfileMaxAge                               Integer32,
        	ltmConnPoolProfileMaxReuse                             Integer32,
        	ltmConnPoolProfileIdleTimeout                          Integer32
	}

ltmConnPoolProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a connection pool profile."
	::= { ltmConnPoolProfileEntry 1 } 

ltmConnPoolProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmConnPoolProfileEntry 2 } 

ltmConnPoolProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmConnPoolProfileEntry 3 } 

ltmConnPoolProfileSrcMaskType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmConnPoolSrcMask"
	::= { ltmConnPoolProfileEntry 4 } 

ltmConnPoolProfileSrcMask OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The mask applied to source address to determine eligibility 
		for reuse. It is interpreted within the context of an 
		ltmConnPoolSrcMaskType value."
	::= { ltmConnPoolProfileEntry 5 } 

ltmConnPoolProfileMaxSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of connections in pool."
	::= { ltmConnPoolProfileEntry 6 } 

ltmConnPoolProfileMaxAge OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum time in seconds to reuse of connections. 
		Don't reuse connections older than max_age seconds."
	::= { ltmConnPoolProfileEntry 7 } 

ltmConnPoolProfileMaxReuse OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum times to reuse of connections. 
		Don't reuse connections older than max_reuse times."
	::= { ltmConnPoolProfileEntry 8 } 

ltmConnPoolProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The idle timeout for connections in the pool."
	::= { ltmConnPoolProfileEntry 9 } 

--==================================================================
-- Profile_connpool_stat
--==================================================================
ltmConnPoolProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmConnPoolProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmConnPoolProfileStat 1 } 

ltmConnPoolProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmConnPoolProfileStat entries in the table."
	::= { ltmConnPoolProfileStat 2 } 

ltmConnPoolProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmConnPoolProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of connection pool profiles."
	::= { ltmConnPoolProfileStat 3 } 

ltmConnPoolProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmConnPoolProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmConnPoolProfileStat Table"
	INDEX {
		ltmConnPoolProfileStatName
	}
	::= { ltmConnPoolProfileStatTable 1 } 

LtmConnPoolProfileStatEntry ::= 
	SEQUENCE {
        	ltmConnPoolProfileStatName                             LongDisplayString,
        	ltmConnPoolProfileStatCurSize                          Integer32,
        	ltmConnPoolProfileStatMaxSize                          Integer32,
        	ltmConnPoolProfileStatReuses                           Integer32,
        	ltmConnPoolProfileStatConnects                         Integer32
	}

ltmConnPoolProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a connection pool profile."
	::= { ltmConnPoolProfileStatEntry 1 } 

ltmConnPoolProfileStatCurSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of currently idle connections in the pool."
	::= { ltmConnPoolProfileStatEntry 2 } 

ltmConnPoolProfileStatMaxSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of idle connections in the pool."
	::= { ltmConnPoolProfileStatEntry 3 } 

ltmConnPoolProfileStatReuses OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of times a connection was reused from the pool."
	::= { ltmConnPoolProfileStatEntry 4 } 

ltmConnPoolProfileStatConnects OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of times a new connection was initiated."
	::= { ltmConnPoolProfileStatEntry 5 } 

--==================================================================
-- Profile_bigproto
--==================================================================
ltmFastL4ProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmFastL4Profile entries in the table."
	::= { ltmFastL4Profile 1 } 

ltmFastL4ProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmFastL4ProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of fast L4  profiles."
	::= { ltmFastL4Profile 2 } 

ltmFastL4ProfileEntry OBJECT-TYPE
	SYNTAX  LtmFastL4ProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmFastL4Profile Table"
	INDEX {
		ltmFastL4ProfileName
	}
	::= { ltmFastL4ProfileTable 1 } 

LtmFastL4ProfileEntry ::= 
	SEQUENCE {
        	ltmFastL4ProfileName                                   LongDisplayString,
        	ltmFastL4ProfileConfigSource                           INTEGER,
        	ltmFastL4ProfileDefaultName                            LongDisplayString,
        	ltmFastL4ProfileResetOnTimeout                         INTEGER,
        	ltmFastL4ProfileIpFragReass                            INTEGER,
        	ltmFastL4ProfileIdleTimeout                            Integer32,
        	ltmFastL4ProfileTcpHandshakeTimeout                    Integer32,
        	ltmFastL4ProfileMssOverride                            Integer32,
        	ltmFastL4ProfilePvaAccelMode                           INTEGER,
        	ltmFastL4ProfileTcpTimestampMode                       INTEGER,
        	ltmFastL4ProfileTcpWscaleMode                          INTEGER,
        	ltmFastL4ProfileTcpGenerateIsn                         INTEGER,
        	ltmFastL4ProfileTcpStripSack                           INTEGER,
        	ltmFastL4ProfileIpTosToClient                          INTEGER,
        	ltmFastL4ProfileIpTosToServer                          INTEGER,
        	ltmFastL4ProfileLinkQosToClient                        INTEGER,
        	ltmFastL4ProfileLinkQosToServer                        INTEGER,
        	ltmFastL4ProfileRttFromClient                          INTEGER,
        	ltmFastL4ProfileRttFromServer                          INTEGER,
        	ltmFastL4ProfileTcpCloseTimeout                        Integer32,
        	ltmFastL4ProfileLooseInitiation                        INTEGER,
        	ltmFastL4ProfileLooseClose                             INTEGER,
        	ltmFastL4ProfileHardSyncookie                          INTEGER,
        	ltmFastL4ProfileSoftSyncookie                          INTEGER
	}

ltmFastL4ProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a fast L4 profile."
	::= { ltmFastL4ProfileEntry 1 } 

ltmFastL4ProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmFastL4ProfileEntry 2 } 

ltmFastL4ProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmFastL4ProfileEntry 3 } 

ltmFastL4ProfileResetOnTimeout OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The feature of reset for idle timeout.
		If true and a TCP connection exceeds its idle_timeout, send a reset 
		in addition to deleting the connection."
	::= { ltmFastL4ProfileEntry 4 } 

ltmFastL4ProfileIpFragReass OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The feature for reassembling IP fragments. If true, reassemble IP fragments."
	::= { ltmFastL4ProfileEntry 5 } 

ltmFastL4ProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds without traffic before a connection is eligible 
		for deletion."
	::= { ltmFastL4ProfileEntry 6 } 

ltmFastL4ProfileTcpHandshakeTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds without traffic before a connection in the SYN 
		received state is eligible for deletion. 
		If set to 0, ltmFastL4ProfileIdleTimeout will be used."
	::= { ltmFastL4ProfileEntry 7 } 

ltmFastL4ProfileMssOverride OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"If non-zero and less than the 1460 default, this value overrides 
		the maximum segment size"
	::= { ltmFastL4ProfileEntry 8 } 

ltmFastL4ProfilePvaAccelMode OBJECT-TYPE 
	SYNTAX INTEGER {
		full(0),
		partial(1),
		none(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The preferred Packet Velocity ASIC (PVA) acceleration mode."
	::= { ltmFastL4ProfileEntry 9 } 

ltmFastL4ProfileTcpTimestampMode OBJECT-TYPE 
	SYNTAX INTEGER {
		preserve(0),
		strip(1),
		rewrite(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to preserver, strip or rewrite TCP timestamps."
	::= { ltmFastL4ProfileEntry 10 } 

ltmFastL4ProfileTcpWscaleMode OBJECT-TYPE 
	SYNTAX INTEGER {
		preserve(0),
		strip(1),
		rewrite(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to preserver or strip window scale option."
	::= { ltmFastL4ProfileEntry 11 } 

ltmFastL4ProfileTcpGenerateIsn OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to generate own sequence numbers on all SYNs conformant
		with RFC1948, and hence allowing timestamp recycling."
	::= { ltmFastL4ProfileEntry 12 } 

ltmFastL4ProfileTcpStripSack OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to block TCP SackOK option from passing to server 
		on an initiating SYN."
	::= { ltmFastL4ProfileEntry 13 } 

ltmFastL4ProfileIpTosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP type of service set in packets sent to the client-side."
	::= { ltmFastL4ProfileEntry 14 } 

ltmFastL4ProfileIpTosToServer OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP type of service set in packets sent to the server-side."
	::= { ltmFastL4ProfileEntry 15 } 

ltmFastL4ProfileLinkQosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The link quality of service set in packets sent to the client-side."
	::= { ltmFastL4ProfileEntry 16 } 

ltmFastL4ProfileLinkQosToServer OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The link quality of service set in packets sent to the server-side."
	::= { ltmFastL4ProfileEntry 17 } 

ltmFastL4ProfileRttFromClient OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to use TCP timestamp options to measure the round trip 
		time to the client."
	::= { ltmFastL4ProfileEntry 18 } 

ltmFastL4ProfileRttFromServer OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to use TCP timestamp options to measure the round trip 
		time to the server."
	::= { ltmFastL4ProfileEntry 19 } 

ltmFastL4ProfileTcpCloseTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds without traffic before a connection in the FIN 
		received state is eligible for deletion. 
		This is only used when ltmFastL4ProfileLooseInitiation or 
		ltmFastL4ProfileLooseClose is enabled."
	::= { ltmFastL4ProfileEntry 20 } 

ltmFastL4ProfileLooseInitiation OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to allow any TCP packet to initiate a connection (rather
		than requiring a SYN."
	::= { ltmFastL4ProfileEntry 21 } 

ltmFastL4ProfileLooseClose OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to aggressively close out a connection by allowing TMM to switch
		the ltmFastL4ProfileIdleTimeout to ltmFastL4ProfileTcpCloseTimeout
		once the first FIN packet has been seen."
	::= { ltmFastL4ProfileEntry 22 } 

ltmFastL4ProfileHardSyncookie OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to enable hardware SYN cookie protection using Packet Velocity ASIC (PVA)."
	::= { ltmFastL4ProfileEntry 23 } 

ltmFastL4ProfileSoftSyncookie OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not software SYN cookie protection is enable."
	::= { ltmFastL4ProfileEntry 24 } 

--==================================================================
-- Profile_ftp
--==================================================================
ltmFtpProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmFtpProfile entries in the table."
	::= { ltmFtpProfile 1 } 

ltmFtpProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmFtpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of FTP profiles."
	::= { ltmFtpProfile 2 } 

ltmFtpProfileEntry OBJECT-TYPE
	SYNTAX  LtmFtpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmFtpProfile Table"
	INDEX {
		ltmFtpProfileName
	}
	::= { ltmFtpProfileTable 1 } 

LtmFtpProfileEntry ::= 
	SEQUENCE {
        	ltmFtpProfileName                                      LongDisplayString,
        	ltmFtpProfileConfigSource                              INTEGER,
        	ltmFtpProfileDefaultName                               LongDisplayString,
        	ltmFtpProfileTranslateExtended                         INTEGER,
        	ltmFtpProfileDataPort                                  INTEGER
	}

ltmFtpProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a FTP profile."
	::= { ltmFtpProfileEntry 1 } 

ltmFtpProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmFtpProfileEntry 2 } 

ltmFtpProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmFtpProfileEntry 3 } 

ltmFtpProfileTranslateExtended OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Whether or not automatically translated RFC2428 extended requests
		EPSV and EPRT to PASV and PORT when talking to IPv4 servers."
	::= { ltmFtpProfileEntry 4 } 

ltmFtpProfileDataPort OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The data channel port used for this FTP profile. By default, 
		this is 20, but may need to be changed for non-default port FTP."
	::= { ltmFtpProfileEntry 5 } 

--==================================================================
-- Profile_http
--==================================================================
ltmHttpProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfile entries in the table."
	::= { ltmHttpProfile 1 } 

ltmHttpProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of HTTP profiles."
	::= { ltmHttpProfile 2 } 

ltmHttpProfileEntry OBJECT-TYPE
	SYNTAX  LtmHttpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpProfile Table"
	INDEX {
		ltmHttpProfileName
	}
	::= { ltmHttpProfileTable 1 } 

LtmHttpProfileEntry ::= 
	SEQUENCE {
        	ltmHttpProfileName                                     LongDisplayString,
        	ltmHttpProfileConfigSource                             INTEGER,
        	ltmHttpProfileDefaultName                              LongDisplayString,
        	ltmHttpProfileBasicAuthRealm                           LongDisplayString,
        	ltmHttpProfileOneConnect                               INTEGER,
        	ltmHttpProfileHeaderInsert                             LongDisplayString,
        	ltmHttpProfileHeaderErase                              LongDisplayString,
        	ltmHttpProfileFallbackHost                             LongDisplayString,
        	ltmHttpProfileCompressMode                             INTEGER,
        	ltmHttpProfileCompressMinSize                          Integer32,
        	ltmHttpProfileCompressBufferSize                       Integer32,
        	ltmHttpProfileCompressVaryHeader                       INTEGER,
        	ltmHttpProfileCompressAllowHttp10                      INTEGER,
        	ltmHttpProfileCompressGzipMemlevel                     Integer32,
        	ltmHttpProfileCompressGzipWindowsize                   Integer32,
        	ltmHttpProfileCompressGzipLevel                        Integer32,
        	ltmHttpProfileCompressKeepAcceptEncoding               INTEGER,
        	ltmHttpProfileCompressBrowserWorkarounds               INTEGER,
        	ltmHttpProfileResponseChunking                         INTEGER,
        	ltmHttpProfileLwsMaxColumn                             Integer32,
        	ltmHttpProfileLwsSeparator                             LongDisplayString,
        	ltmHttpProfileRedirectRewrite                          INTEGER,
        	ltmHttpProfileMaxHeaderSize                            Integer32,
        	ltmHttpProfilePipelining                               INTEGER,
        	ltmHttpProfileInsertXforwardedFor                      INTEGER,
        	ltmHttpProfileMaxRequests                              Integer32,
        	ltmHttpProfileCompressCpusaver                         INTEGER,
        	ltmHttpProfileCompressCpusaverHigh                     Integer32,
        	ltmHttpProfileCompressCpusaverLow                      Integer32,
        	ltmHttpProfileRamcache                                 INTEGER,
        	ltmHttpProfileRamcacheSize                             Integer32,
        	ltmHttpProfileRamcacheMaxEntries                       Integer32,
        	ltmHttpProfileRamcacheMaxAge                           Integer32,
        	ltmHttpProfileRamcacheObjectMinSize                    Integer32,
        	ltmHttpProfileRamcacheObjectMaxSize                    Integer32,
        	ltmHttpProfileRamcacheIgnoreClient                     INTEGER,
        	ltmHttpProfileRamcacheAgingRate                        Integer32,
        	ltmHttpProfileRamcacheInsertAgeHeader                  INTEGER,
        	ltmHttpProfileCompressPreferredMethod                  INTEGER
	}

ltmHttpProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmHttpProfileEntry 1 } 

ltmHttpProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmHttpProfileEntry 2 } 

ltmHttpProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmHttpProfileEntry 3 } 

ltmHttpProfileBasicAuthRealm OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The basic authentication realm of the specified HTTP profile."
	::= { ltmHttpProfileEntry 4 } 

ltmHttpProfileOneConnect OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether OneConnect HTTP header 
		transformation is used for the specified HTTP profile."
	::= { ltmHttpProfileEntry 5 } 

ltmHttpProfileHeaderInsert OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The header to be inserted into the HTTP header for 
		the specified HTTP profile."
	::= { ltmHttpProfileEntry 6 } 

ltmHttpProfileHeaderErase OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The header to be erased into the HTTP header for 
		the specified HTTP profile."
	::= { ltmHttpProfileEntry 7 } 

ltmHttpProfileFallbackHost OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The fallback host name used in HTTP redirect for 
		the specified HTTP profile."
	::= { ltmHttpProfileEntry 8 } 

ltmHttpProfileCompressMode OBJECT-TYPE 
	SYNTAX INTEGER {
		disable(0),
		enable(1),
		selective(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether compression is enabled."
	::= { ltmHttpProfileEntry 9 } 

ltmHttpProfileCompressMinSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The value that specifies the minimum length of the server 
		responses (in bytes) to be considered acceptable for compression."
	::= { ltmHttpProfileEntry 10 } 

ltmHttpProfileCompressBufferSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The value that specifies the maximum number of uncompressed bytes 
		that the compression proxy will buffer before it decides whether or 
		not to compress the server's response, in case the server's response 
		headers don't specify the content length of the response."
	::= { ltmHttpProfileEntry 11 } 

ltmHttpProfileCompressVaryHeader OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether to insert the header 
		'Vary: Accept-Encoding' in the server response for responses that 
		have been compressed. If the 'Vary:' header already exists in the 
		server response, then the value 'Accept-Encoding' will be appended to it."
	::= { ltmHttpProfileEntry 12 } 

ltmHttpProfileCompressAllowHttp10 OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether to allow compression on responses 
		to HTTP 1.0 requests."
	::= { ltmHttpProfileEntry 13 } 

ltmHttpProfileCompressGzipMemlevel OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The amount of memory that the proxy will use when doing compression. 
		It must be an integer no less than 1 and no greater than 9. Higher 
		values produce faster compression at the expense of more memory usage. 
		The default memory level will be 8."
	::= { ltmHttpProfileEntry 14 } 

ltmHttpProfileCompressGzipWindowsize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bits in the window size that the compression proxy 
		will use when compressing the server response. It should be an integer 
		no less than 8 and no greater than 15. Higher values produce better 
		compression ratios at the expense of more memory usage. 
		The default window size will be 15."
	::= { ltmHttpProfileEntry 15 } 

ltmHttpProfileCompressGzipLevel OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The speed of compression that is applied to the response. Minimum
		value is 1, maximum is 9. The lower numbers give faster compression 
		with lower ratios, and higher numbers give slower compression with 
		higher ratios."
	::= { ltmHttpProfileEntry 16 } 

ltmHttpProfileCompressKeepAcceptEncoding OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state of the option to keep client-encoding header."
	::= { ltmHttpProfileEntry 17 } 

ltmHttpProfileCompressBrowserWorkarounds OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option to control whether or not to disable compression for 
		known browsers that cannot handle certain types of compressed 
		responses properly. If it's true, compression for known browsers 
		will be disabled."
	::= { ltmHttpProfileEntry 18 } 

ltmHttpProfileResponseChunking OBJECT-TYPE 
	SYNTAX INTEGER {
		preserve(0),
		selective(1),
		unchunk(2),
		rechunk(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The HTTP chunk mode for the responses."
	::= { ltmHttpProfileEntry 19 } 

ltmHttpProfileLwsMaxColumn OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The linear white space maximum column sizes used to support 
		multi-line header insertion."
	::= { ltmHttpProfileEntry 20 } 

ltmHttpProfileLwsSeparator OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The linear white space separator strings for the specified HTTP profile."
	::= { ltmHttpProfileEntry 21 } 

ltmHttpProfileRedirectRewrite OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		all(1),
		matching(2),
		nodes(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The HTTP redirect/rewrite mode for the responses."
	::= { ltmHttpProfileEntry 22 } 

ltmHttpProfileMaxHeaderSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum size of the headers."
	::= { ltmHttpProfileEntry 23 } 

ltmHttpProfilePipelining OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether pipelining is enabled for this profile."
	::= { ltmHttpProfileEntry 24 } 

ltmHttpProfileInsertXforwardedFor OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether inserting X-Forwarded-For
		is enabled for this profile."
	::= { ltmHttpProfileEntry 25 } 

ltmHttpProfileMaxRequests OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connection requests allowed. The connection will be
		forced closed when this limit is reached."
	::= { ltmHttpProfileEntry 26 } 

ltmHttpProfileCompressCpusaver OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether CPU saving mode is enable or not
		when doing compression."
	::= { ltmHttpProfileEntry 27 } 

ltmHttpProfileCompressCpusaverHigh OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The CPU saver high threshold. When CPU utilization exceeds this value,
		compression is switched to NULL compression."
	::= { ltmHttpProfileEntry 28 } 

ltmHttpProfileCompressCpusaverLow OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The CPU saver low threshold. When CPU utilization drops below
		this value, compression is switched to full throttle."
	::= { ltmHttpProfileEntry 29 } 

ltmHttpProfileRamcache OBJECT-TYPE 
	SYNTAX INTEGER {
		disable(0),
		enable(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state the whether RAM cache is enabled or not."
	::= { ltmHttpProfileEntry 30 } 

ltmHttpProfileRamcacheSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum cache size in MB's."
	::= { ltmHttpProfileEntry 31 } 

ltmHttpProfileRamcacheMaxEntries OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum cache entries."
	::= { ltmHttpProfileEntry 32 } 

ltmHttpProfileRamcacheMaxAge OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum age of cached object."
	::= { ltmHttpProfileEntry 33 } 

ltmHttpProfileRamcacheObjectMinSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The minimum size requirement for cached object in bytes."
	::= { ltmHttpProfileEntry 34 } 

ltmHttpProfileRamcacheObjectMaxSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum size limitation for cached object in bytes."
	::= { ltmHttpProfileEntry 35 } 

ltmHttpProfileRamcacheIgnoreClient OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		maxage(1),
		all(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that Ram cache ignores client cache."
	::= { ltmHttpProfileEntry 36 } 

ltmHttpProfileRamcacheAgingRate OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The aging rate for the RAM cache."
	::= { ltmHttpProfileEntry 37 } 

ltmHttpProfileRamcacheInsertAgeHeader OBJECT-TYPE 
	SYNTAX INTEGER {
		disable(0),
		enable(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The mode that indicates whether to insert the Age headers for RAM cache."
	::= { ltmHttpProfileEntry 38 } 

ltmHttpProfileCompressPreferredMethod OBJECT-TYPE 
	SYNTAX INTEGER {
		deflate(0),
		gzip(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The option for preferred compression method."
	::= { ltmHttpProfileEntry 39 } 

--==================================================================
-- Profile_http_compress_uri_includes
--==================================================================
ltmCompUriInclNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileCompUriIncl entries in the table."
	::= { ltmHttpProfileCompUriIncl 1 } 

ltmCompUriInclTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmCompUriInclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of regular expressions used to match 
		the request URI part of the client requests during compression. 
		A match must be found in at least one of the 'include' fields."
	::= { ltmHttpProfileCompUriIncl 2 } 

ltmCompUriInclEntry OBJECT-TYPE
	SYNTAX  LtmCompUriInclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmCompUriIncl Table"
	INDEX {
		ltmCompUriInclName,
		ltmCompUriInclIndex
	}
	::= { ltmCompUriInclTable 1 } 

LtmCompUriInclEntry ::= 
	SEQUENCE {
        	ltmCompUriInclName                                     LongDisplayString,
        	ltmCompUriInclIndex                                    INTEGER,
        	ltmCompUriInclUri                                      LongDisplayString
	}

ltmCompUriInclName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmCompUriInclEntry 1 } 

ltmCompUriInclIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of the regular expression used to match the request 
		URI part of the client requests during compression in 
		'include' fields for the specified HTTP profile."
	::= { ltmCompUriInclEntry 2 } 

ltmCompUriInclUri OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The regular expression used to match the request URI part 
		of the client requests during compression in 'include' fields 
		for the specified HTTP profile."
	::= { ltmCompUriInclEntry 3 } 

--==================================================================
-- Profile_http_compress_uri_excludes
--==================================================================
ltmCompUriExclNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileCompUriExcl entries in the table."
	::= { ltmHttpProfileCompUriExcl 1 } 

ltmCompUriExclTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmCompUriExclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of regular expressions used to match 
		the request URI part of the client requests during compression. 
		A match must be found in at least one of the 'exclude' fields."
	::= { ltmHttpProfileCompUriExcl 2 } 

ltmCompUriExclEntry OBJECT-TYPE
	SYNTAX  LtmCompUriExclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmCompUriExcl Table"
	INDEX {
		ltmCompUriExclName,
		ltmCompUriExclIndex
	}
	::= { ltmCompUriExclTable 1 } 

LtmCompUriExclEntry ::= 
	SEQUENCE {
        	ltmCompUriExclName                                     LongDisplayString,
        	ltmCompUriExclIndex                                    INTEGER,
        	ltmCompUriExclUri                                      LongDisplayString
	}

ltmCompUriExclName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmCompUriExclEntry 1 } 

ltmCompUriExclIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of the regular expression used to match the request 
		URI part of the client requests during compression in 
		'exclude' fields for the specified HTTP profile."
	::= { ltmCompUriExclEntry 2 } 

ltmCompUriExclUri OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The regular expression used to match the request URI part 
		of the client requests during compression in 'exclude' fields 
		for the specified HTTP profile."
	::= { ltmCompUriExclEntry 3 } 

--==================================================================
-- Profile_http_compress_content_type_includes
--==================================================================
ltmCompContTypeInclNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileCompContTypeIncl entries in the table."
	::= { ltmHttpProfileCompContTypeIncl 1 } 

ltmCompContTypeInclTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmCompContTypeInclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of regular expressions used to match 
		the MIME types in the server response's 'Content-Type:' headers. 
		A match must be found in at least one of the 'include' fields."
	::= { ltmHttpProfileCompContTypeIncl 2 } 

ltmCompContTypeInclEntry OBJECT-TYPE
	SYNTAX  LtmCompContTypeInclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmCompContTypeIncl Table"
	INDEX {
		ltmCompContTypeInclName,
		ltmCompContTypeInclIndex
	}
	::= { ltmCompContTypeInclTable 1 } 

LtmCompContTypeInclEntry ::= 
	SEQUENCE {
        	ltmCompContTypeInclName                                LongDisplayString,
        	ltmCompContTypeInclIndex                               INTEGER,
        	ltmCompContTypeInclContentType                         LongDisplayString
	}

ltmCompContTypeInclName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmCompContTypeInclEntry 1 } 

ltmCompContTypeInclIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of the regular expression to match the MIME types in the 
	        server response's 'Content-Type:' headers in 'include' fields for 
		the specified HTTP profile."
	::= { ltmCompContTypeInclEntry 2 } 

ltmCompContTypeInclContentType OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The regular expression used to match the MIME types in the server 
		response's 'Content-Type:' headers in 'include' fields for the
		specified HTTP profile."
	::= { ltmCompContTypeInclEntry 3 } 

--==================================================================
-- Profile_http_compress_content_type_excludes
--==================================================================
ltmCompContTypeExclNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileCompContTypeExcl entries in the table."
	::= { ltmHttpProfileCompContTypeExcl 1 } 

ltmCompContTypeExclTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmCompContTypeExclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of regular expressions used to match 
		the MIME types in the server response's 'Content-Type:' headers. 
		A match must be found in at least one of the 'exclude' fields."
	::= { ltmHttpProfileCompContTypeExcl 2 } 

ltmCompContTypeExclEntry OBJECT-TYPE
	SYNTAX  LtmCompContTypeExclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmCompContTypeExcl Table"
	INDEX {
		ltmCompContTypeExclName,
		ltmCompContTypeExclIndex
	}
	::= { ltmCompContTypeExclTable 1 } 

LtmCompContTypeExclEntry ::= 
	SEQUENCE {
        	ltmCompContTypeExclName                                LongDisplayString,
        	ltmCompContTypeExclIndex                               INTEGER,
        	ltmCompContTypeExclContentType                         LongDisplayString
	}

ltmCompContTypeExclName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmCompContTypeExclEntry 1 } 

ltmCompContTypeExclIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of the regular expression to match the MIME types in the 
	        server response's 'Content-Type:' headers in 'exclude' fields for 
		the specified HTTP profile."
	::= { ltmCompContTypeExclEntry 2 } 

ltmCompContTypeExclContentType OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The regular expression used to match the MIME types in the server 
		response's 'Content-Type:' headers in 'exclude' fields for the
		specified HTTP profile."
	::= { ltmCompContTypeExclEntry 3 } 

--==================================================================
-- Profile_http_stat
--==================================================================
ltmHttpProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmHttpProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmHttpProfileStat 1 } 

ltmHttpProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileStat entries in the table."
	::= { ltmHttpProfileStat 2 } 

ltmHttpProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of HTTP profiles."
	::= { ltmHttpProfileStat 3 } 

ltmHttpProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmHttpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpProfileStat Table"
	INDEX {
		ltmHttpProfileStatName
	}
	::= { ltmHttpProfileStatTable 1 } 

LtmHttpProfileStatEntry ::= 
	SEQUENCE {
        	ltmHttpProfileStatName                                 LongDisplayString,
        	ltmHttpProfileStatCookiePersistInserts                 Counter64,
        	ltmHttpProfileStatResp2xxCnt                           Counter64,
        	ltmHttpProfileStatResp3xxCnt                           Counter64,
        	ltmHttpProfileStatResp4xxCnt                           Counter64,
        	ltmHttpProfileStatResp5xxCnt                           Counter64,
        	ltmHttpProfileStatNumberReqs                           Counter64,
        	ltmHttpProfileStatGetReqs                              Counter64,
        	ltmHttpProfileStatPostReqs                             Counter64,
        	ltmHttpProfileStatV9Reqs                               Counter64,
        	ltmHttpProfileStatV10Reqs                              Counter64,
        	ltmHttpProfileStatV11Reqs                              Counter64,
        	ltmHttpProfileStatV9Resp                               Counter64,
        	ltmHttpProfileStatV10Resp                              Counter64,
        	ltmHttpProfileStatV11Resp                              Counter64,
        	ltmHttpProfileStatMaxKeepaliveReq                      Counter64,
        	ltmHttpProfileStatRespBucket1k                         Counter64,
        	ltmHttpProfileStatRespBucket4k                         Counter64,
        	ltmHttpProfileStatRespBucket16k                        Counter64,
        	ltmHttpProfileStatRespBucket32k                        Counter64,
        	ltmHttpProfileStatPrecompressBytes                     Counter64,
        	ltmHttpProfileStatPostcompressBytes                    Counter64,
        	ltmHttpProfileStatNullCompressBytes                    Counter64,
        	ltmHttpProfileStatHtmlPrecompressBytes                 Counter64,
        	ltmHttpProfileStatHtmlPostcompressBytes                Counter64,
        	ltmHttpProfileStatCssPrecompressBytes                  Counter64,
        	ltmHttpProfileStatCssPostcompressBytes                 Counter64,
        	ltmHttpProfileStatJsPrecompressBytes                   Counter64,
        	ltmHttpProfileStatJsPostcompressBytes                  Counter64,
        	ltmHttpProfileStatXmlPrecompressBytes                  Counter64,
        	ltmHttpProfileStatXmlPostcompressBytes                 Counter64,
        	ltmHttpProfileStatSgmlPrecompressBytes                 Counter64,
        	ltmHttpProfileStatSgmlPostcompressBytes                Counter64,
        	ltmHttpProfileStatPlainPrecompressBytes                Counter64,
        	ltmHttpProfileStatPlainPostcompressBytes               Counter64,
        	ltmHttpProfileStatOctetPrecompressBytes                Counter64,
        	ltmHttpProfileStatOctetPostcompressBytes               Counter64,
        	ltmHttpProfileStatImagePrecompressBytes                Counter64,
        	ltmHttpProfileStatImagePostcompressBytes               Counter64,
        	ltmHttpProfileStatVideoPrecompressBytes                Counter64,
        	ltmHttpProfileStatVideoPostcompressBytes               Counter64,
        	ltmHttpProfileStatAudioPrecompressBytes                Counter64,
        	ltmHttpProfileStatAudioPostcompressBytes               Counter64,
        	ltmHttpProfileStatOtherPrecompressBytes                Counter64,
        	ltmHttpProfileStatOtherPostcompressBytes               Counter64,
        	ltmHttpProfileStatRamcacheHits                         Counter64,
        	ltmHttpProfileStatRamcacheMisses                       Counter64,
        	ltmHttpProfileStatRamcacheMissesAll                    Counter64,
        	ltmHttpProfileStatRamcacheHitBytes                     Counter64,
        	ltmHttpProfileStatRamcacheMissBytes                    Counter64,
        	ltmHttpProfileStatRamcacheMissBytesAll                 Counter64,
        	ltmHttpProfileStatRamcacheSize                         Counter64,
        	ltmHttpProfileStatRamcacheCount                        Counter64,
        	ltmHttpProfileStatRamcacheEvictions                    Counter64,
        	ltmHttpProfileStatRespBucket64k                        Counter64
	}

ltmHttpProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmHttpProfileStatEntry 1 } 

ltmHttpProfileStatCookiePersistInserts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of successful attempts to insert HTTP headers 
		 for cookie persistence (set-cookie header insertions)."
	::= { ltmHttpProfileStatEntry 2 } 

ltmHttpProfileStatResp2xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 200 to 206 
		 (successful responses)"
	::= { ltmHttpProfileStatEntry 3 } 

ltmHttpProfileStatResp3xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 300 to 307 
		 (redirection responses)."
	::= { ltmHttpProfileStatEntry 4 } 

ltmHttpProfileStatResp4xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 400 to 417  
		 (client errors)."
	::= { ltmHttpProfileStatEntry 5 } 

ltmHttpProfileStatResp5xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 500 to 505 
		 (server errors)."
	::= { ltmHttpProfileStatEntry 6 } 

ltmHttpProfileStatNumberReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of HTTP requests."
	::= { ltmHttpProfileStatEntry 7 } 

ltmHttpProfileStatGetReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of HTTP get requests."
	::= { ltmHttpProfileStatEntry 8 } 

ltmHttpProfileStatPostReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of HTTP post requests."
	::= { ltmHttpProfileStatEntry 9 } 

ltmHttpProfileStatV9Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 9 requests."
	::= { ltmHttpProfileStatEntry 10 } 

ltmHttpProfileStatV10Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 10 requests."
	::= { ltmHttpProfileStatEntry 11 } 

ltmHttpProfileStatV11Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 11 requests."
	::= { ltmHttpProfileStatEntry 12 } 

ltmHttpProfileStatV9Resp OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 9 responses."
	::= { ltmHttpProfileStatEntry 13 } 

ltmHttpProfileStatV10Resp OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 10 responses."
	::= { ltmHttpProfileStatEntry 14 } 

ltmHttpProfileStatV11Resp OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 11 responses."
	::= { ltmHttpProfileStatEntry 15 } 

ltmHttpProfileStatMaxKeepaliveReq OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of requests made in a connection."
	::= { ltmHttpProfileStatEntry 16 } 

ltmHttpProfileStatRespBucket1k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses under 1k."
	::= { ltmHttpProfileStatEntry 17 } 

ltmHttpProfileStatRespBucket4k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses under 1 - 4k."
	::= { ltmHttpProfileStatEntry 18 } 

ltmHttpProfileStatRespBucket16k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses under 4 - 16k."
	::= { ltmHttpProfileStatEntry 19 } 

ltmHttpProfileStatRespBucket32k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses under 16 - 32k."
	::= { ltmHttpProfileStatEntry 20 } 

ltmHttpProfileStatPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of response bytes before compression has taken place."
	::= { ltmHttpProfileStatEntry 21 } 

ltmHttpProfileStatPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of response bytes after compression has taken place."
	::= { ltmHttpProfileStatEntry 22 } 

ltmHttpProfileStatNullCompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes subjected to NULL compression (for license enforcement)."
	::= { ltmHttpProfileStatEntry 23 } 

ltmHttpProfileStatHtmlPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: HTML."
	::= { ltmHttpProfileStatEntry 24 } 

ltmHttpProfileStatHtmlPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: HTML."
	::= { ltmHttpProfileStatEntry 25 } 

ltmHttpProfileStatCssPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: CSS."
	::= { ltmHttpProfileStatEntry 26 } 

ltmHttpProfileStatCssPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: CSS."
	::= { ltmHttpProfileStatEntry 27 } 

ltmHttpProfileStatJsPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Javascript."
	::= { ltmHttpProfileStatEntry 28 } 

ltmHttpProfileStatJsPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Javascript."
	::= { ltmHttpProfileStatEntry 29 } 

ltmHttpProfileStatXmlPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: XML."
	::= { ltmHttpProfileStatEntry 30 } 

ltmHttpProfileStatXmlPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: XML."
	::= { ltmHttpProfileStatEntry 31 } 

ltmHttpProfileStatSgmlPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: SGML."
	::= { ltmHttpProfileStatEntry 32 } 

ltmHttpProfileStatSgmlPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: SGML."
	::= { ltmHttpProfileStatEntry 33 } 

ltmHttpProfileStatPlainPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Plain."
	::= { ltmHttpProfileStatEntry 34 } 

ltmHttpProfileStatPlainPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Plain."
	::= { ltmHttpProfileStatEntry 35 } 

ltmHttpProfileStatOctetPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Octet stream."
	::= { ltmHttpProfileStatEntry 36 } 

ltmHttpProfileStatOctetPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Octet stream."
	::= { ltmHttpProfileStatEntry 37 } 

ltmHttpProfileStatImagePrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Images."
	::= { ltmHttpProfileStatEntry 38 } 

ltmHttpProfileStatImagePostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Images."
	::= { ltmHttpProfileStatEntry 39 } 

ltmHttpProfileStatVideoPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Video files."
	::= { ltmHttpProfileStatEntry 40 } 

ltmHttpProfileStatVideoPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Video files."
	::= { ltmHttpProfileStatEntry 41 } 

ltmHttpProfileStatAudioPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Audio files."
	::= { ltmHttpProfileStatEntry 42 } 

ltmHttpProfileStatAudioPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Audio files."
	::= { ltmHttpProfileStatEntry 43 } 

ltmHttpProfileStatOtherPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: other than 
		HTML, CSS, Javascript, XML, SGML, Plain, Images, Video files, 
		Audio files."
	::= { ltmHttpProfileStatEntry 44 } 

ltmHttpProfileStatOtherPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: other than 
		HTML, CSS, Javascript, XML, SGML, Plain, Images, Video files, 
		Audio files."
	::= { ltmHttpProfileStatEntry 45 } 

ltmHttpProfileStatRamcacheHits OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache hits."
	::= { ltmHttpProfileStatEntry 46 } 

ltmHttpProfileStatRamcacheMisses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache misses, excluding un-cacheable data."
	::= { ltmHttpProfileStatEntry 47 } 

ltmHttpProfileStatRamcacheMissesAll OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of RAM cache misses."
	::= { ltmHttpProfileStatEntry 48 } 

ltmHttpProfileStatRamcacheHitBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache hits in bytes."
	::= { ltmHttpProfileStatEntry 49 } 

ltmHttpProfileStatRamcacheMissBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache misses in bytes, excluding un-cacheable data."
	::= { ltmHttpProfileStatEntry 50 } 

ltmHttpProfileStatRamcacheMissBytesAll OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of RAM cache misses in bytes."
	::= { ltmHttpProfileStatEntry 51 } 

ltmHttpProfileStatRamcacheSize OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The Ram cache current size."
	::= { ltmHttpProfileStatEntry 52 } 

ltmHttpProfileStatRamcacheCount OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of items stored in Ram cache."
	::= { ltmHttpProfileStatEntry 53 } 

ltmHttpProfileStatRamcacheEvictions OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of Ram cache evictions."
	::= { ltmHttpProfileStatEntry 54 } 

ltmHttpProfileStatRespBucket64k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! Please see the new larger bucket sizes"
	::= { ltmHttpProfileStatEntry 55 } 

--==================================================================
-- Profile_persist
--==================================================================
ltmPersistProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmPersistProfile entries in the table."
	::= { ltmPersistProfile 1 } 

ltmPersistProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmPersistProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of persistent profile."
	::= { ltmPersistProfile 2 } 

ltmPersistProfileEntry OBJECT-TYPE
	SYNTAX  LtmPersistProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmPersistProfile Table"
	INDEX {
		ltmPersistProfileName
	}
	::= { ltmPersistProfileTable 1 } 

LtmPersistProfileEntry ::= 
	SEQUENCE {
        	ltmPersistProfileName                                  LongDisplayString,
        	ltmPersistProfileConfigSource                          INTEGER,
        	ltmPersistProfileDefaultName                           LongDisplayString,
        	ltmPersistProfileMode                                  INTEGER,
        	ltmPersistProfileMirror                                INTEGER,
        	ltmPersistProfileTimeout                               Integer32,
        	ltmPersistProfileMaskType                              InetAddressType,
        	ltmPersistProfileMask                                  InetAddress,
        	ltmPersistProfileCookieMethod                          INTEGER,
        	ltmPersistProfileCookieName                            LongDisplayString,
        	ltmPersistProfileCookieExpiration                      Integer32,
        	ltmPersistProfileCookieHashOffset                      INTEGER,
        	ltmPersistProfileCookieHashLength                      INTEGER,
        	ltmPersistProfileMsrdpNoSessionDir                     INTEGER,
        	ltmPersistProfileMapProxies                            INTEGER,
        	ltmPersistProfileAcrossServices                        INTEGER,
        	ltmPersistProfileAcrossVirtuals                        INTEGER,
        	ltmPersistProfileAcrossPools                           INTEGER,
        	ltmPersistProfileUieRule                               LongDisplayString,
        	ltmPersistProfileSipInfo                               LongDisplayString
	}

ltmPersistProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a persist profile."
	::= { ltmPersistProfileEntry 1 } 

ltmPersistProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmPersistProfileEntry 2 } 

ltmPersistProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmPersistProfileEntry 3 } 

ltmPersistProfileMode OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		srcaddr(1),
		dstaddr(2),
		cookie(3),
		msrdp(4),
		sslsid(5),
		sip(6),
		uie(7),
		hash(8)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type of persistence."
	::= { ltmPersistProfileEntry 4 } 

ltmPersistProfileMirror OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state of mirror persistence records."
	::= { ltmPersistProfileEntry 5 } 

ltmPersistProfileTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The value (in seconds) to timeout persist entry."
	::= { ltmPersistProfileEntry 6 } 

ltmPersistProfileMaskType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmPersistMask"
	::= { ltmPersistProfileEntry 7 } 

ltmPersistProfileMask OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The source/destination address mask. It is interpreted 
		within the context of a ltmPersistMaskType value."
	::= { ltmPersistProfileEntry 8 } 

ltmPersistProfileCookieMethod OBJECT-TYPE 
	SYNTAX INTEGER {
		unspecified(0),
		insert(1),
		rewrite(2),
		passive(3),
		hash(4)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type of cookie persistence."
	::= { ltmPersistProfileEntry 9 } 

ltmPersistProfileCookieName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of cookie."
	::= { ltmPersistProfileEntry 10 } 

ltmPersistProfileCookieExpiration OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The cookie expiration in seconds."
	::= { ltmPersistProfileEntry 11 } 

ltmPersistProfileCookieHashOffset OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The offset of cookie for hash mode."
	::= { ltmPersistProfileEntry 12 } 

ltmPersistProfileCookieHashLength OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The length of cookie for hash mode."
	::= { ltmPersistProfileEntry 13 } 

ltmPersistProfileMsrdpNoSessionDir OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This object indicates MS terminal services has been configured
		without a session directory and causes the initial MSRDP
		connection to be load-balanced."
	::= { ltmPersistProfileEntry 14 } 

ltmPersistProfileMapProxies OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This object indicates whether we should map known proxies when
		the persistence mode is src_addr."
	::= { ltmPersistProfileEntry 15 } 

ltmPersistProfileAcrossServices OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This object indicates whether the persistence entries added under
		this profile are available across services."
	::= { ltmPersistProfileEntry 16 } 

ltmPersistProfileAcrossVirtuals OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This object indicates whether the persistence entries added under
		this profile are available across virtuals."
	::= { ltmPersistProfileEntry 17 } 

ltmPersistProfileAcrossPools OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This object indicates whether the persistence entries added under
		this profile are available across pools."
	::= { ltmPersistProfileEntry 18 } 

ltmPersistProfileUieRule OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The rule name for UIE mode."
	::= { ltmPersistProfileEntry 19 } 

ltmPersistProfileSipInfo OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SIP header name for persisting in the specified profile."
	::= { ltmPersistProfileEntry 20 } 

--==================================================================
-- Profile_stream
--==================================================================
ltmStreamProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmStreamProfile entries in the table."
	::= { ltmStreamProfile 1 } 

ltmStreamProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmStreamProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of stream profile."
	::= { ltmStreamProfile 2 } 

ltmStreamProfileEntry OBJECT-TYPE
	SYNTAX  LtmStreamProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmStreamProfile Table"
	INDEX {
		ltmStreamProfileName
	}
	::= { ltmStreamProfileTable 1 } 

LtmStreamProfileEntry ::= 
	SEQUENCE {
        	ltmStreamProfileName                                   LongDisplayString,
        	ltmStreamProfileConfigSource                           INTEGER,
        	ltmStreamProfileDefaultName                            LongDisplayString,
        	ltmStreamProfileSource                                 LongDisplayString,
        	ltmStreamProfileTarget                                 LongDisplayString
	}

ltmStreamProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a stream profile."
	::= { ltmStreamProfileEntry 1 } 

ltmStreamProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmStreamProfileEntry 2 } 

ltmStreamProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmStreamProfileEntry 3 } 

ltmStreamProfileSource OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The source string to search for."
	::= { ltmStreamProfileEntry 4 } 

ltmStreamProfileTarget OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The target string to replace."
	::= { ltmStreamProfileEntry 5 } 

--==================================================================
-- Profile_stream_stat
--==================================================================
ltmStreamProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmStreamProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmStreamProfileStat 1 } 

ltmStreamProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmStreamProfileStat entries in the table."
	::= { ltmStreamProfileStat 2 } 

ltmStreamProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmStreamProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of stream profile."
	::= { ltmStreamProfileStat 3 } 

ltmStreamProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmStreamProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmStreamProfileStat Table"
	INDEX {
		ltmStreamProfileStatName
	}
	::= { ltmStreamProfileStatTable 1 } 

LtmStreamProfileStatEntry ::= 
	SEQUENCE {
        	ltmStreamProfileStatName                               LongDisplayString,
        	ltmStreamProfileStatReplaces                           Counter64
	}

ltmStreamProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a stream profile."
	::= { ltmStreamProfileStatEntry 1 } 

ltmStreamProfileStatReplaces OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of replace operations completed."
	::= { ltmStreamProfileStatEntry 2 } 

--==================================================================
-- Profile_tcp
--==================================================================
ltmTcpProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmTcpProfile entries in the table."
	::= { ltmTcpProfile 1 } 

ltmTcpProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmTcpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of TCP profile."
	::= { ltmTcpProfile 2 } 

ltmTcpProfileEntry OBJECT-TYPE
	SYNTAX  LtmTcpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmTcpProfile Table"
	INDEX {
		ltmTcpProfileName
	}
	::= { ltmTcpProfileTable 1 } 

LtmTcpProfileEntry ::= 
	SEQUENCE {
        	ltmTcpProfileName                                      LongDisplayString,
        	ltmTcpProfileConfigSource                              INTEGER,
        	ltmTcpProfileDefaultName                               LongDisplayString,
        	ltmTcpProfileResetOnTimeout                            INTEGER,
        	ltmTcpProfileTimeWaitRecycle                           INTEGER,
        	ltmTcpProfileDelayedAcks                               INTEGER,
        	ltmTcpProfileProxyMss                                  INTEGER,
        	ltmTcpProfileProxyOptions                              INTEGER,
        	ltmTcpProfileProxyBufferLow                            Integer32,
        	ltmTcpProfileProxyBufferHigh                           Integer32,
        	ltmTcpProfileIdleTimeout                               Integer32,
        	ltmTcpProfileTimeWaitTimeout                           Integer32,
        	ltmTcpProfileFinWaitTimeout                            Integer32,
        	ltmTcpProfileCloseWaitTimeout                          Integer32,
        	ltmTcpProfileSndbuf                                    Integer32,
        	ltmTcpProfileRcvwnd                                    Integer32,
        	ltmTcpProfileKeepAliveInterval                         Integer32,
        	ltmTcpProfileSynMaxrtx                                 Integer32,
        	ltmTcpProfileMaxrtx                                    Integer32,
        	ltmTcpProfileIpTosToClient                             INTEGER,
        	ltmTcpProfileLinkQosToClient                           INTEGER,
        	ltmTcpProfileDeferredAccept                            INTEGER,
        	ltmTcpProfileSelectiveAcks                             INTEGER,
        	ltmTcpProfileEcn                                       INTEGER,
        	ltmTcpProfileLimitedTransmit                           INTEGER,
        	ltmTcpProfileHighPerfTcpExt                            INTEGER,
        	ltmTcpProfileSlowStart                                 INTEGER,
        	ltmTcpProfileBandwidthDelay                            INTEGER,
        	ltmTcpProfileNagle                                     INTEGER,
        	ltmTcpProfileAckOnPush                                 INTEGER,
        	ltmTcpProfileMd5Sig                                    INTEGER,
        	ltmTcpProfileMd5SigPass                                LongDisplayString,
        	ltmTcpProfileAbc                                       INTEGER,
        	ltmTcpProfileCongestionCtrl                            INTEGER,
        	ltmTcpProfileDsack                                     INTEGER,
        	ltmTcpProfileCmetricsCache                             INTEGER,
        	ltmTcpProfileVerifiedAccept                            INTEGER,
        	ltmTcpProfilePktLossIgnoreRate                         Integer32,
        	ltmTcpProfilePktLossIgnoreBurst                        Integer32,
        	ltmTcpProfileZeroWindowTimeout                         Integer32
	}

ltmTcpProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a TCP profile."
	::= { ltmTcpProfileEntry 1 } 

ltmTcpProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmTcpProfileEntry 2 } 

ltmTcpProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmTcpProfileEntry 3 } 

ltmTcpProfileResetOnTimeout OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The feature of reset for idle timeout.
		If true and a TCP connection exceeds its idle_timeout, send a reset 
		in addition to deleting the connection."
	::= { ltmTcpProfileEntry 4 } 

ltmTcpProfileTimeWaitRecycle OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Recycle connection when SYN is received in TIME-WAIT state."
	::= { ltmTcpProfileEntry 5 } 

ltmTcpProfileDelayedAcks OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"If true, Enable delayed ACK to allow coalescing of multiple ACK responses."
	::= { ltmTcpProfileEntry 6 } 

ltmTcpProfileProxyMss OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Whether or not to proxy maximum segment size. 
		If true, advertise the same mss to the server as was 
		negotiated with the client."
	::= { ltmTcpProfileEntry 7 } 

ltmTcpProfileProxyOptions OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Whether or not to proxy an option.
		If true, advertise an option (e.g. time-stamps) to 
		the server only if it was negotiated with the client."
	::= { ltmTcpProfileEntry 8 } 

ltmTcpProfileProxyBufferLow OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The proxy buffer level at which the receive window is opened."
	::= { ltmTcpProfileEntry 9 } 

ltmTcpProfileProxyBufferHigh OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The proxy buffer level at which the receive window is closed."
	::= { ltmTcpProfileEntry 10 } 

ltmTcpProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds without traffic before a connection is 
		eligible for deletion."
	::= { ltmTcpProfileEntry 11 } 

ltmTcpProfileTimeWaitTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The milliseconds in TIME-WAIT before entering CLOSED state."
	::= { ltmTcpProfileEntry 12 } 

ltmTcpProfileFinWaitTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds to remain in FIN-WAIT or CLOSING state 
		before giving up. Zero is forever (or until maxrtx of FIN)."
	::= { ltmTcpProfileEntry 13 } 

ltmTcpProfileCloseWaitTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds to remain in LAST-ACK state before
		giving up. Zero is forever (or until maxrtx of FIN)."
	::= { ltmTcpProfileEntry 14 } 

ltmTcpProfileSndbuf OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Send buffer size in bytes."
	::= { ltmTcpProfileEntry 15 } 

ltmTcpProfileRcvwnd OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Receive window size in bytes."
	::= { ltmTcpProfileEntry 16 } 

ltmTcpProfileKeepAliveInterval OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Keep alive probe interval in milliseconds."
	::= { ltmTcpProfileEntry 17 } 

ltmTcpProfileSynMaxrtx OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of retransmissions of SYN segments."
	::= { ltmTcpProfileEntry 18 } 

ltmTcpProfileMaxrtx OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of retransmissions of data segments."
	::= { ltmTcpProfileEntry 19 } 

ltmTcpProfileIpTosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP type of service set in packets sent to client. Default:None."
	::= { ltmTcpProfileEntry 20 } 

ltmTcpProfileLinkQosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The link quality of service set in packets sent to client. Default:None."
	::= { ltmTcpProfileEntry 21 } 

ltmTcpProfileDeferredAccept OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, defers allocation of connection chain context
		until payload from client has been seen."
	::= { ltmTcpProfileEntry 22 } 

ltmTcpProfileSelectiveAcks OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, enable RFC2018 Selective Acknowledgements."
	::= { ltmTcpProfileEntry 23 } 

ltmTcpProfileEcn OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, enable RFC3168 Extended Congestion Notification (ECN)."
	::= { ltmTcpProfileEntry 24 } 

ltmTcpProfileLimitedTransmit OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, enables support for RFC3042 Limited Transmit Recovery"
	::= { ltmTcpProfileEntry 25 } 

ltmTcpProfileHighPerfTcpExt OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, enables support for RFC1323 timestamps 
		and window scaling (high bandwidth TCP extensions)."
	::= { ltmTcpProfileEntry 26 } 

ltmTcpProfileSlowStart OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state if true, enable TCP slow-start by default. We use RFC3390 to
		slow-start rather than traditional congestion avoidance mechanisms."
	::= { ltmTcpProfileEntry 27 } 

ltmTcpProfileBandwidthDelay OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state if true, attempt to calculate the optimal bandwidth
		to use to the peer based on throughput and round-trip time,
		and don't exceed it."
	::= { ltmTcpProfileEntry 28 } 

ltmTcpProfileNagle OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state if true, delay sending data < MSS in size unless
		all prior data has been ACKed. This leads to less in-flight small-data,
		and less chance for drops, but can harm interactivity. 
		Named after Nagle's algorithm."
	::= { ltmTcpProfileEntry 29 } 

ltmTcpProfileAckOnPush OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state if true, data-bearing in-order TCP segments will elicit 
		immediate ACKs from us if they have the PUSH flag set, regardless of 
		the setting of the delayed-ack profile option."
	::= { ltmTcpProfileEntry 30 } 

ltmTcpProfileMd5Sig OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state if true, use RFC2385 TCP-MD5 signatures to protect 
		TCP traffic against intermediate tampering."
	::= { ltmTcpProfileEntry 31 } 

ltmTcpProfileMd5SigPass OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This is a plaintext passphrase which may be between 1 and 80 
		characters in length, and is used in a shared-secret scheme 
		to implement the spoof-prevention parts of RFC2385."
	::= { ltmTcpProfileEntry 32 } 

ltmTcpProfileAbc OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if it is true, count the number of bytes acked 
		rather than the number of returning ACKs from the peer when 
		in the linear congestion-window expansion phase of a TCP
		connection. This algorithm and its benefits are described 
		in RFC3465 (Appropriate Byte Counting)."
	::= { ltmTcpProfileEntry 33 } 

ltmTcpProfileCongestionCtrl OBJECT-TYPE 
	SYNTAX INTEGER {
		reno(0),
		newreno(1),
		scalable(2),
		highspeed(3),
		none(4)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The TCP congestion control mode, guiding cwnd growth.
		reno - RENO congestion control mode;
		newreno - new RENO congestion control mode;
		scalable - scalable congestion control mode. It will do MIMD
	   	           on cwnd besides NewReno retransmission;
		highspeed - high-speed congestion control mode, per RFC3649;
		none - no congestion control."
	::= { ltmTcpProfileEntry 34 } 

ltmTcpProfileDsack OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, enable support for RFC2883 D-SACK (Duplicate Selective Acknowledgement)."
	::= { ltmTcpProfileEntry 35 } 

ltmTcpProfileCmetricsCache OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, use the routing table metrics cache to
		retrieve the last-known tcp congestion parameters.
		(Congestion window, round-trip-times, bandwidth delay product, and slow-start threshold.)"
	::= { ltmTcpProfileEntry 36 } 

ltmTcpProfileVerifiedAccept OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, the device must not respond to the clients 
	         SYN with a SYN-ACK until it receives a SYN-ACK from 
	         the server, indicating that the port is open."
	::= { ltmTcpProfileEntry 37 } 

ltmTcpProfilePktLossIgnoreRate OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Specifies the threshold of packets lost per million at which the system should perform congestion control.
	         Measured in packets per million. Valid values are from 0 to 1000000."
	::= { ltmTcpProfileEntry 38 } 

ltmTcpProfilePktLossIgnoreBurst OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Specifies the likelihood of performing congestion control when multiple packets in a row are lost even 
	         if the loss threshold has not been exceeded. Valid values are from 0 to 32. Higher values decrease the 
	         likelihood of performing congestion control."
	::= { ltmTcpProfileEntry 39 } 

ltmTcpProfileZeroWindowTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Specifies the timeout in milliseconds for terminating a connection with an effective zero length TCP
		 transmit window. The timeout starts when the peer advertises a zero length TCP window or when enough
		 data has been sent to fill the previously advertised window. The timer is canceled when a non-zero
		 length window is received. The default is 20000 milliseconds."
	::= { ltmTcpProfileEntry 40 } 

--==================================================================
-- Profile_tcp_stat
--==================================================================
ltmTcpProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmTcpProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmTcpProfileStat 1 } 

ltmTcpProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmTcpProfileStat entries in the table."
	::= { ltmTcpProfileStat 2 } 

ltmTcpProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmTcpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of TCP profile."
	::= { ltmTcpProfileStat 3 } 

ltmTcpProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmTcpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmTcpProfileStat Table"
	INDEX {
		ltmTcpProfileStatName
	}
	::= { ltmTcpProfileStatTable 1 } 

LtmTcpProfileStatEntry ::= 
	SEQUENCE {
        	ltmTcpProfileStatName                                  LongDisplayString,
        	ltmTcpProfileStatOpen                                  Integer32,
        	ltmTcpProfileStatCloseWait                             Integer32,
        	ltmTcpProfileStatFinWait                               Integer32,
        	ltmTcpProfileStatTimeWait                              Integer32,
        	ltmTcpProfileStatAccepts                               Counter64,
        	ltmTcpProfileStatAcceptfails                           Counter64,
        	ltmTcpProfileStatConnects                              Counter64,
        	ltmTcpProfileStatConnfails                             Counter64,
        	ltmTcpProfileStatExpires                               Counter64,
        	ltmTcpProfileStatAbandons                              Counter64,
        	ltmTcpProfileStatRxrst                                 Counter64,
        	ltmTcpProfileStatRxbadsum                              Counter64,
        	ltmTcpProfileStatRxbadseg                              Counter64,
        	ltmTcpProfileStatRxooseg                               Counter64,
        	ltmTcpProfileStatRxcookie                              Counter64,
        	ltmTcpProfileStatRxbadcookie                           Counter64,
        	ltmTcpProfileStatSyncacheover                          Counter64,
        	ltmTcpProfileStatTxrexmits                             Counter64
	}

ltmTcpProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a TCP profile."
	::= { ltmTcpProfileStatEntry 1 } 

ltmTcpProfileStatOpen OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of current open connections."
	::= { ltmTcpProfileStatEntry 2 } 

ltmTcpProfileStatCloseWait OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of current connections in CLOSE-WAIT/LAST-ACK."
	::= { ltmTcpProfileStatEntry 3 } 

ltmTcpProfileStatFinWait OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of current connections in FIN-WAIT/CLOSING."
	::= { ltmTcpProfileStatEntry 4 } 

ltmTcpProfileStatTimeWait OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of current connections in TIME-WAIT."
	::= { ltmTcpProfileStatEntry 5 } 

ltmTcpProfileStatAccepts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections accepted."
	::= { ltmTcpProfileStatEntry 6 } 

ltmTcpProfileStatAcceptfails OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections not accepted."
	::= { ltmTcpProfileStatEntry 7 } 

ltmTcpProfileStatConnects OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections established."
	::= { ltmTcpProfileStatEntry 8 } 

ltmTcpProfileStatConnfails OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections failures."
	::= { ltmTcpProfileStatEntry 9 } 

ltmTcpProfileStatExpires OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections expired due to idle timeout."
	::= { ltmTcpProfileStatEntry 10 } 

ltmTcpProfileStatAbandons OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections abandoned connections due to 
		retries/keep-alives."
	::= { ltmTcpProfileStatEntry 11 } 

ltmTcpProfileStatRxrst OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of received RST."
	::= { ltmTcpProfileStatEntry 12 } 

ltmTcpProfileStatRxbadsum OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bad checksum."
	::= { ltmTcpProfileStatEntry 13 } 

ltmTcpProfileStatRxbadseg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of malformed segments."
	::= { ltmTcpProfileStatEntry 14 } 

ltmTcpProfileStatRxooseg OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of out of order segments."
	::= { ltmTcpProfileStatEntry 15 } 

ltmTcpProfileStatRxcookie OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of received SYN-cookies."
	::= { ltmTcpProfileStatEntry 16 } 

ltmTcpProfileStatRxbadcookie OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bad SYN-cookies."
	::= { ltmTcpProfileStatEntry 17 } 

ltmTcpProfileStatSyncacheover OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of SYN-cache overflow."
	::= { ltmTcpProfileStatEntry 18 } 

ltmTcpProfileStatTxrexmits OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of retransmitted segments."
	::= { ltmTcpProfileStatEntry 19 } 

--==================================================================
-- Profile_udp
--==================================================================
ltmUdpProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmUdpProfile entries in the table."
	::= { ltmUdpProfile 1 } 

ltmUdpProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmUdpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of UDP profile."
	::= { ltmUdpProfile 2 } 

ltmUdpProfileEntry OBJECT-TYPE
	SYNTAX  LtmUdpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmUdpProfile Table"
	INDEX {
		ltmUdpProfileName
	}
	::= { ltmUdpProfileTable 1 } 

LtmUdpProfileEntry ::= 
	SEQUENCE {
        	ltmUdpProfileName                                      LongDisplayString,
        	ltmUdpProfileConfigSource                              INTEGER,
        	ltmUdpProfileDefaultName                               LongDisplayString,
        	ltmUdpProfileIdleTimeout                               Integer32,
        	ltmUdpProfileIpTosToClient                             INTEGER,
        	ltmUdpProfileLinkQosToClient                           INTEGER,
        	ltmUdpProfileDatagramLb                                INTEGER,
        	ltmUdpProfileAllowNoPayload                            INTEGER
	}

ltmUdpProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a UDP profile."
	::= { ltmUdpProfileEntry 1 } 

ltmUdpProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmUdpProfileEntry 2 } 

ltmUdpProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmUdpProfileEntry 3 } 

ltmUdpProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The umber of seconds without traffic before a flow is 
		eligible for deletion."
	::= { ltmUdpProfileEntry 4 } 

ltmUdpProfileIpTosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP type of service set in packets sent to client. Default:None."
	::= { ltmUdpProfileEntry 5 } 

ltmUdpProfileLinkQosToClient OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The link quality of service set in packets sent to client. Default:None."
	::= { ltmUdpProfileEntry 6 } 

ltmUdpProfileDatagramLb OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not to load balance each UDP datagram separately."
	::= { ltmUdpProfileEntry 7 } 

ltmUdpProfileAllowNoPayload OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether to not allow the passage of datagrams with no payload."
	::= { ltmUdpProfileEntry 8 } 

--==================================================================
-- Profile_udp_stat
--==================================================================
ltmUdpProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmUdpProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmUdpProfileStat 1 } 

ltmUdpProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmUdpProfileStat entries in the table."
	::= { ltmUdpProfileStat 2 } 

ltmUdpProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmUdpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of UDP profile."
	::= { ltmUdpProfileStat 3 } 

ltmUdpProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmUdpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmUdpProfileStat Table"
	INDEX {
		ltmUdpProfileStatName
	}
	::= { ltmUdpProfileStatTable 1 } 

LtmUdpProfileStatEntry ::= 
	SEQUENCE {
        	ltmUdpProfileStatName                                  LongDisplayString,
        	ltmUdpProfileStatOpen                                  Integer32,
        	ltmUdpProfileStatAccepts                               Counter64,
        	ltmUdpProfileStatAcceptfails                           Counter64,
        	ltmUdpProfileStatConnects                              Counter64,
        	ltmUdpProfileStatConnfails                             Counter64,
        	ltmUdpProfileStatExpires                               Counter64,
        	ltmUdpProfileStatRxdgram                               Counter64,
        	ltmUdpProfileStatRxbaddgram                            Counter64,
        	ltmUdpProfileStatRxunreach                             Counter64,
        	ltmUdpProfileStatRxbadsum                              Counter64,
        	ltmUdpProfileStatRxnosum                               Counter64,
        	ltmUdpProfileStatTxdgram                               Counter64
	}

ltmUdpProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a UDP profile."
	::= { ltmUdpProfileStatEntry 1 } 

ltmUdpProfileStatOpen OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of current open connections."
	::= { ltmUdpProfileStatEntry 2 } 

ltmUdpProfileStatAccepts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections accepted."
	::= { ltmUdpProfileStatEntry 3 } 

ltmUdpProfileStatAcceptfails OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections not accepted."
	::= { ltmUdpProfileStatEntry 4 } 

ltmUdpProfileStatConnects OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections established."
	::= { ltmUdpProfileStatEntry 5 } 

ltmUdpProfileStatConnfails OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections failures."
	::= { ltmUdpProfileStatEntry 6 } 

ltmUdpProfileStatExpires OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of connections expired due to idle timeout."
	::= { ltmUdpProfileStatEntry 7 } 

ltmUdpProfileStatRxdgram OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of received datagrams."
	::= { ltmUdpProfileStatEntry 8 } 

ltmUdpProfileStatRxbaddgram OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of malformed datagrams."
	::= { ltmUdpProfileStatEntry 9 } 

ltmUdpProfileStatRxunreach OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of received ICMP un-reached."
	::= { ltmUdpProfileStatEntry 10 } 

ltmUdpProfileStatRxbadsum OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bad checksum."
	::= { ltmUdpProfileStatEntry 11 } 

ltmUdpProfileStatRxnosum OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of no checksum."
	::= { ltmUdpProfileStatEntry 12 } 

ltmUdpProfileStatTxdgram OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of transmitted datagrams."
	::= { ltmUdpProfileStatEntry 13 } 

--==================================================================
-- Rule
--==================================================================
ltmRuleNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmRule entries in the table."
	::= { ltmRule 1 } 

ltmRuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of rules."
	::= { ltmRule 2 } 

ltmRuleEntry OBJECT-TYPE
	SYNTAX  LtmRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRule Table"
	INDEX {
		ltmRuleName
	}
	::= { ltmRuleTable 1 } 

LtmRuleEntry ::= 
	SEQUENCE {
        	ltmRuleName                                            LongDisplayString,
        	ltmRuleDefinition                                      LongDisplayString,
        	ltmRuleConfigSource                                    INTEGER
	}

ltmRuleName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a rule."
	::= { ltmRuleEntry 1 } 

ltmRuleDefinition OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!
		The definition of the specified rule."
	::= { ltmRuleEntry 2 } 

ltmRuleConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type of rule that the specified rule is associating with.
		It is either a base/pre-configured rule or user defined rule."
	::= { ltmRuleEntry 3 } 

--==================================================================
-- Rule_event
--==================================================================
ltmRuleEventNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmRuleEvent entries in the table."
	::= { ltmRuleEvent 1 } 

ltmRuleEventTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRuleEventEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of rule events."
	::= { ltmRuleEvent 2 } 

ltmRuleEventEntry OBJECT-TYPE
	SYNTAX  LtmRuleEventEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRuleEvent Table"
	INDEX {
		ltmRuleEventName,
		ltmRuleEventEventType,
		ltmRuleEventPriority
	}
	::= { ltmRuleEventTable 1 } 

LtmRuleEventEntry ::= 
	SEQUENCE {
        	ltmRuleEventName                                       LongDisplayString,
        	ltmRuleEventEventType                                  LongDisplayString,
        	ltmRuleEventPriority                                   INTEGER,
        	ltmRuleEventScript                                     LongDisplayString
	}

ltmRuleEventName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a rule."
	::= { ltmRuleEventEntry 1 } 

ltmRuleEventEventType OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The event type which the rule is used for."
	::= { ltmRuleEventEntry 2 } 

ltmRuleEventPriority OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The execution priority of this rule event."
	::= { ltmRuleEventEntry 3 } 

ltmRuleEventScript OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!.
		The TCL script for this rule event."
	::= { ltmRuleEventEntry 4 } 

--==================================================================
-- Rule_stat
--==================================================================
ltmRuleEventStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmRuleEventStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmRuleEventStat 1 } 

ltmRuleEventStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmRuleEventStat entries in the table."
	::= { ltmRuleEventStat 2 } 

ltmRuleEventStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRuleEventStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of rules."
	::= { ltmRuleEventStat 3 } 

ltmRuleEventStatEntry OBJECT-TYPE
	SYNTAX  LtmRuleEventStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRuleEventStat Table"
	INDEX {
		ltmRuleEventStatName,
		ltmRuleEventStatEventType,
		ltmRuleEventStatPriority
	}
	::= { ltmRuleEventStatTable 1 } 

LtmRuleEventStatEntry ::= 
	SEQUENCE {
        	ltmRuleEventStatName                                   LongDisplayString,
        	ltmRuleEventStatEventType                              LongDisplayString,
        	ltmRuleEventStatPriority                               INTEGER,
        	ltmRuleEventStatFailures                               Integer32,
        	ltmRuleEventStatAborts                                 Integer32,
        	ltmRuleEventStatTotalExecutions                        Integer32,
        	ltmRuleEventStatAvgCycles                              Integer32,
        	ltmRuleEventStatMaxCycles                              Integer32,
        	ltmRuleEventStatMinCycles                              Integer32
	}

ltmRuleEventStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a rule."
	::= { ltmRuleEventStatEntry 1 } 

ltmRuleEventStatEventType OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type of the event associated with the specified rule."
	::= { ltmRuleEventStatEntry 2 } 

ltmRuleEventStatPriority OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The rule execution priority."
	::= { ltmRuleEventStatEntry 3 } 

ltmRuleEventStatFailures OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of failures for executing the specified rule."
	::= { ltmRuleEventStatEntry 4 } 

ltmRuleEventStatAborts OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of aborts when executing the specified rule."
	::= { ltmRuleEventStatEntry 5 } 

ltmRuleEventStatTotalExecutions OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of event executions for the specified rule."
	::= { ltmRuleEventStatEntry 6 } 

ltmRuleEventStatAvgCycles OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The average of cycles spent during an execution of the specified rule event."
	::= { ltmRuleEventStatEntry 7 } 

ltmRuleEventStatMaxCycles OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum of cycles spent during an execution of the specified rule event."
	::= { ltmRuleEventStatEntry 8 } 

ltmRuleEventStatMinCycles OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The minimum of cycles spent during an execution of the specified rule event."
	::= { ltmRuleEventStatEntry 9 } 

--==================================================================
-- Snat
--==================================================================
ltmSnatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSnat entries in the table."
	::= { ltmSnat 1 } 

ltmSnatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSnatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of SNAT."
	::= { ltmSnat 2 } 

ltmSnatEntry OBJECT-TYPE
	SYNTAX  LtmSnatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSnat Table"
	INDEX {
		ltmSnatName
	}
	::= { ltmSnatTable 1 } 

LtmSnatEntry ::= 
	SEQUENCE {
        	ltmSnatName                                            LongDisplayString,
        	ltmSnatSfFlags                                         INTEGER,
        	ltmSnatType                                            INTEGER,
        	ltmSnatTransAddrType                                   InetAddressType,
        	ltmSnatTransAddr                                       InetAddress,
        	ltmSnatSnatpoolName                                    LongDisplayString,
        	ltmSnatListedEnabledVlans                              INTEGER
	}

ltmSnatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT. It is a named object in the definition of 
		a standard or a selective SNAT. Standard SNATs translate to 
		a single address, while selective SNATs translate to a pool of 
		translation addresses."
	::= { ltmSnatEntry 1 } 

ltmSnatSfFlags OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether connection mirroring is 
		enabled or not for the specified SNAT."
	::= { ltmSnatEntry 2 } 

ltmSnatType OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		transaddr(1),
		snatpool(2),
		automap(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The translation type of the specified SNAT.
		none - No SNAT (invalid default);
		transaddr - The SNAT uses a single translation address;
		snatpool - The SNAT uses a SNAT pool of translation addresses;
		automap - The SNAT uses self IP addresses."
	::= { ltmSnatEntry 3 } 

ltmSnatTransAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmSnatTransAddr"
	::= { ltmSnatEntry 4 } 

ltmSnatTransAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The translation address used by the specified SNAT 
		if the SNAT translates to a translation address. 
		It is interpreted within the context of a ltmSnatTransAddrType value."
	::= { ltmSnatEntry 5 } 

ltmSnatSnatpoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT pool, which is a pool of SNAT translation addresses.
		It is used by the specified SNAT if the SNAT translates to a pool."
	::= { ltmSnatEntry 6 } 

ltmSnatListedEnabledVlans OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether associated VLANs are SNAT enabled or not.
		The associated VLANs are listed in ltmSnatVlanTable."
	::= { ltmSnatEntry 7 } 

--==================================================================
-- Snat_stat
--==================================================================
ltmSnatStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmSnatStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmSnatStat 1 } 

ltmSnatStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSnatStat entries in the table."
	::= { ltmSnatStat 2 } 

ltmSnatStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSnatStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of SNAT."
	::= { ltmSnatStat 3 } 

ltmSnatStatEntry OBJECT-TYPE
	SYNTAX  LtmSnatStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSnatStat Table"
	INDEX {
		ltmSnatStatName
	}
	::= { ltmSnatStatTable 1 } 

LtmSnatStatEntry ::= 
	SEQUENCE {
        	ltmSnatStatName                                        LongDisplayString,
        	ltmSnatStatClientPktsIn                                Counter64,
        	ltmSnatStatClientBytesIn                               Counter64,
        	ltmSnatStatClientPktsOut                               Counter64,
        	ltmSnatStatClientBytesOut                              Counter64,
        	ltmSnatStatClientMaxConns                              Counter64,
        	ltmSnatStatClientTotConns                              Counter64,
        	ltmSnatStatClientCurConns                              Counter64
	}

ltmSnatStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT."
	::= { ltmSnatStatEntry 1 } 

ltmSnatStatClientPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received from client-side."
	::= { ltmSnatStatEntry 2 } 

ltmSnatStatClientBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received from client-side."
	::= { ltmSnatStatEntry 3 } 

ltmSnatStatClientPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to client-side."
	::= { ltmSnatStatEntry 4 } 

ltmSnatStatClientBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to client-side."
	::= { ltmSnatStatEntry 5 } 

ltmSnatStatClientMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from client-side."
	::= { ltmSnatStatEntry 6 } 

ltmSnatStatClientTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from client-side."
	::= { ltmSnatStatEntry 7 } 

ltmSnatStatClientCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from client-side."
	::= { ltmSnatStatEntry 8 } 

--==================================================================
-- Snat_vlan
--==================================================================
ltmSnatVlanNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSnatVlan entries in the table."
	::= { ltmSnatVlan 1 } 

ltmSnatVlanTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSnatVlanEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing VLAN information associated with SNAT."
	::= { ltmSnatVlan 2 } 

ltmSnatVlanEntry OBJECT-TYPE
	SYNTAX  LtmSnatVlanEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSnatVlan Table"
	INDEX {
		ltmSnatVlanSnatName,
		ltmSnatVlanVlanName
	}
	::= { ltmSnatVlanTable 1 } 

LtmSnatVlanEntry ::= 
	SEQUENCE {
        	ltmSnatVlanSnatName                                    LongDisplayString,
        	ltmSnatVlanVlanName                                    LongDisplayString
	}

ltmSnatVlanSnatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT."
	::= { ltmSnatVlanEntry 1 } 

ltmSnatVlanVlanName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a VLAN associated with the specified SNAT.
		Only when ltmSnatListedEnabledVlans is set to enable, 
		SNAT is enabled on the VLAN. "
	::= { ltmSnatVlanEntry 2 } 

--==================================================================
-- Snat_orig_addr
--==================================================================
ltmSnatOrigAddrNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSnatOrigAddr entries in the table."
	::= { ltmSnatOrigAddr 1 } 

ltmSnatOrigAddrTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSnatOrigAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of SNAT original addresses."
	::= { ltmSnatOrigAddr 2 } 

ltmSnatOrigAddrEntry OBJECT-TYPE
	SYNTAX  LtmSnatOrigAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSnatOrigAddr Table"
	INDEX {
		ltmSnatOrigAddrSnatName,
		ltmSnatOrigAddrAddrType,
		ltmSnatOrigAddrAddr,
		ltmSnatOrigAddrWildmaskType,
		ltmSnatOrigAddrWildmask
	}
	::= { ltmSnatOrigAddrTable 1 } 

LtmSnatOrigAddrEntry ::= 
	SEQUENCE {
        	ltmSnatOrigAddrSnatName                                LongDisplayString,
        	ltmSnatOrigAddrAddrType                                InetAddressType,
        	ltmSnatOrigAddrAddr                                    InetAddress,
        	ltmSnatOrigAddrWildmaskType                            InetAddressType,
        	ltmSnatOrigAddrWildmask                                InetAddress
	}

ltmSnatOrigAddrSnatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT."
	::= { ltmSnatOrigAddrEntry 1 } 

ltmSnatOrigAddrAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmSnatOrigAddrAddr"
	::= { ltmSnatOrigAddrEntry 2 } 

ltmSnatOrigAddrAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The original client address associated with the specified SNAT. 
		It is interpreted within the context of a ltmSnatOrigAddrAddrType value."
	::= { ltmSnatOrigAddrEntry 3 } 

ltmSnatOrigAddrWildmaskType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmSnatOrigWidemask"
	::= { ltmSnatOrigAddrEntry 4 } 

ltmSnatOrigAddrWildmask OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The wildcard netmask associated with the specified SNAT original address. 
		It is interpreted within the context of a ltmSnatOrigAddrWidemaskType value."
	::= { ltmSnatOrigAddrEntry 5 } 

--==================================================================
-- Trans_addr
--==================================================================
ltmTransAddrNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmTransAddr entries in the table."
	::= { ltmTransAddr 1 } 

ltmTransAddrTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmTransAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of SNAT translated addresses."
	::= { ltmTransAddr 2 } 

ltmTransAddrEntry OBJECT-TYPE
	SYNTAX  LtmTransAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmTransAddr Table"
	INDEX {
		ltmTransAddrAddrType,
		ltmTransAddrAddr
	}
	::= { ltmTransAddrTable 1 } 

LtmTransAddrEntry ::= 
	SEQUENCE {
        	ltmTransAddrAddrType                                   InetAddressType,
        	ltmTransAddrAddr                                       InetAddress,
        	ltmTransAddrEnabled                                    INTEGER,
        	ltmTransAddrConnLimit                                  Integer32,
        	ltmTransAddrTcpIdleTimeout                             Integer32,
        	ltmTransAddrUdpIdleTimeout                             Integer32,
        	ltmTransAddrIpIdleTimeout                              Integer32,
        	ltmTransAddrArpEnabled                                 INTEGER,
        	ltmTransAddrUnitId                                     Integer32
	}

ltmTransAddrAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmTransAddrAddr"
	::= { ltmTransAddrEntry 1 } 

ltmTransAddrAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SNAT translation address for use as a server-side client address.
		on the server-side. It is interpreted within the context of 
		an ltmTransAddrAddrType value."
	::= { ltmTransAddrEntry 2 } 

ltmTransAddrEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether the specified SNAT translation address is enabled or not."
	::= { ltmTransAddrEntry 3 } 

ltmTransAddrConnLimit OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of connections the specified SNAT translation address is 
		 allowed to have open at one time."
	::= { ltmTransAddrEntry 4 } 

ltmTransAddrTcpIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The TCP idle timeout (in seconds) of the SNAT specified translation address."
	::= { ltmTransAddrEntry 5 } 

ltmTransAddrUdpIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The UDP idle timeout (in seconds) of the specified SNAT translation address."
	::= { ltmTransAddrEntry 6 } 

ltmTransAddrIpIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP idle timeout (in seconds) of the specified SNAT translation address."
	::= { ltmTransAddrEntry 7 } 

ltmTransAddrArpEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether ARP is enabled or not for the specified SNAT translation address."
	::= { ltmTransAddrEntry 8 } 

ltmTransAddrUnitId OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The unit number associated with the specified SNAT translation address."
	::= { ltmTransAddrEntry 9 } 

--==================================================================
-- Trans_addr_stat
--==================================================================
ltmTransAddrStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmTransAddrStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmTransAddrStat 1 } 

ltmTransAddrStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmTransAddrStat entries in the table."
	::= { ltmTransAddrStat 2 } 

ltmTransAddrStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmTransAddrStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of SNAT translated addresses."
	::= { ltmTransAddrStat 3 } 

ltmTransAddrStatEntry OBJECT-TYPE
	SYNTAX  LtmTransAddrStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmTransAddrStat Table"
	INDEX {
		ltmTransAddrStatAddrType,
		ltmTransAddrStatAddr
	}
	::= { ltmTransAddrStatTable 1 } 

LtmTransAddrStatEntry ::= 
	SEQUENCE {
        	ltmTransAddrStatAddrType                               InetAddressType,
        	ltmTransAddrStatAddr                                   InetAddress,
        	ltmTransAddrStatServerPktsIn                           Counter64,
        	ltmTransAddrStatServerBytesIn                          Counter64,
        	ltmTransAddrStatServerPktsOut                          Counter64,
        	ltmTransAddrStatServerBytesOut                         Counter64,
        	ltmTransAddrStatServerMaxConns                         Counter64,
        	ltmTransAddrStatServerTotConns                         Counter64,
        	ltmTransAddrStatServerCurConns                         Counter64
	}

ltmTransAddrStatAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmTransAddrStatAddr"
	::= { ltmTransAddrStatEntry 1 } 

ltmTransAddrStatAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SNAT translation address for use as a server-side client address.
		on the server-side. It is interpreted within the context of 
		an ltmTransAddrStatAddrType value."
	::= { ltmTransAddrStatEntry 2 } 

ltmTransAddrStatServerPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received from server-side."
	::= { ltmTransAddrStatEntry 3 } 

ltmTransAddrStatServerBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received from server-side."
	::= { ltmTransAddrStatEntry 4 } 

ltmTransAddrStatServerPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to server-side."
	::= { ltmTransAddrStatEntry 5 } 

ltmTransAddrStatServerBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to server-side."
	::= { ltmTransAddrStatEntry 6 } 

ltmTransAddrStatServerMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from server-side."
	::= { ltmTransAddrStatEntry 7 } 

ltmTransAddrStatServerTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from server-side."
	::= { ltmTransAddrStatEntry 8 } 

ltmTransAddrStatServerCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from server-side."
	::= { ltmTransAddrStatEntry 9 } 

--==================================================================
-- Snatpool
--==================================================================
ltmSnatPoolNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSnatPool entries in the table."
	::= { ltmSnatPool 1 } 

ltmSnatPoolTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSnatPoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of SNAT pools."
	::= { ltmSnatPool 2 } 

ltmSnatPoolEntry OBJECT-TYPE
	SYNTAX  LtmSnatPoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSnatPool Table"
	INDEX {
		ltmSnatPoolName
	}
	::= { ltmSnatPoolTable 1 } 

LtmSnatPoolEntry ::= 
	SEQUENCE {
        	ltmSnatPoolName                                        LongDisplayString
	}

ltmSnatPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT pool, which is a pool of SNAT translation addresses."
	::= { ltmSnatPoolEntry 1 } 

--==================================================================
-- Snatpool_stat
--==================================================================
ltmSnatPoolStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmSnatPoolStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmSnatPoolStat 1 } 

ltmSnatPoolStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSnatPoolStat entries in the table."
	::= { ltmSnatPoolStat 2 } 

ltmSnatPoolStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSnatPoolStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of SNAT pools."
	::= { ltmSnatPoolStat 3 } 

ltmSnatPoolStatEntry OBJECT-TYPE
	SYNTAX  LtmSnatPoolStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSnatPoolStat Table"
	INDEX {
		ltmSnatPoolStatName
	}
	::= { ltmSnatPoolStatTable 1 } 

LtmSnatPoolStatEntry ::= 
	SEQUENCE {
        	ltmSnatPoolStatName                                    LongDisplayString,
        	ltmSnatPoolStatServerPktsIn                            Counter64,
        	ltmSnatPoolStatServerBytesIn                           Counter64,
        	ltmSnatPoolStatServerPktsOut                           Counter64,
        	ltmSnatPoolStatServerBytesOut                          Counter64,
        	ltmSnatPoolStatServerMaxConns                          Counter64,
        	ltmSnatPoolStatServerTotConns                          Counter64,
        	ltmSnatPoolStatServerCurConns                          Counter64
	}

ltmSnatPoolStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the SNAT pool."
	::= { ltmSnatPoolStatEntry 1 } 

ltmSnatPoolStatServerPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received from server-side."
	::= { ltmSnatPoolStatEntry 2 } 

ltmSnatPoolStatServerBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received from server-side."
	::= { ltmSnatPoolStatEntry 3 } 

ltmSnatPoolStatServerPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to server-side."
	::= { ltmSnatPoolStatEntry 4 } 

ltmSnatPoolStatServerBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to server-side."
	::= { ltmSnatPoolStatEntry 5 } 

ltmSnatPoolStatServerMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from server-side."
	::= { ltmSnatPoolStatEntry 6 } 

ltmSnatPoolStatServerTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from server-side."
	::= { ltmSnatPoolStatEntry 7 } 

ltmSnatPoolStatServerCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from server-side."
	::= { ltmSnatPoolStatEntry 8 } 

--==================================================================
-- Snatpool_trans_addr
--==================================================================
ltmSnatpoolTransAddrNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSnatpoolTransAddr entries in the table."
	::= { ltmSnatpoolTransAddr 1 } 

ltmSnatpoolTransAddrTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSnatpoolTransAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of joining SnatPool to TransAddr."
	::= { ltmSnatpoolTransAddr 2 } 

ltmSnatpoolTransAddrEntry OBJECT-TYPE
	SYNTAX  LtmSnatpoolTransAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSnatpoolTransAddr Table"
	INDEX {
		ltmSnatpoolTransAddrSnatpoolName,
		ltmSnatpoolTransAddrTransAddrType,
		ltmSnatpoolTransAddrTransAddr
	}
	::= { ltmSnatpoolTransAddrTable 1 } 

LtmSnatpoolTransAddrEntry ::= 
	SEQUENCE {
        	ltmSnatpoolTransAddrSnatpoolName                       LongDisplayString,
        	ltmSnatpoolTransAddrTransAddrType                      InetAddressType,
        	ltmSnatpoolTransAddrTransAddr                          InetAddress
	}

ltmSnatpoolTransAddrSnatpoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT pool."
	::= { ltmSnatpoolTransAddrEntry 1 } 

ltmSnatpoolTransAddrTransAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmTransAddrAddr"
	::= { ltmSnatpoolTransAddrEntry 2 } 

ltmSnatpoolTransAddrTransAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The SNAT translation address associated with the specified SNAT pool.,
		It is interpreted within the context of an ltmSnatpoolTransAddrTransAddrType value."
	::= { ltmSnatpoolTransAddrEntry 3 } 

--==================================================================
-- Virtual_server
--==================================================================
ltmVirtualServNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServ entries in the table."
	::= { ltmVirtualServ 1 } 

ltmVirtualServTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of virtual servers."
	::= { ltmVirtualServ 2 } 

ltmVirtualServEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServ Table"
	INDEX {
		ltmVirtualServName
	}
	::= { ltmVirtualServTable 1 } 

LtmVirtualServEntry ::= 
	SEQUENCE {
        	ltmVirtualServName                                     LongDisplayString,
        	ltmVirtualServAddrType                                 InetAddressType,
        	ltmVirtualServAddr                                     InetAddress,
        	ltmVirtualServWildmaskType                             InetAddressType,
        	ltmVirtualServWildmask                                 InetAddress,
        	ltmVirtualServPort                                     INTEGER,
        	ltmVirtualServIpProto                                  INTEGER,
        	ltmVirtualServListedEnabledVlans                       INTEGER,
        	ltmVirtualServEnabled                                  INTEGER,
        	ltmVirtualServConnLimit                                Integer32,
        	ltmVirtualServRclass                                   LongDisplayString,
        	ltmVirtualServSfFlags                                  INTEGER,
        	ltmVirtualServTranslateAddr                            INTEGER,
        	ltmVirtualServTranslatePort                            INTEGER,
        	ltmVirtualServType                                     INTEGER,
        	ltmVirtualServSnatType                                 INTEGER,
        	ltmVirtualServLasthopPoolName                          LongDisplayString,
        	ltmVirtualServSnatpoolName                             LongDisplayString,
        	ltmVirtualServDefaultPool                              LongDisplayString,
        	ltmVirtualServFallbackPersist                          LongDisplayString,
        	ltmVirtualServActualPvaAccel                           INTEGER,
        	ltmVirtualServAvailabilityState                        INTEGER,
        	ltmVirtualServEnabledState                             INTEGER,
        	ltmVirtualServDisabledParentType                       Integer32,
        	ltmVirtualServStatusReason                             LongDisplayString,
        	ltmVirtualServGtmScore                                 Integer32,
        	ltmVirtualServCmpEnabled                               INTEGER
	}

ltmVirtualServName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServEntry 1 } 

ltmVirtualServAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmVirtualServAddr."
	::= { ltmVirtualServEntry 2 } 

ltmVirtualServAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of the specified virtual server. It is interpreted 
		 within the context of an ltmVitualServAddrType value."
	::= { ltmVirtualServEntry 3 } 

ltmVirtualServWildmaskType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmVirtualServWildmask."
	::= { ltmVirtualServEntry 4 } 

ltmVirtualServWildmask OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The wildcard netmask of the specified virtual server. It is interpreted 
		 within the context of an ltmVitualServWildmaskType value."
	::= { ltmVirtualServEntry 5 } 

ltmVirtualServPort OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The port number of the specified virtual server."
	::= { ltmVirtualServEntry 6 } 

ltmVirtualServIpProto OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP protocol (see RFC 1340) used by the specified virtual server."
	::= { ltmVirtualServEntry 7 } 

ltmVirtualServListedEnabledVlans OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether the specified virtual server is listed 
		as enabled or not on associated VLANs. The associated VLANs are 
		defined in ltmVirtualServVlanTable."
	::= { ltmVirtualServEntry 8 } 

ltmVirtualServEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The state indicating whether the specified virtual server is enabled or not."
	::= { ltmVirtualServEntry 9 } 

ltmVirtualServConnLimit OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of connections the specified virtual server is allowed 
		 to have open at one time."
	::= { ltmVirtualServEntry 10 } 

ltmVirtualServRclass OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The rate class that will be used to rate limit the traffic in 
		the specified virtual server."
	::= { ltmVirtualServEntry 11 } 

ltmVirtualServSfFlags OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The flag to indicate whether connection mirroring is 
		enabled or not for the specified virtual server."
	::= { ltmVirtualServEntry 12 } 

ltmVirtualServTranslateAddr OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether the address of the specified virtual server 
		should be translated."
	::= { ltmVirtualServEntry 13 } 

ltmVirtualServTranslatePort OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether the port of the specified virtual server 
		should be translated."
	::= { ltmVirtualServEntry 14 } 

ltmVirtualServType OBJECT-TYPE 
	SYNTAX INTEGER {
		poolbased(0),
		ipforward(1),
		l2forward(2),
		reject(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type supported by the specified virtual server.
		poolbased - The virtual server is based on a pool;
		ipforward - The virtual server only supports IP forwarding. 
		            There is no load balancing on this type of virtual server;
		l2forward - The virtual server only supports L2 forwarding. 
		            There is no load balancing on this type of virtual server;
		reject - All connections going to this virtual server will be rejected, and resets will be sent."
	::= { ltmVirtualServEntry 15 } 

ltmVirtualServSnatType OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		transaddr(1),
		snatpool(2),
		automap(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type of SNAT associated with the specified virtual server.
		none - No SNAT used by the virtual server;
		transaddr - The SNAT uses a single translation address (invalid type);
		snatpool - The SNAT uses a SNAT pool of translation addresses;
		automap - The SNAT uses self IP addresses."
	::= { ltmVirtualServEntry 16 } 

ltmVirtualServLasthopPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The last hop pool for the specified virtual server if traffic is 
		 transparent."
	::= { ltmVirtualServEntry 17 } 

ltmVirtualServSnatpoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SNAT pool used by the specified virtual server."
	::= { ltmVirtualServEntry 18 } 

ltmVirtualServDefaultPool OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a default pool used by the specified virtual server."
	::= { ltmVirtualServEntry 19 } 

ltmVirtualServFallbackPersist OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The persist profile name to use for fallback by the specified virtual server."
	::= { ltmVirtualServEntry 20 } 

ltmVirtualServActualPvaAccel OBJECT-TYPE 
	SYNTAX INTEGER {
		full(0),
		partial(1),
		none(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The actual hardware acceleration mode for the specified virtual server."
	::= { ltmVirtualServEntry 21 } 

ltmVirtualServAvailabilityState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsServStatusAvailState under ltmVirtualServStatus.
		The state of the specified virtual server availability indicated in color."
	::= { ltmVirtualServEntry 22 } 

ltmVirtualServEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsServStatusEnabledState under ltmVirtualServStatus.
		The state of the specified virtual server activity status, as specified 
		by the user."
	::= { ltmVirtualServEntry 23 } 

ltmVirtualServDisabledParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsServStatusParentType under ltmVirtualServStatus.
		The type of parent object which disabled the specified virtual server."
	::= { ltmVirtualServEntry 24 } 

ltmVirtualServStatusReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsServStatusDetailReason under ltmVirtualServStatus.
		The detail description of the node's status of parent object 
		which disabled the specified virtual server."
	::= { ltmVirtualServEntry 25 } 

ltmVirtualServGtmScore OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"A user-defined value that specifies the ranking of the virtual server 
		when compared to other virtual servers within the same pool"
	::= { ltmVirtualServEntry 26 } 

ltmVirtualServCmpEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether CMP (Cluster Multiple Processor) is enabled or not for the specified virtual server."
	::= { ltmVirtualServEntry 27 } 

--==================================================================
-- Virtual_server_stat
--==================================================================
ltmVirtualServStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmVirtualServStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmVirtualServStat 1 } 

ltmVirtualServStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServStat entries in the table."
	::= { ltmVirtualServStat 2 } 

ltmVirtualServStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of virtual servers."
	::= { ltmVirtualServStat 3 } 

ltmVirtualServStatEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServStat Table"
	INDEX {
		ltmVirtualServStatName
	}
	::= { ltmVirtualServStatTable 1 } 

LtmVirtualServStatEntry ::= 
	SEQUENCE {
        	ltmVirtualServStatName                                 LongDisplayString,
        	ltmVirtualServStatCsMinConnDur                         Counter64,
        	ltmVirtualServStatCsMaxConnDur                         Counter64,
        	ltmVirtualServStatCsMeanConnDur                        Counter64,
        	ltmVirtualServStatNoNodesErrors                        Counter64,
        	ltmVirtualServStatClientPktsIn                         Counter64,
        	ltmVirtualServStatClientBytesIn                        Counter64,
        	ltmVirtualServStatClientPktsOut                        Counter64,
        	ltmVirtualServStatClientBytesOut                       Counter64,
        	ltmVirtualServStatClientMaxConns                       Counter64,
        	ltmVirtualServStatClientTotConns                       Counter64,
        	ltmVirtualServStatClientCurConns                       Counter64,
        	ltmVirtualServStatEphemeralPktsIn                      Counter64,
        	ltmVirtualServStatEphemeralBytesIn                     Counter64,
        	ltmVirtualServStatEphemeralPktsOut                     Counter64,
        	ltmVirtualServStatEphemeralBytesOut                    Counter64,
        	ltmVirtualServStatEphemeralMaxConns                    Counter64,
        	ltmVirtualServStatEphemeralTotConns                    Counter64,
        	ltmVirtualServStatEphemeralCurConns                    Counter64,
        	ltmVirtualServStatPvaPktsIn                            Counter64,
        	ltmVirtualServStatPvaBytesIn                           Counter64,
        	ltmVirtualServStatPvaPktsOut                           Counter64,
        	ltmVirtualServStatPvaBytesOut                          Counter64,
        	ltmVirtualServStatPvaMaxConns                          Counter64,
        	ltmVirtualServStatPvaTotConns                          Counter64,
        	ltmVirtualServStatPvaCurConns                          Counter64,
        	ltmVirtualServStatTotRequests                          Counter64,
        	ltmVirtualServStatTotPvaAssistConn                     Counter64,
        	ltmVirtualServStatCurrPvaAssistConn                    Counter64
	}

ltmVirtualServStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServStatEntry 1 } 

ltmVirtualServStatCsMinConnDur OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The minimum connection duration in milliseconds among all connections 
		through the specified virtual server."
	::= { ltmVirtualServStatEntry 2 } 

ltmVirtualServStatCsMaxConnDur OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connection duration in milliseconds among all connections 
		through the specified virtual server."
	::= { ltmVirtualServStatEntry 3 } 

ltmVirtualServStatCsMeanConnDur OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The average connection duration in milliseconds for all connections 
		through the specified virtual server."
	::= { ltmVirtualServStatEntry 4 } 

ltmVirtualServStatNoNodesErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of no-node errors. If active server node is zero, 
	         this counter is incremented."
	::= { ltmVirtualServStatEntry 5 } 

ltmVirtualServStatClientPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received by the specified virtual server from client-side."
	::= { ltmVirtualServStatEntry 6 } 

ltmVirtualServStatClientBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received by the specified virtual server from client-side."
	::= { ltmVirtualServStatEntry 7 } 

ltmVirtualServStatClientPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to client-side from the specified virtual server."
	::= { ltmVirtualServStatEntry 8 } 

ltmVirtualServStatClientBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to client-side from the specified virtual server."
	::= { ltmVirtualServStatEntry 9 } 

ltmVirtualServStatClientMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections from client-side to the specified virtual server."
	::= { ltmVirtualServStatEntry 10 } 

ltmVirtualServStatClientTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections from client-side to the specified virtual server."
	::= { ltmVirtualServStatEntry 11 } 

ltmVirtualServStatClientCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections from client-side to the specified virtual server."
	::= { ltmVirtualServStatEntry 12 } 

ltmVirtualServStatEphemeralPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received ephemeral by the specified virtual server."
	::= { ltmVirtualServStatEntry 13 } 

ltmVirtualServStatEphemeralBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received ephemeral by the specified virtual server."
	::= { ltmVirtualServStatEntry 14 } 

ltmVirtualServStatEphemeralPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets transmitted ephemeral from the specified virtual server."
	::= { ltmVirtualServStatEntry 15 } 

ltmVirtualServStatEphemeralBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes transmitted ephemeral from the specified virtual server."
	::= { ltmVirtualServStatEntry 16 } 

ltmVirtualServStatEphemeralMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum ephemeral connections to the specified virtual server."
	::= { ltmVirtualServStatEntry 17 } 

ltmVirtualServStatEphemeralTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total ephemeral connections to the specified virtual server."
	::= { ltmVirtualServStatEntry 18 } 

ltmVirtualServStatEphemeralCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current ephemeral connections to the specified virtual server."
	::= { ltmVirtualServStatEntry 19 } 

ltmVirtualServStatPvaPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated packets received by the specified virtual server."
	::= { ltmVirtualServStatEntry 20 } 

ltmVirtualServStatPvaBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated bytes received by the specified virtual server."
	::= { ltmVirtualServStatEntry 21 } 

ltmVirtualServStatPvaPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated packets sent out from the specified virtual server."
	::= { ltmVirtualServStatEntry 22 } 

ltmVirtualServStatPvaBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of hardware accelerated bytes sent out from the specified virtual server."
	::= { ltmVirtualServStatEntry 23 } 

ltmVirtualServStatPvaMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum hardware accelerated connections to the specified virtual server."
	::= { ltmVirtualServStatEntry 24 } 

ltmVirtualServStatPvaTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total hardware accelerated connections to the specified virtual server."
	::= { ltmVirtualServStatEntry 25 } 

ltmVirtualServStatPvaCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current hardware accelerated connections to the specified virtual server."
	::= { ltmVirtualServStatEntry 26 } 

ltmVirtualServStatTotRequests OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of requests going through the specified virtual server."
	::= { ltmVirtualServStatEntry 27 } 

ltmVirtualServStatTotPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections to the specified virtual server, which 
		are partially hardware accelerated."
	::= { ltmVirtualServStatEntry 28 } 

ltmVirtualServStatCurrPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of connections to the specified virtual server, which
		are partially hardware accelerated."
	::= { ltmVirtualServStatEntry 29 } 

--==================================================================
-- Virtual_server_auth
--==================================================================
ltmVirtualServAuthNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServAuth entries in the table."
	::= { ltmVirtualServAuth 1 } 

ltmVirtualServAuthTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServAuthEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of virtual server auth profiles."
	::= { ltmVirtualServAuth 2 } 

ltmVirtualServAuthEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServAuthEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServAuth Table"
	INDEX {
		ltmVirtualServAuthVsName,
		ltmVirtualServAuthProfileName
	}
	::= { ltmVirtualServAuthTable 1 } 

LtmVirtualServAuthEntry ::= 
	SEQUENCE {
        	ltmVirtualServAuthVsName                               LongDisplayString,
        	ltmVirtualServAuthProfileName                          LongDisplayString
	}

ltmVirtualServAuthVsName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServAuthEntry 1 } 

ltmVirtualServAuthProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of an auth profile associated with the specified virtual server."
	::= { ltmVirtualServAuthEntry 2 } 

--==================================================================
-- Virtual_server_persist
--==================================================================
ltmVirtualServPersistNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServPersist entries in the table."
	::= { ltmVirtualServPersist 1 } 

ltmVirtualServPersistTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServPersistEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of virtual server persistence profiles."
	::= { ltmVirtualServPersist 2 } 

ltmVirtualServPersistEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServPersistEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServPersist Table"
	INDEX {
		ltmVirtualServPersistVsName,
		ltmVirtualServPersistProfileName
	}
	::= { ltmVirtualServPersistTable 1 } 

LtmVirtualServPersistEntry ::= 
	SEQUENCE {
        	ltmVirtualServPersistVsName                            LongDisplayString,
        	ltmVirtualServPersistProfileName                       LongDisplayString,
        	ltmVirtualServPersistUseDefault                        INTEGER
	}

ltmVirtualServPersistVsName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServPersistEntry 1 } 

ltmVirtualServPersistProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a persist profile associated with the specified virtual server."
	::= { ltmVirtualServPersistEntry 2 } 

ltmVirtualServPersistUseDefault OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The persist profile is to be used if a rule does not 
		select a persist type."
	::= { ltmVirtualServPersistEntry 3 } 

--==================================================================
-- Virtual_server_profile
--==================================================================
ltmVirtualServProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServProfile entries in the table."
	::= { ltmVirtualServProfile 1 } 

ltmVirtualServProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of virtual server profiles."
	::= { ltmVirtualServProfile 2 } 

ltmVirtualServProfileEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServProfile Table"
	INDEX {
		ltmVirtualServProfileVsName,
		ltmVirtualServProfileProfileName
	}
	::= { ltmVirtualServProfileTable 1 } 

LtmVirtualServProfileEntry ::= 
	SEQUENCE {
        	ltmVirtualServProfileVsName                            LongDisplayString,
        	ltmVirtualServProfileProfileName                       LongDisplayString,
        	ltmVirtualServProfileType                              INTEGER,
        	ltmVirtualServProfileContext                           INTEGER
	}

ltmVirtualServProfileVsName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServProfileEntry 1 } 

ltmVirtualServProfileProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a profile associated with the specified virtual server."
	::= { ltmVirtualServProfileEntry 2 } 

ltmVirtualServProfileType OBJECT-TYPE 
	SYNTAX INTEGER {
		auth(0),
		http(1),
		serverssl(2),
		clientssl(3),
		fastl4(4),
		tcp(5),
		udp(6),
		ftp(7),
		persist(8),
		connpool(9),
		stream(10),
		xml(11),
		fasthttp(12),
		iiop(13),
		rtsp(14),
		user(15),
		httpclass(16),
		dns(17),
		sctp(18),
		instance(19),
		sipp(20)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type of the profile used by the specified virtual server."
	::= { ltmVirtualServProfileEntry 3 } 

ltmVirtualServProfileContext OBJECT-TYPE 
	SYNTAX INTEGER {
		all(0),
		client(1),
		server(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This is used to determine which side of the proxy a protocol
		type profile (specifically  TCP/UDP) is applied to.	
		none   - for profiles that don't need any context;
		all    - profile applies to both client and server;
		client - profile applies to the client-side;
		server - profile applies to the server-side."
	::= { ltmVirtualServProfileEntry 4 } 

--==================================================================
-- Virtual_server_pool
--==================================================================
ltmVirtualServPoolNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServPool entries in the table."
	::= { ltmVirtualServPool 1 } 

ltmVirtualServPoolTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServPoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of non-default pools related to virtual servers."
	::= { ltmVirtualServPool 2 } 

ltmVirtualServPoolEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServPoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServPool Table"
	INDEX {
		ltmVirtualServPoolVirtualServerName,
		ltmVirtualServPoolPoolName
	}
	::= { ltmVirtualServPoolTable 1 } 

LtmVirtualServPoolEntry ::= 
	SEQUENCE {
        	ltmVirtualServPoolVirtualServerName                    LongDisplayString,
        	ltmVirtualServPoolPoolName                             LongDisplayString,
        	ltmVirtualServPoolRuleName                             LongDisplayString
	}

ltmVirtualServPoolVirtualServerName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServPoolEntry 1 } 

ltmVirtualServPoolPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a non-default pool that the specified virtual server is referencing."
	::= { ltmVirtualServPoolEntry 2 } 

ltmVirtualServPoolRuleName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a rule that the specified virtual server is referencing.
		This is for future use and has not been supported in current version."
	::= { ltmVirtualServPoolEntry 3 } 

--==================================================================
-- Virtual_server_clone_pool
--==================================================================
ltmVirtualServClonePoolNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServClonePool entries in the table."
	::= { ltmVirtualServClonePool 1 } 

ltmVirtualServClonePoolTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServClonePoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of pools related to virtual servers."
	::= { ltmVirtualServClonePool 2 } 

ltmVirtualServClonePoolEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServClonePoolEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServClonePool Table"
	INDEX {
		ltmVirtualServClonePoolVirtualServerName,
		ltmVirtualServClonePoolPoolName,
		ltmVirtualServClonePoolType
	}
	::= { ltmVirtualServClonePoolTable 1 } 

LtmVirtualServClonePoolEntry ::= 
	SEQUENCE {
        	ltmVirtualServClonePoolVirtualServerName               LongDisplayString,
        	ltmVirtualServClonePoolPoolName                        LongDisplayString,
        	ltmVirtualServClonePoolType                            INTEGER
	}

ltmVirtualServClonePoolVirtualServerName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServClonePoolEntry 1 } 

ltmVirtualServClonePoolPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a clone pool associated with the specified virtual server."
	::= { ltmVirtualServClonePoolEntry 2 } 

ltmVirtualServClonePoolType OBJECT-TYPE 
	SYNTAX INTEGER {
		unspec(0),
		clientside(1),
		serverside(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The type of the clone pool associated with the specified virtual server."
	::= { ltmVirtualServClonePoolEntry 3 } 

--==================================================================
-- Virtual_server_rule
--==================================================================
ltmVirtualServRuleNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServRule entries in the table."
	::= { ltmVirtualServRule 1 } 

ltmVirtualServRuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of rules related to virtual servers."
	::= { ltmVirtualServRule 2 } 

ltmVirtualServRuleEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServRule Table"
	INDEX {
		ltmVirtualServRuleVirtualServerName,
		ltmVirtualServRuleRuleName
	}
	::= { ltmVirtualServRuleTable 1 } 

LtmVirtualServRuleEntry ::= 
	SEQUENCE {
        	ltmVirtualServRuleVirtualServerName                    LongDisplayString,
        	ltmVirtualServRuleRuleName                             LongDisplayString,
        	ltmVirtualServRulePriority                             INTEGER
	}

ltmVirtualServRuleVirtualServerName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServRuleEntry 1 } 

ltmVirtualServRuleRuleName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a rule associated with the specified virtual server."
	::= { ltmVirtualServRuleEntry 2 } 

ltmVirtualServRulePriority OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The priority of the rule among rules used by the specified virtual server."
	::= { ltmVirtualServRuleEntry 3 } 

--==================================================================
-- Virtual_server_vlan
--==================================================================
ltmVirtualServVlanNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServVlan entries in the table."
	::= { ltmVirtualServVlan 1 } 

ltmVirtualServVlanTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualServVlanEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing VLAN information associated with virtual server."
	::= { ltmVirtualServVlan 2 } 

ltmVirtualServVlanEntry OBJECT-TYPE
	SYNTAX  LtmVirtualServVlanEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualServVlan Table"
	INDEX {
		ltmVirtualServVlanVsName,
		ltmVirtualServVlanVlanName
	}
	::= { ltmVirtualServVlanTable 1 } 

LtmVirtualServVlanEntry ::= 
	SEQUENCE {
        	ltmVirtualServVlanVsName                               LongDisplayString,
        	ltmVirtualServVlanVlanName                             LongDisplayString
	}

ltmVirtualServVlanVsName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVirtualServVlanEntry 1 } 

ltmVirtualServVlanVlanName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a VLAN which the specified virtual server associated with."
	::= { ltmVirtualServVlanEntry 2 } 

--==================================================================
-- Virtual_address
--==================================================================
ltmVirtualAddrNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualAddr entries in the table."
	::= { ltmVirtualAddr 1 } 

ltmVirtualAddrTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of virtual server addresses."
	::= { ltmVirtualAddr 2 } 

ltmVirtualAddrEntry OBJECT-TYPE
	SYNTAX  LtmVirtualAddrEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualAddr Table"
	INDEX {
		ltmVirtualAddrAddrType,
		ltmVirtualAddrAddr
	}
	::= { ltmVirtualAddrTable 1 } 

LtmVirtualAddrEntry ::= 
	SEQUENCE {
        	ltmVirtualAddrAddrType                                 InetAddressType,
        	ltmVirtualAddrAddr                                     InetAddress,
        	ltmVirtualAddrEnabled                                  INTEGER,
        	ltmVirtualAddrConnLimit                                Integer32,
        	ltmVirtualAddrArpEnabled                               INTEGER,
        	ltmVirtualAddrSfFlags                                  INTEGER,
        	ltmVirtualAddrUnitId                                   Integer32,
        	ltmVirtualAddrRouteAdvertisement                       INTEGER,
        	ltmVirtualAddrAvailabilityState                        INTEGER,
        	ltmVirtualAddrEnabledState                             INTEGER,
        	ltmVirtualAddrDisabledParentType                       Integer32,
        	ltmVirtualAddrStatusReason                             LongDisplayString,
        	ltmVirtualAddrServer                                   INTEGER,
        	ltmVirtualAddrIsFloat                                  INTEGER
	}

ltmVirtualAddrAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmVirtualAddrAddr"
	::= { ltmVirtualAddrEntry 1 } 

ltmVirtualAddrAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a virtual address. 
		It is interpreted within the context of an ltmVitualAddrAddrType value."
	::= { ltmVirtualAddrEntry 2 } 

ltmVirtualAddrEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The state indicating whether the specified virtual address is enabled or not."
	::= { ltmVirtualAddrEntry 3 } 

ltmVirtualAddrConnLimit OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of connections the specified virtual address is 
		 allowed to have open at one time."
	::= { ltmVirtualAddrEntry 4 } 

ltmVirtualAddrArpEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether ARP for the specified virtual address 
		is enabled or not."
	::= { ltmVirtualAddrEntry 5 } 

ltmVirtualAddrSfFlags OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! This feature has been eliminated.
		The flag to indicate whether connection mirroring is 
		enabled for the specified virtual address."
	::= { ltmVirtualAddrEntry 6 } 

ltmVirtualAddrUnitId OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The unit number associated with the specified virtual address."
	::= { ltmVirtualAddrEntry 7 } 

ltmVirtualAddrRouteAdvertisement OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state to determine if the specified virtual address should be 
		readvertised by the ZebOS routing daemons or not."
	::= { ltmVirtualAddrEntry 8 } 

ltmVirtualAddrAvailabilityState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsAddrStatusAvailState under ltmVirtualAddrStatus.
		The state of the specified virtual address availability indicated in color."
	::= { ltmVirtualAddrEntry 9 } 

ltmVirtualAddrEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsAddrStatusEnabledState under ltmVirtualAddrStatus.
		The state of the specified virtual address activity status, 
		as specified by the user."
	::= { ltmVirtualAddrEntry 10 } 

ltmVirtualAddrDisabledParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsAddrStatusParentType under ltmVirtualAddrStatus.
		The type of parent object which disabled the specified virtual address."
	::= { ltmVirtualAddrEntry 11 } 

ltmVirtualAddrStatusReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated!  
		Replaced by ltmVsAddrStatusDetailReason under ltmVirtualAddrStatus.
		The detail description of the virtual address's status of parent object 
		which disabled the specified virtual address."
	::= { ltmVirtualAddrEntry 12 } 

ltmVirtualAddrServer OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		any(1),
		all(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"That state to control how status of virtual address is depending on 
		status of virtual server.
		none: virtual address is always green regardless of virtual server status.
		any: any virtual server is green, virtual address is green.
		all: all virtual servers must be green before virtual address is declared as green."
	::= { ltmVirtualAddrEntry 13 } 

ltmVirtualAddrIsFloat OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether the virtual address should be shared 
		between the redundant pair. This is typically used in one-armed 
		Combo pair, where GTM is only licensed on one of the boxes."
	::= { ltmVirtualAddrEntry 14 } 

--==================================================================
-- Virtual_address_stat
--==================================================================
ltmVirtualAddrStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmVirtualAddrStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmVirtualAddrStat 1 } 

ltmVirtualAddrStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualAddrStat entries in the table."
	::= { ltmVirtualAddrStat 2 } 

ltmVirtualAddrStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualAddrStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of virtual server addresses."
	::= { ltmVirtualAddrStat 3 } 

ltmVirtualAddrStatEntry OBJECT-TYPE
	SYNTAX  LtmVirtualAddrStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualAddrStat Table"
	INDEX {
		ltmVirtualAddrStatAddrType,
		ltmVirtualAddrStatAddr
	}
	::= { ltmVirtualAddrStatTable 1 } 

LtmVirtualAddrStatEntry ::= 
	SEQUENCE {
        	ltmVirtualAddrStatAddrType                             InetAddressType,
        	ltmVirtualAddrStatAddr                                 InetAddress,
        	ltmVirtualAddrStatClientPktsIn                         Counter64,
        	ltmVirtualAddrStatClientBytesIn                        Counter64,
        	ltmVirtualAddrStatClientPktsOut                        Counter64,
        	ltmVirtualAddrStatClientBytesOut                       Counter64,
        	ltmVirtualAddrStatClientMaxConns                       Counter64,
        	ltmVirtualAddrStatClientTotConns                       Counter64,
        	ltmVirtualAddrStatClientCurConns                       Counter64,
        	ltmVirtualAddrStatPvaPktsIn                            Counter64,
        	ltmVirtualAddrStatPvaBytesIn                           Counter64,
        	ltmVirtualAddrStatPvaPktsOut                           Counter64,
        	ltmVirtualAddrStatPvaBytesOut                          Counter64,
        	ltmVirtualAddrStatPvaMaxConns                          Counter64,
        	ltmVirtualAddrStatPvaTotConns                          Counter64,
        	ltmVirtualAddrStatPvaCurConns                          Counter64,
        	ltmVirtualAddrStatTotPvaAssistConn                     Counter64,
        	ltmVirtualAddrStatCurrPvaAssistConn                    Counter64
	}

ltmVirtualAddrStatAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmVirtualAddrStatAddr"
	::= { ltmVirtualAddrStatEntry 1 } 

ltmVirtualAddrStatAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a virtual address. It is interpreted 
		 within the context of a ltmVitualAddrStatAddrType value."
	::= { ltmVirtualAddrStatEntry 2 } 

ltmVirtualAddrStatClientPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets received by the specified virtual address
		from client-side."
	::= { ltmVirtualAddrStatEntry 3 } 

ltmVirtualAddrStatClientBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes received by the specified virtual address 
		from client-side."
	::= { ltmVirtualAddrStatEntry 4 } 

ltmVirtualAddrStatClientPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of packets sent to client-side from the specified virtual address."
	::= { ltmVirtualAddrStatEntry 5 } 

ltmVirtualAddrStatClientBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes sent to client-side from the specified virtual address."
	::= { ltmVirtualAddrStatEntry 6 } 

ltmVirtualAddrStatClientMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum connections to the specified virtual address from client-side."
	::= { ltmVirtualAddrStatEntry 7 } 

ltmVirtualAddrStatClientTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total connections to the specified virtual address from client-side."
	::= { ltmVirtualAddrStatEntry 8 } 

ltmVirtualAddrStatClientCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current connections to the specified virtual address from client-side."
	::= { ltmVirtualAddrStatEntry 9 } 

ltmVirtualAddrStatPvaPktsIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated packets received by the specified virtual address."
	::= { ltmVirtualAddrStatEntry 10 } 

ltmVirtualAddrStatPvaBytesIn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated bytes received by the specified virtual address."
	::= { ltmVirtualAddrStatEntry 11 } 

ltmVirtualAddrStatPvaPktsOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated packets sent out from  the specified virtual address."
	::= { ltmVirtualAddrStatEntry 12 } 

ltmVirtualAddrStatPvaBytesOut OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of hardware accelerated bytes sent out from the specified virtual address."
	::= { ltmVirtualAddrStatEntry 13 } 

ltmVirtualAddrStatPvaMaxConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum hardware accelerated connections to the specified virtual address."
	::= { ltmVirtualAddrStatEntry 14 } 

ltmVirtualAddrStatPvaTotConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total hardware accelerated connections to the specified virtual address."
	::= { ltmVirtualAddrStatEntry 15 } 

ltmVirtualAddrStatPvaCurConns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current hardware accelerated connections to the specified virtual address."
	::= { ltmVirtualAddrStatEntry 16 } 

ltmVirtualAddrStatTotPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections to the specified virtual address,
		which are partially hardware accelerated."
	::= { ltmVirtualAddrStatEntry 17 } 

ltmVirtualAddrStatCurrPvaAssistConn OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of connections to the specified virtual address,
		which are partially hardware accelerated."
	::= { ltmVirtualAddrStatEntry 18 } 

--==================================================================
-- Profile_fasthttp
--==================================================================
ltmFastHttpProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmFastHttpProfile entries in the table."
	::= { ltmFastHttpProfile 1 } 

ltmFastHttpProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmFastHttpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of Fast HTTP profile."
	::= { ltmFastHttpProfile 2 } 

ltmFastHttpProfileEntry OBJECT-TYPE
	SYNTAX  LtmFastHttpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmFastHttpProfile Table"
	INDEX {
		ltmFastHttpProfileName
	}
	::= { ltmFastHttpProfileTable 1 } 

LtmFastHttpProfileEntry ::= 
	SEQUENCE {
        	ltmFastHttpProfileName                                 LongDisplayString,
        	ltmFastHttpProfileConfigSource                         INTEGER,
        	ltmFastHttpProfileDefaultName                          LongDisplayString,
        	ltmFastHttpProfileResetOnTimeout                       INTEGER,
        	ltmFastHttpProfileIdleTimeout                          Integer32,
        	ltmFastHttpProfileMssOverride                          Integer32,
        	ltmFastHttpProfileClientCloseTimeout                   Integer32,
        	ltmFastHttpProfileServerCloseTimeout                   Integer32,
        	ltmFastHttpProfileConnpoolMaxSize                      Integer32,
        	ltmFastHttpProfileConnpoolMinSize                      Integer32,
        	ltmFastHttpProfileConnpoolStep                         Integer32,
        	ltmFastHttpProfileConnpoolMaxReuse                     Integer32,
        	ltmFastHttpProfileConnpoolIdleTimeout                  Integer32,
        	ltmFastHttpProfileMaxHeaderSize                        Integer32,
        	ltmFastHttpProfileMaxRequests                          Integer32,
        	ltmFastHttpProfileInsertXforwardedFor                  INTEGER,
        	ltmFastHttpProfileHttp11CloseWorkarounds               INTEGER,
        	ltmFastHttpProfileHeaderInsert                         LongDisplayString,
        	ltmFastHttpProfileUncleanShutdown                      INTEGER,
        	ltmFastHttpProfileForceHttp10Response                  INTEGER,
        	ltmFastHttpProfileLayer7                               INTEGER,
        	ltmFastHttpProfileConnpoolReplenish                    INTEGER
	}

ltmFastHttpProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a fast HTTP profile."
	::= { ltmFastHttpProfileEntry 1 } 

ltmFastHttpProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmFastHttpProfileEntry 2 } 

ltmFastHttpProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmFastHttpProfileEntry 3 } 

ltmFastHttpProfileResetOnTimeout OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"If true and a TCP connection exceeds its idle_timeout,
		send a reset in addition to deleting the connection."
	::= { ltmFastHttpProfileEntry 4 } 

ltmFastHttpProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of seconds without traffic before a connection 
		is eligible for deletion."
	::= { ltmFastHttpProfileEntry 5 } 

ltmFastHttpProfileMssOverride OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"If non-zero and less than the 1460 default, this value 
		overrides the maximum segment size for server-side flows."
	::= { ltmFastHttpProfileEntry 6 } 

ltmFastHttpProfileClientCloseTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Idle timeout override when waiting for the client to close. 
		This occurs after a client FIN is received or after a FIN 
		is sent. 0 is immediate, -1 is indefinite."
	::= { ltmFastHttpProfileEntry 7 } 

ltmFastHttpProfileServerCloseTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Idle timeout override when waiting for the server to close. 
		This occurs if the server flow is not suitable for reuse or 
		after a FIN is received on an unspliced server connection. 
		0 is immediate, -1 is indefinite."
	::= { ltmFastHttpProfileEntry 8 } 

ltmFastHttpProfileConnpoolMaxSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum number of connections to any given LB pool.
		0 for unlimited."
	::= { ltmFastHttpProfileEntry 9 } 

ltmFastHttpProfileConnpoolMinSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Minimum number of connections to any given LB pool.
		0 is an acceptable value."
	::= { ltmFastHttpProfileEntry 10 } 

ltmFastHttpProfileConnpoolStep OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Connection ramp-up increment. Must be greater than 0."
	::= { ltmFastHttpProfileEntry 11 } 

ltmFastHttpProfileConnpoolMaxReuse OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum number of times a server-side flow will be reused. 
		0 for unlimited."
	::= { ltmFastHttpProfileEntry 12 } 

ltmFastHttpProfileConnpoolIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Idle timeout override for unspliced server-side flows in the 
		reuse pool. 0 is disabled, i.e. use the default idle timeout."
	::= { ltmFastHttpProfileEntry 13 } 

ltmFastHttpProfileMaxHeaderSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum amount of data that will be buffered in order to 
		make a content-switching decision."
	::= { ltmFastHttpProfileEntry 14 } 

ltmFastHttpProfileMaxRequests OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum number of requests on a client-side flow before 
		the flow is shutdown. 0 for unlimited."
	::= { ltmFastHttpProfileEntry 15 } 

ltmFastHttpProfileInsertXforwardedFor OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state whether to insert or replace X-Forwarded-For header 
		with client IP."
	::= { ltmFastHttpProfileEntry 16 } 

ltmFastHttpProfileHttp11CloseWorkarounds OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state to workaround problems with certain brands of benchmarking
		software that cannot handle FIN-PUSH on HTTP/1.1 responses."
	::= { ltmFastHttpProfileEntry 17 } 

ltmFastHttpProfileHeaderInsert OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Insert the given string as a header. If the header already 
		exists, it is not replaced. Unlike HTTP, this string does not 
		support rule command expansion."
	::= { ltmFastHttpProfileEntry 18 } 

ltmFastHttpProfileUncleanShutdown OBJECT-TYPE 
	SYNTAX INTEGER {
		disable(0),
		enable(1),
		fast(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The mode to indicate whether to do unclean shutdown for client connections."
	::= { ltmFastHttpProfileEntry 19 } 

ltmFastHttpProfileForceHttp10Response OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state to indicate whether to rewrite server's HTTP version to 1.0 in status
		line in order to dissuade the client from pipelining or chunking."
	::= { ltmFastHttpProfileEntry 20 } 

ltmFastHttpProfileLayer7 OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if false, we don't parse HTTP requests. This is useful for 
		providing SYN-proxy protection for L4 connections through a SNAT where the 
		client sends data to the server before the server responds."
	::= { ltmFastHttpProfileEntry 21 } 

ltmFastHttpProfileConnpoolReplenish OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether the connpool should be replenished 
		to its prior number of connections when a connection is closed 
		by the server. If this is disabled, then we  will only replenish 
		a closed server side connection residing in the connpool if there are 
		less than ltmFastHttpProfileMinSizei (see above) connections 
		in the pool."
	::= { ltmFastHttpProfileEntry 22 } 

--==================================================================
-- Profile_fasthttp_stat
--==================================================================
ltmFastHttpProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmFastHttpProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmFastHttpProfileStat 1 } 

ltmFastHttpProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmFastHttpProfileStat entries in the table."
	::= { ltmFastHttpProfileStat 2 } 

ltmFastHttpProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmFastHttpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of Fast HTTP profile."
	::= { ltmFastHttpProfileStat 3 } 

ltmFastHttpProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmFastHttpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmFastHttpProfileStat Table"
	INDEX {
		ltmFastHttpProfileStatName
	}
	::= { ltmFastHttpProfileStatTable 1 } 

LtmFastHttpProfileStatEntry ::= 
	SEQUENCE {
        	ltmFastHttpProfileStatName                             LongDisplayString,
        	ltmFastHttpProfileStatClientSyns                       Counter64,
        	ltmFastHttpProfileStatClientAccepts                    Counter64,
        	ltmFastHttpProfileStatServerConnects                   Counter64,
        	ltmFastHttpProfileStatConnpoolCurSize                  Integer32,
        	ltmFastHttpProfileStatConnpoolMaxSize                  Integer32,
        	ltmFastHttpProfileStatConnpoolReuses                   Counter64,
        	ltmFastHttpProfileStatConnpoolExhausted                Counter64,
        	ltmFastHttpProfileStatNumberReqs                       Counter64,
        	ltmFastHttpProfileStatUnbufferedReqs                   Counter64,
        	ltmFastHttpProfileStatGetReqs                          Counter64,
        	ltmFastHttpProfileStatPostReqs                         Counter64,
        	ltmFastHttpProfileStatV9Reqs                           Counter64,
        	ltmFastHttpProfileStatV10Reqs                          Counter64,
        	ltmFastHttpProfileStatV11Reqs                          Counter64,
        	ltmFastHttpProfileStatResp2xxCnt                       Counter64,
        	ltmFastHttpProfileStatResp3xxCnt                       Counter64,
        	ltmFastHttpProfileStatResp4xxCnt                       Counter64,
        	ltmFastHttpProfileStatResp5xxCnt                       Counter64,
        	ltmFastHttpProfileStatReqParseErrors                   Counter64,
        	ltmFastHttpProfileStatRespParseErrors                  Counter64,
        	ltmFastHttpProfileStatClientRxBad                      Counter64,
        	ltmFastHttpProfileStatServerRxBad                      Counter64,
        	ltmFastHttpProfileStatPipelinedReqs                    Counter64
	}

ltmFastHttpProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a fast HTTP profile."
	::= { ltmFastHttpProfileStatEntry 1 } 

ltmFastHttpProfileStatClientSyns OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of client SYN cookies generated."
	::= { ltmFastHttpProfileStatEntry 2 } 

ltmFastHttpProfileStatClientAccepts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of client TCP accepts."
	::= { ltmFastHttpProfileStatEntry 3 } 

ltmFastHttpProfileStatServerConnects OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of server TCP connects."
	::= { ltmFastHttpProfileStatEntry 4 } 

ltmFastHttpProfileStatConnpoolCurSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of available server-side flows in the reuse pool."
	::= { ltmFastHttpProfileStatEntry 5 } 

ltmFastHttpProfileStatConnpoolMaxSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Max number of available server-side flows in the reuse pool."
	::= { ltmFastHttpProfileStatEntry 6 } 

ltmFastHttpProfileStatConnpoolReuses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of times a server-side flow was reused from the pool."
	::= { ltmFastHttpProfileStatEntry 7 } 

ltmFastHttpProfileStatConnpoolExhausted OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of times the reuse pool was exhausted."
	::= { ltmFastHttpProfileStatEntry 8 } 

ltmFastHttpProfileStatNumberReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of http requests."
	::= { ltmFastHttpProfileStatEntry 9 } 

ltmFastHttpProfileStatUnbufferedReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of unbuffered requests."
	::= { ltmFastHttpProfileStatEntry 10 } 

ltmFastHttpProfileStatGetReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of get requests."
	::= { ltmFastHttpProfileStatEntry 11 } 

ltmFastHttpProfileStatPostReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of post requests."
	::= { ltmFastHttpProfileStatEntry 12 } 

ltmFastHttpProfileStatV9Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 9 requests."
	::= { ltmFastHttpProfileStatEntry 13 } 

ltmFastHttpProfileStatV10Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 10 requests."
	::= { ltmFastHttpProfileStatEntry 14 } 

ltmFastHttpProfileStatV11Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 11 requests."
	::= { ltmFastHttpProfileStatEntry 15 } 

ltmFastHttpProfileStatResp2xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of server-side responses in range of 200 to 206 
		(successful responses)."
	::= { ltmFastHttpProfileStatEntry 16 } 

ltmFastHttpProfileStatResp3xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of server-side responses in range of 300 to 307 
		(redirection responses)."
	::= { ltmFastHttpProfileStatEntry 17 } 

ltmFastHttpProfileStatResp4xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of server-side responses in range of 400 to 417 (client errors). "
	::= { ltmFastHttpProfileStatEntry 18 } 

ltmFastHttpProfileStatResp5xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of server-side responses in range of 500 to 505 (server errors)."
	::= { ltmFastHttpProfileStatEntry 19 } 

ltmFastHttpProfileStatReqParseErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of request parse errors."
	::= { ltmFastHttpProfileStatEntry 20 } 

ltmFastHttpProfileStatRespParseErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of response parse errors."
	::= { ltmFastHttpProfileStatEntry 21 } 

ltmFastHttpProfileStatClientRxBad OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of bad TCP segments dropped from client-side."
	::= { ltmFastHttpProfileStatEntry 22 } 

ltmFastHttpProfileStatServerRxBad OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of bad TCP segments dropped from server-side."
	::= { ltmFastHttpProfileStatEntry 23 } 

ltmFastHttpProfileStatPipelinedReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of pipelined HTTP requests detected."
	::= { ltmFastHttpProfileStatEntry 24 } 

--==================================================================
-- Profile_xml
--==================================================================
ltmXmlProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmXmlProfile entries in the table."
	::= { ltmXmlProfile 1 } 

ltmXmlProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmXmlProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of XML profile."
	::= { ltmXmlProfile 2 } 

ltmXmlProfileEntry OBJECT-TYPE
	SYNTAX  LtmXmlProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmXmlProfile Table"
	INDEX {
		ltmXmlProfileName
	}
	::= { ltmXmlProfileTable 1 } 

LtmXmlProfileEntry ::= 
	SEQUENCE {
        	ltmXmlProfileName                                      LongDisplayString,
        	ltmXmlProfileConfigSource                              INTEGER,
        	ltmXmlProfileDefaultName                               LongDisplayString,
        	ltmXmlProfileAbortOnError                              INTEGER,
        	ltmXmlProfileMaxBufferSize                             Integer32
	}

ltmXmlProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a XML profile."
	::= { ltmXmlProfileEntry 1 } 

ltmXmlProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmXmlProfileEntry 2 } 

ltmXmlProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmXmlProfileEntry 3 } 

ltmXmlProfileAbortOnError OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! The state that if true, abort the connection on errors."
	::= { ltmXmlProfileEntry 4 } 

ltmXmlProfileMaxBufferSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! The value that specifies the maximum buffer size for the specified profile."
	::= { ltmXmlProfileEntry 5 } 

--==================================================================
-- Profile_xml_stat
--==================================================================
ltmXmlProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmXmlProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmXmlProfileStat 1 } 

ltmXmlProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmXmlProfileStat entries in the table."
	::= { ltmXmlProfileStat 2 } 

ltmXmlProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmXmlProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of XML profile."
	::= { ltmXmlProfileStat 3 } 

ltmXmlProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmXmlProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmXmlProfileStat Table"
	INDEX {
		ltmXmlProfileStatName
	}
	::= { ltmXmlProfileStatTable 1 } 

LtmXmlProfileStatEntry ::= 
	SEQUENCE {
        	ltmXmlProfileStatName                                  LongDisplayString,
        	ltmXmlProfileStatNumErrors                             Counter64,
        	ltmXmlProfileStatNumInspectedDocuments                 Counter64,
        	ltmXmlProfileStatNumDocumentsWithOneMatch              Counter64,
        	ltmXmlProfileStatNumDocumentsWithTwoMatches            Counter64,
        	ltmXmlProfileStatNumDocumentsWithThreeMatches          Counter64,
        	ltmXmlProfileStatNumDocumentsWithNoMatches             Counter64,
        	ltmXmlProfileStatNumMalformedDocuments                 Counter64
	}

ltmXmlProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a XML profile."
	::= { ltmXmlProfileStatEntry 1 } 

ltmXmlProfileStatNumErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! The total number of XML parsing errors."
	::= { ltmXmlProfileStatEntry 2 } 

ltmXmlProfileStatNumInspectedDocuments OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of inspected XML documents."
	::= { ltmXmlProfileStatEntry 3 } 

ltmXmlProfileStatNumDocumentsWithOneMatch OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of XML documents in which one XPath query match was found."
	::= { ltmXmlProfileStatEntry 4 } 

ltmXmlProfileStatNumDocumentsWithTwoMatches OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of XML documents in which two XPath query matches were found."
	::= { ltmXmlProfileStatEntry 5 } 

ltmXmlProfileStatNumDocumentsWithThreeMatches OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of XML documents in which three XPath query matches were found."
	::= { ltmXmlProfileStatEntry 6 } 

ltmXmlProfileStatNumDocumentsWithNoMatches OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of XML documents in which no XPath query matches were found."
	::= { ltmXmlProfileStatEntry 7 } 

ltmXmlProfileStatNumMalformedDocuments OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of malformed XML documents."
	::= { ltmXmlProfileStatEntry 8 } 

--==================================================================
-- Profile_http_ramcache_uri_excludes
--==================================================================
ltmRamUriExclNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileRamUriExcl entries in the table."
	::= { ltmHttpProfileRamUriExcl 1 } 

ltmRamUriExclTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRamUriExclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of RAM cached excludes URI's  
		in HTTP profiles."
	::= { ltmHttpProfileRamUriExcl 2 } 

ltmRamUriExclEntry OBJECT-TYPE
	SYNTAX  LtmRamUriExclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRamUriExcl Table"
	INDEX {
		ltmRamUriExclName,
		ltmRamUriExclIndex
	}
	::= { ltmRamUriExclTable 1 } 

LtmRamUriExclEntry ::= 
	SEQUENCE {
        	ltmRamUriExclName                                      LongDisplayString,
        	ltmRamUriExclIndex                                     INTEGER,
        	ltmRamUriExclUri                                       LongDisplayString
	}

ltmRamUriExclName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmRamUriExclEntry 1 } 

ltmRamUriExclIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of RAM cached excludes URI for the specified HTTP profile."
	::= { ltmRamUriExclEntry 2 } 

ltmRamUriExclUri OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The RAM cached excludes URI for the specified profile."
	::= { ltmRamUriExclEntry 3 } 

--==================================================================
-- Profile_http_ramcache_uri_includes
--==================================================================
ltmRamUriInclNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileRamUriIncl entries in the table."
	::= { ltmHttpProfileRamUriIncl 1 } 

ltmRamUriInclTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRamUriInclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of RAM cached includes URI's  
		in HTTP profiles."
	::= { ltmHttpProfileRamUriIncl 2 } 

ltmRamUriInclEntry OBJECT-TYPE
	SYNTAX  LtmRamUriInclEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRamUriIncl Table"
	INDEX {
		ltmRamUriInclName,
		ltmRamUriInclIndex
	}
	::= { ltmRamUriInclTable 1 } 

LtmRamUriInclEntry ::= 
	SEQUENCE {
        	ltmRamUriInclName                                      LongDisplayString,
        	ltmRamUriInclIndex                                     INTEGER,
        	ltmRamUriInclUri                                       LongDisplayString
	}

ltmRamUriInclName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmRamUriInclEntry 1 } 

ltmRamUriInclIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of RAM cached includes URI for the specified HTTP profile."
	::= { ltmRamUriInclEntry 2 } 

ltmRamUriInclUri OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The RAM cached includes URI for the specified profile."
	::= { ltmRamUriInclEntry 3 } 

--==================================================================
-- Profile_http_ramcache_uri_pinned
--==================================================================
ltmRamUriPinNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileRamUriPin entries in the table."
	::= { ltmHttpProfileRamUriPin 1 } 

ltmRamUriPinTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRamUriPinEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of RAM cached URI's pinned
		in HTTP profiles."
	::= { ltmHttpProfileRamUriPin 2 } 

ltmRamUriPinEntry OBJECT-TYPE
	SYNTAX  LtmRamUriPinEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRamUriPin Table"
	INDEX {
		ltmRamUriPinName,
		ltmRamUriPinIndex
	}
	::= { ltmRamUriPinTable 1 } 

LtmRamUriPinEntry ::= 
	SEQUENCE {
        	ltmRamUriPinName                                       LongDisplayString,
        	ltmRamUriPinIndex                                      INTEGER,
        	ltmRamUriPinUri                                        LongDisplayString
	}

ltmRamUriPinName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmRamUriPinEntry 1 } 

ltmRamUriPinIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of RAM cached URI pinned for the specified HTTP profile."
	::= { ltmRamUriPinEntry 2 } 

ltmRamUriPinUri OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The RAM cached URI pinned for the specified profile."
	::= { ltmRamUriPinEntry 3 } 

--==================================================================
-- Profile_dns
--==================================================================
ltmDnsProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmDnsProfile entries in the table."
	::= { ltmDnsProfile 1 } 

ltmDnsProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmDnsProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of DNS profile."
	::= { ltmDnsProfile 2 } 

ltmDnsProfileEntry OBJECT-TYPE
	SYNTAX  LtmDnsProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmDnsProfile Table"
	INDEX {
		ltmDnsProfileName
	}
	::= { ltmDnsProfileTable 1 } 

LtmDnsProfileEntry ::= 
	SEQUENCE {
        	ltmDnsProfileName                                      LongDisplayString,
        	ltmDnsProfileConfigSource                              INTEGER,
        	ltmDnsProfileDefaultName                               LongDisplayString,
        	ltmDnsProfileGtmEnabled                                INTEGER
	}

ltmDnsProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a IIOP profile."
	::= { ltmDnsProfileEntry 1 } 

ltmDnsProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmDnsProfileEntry 2 } 

ltmDnsProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives
		its attribute default values."
	::= { ltmDnsProfileEntry 3 } 

ltmDnsProfileGtmEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not to allow GTMD (Global Traffic Management
		Daemon) to handle DNS resolution for DNS queries and responses that contain
		wide IP names."
	::= { ltmDnsProfileEntry 4 } 

--==================================================================
-- Profile_httpclass
--==================================================================
ltmHttpClassNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpClassProfile entries in the table."
	::= { ltmHttpClassProfile 1 } 

ltmHttpClassTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpClassEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of HTTP class profile."
	::= { ltmHttpClassProfile 2 } 

ltmHttpClassEntry OBJECT-TYPE
	SYNTAX  LtmHttpClassEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpClass Table"
	INDEX {
		ltmHttpClassName
	}
	::= { ltmHttpClassTable 1 } 

LtmHttpClassEntry ::= 
	SEQUENCE {
        	ltmHttpClassName                                       LongDisplayString,
        	ltmHttpClassConfigSource                               INTEGER,
        	ltmHttpClassDefaultName                                LongDisplayString,
        	ltmHttpClassPoolName                                   LongDisplayString,
        	ltmHttpClassAsmEnabled                                 INTEGER,
        	ltmHttpClassWaEnabled                                  INTEGER,
        	ltmHttpClassRedirectLocation                           LongDisplayString,
        	ltmHttpClassUrlRewrite                                 LongDisplayString
	}

ltmHttpClassName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP class profile."
	::= { ltmHttpClassEntry 1 } 

ltmHttpClassConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmHttpClassEntry 2 } 

ltmHttpClassDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmHttpClassEntry 3 } 

ltmHttpClassPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The pool name which will be used when the specified class matches."
	::= { ltmHttpClassEntry 4 } 

ltmHttpClassAsmEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether this is an Application Security Module class or not."
	::= { ltmHttpClassEntry 5 } 

ltmHttpClassWaEnabled OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether this is a Web Accelerator class or not."
	::= { ltmHttpClassEntry 6 } 

ltmHttpClassRedirectLocation OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The string (which may include a TCL expression) to indicate where to 
		redirect the original HTTP request once a match occurs."
	::= { ltmHttpClassEntry 7 } 

ltmHttpClassUrlRewrite OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The string (which may include a TCL expression) with which to rewrite 
		the URLs."
	::= { ltmHttpClassEntry 8 } 

--==================================================================
-- Profile_httpclass_match_host
--==================================================================
ltmHttpClassHostNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpClassProfileHost entries in the table."
	::= { ltmHttpClassProfileHost 1 } 

ltmHttpClassHostTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpClassHostEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of host match patterns in HTTP class profiles."
	::= { ltmHttpClassProfileHost 2 } 

ltmHttpClassHostEntry OBJECT-TYPE
	SYNTAX  LtmHttpClassHostEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpClassHost Table"
	INDEX {
		ltmHttpClassHostName,
		ltmHttpClassHostIndex
	}
	::= { ltmHttpClassHostTable 1 } 

LtmHttpClassHostEntry ::= 
	SEQUENCE {
        	ltmHttpClassHostName                                   LongDisplayString,
        	ltmHttpClassHostIndex                                  INTEGER,
        	ltmHttpClassHostString                                 LongDisplayString
	}

ltmHttpClassHostName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP class profile."
	::= { ltmHttpClassHostEntry 1 } 

ltmHttpClassHostIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of host match patterns for the specified HTTP class profile."
	::= { ltmHttpClassHostEntry 2 } 

ltmHttpClassHostString OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The host match pattern for the specified profile."
	::= { ltmHttpClassHostEntry 3 } 

--==================================================================
-- Profile_httpclass_match_path
--==================================================================
ltmHttpClassUriNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpClassProfileUri entries in the table."
	::= { ltmHttpClassProfileUri 1 } 

ltmHttpClassUriTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpClassUriEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of URI match patterns in HTTP class profiles."
	::= { ltmHttpClassProfileUri 2 } 

ltmHttpClassUriEntry OBJECT-TYPE
	SYNTAX  LtmHttpClassUriEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpClassUri Table"
	INDEX {
		ltmHttpClassUriName,
		ltmHttpClassUriIndex
	}
	::= { ltmHttpClassUriTable 1 } 

LtmHttpClassUriEntry ::= 
	SEQUENCE {
        	ltmHttpClassUriName                                    LongDisplayString,
        	ltmHttpClassUriIndex                                   INTEGER,
        	ltmHttpClassUriString                                  LongDisplayString
	}

ltmHttpClassUriName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP class profile."
	::= { ltmHttpClassUriEntry 1 } 

ltmHttpClassUriIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of URI match patterns for the specified HTTP class profile."
	::= { ltmHttpClassUriEntry 2 } 

ltmHttpClassUriString OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The URI match pattern for the specified profile."
	::= { ltmHttpClassUriEntry 3 } 

--==================================================================
-- Profile_httpclass_match_header
--==================================================================
ltmHttpClassHeadNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpClassProfileHead entries in the table."
	::= { ltmHttpClassProfileHead 1 } 

ltmHttpClassHeadTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpClassHeadEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of HTTP request header match patterns in HTTP class profiles."
	::= { ltmHttpClassProfileHead 2 } 

ltmHttpClassHeadEntry OBJECT-TYPE
	SYNTAX  LtmHttpClassHeadEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpClassHead Table"
	INDEX {
		ltmHttpClassHeadName,
		ltmHttpClassHeadIndex
	}
	::= { ltmHttpClassHeadTable 1 } 

LtmHttpClassHeadEntry ::= 
	SEQUENCE {
        	ltmHttpClassHeadName                                   LongDisplayString,
        	ltmHttpClassHeadIndex                                  INTEGER,
        	ltmHttpClassHeadString                                 LongDisplayString
	}

ltmHttpClassHeadName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP class profile."
	::= { ltmHttpClassHeadEntry 1 } 

ltmHttpClassHeadIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of HTTP request header match patterns for the specified HTTP class profile."
	::= { ltmHttpClassHeadEntry 2 } 

ltmHttpClassHeadString OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The HTTP request header match pattern for the specified profile."
	::= { ltmHttpClassHeadEntry 3 } 

--==================================================================
-- Profile_httpclass_match_cookies
--==================================================================
ltmHttpClassCookNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpClassProfileCook entries in the table."
	::= { ltmHttpClassProfileCook 1 } 

ltmHttpClassCookTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpClassCookEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of HTTP cookie match patterns in HTTP class profiles."
	::= { ltmHttpClassProfileCook 2 } 

ltmHttpClassCookEntry OBJECT-TYPE
	SYNTAX  LtmHttpClassCookEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpClassCook Table"
	INDEX {
		ltmHttpClassCookName,
		ltmHttpClassCookIndex
	}
	::= { ltmHttpClassCookTable 1 } 

LtmHttpClassCookEntry ::= 
	SEQUENCE {
        	ltmHttpClassCookName                                   LongDisplayString,
        	ltmHttpClassCookIndex                                  INTEGER,
        	ltmHttpClassCookString                                 LongDisplayString
	}

ltmHttpClassCookName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP class profile."
	::= { ltmHttpClassCookEntry 1 } 

ltmHttpClassCookIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of HTTP cookie match patterns for the specified HTTP class profile."
	::= { ltmHttpClassCookEntry 2 } 

ltmHttpClassCookString OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The HTTP cookie match pattern for the specified profile."
	::= { ltmHttpClassCookEntry 3 } 

--==================================================================
-- Profile_httpclass_stat
--==================================================================
ltmHttpClassStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmHttpClassProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmHttpClassProfileStat 1 } 

ltmHttpClassStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpClassProfileStat entries in the table."
	::= { ltmHttpClassProfileStat 2 } 

ltmHttpClassStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmHttpClassStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistics information of HTTP class profile."
	::= { ltmHttpClassProfileStat 3 } 

ltmHttpClassStatEntry OBJECT-TYPE
	SYNTAX  LtmHttpClassStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmHttpClassStat Table"
	INDEX {
		ltmHttpClassStatName
	}
	::= { ltmHttpClassStatTable 1 } 

LtmHttpClassStatEntry ::= 
	SEQUENCE {
        	ltmHttpClassStatName                                   LongDisplayString,
        	ltmHttpClassStatCookiePersistInserts                   Counter64,
        	ltmHttpClassStatResp2xxCnt                             Counter64,
        	ltmHttpClassStatResp3xxCnt                             Counter64,
        	ltmHttpClassStatResp4xxCnt                             Counter64,
        	ltmHttpClassStatResp5xxCnt                             Counter64,
        	ltmHttpClassStatNumberReqs                             Counter64,
        	ltmHttpClassStatGetReqs                                Counter64,
        	ltmHttpClassStatPostReqs                               Counter64,
        	ltmHttpClassStatV9Reqs                                 Counter64,
        	ltmHttpClassStatV10Reqs                                Counter64,
        	ltmHttpClassStatV11Reqs                                Counter64,
        	ltmHttpClassStatV9Resp                                 Counter64,
        	ltmHttpClassStatV10Resp                                Counter64,
        	ltmHttpClassStatV11Resp                                Counter64,
        	ltmHttpClassStatMaxKeepaliveReq                        Counter64,
        	ltmHttpClassStatRespBucket1k                           Counter64,
        	ltmHttpClassStatRespBucket4k                           Counter64,
        	ltmHttpClassStatRespBucket16k                          Counter64,
        	ltmHttpClassStatRespBucket32k                          Counter64,
        	ltmHttpClassStatRespBucket64k                          Counter64,
        	ltmHttpClassStatPrecompressBytes                       Counter64,
        	ltmHttpClassStatPostcompressBytes                      Counter64,
        	ltmHttpClassStatNullCompressBytes                      Counter64,
        	ltmHttpClassStatHtmlPrecompressBytes                   Counter64,
        	ltmHttpClassStatHtmlPostcompressBytes                  Counter64,
        	ltmHttpClassStatCssPrecompressBytes                    Counter64,
        	ltmHttpClassStatCssPostcompressBytes                   Counter64,
        	ltmHttpClassStatJsPrecompressBytes                     Counter64,
        	ltmHttpClassStatJsPostcompressBytes                    Counter64,
        	ltmHttpClassStatXmlPrecompressBytes                    Counter64,
        	ltmHttpClassStatXmlPostcompressBytes                   Counter64,
        	ltmHttpClassStatSgmlPrecompressBytes                   Counter64,
        	ltmHttpClassStatSgmlPostcompressBytes                  Counter64,
        	ltmHttpClassStatPlainPrecompressBytes                  Counter64,
        	ltmHttpClassStatPlainPostcompressBytes                 Counter64,
        	ltmHttpClassStatOctetPrecompressBytes                  Counter64,
        	ltmHttpClassStatOctetPostcompressBytes                 Counter64,
        	ltmHttpClassStatImagePrecompressBytes                  Counter64,
        	ltmHttpClassStatImagePostcompressBytes                 Counter64,
        	ltmHttpClassStatVideoPrecompressBytes                  Counter64,
        	ltmHttpClassStatVideoPostcompressBytes                 Counter64,
        	ltmHttpClassStatAudioPrecompressBytes                  Counter64,
        	ltmHttpClassStatAudioPostcompressBytes                 Counter64,
        	ltmHttpClassStatOtherPrecompressBytes                  Counter64,
        	ltmHttpClassStatOtherPostcompressBytes                 Counter64,
        	ltmHttpClassStatRamcacheHits                           Counter64,
        	ltmHttpClassStatRamcacheMisses                         Counter64,
        	ltmHttpClassStatRamcacheMissesAll                      Counter64,
        	ltmHttpClassStatRamcacheHitBytes                       Counter64,
        	ltmHttpClassStatRamcacheMissBytes                      Counter64,
        	ltmHttpClassStatRamcacheMissBytesAll                   Counter64
	}

ltmHttpClassStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP class profile."
	::= { ltmHttpClassStatEntry 1 } 

ltmHttpClassStatCookiePersistInserts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of successful attempts to insert HTTP headers 
		 for cookie persistence (set-cookie header insertions)."
	::= { ltmHttpClassStatEntry 2 } 

ltmHttpClassStatResp2xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 200 to 206 
		 (successful responses)"
	::= { ltmHttpClassStatEntry 3 } 

ltmHttpClassStatResp3xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 300 to 307 
		 (redirection responses)."
	::= { ltmHttpClassStatEntry 4 } 

ltmHttpClassStatResp4xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 400 to 417  
		 (client errors)."
	::= { ltmHttpClassStatEntry 5 } 

ltmHttpClassStatResp5xxCnt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of server-side responses in range of 500 to 505 
		 (server errors)."
	::= { ltmHttpClassStatEntry 6 } 

ltmHttpClassStatNumberReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of HTTP requests."
	::= { ltmHttpClassStatEntry 7 } 

ltmHttpClassStatGetReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of HTTP get requests."
	::= { ltmHttpClassStatEntry 8 } 

ltmHttpClassStatPostReqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of HTTP post requests."
	::= { ltmHttpClassStatEntry 9 } 

ltmHttpClassStatV9Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 9 requests."
	::= { ltmHttpClassStatEntry 10 } 

ltmHttpClassStatV10Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 10 requests."
	::= { ltmHttpClassStatEntry 11 } 

ltmHttpClassStatV11Reqs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 11 requests."
	::= { ltmHttpClassStatEntry 12 } 

ltmHttpClassStatV9Resp OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 9 responses."
	::= { ltmHttpClassStatEntry 13 } 

ltmHttpClassStatV10Resp OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 10 responses."
	::= { ltmHttpClassStatEntry 14 } 

ltmHttpClassStatV11Resp OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of version 11 responses."
	::= { ltmHttpClassStatEntry 15 } 

ltmHttpClassStatMaxKeepaliveReq OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of requests made in a connection."
	::= { ltmHttpClassStatEntry 16 } 

ltmHttpClassStatRespBucket1k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses under 1k."
	::= { ltmHttpClassStatEntry 17 } 

ltmHttpClassStatRespBucket4k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses between 1 - 4k."
	::= { ltmHttpClassStatEntry 18 } 

ltmHttpClassStatRespBucket16k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses between 4 - 16k."
	::= { ltmHttpClassStatEntry 19 } 

ltmHttpClassStatRespBucket32k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of responses between 16 - 32k."
	::= { ltmHttpClassStatEntry 20 } 

ltmHttpClassStatRespBucket64k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! Please use larger buckets"
	::= { ltmHttpClassStatEntry 21 } 

ltmHttpClassStatPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of response bytes before compression has taken place."
	::= { ltmHttpClassStatEntry 22 } 

ltmHttpClassStatPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of response bytes after compression has taken place."
	::= { ltmHttpClassStatEntry 23 } 

ltmHttpClassStatNullCompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bytes subjected to NULL compression (for license enforcement)."
	::= { ltmHttpClassStatEntry 24 } 

ltmHttpClassStatHtmlPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: HTML."
	::= { ltmHttpClassStatEntry 25 } 

ltmHttpClassStatHtmlPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: HTML."
	::= { ltmHttpClassStatEntry 26 } 

ltmHttpClassStatCssPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: CSS."
	::= { ltmHttpClassStatEntry 27 } 

ltmHttpClassStatCssPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: CSS."
	::= { ltmHttpClassStatEntry 28 } 

ltmHttpClassStatJsPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Javascript."
	::= { ltmHttpClassStatEntry 29 } 

ltmHttpClassStatJsPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Javascript."
	::= { ltmHttpClassStatEntry 30 } 

ltmHttpClassStatXmlPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: XML."
	::= { ltmHttpClassStatEntry 31 } 

ltmHttpClassStatXmlPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: XML."
	::= { ltmHttpClassStatEntry 32 } 

ltmHttpClassStatSgmlPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: SGML."
	::= { ltmHttpClassStatEntry 33 } 

ltmHttpClassStatSgmlPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: SGML."
	::= { ltmHttpClassStatEntry 34 } 

ltmHttpClassStatPlainPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Plain."
	::= { ltmHttpClassStatEntry 35 } 

ltmHttpClassStatPlainPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Plain."
	::= { ltmHttpClassStatEntry 36 } 

ltmHttpClassStatOctetPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Octet stream."
	::= { ltmHttpClassStatEntry 37 } 

ltmHttpClassStatOctetPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Octet stream."
	::= { ltmHttpClassStatEntry 38 } 

ltmHttpClassStatImagePrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Images."
	::= { ltmHttpClassStatEntry 39 } 

ltmHttpClassStatImagePostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Images."
	::= { ltmHttpClassStatEntry 40 } 

ltmHttpClassStatVideoPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Video files."
	::= { ltmHttpClassStatEntry 41 } 

ltmHttpClassStatVideoPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Video files."
	::= { ltmHttpClassStatEntry 42 } 

ltmHttpClassStatAudioPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: Audio files."
	::= { ltmHttpClassStatEntry 43 } 

ltmHttpClassStatAudioPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: Audio files."
	::= { ltmHttpClassStatEntry 44 } 

ltmHttpClassStatOtherPrecompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of pre-compressed bytes for the MIME-Types: other than 
		HTML, CSS, Javascript, XML, SGML, Plain, Images, Video files, 
		Audio files."
	::= { ltmHttpClassStatEntry 45 } 

ltmHttpClassStatOtherPostcompressBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of post-compressed bytes for the MIME-Types: other than 
		HTML, CSS, Javascript, XML, SGML, Plain, Images, Video files, 
		Audio files."
	::= { ltmHttpClassStatEntry 46 } 

ltmHttpClassStatRamcacheHits OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache hits."
	::= { ltmHttpClassStatEntry 47 } 

ltmHttpClassStatRamcacheMisses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache misses, excluding un-cacheable data."
	::= { ltmHttpClassStatEntry 48 } 

ltmHttpClassStatRamcacheMissesAll OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of RAM cache misses."
	::= { ltmHttpClassStatEntry 49 } 

ltmHttpClassStatRamcacheHitBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache hits in bytes."
	::= { ltmHttpClassStatEntry 50 } 

ltmHttpClassStatRamcacheMissBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of RAM cache misses in bytes, excluding un-cacheable data."
	::= { ltmHttpClassStatEntry 51 } 

ltmHttpClassStatRamcacheMissBytesAll OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of RAM cache misses in bytes."
	::= { ltmHttpClassStatEntry 52 } 

--==================================================================
-- Profile_iiop
--==================================================================
ltmIiopProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmIiopProfile entries in the table."
	::= { ltmIiopProfile 1 } 

ltmIiopProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmIiopProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of IIOP profile."
	::= { ltmIiopProfile 2 } 

ltmIiopProfileEntry OBJECT-TYPE
	SYNTAX  LtmIiopProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmIiopProfile Table"
	INDEX {
		ltmIiopProfileName
	}
	::= { ltmIiopProfileTable 1 } 

LtmIiopProfileEntry ::= 
	SEQUENCE {
        	ltmIiopProfileName                                     LongDisplayString,
        	ltmIiopProfileConfigSource                             INTEGER,
        	ltmIiopProfileDefaultName                              LongDisplayString,
        	ltmIiopProfilePersistRequestId                         INTEGER,
        	ltmIiopProfilePersistObjectKey                         INTEGER,
        	ltmIiopProfileAbortOnTimeout                           INTEGER,
        	ltmIiopProfileTimeout                                  Integer32
	}

ltmIiopProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a IIOP profile."
	::= { ltmIiopProfileEntry 1 } 

ltmIiopProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmIiopProfileEntry 2 } 

ltmIiopProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives
	        its attribute default values."
	::= { ltmIiopProfileEntry 3 } 

ltmIiopProfilePersistRequestId OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, persist the request ID."
	::= { ltmIiopProfileEntry 4 } 

ltmIiopProfilePersistObjectKey OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, persist the object key."
	::= { ltmIiopProfileEntry 5 } 

ltmIiopProfileAbortOnTimeout OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that if true, abort the connection when response is
	        timed out."
	::= { ltmIiopProfileEntry 6 } 

ltmIiopProfileTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The response timeout for the specified IIOP profile."
	::= { ltmIiopProfileEntry 7 } 

--==================================================================
-- Profile_iiop_stat
--==================================================================
ltmIiopProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmIiopProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmIiopProfileStat 1 } 

ltmIiopProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmIiopProfileStat entries in the table."
	::= { ltmIiopProfileStat 2 } 

ltmIiopProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmIiopProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of IIOP profile."
	::= { ltmIiopProfileStat 3 } 

ltmIiopProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmIiopProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmIiopProfileStat Table"
	INDEX {
		ltmIiopProfileStatName
	}
	::= { ltmIiopProfileStatTable 1 } 

LtmIiopProfileStatEntry ::= 
	SEQUENCE {
        	ltmIiopProfileStatName                                 LongDisplayString,
        	ltmIiopProfileStatNumRequests                          Counter64,
        	ltmIiopProfileStatNumResponses                         Counter64,
        	ltmIiopProfileStatNumCancels                           Counter64,
        	ltmIiopProfileStatNumErrors                            Counter64,
        	ltmIiopProfileStatNumFragments                         Counter64
	}

ltmIiopProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a IIOP profile."
	::= { ltmIiopProfileStatEntry 1 } 

ltmIiopProfileStatNumRequests OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of IIOP requests."
	::= { ltmIiopProfileStatEntry 2 } 

ltmIiopProfileStatNumResponses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of IIOP responses."
	::= { ltmIiopProfileStatEntry 3 } 

ltmIiopProfileStatNumCancels OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of IIOP cancel messages."
	::= { ltmIiopProfileStatEntry 4 } 

ltmIiopProfileStatNumErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of IIOP error messages."
	::= { ltmIiopProfileStatEntry 5 } 

ltmIiopProfileStatNumFragments OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of IIOP fragments."
	::= { ltmIiopProfileStatEntry 6 } 

--==================================================================
-- Profile_rtsp
--==================================================================
ltmRtspProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmRtspProfile entries in the table."
	::= { ltmRtspProfile 1 } 

ltmRtspProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRtspProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of RTSP profile."
	::= { ltmRtspProfile 2 } 

ltmRtspProfileEntry OBJECT-TYPE
	SYNTAX  LtmRtspProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRtspProfile Table"
	INDEX {
		ltmRtspProfileName
	}
	::= { ltmRtspProfileTable 1 } 

LtmRtspProfileEntry ::= 
	SEQUENCE {
        	ltmRtspProfileName                                     LongDisplayString,
        	ltmRtspProfileConfigSource                             INTEGER,
        	ltmRtspProfileDefaultName                              LongDisplayString,
        	ltmRtspProfileIdleTimeout                              Integer32,
        	ltmRtspProfileMaxHeaderSize                            Integer32,
        	ltmRtspProfileMaxQueuedData                            Integer32,
        	ltmRtspProfileUnicastRedirect                          INTEGER,
        	ltmRtspProfileMulticastRedirect                        INTEGER,
        	ltmRtspProfileSessionReconnect                         INTEGER,
        	ltmRtspProfileRealHttpPersistence                      INTEGER,
        	ltmRtspProfileProxy                                    INTEGER,
        	ltmRtspProfileProxyHeader                              LongDisplayString,
        	ltmRtspProfileRtpPort                                  INTEGER,
        	ltmRtspProfileRtcpPort                                 INTEGER
	}

ltmRtspProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a RTSP profile."
	::= { ltmRtspProfileEntry 1 } 

ltmRtspProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmRtspProfileEntry 2 } 

ltmRtspProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives
	        its attribute default values."
	::= { ltmRtspProfileEntry 3 } 

ltmRtspProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The idle timeout (in seconds) for the specified RTSP profile."
	::= { ltmRtspProfileEntry 4 } 

ltmRtspProfileMaxHeaderSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum header size in bytes for the specified RTSP profile."
	::= { ltmRtspProfileEntry 5 } 

ltmRtspProfileMaxQueuedData OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum queued data in bytes for the specified RTSP profile."
	::= { ltmRtspProfileEntry 6 } 

ltmRtspProfileUnicastRedirect OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether unicast redirect is enable or not
		for the specified RTSP profile."
	::= { ltmRtspProfileEntry 7 } 

ltmRtspProfileMulticastRedirect OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether multicast redirect is enable or not
		for the specified RTSP profile."
	::= { ltmRtspProfileEntry 8 } 

ltmRtspProfileSessionReconnect OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether session reconnecting is enable or not
		for the specified RTSP profile."
	::= { ltmRtspProfileEntry 9 } 

ltmRtspProfileRealHttpPersistence OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether real HTTP persistence is enable or not
		for the specified RTSP profile."
	::= { ltmRtspProfileEntry 10 } 

ltmRtspProfileProxy OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		external(1),
		internal(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The proxy state for the specified RTSP profile."
	::= { ltmRtspProfileEntry 11 } 

ltmRtspProfileProxyHeader OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The proxy header for the specified RTSP profile."
	::= { ltmRtspProfileEntry 12 } 

ltmRtspProfileRtpPort OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The RTP port for the specified RTSP profile."
	::= { ltmRtspProfileEntry 13 } 

ltmRtspProfileRtcpPort OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The RTCP port for the specified RTSP profile."
	::= { ltmRtspProfileEntry 14 } 

--==================================================================
-- Profile_rtsp_stat
--==================================================================
ltmRtspProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmRtspProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmRtspProfileStat 1 } 

ltmRtspProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmRtspProfileStat entries in the table."
	::= { ltmRtspProfileStat 2 } 

ltmRtspProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRtspProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of RTSP profile."
	::= { ltmRtspProfileStat 3 } 

ltmRtspProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmRtspProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRtspProfileStat Table"
	INDEX {
		ltmRtspProfileStatName
	}
	::= { ltmRtspProfileStatTable 1 } 

LtmRtspProfileStatEntry ::= 
	SEQUENCE {
        	ltmRtspProfileStatName                                 LongDisplayString,
        	ltmRtspProfileStatNumRequests                          Counter64,
        	ltmRtspProfileStatNumResponses                         Counter64,
        	ltmRtspProfileStatNumErrors                            Counter64,
        	ltmRtspProfileStatNumInterleaved                       Counter64
	}

ltmRtspProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a RTSP profile."
	::= { ltmRtspProfileStatEntry 1 } 

ltmRtspProfileStatNumRequests OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of RTSP requests for the specified RTSP profile."
	::= { ltmRtspProfileStatEntry 2 } 

ltmRtspProfileStatNumResponses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of RTSP responses for the specified RTSP profile."
	::= { ltmRtspProfileStatEntry 3 } 

ltmRtspProfileStatNumErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of RTSP errors for the specified RTSP profile."
	::= { ltmRtspProfileStatEntry 4 } 

ltmRtspProfileStatNumInterleaved OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of interleaved RTSP data packets for the specified RTSP profile."
	::= { ltmRtspProfileStatEntry 5 } 

--==================================================================
-- Profile_sctp
--==================================================================
ltmSctpProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSctpProfile entries in the table."
	::= { ltmSctpProfile 1 } 

ltmSctpProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSctpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of SCTP profile."
	::= { ltmSctpProfile 2 } 

ltmSctpProfileEntry OBJECT-TYPE
	SYNTAX  LtmSctpProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSctpProfile Table"
	INDEX {
		ltmSctpProfileName
	}
	::= { ltmSctpProfileTable 1 } 

LtmSctpProfileEntry ::= 
	SEQUENCE {
        	ltmSctpProfileName                                     LongDisplayString,
        	ltmSctpProfileConfigSource                             INTEGER,
        	ltmSctpProfileDefaultName                              LongDisplayString,
        	ltmSctpProfileRcvOrdered                               INTEGER,
        	ltmSctpProfileSndPartial                               INTEGER,
        	ltmSctpProfileTcpShutdown                              INTEGER,
        	ltmSctpProfileResetOnTimeout                           INTEGER,
        	ltmSctpProfileOutStreams                               Integer32,
        	ltmSctpProfileInStreams                                Integer32,
        	ltmSctpProfileSndbuf                                   Integer32,
        	ltmSctpProfileRcvwnd                                   Integer32,
        	ltmSctpProfileTxChunks                                 Integer32,
        	ltmSctpProfileRxChunks                                 Integer32,
        	ltmSctpProfileCookieExpiration                         Integer32,
        	ltmSctpProfileInitMaxrtx                               Integer32,
        	ltmSctpProfileAssocMaxrtx                              Integer32,
        	ltmSctpProfileProxyBufferLow                           Integer32,
        	ltmSctpProfileProxyBufferHigh                          Integer32,
        	ltmSctpProfileIdleTimeout                              Integer32,
        	ltmSctpProfileHeartbeatInterval                        Integer32,
        	ltmSctpProfileIpTosToPeer                              INTEGER,
        	ltmSctpProfileLinkQosToPeer                            INTEGER,
        	ltmSctpProfileSecret                                   LongDisplayString
	}

ltmSctpProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SCTP profile."
	::= { ltmSctpProfileEntry 1 } 

ltmSctpProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmSctpProfileEntry 2 } 

ltmSctpProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives
	        its attribute default values."
	::= { ltmSctpProfileEntry 3 } 

ltmSctpProfileRcvOrdered OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not to in-order deliver messages to upper layer 
		for the specified profile."
	::= { ltmSctpProfileEntry 4 } 

ltmSctpProfileSndPartial OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not to accept partial of application data
		for the specified profile."
	::= { ltmSctpProfileEntry 5 } 

ltmSctpProfileTcpShutdown OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not to emulate TCP closing
		for the specified profile."
	::= { ltmSctpProfileEntry 6 } 

ltmSctpProfileResetOnTimeout OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not reset connection when timeout
		for the specified profile."
	::= { ltmSctpProfileEntry 7 } 

ltmSctpProfileOutStreams OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of out-bound streams for the specified profile."
	::= { ltmSctpProfileEntry 8 } 

ltmSctpProfileInStreams OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of in-bound streams for the specified profile."
	::= { ltmSctpProfileEntry 9 } 

ltmSctpProfileSndbuf OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The send buffer size in bytes for the specified profile."
	::= { ltmSctpProfileEntry 10 } 

ltmSctpProfileRcvwnd OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The received window size, should be prorated to ltmSctpProfileRxChuncks 
		for the specified profile."
	::= { ltmSctpProfileEntry 11 } 

ltmSctpProfileTxChunks OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of sending chunk buffer for the specified profile."
	::= { ltmSctpProfileEntry 12 } 

ltmSctpProfileRxChunks OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of receiving chunk buffer for the specified profile."
	::= { ltmSctpProfileEntry 13 } 

ltmSctpProfileCookieExpiration OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The valid duration of cookie for the specified profile."
	::= { ltmSctpProfileEntry 14 } 

ltmSctpProfileInitMaxrtx OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of retries to establish a connection for the specified profile."
	::= { ltmSctpProfileEntry 15 } 

ltmSctpProfileAssocMaxrtx OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of retries to send data for the specified profile."
	::= { ltmSctpProfileEntry 16 } 

ltmSctpProfileProxyBufferLow OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The proxy buffer level at which the receive window is opened 
		for the specified profile."
	::= { ltmSctpProfileEntry 17 } 

ltmSctpProfileProxyBufferHigh OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The proxy buffer level at which the receive window is closed 
		for the specified profile."
	::= { ltmSctpProfileEntry 18 } 

ltmSctpProfileIdleTimeout OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds without traffic before a connection is eligible 
		for deletion for the specified profile."
	::= { ltmSctpProfileEntry 19 } 

ltmSctpProfileHeartbeatInterval OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of seconds to send heartbeat for the specified profile."
	::= { ltmSctpProfileEntry 20 } 

ltmSctpProfileIpTosToPeer OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP type of service set in packets sent to peer for the specified profile."
	::= { ltmSctpProfileEntry 21 } 

ltmSctpProfileLinkQosToPeer OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The link quality of service set in packets sent to peer for the specified profile."
	::= { ltmSctpProfileEntry 22 } 

ltmSctpProfileSecret OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The internal secret string used to HMAC cookie for the specified profile."
	::= { ltmSctpProfileEntry 23 } 

--==================================================================
-- Profile_sctp_stat
--==================================================================
ltmSctpProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmSctpProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmSctpProfileStat 1 } 

ltmSctpProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSctpProfileStat entries in the table."
	::= { ltmSctpProfileStat 2 } 

ltmSctpProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSctpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistic information of SCTP profile."
	::= { ltmSctpProfileStat 3 } 

ltmSctpProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmSctpProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSctpProfileStat Table"
	INDEX {
		ltmSctpProfileStatName
	}
	::= { ltmSctpProfileStatTable 1 } 

LtmSctpProfileStatEntry ::= 
	SEQUENCE {
        	ltmSctpProfileStatName                                 LongDisplayString,
        	ltmSctpProfileStatAccepts                              Counter64,
        	ltmSctpProfileStatAcceptfails                          Counter64,
        	ltmSctpProfileStatConnects                             Counter64,
        	ltmSctpProfileStatConnfails                            Counter64,
        	ltmSctpProfileStatExpires                              Counter64,
        	ltmSctpProfileStatAbandons                             Counter64,
        	ltmSctpProfileStatRxrst                                Counter64,
        	ltmSctpProfileStatRxbadsum                             Counter64,
        	ltmSctpProfileStatRxcookie                             Counter64,
        	ltmSctpProfileStatRxbadcookie                          Counter64
	}

ltmSctpProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SCTP profile."
	::= { ltmSctpProfileStatEntry 1 } 

ltmSctpProfileStatAccepts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of accepted connections for the specified profile."
	::= { ltmSctpProfileStatEntry 2 } 

ltmSctpProfileStatAcceptfails OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of not accepted responses for the specified profile."
	::= { ltmSctpProfileStatEntry 3 } 

ltmSctpProfileStatConnects OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of established connections for the specified profile."
	::= { ltmSctpProfileStatEntry 4 } 

ltmSctpProfileStatConnfails OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of connections failures for the specified profile."
	::= { ltmSctpProfileStatEntry 5 } 

ltmSctpProfileStatExpires OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of expired connections due to idle timeout for the specified profile."
	::= { ltmSctpProfileStatEntry 6 } 

ltmSctpProfileStatAbandons OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of abandoned connections due to retries/keep-alives  for the specified profile."
	::= { ltmSctpProfileStatEntry 7 } 

ltmSctpProfileStatRxrst OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of received Abort chunks for the specified profile."
	::= { ltmSctpProfileStatEntry 8 } 

ltmSctpProfileStatRxbadsum OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of bad checksum in received packets for the specified profile."
	::= { ltmSctpProfileStatEntry 9 } 

ltmSctpProfileStatRxcookie OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of received SCTP cookies (including bad and good ones) for the specified profile."
	::= { ltmSctpProfileStatEntry 10 } 

ltmSctpProfileStatRxbadcookie OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of received bad SCTP cookies for the specified profile."
	::= { ltmSctpProfileStatEntry 11 } 

--==================================================================
-- Profile_statistics
--==================================================================
ltmUserStatProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmUserStatProfile entries in the table."
	::= { ltmUserStatProfile 1 } 

ltmUserStatProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmUserStatProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing basic information of user-defined statistics profiles., 
		The user can define up to 32 statistic fields in each profile. 
		See ltmUserStatProfileStatTable for user-defined fields for each profile."
	::= { ltmUserStatProfile 2 } 

ltmUserStatProfileEntry OBJECT-TYPE
	SYNTAX  LtmUserStatProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmUserStatProfile Table"
	INDEX {
		ltmUserStatProfileName
	}
	::= { ltmUserStatProfileTable 1 } 

LtmUserStatProfileEntry ::= 
	SEQUENCE {
        	ltmUserStatProfileName                                 LongDisplayString,
        	ltmUserStatProfileConfigSource                         INTEGER,
        	ltmUserStatProfileDefaultName                          LongDisplayString
	}

ltmUserStatProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of an user-defined statistics profile."
	::= { ltmUserStatProfileEntry 1 } 

ltmUserStatProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmUserStatProfileEntry 2 } 

ltmUserStatProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmUserStatProfileEntry 3 } 

--==================================================================
-- Profile_user_stat
--==================================================================
ltmUserStatProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmUserStatProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmUserStatProfileStat 1 } 

ltmUserStatProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmUserStatProfileStat entries in the table."
	::= { ltmUserStatProfileStat 2 } 

ltmUserStatProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmUserStatProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing user-defined statistics information for related profiles.
		The maximum for user-defined statistic fields is 32 for each profile."
	::= { ltmUserStatProfileStat 3 } 

ltmUserStatProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmUserStatProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmUserStatProfileStat Table"
	INDEX {
		ltmUserStatProfileStatName,
		ltmUserStatProfileStatFieldId
	}
	::= { ltmUserStatProfileStatTable 1 } 

LtmUserStatProfileStatEntry ::= 
	SEQUENCE {
        	ltmUserStatProfileStatName                             LongDisplayString,
        	ltmUserStatProfileStatFieldId                          INTEGER,
        	ltmUserStatProfileStatFieldName                        LongDisplayString,
        	ltmUserStatProfileStatFieldValue                       Counter64
	}

ltmUserStatProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of an user-defined statistics profile."
	::= { ltmUserStatProfileStatEntry 1 } 

ltmUserStatProfileStatFieldId OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of the user-defined statistics field."
	::= { ltmUserStatProfileStatEntry 2 } 

ltmUserStatProfileStatFieldName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the related user-defined statistic field."
	::= { ltmUserStatProfileStatEntry 3 } 

ltmUserStatProfileStatFieldValue OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The value of the related user-defined statistic field."
	::= { ltmUserStatProfileStatEntry 4 } 

--==================================================================
-- Virtual_server_httpclass
--==================================================================
ltmVsHttpClassNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServHttpClass entries in the table."
	::= { ltmVirtualServHttpClass 1 } 

ltmVsHttpClassTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVsHttpClassEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of HTTP class profiles with which the specified virtual servers associate."
	::= { ltmVirtualServHttpClass 2 } 

ltmVsHttpClassEntry OBJECT-TYPE
	SYNTAX  LtmVsHttpClassEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVsHttpClass Table"
	INDEX {
		ltmVsHttpClassVsName,
		ltmVsHttpClassProfileName
	}
	::= { ltmVsHttpClassTable 1 } 

LtmVsHttpClassEntry ::= 
	SEQUENCE {
        	ltmVsHttpClassVsName                                   LongDisplayString,
        	ltmVsHttpClassProfileName                              LongDisplayString,
        	ltmVsHttpClassPriority                                 Integer32
	}

ltmVsHttpClassVsName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVsHttpClassEntry 1 } 

ltmVsHttpClassProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of HTTP class profile with which the specified virtual server associate."
	::= { ltmVsHttpClassEntry 2 } 

ltmVsHttpClassPriority OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The priority of the profile among profiles used by the specified virtual server."
	::= { ltmVsHttpClassEntry 3 } 

--==================================================================
-- Node_address_status
--==================================================================
ltmNodeAddrStatusNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmNodeAddrStatus entries in the table."
	::= { ltmNodeAddrStatus 1 } 

ltmNodeAddrStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmNodeAddrStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing status information of node addresses."
	::= { ltmNodeAddrStatus 2 } 

ltmNodeAddrStatusEntry OBJECT-TYPE
	SYNTAX  LtmNodeAddrStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmNodeAddrStatus Table"
	INDEX {
		ltmNodeAddrStatusAddrType,
		ltmNodeAddrStatusAddr
	}
	::= { ltmNodeAddrStatusTable 1 } 

LtmNodeAddrStatusEntry ::= 
	SEQUENCE {
        	ltmNodeAddrStatusAddrType                              InetAddressType,
        	ltmNodeAddrStatusAddr                                  InetAddress,
        	ltmNodeAddrStatusAvailState                            INTEGER,
        	ltmNodeAddrStatusEnabledState                          INTEGER,
        	ltmNodeAddrStatusParentType                            Integer32,
        	ltmNodeAddrStatusDetailReason                          LongDisplayString
	}

ltmNodeAddrStatusAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmNodeAddrStatusAddr."
	::= { ltmNodeAddrStatusEntry 1 } 

ltmNodeAddrStatusAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a node. It is interpreted within 
		 the context of a ltmNodeAddrStatusAddrType value."
	::= { ltmNodeAddrStatusEntry 2 } 

ltmNodeAddrStatusAvailState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4),
		gray(5)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The availability of the specified node address indicated in color.
		none - error;
		green - available in some capacity;
		yellow - not currently available;
		red - not available;
		blue - availability is unknown;
		gray - unlicensed."
	::= { ltmNodeAddrStatusEntry 3 } 

ltmNodeAddrStatusEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The activity status of the specified node address, as specified 
		by the user."
	::= { ltmNodeAddrStatusEntry 4 } 

ltmNodeAddrStatusParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! This is an internal data.
		The type of parent object which disabled the specified node address."
	::= { ltmNodeAddrStatusEntry 5 } 

ltmNodeAddrStatusDetailReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The detail description of the specified node's status."
	::= { ltmNodeAddrStatusEntry 6 } 

--==================================================================
-- Pool_status
--==================================================================
ltmPoolStatusNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmPoolStatus entries in the table."
	::= { ltmPoolStatus 1 } 

ltmPoolStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmPoolStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing status information of pools."
	::= { ltmPoolStatus 2 } 

ltmPoolStatusEntry OBJECT-TYPE
	SYNTAX  LtmPoolStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmPoolStatus Table"
	INDEX {
		ltmPoolStatusName
	}
	::= { ltmPoolStatusTable 1 } 

LtmPoolStatusEntry ::= 
	SEQUENCE {
        	ltmPoolStatusName                                      LongDisplayString,
        	ltmPoolStatusAvailState                                INTEGER,
        	ltmPoolStatusEnabledState                              INTEGER,
        	ltmPoolStatusParentType                                Integer32,
        	ltmPoolStatusDetailReason                              LongDisplayString
	}

ltmPoolStatusName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a pool."
	::= { ltmPoolStatusEntry 1 } 

ltmPoolStatusAvailState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4),
		grey(5)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The availability of the specified pool indicated in color.
		none - error;
		green - available in some capacity;
		yellow - not currently available;
		red - not available;
		blue - availability is unknown;
		gray - unlicensed"
	::= { ltmPoolStatusEntry 2 } 

ltmPoolStatusEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The activity status of the specified pool, as specified 
		by the user."
	::= { ltmPoolStatusEntry 3 } 

ltmPoolStatusParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! This is an internal data.
		The type of parent object which disabled the specified pool."
	::= { ltmPoolStatusEntry 4 } 

ltmPoolStatusDetailReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The detail description of the specified pool's status."
	::= { ltmPoolStatusEntry 5 } 

--==================================================================
-- Pool_member_status
--==================================================================
ltmPoolMbrStatusNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmPoolMemberStatus entries in the table."
	::= { ltmPoolMemberStatus 1 } 

ltmPoolMbrStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmPoolMbrStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing status information of pool members."
	::= { ltmPoolMemberStatus 2 } 

ltmPoolMbrStatusEntry OBJECT-TYPE
	SYNTAX  LtmPoolMbrStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmPoolMbrStatus Table"
	INDEX {
		ltmPoolMbrStatusPoolName,
		ltmPoolMbrStatusAddrType,
		ltmPoolMbrStatusAddr,
		ltmPoolMbrStatusPort
	}
	::= { ltmPoolMbrStatusTable 1 } 

LtmPoolMbrStatusEntry ::= 
	SEQUENCE {
        	ltmPoolMbrStatusPoolName                               LongDisplayString,
        	ltmPoolMbrStatusAddrType                               InetAddressType,
        	ltmPoolMbrStatusAddr                                   InetAddress,
        	ltmPoolMbrStatusPort                                   INTEGER,
        	ltmPoolMbrStatusAvailState                             INTEGER,
        	ltmPoolMbrStatusEnabledState                           INTEGER,
        	ltmPoolMbrStatusParentType                             Integer32,
        	ltmPoolMbrStatusDetailReason                           LongDisplayString
	}

ltmPoolMbrStatusPoolName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a pool."
	::= { ltmPoolMbrStatusEntry 1 } 

ltmPoolMbrStatusAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmPoolMbrStatusAddr."
	::= { ltmPoolMbrStatusEntry 2 } 

ltmPoolMbrStatusAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a pool member in the specified pool.  
		It is interpreted within the context of an ltmPoolMbrStatusAddrType value."
	::= { ltmPoolMbrStatusEntry 3 } 

ltmPoolMbrStatusPort OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The port number of the specified pool member."
	::= { ltmPoolMbrStatusEntry 4 } 

ltmPoolMbrStatusAvailState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4),
		gray(5)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The availability of the specified pool member indicated in color.
		none - error;
		green - available in some capacity;
		yellow - not currently available;
		red - not available;
		blue - availability is unknown;
		gray - unlicensed."
	::= { ltmPoolMbrStatusEntry 5 } 

ltmPoolMbrStatusEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The activity status of the specified pool member, as specified 
		by the user."
	::= { ltmPoolMbrStatusEntry 6 } 

ltmPoolMbrStatusParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! This is an internal data.
		The type of parent object which disabled the specified pool member."
	::= { ltmPoolMbrStatusEntry 7 } 

ltmPoolMbrStatusDetailReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The detail description of the specified pool member's status."
	::= { ltmPoolMbrStatusEntry 8 } 

--==================================================================
-- Virtual_server_status
--==================================================================
ltmVsStatusNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualServStatus entries in the table."
	::= { ltmVirtualServStatus 1 } 

ltmVsStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVsStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing status information of virtual servers."
	::= { ltmVirtualServStatus 2 } 

ltmVsStatusEntry OBJECT-TYPE
	SYNTAX  LtmVsStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVsStatus Table"
	INDEX {
		ltmVsStatusName
	}
	::= { ltmVsStatusTable 1 } 

LtmVsStatusEntry ::= 
	SEQUENCE {
        	ltmVsStatusName                                        LongDisplayString,
        	ltmVsStatusAvailState                                  INTEGER,
        	ltmVsStatusEnabledState                                INTEGER,
        	ltmVsStatusParentType                                  Integer32,
        	ltmVsStatusDetailReason                                LongDisplayString
	}

ltmVsStatusName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a virtual server."
	::= { ltmVsStatusEntry 1 } 

ltmVsStatusAvailState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4),
		gray(5)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The availability of the specified virtual server indicated in color.
		none - error;
		green - available in some capacity;
		yellow - not currently available;
		red - not available;
		blue - availability is unknown;
		gray - unlicensed."
	::= { ltmVsStatusEntry 2 } 

ltmVsStatusEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The activity status of the specified virtual server, as specified 
		by the user."
	::= { ltmVsStatusEntry 3 } 

ltmVsStatusParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! This is an internal data.
		The type of parent object which disabled the specified virtual server."
	::= { ltmVsStatusEntry 4 } 

ltmVsStatusDetailReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The detail description of the specified virtual server's status."
	::= { ltmVsStatusEntry 5 } 

--==================================================================
-- Virtual_address_status
--==================================================================
ltmVAddrStatusNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualAddrStatus entries in the table."
	::= { ltmVirtualAddrStatus 1 } 

ltmVAddrStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVAddrStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing status information of virtual addressess."
	::= { ltmVirtualAddrStatus 2 } 

ltmVAddrStatusEntry OBJECT-TYPE
	SYNTAX  LtmVAddrStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVAddrStatus Table"
	INDEX {
		ltmVAddrStatusAddrType,
		ltmVAddrStatusAddr
	}
	::= { ltmVAddrStatusTable 1 } 

LtmVAddrStatusEntry ::= 
	SEQUENCE {
        	ltmVAddrStatusAddrType                                 InetAddressType,
        	ltmVAddrStatusAddr                                     InetAddress,
        	ltmVAddrStatusAvailState                               INTEGER,
        	ltmVAddrStatusEnabledState                             INTEGER,
        	ltmVAddrStatusParentType                               Integer32,
        	ltmVAddrStatusDetailReason                             LongDisplayString
	}

ltmVAddrStatusAddrType OBJECT-TYPE 
	SYNTAX InetAddressType
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address type of ltmVsAddrStatusAddr"
	::= { ltmVAddrStatusEntry 1 } 

ltmVAddrStatusAddr OBJECT-TYPE 
	SYNTAX InetAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The IP address of a virtual address. It is interpreted 
		 within the context of a ltmVsAddrAddrType value."
	::= { ltmVAddrStatusEntry 2 } 

ltmVAddrStatusAvailState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		green(1),
		yellow(2),
		red(3),
		blue(4),
		gray(5)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The availability of the specified virtual address indicated in color.
		none - error;
		green - available in some capacity;
		yellow - not currently available;
		red - not available;
		blue - availability is unknown;
		gray - unlicensed."
	::= { ltmVAddrStatusEntry 3 } 

ltmVAddrStatusEnabledState OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		enabled(1),
		disabled(2),
		disabledbyparent(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The activity status of the specified virtual address, as specified 
		by the user."
	::= { ltmVAddrStatusEntry 4 } 

ltmVAddrStatusParentType OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS	 deprecated
	DESCRIPTION
		"Deprecated! This is an internal data.
		The type of parent object which disabled the specified virtual address."
	::= { ltmVAddrStatusEntry 5 } 

ltmVAddrStatusDetailReason OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The detail description of the specified virtual address's status."
	::= { ltmVAddrStatusEntry 6 } 

--==================================================================
-- Profile_http_fallback_status_codes
--==================================================================
ltmFallbackStatusNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileFallbackStatus entries in the table."
	::= { ltmHttpProfileFallbackStatus 1 } 

ltmFallbackStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmFallbackStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of status codes that when matched, 
		traffic will be sent to the 'fallback_host' for HTTP profiles."
	::= { ltmHttpProfileFallbackStatus 2 } 

ltmFallbackStatusEntry OBJECT-TYPE
	SYNTAX  LtmFallbackStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmFallbackStatus Table"
	INDEX {
		ltmFallbackStatusName,
		ltmFallbackStatusIndex
	}
	::= { ltmFallbackStatusTable 1 } 

LtmFallbackStatusEntry ::= 
	SEQUENCE {
        	ltmFallbackStatusName                                  LongDisplayString,
        	ltmFallbackStatusIndex                                 INTEGER,
        	ltmFallbackStatusCode                                  LongDisplayString
	}

ltmFallbackStatusName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmFallbackStatusEntry 1 } 

ltmFallbackStatusIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of status code for the specified HTTP profile."
	::= { ltmFallbackStatusEntry 2 } 

ltmFallbackStatusCode OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The status code that when matched, traffic will be sent to the 'fallback_host' for the specified profile."
	::= { ltmFallbackStatusEntry 3 } 

--==================================================================
-- Profile_http_response_headers_permitted
--==================================================================
ltmRespHeadersPermNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileRespHeadersPerm entries in the table."
	::= { ltmHttpProfileRespHeadersPerm 1 } 

ltmRespHeadersPermTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmRespHeadersPermEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of permitted headers in the 
		responses for HTTP profiles."
	::= { ltmHttpProfileRespHeadersPerm 2 } 

ltmRespHeadersPermEntry OBJECT-TYPE
	SYNTAX  LtmRespHeadersPermEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmRespHeadersPerm Table"
	INDEX {
		ltmRespHeadersPermName,
		ltmRespHeadersPermIndex
	}
	::= { ltmRespHeadersPermTable 1 } 

LtmRespHeadersPermEntry ::= 
	SEQUENCE {
        	ltmRespHeadersPermName                                 LongDisplayString,
        	ltmRespHeadersPermIndex                                INTEGER,
        	ltmRespHeadersPermStr                                  LongDisplayString
	}

ltmRespHeadersPermName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmRespHeadersPermEntry 1 } 

ltmRespHeadersPermIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of permitted header in a response for the specified HTTP profile."
	::= { ltmRespHeadersPermEntry 2 } 

ltmRespHeadersPermStr OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The permitted header in a response for the specified profile."
	::= { ltmRespHeadersPermEntry 3 } 

--==================================================================
-- Profile_http_encrypt_cookies
--==================================================================
ltmEncCookiesNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmHttpProfileEncCookies entries in the table."
	::= { ltmHttpProfileEncCookies 1 } 

ltmEncCookiesTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmEncCookiesEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of cookies to be encrypted before
		sending them to the clients for HTTP profiles."
	::= { ltmHttpProfileEncCookies 2 } 

ltmEncCookiesEntry OBJECT-TYPE
	SYNTAX  LtmEncCookiesEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmEncCookies Table"
	INDEX {
		ltmEncCookiesName,
		ltmEncCookiesIndex
	}
	::= { ltmEncCookiesTable 1 } 

LtmEncCookiesEntry ::= 
	SEQUENCE {
        	ltmEncCookiesName                                      LongDisplayString,
        	ltmEncCookiesIndex                                     INTEGER,
        	ltmEncCookiesStr                                       LongDisplayString
	}

ltmEncCookiesName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a HTTP profile."
	::= { ltmEncCookiesEntry 1 } 

ltmEncCookiesIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of cookie to be encrypted before sending it to the client
		 for the specified HTTP profile."
	::= { ltmEncCookiesEntry 2 } 

ltmEncCookiesStr OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The cookie to be encrypted before sending it to the client
		for the specified profile."
	::= { ltmEncCookiesEntry 3 } 

--==================================================================
-- Profile_bigproto_stat
--==================================================================
ltmFastL4ProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmFastL4ProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmFastL4ProfileStat 1 } 

ltmFastL4ProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmFastL4ProfileStat entries in the table."
	::= { ltmFastL4ProfileStat 2 } 

ltmFastL4ProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmFastL4ProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistics information of fast L4 profiles."
	::= { ltmFastL4ProfileStat 3 } 

ltmFastL4ProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmFastL4ProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmFastL4ProfileStat Table"
	INDEX {
		ltmFastL4ProfileStatName
	}
	::= { ltmFastL4ProfileStatTable 1 } 

LtmFastL4ProfileStatEntry ::= 
	SEQUENCE {
        	ltmFastL4ProfileStatName                               LongDisplayString,
        	ltmFastL4ProfileStatOpen                               Integer32,
        	ltmFastL4ProfileStatAccepts                            Counter64,
        	ltmFastL4ProfileStatAcceptfails                        Counter64,
        	ltmFastL4ProfileStatExpires                            Counter64,
        	ltmFastL4ProfileStatRxbadpkt                           Counter64,
        	ltmFastL4ProfileStatRxunreach                          Counter64,
        	ltmFastL4ProfileStatRxbadunreach                       Counter64,
        	ltmFastL4ProfileStatRxbadsum                           Counter64,
        	ltmFastL4ProfileStatTxerrors                           Counter64,
        	ltmFastL4ProfileStatSyncookIssue                       Counter64,
        	ltmFastL4ProfileStatSyncookAccept                      Counter64,
        	ltmFastL4ProfileStatSyncookReject                      Counter64,
        	ltmFastL4ProfileStatServersynrtx                       Counter64
	}

ltmFastL4ProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 1 } 

ltmFastL4ProfileStatOpen OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of current open connections for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 2 } 

ltmFastL4ProfileStatAccepts OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of accepted connections for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 3 } 

ltmFastL4ProfileStatAcceptfails OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of not accepted connections for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 4 } 

ltmFastL4ProfileStatExpires OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of expired connections due to idle timeout for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 5 } 

ltmFastL4ProfileStatRxbadpkt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of malformed packets for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 6 } 

ltmFastL4ProfileStatRxunreach OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of received ICMP unreach/TCP RST for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 7 } 

ltmFastL4ProfileStatRxbadunreach OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of received TCP RST outside the current window for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 8 } 

ltmFastL4ProfileStatRxbadsum OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of bad checksum for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 9 } 

ltmFastL4ProfileStatTxerrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of transmit datagram errors for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 10 } 

ltmFastL4ProfileStatSyncookIssue OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of syncookies issued for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 11 } 

ltmFastL4ProfileStatSyncookAccept OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of syncookies accepted for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 12 } 

ltmFastL4ProfileStatSyncookReject OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of syncookies rejected for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 13 } 

ltmFastL4ProfileStatServersynrtx OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of retransmissions of SYN to server for a syncookied connection for the specified fast L4 profile."
	::= { ltmFastL4ProfileStatEntry 14 } 

--==================================================================
-- Profile_sipp
--==================================================================
ltmSipProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSipProfile entries in the table."
	::= { ltmSipProfile 1 } 

ltmSipProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSipProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing configuratin information of SIP profiles."
	::= { ltmSipProfile 2 } 

ltmSipProfileEntry OBJECT-TYPE
	SYNTAX  LtmSipProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSipProfile Table"
	INDEX {
		ltmSipProfileName
	}
	::= { ltmSipProfileTable 1 } 

LtmSipProfileEntry ::= 
	SEQUENCE {
        	ltmSipProfileName                                      LongDisplayString,
        	ltmSipProfileConfigSource                              INTEGER,
        	ltmSipProfileDefaultName                               LongDisplayString,
        	ltmSipProfileMaxSize                                   Integer32,
        	ltmSipProfileTerminateBye                              INTEGER,
        	ltmSipProfileInsertVia                                 INTEGER,
        	ltmSipProfileSecureVia                                 INTEGER,
        	ltmSipProfileInsertRecordRoute                         INTEGER
	}

ltmSipProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SIP profile."
	::= { ltmSipProfileEntry 1 } 

ltmSipProfileConfigSource OBJECT-TYPE 
	SYNTAX INTEGER {
		usercfg(0),
		basecfg(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state that specifies whether this is a base/pre-configured profile 
		or user defined profile."
	::= { ltmSipProfileEntry 2 } 

ltmSipProfileDefaultName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the profile from which the specified profile derives 
		its attribute default values."
	::= { ltmSipProfileEntry 3 } 

ltmSipProfileMaxSize OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The acceptable maximum SIP message size for the specified profile."
	::= { ltmSipProfileEntry 4 } 

ltmSipProfileTerminateBye OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether  or not to terminate connection after bye (200 BYE) message for the specified profile."
	::= { ltmSipProfileEntry 5 } 

ltmSipProfileInsertVia OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not to insert Via for the specified profile."
	::= { ltmSipProfileEntry 6 } 

ltmSipProfileSecureVia OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not it is SIPS/2.0/TLS for the specified profile."
	::= { ltmSipProfileEntry 7 } 

ltmSipProfileInsertRecordRoute OBJECT-TYPE 
	SYNTAX INTEGER {
		false(0),
		true(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The state indicating whether or not insert Record-route for the specified profile."
	::= { ltmSipProfileEntry 8 } 

--==================================================================
-- Profile_sipp_stat
--==================================================================
ltmSipProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmSipProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmSipProfileStat 1 } 

ltmSipProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmSipProfileStat entries in the table."
	::= { ltmSipProfileStat 2 } 

ltmSipProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmSipProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistics information of SIP profiles."
	::= { ltmSipProfileStat 3 } 

ltmSipProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmSipProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmSipProfileStat Table"
	INDEX {
		ltmSipProfileStatName
	}
	::= { ltmSipProfileStatTable 1 } 

LtmSipProfileStatEntry ::= 
	SEQUENCE {
        	ltmSipProfileStatName                                  LongDisplayString,
        	ltmSipProfileStatRequests                              Counter64,
        	ltmSipProfileStatResponses                             Counter64,
        	ltmSipProfileStatBadmsgs                               Counter64,
        	ltmSipProfileStatDrops                                 Counter64
	}

ltmSipProfileStatName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a SIP profile."
	::= { ltmSipProfileStatEntry 1 } 

ltmSipProfileStatRequests OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of requests received for the specified profile."
	::= { ltmSipProfileStatEntry 2 } 

ltmSipProfileStatResponses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of responses sent for the specified profile."
	::= { ltmSipProfileStatEntry 3 } 

ltmSipProfileStatBadmsgs OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of bad messages for the specified profile."
	::= { ltmSipProfileStatEntry 4 } 

ltmSipProfileStatDrops OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of dropped packets for the specified profile."
	::= { ltmSipProfileStatEntry 5 } 

--==================================================================
-- Gtm_vs_score
--==================================================================
ltmVirtualModuleScoreNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmVirtualModuleScore entries in the table."
	::= { ltmVirtualModuleScore 1 } 

ltmVirtualModuleScoreTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmVirtualModuleScoreEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing module capacity scores for virtual servers"
	::= { ltmVirtualModuleScore 2 } 

ltmVirtualModuleScoreEntry OBJECT-TYPE
	SYNTAX  LtmVirtualModuleScoreEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmVirtualModuleScore Table"
	INDEX {
		ltmVirtualModuleScoreVsName,
		ltmVirtualModuleScoreModuleType
	}
	::= { ltmVirtualModuleScoreTable 1 } 

LtmVirtualModuleScoreEntry ::= 
	SEQUENCE {
        	ltmVirtualModuleScoreVsName                            LongDisplayString,
        	ltmVirtualModuleScoreModuleType                        INTEGER,
        	ltmVirtualModuleScoreScore                             Integer32
	}

ltmVirtualModuleScoreVsName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of the virtual server this score applies to."
	::= { ltmVirtualModuleScoreEntry 1 } 

ltmVirtualModuleScoreModuleType OBJECT-TYPE 
	SYNTAX INTEGER {
		ASM(0),
		SAM(1),
		WAM(2)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The bigip module that this score applites to."
	::= { ltmVirtualModuleScoreEntry 2 } 

ltmVirtualModuleScoreScore OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The score represents how much capacity the module estimates it has left."
	::= { ltmVirtualModuleScoreEntry 3 } 

--==================================================================
-- Profile_isession
--==================================================================
ltmIsessionProfileNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmIsessionProfile entries in the table."
	::= { ltmIsessionProfile 1 } 

ltmIsessionProfileTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmIsessionProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing configuratin information of Isession profiles."
	::= { ltmIsessionProfile 2 } 

ltmIsessionProfileEntry OBJECT-TYPE
	SYNTAX  LtmIsessionProfileEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmIsessionProfile Table"
	INDEX {
		ltmIsessionProfileName
	}
	::= { ltmIsessionProfileTable 1 } 

LtmIsessionProfileEntry ::= 
	SEQUENCE {
        	ltmIsessionProfileName                                 LongDisplayString,
        	ltmIsessionProfileMode                                 INTEGER,
        	ltmIsessionProfileConnectionReuse                      INTEGER,
        	ltmIsessionProfileCompressionNull                      INTEGER,
        	ltmIsessionProfileCompressionDeflate                   INTEGER,
        	ltmIsessionProfileCompressionLzo                       INTEGER,
        	ltmIsessionProfileCompressionAdaptive                  INTEGER,
        	ltmIsessionProfileDeduplication                        INTEGER,
        	ltmIsessionProfilePortTransparency                     INTEGER,
        	ltmIsessionProfileTargetVirtual                        INTEGER,
        	ltmIsessionProfileEndpointPool                         LongDisplayString,
        	ltmIsessionProfileCompressionDeflateLevel              Integer32
	}

ltmIsessionProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a iSession profile."
	::= { ltmIsessionProfileEntry 1 } 

ltmIsessionProfileMode OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Enable/disable this profile."
	::= { ltmIsessionProfileEntry 2 } 

ltmIsessionProfileConnectionReuse OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Enable/disable connection reuse."
	::= { ltmIsessionProfileEntry 3 } 

ltmIsessionProfileCompressionNull OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Select null compression method if enabled."
	::= { ltmIsessionProfileEntry 4 } 

ltmIsessionProfileCompressionDeflate OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Select deflate compression method if enabled."
	::= { ltmIsessionProfileEntry 5 } 

ltmIsessionProfileCompressionLzo OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Select lzo compression method if enabled."
	::= { ltmIsessionProfileEntry 6 } 

ltmIsessionProfileCompressionAdaptive OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Select adaptive compression method if enabled."
	::= { ltmIsessionProfileEntry 7 } 

ltmIsessionProfileDeduplication OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Enable/disable deduplication functionality."
	::= { ltmIsessionProfileEntry 8 } 

ltmIsessionProfilePortTransparency OBJECT-TYPE 
	SYNTAX INTEGER {
		disabled(0),
		enabled(1)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Use same destination port over WAN as specified by the client."
	::= { ltmIsessionProfileEntry 9 } 

ltmIsessionProfileTargetVirtual OBJECT-TYPE 
	SYNTAX INTEGER {
		none(0),
		hostmatchnoisession(1),
		hostmatchall(2),
		matchall(3)
	}
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Use to provide good match for targetted virtual."
	::= { ltmIsessionProfileEntry 10 } 

ltmIsessionProfileEndpointPool OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a LTM pool for paired tunneling."
	::= { ltmIsessionProfileEntry 11 } 

ltmIsessionProfileCompressionDeflateLevel OBJECT-TYPE 
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Select compression level [1-9] when deflate compression method is enabled."
	::= { ltmIsessionProfileEntry 12 } 

--==================================================================
-- Profile_isession_stat
--==================================================================
ltmIsessionProfileStatResetStats OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"The action to reset resetable statistics data in  ltmIsessionProfileStat. 
		 Setting this value to 1 will reset statistics data. 
		 Note, some statistics data may not be reset including data that are incremental counters."
	::= { ltmIsessionProfileStat 1 } 

ltmIsessionProfileStatNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmIsessionProfileStat entries in the table."
	::= { ltmIsessionProfileStat 2 } 

ltmIsessionProfileStatTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmIsessionProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing statistics information for virtual servers with iSession profiles"
	::= { ltmIsessionProfileStat 3 } 

ltmIsessionProfileStatEntry OBJECT-TYPE
	SYNTAX  LtmIsessionProfileStatEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmIsessionProfileStat Table"
	INDEX {
		ltmIsessionProfileStatVirtualName
	}
	::= { ltmIsessionProfileStatTable 1 } 

LtmIsessionProfileStatEntry ::= 
	SEQUENCE {
        	ltmIsessionProfileStatVirtualName                      LongDisplayString,
        	ltmIsessionProfileStatProfileName                      LongDisplayString,
        	ltmIsessionProfileStatNullInUses                       Counter64,
        	ltmIsessionProfileStatNullInErrors                     Counter64,
        	ltmIsessionProfileStatNullInBytesOpt                   Counter64,
        	ltmIsessionProfileStatNullInBytesRaw                   Counter64,
        	ltmIsessionProfileStatNullOutUses                      Counter64,
        	ltmIsessionProfileStatNullOutErrors                    Counter64,
        	ltmIsessionProfileStatNullOutBytesOpt                  Counter64,
        	ltmIsessionProfileStatNullOutBytesRaw                  Counter64,
        	ltmIsessionProfileStatLzoInUses                        Counter64,
        	ltmIsessionProfileStatLzoInErrors                      Counter64,
        	ltmIsessionProfileStatLzoInBytesOpt                    Counter64,
        	ltmIsessionProfileStatLzoInBytesRaw                    Counter64,
        	ltmIsessionProfileStatLzoOutUses                       Counter64,
        	ltmIsessionProfileStatLzoOutErrors                     Counter64,
        	ltmIsessionProfileStatLzoOutBytesOpt                   Counter64,
        	ltmIsessionProfileStatLzoOutBytesRaw                   Counter64,
        	ltmIsessionProfileStatDeflateInUses                    Counter64,
        	ltmIsessionProfileStatDeflateInErrors                  Counter64,
        	ltmIsessionProfileStatDeflateInBytesOpt                Counter64,
        	ltmIsessionProfileStatDeflateInBytesRaw                Counter64,
        	ltmIsessionProfileStatDeflateOutUses                   Counter64,
        	ltmIsessionProfileStatDeflateOutErrors                 Counter64,
        	ltmIsessionProfileStatDeflateOutBytesOpt               Counter64,
        	ltmIsessionProfileStatDeflateOutBytesRaw               Counter64,
        	ltmIsessionProfileStatDedupInUses                      Counter64,
        	ltmIsessionProfileStatDedupInErrors                    Counter64,
        	ltmIsessionProfileStatDedupInBytesOpt                  Counter64,
        	ltmIsessionProfileStatDedupInBytesRaw                  Counter64,
        	ltmIsessionProfileStatDedupOutUses                     Counter64,
        	ltmIsessionProfileStatDedupOutErrors                   Counter64,
        	ltmIsessionProfileStatDedupOutBytesOpt                 Counter64,
        	ltmIsessionProfileStatDedupOutBytesRaw                 Counter64,
        	ltmIsessionProfileStatDedupInHits                      Counter64,
        	ltmIsessionProfileStatDedupInHitBytes                  Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket1k           Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket2k           Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket4k           Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket8k           Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket16k          Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket32k          Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket64k          Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket128k         Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket256k         Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket512k         Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucket1m           Counter64,
        	ltmIsessionProfileStatDedupInHitHistBucketLarge        Counter64,
        	ltmIsessionProfileStatDedupInMisses                    Counter64,
        	ltmIsessionProfileStatDedupInMissBytes                 Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket1k          Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket2k          Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket4k          Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket8k          Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket16k         Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket32k         Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket64k         Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket128k        Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket256k        Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket512k        Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucket1m          Counter64,
        	ltmIsessionProfileStatDedupInMissHistBucketLarge       Counter64,
        	ltmIsessionProfileStatDedupOutHits                     Counter64,
        	ltmIsessionProfileStatDedupOutHitBytes                 Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket1k          Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket2k          Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket4k          Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket8k          Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket16k         Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket32k         Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket64k         Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket128k        Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket256k        Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket512k        Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucket1m          Counter64,
        	ltmIsessionProfileStatDedupOutHitHistBucketLarge       Counter64,
        	ltmIsessionProfileStatDedupOutMisses                   Counter64,
        	ltmIsessionProfileStatDedupOutMissBytes                Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket1k         Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket2k         Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket4k         Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket8k         Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket16k        Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket32k        Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket64k        Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket128k       Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket256k       Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket512k       Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucket1m         Counter64,
        	ltmIsessionProfileStatDedupOutMissHistBucketLarge      Counter64,
        	ltmIsessionProfileStatOutgoingConnsIdleCur             Counter64,
        	ltmIsessionProfileStatOutgoingConnsIdleMax             Counter64,
        	ltmIsessionProfileStatOutgoingConnsIdleTot             Counter64,
        	ltmIsessionProfileStatOutgoingConnsActiveCur           Counter64,
        	ltmIsessionProfileStatOutgoingConnsActiveMax           Counter64,
        	ltmIsessionProfileStatOutgoingConnsActiveTot           Counter64,
        	ltmIsessionProfileStatOutgoingConnsErrors              Counter64,
        	ltmIsessionProfileStatOutgoingConnsPassthruTot         Counter64,
        	ltmIsessionProfileStatIncomingConnsActiveCur           Counter64,
        	ltmIsessionProfileStatIncomingConnsActiveMax           Counter64,
        	ltmIsessionProfileStatIncomingConnsActiveTot           Counter64,
        	ltmIsessionProfileStatIncomingConnsErrors              Counter64
	}

ltmIsessionProfileStatVirtualName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a iSession virtual server."
	::= { ltmIsessionProfileStatEntry 1 } 

ltmIsessionProfileStatProfileName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of a iSession profile."
	::= { ltmIsessionProfileStatEntry 2 } 

ltmIsessionProfileStatNullInUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses NULL compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 3 } 

ltmIsessionProfileStatNullInErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use NULL compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 4 } 

ltmIsessionProfileStatNullInBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes NULL compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 5 } 

ltmIsessionProfileStatNullInBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes NULL compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 6 } 

ltmIsessionProfileStatNullOutUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses NULL compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 7 } 

ltmIsessionProfileStatNullOutErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use NULL compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 8 } 

ltmIsessionProfileStatNullOutBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes NULL compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 9 } 

ltmIsessionProfileStatNullOutBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes NULL compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 10 } 

ltmIsessionProfileStatLzoInUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses LZO compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 11 } 

ltmIsessionProfileStatLzoInErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use LZO compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 12 } 

ltmIsessionProfileStatLzoInBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes LZO compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 13 } 

ltmIsessionProfileStatLzoInBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes LZO compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 14 } 

ltmIsessionProfileStatLzoOutUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses LZO compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 15 } 

ltmIsessionProfileStatLzoOutErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use LZO compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 16 } 

ltmIsessionProfileStatLzoOutBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes LZO compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 17 } 

ltmIsessionProfileStatLzoOutBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes LZO compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 18 } 

ltmIsessionProfileStatDeflateInUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses DEFLATE compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 19 } 

ltmIsessionProfileStatDeflateInErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use DEFLATE compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 20 } 

ltmIsessionProfileStatDeflateInBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes DEFLATE compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 21 } 

ltmIsessionProfileStatDeflateInBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes DEFLATE compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 22 } 

ltmIsessionProfileStatDeflateOutUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses DEFLATE compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 23 } 

ltmIsessionProfileStatDeflateOutErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use DEFLATE compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 24 } 

ltmIsessionProfileStatDeflateOutBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes DEFLATE compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 25 } 

ltmIsessionProfileStatDeflateOutBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes DEFLATE compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 26 } 

ltmIsessionProfileStatDedupInUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses DEDUPLICATION compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 27 } 

ltmIsessionProfileStatDedupInErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use DEDUPLICATION compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 28 } 

ltmIsessionProfileStatDedupInBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes DEDUPLICATION compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 29 } 

ltmIsessionProfileStatDedupInBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes DEDUPLICATION compression for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 30 } 

ltmIsessionProfileStatDedupOutUses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of uses DEDUPLICATION compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 31 } 

ltmIsessionProfileStatDedupOutErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of errors in use DEDUPLICATION compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 32 } 

ltmIsessionProfileStatDedupOutBytesOpt OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of opt bytes DEDUPLICATION compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 33 } 

ltmIsessionProfileStatDedupOutBytesRaw OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of raw bytes DEDUPLICATION compression for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 34 } 

ltmIsessionProfileStatDedupInHits OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 35 } 

ltmIsessionProfileStatDedupInHitBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hit bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 36 } 

ltmIsessionProfileStatDedupInHitHistBucket1k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size less than 1k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 37 } 

ltmIsessionProfileStatDedupInHitHistBucket2k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 1k and 2k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 38 } 

ltmIsessionProfileStatDedupInHitHistBucket4k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 2k and 4k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 39 } 

ltmIsessionProfileStatDedupInHitHistBucket8k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 4k and 8k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 40 } 

ltmIsessionProfileStatDedupInHitHistBucket16k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 8k and 16k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 41 } 

ltmIsessionProfileStatDedupInHitHistBucket32k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 16k and 32k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 42 } 

ltmIsessionProfileStatDedupInHitHistBucket64k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 32k and 64k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 43 } 

ltmIsessionProfileStatDedupInHitHistBucket128k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 64k and 128k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 44 } 

ltmIsessionProfileStatDedupInHitHistBucket256k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 128k and 256k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 45 } 

ltmIsessionProfileStatDedupInHitHistBucket512k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 256k and 512k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 46 } 

ltmIsessionProfileStatDedupInHitHistBucket1m OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 512k and 1m bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 47 } 

ltmIsessionProfileStatDedupInHitHistBucketLarge OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size more than 1m bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 48 } 

ltmIsessionProfileStatDedupInMisses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 49 } 

ltmIsessionProfileStatDedupInMissBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 50 } 

ltmIsessionProfileStatDedupInMissHistBucket1k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size less than 1k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 51 } 

ltmIsessionProfileStatDedupInMissHistBucket2k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 1k and 2k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 52 } 

ltmIsessionProfileStatDedupInMissHistBucket4k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 2k and 4k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 53 } 

ltmIsessionProfileStatDedupInMissHistBucket8k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 4k and 8k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 54 } 

ltmIsessionProfileStatDedupInMissHistBucket16k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 8k and 16k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 55 } 

ltmIsessionProfileStatDedupInMissHistBucket32k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 16k and 32k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 56 } 

ltmIsessionProfileStatDedupInMissHistBucket64k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 32k and 64k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 57 } 

ltmIsessionProfileStatDedupInMissHistBucket128k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 64k and 128k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 58 } 

ltmIsessionProfileStatDedupInMissHistBucket256k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 128k and 256k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 59 } 

ltmIsessionProfileStatDedupInMissHistBucket512k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 256k and 512k bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 60 } 

ltmIsessionProfileStatDedupInMissHistBucket1m OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 512k and 1m bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 61 } 

ltmIsessionProfileStatDedupInMissHistBucketLarge OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size more than 1m bytes for IN towards LAN"
	::= { ltmIsessionProfileStatEntry 62 } 

ltmIsessionProfileStatDedupOutHits OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 63 } 

ltmIsessionProfileStatDedupOutHitBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hit bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 64 } 

ltmIsessionProfileStatDedupOutHitHistBucket1k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size less than 1k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 65 } 

ltmIsessionProfileStatDedupOutHitHistBucket2k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 1k and 2k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 66 } 

ltmIsessionProfileStatDedupOutHitHistBucket4k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 2k and 4k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 67 } 

ltmIsessionProfileStatDedupOutHitHistBucket8k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 4k and 8k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 68 } 

ltmIsessionProfileStatDedupOutHitHistBucket16k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 8k and 16k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 69 } 

ltmIsessionProfileStatDedupOutHitHistBucket32k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 16k and 32k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 70 } 

ltmIsessionProfileStatDedupOutHitHistBucket64k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 32k and 64k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 71 } 

ltmIsessionProfileStatDedupOutHitHistBucket128k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 64k and 128k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 72 } 

ltmIsessionProfileStatDedupOutHitHistBucket256k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 128k and 256k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 73 } 

ltmIsessionProfileStatDedupOutHitHistBucket512k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 256k and 512k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 74 } 

ltmIsessionProfileStatDedupOutHitHistBucket1m OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size between 512k and 1m bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 75 } 

ltmIsessionProfileStatDedupOutHitHistBucketLarge OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication hits with size more than 1m bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 76 } 

ltmIsessionProfileStatDedupOutMisses OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 77 } 

ltmIsessionProfileStatDedupOutMissBytes OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 78 } 

ltmIsessionProfileStatDedupOutMissHistBucket1k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size less than 1k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 79 } 

ltmIsessionProfileStatDedupOutMissHistBucket2k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 1k and 2k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 80 } 

ltmIsessionProfileStatDedupOutMissHistBucket4k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 2k and 4k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 81 } 

ltmIsessionProfileStatDedupOutMissHistBucket8k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 4k and 8k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 82 } 

ltmIsessionProfileStatDedupOutMissHistBucket16k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 8k and 16k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 83 } 

ltmIsessionProfileStatDedupOutMissHistBucket32k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 16k and 32k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 84 } 

ltmIsessionProfileStatDedupOutMissHistBucket64k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 32k and 64k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 85 } 

ltmIsessionProfileStatDedupOutMissHistBucket128k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 64k and 128k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 86 } 

ltmIsessionProfileStatDedupOutMissHistBucket256k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 128k and 256k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 87 } 

ltmIsessionProfileStatDedupOutMissHistBucket512k OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 256k and 512k bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 88 } 

ltmIsessionProfileStatDedupOutMissHistBucket1m OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size between 512k and 1m bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 89 } 

ltmIsessionProfileStatDedupOutMissHistBucketLarge OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of deduplication misses with size more than 1m bytes for OUT towards WAN"
	::= { ltmIsessionProfileStatEntry 90 } 

ltmIsessionProfileStatOutgoingConnsIdleCur OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of outgoing idle connections"
	::= { ltmIsessionProfileStatEntry 91 } 

ltmIsessionProfileStatOutgoingConnsIdleMax OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of outgoing idle connections"
	::= { ltmIsessionProfileStatEntry 92 } 

ltmIsessionProfileStatOutgoingConnsIdleTot OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of outgoing idle connections"
	::= { ltmIsessionProfileStatEntry 93 } 

ltmIsessionProfileStatOutgoingConnsActiveCur OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of outgoing active connections"
	::= { ltmIsessionProfileStatEntry 94 } 

ltmIsessionProfileStatOutgoingConnsActiveMax OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of outgoing active connections"
	::= { ltmIsessionProfileStatEntry 95 } 

ltmIsessionProfileStatOutgoingConnsActiveTot OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of outgoing active connections"
	::= { ltmIsessionProfileStatEntry 96 } 

ltmIsessionProfileStatOutgoingConnsErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of outgoing connection errors"
	::= { ltmIsessionProfileStatEntry 97 } 

ltmIsessionProfileStatOutgoingConnsPassthruTot OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of outgoing passthrough connections"
	::= { ltmIsessionProfileStatEntry 98 } 

ltmIsessionProfileStatIncomingConnsActiveCur OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The current number of incoming active connections"
	::= { ltmIsessionProfileStatEntry 99 } 

ltmIsessionProfileStatIncomingConnsActiveMax OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The maximum number of incoming active connections"
	::= { ltmIsessionProfileStatEntry 100 } 

ltmIsessionProfileStatIncomingConnsActiveTot OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The total number of incoming active connections"
	::= { ltmIsessionProfileStatEntry 101 } 

ltmIsessionProfileStatIncomingConnsErrors OBJECT-TYPE 
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of incoming connection errors"
	::= { ltmIsessionProfileStatEntry 102 } 

--==================================================================
-- Profile_xml_xpath_queries
--==================================================================
ltmXmlProfileXpathQueriesNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmXmlProfileXpathQueries entries in the table."
	::= { ltmXmlProfileXpathQueries 1 } 

ltmXmlProfileXpathQueriesTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmXmlProfileXpathQueriesEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of XPath queries in xml profiles."
	::= { ltmXmlProfileXpathQueries 2 } 

ltmXmlProfileXpathQueriesEntry OBJECT-TYPE
	SYNTAX  LtmXmlProfileXpathQueriesEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmXmlProfileXpathQueries Table"
	INDEX {
		ltmXmlProfileXpathQueriesName,
		ltmXmlProfileXpathQueriesIndex
	}
	::= { ltmXmlProfileXpathQueriesTable 1 } 

LtmXmlProfileXpathQueriesEntry ::= 
	SEQUENCE {
        	ltmXmlProfileXpathQueriesName                          LongDisplayString,
        	ltmXmlProfileXpathQueriesIndex                         INTEGER,
        	ltmXmlProfileXpathQueriesString                        LongDisplayString
	}

ltmXmlProfileXpathQueriesName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of an xml profile."
	::= { ltmXmlProfileXpathQueriesEntry 1 } 

ltmXmlProfileXpathQueriesIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of XPath quereies for the specified xml profile."
	::= { ltmXmlProfileXpathQueriesEntry 2 } 

ltmXmlProfileXpathQueriesString OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The XPath query for the specified profile."
	::= { ltmXmlProfileXpathQueriesEntry 3 } 

--==================================================================
-- Profile_xml_namespace_mappings
--==================================================================
ltmXmlProfileNamespaceMappingsNumber OBJECT-TYPE 
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The number of ltmXmlProfileNamespaceMappings entries in the table."
	::= { ltmXmlProfileNamespaceMappings 1 } 

ltmXmlProfileNamespaceMappingsTable OBJECT-TYPE
	SYNTAX SEQUENCE OF LtmXmlProfileNamespaceMappingsEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"A table containing information of namespace mappings in xml profiles."
	::= { ltmXmlProfileNamespaceMappings 2 } 

ltmXmlProfileNamespaceMappingsEntry OBJECT-TYPE
	SYNTAX  LtmXmlProfileNamespaceMappingsEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Columns in the ltmXmlProfileNamespaceMappings Table"
	INDEX {
		ltmXmlProfileNamespaceMappingsName,
		ltmXmlProfileNamespaceMappingsIndex
	}
	::= { ltmXmlProfileNamespaceMappingsTable 1 } 

LtmXmlProfileNamespaceMappingsEntry ::= 
	SEQUENCE {
        	ltmXmlProfileNamespaceMappingsName                     LongDisplayString,
        	ltmXmlProfileNamespaceMappingsIndex                    INTEGER,
        	ltmXmlProfileNamespaceMappingsMappingPrefix            LongDisplayString,
        	ltmXmlProfileNamespaceMappingsMappingNamespace         LongDisplayString
	}

ltmXmlProfileNamespaceMappingsName OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The name of an xml profile."
	::= { ltmXmlProfileNamespaceMappingsEntry 1 } 

ltmXmlProfileNamespaceMappingsIndex OBJECT-TYPE 
	SYNTAX INTEGER(1..2147483647)
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The index of Namespace Mappings for the specified xml profile."
	::= { ltmXmlProfileNamespaceMappingsEntry 2 } 

ltmXmlProfileNamespaceMappingsMappingPrefix OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The Namespace Mapping Prefix for the specified profile."
	::= { ltmXmlProfileNamespaceMappingsEntry 3 } 

ltmXmlProfileNamespaceMappingsMappingNamespace OBJECT-TYPE 
	SYNTAX LongDisplayString
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"The Namespace Mapping Namespace for the specified profile."
	::= { ltmXmlProfileNamespaceMappingsEntry 4 } 

--================================================================
 -- Compliance and Group
--================================================================

bigipLocalTMCompliance	MODULE-COMPLIANCE 
	STATUS current
	DESCRIPTION
		"This specifies the objects that are required to claim 
                 compliance to F5 Traffic Management System."
	MODULE
	  MANDATORY-GROUPS { bigipLocalTMGroups } 
	::= { bigipCompliances 2 } 

bigipLocalTMGroups  OBJECT IDENTIFIER ::= {  bigipGroups 2 }

ltmAttrGroup OBJECT-GROUP
	 OBJECTS {
		ltmAttrLbmodeFastestMaxIdleTime,
		ltmAttrMirrorState,
		ltmAttrPersistDestAddrLimitMode,
		ltmAttrPersistDestAddrMaxCount,
		ltmAttrSnatAnyIpProtocol,
		ltmAttrMirrorPeerIpAddr
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmGlobalAttr MIB."
	::= { bigipLocalTMGroups 1 }

ltmRateFilterGroup OBJECT-GROUP
	 OBJECTS {
		ltmRateFilterNumber,
		ltmRateFilterCname,
		ltmRateFilterRate,
		ltmRateFilterCeil,
		ltmRateFilterBurst,
		ltmRateFilterPname,
		ltmRateFilterQtype,
		ltmRateFilterDirection
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmRateFilter MIB."
	::= { bigipLocalTMGroups 2 }

ltmRateFilterStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmRateFilterStatResetStats,
		ltmRateFilterStatNumber,
		ltmRateFilterStatCname,
		ltmRateFilterStatRateBytes,
		ltmRateFilterStatBurstBytes,
		ltmRateFilterStatDroppedBytes,
		ltmRateFilterStatBytesQueued,
		ltmRateFilterStatBytesPerSec,
		ltmRateFilterStatDropTailPkts,
		ltmRateFilterStatDropTailBytes,
		ltmRateFilterStatDropRandPkts,
		ltmRateFilterStatDropRandBytes,
		ltmRateFilterStatDropTotPkts,
		ltmRateFilterStatDropTotBytes
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmRateFilterStat MIB."
	::= { bigipLocalTMGroups 3 }

ltmMirrorPortGroup OBJECT-GROUP
	 OBJECTS {
		ltmMirrorPortNumber,
		ltmMirrorPortName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmMirrorPort MIB."
	::= { bigipLocalTMGroups 4 }

ltmMirrorPortMemberGroup OBJECT-GROUP
	 OBJECTS {
		ltmMirrorPortMemberNumber,
		ltmMirrorPortMemberToName,
		ltmMirrorPortMemberName,
		ltmMirrorPortMemberConduitName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmMirrorPortMember MIB."
	::= { bigipLocalTMGroups 5 }

ltmNatGroup OBJECT-GROUP
	 OBJECTS {
		ltmNatNumber,
		ltmNatTransAddrType,
		ltmNatTransAddr,
		ltmNatOrigAddrType,
		ltmNatOrigAddr,
		ltmNatEnabled,
		ltmNatArpEnabled,
		ltmNatUnitId,
		ltmNatListedEnabledVlans
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmNat MIB."
	::= { bigipLocalTMGroups 6 }

ltmNatStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmNatStatResetStats,
		ltmNatStatNumber,
		ltmNatStatTransAddrType,
		ltmNatStatTransAddr,
		ltmNatStatServerPktsIn,
		ltmNatStatServerBytesIn,
		ltmNatStatServerPktsOut,
		ltmNatStatServerBytesOut,
		ltmNatStatServerMaxConns,
		ltmNatStatServerTotConns,
		ltmNatStatServerCurConns
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmNatStat MIB."
	::= { bigipLocalTMGroups 7 }

ltmNatVlanGroup OBJECT-GROUP
	 OBJECTS {
		ltmNatVlanNumber,
		ltmNatVlanTransAddrType,
		ltmNatVlanTransAddr,
		ltmNatVlanVlanName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmNatVlan MIB."
	::= { bigipLocalTMGroups 8 }

ltmNodeAddrGroup OBJECT-GROUP
	 OBJECTS {
		ltmNodeAddrNumber,
		ltmNodeAddrAddrType,
		ltmNodeAddrAddr,
		ltmNodeAddrConnLimit,
		ltmNodeAddrRatio,
		ltmNodeAddrDynamicRatio,
		ltmNodeAddrMonitorState,
		ltmNodeAddrMonitorStatus,
		ltmNodeAddrMonitorRule,
		ltmNodeAddrNewSessionEnable,
		ltmNodeAddrSessionStatus,
		ltmNodeAddrPoolMemberRefCount,
		ltmNodeAddrScreenName,
		ltmNodeAddrAvailabilityState,
		ltmNodeAddrEnabledState,
		ltmNodeAddrDisabledParentType,
		ltmNodeAddrStatusReason
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmNodeAddr MIB."
	::= { bigipLocalTMGroups 9 }

ltmNodeAddrStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmNodeAddrStatResetStats,
		ltmNodeAddrStatNumber,
		ltmNodeAddrStatAddrType,
		ltmNodeAddrStatAddr,
		ltmNodeAddrStatServerPktsIn,
		ltmNodeAddrStatServerBytesIn,
		ltmNodeAddrStatServerPktsOut,
		ltmNodeAddrStatServerBytesOut,
		ltmNodeAddrStatServerMaxConns,
		ltmNodeAddrStatServerTotConns,
		ltmNodeAddrStatServerCurConns,
		ltmNodeAddrStatPvaPktsIn,
		ltmNodeAddrStatPvaBytesIn,
		ltmNodeAddrStatPvaPktsOut,
		ltmNodeAddrStatPvaBytesOut,
		ltmNodeAddrStatPvaMaxConns,
		ltmNodeAddrStatPvaTotConns,
		ltmNodeAddrStatPvaCurConns,
		ltmNodeAddrStatTotRequests,
		ltmNodeAddrStatTotPvaAssistConn,
		ltmNodeAddrStatCurrPvaAssistConn
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmNodeAddrStat MIB."
	::= { bigipLocalTMGroups 10 }

ltmPoolGroup OBJECT-GROUP
	 OBJECTS {
		ltmPoolNumber,
		ltmPoolName,
		ltmPoolLbMode,
		ltmPoolActionOnServiceDown,
		ltmPoolMinUpMembers,
		ltmPoolMinUpMembersEnable,
		ltmPoolMinUpMemberAction,
		ltmPoolMinActiveMembers,
		ltmPoolActiveMemberCnt,
		ltmPoolDisallowSnat,
		ltmPoolDisallowNat,
		ltmPoolSimpleTimeout,
		ltmPoolIpTosToClient,
		ltmPoolIpTosToServer,
		ltmPoolLinkQosToClient,
		ltmPoolLinkQosToServer,
		ltmPoolDynamicRatioSum,
		ltmPoolMonitorRule,
		ltmPoolAvailabilityState,
		ltmPoolEnabledState,
		ltmPoolDisabledParentType,
		ltmPoolStatusReason,
		ltmPoolSlowRampTime,
		ltmPoolMemberCnt
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmPool MIB."
	::= { bigipLocalTMGroups 11 }

ltmPoolStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmPoolStatResetStats,
		ltmPoolStatNumber,
		ltmPoolStatName,
		ltmPoolStatServerPktsIn,
		ltmPoolStatServerBytesIn,
		ltmPoolStatServerPktsOut,
		ltmPoolStatServerBytesOut,
		ltmPoolStatServerMaxConns,
		ltmPoolStatServerTotConns,
		ltmPoolStatServerCurConns,
		ltmPoolStatPvaPktsIn,
		ltmPoolStatPvaBytesIn,
		ltmPoolStatPvaPktsOut,
		ltmPoolStatPvaBytesOut,
		ltmPoolStatPvaMaxConns,
		ltmPoolStatPvaTotConns,
		ltmPoolStatPvaCurConns,
		ltmPoolStatTotPvaAssistConn,
		ltmPoolStatCurrPvaAssistConn
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmPoolStat MIB."
	::= { bigipLocalTMGroups 12 }

ltmPoolMemberGroup OBJECT-GROUP
	 OBJECTS {
		ltmPoolMemberNumber,
		ltmPoolMemberPoolName,
		ltmPoolMemberAddrType,
		ltmPoolMemberAddr,
		ltmPoolMemberPort,
		ltmPoolMemberConnLimit,
		ltmPoolMemberRatio,
		ltmPoolMemberWeight,
		ltmPoolMemberPriority,
		ltmPoolMemberDynamicRatio,
		ltmPoolMemberMonitorState,
		ltmPoolMemberMonitorStatus,
		ltmPoolMemberNewSessionEnable,
		ltmPoolMemberSessionStatus,
		ltmPoolMemberMonitorRule,
		ltmPoolMemberAvailabilityState,
		ltmPoolMemberEnabledState,
		ltmPoolMemberDisabledParentType,
		ltmPoolMemberStatusReason
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmPoolMember MIB."
	::= { bigipLocalTMGroups 13 }

ltmPoolMemberStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmPoolMemberStatResetStats,
		ltmPoolMemberStatNumber,
		ltmPoolMemberStatPoolName,
		ltmPoolMemberStatAddrType,
		ltmPoolMemberStatAddr,
		ltmPoolMemberStatPort,
		ltmPoolMemberStatServerPktsIn,
		ltmPoolMemberStatServerBytesIn,
		ltmPoolMemberStatServerPktsOut,
		ltmPoolMemberStatServerBytesOut,
		ltmPoolMemberStatServerMaxConns,
		ltmPoolMemberStatServerTotConns,
		ltmPoolMemberStatServerCurConns,
		ltmPoolMemberStatPvaPktsIn,
		ltmPoolMemberStatPvaBytesIn,
		ltmPoolMemberStatPvaPktsOut,
		ltmPoolMemberStatPvaBytesOut,
		ltmPoolMemberStatPvaMaxConns,
		ltmPoolMemberStatPvaTotConns,
		ltmPoolMemberStatPvaCurConns,
		ltmPoolMemberStatTotRequests,
		ltmPoolMemberStatTotPvaAssistConn,
		ltmPoolMemberStatCurrPvaAssistConn
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmPoolMemberStat MIB."
	::= { bigipLocalTMGroups 14 }

ltmAuthProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmAuthProfileNumber,
		ltmAuthProfileName,
		ltmAuthProfileConfigSource,
		ltmAuthProfileDefaultName,
		ltmAuthProfileConfigName,
		ltmAuthProfileType,
		ltmAuthProfileMode,
		ltmAuthProfileCredentialSource,
		ltmAuthProfileRuleName,
		ltmAuthProfileIdleTimeout
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmAuthProfile MIB."
	::= { bigipLocalTMGroups 15 }

ltmAuthProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmAuthProfileStatResetStats,
		ltmAuthProfileStatNumber,
		ltmAuthProfileStatName,
		ltmAuthProfileStatTotSessions,
		ltmAuthProfileStatCurSessions,
		ltmAuthProfileStatMaxSessions,
		ltmAuthProfileStatSuccessResults,
		ltmAuthProfileStatFailureResults,
		ltmAuthProfileStatWantcredentialResults,
		ltmAuthProfileStatErrorResults
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmAuthProfileStat MIB."
	::= { bigipLocalTMGroups 16 }

ltmClientSslGroup OBJECT-GROUP
	 OBJECTS {
		ltmClientSslNumber,
		ltmClientSslName,
		ltmClientSslConfigSource,
		ltmClientSslDefaultName,
		ltmClientSslMode,
		ltmClientSslKey,
		ltmClientSslCert,
		ltmClientSslChain,
		ltmClientSslCafile,
		ltmClientSslCrlfile,
		ltmClientSslClientcertca,
		ltmClientSslCiphers,
		ltmClientSslPassphrase,
		ltmClientSslOptions,
		ltmClientSslModsslmethods,
		ltmClientSslCacheSize,
		ltmClientSslCacheTimeout,
		ltmClientSslRenegotiatePeriod,
		ltmClientSslRenegotiateSize,
		ltmClientSslRenegotiateMaxRecordDelay,
		ltmClientSslHandshakeTimeout,
		ltmClientSslAlertTimeout,
		ltmClientSslPeerCertMode,
		ltmClientSslAuthenticateOnce,
		ltmClientSslAuthenticateDepth,
		ltmClientSslUncleanShutdown,
		ltmClientSslStrictResume,
		ltmClientSslAllowNonssl
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmClientSslProfile MIB."
	::= { bigipLocalTMGroups 17 }

ltmClientSslStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmClientSslStatResetStats,
		ltmClientSslStatNumber,
		ltmClientSslStatName,
		ltmClientSslStatCurConns,
		ltmClientSslStatMaxConns,
		ltmClientSslStatCurNativeConns,
		ltmClientSslStatMaxNativeConns,
		ltmClientSslStatTotNativeConns,
		ltmClientSslStatCurCompatConns,
		ltmClientSslStatMaxCompatConns,
		ltmClientSslStatTotCompatConns,
		ltmClientSslStatEncryptedBytesIn,
		ltmClientSslStatEncryptedBytesOut,
		ltmClientSslStatDecryptedBytesIn,
		ltmClientSslStatDecryptedBytesOut,
		ltmClientSslStatRecordsIn,
		ltmClientSslStatRecordsOut,
		ltmClientSslStatFullyHwAcceleratedConns,
		ltmClientSslStatPartiallyHwAcceleratedConns,
		ltmClientSslStatNonHwAcceleratedConns,
		ltmClientSslStatPrematureDisconnects,
		ltmClientSslStatMidstreamRenegotiations,
		ltmClientSslStatSessCacheCurEntries,
		ltmClientSslStatSessCacheHits,
		ltmClientSslStatSessCacheLookups,
		ltmClientSslStatSessCacheOverflows,
		ltmClientSslStatSessCacheInvalidations,
		ltmClientSslStatPeercertValid,
		ltmClientSslStatPeercertInvalid,
		ltmClientSslStatPeercertNone,
		ltmClientSslStatHandshakeFailures,
		ltmClientSslStatBadRecords,
		ltmClientSslStatFatalAlerts,
		ltmClientSslStatSslv2,
		ltmClientSslStatSslv3,
		ltmClientSslStatTlsv1,
		ltmClientSslStatAdhKeyxchg,
		ltmClientSslStatDhDssKeyxchg,
		ltmClientSslStatDhRsaKeyxchg,
		ltmClientSslStatDssKeyxchg,
		ltmClientSslStatEdhDssKeyxchg,
		ltmClientSslStatRsaKeyxchg,
		ltmClientSslStatNullBulk,
		ltmClientSslStatAesBulk,
		ltmClientSslStatDesBulk,
		ltmClientSslStatIdeaBulk,
		ltmClientSslStatRc2Bulk,
		ltmClientSslStatRc4Bulk,
		ltmClientSslStatNullDigest,
		ltmClientSslStatMd5Digest,
		ltmClientSslStatShaDigest,
		ltmClientSslStatNotssl,
		ltmClientSslStatEdhRsaKeyxchg
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmClientSslProfileStat MIB."
	::= { bigipLocalTMGroups 18 }

ltmServerSslGroup OBJECT-GROUP
	 OBJECTS {
		ltmServerSslNumber,
		ltmServerSslName,
		ltmServerSslConfigSource,
		ltmServerSslDefaultName,
		ltmServerSslMode,
		ltmServerSslKey,
		ltmServerSslCert,
		ltmServerSslChain,
		ltmServerSslCafile,
		ltmServerSslCrlfile,
		ltmServerSslCiphers,
		ltmServerSslPassphrase,
		ltmServerSslOptions,
		ltmServerSslModsslmethods,
		ltmServerSslRenegotiatePeriod,
		ltmServerSslRenegotiateSize,
		ltmServerSslPeerCertMode,
		ltmServerSslAuthenticateOnce,
		ltmServerSslAuthenticateDepth,
		ltmServerSslAuthenticateName,
		ltmServerSslUncleanShutdown,
		ltmServerSslStrictResume,
		ltmServerSslHandshakeTimeout,
		ltmServerSslAlertTimeout,
		ltmServerSslCacheSize,
		ltmServerSslCacheTimeout
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmServerSslProfile MIB."
	::= { bigipLocalTMGroups 19 }

ltmServerSslStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmServerSslStatResetStats,
		ltmServerSslStatNumber,
		ltmServerSslStatName,
		ltmServerSslStatCurConns,
		ltmServerSslStatMaxConns,
		ltmServerSslStatCurNativeConns,
		ltmServerSslStatMaxNativeConns,
		ltmServerSslStatTotNativeConns,
		ltmServerSslStatCurCompatConns,
		ltmServerSslStatMaxCompatConns,
		ltmServerSslStatTotCompatConns,
		ltmServerSslStatEncryptedBytesIn,
		ltmServerSslStatEncryptedBytesOut,
		ltmServerSslStatDecryptedBytesIn,
		ltmServerSslStatDecryptedBytesOut,
		ltmServerSslStatRecordsIn,
		ltmServerSslStatRecordsOut,
		ltmServerSslStatFullyHwAcceleratedConns,
		ltmServerSslStatPartiallyHwAcceleratedConns,
		ltmServerSslStatNonHwAcceleratedConns,
		ltmServerSslStatPrematureDisconnects,
		ltmServerSslStatMidstreamRenegotiations,
		ltmServerSslStatSessCacheCurEntries,
		ltmServerSslStatSessCacheHits,
		ltmServerSslStatSessCacheLookups,
		ltmServerSslStatSessCacheOverflows,
		ltmServerSslStatSessCacheInvalidations,
		ltmServerSslStatPeercertValid,
		ltmServerSslStatPeercertInvalid,
		ltmServerSslStatPeercertNone,
		ltmServerSslStatHandshakeFailures,
		ltmServerSslStatBadRecords,
		ltmServerSslStatFatalAlerts,
		ltmServerSslStatSslv2,
		ltmServerSslStatSslv3,
		ltmServerSslStatTlsv1,
		ltmServerSslStatAdhKeyxchg,
		ltmServerSslStatDhDssKeyxchg,
		ltmServerSslStatDhRsaKeyxchg,
		ltmServerSslStatDssKeyxchg,
		ltmServerSslStatEdhDssKeyxchg,
		ltmServerSslStatRsaKeyxchg,
		ltmServerSslStatNullBulk,
		ltmServerSslStatAesBulk,
		ltmServerSslStatDesBulk,
		ltmServerSslStatIdeaBulk,
		ltmServerSslStatRc2Bulk,
		ltmServerSslStatRc4Bulk,
		ltmServerSslStatNullDigest,
		ltmServerSslStatMd5Digest,
		ltmServerSslStatShaDigest,
		ltmServerSslStatNotssl,
		ltmServerSslStatEdhRsaKeyxchg
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmServerSslProfileStat MIB."
	::= { bigipLocalTMGroups 20 }

ltmConnPoolProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmConnPoolProfileNumber,
		ltmConnPoolProfileName,
		ltmConnPoolProfileConfigSource,
		ltmConnPoolProfileDefaultName,
		ltmConnPoolProfileSrcMaskType,
		ltmConnPoolProfileSrcMask,
		ltmConnPoolProfileMaxSize,
		ltmConnPoolProfileMaxAge,
		ltmConnPoolProfileMaxReuse,
		ltmConnPoolProfileIdleTimeout
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmConnPoolProfile MIB."
	::= { bigipLocalTMGroups 21 }

ltmConnPoolProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmConnPoolProfileStatResetStats,
		ltmConnPoolProfileStatNumber,
		ltmConnPoolProfileStatName,
		ltmConnPoolProfileStatCurSize,
		ltmConnPoolProfileStatMaxSize,
		ltmConnPoolProfileStatReuses,
		ltmConnPoolProfileStatConnects
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmConnPoolProfileStat MIB."
	::= { bigipLocalTMGroups 22 }

ltmFastL4ProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmFastL4ProfileNumber,
		ltmFastL4ProfileName,
		ltmFastL4ProfileConfigSource,
		ltmFastL4ProfileDefaultName,
		ltmFastL4ProfileResetOnTimeout,
		ltmFastL4ProfileIpFragReass,
		ltmFastL4ProfileIdleTimeout,
		ltmFastL4ProfileTcpHandshakeTimeout,
		ltmFastL4ProfileMssOverride,
		ltmFastL4ProfilePvaAccelMode,
		ltmFastL4ProfileTcpTimestampMode,
		ltmFastL4ProfileTcpWscaleMode,
		ltmFastL4ProfileTcpGenerateIsn,
		ltmFastL4ProfileTcpStripSack,
		ltmFastL4ProfileIpTosToClient,
		ltmFastL4ProfileIpTosToServer,
		ltmFastL4ProfileLinkQosToClient,
		ltmFastL4ProfileLinkQosToServer,
		ltmFastL4ProfileRttFromClient,
		ltmFastL4ProfileRttFromServer,
		ltmFastL4ProfileTcpCloseTimeout,
		ltmFastL4ProfileLooseInitiation,
		ltmFastL4ProfileLooseClose,
		ltmFastL4ProfileHardSyncookie,
		ltmFastL4ProfileSoftSyncookie
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmFastL4Profile MIB."
	::= { bigipLocalTMGroups 23 }

ltmFtpProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmFtpProfileNumber,
		ltmFtpProfileName,
		ltmFtpProfileConfigSource,
		ltmFtpProfileDefaultName,
		ltmFtpProfileTranslateExtended,
		ltmFtpProfileDataPort
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmFtpProfile MIB."
	::= { bigipLocalTMGroups 24 }

ltmHttpProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpProfileNumber,
		ltmHttpProfileName,
		ltmHttpProfileConfigSource,
		ltmHttpProfileDefaultName,
		ltmHttpProfileBasicAuthRealm,
		ltmHttpProfileOneConnect,
		ltmHttpProfileHeaderInsert,
		ltmHttpProfileHeaderErase,
		ltmHttpProfileFallbackHost,
		ltmHttpProfileCompressMode,
		ltmHttpProfileCompressMinSize,
		ltmHttpProfileCompressBufferSize,
		ltmHttpProfileCompressVaryHeader,
		ltmHttpProfileCompressAllowHttp10,
		ltmHttpProfileCompressGzipMemlevel,
		ltmHttpProfileCompressGzipWindowsize,
		ltmHttpProfileCompressGzipLevel,
		ltmHttpProfileCompressKeepAcceptEncoding,
		ltmHttpProfileCompressBrowserWorkarounds,
		ltmHttpProfileResponseChunking,
		ltmHttpProfileLwsMaxColumn,
		ltmHttpProfileLwsSeparator,
		ltmHttpProfileRedirectRewrite,
		ltmHttpProfileMaxHeaderSize,
		ltmHttpProfilePipelining,
		ltmHttpProfileInsertXforwardedFor,
		ltmHttpProfileMaxRequests,
		ltmHttpProfileCompressCpusaver,
		ltmHttpProfileCompressCpusaverHigh,
		ltmHttpProfileCompressCpusaverLow,
		ltmHttpProfileRamcache,
		ltmHttpProfileRamcacheSize,
		ltmHttpProfileRamcacheMaxEntries,
		ltmHttpProfileRamcacheMaxAge,
		ltmHttpProfileRamcacheObjectMinSize,
		ltmHttpProfileRamcacheObjectMaxSize,
		ltmHttpProfileRamcacheIgnoreClient,
		ltmHttpProfileRamcacheAgingRate,
		ltmHttpProfileRamcacheInsertAgeHeader,
		ltmHttpProfileCompressPreferredMethod
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfile MIB."
	::= { bigipLocalTMGroups 25 }

ltmCompUriInclGroup OBJECT-GROUP
	 OBJECTS {
		ltmCompUriInclNumber,
		ltmCompUriInclName,
		ltmCompUriInclIndex,
		ltmCompUriInclUri
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileCompUriIncl MIB."
	::= { bigipLocalTMGroups 26 }

ltmCompUriExclGroup OBJECT-GROUP
	 OBJECTS {
		ltmCompUriExclNumber,
		ltmCompUriExclName,
		ltmCompUriExclIndex,
		ltmCompUriExclUri
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileCompUriExcl MIB."
	::= { bigipLocalTMGroups 27 }

ltmCompContTypeInclGroup OBJECT-GROUP
	 OBJECTS {
		ltmCompContTypeInclNumber,
		ltmCompContTypeInclName,
		ltmCompContTypeInclIndex,
		ltmCompContTypeInclContentType
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileCompContTypeIncl MIB."
	::= { bigipLocalTMGroups 28 }

ltmCompContTypeExclGroup OBJECT-GROUP
	 OBJECTS {
		ltmCompContTypeExclNumber,
		ltmCompContTypeExclName,
		ltmCompContTypeExclIndex,
		ltmCompContTypeExclContentType
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileCompContTypeExcl MIB."
	::= { bigipLocalTMGroups 29 }

ltmHttpProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpProfileStatResetStats,
		ltmHttpProfileStatNumber,
		ltmHttpProfileStatName,
		ltmHttpProfileStatCookiePersistInserts,
		ltmHttpProfileStatResp2xxCnt,
		ltmHttpProfileStatResp3xxCnt,
		ltmHttpProfileStatResp4xxCnt,
		ltmHttpProfileStatResp5xxCnt,
		ltmHttpProfileStatNumberReqs,
		ltmHttpProfileStatGetReqs,
		ltmHttpProfileStatPostReqs,
		ltmHttpProfileStatV9Reqs,
		ltmHttpProfileStatV10Reqs,
		ltmHttpProfileStatV11Reqs,
		ltmHttpProfileStatV9Resp,
		ltmHttpProfileStatV10Resp,
		ltmHttpProfileStatV11Resp,
		ltmHttpProfileStatMaxKeepaliveReq,
		ltmHttpProfileStatRespBucket1k,
		ltmHttpProfileStatRespBucket4k,
		ltmHttpProfileStatRespBucket16k,
		ltmHttpProfileStatRespBucket32k,
		ltmHttpProfileStatPrecompressBytes,
		ltmHttpProfileStatPostcompressBytes,
		ltmHttpProfileStatNullCompressBytes,
		ltmHttpProfileStatHtmlPrecompressBytes,
		ltmHttpProfileStatHtmlPostcompressBytes,
		ltmHttpProfileStatCssPrecompressBytes,
		ltmHttpProfileStatCssPostcompressBytes,
		ltmHttpProfileStatJsPrecompressBytes,
		ltmHttpProfileStatJsPostcompressBytes,
		ltmHttpProfileStatXmlPrecompressBytes,
		ltmHttpProfileStatXmlPostcompressBytes,
		ltmHttpProfileStatSgmlPrecompressBytes,
		ltmHttpProfileStatSgmlPostcompressBytes,
		ltmHttpProfileStatPlainPrecompressBytes,
		ltmHttpProfileStatPlainPostcompressBytes,
		ltmHttpProfileStatOctetPrecompressBytes,
		ltmHttpProfileStatOctetPostcompressBytes,
		ltmHttpProfileStatImagePrecompressBytes,
		ltmHttpProfileStatImagePostcompressBytes,
		ltmHttpProfileStatVideoPrecompressBytes,
		ltmHttpProfileStatVideoPostcompressBytes,
		ltmHttpProfileStatAudioPrecompressBytes,
		ltmHttpProfileStatAudioPostcompressBytes,
		ltmHttpProfileStatOtherPrecompressBytes,
		ltmHttpProfileStatOtherPostcompressBytes,
		ltmHttpProfileStatRamcacheHits,
		ltmHttpProfileStatRamcacheMisses,
		ltmHttpProfileStatRamcacheMissesAll,
		ltmHttpProfileStatRamcacheHitBytes,
		ltmHttpProfileStatRamcacheMissBytes,
		ltmHttpProfileStatRamcacheMissBytesAll,
		ltmHttpProfileStatRamcacheSize,
		ltmHttpProfileStatRamcacheCount,
		ltmHttpProfileStatRamcacheEvictions,
		ltmHttpProfileStatRespBucket64k
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileStat MIB."
	::= { bigipLocalTMGroups 30 }

ltmPersistProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmPersistProfileNumber,
		ltmPersistProfileName,
		ltmPersistProfileConfigSource,
		ltmPersistProfileDefaultName,
		ltmPersistProfileMode,
		ltmPersistProfileMirror,
		ltmPersistProfileTimeout,
		ltmPersistProfileMaskType,
		ltmPersistProfileMask,
		ltmPersistProfileCookieMethod,
		ltmPersistProfileCookieName,
		ltmPersistProfileCookieExpiration,
		ltmPersistProfileCookieHashOffset,
		ltmPersistProfileCookieHashLength,
		ltmPersistProfileMsrdpNoSessionDir,
		ltmPersistProfileMapProxies,
		ltmPersistProfileAcrossServices,
		ltmPersistProfileAcrossVirtuals,
		ltmPersistProfileAcrossPools,
		ltmPersistProfileUieRule,
		ltmPersistProfileSipInfo
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmPersistProfile MIB."
	::= { bigipLocalTMGroups 31 }

ltmStreamProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmStreamProfileNumber,
		ltmStreamProfileName,
		ltmStreamProfileConfigSource,
		ltmStreamProfileDefaultName,
		ltmStreamProfileSource,
		ltmStreamProfileTarget
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmStreamProfile MIB."
	::= { bigipLocalTMGroups 32 }

ltmStreamProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmStreamProfileStatResetStats,
		ltmStreamProfileStatNumber,
		ltmStreamProfileStatName,
		ltmStreamProfileStatReplaces
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmStreamProfileStat MIB."
	::= { bigipLocalTMGroups 33 }

ltmTcpProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmTcpProfileNumber,
		ltmTcpProfileName,
		ltmTcpProfileConfigSource,
		ltmTcpProfileDefaultName,
		ltmTcpProfileResetOnTimeout,
		ltmTcpProfileTimeWaitRecycle,
		ltmTcpProfileDelayedAcks,
		ltmTcpProfileProxyMss,
		ltmTcpProfileProxyOptions,
		ltmTcpProfileProxyBufferLow,
		ltmTcpProfileProxyBufferHigh,
		ltmTcpProfileIdleTimeout,
		ltmTcpProfileTimeWaitTimeout,
		ltmTcpProfileFinWaitTimeout,
		ltmTcpProfileCloseWaitTimeout,
		ltmTcpProfileSndbuf,
		ltmTcpProfileRcvwnd,
		ltmTcpProfileKeepAliveInterval,
		ltmTcpProfileSynMaxrtx,
		ltmTcpProfileMaxrtx,
		ltmTcpProfileIpTosToClient,
		ltmTcpProfileLinkQosToClient,
		ltmTcpProfileDeferredAccept,
		ltmTcpProfileSelectiveAcks,
		ltmTcpProfileEcn,
		ltmTcpProfileLimitedTransmit,
		ltmTcpProfileHighPerfTcpExt,
		ltmTcpProfileSlowStart,
		ltmTcpProfileBandwidthDelay,
		ltmTcpProfileNagle,
		ltmTcpProfileAckOnPush,
		ltmTcpProfileMd5Sig,
		ltmTcpProfileMd5SigPass,
		ltmTcpProfileAbc,
		ltmTcpProfileCongestionCtrl,
		ltmTcpProfileDsack,
		ltmTcpProfileCmetricsCache,
		ltmTcpProfileVerifiedAccept,
		ltmTcpProfilePktLossIgnoreRate,
		ltmTcpProfilePktLossIgnoreBurst,
		ltmTcpProfileZeroWindowTimeout
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmTcpProfile MIB."
	::= { bigipLocalTMGroups 34 }

ltmTcpProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmTcpProfileStatResetStats,
		ltmTcpProfileStatNumber,
		ltmTcpProfileStatName,
		ltmTcpProfileStatOpen,
		ltmTcpProfileStatCloseWait,
		ltmTcpProfileStatFinWait,
		ltmTcpProfileStatTimeWait,
		ltmTcpProfileStatAccepts,
		ltmTcpProfileStatAcceptfails,
		ltmTcpProfileStatConnects,
		ltmTcpProfileStatConnfails,
		ltmTcpProfileStatExpires,
		ltmTcpProfileStatAbandons,
		ltmTcpProfileStatRxrst,
		ltmTcpProfileStatRxbadsum,
		ltmTcpProfileStatRxbadseg,
		ltmTcpProfileStatRxooseg,
		ltmTcpProfileStatRxcookie,
		ltmTcpProfileStatRxbadcookie,
		ltmTcpProfileStatSyncacheover,
		ltmTcpProfileStatTxrexmits
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmTcpProfileStat MIB."
	::= { bigipLocalTMGroups 35 }

ltmUdpProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmUdpProfileNumber,
		ltmUdpProfileName,
		ltmUdpProfileConfigSource,
		ltmUdpProfileDefaultName,
		ltmUdpProfileIdleTimeout,
		ltmUdpProfileIpTosToClient,
		ltmUdpProfileLinkQosToClient,
		ltmUdpProfileDatagramLb,
		ltmUdpProfileAllowNoPayload
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmUdpProfile MIB."
	::= { bigipLocalTMGroups 36 }

ltmUdpProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmUdpProfileStatResetStats,
		ltmUdpProfileStatNumber,
		ltmUdpProfileStatName,
		ltmUdpProfileStatOpen,
		ltmUdpProfileStatAccepts,
		ltmUdpProfileStatAcceptfails,
		ltmUdpProfileStatConnects,
		ltmUdpProfileStatConnfails,
		ltmUdpProfileStatExpires,
		ltmUdpProfileStatRxdgram,
		ltmUdpProfileStatRxbaddgram,
		ltmUdpProfileStatRxunreach,
		ltmUdpProfileStatRxbadsum,
		ltmUdpProfileStatRxnosum,
		ltmUdpProfileStatTxdgram
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmUdpProfileStat MIB."
	::= { bigipLocalTMGroups 37 }

ltmRuleGroup OBJECT-GROUP
	 OBJECTS {
		ltmRuleNumber,
		ltmRuleName,
		ltmRuleDefinition,
		ltmRuleConfigSource
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmRule MIB."
	::= { bigipLocalTMGroups 38 }

ltmRuleEventGroup OBJECT-GROUP
	 OBJECTS {
		ltmRuleEventNumber,
		ltmRuleEventName,
		ltmRuleEventEventType,
		ltmRuleEventPriority,
		ltmRuleEventScript
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmRuleEvent MIB."
	::= { bigipLocalTMGroups 39 }

ltmRuleEventStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmRuleEventStatResetStats,
		ltmRuleEventStatNumber,
		ltmRuleEventStatName,
		ltmRuleEventStatEventType,
		ltmRuleEventStatPriority,
		ltmRuleEventStatFailures,
		ltmRuleEventStatAborts,
		ltmRuleEventStatTotalExecutions,
		ltmRuleEventStatAvgCycles,
		ltmRuleEventStatMaxCycles,
		ltmRuleEventStatMinCycles
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmRuleEventStat MIB."
	::= { bigipLocalTMGroups 40 }

ltmSnatGroup OBJECT-GROUP
	 OBJECTS {
		ltmSnatNumber,
		ltmSnatName,
		ltmSnatSfFlags,
		ltmSnatType,
		ltmSnatTransAddrType,
		ltmSnatTransAddr,
		ltmSnatSnatpoolName,
		ltmSnatListedEnabledVlans
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSnat MIB."
	::= { bigipLocalTMGroups 41 }

ltmSnatStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmSnatStatResetStats,
		ltmSnatStatNumber,
		ltmSnatStatName,
		ltmSnatStatClientPktsIn,
		ltmSnatStatClientBytesIn,
		ltmSnatStatClientPktsOut,
		ltmSnatStatClientBytesOut,
		ltmSnatStatClientMaxConns,
		ltmSnatStatClientTotConns,
		ltmSnatStatClientCurConns
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSnatStat MIB."
	::= { bigipLocalTMGroups 42 }

ltmSnatVlanGroup OBJECT-GROUP
	 OBJECTS {
		ltmSnatVlanNumber,
		ltmSnatVlanSnatName,
		ltmSnatVlanVlanName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSnatVlan MIB."
	::= { bigipLocalTMGroups 43 }

ltmSnatOrigAddrGroup OBJECT-GROUP
	 OBJECTS {
		ltmSnatOrigAddrNumber,
		ltmSnatOrigAddrSnatName,
		ltmSnatOrigAddrAddrType,
		ltmSnatOrigAddrAddr,
		ltmSnatOrigAddrWildmaskType,
		ltmSnatOrigAddrWildmask
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSnatOrigAddr MIB."
	::= { bigipLocalTMGroups 44 }

ltmTransAddrGroup OBJECT-GROUP
	 OBJECTS {
		ltmTransAddrNumber,
		ltmTransAddrAddrType,
		ltmTransAddrAddr,
		ltmTransAddrEnabled,
		ltmTransAddrConnLimit,
		ltmTransAddrTcpIdleTimeout,
		ltmTransAddrUdpIdleTimeout,
		ltmTransAddrIpIdleTimeout,
		ltmTransAddrArpEnabled,
		ltmTransAddrUnitId
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmTransAddr MIB."
	::= { bigipLocalTMGroups 45 }

ltmTransAddrStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmTransAddrStatResetStats,
		ltmTransAddrStatNumber,
		ltmTransAddrStatAddrType,
		ltmTransAddrStatAddr,
		ltmTransAddrStatServerPktsIn,
		ltmTransAddrStatServerBytesIn,
		ltmTransAddrStatServerPktsOut,
		ltmTransAddrStatServerBytesOut,
		ltmTransAddrStatServerMaxConns,
		ltmTransAddrStatServerTotConns,
		ltmTransAddrStatServerCurConns
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmTransAddrStat MIB."
	::= { bigipLocalTMGroups 46 }

ltmSnatPoolGroup OBJECT-GROUP
	 OBJECTS {
		ltmSnatPoolNumber,
		ltmSnatPoolName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSnatPool MIB."
	::= { bigipLocalTMGroups 47 }

ltmSnatPoolStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmSnatPoolStatResetStats,
		ltmSnatPoolStatNumber,
		ltmSnatPoolStatName,
		ltmSnatPoolStatServerPktsIn,
		ltmSnatPoolStatServerBytesIn,
		ltmSnatPoolStatServerPktsOut,
		ltmSnatPoolStatServerBytesOut,
		ltmSnatPoolStatServerMaxConns,
		ltmSnatPoolStatServerTotConns,
		ltmSnatPoolStatServerCurConns
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSnatPoolStat MIB."
	::= { bigipLocalTMGroups 48 }

ltmSnatpoolTransAddrGroup OBJECT-GROUP
	 OBJECTS {
		ltmSnatpoolTransAddrNumber,
		ltmSnatpoolTransAddrSnatpoolName,
		ltmSnatpoolTransAddrTransAddrType,
		ltmSnatpoolTransAddrTransAddr
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSnatpoolTransAddr MIB."
	::= { bigipLocalTMGroups 49 }

ltmVirtualServGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServNumber,
		ltmVirtualServName,
		ltmVirtualServAddrType,
		ltmVirtualServAddr,
		ltmVirtualServWildmaskType,
		ltmVirtualServWildmask,
		ltmVirtualServPort,
		ltmVirtualServIpProto,
		ltmVirtualServListedEnabledVlans,
		ltmVirtualServEnabled,
		ltmVirtualServConnLimit,
		ltmVirtualServRclass,
		ltmVirtualServSfFlags,
		ltmVirtualServTranslateAddr,
		ltmVirtualServTranslatePort,
		ltmVirtualServType,
		ltmVirtualServSnatType,
		ltmVirtualServLasthopPoolName,
		ltmVirtualServSnatpoolName,
		ltmVirtualServDefaultPool,
		ltmVirtualServFallbackPersist,
		ltmVirtualServActualPvaAccel,
		ltmVirtualServAvailabilityState,
		ltmVirtualServEnabledState,
		ltmVirtualServDisabledParentType,
		ltmVirtualServStatusReason,
		ltmVirtualServGtmScore,
		ltmVirtualServCmpEnabled
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServ MIB."
	::= { bigipLocalTMGroups 50 }

ltmVirtualServStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServStatResetStats,
		ltmVirtualServStatNumber,
		ltmVirtualServStatName,
		ltmVirtualServStatCsMinConnDur,
		ltmVirtualServStatCsMaxConnDur,
		ltmVirtualServStatCsMeanConnDur,
		ltmVirtualServStatNoNodesErrors,
		ltmVirtualServStatClientPktsIn,
		ltmVirtualServStatClientBytesIn,
		ltmVirtualServStatClientPktsOut,
		ltmVirtualServStatClientBytesOut,
		ltmVirtualServStatClientMaxConns,
		ltmVirtualServStatClientTotConns,
		ltmVirtualServStatClientCurConns,
		ltmVirtualServStatEphemeralPktsIn,
		ltmVirtualServStatEphemeralBytesIn,
		ltmVirtualServStatEphemeralPktsOut,
		ltmVirtualServStatEphemeralBytesOut,
		ltmVirtualServStatEphemeralMaxConns,
		ltmVirtualServStatEphemeralTotConns,
		ltmVirtualServStatEphemeralCurConns,
		ltmVirtualServStatPvaPktsIn,
		ltmVirtualServStatPvaBytesIn,
		ltmVirtualServStatPvaPktsOut,
		ltmVirtualServStatPvaBytesOut,
		ltmVirtualServStatPvaMaxConns,
		ltmVirtualServStatPvaTotConns,
		ltmVirtualServStatPvaCurConns,
		ltmVirtualServStatTotRequests,
		ltmVirtualServStatTotPvaAssistConn,
		ltmVirtualServStatCurrPvaAssistConn
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServStat MIB."
	::= { bigipLocalTMGroups 51 }

ltmVirtualServAuthGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServAuthNumber,
		ltmVirtualServAuthVsName,
		ltmVirtualServAuthProfileName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServAuth MIB."
	::= { bigipLocalTMGroups 52 }

ltmVirtualServPersistGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServPersistNumber,
		ltmVirtualServPersistVsName,
		ltmVirtualServPersistProfileName,
		ltmVirtualServPersistUseDefault
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServPersist MIB."
	::= { bigipLocalTMGroups 53 }

ltmVirtualServProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServProfileNumber,
		ltmVirtualServProfileVsName,
		ltmVirtualServProfileProfileName,
		ltmVirtualServProfileType,
		ltmVirtualServProfileContext
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServProfile MIB."
	::= { bigipLocalTMGroups 54 }

ltmVirtualServPoolGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServPoolNumber,
		ltmVirtualServPoolVirtualServerName,
		ltmVirtualServPoolPoolName,
		ltmVirtualServPoolRuleName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServPool MIB."
	::= { bigipLocalTMGroups 55 }

ltmVirtualServClonePoolGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServClonePoolNumber,
		ltmVirtualServClonePoolVirtualServerName,
		ltmVirtualServClonePoolPoolName,
		ltmVirtualServClonePoolType
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServClonePool MIB."
	::= { bigipLocalTMGroups 56 }

ltmVirtualServRuleGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServRuleNumber,
		ltmVirtualServRuleVirtualServerName,
		ltmVirtualServRuleRuleName,
		ltmVirtualServRulePriority
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServRule MIB."
	::= { bigipLocalTMGroups 57 }

ltmVirtualServVlanGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualServVlanNumber,
		ltmVirtualServVlanVsName,
		ltmVirtualServVlanVlanName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServVlan MIB."
	::= { bigipLocalTMGroups 58 }

ltmVirtualAddrGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualAddrNumber,
		ltmVirtualAddrAddrType,
		ltmVirtualAddrAddr,
		ltmVirtualAddrEnabled,
		ltmVirtualAddrConnLimit,
		ltmVirtualAddrArpEnabled,
		ltmVirtualAddrSfFlags,
		ltmVirtualAddrUnitId,
		ltmVirtualAddrRouteAdvertisement,
		ltmVirtualAddrAvailabilityState,
		ltmVirtualAddrEnabledState,
		ltmVirtualAddrDisabledParentType,
		ltmVirtualAddrStatusReason,
		ltmVirtualAddrServer,
		ltmVirtualAddrIsFloat
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualAddr MIB."
	::= { bigipLocalTMGroups 59 }

ltmVirtualAddrStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualAddrStatResetStats,
		ltmVirtualAddrStatNumber,
		ltmVirtualAddrStatAddrType,
		ltmVirtualAddrStatAddr,
		ltmVirtualAddrStatClientPktsIn,
		ltmVirtualAddrStatClientBytesIn,
		ltmVirtualAddrStatClientPktsOut,
		ltmVirtualAddrStatClientBytesOut,
		ltmVirtualAddrStatClientMaxConns,
		ltmVirtualAddrStatClientTotConns,
		ltmVirtualAddrStatClientCurConns,
		ltmVirtualAddrStatPvaPktsIn,
		ltmVirtualAddrStatPvaBytesIn,
		ltmVirtualAddrStatPvaPktsOut,
		ltmVirtualAddrStatPvaBytesOut,
		ltmVirtualAddrStatPvaMaxConns,
		ltmVirtualAddrStatPvaTotConns,
		ltmVirtualAddrStatPvaCurConns,
		ltmVirtualAddrStatTotPvaAssistConn,
		ltmVirtualAddrStatCurrPvaAssistConn
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualAddrStat MIB."
	::= { bigipLocalTMGroups 60 }

ltmFastHttpProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmFastHttpProfileNumber,
		ltmFastHttpProfileName,
		ltmFastHttpProfileConfigSource,
		ltmFastHttpProfileDefaultName,
		ltmFastHttpProfileResetOnTimeout,
		ltmFastHttpProfileIdleTimeout,
		ltmFastHttpProfileMssOverride,
		ltmFastHttpProfileClientCloseTimeout,
		ltmFastHttpProfileServerCloseTimeout,
		ltmFastHttpProfileConnpoolMaxSize,
		ltmFastHttpProfileConnpoolMinSize,
		ltmFastHttpProfileConnpoolStep,
		ltmFastHttpProfileConnpoolMaxReuse,
		ltmFastHttpProfileConnpoolIdleTimeout,
		ltmFastHttpProfileMaxHeaderSize,
		ltmFastHttpProfileMaxRequests,
		ltmFastHttpProfileInsertXforwardedFor,
		ltmFastHttpProfileHttp11CloseWorkarounds,
		ltmFastHttpProfileHeaderInsert,
		ltmFastHttpProfileUncleanShutdown,
		ltmFastHttpProfileForceHttp10Response,
		ltmFastHttpProfileLayer7,
		ltmFastHttpProfileConnpoolReplenish
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmFastHttpProfile MIB."
	::= { bigipLocalTMGroups 61 }

ltmFastHttpProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmFastHttpProfileStatResetStats,
		ltmFastHttpProfileStatNumber,
		ltmFastHttpProfileStatName,
		ltmFastHttpProfileStatClientSyns,
		ltmFastHttpProfileStatClientAccepts,
		ltmFastHttpProfileStatServerConnects,
		ltmFastHttpProfileStatConnpoolCurSize,
		ltmFastHttpProfileStatConnpoolMaxSize,
		ltmFastHttpProfileStatConnpoolReuses,
		ltmFastHttpProfileStatConnpoolExhausted,
		ltmFastHttpProfileStatNumberReqs,
		ltmFastHttpProfileStatUnbufferedReqs,
		ltmFastHttpProfileStatGetReqs,
		ltmFastHttpProfileStatPostReqs,
		ltmFastHttpProfileStatV9Reqs,
		ltmFastHttpProfileStatV10Reqs,
		ltmFastHttpProfileStatV11Reqs,
		ltmFastHttpProfileStatResp2xxCnt,
		ltmFastHttpProfileStatResp3xxCnt,
		ltmFastHttpProfileStatResp4xxCnt,
		ltmFastHttpProfileStatResp5xxCnt,
		ltmFastHttpProfileStatReqParseErrors,
		ltmFastHttpProfileStatRespParseErrors,
		ltmFastHttpProfileStatClientRxBad,
		ltmFastHttpProfileStatServerRxBad,
		ltmFastHttpProfileStatPipelinedReqs
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmFastHttpProfileStat MIB."
	::= { bigipLocalTMGroups 62 }

ltmXmlProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmXmlProfileNumber,
		ltmXmlProfileName,
		ltmXmlProfileConfigSource,
		ltmXmlProfileDefaultName,
		ltmXmlProfileAbortOnError,
		ltmXmlProfileMaxBufferSize
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmXmlProfile MIB."
	::= { bigipLocalTMGroups 63 }

ltmXmlProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmXmlProfileStatResetStats,
		ltmXmlProfileStatNumber,
		ltmXmlProfileStatName,
		ltmXmlProfileStatNumErrors,
		ltmXmlProfileStatNumInspectedDocuments,
		ltmXmlProfileStatNumDocumentsWithOneMatch,
		ltmXmlProfileStatNumDocumentsWithTwoMatches,
		ltmXmlProfileStatNumDocumentsWithThreeMatches,
		ltmXmlProfileStatNumDocumentsWithNoMatches,
		ltmXmlProfileStatNumMalformedDocuments
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmXmlProfileStat MIB."
	::= { bigipLocalTMGroups 64 }

ltmRamUriExclGroup OBJECT-GROUP
	 OBJECTS {
		ltmRamUriExclNumber,
		ltmRamUriExclName,
		ltmRamUriExclIndex,
		ltmRamUriExclUri
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileRamUriExcl MIB."
	::= { bigipLocalTMGroups 65 }

ltmRamUriInclGroup OBJECT-GROUP
	 OBJECTS {
		ltmRamUriInclNumber,
		ltmRamUriInclName,
		ltmRamUriInclIndex,
		ltmRamUriInclUri
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileRamUriIncl MIB."
	::= { bigipLocalTMGroups 66 }

ltmRamUriPinGroup OBJECT-GROUP
	 OBJECTS {
		ltmRamUriPinNumber,
		ltmRamUriPinName,
		ltmRamUriPinIndex,
		ltmRamUriPinUri
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileRamUriPin MIB."
	::= { bigipLocalTMGroups 67 }

ltmDnsProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmDnsProfileNumber,
		ltmDnsProfileName,
		ltmDnsProfileConfigSource,
		ltmDnsProfileDefaultName,
		ltmDnsProfileGtmEnabled
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmDnsProfile MIB."
	::= { bigipLocalTMGroups 68 }

ltmHttpClassGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpClassNumber,
		ltmHttpClassName,
		ltmHttpClassConfigSource,
		ltmHttpClassDefaultName,
		ltmHttpClassPoolName,
		ltmHttpClassAsmEnabled,
		ltmHttpClassWaEnabled,
		ltmHttpClassRedirectLocation,
		ltmHttpClassUrlRewrite
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpClassProfile MIB."
	::= { bigipLocalTMGroups 69 }

ltmHttpClassHostGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpClassHostNumber,
		ltmHttpClassHostName,
		ltmHttpClassHostIndex,
		ltmHttpClassHostString
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpClassProfileHost MIB."
	::= { bigipLocalTMGroups 70 }

ltmHttpClassUriGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpClassUriNumber,
		ltmHttpClassUriName,
		ltmHttpClassUriIndex,
		ltmHttpClassUriString
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpClassProfileUri MIB."
	::= { bigipLocalTMGroups 71 }

ltmHttpClassHeadGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpClassHeadNumber,
		ltmHttpClassHeadName,
		ltmHttpClassHeadIndex,
		ltmHttpClassHeadString
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpClassProfileHead MIB."
	::= { bigipLocalTMGroups 72 }

ltmHttpClassCookGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpClassCookNumber,
		ltmHttpClassCookName,
		ltmHttpClassCookIndex,
		ltmHttpClassCookString
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpClassProfileCook MIB."
	::= { bigipLocalTMGroups 73 }

ltmHttpClassStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmHttpClassStatResetStats,
		ltmHttpClassStatNumber,
		ltmHttpClassStatName,
		ltmHttpClassStatCookiePersistInserts,
		ltmHttpClassStatResp2xxCnt,
		ltmHttpClassStatResp3xxCnt,
		ltmHttpClassStatResp4xxCnt,
		ltmHttpClassStatResp5xxCnt,
		ltmHttpClassStatNumberReqs,
		ltmHttpClassStatGetReqs,
		ltmHttpClassStatPostReqs,
		ltmHttpClassStatV9Reqs,
		ltmHttpClassStatV10Reqs,
		ltmHttpClassStatV11Reqs,
		ltmHttpClassStatV9Resp,
		ltmHttpClassStatV10Resp,
		ltmHttpClassStatV11Resp,
		ltmHttpClassStatMaxKeepaliveReq,
		ltmHttpClassStatRespBucket1k,
		ltmHttpClassStatRespBucket4k,
		ltmHttpClassStatRespBucket16k,
		ltmHttpClassStatRespBucket32k,
		ltmHttpClassStatRespBucket64k,
		ltmHttpClassStatPrecompressBytes,
		ltmHttpClassStatPostcompressBytes,
		ltmHttpClassStatNullCompressBytes,
		ltmHttpClassStatHtmlPrecompressBytes,
		ltmHttpClassStatHtmlPostcompressBytes,
		ltmHttpClassStatCssPrecompressBytes,
		ltmHttpClassStatCssPostcompressBytes,
		ltmHttpClassStatJsPrecompressBytes,
		ltmHttpClassStatJsPostcompressBytes,
		ltmHttpClassStatXmlPrecompressBytes,
		ltmHttpClassStatXmlPostcompressBytes,
		ltmHttpClassStatSgmlPrecompressBytes,
		ltmHttpClassStatSgmlPostcompressBytes,
		ltmHttpClassStatPlainPrecompressBytes,
		ltmHttpClassStatPlainPostcompressBytes,
		ltmHttpClassStatOctetPrecompressBytes,
		ltmHttpClassStatOctetPostcompressBytes,
		ltmHttpClassStatImagePrecompressBytes,
		ltmHttpClassStatImagePostcompressBytes,
		ltmHttpClassStatVideoPrecompressBytes,
		ltmHttpClassStatVideoPostcompressBytes,
		ltmHttpClassStatAudioPrecompressBytes,
		ltmHttpClassStatAudioPostcompressBytes,
		ltmHttpClassStatOtherPrecompressBytes,
		ltmHttpClassStatOtherPostcompressBytes,
		ltmHttpClassStatRamcacheHits,
		ltmHttpClassStatRamcacheMisses,
		ltmHttpClassStatRamcacheMissesAll,
		ltmHttpClassStatRamcacheHitBytes,
		ltmHttpClassStatRamcacheMissBytes,
		ltmHttpClassStatRamcacheMissBytesAll
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpClassProfileStat MIB."
	::= { bigipLocalTMGroups 74 }

ltmIiopProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmIiopProfileNumber,
		ltmIiopProfileName,
		ltmIiopProfileConfigSource,
		ltmIiopProfileDefaultName,
		ltmIiopProfilePersistRequestId,
		ltmIiopProfilePersistObjectKey,
		ltmIiopProfileAbortOnTimeout,
		ltmIiopProfileTimeout
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmIiopProfile MIB."
	::= { bigipLocalTMGroups 75 }

ltmIiopProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmIiopProfileStatResetStats,
		ltmIiopProfileStatNumber,
		ltmIiopProfileStatName,
		ltmIiopProfileStatNumRequests,
		ltmIiopProfileStatNumResponses,
		ltmIiopProfileStatNumCancels,
		ltmIiopProfileStatNumErrors,
		ltmIiopProfileStatNumFragments
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmIiopProfileStat MIB."
	::= { bigipLocalTMGroups 76 }

ltmRtspProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmRtspProfileNumber,
		ltmRtspProfileName,
		ltmRtspProfileConfigSource,
		ltmRtspProfileDefaultName,
		ltmRtspProfileIdleTimeout,
		ltmRtspProfileMaxHeaderSize,
		ltmRtspProfileMaxQueuedData,
		ltmRtspProfileUnicastRedirect,
		ltmRtspProfileMulticastRedirect,
		ltmRtspProfileSessionReconnect,
		ltmRtspProfileRealHttpPersistence,
		ltmRtspProfileProxy,
		ltmRtspProfileProxyHeader,
		ltmRtspProfileRtpPort,
		ltmRtspProfileRtcpPort
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmRtspProfile MIB."
	::= { bigipLocalTMGroups 77 }

ltmRtspProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmRtspProfileStatResetStats,
		ltmRtspProfileStatNumber,
		ltmRtspProfileStatName,
		ltmRtspProfileStatNumRequests,
		ltmRtspProfileStatNumResponses,
		ltmRtspProfileStatNumErrors,
		ltmRtspProfileStatNumInterleaved
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmRtspProfileStat MIB."
	::= { bigipLocalTMGroups 78 }

ltmSctpProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmSctpProfileNumber,
		ltmSctpProfileName,
		ltmSctpProfileConfigSource,
		ltmSctpProfileDefaultName,
		ltmSctpProfileRcvOrdered,
		ltmSctpProfileSndPartial,
		ltmSctpProfileTcpShutdown,
		ltmSctpProfileResetOnTimeout,
		ltmSctpProfileOutStreams,
		ltmSctpProfileInStreams,
		ltmSctpProfileSndbuf,
		ltmSctpProfileRcvwnd,
		ltmSctpProfileTxChunks,
		ltmSctpProfileRxChunks,
		ltmSctpProfileCookieExpiration,
		ltmSctpProfileInitMaxrtx,
		ltmSctpProfileAssocMaxrtx,
		ltmSctpProfileProxyBufferLow,
		ltmSctpProfileProxyBufferHigh,
		ltmSctpProfileIdleTimeout,
		ltmSctpProfileHeartbeatInterval,
		ltmSctpProfileIpTosToPeer,
		ltmSctpProfileLinkQosToPeer,
		ltmSctpProfileSecret
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSctpProfile MIB."
	::= { bigipLocalTMGroups 79 }

ltmSctpProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmSctpProfileStatResetStats,
		ltmSctpProfileStatNumber,
		ltmSctpProfileStatName,
		ltmSctpProfileStatAccepts,
		ltmSctpProfileStatAcceptfails,
		ltmSctpProfileStatConnects,
		ltmSctpProfileStatConnfails,
		ltmSctpProfileStatExpires,
		ltmSctpProfileStatAbandons,
		ltmSctpProfileStatRxrst,
		ltmSctpProfileStatRxbadsum,
		ltmSctpProfileStatRxcookie,
		ltmSctpProfileStatRxbadcookie
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSctpProfileStat MIB."
	::= { bigipLocalTMGroups 80 }

ltmUserStatProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmUserStatProfileNumber,
		ltmUserStatProfileName,
		ltmUserStatProfileConfigSource,
		ltmUserStatProfileDefaultName
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmUserStatProfile MIB."
	::= { bigipLocalTMGroups 81 }

ltmUserStatProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmUserStatProfileStatResetStats,
		ltmUserStatProfileStatNumber,
		ltmUserStatProfileStatName,
		ltmUserStatProfileStatFieldId,
		ltmUserStatProfileStatFieldName,
		ltmUserStatProfileStatFieldValue
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmUserStatProfileStat MIB."
	::= { bigipLocalTMGroups 83 }

ltmVsHttpClassGroup OBJECT-GROUP
	 OBJECTS {
		ltmVsHttpClassNumber,
		ltmVsHttpClassVsName,
		ltmVsHttpClassProfileName,
		ltmVsHttpClassPriority
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServHttpClass MIB."
	::= { bigipLocalTMGroups 84 }

ltmNodeAddrStatusGroup OBJECT-GROUP
	 OBJECTS {
		ltmNodeAddrStatusNumber,
		ltmNodeAddrStatusAddrType,
		ltmNodeAddrStatusAddr,
		ltmNodeAddrStatusAvailState,
		ltmNodeAddrStatusEnabledState,
		ltmNodeAddrStatusParentType,
		ltmNodeAddrStatusDetailReason
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmNodeAddrStatus MIB."
	::= { bigipLocalTMGroups 85 }

ltmPoolStatusGroup OBJECT-GROUP
	 OBJECTS {
		ltmPoolStatusNumber,
		ltmPoolStatusName,
		ltmPoolStatusAvailState,
		ltmPoolStatusEnabledState,
		ltmPoolStatusParentType,
		ltmPoolStatusDetailReason
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmPoolStatus MIB."
	::= { bigipLocalTMGroups 86 }

ltmPoolMbrStatusGroup OBJECT-GROUP
	 OBJECTS {
		ltmPoolMbrStatusNumber,
		ltmPoolMbrStatusPoolName,
		ltmPoolMbrStatusAddrType,
		ltmPoolMbrStatusAddr,
		ltmPoolMbrStatusPort,
		ltmPoolMbrStatusAvailState,
		ltmPoolMbrStatusEnabledState,
		ltmPoolMbrStatusParentType,
		ltmPoolMbrStatusDetailReason
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmPoolMemberStatus MIB."
	::= { bigipLocalTMGroups 87 }

ltmVsStatusGroup OBJECT-GROUP
	 OBJECTS {
		ltmVsStatusNumber,
		ltmVsStatusName,
		ltmVsStatusAvailState,
		ltmVsStatusEnabledState,
		ltmVsStatusParentType,
		ltmVsStatusDetailReason
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualServStatus MIB."
	::= { bigipLocalTMGroups 88 }

ltmVAddrStatusGroup OBJECT-GROUP
	 OBJECTS {
		ltmVAddrStatusNumber,
		ltmVAddrStatusAddrType,
		ltmVAddrStatusAddr,
		ltmVAddrStatusAvailState,
		ltmVAddrStatusEnabledState,
		ltmVAddrStatusParentType,
		ltmVAddrStatusDetailReason
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualAddrStatus MIB."
	::= { bigipLocalTMGroups 89 }

ltmFallbackStatusGroup OBJECT-GROUP
	 OBJECTS {
		ltmFallbackStatusNumber,
		ltmFallbackStatusName,
		ltmFallbackStatusIndex,
		ltmFallbackStatusCode
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileFallbackStatus MIB."
	::= { bigipLocalTMGroups 90 }

ltmRespHeadersPermGroup OBJECT-GROUP
	 OBJECTS {
		ltmRespHeadersPermNumber,
		ltmRespHeadersPermName,
		ltmRespHeadersPermIndex,
		ltmRespHeadersPermStr
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileRespHeadersPerm MIB."
	::= { bigipLocalTMGroups 91 }

ltmEncCookiesGroup OBJECT-GROUP
	 OBJECTS {
		ltmEncCookiesNumber,
		ltmEncCookiesName,
		ltmEncCookiesIndex,
		ltmEncCookiesStr
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmHttpProfileEncCookies MIB."
	::= { bigipLocalTMGroups 92 }

ltmFastL4ProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmFastL4ProfileStatResetStats,
		ltmFastL4ProfileStatNumber,
		ltmFastL4ProfileStatName,
		ltmFastL4ProfileStatOpen,
		ltmFastL4ProfileStatAccepts,
		ltmFastL4ProfileStatAcceptfails,
		ltmFastL4ProfileStatExpires,
		ltmFastL4ProfileStatRxbadpkt,
		ltmFastL4ProfileStatRxunreach,
		ltmFastL4ProfileStatRxbadunreach,
		ltmFastL4ProfileStatRxbadsum,
		ltmFastL4ProfileStatTxerrors,
		ltmFastL4ProfileStatSyncookIssue,
		ltmFastL4ProfileStatSyncookAccept,
		ltmFastL4ProfileStatSyncookReject,
		ltmFastL4ProfileStatServersynrtx
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmFastL4ProfileStat MIB."
	::= { bigipLocalTMGroups 93 }

ltmSipProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmSipProfileNumber,
		ltmSipProfileName,
		ltmSipProfileConfigSource,
		ltmSipProfileDefaultName,
		ltmSipProfileMaxSize,
		ltmSipProfileTerminateBye,
		ltmSipProfileInsertVia,
		ltmSipProfileSecureVia,
		ltmSipProfileInsertRecordRoute
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSipProfile MIB."
	::= { bigipLocalTMGroups 94 }

ltmSipProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmSipProfileStatResetStats,
		ltmSipProfileStatNumber,
		ltmSipProfileStatName,
		ltmSipProfileStatRequests,
		ltmSipProfileStatResponses,
		ltmSipProfileStatBadmsgs,
		ltmSipProfileStatDrops
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmSipProfileStat MIB."
	::= { bigipLocalTMGroups 95 }

ltmVirtualModuleScoreGroup OBJECT-GROUP
	 OBJECTS {
		ltmVirtualModuleScoreNumber,
		ltmVirtualModuleScoreVsName,
		ltmVirtualModuleScoreModuleType,
		ltmVirtualModuleScoreScore
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmVirtualModuleScore MIB."
	::= { bigipLocalTMGroups 96 }

ltmIsessionProfileGroup OBJECT-GROUP
	 OBJECTS {
		ltmIsessionProfileNumber,
		ltmIsessionProfileName,
		ltmIsessionProfileMode,
		ltmIsessionProfileConnectionReuse,
		ltmIsessionProfileCompressionNull,
		ltmIsessionProfileCompressionDeflate,
		ltmIsessionProfileCompressionLzo,
		ltmIsessionProfileCompressionAdaptive,
		ltmIsessionProfileDeduplication,
		ltmIsessionProfilePortTransparency,
		ltmIsessionProfileTargetVirtual,
		ltmIsessionProfileEndpointPool,
		ltmIsessionProfileCompressionDeflateLevel
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmIsessionProfile MIB."
	::= { bigipLocalTMGroups 97 }

ltmIsessionProfileStatGroup OBJECT-GROUP
	 OBJECTS {
		ltmIsessionProfileStatResetStats,
		ltmIsessionProfileStatNumber,
		ltmIsessionProfileStatVirtualName,
		ltmIsessionProfileStatProfileName,
		ltmIsessionProfileStatNullInUses,
		ltmIsessionProfileStatNullInErrors,
		ltmIsessionProfileStatNullInBytesOpt,
		ltmIsessionProfileStatNullInBytesRaw,
		ltmIsessionProfileStatNullOutUses,
		ltmIsessionProfileStatNullOutErrors,
		ltmIsessionProfileStatNullOutBytesOpt,
		ltmIsessionProfileStatNullOutBytesRaw,
		ltmIsessionProfileStatLzoInUses,
		ltmIsessionProfileStatLzoInErrors,
		ltmIsessionProfileStatLzoInBytesOpt,
		ltmIsessionProfileStatLzoInBytesRaw,
		ltmIsessionProfileStatLzoOutUses,
		ltmIsessionProfileStatLzoOutErrors,
		ltmIsessionProfileStatLzoOutBytesOpt,
		ltmIsessionProfileStatLzoOutBytesRaw,
		ltmIsessionProfileStatDeflateInUses,
		ltmIsessionProfileStatDeflateInErrors,
		ltmIsessionProfileStatDeflateInBytesOpt,
		ltmIsessionProfileStatDeflateInBytesRaw,
		ltmIsessionProfileStatDeflateOutUses,
		ltmIsessionProfileStatDeflateOutErrors,
		ltmIsessionProfileStatDeflateOutBytesOpt,
		ltmIsessionProfileStatDeflateOutBytesRaw,
		ltmIsessionProfileStatDedupInUses,
		ltmIsessionProfileStatDedupInErrors,
		ltmIsessionProfileStatDedupInBytesOpt,
		ltmIsessionProfileStatDedupInBytesRaw,
		ltmIsessionProfileStatDedupOutUses,
		ltmIsessionProfileStatDedupOutErrors,
		ltmIsessionProfileStatDedupOutBytesOpt,
		ltmIsessionProfileStatDedupOutBytesRaw,
		ltmIsessionProfileStatDedupInHits,
		ltmIsessionProfileStatDedupInHitBytes,
		ltmIsessionProfileStatDedupInHitHistBucket1k,
		ltmIsessionProfileStatDedupInHitHistBucket2k,
		ltmIsessionProfileStatDedupInHitHistBucket4k,
		ltmIsessionProfileStatDedupInHitHistBucket8k,
		ltmIsessionProfileStatDedupInHitHistBucket16k,
		ltmIsessionProfileStatDedupInHitHistBucket32k,
		ltmIsessionProfileStatDedupInHitHistBucket64k,
		ltmIsessionProfileStatDedupInHitHistBucket128k,
		ltmIsessionProfileStatDedupInHitHistBucket256k,
		ltmIsessionProfileStatDedupInHitHistBucket512k,
		ltmIsessionProfileStatDedupInHitHistBucket1m,
		ltmIsessionProfileStatDedupInHitHistBucketLarge,
		ltmIsessionProfileStatDedupInMisses,
		ltmIsessionProfileStatDedupInMissBytes,
		ltmIsessionProfileStatDedupInMissHistBucket1k,
		ltmIsessionProfileStatDedupInMissHistBucket2k,
		ltmIsessionProfileStatDedupInMissHistBucket4k,
		ltmIsessionProfileStatDedupInMissHistBucket8k,
		ltmIsessionProfileStatDedupInMissHistBucket16k,
		ltmIsessionProfileStatDedupInMissHistBucket32k,
		ltmIsessionProfileStatDedupInMissHistBucket64k,
		ltmIsessionProfileStatDedupInMissHistBucket128k,
		ltmIsessionProfileStatDedupInMissHistBucket256k,
		ltmIsessionProfileStatDedupInMissHistBucket512k,
		ltmIsessionProfileStatDedupInMissHistBucket1m,
		ltmIsessionProfileStatDedupInMissHistBucketLarge,
		ltmIsessionProfileStatDedupOutHits,
		ltmIsessionProfileStatDedupOutHitBytes,
		ltmIsessionProfileStatDedupOutHitHistBucket1k,
		ltmIsessionProfileStatDedupOutHitHistBucket2k,
		ltmIsessionProfileStatDedupOutHitHistBucket4k,
		ltmIsessionProfileStatDedupOutHitHistBucket8k,
		ltmIsessionProfileStatDedupOutHitHistBucket16k,
		ltmIsessionProfileStatDedupOutHitHistBucket32k,
		ltmIsessionProfileStatDedupOutHitHistBucket64k,
		ltmIsessionProfileStatDedupOutHitHistBucket128k,
		ltmIsessionProfileStatDedupOutHitHistBucket256k,
		ltmIsessionProfileStatDedupOutHitHistBucket512k,
		ltmIsessionProfileStatDedupOutHitHistBucket1m,
		ltmIsessionProfileStatDedupOutHitHistBucketLarge,
		ltmIsessionProfileStatDedupOutMisses,
		ltmIsessionProfileStatDedupOutMissBytes,
		ltmIsessionProfileStatDedupOutMissHistBucket1k,
		ltmIsessionProfileStatDedupOutMissHistBucket2k,
		ltmIsessionProfileStatDedupOutMissHistBucket4k,
		ltmIsessionProfileStatDedupOutMissHistBucket8k,
		ltmIsessionProfileStatDedupOutMissHistBucket16k,
		ltmIsessionProfileStatDedupOutMissHistBucket32k,
		ltmIsessionProfileStatDedupOutMissHistBucket64k,
		ltmIsessionProfileStatDedupOutMissHistBucket128k,
		ltmIsessionProfileStatDedupOutMissHistBucket256k,
		ltmIsessionProfileStatDedupOutMissHistBucket512k,
		ltmIsessionProfileStatDedupOutMissHistBucket1m,
		ltmIsessionProfileStatDedupOutMissHistBucketLarge,
		ltmIsessionProfileStatOutgoingConnsIdleCur,
		ltmIsessionProfileStatOutgoingConnsIdleMax,
		ltmIsessionProfileStatOutgoingConnsIdleTot,
		ltmIsessionProfileStatOutgoingConnsActiveCur,
		ltmIsessionProfileStatOutgoingConnsActiveMax,
		ltmIsessionProfileStatOutgoingConnsActiveTot,
		ltmIsessionProfileStatOutgoingConnsErrors,
		ltmIsessionProfileStatOutgoingConnsPassthruTot,
		ltmIsessionProfileStatIncomingConnsActiveCur,
		ltmIsessionProfileStatIncomingConnsActiveMax,
		ltmIsessionProfileStatIncomingConnsActiveTot,
		ltmIsessionProfileStatIncomingConnsErrors
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmIsessionProfileStat MIB."
	::= { bigipLocalTMGroups 98 }

ltmXmlProfileXpathQueriesGroup OBJECT-GROUP
	 OBJECTS {
		ltmXmlProfileXpathQueriesNumber,
		ltmXmlProfileXpathQueriesName,
		ltmXmlProfileXpathQueriesIndex,
		ltmXmlProfileXpathQueriesString
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmXmlProfileXpathQueries MIB."
	::= { bigipLocalTMGroups 99 }

ltmXmlProfileNamespaceMappingsGroup OBJECT-GROUP
	 OBJECTS {
		ltmXmlProfileNamespaceMappingsNumber,
		ltmXmlProfileNamespaceMappingsName,
		ltmXmlProfileNamespaceMappingsIndex,
		ltmXmlProfileNamespaceMappingsMappingPrefix,
		ltmXmlProfileNamespaceMappingsMappingNamespace
	}
	STATUS	 current
	DESCRIPTION
		"A collection of objects of ltmXmlProfileNamespaceMappings MIB."
	::= { bigipLocalTMGroups 100 }
END
