

--
-- Juniper Enterprise Specifics MIB
-- 
-- Copyright (c) 2010 Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--

JNX-PPP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, IpAddress, TimeTicks, Unsigned32   
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue, RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    ifIndex, InterfaceIndex, InterfaceIndexOrZero
        FROM IF-MIB
    Ipv6AddressIfIdentifier
        FROM IPV6-TC
    jnxPppMibRoot
        FROM JUNIPER-SMI ;                                  


jnxPppMIB  MODULE-IDENTITY
    LAST-UPDATED "201007220942Z"  -- 22-Jul-10 03:12 PM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "he Point-to-Point Protocol (PPP) MIB for the Juniper enterprise."
    -- Revision History

    REVISION    "201111290000Z"  -- 29-Nov-11 03:12 PM EST  - JUNOS 11.4
    DESCRIPTION
        "Deprecated Integer32 type jnxPppLinkStatusLocalMagicNumber, 
         jnxPppLinkStatusRemoteMagicNumber and added Unsigned32 type
         jnxPppLinkStatusLocalMagicNumber1, jnxPppLinkStatusLocalMagicNumber1
         under jnxPppLinkStatusTable"
    
    REVISION    "201007220942Z"  -- 22-Jul-10 03:12 PM EST  - JUNOS 11.0
    DESCRIPTION
        "Initial version."
    ::= { jnxPppMibRoot 1 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
JnxPppAuthentication ::= TEXTUAL-CONVENTION
    STATUS      deprecated
    DESCRIPTION
        "Specifies the type(s) of PPP authentication used, if any:
          none      No authentication is negotiated.
          pap       PAP negotiation only.
          chap      CHAP negotiation only.
          papChap   PAP negotiation is attempted first; if fails, attempt CHAP.
          chapPap   CHAP negotiation is attempted first; if fails, attempt PAP."
    SYNTAX      INTEGER {
                    none (0),
                    pap (1),
                    chap (2),
                    papChap (3),
                    chapPap (4) }

--+++++++++

JnxPppMlPppBundleName ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "MLPPP Bundle name.  The bundle name is a characteristic of a MLPPP
        network interface."
    SYNTAX OCTET STRING (SIZE(1..60))


--+++++

JnxPppAuthentication2 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Specifies the type(s) of PPP authentication used, if any:
          none      No authentication is negotiated.
          pap       PAP negotiation.
          chap      CHAP negotiation.
          eap       EAP negotiation." 

    SYNTAX      INTEGER {
                    none (0),
                    pap (1),
                    chap (2),
                    eap (3) }


JnxNibbleConfig ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A configuration variable comprised of nibbles i.e. 4 bits, such that 
         a client can supply a list of 0 to 8 selections.  The least 
         significant nibble is the first value of the list, and the most 
         significant nibble is the last value.  The value in each field 
         ranges from 0 to 15, however the first nibble with value 0 indicates
         the end of the list.  Repetition of values is not allowed. 
         Segregation of values in not allowed.

         Example valid encoding:
         0x00000321
         0x00083E12

         Not a valid encoding:
         0x00000121 will return an error
         0x01002001 will return an error."
    SYNTAX INTEGER

-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++


jnxPPPObjects        OBJECT IDENTIFIER ::= { jnxPppMIB 1 }

--
-- This MIB contains managed objects for PPP interfaces. Management objects are
-- provided to query for an available interface index, and to create/delete 
-- interfaces of this type. Creating/deleting this interface type using this 
-- MIB has the side effect of creating/deleting corresponding entries in the
-- Interface MIB ifTable/ifXTable, and in the Jnxper Enterprise Interface MIB
-- jnxIfTable. 
--This MIB acts as a supplement to IETF MIBs RFC1471 PPP-LCP-MIB .

-- MIB object definitions are organized into the following
-- Functional sections:
--
jnxPppLcp 	                OBJECT IDENTIFIER   ::= { jnxPPPObjects 1 }
jnxPppSec            	        OBJECT IDENTIFIER   ::= { jnxPPPObjects 2 }     
jnxPppIp                        OBJECT IDENTIFIER   ::= { jnxPPPObjects 3 }
jnxPppOsi                       OBJECT IDENTIFIER   ::= { jnxPPPObjects 4 }
jnxPppSession                   OBJECT IDENTIFIER   ::= { jnxPPPObjects 5 }
jnxPppMlPpp                     OBJECT IDENTIFIER   ::= { jnxPPPObjects 6 }
jnxPppSummary                   OBJECT IDENTIFIER   ::= { jnxPPPObjects 7 }
jnxPppIpv6                      OBJECT IDENTIFIER   ::= { jnxPPPObjects 8 }
jnxPppGlobalConfig              OBJECT IDENTIFIER   ::= { jnxPPPObjects 9 }




-- /////////////////////////////////////////////////////////////////////////////
-- PPP LCP
-- This section defines objects used to manage the PPP Link / LCP layer of PPP.
-- The jnxPppLinkStatusTable complements RFC1471 pppLinkStatusTable, providing 
--status indications regarding the operation of network protocols over each
-- link. The addition/removal of a network protocol service is accomplished 
-- outside this MIB. The jnxPppLinkConfigTable complements RFC1471 
-- providing the ability to create/delete instances of PPP links and providing 
-- for configuration of option parameter values (if any) not found in the 
-- standard MIB, to be used during LCP negotiation.

-- /////////////////////////////////////////////////////////////////////////////
-- The PPP Link Status Table
--
jnxPppLinkStatusTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppLinkStatusEntry
    MAX-ACCESS                        not-accessible
    STATUS                                   current
    DESCRIPTION
        "This table contains entries for PPP interfaces present in the system."
    ::= { jnxPppLcp 1 }

jnxPppLinkStatusEntry OBJECT-TYPE
    SYNTAX                                JnxPppLinkStatusEntry
    MAX-ACCESS                      not-accessible
    STATUS                                 current
    DESCRIPTION
        "Each entry describes the characteristics of a PPP interface."
    INDEX     { ifIndex }
    ::= { jnxPppLinkStatusTable 1 }

JnxPppLinkStatusEntry ::= SEQUENCE {
    jnxPppLinkStatusTerminateReason               INTEGER,
    jnxPppLinkStatusTerminateNegFailOption        INTEGER,
    jnxPppLinkStatusInKeepaliveRequests           Counter32,                  
    jnxPppLinkStatusOutKeepaliveRequests          Counter32,
    jnxPppLinkStatusInKeepaliveReplies            Counter32,
    jnxPppLinkStatusOutKeepaliveReplies           Counter32,
    jnxPppLinkStatusKeepaliveFailures             Counter32,
    jnxPppLinkStatusLocalMagicNumber              Integer32,
    jnxPppLinkStatusRemoteMagicNumber             Integer32,
    jnxPppLinkStatusLocalAuthentication           JnxPppAuthentication2,
    jnxPppLinkStatusTunnelIfIndex                 InterfaceIndexOrZero,
    jnxPppLinkStatuslcpRenegoTerminates           Counter32,
    jnxPppLinkStatusLocalMagicNumber1             Unsigned32,
    jnxPppLinkStatusRemoteMagicNumber1            Unsigned32}

jnxPppLinkStatusTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    adminDisable(2),
                    lowerLayerDown(3),
                    noUpperInterface(4),
                    authenticationFailure(5),
                    peerTerminated(6),
                    peerRenegotiated(7),
                    maxRetriesExceeded(8),
                    negotiationFailure(9),
                    keepaliveFailure(10),
                    sessionTimeout(11),
                    inactivityTimeout(12),
                    addressLeaseExpired(13),
                    adminLogout(14),
                    tunnelFailed(15),
                    tunnelDisconnected(16),
                    loopback(17) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the PPP link was terminated:
            none                    None.
            other                   Not specified.
            adminDisable            Interface administratively disabled.
            lowerLayerDown          Underlying interface is down.
            noUpperInterface        No interface above PPP.
            authenticationFailure   Authentication failed.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate LCP option.                    
            keepaliveFailure        Keepalive failed.
            sessionTimeout          Maximum session period expired.
            inactivityTimeout       Maximum inactivity period expired.
            addressLeaseExpired     Lease for network address expired.
            adminLogout             Session administratively terminated.
            tunnelFailed            Associated tunnel failed.
            tunnelDisconnected      Associated tunnel disconnected.
            loopback                Loopback detected."
    ::= { jnxPppLinkStatusEntry 1 }

jnxPppLinkStatusTerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localMru(2),
                    remoteMru(3),
                    localMagicNumber(4),
                    remoteMagicNumber(5),
                    localAuthentication(6),
                    localToRemoteProtocolCompression(7),
                    localToRemoteACCompression(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP LCP option for which negotiation failed, 
        when jnxPppLinkStatusTerminateReason has the value negotiationFailure."
    ::= { jnxPppLinkStatusEntry 2 }

jnxPppLinkStatusInKeepaliveRequests OBJECT-TYPE
    SYNTAX            Counter32
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "Number of keepalive requests received."
    ::= { jnxPppLinkStatusEntry 3 }

jnxPppLinkStatusOutKeepaliveRequests OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of keepalive requests transmitted."
    ::= { jnxPppLinkStatusEntry 4 }

jnxPppLinkStatusInKeepaliveReplies OBJECT-TYPE
    SYNTAX            Counter32
    MAX-ACCESS   read-only
    STATUS             current
    DESCRIPTION
        "Number of keepalive replies received."
    ::= { jnxPppLinkStatusEntry 5 }

jnxPppLinkStatusOutKeepaliveReplies OBJECT-TYPE
    SYNTAX            Counter32
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "Number of keepalive replies transmitted."
    ::= { jnxPppLinkStatusEntry 6 }

jnxPppLinkStatusKeepaliveFailures OBJECT-TYPE
    SYNTAX            Counter32
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "Number of keepalive failures detected."
    ::= { jnxPppLinkStatusEntry 7 }

jnxPppLinkStatusLocalMagicNumber OBJECT-TYPE
    SYNTAX            Integer32
    MAX-ACCESS         read-only
    STATUS             deprecated
    DESCRIPTION
        "Magic number negotiated for the local side.
         This has been deprecated and replaced by 
         jnxPppLinkStatusLocalMagicNumber1"
    ::= { jnxPppLinkStatusEntry 8 }

jnxPppLinkStatusRemoteMagicNumber OBJECT-TYPE
    SYNTAX            Integer32
    MAX-ACCESS         read-only
    STATUS             deprecated
    DESCRIPTION
        "Magic number negotiated for the remote side.
         This has been deprecated and replaced by
         jnxPppLinkStatusRemoteMagicNumber1"
    ::= { jnxPppLinkStatusEntry 9 }

jnxPppLinkStatusLocalAuthentication OBJECT-TYPE
    SYNTAX            JnxPppAuthentication2
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "Authentication protocol negotiated for the local side."
    ::= { jnxPppLinkStatusEntry 10 }

jnxPppLinkStatusTunnelIfIndex OBJECT-TYPE
    SYNTAX            InterfaceIndexOrZero
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "The ifIndex of an associated interface pertaining to a tunneling 
        protocol, or zero if no such interface exists.The type of tunneling
        interface can be identified from information in the entries in 
        ifTable and jnxIfTable for this tunnel interface."
    ::= { jnxPppLinkStatusEntry 11 }

jnxPppLinkStatuslcpRenegoTerminates OBJECT-TYPE
    SYNTAX            Counter32
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "Number of times lcp terminated due to peer exceeding max renegotiation 
         attempts."
    ::= { jnxPppLinkStatusEntry 12 }


jnxPppLinkStatusLocalMagicNumber1 OBJECT-TYPE
    SYNTAX             Unsigned32
    MAX-ACCESS         read-only
    STATUS             current
    DESCRIPTION
        "Magic number negotiated for the local side."
    ::= { jnxPppLinkStatusEntry 13 }

jnxPppLinkStatusRemoteMagicNumber1 OBJECT-TYPE
    SYNTAX             Unsigned32
    MAX-ACCESS         read-only
    STATUS             current
    DESCRIPTION
        "Magic number negotiated for the remote side."
    ::= { jnxPppLinkStatusEntry 14 }

--
-- The PPP Link Configuration Table
--
jnxPppLinkConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppLinkConfigEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "This table contains entries for PPP interfaces present in the system."
    ::= { jnxPppLcp 2 }

jnxPppLinkConfigEntry OBJECT-TYPE
    SYNTAX             JnxPppLinkConfigEntry
    MAX-ACCESS         not-accessible
    STATUS             current
    DESCRIPTION
        "Each entry describes the characteristics of a PPP interface.
        Creating or deleting entries in this table causes corresponding entries 
        for be created or deleted in ifTable,ifXTable,jnxIfTable."
   INDEX     { jnxPppLinkConfigIfIndex }
    ::= { jnxPppLinkConfigTable 1 }

JnxPppLinkConfigEntry ::= SEQUENCE {
    jnxPppLinkConfigIfIndex                             InterfaceIndex,
    jnxPppLinkConfigRowStatus                           RowStatus,
    jnxPppLinkConfigLowerIfIndex                        InterfaceIndexOrZero,
    jnxPppLinkConfigKeepalive                           Integer32,
    jnxPppLinkConfigAuthentication                      JnxPppAuthentication,
    jnxPppLinkConfigMaxAuthenRetries                    Integer32,
    jnxPppLinkConfigStandardIfIndex                     InterfaceIndex,
    jnxPppLinkConfigChapMinChallengeLength              Integer32,
    jnxPppLinkConfigChapMaxChallengeLength              Integer32,
    jnxPppLinkConfigPassiveMode                         INTEGER,
    jnxPppLinkConfigAuthenticatorLogicalSystem          OCTET STRING,
    jnxPppLinkConfigAuthenticatorRoutingInstance        OCTET STRING,
    jnxPppLinkConfigAaaProfile                          OCTET STRING,
    jnxPppLinkConfigAuthentication2                     JnxNibbleConfig,
    jnxPppLinkConfigIgnoreMagicNumberMismatch           INTEGER,
    jnxPppLinkConfigMaxLcpRenegotiation                 Integer32}

jnxPppLinkConfigIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the PPP interface.  When creating entries in this
         table, suitable values for this object are determined by reading 
         jnxPppNextIfIndex."
    ::= { jnxPppLinkConfigEntry 1 }

jnxPppLinkConfigRowStatus OBJECT-TYPE
    SYNTAX            RowStatus
    MAX-ACCESS         read-only
    STATUS             current
    DESCRIPTION
       "Controls creation or deletion of entries in this table with READ-CREATE
        maximum access according to the RowStatus textual convention,
        constrained to support the following values only:
            createAndGo
            destroy
        To create an entry in this table, the following entry objects MUST be
         explicitly configured:
            jnxPppLinkConfigRowStatus
            jnxPppLinkConfigLowerIfIndex

        In addition, when creating an entry the following conditions must hold:
            A value for jnxPppLinkConfigIndex must have been determined 
            previously, by reading jnxPppNextIfIndex.The interface identified 
            by jnxPppLinkConfigLowerIfIndex must exist. A corresponding entry  
           in Table or ifXTable or jnxIfTable is created or destroyed as a 
             result of creating or destroying an entry in this table.

         The following values can be read from this object:
             active(1)"
    ::= { jnxPppLinkConfigEntry 2 }

jnxPppLinkConfigLowerIfIndex OBJECT-TYPE
    SYNTAX            InterfaceIndexOrZero
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
       "The ifIndex of an interface over which this PPP interface is to be 
       layered.A value of zero indicates no layering.  An implementation may
      choose to require that a non-zero value be configured at entry creation."
    ::= { jnxPppLinkConfigEntry 3 }

jnxPppLinkConfigKeepalive OBJECT-TYPE
    SYNTAX             Integer32 (0..64800)
    UNITS               "seconds"
    MAX-ACCESS          read-only
    STATUS              current
    DESCRIPTION
        "Keepalive interval in seconds.  A value of zero disables keepalive. 
        Keepalive is performed using LCP Echo."
    DEFVAL    { 30 }
    ::= { jnxPppLinkConfigEntry 4 }

jnxPppLinkConfigAuthentication OBJECT-TYPE
    SYNTAX      JnxPppAuthentication
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "Specifies the type(s) of authentication, if any, to be negotiated
         with the peer:
          none      No authentication is negotiated.
          pap       PAP negotiation only.
          chap      CHAP negotiation only.
          papChap   PAP negotiation is attempted first; if fails, attempt CHAP.
          chapPap   CHAP negotiation is attempted first; if fails, attempt PAP.

        If authentication negotiation is not supported for this PPP interface, 
        then any attempt to explicitely set this object if READ-CREATE maximum
        access is supported will result in a notWritable error and it will be
        implicitily set to the DEFVAL on row creation. Setting this object to
        none(0) will set jnxPppLinkConfigAuthenticatorRouting Instance object
        to an empty string.
 This object returns a null(0) value on the get operation. New object 
 jnxPppLinkConfigAuthentication2 will reflect the configured values. Setting
 this object along with the jnxPppLinkConfigAuthentication2 object will return  
 an inconsistentValue error."
    DEFVAL    { none }
    ::= { jnxPppLinkConfigEntry 5 }

jnxPppLinkConfigMaxAuthenRetries OBJECT-TYPE
    SYNTAX            Integer32 (0..7)
    MAX-ACCESS         read-only
    STATUS             current
    DESCRIPTION
        "The number of authentication retries permitted, in addition to a
         failed initial attempt.  If all retries fail, the link is reset. 
         If authentication negotiation is not supported for this PPP interface,
         then any attempt to explicitely set this object  if READ-CREATE 
         maximum access is supported will result in a notWritable error and
         it will be implicitily set to the DEFVAL on row creation."
    DEFVAL    { 0 }
    ::= { jnxPppLinkConfigEntry 6 }

jnxPppLinkConfigStandardIfIndex OBJECT-TYPE
    SYNTAX            InterfaceIndex
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "The ifIndex value for this interface in the standard PPP MIBs. 
         The ifIndex value for PPP interfaces is not the same for both 
         proprietary and standard MIB tables pertaining to PPP interface.
        Therefore this value is provide to simply cross referencing 
        standard PPP and proprietary PPP MIB information."
    ::= { jnxPppLinkConfigEntry 7 }

jnxPppLinkConfigChapMinChallengeLength OBJECT-TYPE
    SYNTAX            Integer32 (8..63)
    MAX-ACCESS        read-only
    STATUS             current
    DESCRIPTION
        "Minimum value of the CHAP authenticator challenge length value.
         This value is never greater than
         jnxPppLinkConfigChapMaxChallengeLength."
    DEFVAL    { 16 }
    ::= { jnxPppLinkConfigEntry 8 }

jnxPppLinkConfigChapMaxChallengeLength OBJECT-TYPE
    SYNTAX            Integer32 (8..63)
    MAX-ACCESS         read-only
    STATUS             current
    DESCRIPTION
        "Maximum value of the CHAP authenticator challenge length value. 
        This value is never less than  jnxPppLinkConfigChapMinChallengeLength."
    DEFVAL    { 32 }
    ::= { jnxPppLinkConfigEntry 9 }

jnxPppLinkConfigPassiveMode OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS        read-only
    STATUS             current
    DESCRIPTION
    "When enabled, LCP state machine is forced into passive mode on lower layer
         UP message.  It adds compatibility with slow and buggy clients."
    DEFVAL    { disable }
    ::= { jnxPppLinkConfigEntry 10 }

jnxPppLinkConfigAuthenticatorLogicalSystem OBJECT-TYPE
    SYNTAX            OCTET STRING
    MAX-ACCESS        read-only
    STATUS             current
    DESCRIPTION
        "The name of the logical system to  be used for authentication on the
         PPP interface.With READ-CREATE maximum access , setting this object 
         statically binds the authenticating logical system with the PPP
         interface.  If this object is not explicitly set or it is set to null
         string, then this object is ignored and the virtual router used for
         authentication is determined by other means. 
         On a Set operation, if the value of this object is not null and does 
         not correspond to an existing virtual router, then an
         inconsistentValue error is returned. Setting this object to a non-null
        string returns inconsistentValue error if jnxPppLinkConfigAuthentication
        object is none(0) or not configured."
    ::= { jnxPppLinkConfigEntry 11 }

jnxPppLinkConfigAuthenticatorRoutingInstance OBJECT-TYPE
    SYNTAX             OCTET STRING
    MAX-ACCESS         read-only
    STATUS             current
    DESCRIPTION
        "The name of the routing instancebe used for authentication on the 
        PPP interface. With READ-CREATE maximum access, setting this object 
        statically binds the authenticating routing instance with the PPP 
        interface.If this object is not explicitly set or it is set to null
        string, then this object is ignored and the virtual router used for
        authentication is determined by other means.  On a Set operation,
        if the value of this object is not null and does not correspond to
       an existing virtual router, then an inconsistentValue error is returned.
       Setting this object to a non-null string returns inconsistentValue error
       if jnxPppLinkConfigAuthentication object is
          none(0) or not configured."
    ::= { jnxPppLinkConfigEntry 12 }


jnxPppLinkConfigAaaProfile OBJECT-TYPE
    SYNTAX            OCTET STRING
    MAX-ACCESS        read-only
    STATUS             current
    DESCRIPTION
        "The name of the AAA profile to be used for authentication on the
         PPP interface. With READ-CREATE maximum access, setting this 
         object statically binds the AAA profile with the PPP interface.
         If this object is not explicitly set or it is set to null string, 
         then this object is ignored.  On a Set operation, if the value of 
         this object is not null and does not correspond to an existing
         AAA profile, then an inconsistentValue error is returned."
    ::= { jnxPppLinkConfigEntry 13 }

jnxPppLinkConfigAuthentication2 OBJECT-TYPE
    SYNTAX         JnxNibbleConfig
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "A configuration variable comprised of nibbles i.e. 4 bits, such
         that a client can supply a list of 0 to 8 selections.  The least
          significant nibble is the first value of the list, and the most
          significant nibble is the last value.  The value in each field 
          ranges from 0 to 15, however the first nibble with value 0 
          indicates the end of the list.  Repetition of values is not allowed.
          Segregation
           of values is not allowed.

         Valid Values are:
         none - 0
         pap  - 1
         chap - 2
         eap  - 3

         Example valid encoding:
         0x00000321
         0x00000012

         Not a valid encoding:
         0x00000121
         0x01002001

         If authentication negotiation is not supported for this PPP interface
        and with READ-CREATE maximum access ,any attempt to explicitly set this
         object will result in a notWritable error and it will be implicitly 
        set to the DEFVAL on row creation. Setting this object to null will set
        jnxPppLinkConfigAuthenticatorRoutingInstance object to an empty string.
        Setting this object along with the jnxPppLinkConfigAuthentication object
         will return an inconsistentValue error."
    DEFVAL    { 0 }
    ::= { jnxPppLinkConfigEntry 14 }
    
jnxPppLinkConfigIgnoreMagicNumberMismatch OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS          read-only
    STATUS              current
    DESCRIPTION
        "The ignore magic number mismatch option of the PPP interface determines
         the action to be taken, when the peer has not negotiated any value yet 
         sent null or invalid magic number in the LCP echo packets.
         The two actions
         that can be configured are:
            1)	Ignore the mismatch and retain connection
            2)	Disallow the mismatch and terminate connection"
    DEFVAL    { disable }
    ::= { jnxPppLinkConfigEntry 15 }

jnxPppLinkConfigMaxLcpRenegotiation OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of allowed lcp renegotiation attempts from peer."
    DEFVAL    { 30 }
    ::= { jnxPppLinkConfigEntry 16 }


--
-- IfIndex selection for creating new PPP interfaces in jnxPppLinkConfigTable.
--
-- NOTE: This object is placed after jnxPppLinkConfigTable so
-- that jnxPppLinkStatusTable and jnxPppLinkConfigTable have the
-- same relative MIB node positions below the jnxPppLcp node
-- (jnxPppLcp.1 and jnxPppLcp.2, respectively) as their counterpart
-- Status and Config tables in RFC1471.
--
jnxPppNextIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in the 
       jnxPppLinkConfigTable. A GET of this object returns the next available
       ifIndex value to be used to create an entry in the associated interface
       table; or zero, if no valid ifIndex value is available.This object
       also returns a value of zero when it is the lexicographic successor
       of a varbind presented in an SNMP GETNEXT or GETBULK request, for which
       circumstance it is assumed that ifIndex allocation is unintended.
       Successive GETs will typically return different values, thus avoiding
       collisions among cooperating management clients seeking to create table
       entries simultaneously."
    ::= { jnxPppLcp 3 }




-- ////////////////////////////////////////////////////////////////////////////
-- PPP Security
-- This section defines objects used to manage the PPP Security
-- functionality of PPP.
-- ////////////////////////////////////////////////////////////////////////////
-- No objects are currently defined.
-- ////////////////////////////////////////////////////////////////////////////
-- PPP IP NCP
-- This section defines objects used to manage the PPP Network Control Protocol
-- for IP protocol operation (IPCP).
-- /////////////////////////////////////////////////////////////////////////////
-- The PPP IP Table
jnxPppIpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppIpEntry
    MAX-ACCESS   not-accessible
    STATUS             current
    DESCRIPTION
        "Table containing the IP parameters for the local PPP entity."
    ::= { jnxPppIp 1 }

jnxPppIpEntry OBJECT-TYPE
    SYNTAX      JnxPppIpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPCP status information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { jnxPppIpTable 1 }

JnxPppIpEntry ::= SEQUENCE {
    jnxPppIpServiceStatus                      INTEGER,
    jnxPppIpTerminateReason                    INTEGER,
    jnxPppIpTerminateNegFailOption             INTEGER,
    jnxPppIpLocalIpAddress                     IpAddress,
    jnxPppIpRemoteIpAddress                    IpAddress,
    jnxPppIpRemotePrimaryDnsAddress            IpAddress,
    jnxPppIpRemoteSecondaryDnsAddress          IpAddress,
    jnxPppIpRemotePrimaryWinsAddress           IpAddress,
    jnxPppIpRemoteSecondaryWinsAddress         IpAddress,
    jnxPppIpNetworkStatusIpcpRenegoTerminates  Counter32}

jnxPppIpServiceStatus OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether IP protocol service is operating over this PPP link.
         Service is established on this link through means outside this MIB."
    ::= { jnxPppIpEntry 1 }

jnxPppIpTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    noService(2),
                    admin(3),
                    linkDown(4),
                    peerTerminated(5),
                    peerRenegotiated(6),
                    maxRetriesExceeded(7),
                    negotiationFailure(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the IPCP link was terminated:
            none                    None.
            other                   Not specified.
            noService               No IP service configured on this PPP link.
            admin                   Administratively disabled.
            linkDown                Underlying link is down.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate IPCP option.  See                                
             jnxPppIpTerminateNegFailOption."
    ::= { jnxPppIpEntry 2 }

jnxPppIpTerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localIpAddress(2),
                    remoteIpAddress(3),
                    remotePrimaryDnsAddress(4),
                    remoteSecondaryDnsAddress(5),
                    remotePrimaryWinsAddress(6),
                    remoteSecondaryWinsAddress(7),
                    localIpAddressMask(8),
                    remoteIpAddressMask(9) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP IPCP option for which negotiation failed, when 
        jnxPppIpTerminateReason has the value 'negotiationFailure'."
    ::= { jnxPppIpEntry 3 }

jnxPppIpLocalIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IP Address used by the local side."
    ::= { jnxPppIpEntry 4 }

jnxPppIpRemoteIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IP Address used by the remote side."
    ::= { jnxPppIpEntry 5 }

jnxPppIpRemotePrimaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Primary DNS server used by the remote side."
    ::= { jnxPppIpEntry 6 }

jnxPppIpRemoteSecondaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Secondary DNS server used by the remote side."
    ::= { jnxPppIpEntry 7 }

jnxPppIpRemotePrimaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Primary WINS server used by the remote side."
    ::= { jnxPppIpEntry 8 }

jnxPppIpRemoteSecondaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Secondary WINS server used by the remote side."
    ::= { jnxPppIpEntry 9 }

jnxPppIpNetworkStatusIpcpRenegoTerminates OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times ipcp terminated due to peer exceeding max 
        renegotiation attempts."
    ::= { jnxPppIpEntry 10 }

--
-- The PPP IP Config Table
--
jnxPppIpConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppIpConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the IP parameters for the local PPP entity."
    ::= { jnxPppIp 2 }

jnxPppIpConfigEntry OBJECT-TYPE
    SYNTAX      JnxPppIpConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPCP configuration information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { jnxPppIpConfigTable 1 }

JnxPppIpConfigEntry ::= SEQUENCE {
    jnxPppIpConfigPeerDnsPriority      INTEGER,
    jnxPppIpConfigPeerWinsPriority     INTEGER,
    jnxPppIpConfigIpcpNetmask          INTEGER,
    jnxPppIpConfigInitiateIp           INTEGER,
    jnxPppIpConfigMaxIpcpRenegotiation Integer32,
    jnxPppIpConfigPromptIpcpDnsOption  INTEGER,
    jnxPppIpConfigIpcpLockout          INTEGER}

jnxPppIpConfigPeerDnsPriority OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When enabled, allows peer's DNS address to prevail in the event of a 
        negotiation conflict; when disabled, the local PPP interface's DNS 
        address prevails."
    ::= { jnxPppIpConfigEntry 1 }

jnxPppIpConfigPeerWinsPriority OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When enabled, allows peer's WINS address to prevail in the event of a 
        negotiation conflict; when disabled, the local PPP interface's WINS
         address prevails."
    ::= { jnxPppIpConfigEntry 2 }

jnxPppIpConfigIpcpNetmask OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables the negotiation of the IPCP option netmask (0x90) during 
        IPCP negotiation."
    DEFVAL    { disable }
    ::= { jnxPppIpConfigEntry 3 }

jnxPppIpConfigInitiateIp OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables the initiation of negotiation of the IPCP."
    DEFVAL    { disable }
    ::= { jnxPppIpConfigEntry 4 }

jnxPppIpConfigMaxIpcpRenegotiation OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of allowed ipcp renegotiation attempts from peer."
    DEFVAL    { 30 }
    ::= { jnxPppIpConfigEntry 5 }

jnxPppIpConfigPromptIpcpDnsOption OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Control prompting of IPCP DNS option to remote peer."
    DEFVAL    { disable }
    ::= { jnxPppIpConfigEntry 6 }

jnxPppIpConfigIpcpLockout OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables IPCP lockout. It determines whether this NCP can be negotiated
         when the interface is already running a different NCP. On enabling 
         this option, the IPCP negotiation will be blocked after a different 
         NCP service is up and waited for 10 seconds for IPCP initiation 
         from peer."
    DEFVAL    { disable }
    ::= { jnxPppIpConfigEntry 7 }

-- /////////////////////////////////////////////////////////////////////////////
-- PPP OSI NCP
-- This section defines objects used to manage the PPP Network Control Protocol
-- for OSI protocol operation (OSICP). The IETF does not define a standard MIB
-- for managing an OSI NCP. For consistency, this MIB follows the model of 
--- RFC1473 for IP NCP: 
-- A status table reports the condition of the NCP state machine, and the outcome 
--of option parameter negotiation (if any) when the OperStatus object has the
-- value 'opened(1)'; a configuration table provides administrative control over
-- the NCP state machine, and permits configuration of proposed option parameter
-- values (if any) to be used during NCP negotiation.
-- /////////////////////////////////////////////////////////////////////////////
-- PPP OSI Status Table
--
jnxPppOsiTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppOsiEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the OSI parameters for the local PPP entity."
    ::= { jnxPppOsi 1 }

jnxPppOsiEntry OBJECT-TYPE
    SYNTAX      JnxPppOsiEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "OSICP status information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { jnxPppOsiTable 1 }

JnxPppOsiEntry ::= SEQUENCE {
    jnxPppOsiServiceStatus          INTEGER,
    jnxPppOsiOperStatus             INTEGER,
    jnxPppOsiTerminateReason        INTEGER,
    jnxPppOsiTerminateNegFailOption INTEGER,
    jnxPppOsiLocalAlignNpdu         INTEGER,
    jnxPppOsiRemoteAlignNpdu        INTEGER }

jnxPppOsiServiceStatus OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether OSI protocol service is operating over this PPP link.
         Service is established on this link through means outside this MIB."
    ::= { jnxPppOsiEntry 1 }

jnxPppOsiOperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    opened(1),
                    notOpened(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational status of the OSI network protocol.  If the value of
         this object is up then the finite state machine for the OSI network
          protocol has reached the Opened state."
    ::= { jnxPppOsiEntry 2 }

jnxPppOsiTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    noService(2),
                    admin(3),
                    linkDown(4),
                    peerTerminated(5),
                    peerRenegotiated(6),
                    maxRetriesExceeded(7),
                    negotiationFailure(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the OSICP link was terminated:
            none                    None.
            other                   Not specified.
            noService               No OSI service configured on this PPP link.
            admin                   Administratively disabled.
            linkDown                Underlying link is down.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate IPCP option.  See
                                    jnxPppOsiTerminateNegFailOption."
    ::= { jnxPppOsiEntry 3 }

jnxPppOsiTerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localAlignNpdu(2),
                    remoteAlignNpdu(3) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP OSICP option for which negotiation failed, when 
        jnxPppOsiTerminateReason has the value 'negotiationFailure'."
    ::= { jnxPppOsiEntry 4 }

jnxPppOsiLocalAlignNpdu OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    oneModulo4(1),
                    twoModulo4(2),
                    threeModulo4(3),
                    fourModulo4(4),
                    even(254),
                    odd(255) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Local alignment of network PDU:
            none            No alignment specified.
            oneModulo4      Alignment on first octet (out of four).
            twoModulo4      Alignment on second octet (out of four).
            threeModulo4    Alignment on third octet (out of four).
            fourModulo4     Alignment on fourth octet (out of four).
            even            Alignment on even-octet boundary.
            odd             Alignment on odd-octet boundary."
    ::= { jnxPppOsiEntry 5 }

jnxPppOsiRemoteAlignNpdu OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    oneModulo4(1),
                    twoModulo4(2),
                    threeModulo4(3),
                    fourModulo4(4),
                    even(254),
                    odd(255) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote alignment of network PDU.
            none            No alignment specified.
            oneModulo4      Alignment on first octet (out of four).
            twoModulo4      Alignment on second octet (out of four).
            threeModulo4    Alignment on third octet (out of four).
            fourModulo4     Alignment on fourth octet (out of four).
            even            Alignment on even-octet boundary.
            odd             Alignment on odd-octet boundary."
    ::= { jnxPppOsiEntry 6 }

--
-- The PPP OSI Configuration Table
--
jnxPppOsiConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppOsiConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing configuration variables for the OSICP for the 
        local PPP entity."
    ::= { jnxPppOsi 2 }

jnxPppOsiConfigEntry   OBJECT-TYPE
    SYNTAX      JnxPppOsiConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "OSICP information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { jnxPppOsiConfigTable 1 }

JnxPppOsiConfigEntry ::= SEQUENCE {
    jnxPppOsiConfigAdminStatus  INTEGER }

jnxPppOsiConfigAdminStatus   OBJECT-TYPE
    SYNTAX      INTEGER {
                    open(1),
                    close(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The immediate desired status of the OSI network protocol. 
         Setting this object to open will inject an administrative open event
          into the OSI network protocol's finite state machine.  Setting this
           object to close will inject an administrative close event into the
            OSI network protocol's finite state machine."
    ::= { jnxPppOsiConfigEntry 1 }

-- /////////////////////////////////////////////////////////////////////////////
-- PPP Session
-- This section defines objects used to manage the PPP sessions.
-- The jnxPppSessionTable provides status of each PPP session.

-- /////////////////////////////////////////////////////////////////////////////
-- The PPP Session Table
--
jnxPppSessionTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for PPP interfaces present in the system."
    ::= { jnxPppSession 1 }

jnxPppSessionEntry OBJECT-TYPE
    SYNTAX      JnxPppSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a PPP interface."
    INDEX     { ifIndex }
    ::= { jnxPppSessionTable 1 }

JnxPppSessionEntry ::= SEQUENCE {
    jnxPppSessionGrant                         TruthValue,
    jnxPppSessionTerminateReason               INTEGER,
    jnxPppSessionStartTime                     TimeTicks,
    jnxPppSessionInOctets                      Counter32,
    jnxPppSessionOutOctets                     Counter32,
    jnxPppSessionInPackets                     Counter32,
    jnxPppSessionOutPackets                    Counter32,
    jnxPppSessionSessionTimeout                Integer32,
    jnxPppSessionInactivityTimeout             Integer32,
    jnxPppSessionAccountingInterval            Integer32,
    jnxPppSessionRemoteIpAddress               IpAddress,
    jnxPppSessionRemotePrimaryDnsAddress       IpAddress,
    jnxPppSessionRemoteSecondaryDnsAddress     IpAddress,
    jnxPppSessionRemotePrimaryWinsAddress      IpAddress,
    jnxPppSessionRemoteSecondaryWinsAddress    IpAddress,
    jnxPppSessionRemoteIpv6AddressIfIdentifier Ipv6AddressIfIdentifier,
    jnxPppSessionInhibitIp                     INTEGER,
    jnxPppSessionInhibitIpv6                   INTEGER,
    jnxPppSessionInOctets64                    Counter64,
    jnxPppSessionOutOctets64                   Counter64,
    jnxPppSessionInPackets64                   Counter64,
    jnxPppSessionOutPackets64                  Counter64}

jnxPppSessionGrant OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether a session has been granted via the authentication
        mechanism."
    ::= { jnxPppSessionEntry 1 }

jnxPppSessionTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    unknown(1),
                    userRequest(2),
                    keepaliveFailure(3),
                    sessionTimeout(4),
                    inactivityTimeout(5),
                    adminDisable(6),
                    lowerLayerDown(7),
                    noUpperInterface(8),
                    deny(9),
                    noHardware(10),
                    noResources(11),
                    noInterface(12),
                    challengeTimeout(13),
                    requestTimeout(14),
                    authenticatorTimeout(15),
                    addressLeaseExpired(16),
                    adminLogout(17),
                    tunnelFailed(18) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The reason the session was terminated."
    ::= { jnxPppSessionEntry 2 }

jnxPppSessionStartTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this session last became active."
    ::= { jnxPppSessionEntry 3 }

jnxPppSessionInOctets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "octets"
    MAX-ACCESS  read-only
    STATUS      deprecated 
    DESCRIPTION
        "Number of octets received since this session last became active, as 
        denoted by jnxPppSessionStartTime. This has been deprecated and 
        replaced by jnxPppSessionInOctets64"
    ::= { jnxPppSessionEntry 4 }

jnxPppSessionOutOctets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "octets"
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "Number of octets sent since this session last became active, as 
        denoted by jnxPppSessionStartTime. This has been deprecated and
        replaced by jnxPppSessionOutOctets64"
    ::= { jnxPppSessionEntry 5 }

jnxPppSessionInPackets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "Number of packets received since this session last became active, as
         denoted by jnxPppSessionStartTime. This has been deprecated and
         replaced by jnxPppSessionInPackets64"
    ::= { jnxPppSessionEntry 6 }

jnxPppSessionOutPackets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "Number of packets sent since this session last became active, as 
        denoted by jnxPppSessionStartTime. This has been deprecated and
        replaced by jnxPppSessionOutPackets64"
    ::= { jnxPppSessionEntry 7 }

jnxPppSessionSessionTimeout OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum duration for the session, after which the session terminates
         automatically."
    ::= { jnxPppSessionEntry 8 }

jnxPppSessionInactivityTimeout OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum inactivity duration for the session, after which the session
         terminates automatically."
    ::= { jnxPppSessionEntry 9 }

jnxPppSessionAccountingInterval OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Interval that must elapse between generation of accounting records
         for this session."
    ::= { jnxPppSessionEntry 10 }

jnxPppSessionRemoteIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote IP address, obtained from the authentication service, to be 
        used during IPCP negotiation with the remote side."
    ::= { jnxPppSessionEntry 11 }

jnxPppSessionRemotePrimaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote primary DNS IP address, obtained from the authentication 
        service, to be used during IPCP negotiation with the remote side."
    ::= { jnxPppSessionEntry 12 }

jnxPppSessionRemoteSecondaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote secondary DNS IP address, obtained from the authentication 
        service, to be used during IPCP negotiation with the remote side."
    ::= { jnxPppSessionEntry 13 }

jnxPppSessionRemotePrimaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote primary WINS IP address, obtained from the authentication
         service, to be used during IPCP negotiation with the remote side."
    ::= { jnxPppSessionEntry 14 }

jnxPppSessionRemoteSecondaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote secondary WINS IP address, obtained from the authentication
         service, to be used during IPCP negotiation with the remote side."
    ::= { jnxPppSessionEntry 15 }

jnxPppSessionRemoteIpv6AddressIfIdentifier OBJECT-TYPE
    SYNTAX      Ipv6AddressIfIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IPV6 Address Interface Identifier obtained from the authentication
         service, to be used during IPCP negotiation with the remote side."
    ::= { jnxPppSessionEntry 16 }

jnxPppSessionInhibitIp OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether a session has had its IP service inhibited by the
         authentication mechanism."
    ::= { jnxPppSessionEntry 17 }

jnxPppSessionInhibitIpv6 OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether a session has had its IPv6 service inhibited by the
         authentication mechanism."
    ::= { jnxPppSessionEntry 18 }

jnxPppSessionInOctets64 OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of octets received since this session last became active, as 
        denoted by jnxPppSessionStartTime."
    ::= { jnxPppSessionEntry 19 }

jnxPppSessionOutOctets64 OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of octets sent since this session last became active, as 
        denoted by jnxPppSessionStartTime."
    ::= { jnxPppSessionEntry 20 }

jnxPppSessionInPackets64 OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received since this session last became active, as
         denoted by jnxPppSessionStartTime."
    ::= { jnxPppSessionEntry 21 }

jnxPppSessionOutPackets64 OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets sent since this session last became active, as 
        denoted by jnxPppSessionStartTime."
    ::= { jnxPppSessionEntry 22 }


-- /////////////////////////////////////////////////////////////////////////////
-- Multi-Link PPP  (MLPPP)
-- This section defines objects used to manage the MLPPP.
-- /////////////////////////////////////////////////////////////////////////////
--
-- The MLPPP BundleTable
--
jnxPppMlPppBundleTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppMlPppBundleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP bundles present in the system."
    ::= { jnxPppMlPpp 1 }

jnxPppMlPppBundleEntry OBJECT-TYPE
    SYNTAX      JnxPppMlPppBundleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a MLPPP bundle."
    INDEX     { jnxPppMlPppBundleName }
    ::= { jnxPppMlPppBundleTable 1 }

JnxPppMlPppBundleEntry ::= SEQUENCE {
    jnxPppMlPppBundleName           JnxPppMlPppBundleName,
    jnxPppMlPppBundleRowStatus      RowStatus,
    jnxPppMlPppBundleNetworkIfIndex InterfaceIndex }

jnxPppMlPppBundleName OBJECT-TYPE
    SYNTAX      JnxPppMlPppBundleName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The administrative name of the MLPPP bundle associated with this
         MLPPP network interface."
    ::= { jnxPppMlPppBundleEntry 1 }

jnxPppMlPppBundleRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The rowStatus for this entry.  The following sets are supported 
        with read-create maximum access:
             createAndGo(4),
             destroy(6)

         The following values can be read from this object:
             active(1) "
    ::= { jnxPppMlPppBundleEntry 2 }

jnxPppMlPppBundleNetworkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of this MLPPP network interface.  It is a valid ifIndex
         even if there is no corresponding network interface instance in 
         the jnxPppMlPppLinkConfigTable."
    ::= { jnxPppMlPppBundleEntry 3 }

--
-- IfIndex selection for creating new MLPPP Link interfaces in
-- jnxPppLinkConfigTable.
--
-- NOTE: This object is placed after jnxPppLinkConfigTable so that jnxPppLinkStatusTable and jnxPppLinkConfigTable have the same relative MIB node positions below the jnxPppLcp node (jnxPppLcp.1 and jnxPppLcp.2, respectively) as their counterpart Status and Config tables in RFC1471.

jnxPppMlPppNextLinkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in 
        jnxPppMlPppLinkConfigTable. A GET of this object returns the next 
        available ifIndex value to be used to create an entry in the 
        associated interface table; or zero, if no valid ifIndex value is
        available.  This object also returns a value of zero when it is the
        lexicographic successor of a varbind presented in an SNMP GETNEXT 
        or GETBULK request, for which circumstance it is assumed that ifIndex
        allocation is unintended. Successive GETs will typically return 
        different values, thus avoiding collisions among cooperating management
        clients seeking to create table entries simultaneously."
    ::= { jnxPppMlPpp 2 }

--
-- The MLPPP Link Configuration Table
--
jnxPppMlPppLinkConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppMlPppLinkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP interfaces present in the system."
    ::= { jnxPppMlPpp 3 }

jnxPppMlPppLinkConfigEntry OBJECT-TYPE
    SYNTAX      JnxPppMlPppLinkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of MLPPP interface. 
        With read-create maximum access,creating/deleting entries in this
        table causes corresponding entries for be created/deleted in
       ifTable/ifXTable/jnxIfTable."
    INDEX     { jnxPppMlPppLinkConfigIfIndex }
    ::= { jnxPppMlPppLinkConfigTable 1 }

JnxPppMlPppLinkConfigEntry ::= SEQUENCE {
    jnxPppMlPppLinkConfigIfIndex                      InterfaceIndex,
    jnxPppMlPppLinkConfigLowerIfIndex                 InterfaceIndexOrZero,
    jnxPppMlPppLinkConfigKeepalive                    Integer32,
    jnxPppMlPppLinkConfigAuthentication               JnxPppAuthentication,
    jnxPppMlPppLinkConfigMaxAuthenRetries             Integer32,
    jnxPppMlPppLinkConfigRowStatus                    RowStatus,
    jnxPppMlPppLinkConfigAaaProfile                   OCTET STRING,
    jnxPppMlPppLinkConfigChapMinChallengeLength       Integer32,
    jnxPppMlPppLinkConfigChapMaxChallengeLength       Integer32,
    jnxPppMlPppLinkConfigPassiveMode                  INTEGER,
    jnxPppMlPppLinkConfigAuthenticatorLogicalSystem   OCTET STRING,
    jnxPppMlPppLinkConfigAuthenticatorRoutingInstance OCTET STRING,
    jnxPppMlPppLinkConfigFragmentation                INTEGER,
    jnxPppMlPppLinkConfigReassembly                   INTEGER,
    jnxPppMlPppLinkConfigMaxReceiveReconstructedUnit  Integer32,
    jnxPppMlPppLinkConfigFragmentSize                 Integer32,
    jnxPppMlPppLinkConfigHashLinkSelection            INTEGER,
    jnxPppMlPppLinkConfigAuthentication2              JnxNibbleConfig,
    jnxPppMlPppLinkConfigIgnoreMagicNumberMismatch    INTEGER,
    jnxPppMlPppLinkConfigMultilinkMulticlass          INTEGER,
    jnxPppMlPppLinkConfigMultilinkMaxMultiClasses     INTEGER}

jnxPppMlPppLinkConfigIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the MLPPP interface.  When creating entries in this 
        table, suitable values for this object are determined by reading 
        jnxPppMlPppNextLinkIfIndex."
    ::= { jnxPppMlPppLinkConfigEntry 1 }

jnxPppMlPppLinkConfigLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of an interface over which this PPP interface is to be 
        layered.  A value of zero indicates no layering.  An implementation 
        may choose to require that a non-zero value be configured at entry
         creation."
    ::= { jnxPppMlPppLinkConfigEntry 2 }

jnxPppMlPppLinkConfigKeepalive OBJECT-TYPE
    SYNTAX      Integer32 (0|10..64800)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Keepalive interval in seconds.  A value of zero disables keepalive.
         Keepalive is performed using LCP Echo."
    DEFVAL    { 30 }
    ::= { jnxPppMlPppLinkConfigEntry 4 }

jnxPppMlPppLinkConfigAuthentication OBJECT-TYPE
    SYNTAX      JnxPppAuthentication
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "Specifies the type(s) of authentication, if any, to be 
        negotiated with the peer:
          none      No authentication is negotiated.
          pap       PAP negotiation only.
          chap      CHAP negotiation only.
          papChap   PAP negotiation is attempted first; if fails, attempt CHAP.
          chapPap   CHAP negotiation is attempted first; if fails, attempt PAP.

       If authentication negotiation is not supported for this MLPPP interface,
       then any attempt to explicitely set this object will result in a 
       notWritable error and it will be implicitily set to the DEFVAL on
       row creation. 
       This object returns a none (0) value on the get operation.
       New object jnxPppMlPppLinkConfigAuthentication2 will reflect the configured 
       values. Setting this object along with the jnxPppMlPppLinkConfigAuthentication2
        object will return an inconsistentValue error."
    DEFVAL    { none }
    ::= { jnxPppMlPppLinkConfigEntry 5 }

jnxPppMlPppLinkConfigMaxAuthenRetries OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of authentication retries permitted, in addition to a
         failed initial attempt.  If all retries fail, the link is reset."
    DEFVAL    { 0 }
    ::= { jnxPppMlPppLinkConfigEntry 6 }

jnxPppMlPppLinkConfigRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with read-carete 
        maximum access,according to the RowStatus textual convention, 
        constrained to support the following values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be 
        explicitly configured:
            jnxPppMlPppLinkConfigRowStatus
            jnxPppMlPppLinkConfigLowerIfIndex
        In addition, when creating an entry the following conditions must hold:
            A value for jnxPppMlPppLinkConfigIndex must have been
             determined previously, by reading jnxPppMlPppNextIfIndex. 
             The interface identified by jnxPppMlPppLinkConfigLowerIfIndex
             must exist.
            A corresponding entry in ifTable/ifXTable/jnxIfTable is 
            created/destroyed as a result of creating/destroying an entry in 
            this table.

        The following values can be read from this object:
             active(1) "
    ::= { jnxPppMlPppLinkConfigEntry 7 }

jnxPppMlPppLinkConfigAaaProfile OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the AAA profile to be used for authentication on the 
        PPP interface.Setting this object statically binds the AAA profile
        with the PPP interface. If this object is not explicitly set or it
        is set to null string, then this object is ignored. On a Set operation,
        if the value of this object is not null and does not correspond to an
         existin AAA profile, then an inconsistentValue error is returned."
    ::= { jnxPppMlPppLinkConfigEntry 8 }

jnxPppMlPppLinkConfigChapMinChallengeLength OBJECT-TYPE
    SYNTAX      Integer32 (8..63)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Minimum value of the CHAP authenticator challenge length value.
       This value is never allowed to be set to a value greater than 
       jnxPppMlPppLinkConfigChapMaxChallengeLength."
    DEFVAL    { 16 }
    ::= { jnxPppMlPppLinkConfigEntry 9 }

jnxPppMlPppLinkConfigChapMaxChallengeLength OBJECT-TYPE
    SYNTAX      Integer32 (8..63)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum value of the CHAP authenticator challenge length value."
    DEFVAL    { 32 }
    ::= { jnxPppMlPppLinkConfigEntry 10 }

jnxPppMlPppLinkConfigPassiveMode OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When enabled, LCP state machine is forced into passive mode on lower 
        layer UP message.  It adds compatibility with slow and buggy clients."
    DEFVAL    { disable }
    ::= { jnxPppMlPppLinkConfigEntry 11 }

jnxPppMlPppLinkConfigAuthenticatorLogicalSystem OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the Logical System (Jnxper-ROUTER-MIB.jnxRouterName) to 
        be used for authentication on the PPP interface.  Setting this object
         statically binds the authenticating virtual router with the link interface.
         With read-create maximum access, if this object is not explicitly set or 
         it is set to null string, then this object is ignored and the
          virtual router used for     authentication is determined by other means.
            On a Set operation, if the value of this object is not null and does not
             correspond to an existing virtual router, then an inconsistentValue
              error is returned."
    ::= { jnxPppMlPppLinkConfigEntry 12 }

 jnxPppMlPppLinkConfigAuthenticatorRoutingInstance OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the Routing Instance (Jnxper-ROUTER-MIB.jnxRouterName) 
        to be used for authentication on the PPP interface.  Setting this 
        object statically binds the authenticating virtual router with the 
        link interface. With read-create maximum access, if this object is
         not explicitly set or it is set to null string, then this object is
          ignored and the virtual router used for     authentication is
           determined by other means.  On a Set operation, if the value of
            this object is not null and does not correspond to an existing
             virtual router, then an inconsistentValue error is returned."
    ::= { jnxPppMlPppLinkConfigEntry 13 }

jnxPppMlPppLinkConfigFragmentation OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables MLPPP fragmentation.With read-create maximum access,
        changing this object has an effect when the link is next restarted."
    DEFVAL    { disable }
    ::= { jnxPppMlPppLinkConfigEntry 14 }

jnxPppMlPppLinkConfigReassembly OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables MLPPP reassembly. With read-create maximum access,
         changing this object has an effect when the link is next restarted."
    DEFVAL    { disable }
    ::= { jnxPppMlPppLinkConfigEntry 15 }

jnxPppMlPppLinkConfigMaxReceiveReconstructedUnit OBJECT-TYPE
    SYNTAX      Integer32 (1|64..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Maximum Receive Reconstructed Unit (MRRU) that the local 
        PPP entity will advertise to the remote entity.  If the value of
        this variable is 1, then the MRRU is set to the local MRU value. 
        With read-create maximum access, changing this object has an effect
        when the link is next restarted."
    DEFVAL    { 1 }
    ::= { jnxPppMlPppLinkConfigEntry 16 }

jnxPppMlPppLinkConfigFragmentSize OBJECT-TYPE
    SYNTAX      Integer32 (1|128..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The size of fragments transmitted by the local PPP entity.
        If the value of this variable is 1, then the fragment size is set to 
        the link's MTU value. With read-create maximum access, 
        changing this object has an effect when the link is next restarted."
    DEFVAL    { 1 }
    ::= { jnxPppMlPppLinkConfigEntry 17 }

jnxPppMlPppLinkConfigHashLinkSelection OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables MLPPP hash-based link selection for non-best-effort traffic.
        With read-create maximum access,changing this object has an effect
         when the link is next restarted."
    DEFVAL    { disable }
    ::= { jnxPppMlPppLinkConfigEntry 18 }

jnxPppMlPppLinkConfigAuthentication2 OBJECT-TYPE
    SYNTAX      JnxNibbleConfig
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A configuration variable comprised of nibbles i.e. 4 bits, such 
        that a client can supply a list of 0 to 8 selections.  The least
         significant nibble is the first value of the list, and the most 
         significant nibble is the last value.  The value in each field
         ranges from 0 to 15, however the first nibble with value 0 indicates
          the end of the list.  Repetition of values is not allowed. 
          Segregation of values is not allowed.

         Valid Values are:
         none - 0
         pap  - 1
         chap - 2
         eap  - 3

         Example valid encoding:
         0x00000321
         0x00000012

         Not a valid encoding:
         0x00000121
         0x01002001

         If authentication negotiation is not supported for this PPP interface
         and With read-create maximum access, then any attempt to explicitly 
         set this object will result in a notWritable error and it will be 
         implicitly set to the DEFVAL on row creation. Setting this object to 
         null will set jnxPppMlPppLinkConfigAuthenticatorVirtualRouter object 
         to an empty string.Setting this object along with the 
         jnxPppMlPppLinkConfigAuthentication object will return an i
         nconsistentValue error."
    DEFVAL    { 0 }
    ::= { jnxPppMlPppLinkConfigEntry 19 }
    
jnxPppMlPppLinkConfigIgnoreMagicNumberMismatch OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The ignore magic number mismatch option of the PPP interface determines
         the action to be taken, when the peer has not negotiated any value yet
          sent null or invalid magic number in the LCP echo packets. The two 
          actions that can be configured are:
            1)	Ignore the mismatch and retain connection
            2)	Disallow the mismatch and terminate connection"
    DEFVAL    { disable }
    ::= { jnxPppMlPppLinkConfigEntry 20 }

jnxPppMlPppLinkConfigMultilinkMulticlass OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables Multiclass Multilink PPP (MCML). With read-create maximum
         access,changing this object has an effect when the link is next
          restarted."
    DEFVAL    {disable}
    ::= { jnxPppMlPppLinkConfigEntry 21 }

jnxPppMlPppLinkConfigMultilinkMaxMultiClasses OBJECT-TYPE
    SYNTAX      INTEGER (0..8)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of MCML classes to be negotiated.With read-create
         maximum access,changing this object has an effect when the link
          is next restarted."
    DEFVAL    {0}
    ::= { jnxPppMlPppLinkConfigEntry 22 }

jnxPppMlPppNextNetworkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in
        jnxPppMlPppNetworkConfigTable. A GET of this object returns the next
        available ifIndex value to be used to create an entry in the associated
        interface table; or zero, if no        valid ifIndex value is available.
        This object also returns a value of zero when it is the lexicographic
        successor of a varbind presented in an SNMP GETNEXT or GETBULK request,
        for which circumstance it is assumed that ifIndex allocation 
        is unintended. Successive GETs will typically return different values,
         thus avoiding collisions among cooperating management clients seeking 
         to create table entries simultaneously."
    ::= { jnxPppMlPpp 4 }


--
-- The MLPPP Network Configuration Table
--
jnxPppMlPppNetworkConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppMlPppNetworkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP network interfaces 
        present in the system."
    ::= { jnxPppMlPpp 5 }

jnxPppMlPppNetworkConfigEntry OBJECT-TYPE
    SYNTAX      JnxPppMlPppNetworkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of MLPPP interface.
         With read-create maximum access,creating/deleting entries in 
         this table causes corresponding entries for be created/deleted 
         in ifTable/ifXTable/jnxIfTable."
    INDEX     { jnxPppMlPppNetworkConfigIfIndex }
    ::= { jnxPppMlPppNetworkConfigTable 1 }

JnxPppMlPppNetworkConfigEntry ::= SEQUENCE {
    jnxPppMlPppNetworkConfigIfIndex         InterfaceIndex,
    jnxPppMlPppNetworkConfigLowerIfIndex    InterfaceIndex,
    jnxPppMlPppNetworkBundleName            JnxPppMlPppBundleName,
    jnxPppMlPppNetworkRowStatus             RowStatus }

jnxPppMlPppNetworkConfigIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the MLPPP network interface.  When creating entries
         in this table, suitable values for this object are determined by 
         reading jnxPppMlPppNextNetworkIfIndex."
    ::= { jnxPppMlPppNetworkConfigEntry 1 }

jnxPppMlPppNetworkConfigLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of a PPP link interface over which this PPP network 
        interface is to be layered.  On sets, the value of this object must 
        equal on of the previously created PPP link interfaces created in 
        the jnxPppMlPppLinkConfigTable.  On gets, the value of this object 
        is the lexicographically least PPP link interface in a potential
         bundle of PPP link interfaces."
    ::= { jnxPppMlPppNetworkConfigEntry 2 }

jnxPppMlPppNetworkBundleName OBJECT-TYPE
    SYNTAX     JnxPppMlPppBundleName
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The MLPPP bundle name administratively assigned."
    ::= { jnxPppMlPppNetworkConfigEntry 3 }

jnxPppMlPppNetworkRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with read-create
         maximum access , according to the RowStatus textual convention,
          constrained to support the following values only:
            createAndGo
            destroy
        To create an entry in this table, the following entry objects MUST be 
        explicitly configured:

            jnxPppMlPppNetworkConfigLowerIfIndex
            jnxPppMlPppNetworkBundleName
            jnxPppMlPppNetworkConfigRowStatus

        In addition, when creating an entry the following conditions must hold:
           A value for jnxPppMlPppNetworkConfigIndex must have been determined
            previously, by reading jnxPppMlPppNextNetworkIfIndex. The 
            interface identified by jnxPppMlPppNetworkConfigLowerIfInde must 
            exist by a creation request to the jnxPppMlPppLinkConfigTable.
           The bundleName specified in jnxPppMlPppNetworkBundleName must have
            been created first in the jnxPppMlPppBundleTable. A corresponding
             entry in ifTable/ifXTable/jnxIfTable is created/destroyed as a 
             result of creating/destroying an entry in this table.

        The following values can be read from this object:
             active(1) "
    ::= { jnxPppMlPppNetworkConfigEntry 4 }


--
-- The MLPPP Link Bind Table
--
jnxPppMlPppLinkBindTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppMlPppLinkBindEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP Link interface to MLPPP 
        network interfaces bindings."
    ::= { jnxPppMlPpp 6 }

jnxPppMlPppLinkBindEntry OBJECT-TYPE
    SYNTAX      JnxPppMlPppLinkBindEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the MLPPP link interface to MLPPP network 
        interface bindings."
    INDEX     { jnxPppMlPppBindNetworkIfIndex,
                jnxPppMlPppBindLinkIfIndex }
    ::= { jnxPppMlPppLinkBindTable 1 }

JnxPppMlPppLinkBindEntry ::= SEQUENCE {
    jnxPppMlPppBindNetworkIfIndex   InterfaceIndex,
    jnxPppMlPppBindLinkIfIndex      InterfaceIndex,
    jnxPppMlPppBindRowStatus        RowStatus }

jnxPppMlPppBindNetworkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the MLPPP network interface."
    ::= { jnxPppMlPppLinkBindEntry 1 }

jnxPppMlPppBindLinkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of a MLPPP link interface bound by the MLPPP network
         interface defined by jnxPppMlPppBindNetworkIfIndex."
    ::= { jnxPppMlPppLinkBindEntry 2 }

jnxPppMlPppBindRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table with read-create
         maximum access, according to the RowStatus textual convention, 
         constrained to support the following values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST
        be explicitly configured:
            jnxPppMlPppBindRowStatus

        In addition, when creating an entry the following conditions must hold:
        The interfaces identified by jnxPppMlPppBindNetworkIfIndex and 
        jnxPppMlPppBindLinkIfIndex must be created in the 
        jnxPppMlPppNetworkConfigTable and jnxPppMlPppLinkConfigTable 
        respectively. A MLPPP bundle must be associated with the 
        jnxPppMlPppNetworkIfIndex and exist in the jnxPppMibPppBundleTable. 
        A corresponding entry in ifStackTable is created/destroyed as a result
         of creating/destroying an entry in this table.

        The following values can be read from this object:
             active(1) "
    ::= { jnxPppMlPppLinkBindEntry 3 }

-- /////////////////////////////////////////////////////////////////////////////
-- PPP Interface Summary Counts
-- /////////////////////////////////////////////////////////////////////////////

jnxPppSummaryPppInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces configured in the system."
    ::= { jnxPppSummary 1 }

jnxPppSummaryPppIpNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IP NCPs configured in the system."
    ::= { jnxPppSummary 2 }

jnxPppSummaryPppOsiNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs configured in the system."
    ::= { jnxPppSummary 3 }

jnxPppSummaryPppIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system that are
         administratively configured to up(1)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { jnxPppSummary 4 }

jnxPppSummaryPppIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system that are
         administrateively configued to down(2)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { jnxPppSummary 5 }

jnxPppSummaryPppIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an 
        operational state of up(1)."
    REFERENCE
        "IF-MIB.ifOperstatus"
    ::= { jnxPppSummary 7 }

jnxPppSummaryPppIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an 
        operational state of down(2)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 8 }

jnxPppSummaryPppIfOperDormant OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an
         operational state of dormant(5)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 9 }

jnxPppSummaryPppIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an 
        operational state of notPresent(6)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 10 }

jnxPppSummaryPppIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an 
        operational state of lowerLayerDown(7)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 11 }

jnxPppSummaryPppIpNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an
         operational state of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 12 }

jnxPppSummaryPppIpNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an 
        operational state of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 13 }

jnxPppSummaryPppOsiNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an 
        operational state of opened."
    ::= { jnxPppSummary 14 }

jnxPppSummaryPppOsiNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an 
        operational state of closed."
    ::= { jnxPppSummary 15 }

jnxPppSummaryPppIfLastChangeTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The value of the sysUpTime at the time of the last PPP interface
         creation or deletion in the system.  If the number of PPP interfaces has been unchanged since the last re-initialization of the system, then this object contains a zero value. "
    ::= { jnxPppSummary 16 }

jnxPppSummaryPppLinkInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces configured in the system."
    ::= { jnxPppSummary 17 }

jnxPppSummaryPppLinkIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system that are
         administratively configured to up(1)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { jnxPppSummary 18 }

jnxPppSummaryPppLinkIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system that are
         administrateively configued to down(2)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { jnxPppSummary 19 }

jnxPppSummaryPppLinkIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an 
        operational state of up(1)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 20 }

jnxPppSummaryPppLinkIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an
         operational state of down(2)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 21 }

jnxPppSummaryPppLinkIfOperDormant OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an 
        operational state of dormant(5)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 22 }

jnxPppSummaryPppLinkIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP link interfaces in the system with an
         operational state of notPresent(6)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 23 }

jnxPppSummaryPppLinkIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an 
        operational state of lowerLayerDown(7)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 24 }

jnxPppSummaryPppLinkIfLastChangeTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The value of the sysUpTime at the time of the last PPP Link interface
         creation or deletion in the system.  If the number of PPP interfaces has been unchanged since the last re-initialization of the system, then this object contains a zero value. "
    ::= { jnxPppSummary 25 }

jnxPppSummaryPppNetworkInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces configured in the system."
    ::= { jnxPppSummary 26 }

jnxPppSummaryPppNetworkIpNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IP NCPs in the system configured on 
        PPP network interfaces."
    ::= { jnxPppSummary 27 }

jnxPppSummaryPppNetworkOsiNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on 
        PPP network interfaces."
    ::= { jnxPppSummary 28 }

jnxPppSummaryPppNetworkIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system that are
         administratively configured to up(1)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { jnxPppSummary 29 }

jnxPppSummaryPppNetworkIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system that are 
        administrateively configued to down(2)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { jnxPppSummary 30 }

jnxPppSummaryPppNetworkIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
         operational state of up(1)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 31 }

jnxPppSummaryPppNetworkIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an 
        operational state of down(2)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 32 }

jnxPppSummaryPppNetworkIfOperDormant OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS   read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
         operational state of dormant(5)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 33 }

jnxPppSummaryPppNetworkIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
         operational state of notPresent(6)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 34 }

jnxPppSummaryPppNetworkIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
         operational state of lowerLayerDown(7)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { jnxPppSummary 35 }

jnxPppSummaryPppNetworkIpNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational 
        state of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 36 }

jnxPppSummaryPppNetworkIpNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational 
        state of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 37 }

jnxPppSummaryPppNetworkOsiNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational 
        state of opened."
    ::= { jnxPppSummary 38 }

jnxPppSummaryPppNetworkOsiNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational
        state of closed."
    ::= { jnxPppSummary 39 }

jnxPppSummaryPppNetworkIfLastChangeTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the sysUpTime at the time of the last PPP network
        interface creation or deletion in the system.  If the number of PPP
        network interfaces has been unchanged since the last re-initialization
        of the system, then this object contains a zero value. "
    ::= { jnxPppSummary 40 }

jnxPppSummaryPppIpv6NCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IPv6 NCPs configured in the system."
    ::= { jnxPppSummary 41 }

jnxPppSummaryPppIpv6NcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 42 }

jnxPppSummaryPppIpv6NcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 43 }

jnxPppSummaryPppNetworkIpv6NCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IPv6 NCPs configured in the system."
    ::= { jnxPppSummary 44 }

jnxPppSummaryPppNetworkIpv6NcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 45 }

jnxPppSummaryPppNetworkIpv6NcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 46 }

jnxPppSummaryPppStaticInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of static PPP interfaces configured in the system."
    ::= { jnxPppSummary 47 }

jnxPppSummaryPppMplsNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number MPLS NCPs configured in the system."
    ::= { jnxPppSummary 48 }

jnxPppSummaryPppIpAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system that are
        administratively configured to open(1)."
    ::= { jnxPppSummary 49 }

jnxPppSummaryPppIpAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system that are
        administratively configured to close(2)."
    ::= { jnxPppSummary 50 }

jnxPppSummaryPppIpv6AdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system that are
        administratively configured to open(1)."
    ::= { jnxPppSummary 51 }

jnxPppSummaryPppIpv6AdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system that are
        administratively configured to close(2)."
    ::= { jnxPppSummary 52 }

jnxPppSummaryPppOsiAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system that are
        administratively configured to open(1)."
    ::= { jnxPppSummary 53 }

jnxPppSummaryPppOsiAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system that are
        administratively configured to close(2)."
    ::= { jnxPppSummary 54 }

jnxPppSummaryPppMplsAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system that are
        administratively configured to open(1)."
    ::= { jnxPppSummary 55 }

jnxPppSummaryPppMplsAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system that are
        administratively configured to close(2)."
    ::= { jnxPppSummary 56 }

jnxPppSummaryPppIpNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational state
        of notPresent(3)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 57}

jnxPppSummaryPppIpNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational
        state of noResources(4)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 58 }

jnxPppSummaryPppIpv6NcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPV6 NCPs in the system with an operational state
        of notPresent(3)."
    ::= { jnxPppSummary 59 }

jnxPppSummaryPppIpv6NcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPV6 NCPs in the system with an operational
        state of noResources(4)."
    ::= { jnxPppSummary 60 }

jnxPppSummaryPppOsiNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational state
        of notPresent(3)."
    ::= { jnxPppSummary 61 }

jnxPppSummaryPppOsiNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational
        state of noResources(4)."
    ::= { jnxPppSummary 62 }

jnxPppSummaryPppMplsNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational state
        of opened(1)."
    ::= { jnxPppSummary 63 }

jnxPppSummaryPppMplsNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational
        state of not-opened(2)."
    ::= { jnxPppSummary 64 }

jnxPppSummaryPppMplsNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational state
        of notPresent(3)."
    ::= { jnxPppSummary 65 }

jnxPppSummaryPppMplsNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational
        state of noResources(4)."
    ::= { jnxPppSummary 66 }

jnxPppSummaryPppLinkStaticInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of static PPP Link interfaces configured in the system."
    ::= { jnxPppSummary 67 }

jnxPppSummaryPppNetworkStaticInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of static PPP network interfaces configured in the system."
    ::= { jnxPppSummary 68 }

jnxPppSummaryPppNetworkMplsNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces."
    ::= { jnxPppSummary 69 }

jnxPppSummaryPppNetworkIpAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { jnxPppSummary 70 }

jnxPppSummaryPppNetworkIpAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { jnxPppSummary 71 }

jnxPppSummaryPppNetworkIpv6AdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { jnxPppSummary 72 }

jnxPppSummaryPppNetworkIpv6AdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { jnxPppSummary 73 }

jnxPppSummaryPppNetworkOsiAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { jnxPppSummary 74 }

jnxPppSummaryPppNetworkOsiAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { jnxPppSummary 75 }

jnxPppSummaryPppNetworkMplsAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { jnxPppSummary 76 }

jnxPppSummaryPppNetworkMplsAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { jnxPppSummary 77 }

jnxPppSummaryPppNetworkIpNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 78 }

jnxPppSummaryPppNetworkIpNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { jnxPppSummary 79 }

jnxPppSummaryPppNetworkIpv6NcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    ::= { jnxPppSummary 80 }

jnxPppSummaryPppNetworkIpv6NcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    ::= { jnxPppSummary 81 }

jnxPppSummaryPppNetworkOsiNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    ::= { jnxPppSummary 82 }

jnxPppSummaryPppNetworkOsiNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    ::= { jnxPppSummary 83 }

jnxPppSummaryPppNetworkMplsNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of opened(1)."
    ::= { jnxPppSummary 84 }

jnxPppSummaryPppNetworkMplsNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of not-opened(2)."
    ::= { jnxPppSummary 85 }

jnxPppSummaryPppNetworkMplsNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    ::= { jnxPppSummary 86 }

jnxPppSummaryPppNetworkMplsNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    ::= { jnxPppSummary 87 }

-- ////////////////////////////////////////////////////////////////////////////
--
-- PPP IPv6 NCP
--
-- This section defines objects used to manage the PPP Network
-- Control Protocol for IPv6 protocol operation (IPV6CP).
--
-- ////////////////////////////////////////////////////////////////////////////
--
-- The PPP IPv6 Table
--
jnxPppIpv6Table OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppIpv6Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the IPv6 parameters for the local PPP entity."
    ::= { jnxPppIpv6 1 }

jnxPppIpv6Entry OBJECT-TYPE
    SYNTAX      JnxPppIpv6Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPV6CP status information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { jnxPppIpv6Table 1 }

JnxPppIpv6Entry ::= SEQUENCE {
    jnxPppIpv6ServiceStatus                       INTEGER,
    jnxPppIpv6OperStatus                          INTEGER,
    jnxPppIpv6TerminateReason                     INTEGER,
    jnxPppIpv6TerminateNegFailOption              INTEGER,
    jnxPppIpv6LocalIpv6AddressIfIdentifier        Ipv6AddressIfIdentifier,
    jnxPppIpv6RemoteIpv6AddressIfIdentifier       Ipv6AddressIfIdentifier,
    jnxPppIpv6NetworkStatusIpv6cpRenegoTerminates Counter32}

jnxPppIpv6ServiceStatus OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether IPv6 protocol service is operating over this PPP
        link.  Service is established on this link through means outside this
        MIB."
    ::= { jnxPppIpv6Entry 1 }

jnxPppIpv6OperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    opened(1),
                    notOpened(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational status of the IPv6 network protocol.  If the value of
        this object is up then the finite state machine for the IPv6 network
        protocol has reached the Opened state."
    ::= { jnxPppIpv6Entry 2 }

jnxPppIpv6TerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    noService(2),
                    admin(3),
                    linkDown(4),
                    peerTerminated(5),
                    peerRenegotiated(6),
                    maxRetriesExceeded(7),
                    negotiationFailure(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the IPV6CP link was terminated:
            none                    None.
            other                   Not specified.
            noService              No IPv6 service configured on this PPP link.
            admin                   Administratively disabled.
            linkDown                Underlying link is down.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate IPV6CP option.  See
                                    jnxPppIpv6TerminateNegFailOption."
    ::= { jnxPppIpv6Entry 3 }

jnxPppIpv6TerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localIpv6AddressIfIdentifier(2),
                    remoteIpv6AddressIfIdentifier(3) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP IPV6CP option for which negotiation failed, when
        jnxPppIpv6TerminateReason has the value 'negotiationFailure'."
    ::= { jnxPppIpv6Entry 4 }

jnxPppIpv6LocalIpv6AddressIfIdentifier OBJECT-TYPE
    SYNTAX      Ipv6AddressIfIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IPv6 Address Interface Identifier used by the local side."
    ::= { jnxPppIpv6Entry 5 }

jnxPppIpv6RemoteIpv6AddressIfIdentifier OBJECT-TYPE
    SYNTAX      Ipv6AddressIfIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IPv6 Address Interface Identifier used by the remote side."
    ::= { jnxPppIpv6Entry 6 }

jnxPppIpv6NetworkStatusIpv6cpRenegoTerminates OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times ipv6cp terminated due to peer exceeding max
        renegotiation attempts."
    ::= { jnxPppIpv6Entry 7 }

--
-- The PPP IPv6 Config Table
--
jnxPppIpv6ConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JnxPppIpv6ConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the IPv6 parameters for the local PPP entity."
    ::= { jnxPppIpv6 2 }

jnxPppIpv6ConfigEntry OBJECT-TYPE
    SYNTAX      JnxPppIpv6ConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPV6CP configuration information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { jnxPppIpv6ConfigTable 1 }

JnxPppIpv6ConfigEntry ::= SEQUENCE {
    jnxPppIpv6ConfigAdminStatus            INTEGER,
    jnxPppIpv6ConfigInitiateIpv6           INTEGER,
    jnxPppIpv6ConfigMaxIpv6cpRenegotiation Integer32 }

jnxPppIpv6ConfigAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    open(1),
                    close(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The immediate desired status of the IPv6 network protocol.  Setting
        this object to open will inject an administrative open event into the
        IPv6 network protocol's finite state machine.  Setting this object to
        close will inject an administrative close event into the IPv6 network
        protocol's finite state machine."
    ::= { jnxPppIpv6ConfigEntry 1 }

jnxPppIpv6ConfigInitiateIpv6 OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Enables the initiation of negotiation of the IPv6CP."
    DEFVAL { disable }
    ::= { jnxPppIpv6ConfigEntry 2 }

jnxPppIpv6ConfigMaxIpv6cpRenegotiation OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of allowed ipv6cp renegotiation attempts from peer."
    DEFVAL { 30 }
    ::= { jnxPppIpv6ConfigEntry 3 }


-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP Globals
--
--  The globals are non interface based objects
--
-- /////////////////////////////////////////////////////////////////////////////
jnxPppPeerIpAddressOptional OBJECT-TYPE
    SYNTAX          INTEGER  { enable(1), disable(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This option is used to ignore the conflicts between ppp client's  
         requested IP address and radius/local pool returned address in server 
         during IPNCP  negotiation. Enabling this will ensure the IPNCP  
         negotiation to succeed even though the client does not include 
         IP address option in the  IPNCP configure request."    
    ::= { jnxPppGlobalConfig 1 }



END
