WATCHGUARD-IPSEC-SA-MON-MIB-EXT DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, Counter32, Gauge32,
       Integer32, Integer32, NOTIFICATION-TYPE,
       OBJECT-IDENTITY, enterprises 
                                       FROM SNMPv2-SMI
       TEXTUAL-CONVENTION, TruthValue
                                       FROM SNMPv2-TC
       ifIndex                         FROM RFC1213-MIB
       IpsecDoiIdentType,
       IpsecDoiEncapsulationMode,
       IpsecDoiEspTransform,
       IpsecDoiAhTransform,
       IpsecDoiAuthAlgorithm,
       IpsecDoiIpcompTransform,
       IpsecDoiSecProtocolId
                                       FROM IPSEC-ISAKMP-IKE-DOI-TC
       watchguard
                                       FROM WATCHGUARD-MIB;

    wgIpsecSaMonModule MODULE-IDENTITY
        LAST-UPDATED "200701251200Z"
        ORGANIZATION "WatchGuard Technologies, Inc."
        CONTACT-INFO
                  "   Ella Yu
                      WatchGuard Technologies, Inc.
                      1841 Zanker Road
                      San Jose, CA 95112
                      USA

                      408-519-4888
                      ella.yu@watchguard.com "

        DESCRIPTION
            "The MIB module describes generic IPSec objects
            defined in IETF working draft 
            'draft-ieft-ipsec-monitor-mib-01' and WatchGuard's
            extension."
        REVISION      "200701251200Z"
        DESCRIPTION
            "Initial revision."
        ::= { watchguard 3 }

    IpsecSaCreatorIdent ::= TEXTUAL-CONVENTION
        DISPLAY-HINT "d"
        STATUS      current
        DESCRIPTION
            "A value indicating how an SA was created."
        SYNTAX      INTEGER {
                        unknown(0),
                        static(1),     -- statically created
                        ike(2),        -- IKE
                        other(3)
                    }

    IpsecIpv6Address ::= TEXTUAL-CONVENTION
        DISPLAY-HINT "2x:2x:2x:2x:2x:2x:1d.1d.1d.1d"
        STATUS      current
        DESCRIPTION
            "This data type is used to model IPv6 address prefixes. This
            is a binary string of 16 octets in network byte-order."
        SYNTAX      OCTET STRING (SIZE (16))

    wgIpsecSaMonitorMIB OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This is the base object identifier for all IPSec branches."
        ::= { wgIpsecSaMonModule 1 }

   -- significant branches

    wgSaTables OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This is the base object identifier for all SA tables."
        ::= { wgIpsecSaMonitorMIB 1 }

    wgSaStatistics OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This is the base object identifier for all objects which
            are global counters for IPSec security associations."
        ::= { wgIpsecSaMonitorMIB 2 }

    wgSaErrors OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This is the base object identifier for all objects which
            are global error counters for IPSec security associations."
        ::= { wgIpsecSaMonitorMIB 3 }

    -- the IPSec Inbound ESP MIB-Group
    --
    -- a collection of objects providing information about
    -- IPSec Inbound ESP SAs

    wgIpsecSaEspInTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF WGIpsecSaEspInEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The (conceptual) table containing information on IPSec
            inbound ESP SAs.

            There should be one row for every inbound ESP security
            association that exists in the entity. The maximum number of
            rows is implementation dependent."
        ::= { wgSaTables 1 }

    wgIpsecSaEspInEntry OBJECT-TYPE
        SYNTAX      WGIpsecSaEspInEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry (conceptual row) containing the information on a
            particular IPSec inbound ESP SA.

            A row in this table cannot be created or deleted by SNMP
            operations on columns of the table."
        INDEX{ wgIpsecSaEspInAddress, wgIpsecSaEspInSpi }
        ::= { wgIpsecSaEspInTable 1 }

    WGIpsecSaEspInEntry ::= SEQUENCE {

    wgIpsecSaEspInAddress       IpAddress,
    wgIpsecSaEspInSpi           Integer32,

    wgIpsecSaEspInDestId        OCTET STRING,
    wgIpsecSaEspInDestIdType    IpsecDoiIdentType,
    wgIpsecSaEspInSourceId      OCTET STRING,
    wgIpsecSaEspInSourceIdType  IpsecDoiIdentType,
    wgIpsecSaEspInProtocol      Integer32,
    wgIpsecSaEspInDestPort      Integer32,
    wgIpsecSaEspInSourcePort    Integer32,

    wgIpsecSaEspInCreator       IpsecSaCreatorIdent,

    wgIpsecSaEspInEncapsulation IpsecDoiEncapsulationMode,
    wgIpsecSaEspInEncAlg        IpsecDoiEspTransform,
    wgIpsecSaEspInEncKeyLength  Integer32,
    wgIpsecSaEspInAuthAlg       IpsecDoiAuthAlgorithm,

    wgIpsecSaEspInLimitSeconds  Integer32,
    wgIpsecSaEspInLimitKbytes   Integer32,

    wgIpsecSaEspInAccSeconds    Counter32,
    wgIpsecSaEspInAccKbytes     Counter32,
    wgIpsecSaEspInUserOctets    Counter32,
    wgIpsecSaEspInPackets       Counter32,

    wgIpsecSaEspInDecryptErrors Counter32,
    wgIpsecSaEspInAuthErrors    Counter32,
    wgIpsecSaEspInReplayErrors  Counter32,
    wgIpsecSaEspInPolicyErrors  Counter32,
    wgIpsecSaEspInPadErrors     Counter32,
    wgIpsecSaEspInOtherReceiveErrors Counter32

    
    }

    wgIpsecSaEspInAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
            "The destination address of the SA.

            For implementations that do not support IPv6, this address
            should appear as one of the IPv4-mapped IPv6 addresses as
            defined in Section 2.5.4 of [IPV6AA].

            Specifically, the prefix '0000:0000:0000:0000:0000:FFFF:' is
            used for IPv4 only nodes, while the prefix
            '0000:0000:0000:0000:0000:0000:' is used for bi-lingual
            nodes."
        ::= { wgIpsecSaEspInEntry 1 }

    wgIpsecSaEspInSpi OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The security parameters index of the SA."
        REFERENCE "RFC 2406 Section 2.1"
        ::= { wgIpsecSaEspInEntry 2 }

   wgIpsecSaEspInDestId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination identifier of the SA, or 0 if unknown or if
            the SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchanged during SA creation negotiation."
        ::= { wgIpsecSaEspInEntry 3 }

   wgIpsecSaEspInDestIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by 'wgIpsecSaEspInDestId',
            or 0 if unknown or if the SA uses transport mode
            encapsulation."
        ::= { wgIpsecSaEspInEntry 4 }

    wgIpsecSaEspInSourceId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source identifier of the SA, or 0 if unknown or if the
            SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchange during SA creation negotiation."
        ::= { wgIpsecSaEspInEntry 5 }

    wgIpsecSaEspInSourceIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by 'wgIpsecSaEspInSourceId',
            or 0 if unknown or if the SA uses transport mode
            encapsulation."
        ::= { wgIpsecSaEspInEntry 6 }

    wgIpsecSaEspInProtocol OBJECT-TYPE
        SYNTAX      Integer32 (0..255)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The transport-layer protocol number that this SA carries,
            or 0 if it carries any protocol."
        REFERENCE  "RFC2401 section 4.4.2"
        ::= { wgIpsecSaEspInEntry 7 }

   wgIpsecSaEspInDestPort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE  "RFC2401 section 4.4.2"
        ::= { wgIpsecSaEspInEntry 8 }

   wgIpsecSaEspInSourcePort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE  "RFC2401 section 4.4.2"
        ::= { wgIpsecSaEspInEntry 9 }

    wgIpsecSaEspInCreator OBJECT-TYPE
        SYNTAX      IpsecSaCreatorIdent
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The creator of this SA.

            This MIB makes no assumptions about how the SAs are created.
            They may be created statically, or by a key exchange
            protocol such as IKE, or by some other method."
        ::= { wgIpsecSaEspInEntry 10 }

   wgIpsecSaEspInEncapsulation OBJECT-TYPE
        SYNTAX      IpsecDoiEncapsulationMode
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of encapsulation used by this SA."
        ::= { wgIpsecSaEspInEntry 11 }

   wgIpsecSaEspInEncAlg OBJECT-TYPE
        SYNTAX      IpsecDoiEspTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the encryption algorithm
            applied to traffic or 0 if there is no encryption used."
        ::= { wgIpsecSaEspInEntry 12 }

   wgIpsecSaEspInEncKeyLength OBJECT-TYPE
        SYNTAX      Integer32 (0..65531)
        UNITS       "bits"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The length of the encryption key in bits used for the
            algorithm specified in the 'wgIpsecSaEspInEncAlg' object, or 0
            if the key length is implicit in the specified algorithm or
            there is no encryption specified."
        ::= { wgIpsecSaEspInEntry 13 }

    wgIpsecSaEspInAuthAlg OBJECT-TYPE
        SYNTAX      IpsecDoiAuthAlgorithm
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the hash algorithm applied to
            traffic or 0 if there is no authentication used."
        ::= { wgIpsecSaEspInEntry 14 }

    wgIpsecSaEspInLimitSeconds OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum lifetime in seconds of the SA, or 0 if there is
            no time constraint on its expiration.
            The display value is limited to 4294967295 seconds (more
            than 136 years); values greater than that value will be
            truncated."
        ::= { wgIpsecSaEspInEntry 15 }

    wgIpsecSaEspInLimitKbytes OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum traffic in kilobytes that the SA is allowed to
            support, or 0 if there is no traffic constraint on its
            expiration.

            The display value is limited to 4294967295 kilobytes; values
            greater than that value will be truncated."
        ::= { wgIpsecSaEspInEntry 16 }

    wgIpsecSaEspInAccSeconds OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of seconds accumulated against the SA's
            expiration by time.

            This is also the number of seconds that the SA has existed."
        ::= { wgIpsecSaEspInEntry 17 }

    wgIpsecSaEspInAccKbytes OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of traffic accumulated that counts against the
            SA's expiration by traffic limitation, measured in Kbytes.

            This value may be 0 if the SA does not expire based on
            traffic."
        ::= { wgIpsecSaEspInEntry 18 }

   wgIpsecSaEspInUserOctets OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "bytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of user level traffic measured in bytes handled
            by the SA.

            This is not necessarily the same as the amount of traffic
            applied against the traffic expiration limit."
        ::= { wgIpsecSaEspInEntry 19 }

    wgIpsecSaEspInPackets OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets handled by the SA."
        ::= { wgIpsecSaEspInEntry 20 }

   wgIpsecSaEspInDecryptErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to decryption
            errors."
        ::= { wgIpsecSaEspInEntry 21 }

   wgIpsecSaEspInAuthErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to
            authentication errors."
        ::= { wgIpsecSaEspInEntry 22 }

   wgIpsecSaEspInReplayErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to replay
            errors."
        ::= { wgIpsecSaEspInEntry 23 }

   wgIpsecSaEspInPolicyErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to policy
            errors. This includes packets where the next protocol is
            invalid."
        ::= { wgIpsecSaEspInEntry 24 }

   wgIpsecSaEspInPadErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to pad value
            errors.

            Implementations that do not check this must not support this
            object."
        REFERENCE   "RFC 2406 section 2.4"
        ::= { wgIpsecSaEspInEntry 25 }

    wgIpsecSaEspInOtherReceiveErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to errors
            other than decryption, authentication or replay errors. This
            may include packets dropped due to a lack of receive
            buffers, and may include packets dropped due to congestion
            at the decryption element."
        ::= { wgIpsecSaEspInEntry 26 }

   -- the IPSec Inbound AH MIB-Group
   --
   -- a collection of objects providing information about
    -- IPSec Inbound AH SAs

    wgIpsecSaAhInTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF WGIpsecSaAhInEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The (conceptual) table containing information on IPSec
            inbound AH SAs.
            There should be one row for every inbound AH security
            association that exists in the entity. The maximum number of
            rows is implementation dependent."
        ::= { wgSaTables 2 }

    wgIpsecSaAhInEntry OBJECT-TYPE
        SYNTAX      WGIpsecSaAhInEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry (conceptual row) containing the information on a
            particular IPSec inbound AH SA.

            A row in this table cannot be created or deleted by SNMP
            operations on columns of the table."
        INDEX{ wgIpsecSaAhInAddress, wgIpsecSaAhInSpi }
        ::= { wgIpsecSaAhInTable 1 }

    WGIpsecSaAhInEntry ::= SEQUENCE {

    wgIpsecSaAhInAddress        IpAddress,
    wgIpsecSaAhInSpi            Integer32,

    wgIpsecSaAhInDestId         OCTET STRING,
    wgIpsecSaAhInDestIdType     IpsecDoiIdentType,
    wgIpsecSaAhInSourceId       OCTET STRING,
    wgIpsecSaAhInSourceIdType   IpsecDoiIdentType,
    wgIpsecSaAhInProtocol       Integer32,
    wgIpsecSaAhInDestPort       Integer32,
    wgIpsecSaAhInSourcePort     Integer32,

    wgIpsecSaAhInCreator        IpsecSaCreatorIdent,

    wgIpsecSaAhInEncapsulation  IpsecDoiEncapsulationMode,
    wgIpsecSaAhInAuthAlg        IpsecDoiAhTransform,

    wgIpsecSaAhInLimitSeconds   Integer32,
    wgIpsecSaAhInLimitKbytes    Integer32,

    wgIpsecSaAhInAccSeconds     Counter32,
    wgIpsecSaAhInAccKbytes      Counter32,
    wgIpsecSaAhInUserOctets     Counter32,
    wgIpsecSaAhInPackets        Counter32,

    -- error statistics
    wgIpsecSaAhInAuthErrors     Counter32,
    wgIpsecSaAhInReplayErrors   Counter32,
    wgIpsecSaAhInPolicyErrors   Counter32,
    wgIpsecSaAhInOtherReceiveErrors   Counter32
    }

    wgIpsecSaAhInAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination address of the SA.

            For implementations that do not support IPv6, this address
            should appear as one of the IPv4-mapped IPv6 addresses as
            defined in Section 2.5.4 of [IPV6AA].

            Specifically, the prefix '0000:0000:0000:0000:0000:FFFF:' is
            used for IPv4 only nodes, while the prefix
            '0000:0000:0000:0000:0000:0000:' is used for bi-lingual
            nodes."
        ::= { wgIpsecSaAhInEntry 1 }

   wgIpsecSaAhInSpi OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The security parameters index of the SA."
        REFERENCE   "RFC 2402 Section 2.4"
        ::= { wgIpsecSaAhInEntry 2 }

    wgIpsecSaAhInDestId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination identifier of the SA, or 0 if unknown or if
            the SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchange during SA creation negotiation."
        ::= { wgIpsecSaAhInEntry 3 }

    wgIpsecSaAhInDestIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by 'wgIpsecSaAhInDestId', or
            0 if unknown or if the SA uses transport mode
            encapsulation."
        ::= { wgIpsecSaAhInEntry 4 }

    wgIpsecSaAhInSourceId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source identifier of the SA, or 0 if unknown or if the
            SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchange during SA creation negotiation."
        ::= { wgIpsecSaAhInEntry 5 }

    wgIpsecSaAhInSourceIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by 'wgIpsecSaAhInSourceId',
            or 0 if unknown or if the SA uses transport mode
            encapsulation."
        ::= { wgIpsecSaAhInEntry 6 }

   wgIpsecSaAhInProtocol OBJECT-TYPE
        SYNTAX      Integer32 (0..255)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The transport-layer protocol number that this SA carries,
            or 0 if it carries any protocol."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaAhInEntry 7 }

   wgIpsecSaAhInDestPort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaAhInEntry 8 }

   wgIpsecSaAhInSourcePort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaAhInEntry 9 }

    wgIpsecSaAhInCreator OBJECT-TYPE
        SYNTAX      IpsecSaCreatorIdent
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The creator of this SA.

            This MIB makes no assumptions about how the SAs are created.
            They may be created statically, or by a key exchange
            protocol such as IKE, or by some other method."
        ::= { wgIpsecSaAhInEntry 10 }

   wgIpsecSaAhInEncapsulation OBJECT-TYPE
        SYNTAX      IpsecDoiEncapsulationMode
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of encapsulation used by this SA."
        ::= { wgIpsecSaAhInEntry 11 }

    wgIpsecSaAhInAuthAlg OBJECT-TYPE
        SYNTAX      IpsecDoiAhTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the hash algorithm applied to
            traffic carried by this SA if it uses ESP or 0 if there is
            no authentication applied by ESP."
        ::= { wgIpsecSaAhInEntry 12 }

    wgIpsecSaAhInLimitSeconds OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum lifetime in seconds of the SA, or 0 if there is
            no time constraint on its expiration.

            The display value is limited to 4294967295 seconds (more
            than 136 years); values greater than that value will be
            truncated."
        ::= { wgIpsecSaAhInEntry 13 }

    wgIpsecSaAhInLimitKbytes OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum traffic in Kbytes that the SA is allowed to
            support, or 0 if there is no traffic constraint on its
            expiration.

            The display value is limited to 4294967295 kilobytes; values
            greater than that value will be truncated."
        ::= { wgIpsecSaAhInEntry 14 }

    wgIpsecSaAhInAccSeconds OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of seconds accumulated against the SA's
            expiration by time.

            This is also the number of seconds that the SA has existed."
        ::= { wgIpsecSaAhInEntry 15 }

   wgIpsecSaAhInAccKbytes OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of traffic accumulated that counts against the
            SA's expiration by traffic limitation, measured in Kbytes.
            This value may be 0 if the SA does not expire based on
            traffic."
        ::= { wgIpsecSaAhInEntry 16 }

   wgIpsecSaAhInUserOctets OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "bytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of user level traffic measured in bytes handled
            by the SA.

            This is not necessarily the same as the amount of traffic
            applied against the traffic expiration limit."
        ::= { wgIpsecSaAhInEntry 17 }

    wgIpsecSaAhInPackets OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets handled by the SA."
        ::= { wgIpsecSaAhInEntry 18 }

   wgIpsecSaAhInAuthErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to
            authentication errors."
        ::= { wgIpsecSaAhInEntry 19 }

   wgIpsecSaAhInReplayErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to replay
            errors."
        ::= { wgIpsecSaAhInEntry 20 }

   wgIpsecSaAhInPolicyErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to policy
            errors. This includes packets where the next protocol is
            invalid."
        ::= { wgIpsecSaAhInEntry 21 }

    wgIpsecSaAhInOtherReceiveErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to errors
            other than decryption, authentication or replay errors. This
            may include packets dropped due to a lack of receive
            buffers, and may include packets dropped due to congestion
            at the authentication element."
        ::= { wgIpsecSaAhInEntry 22 }


    -- the IPSec Inbound IPCOMP MIB-Group
    --
    -- a collection of objects providing information about
    -- IPSec Inbound IPCOMP SAs

    wgIpsecSaIpcompInTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF WGIpsecSaIpcompInEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The (conceptual) table containing information on IPSec
            inbound IPCOMP SAs.

            There should be one row for every inbound IPCOMP (security)
            association that exists in the entity. The maximum number of
            rows is implementation dependent."
        ::= { wgSaTables 3 }

   wgIpsecSaIpcompInEntry OBJECT-TYPE
        SYNTAX      WGIpsecSaIpcompInEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry (conceptual row) containing the information on a
            particular IPSec inbound IPCOMP SA.
            A row in this table cannot be created or deleted by SNMP
            operations on columns of the table."
        INDEX{ wgIpsecSaIpcompInAddress, wgIpsecSaIpcompInCpi }
        ::= { wgIpsecSaIpcompInTable 1 }

    WGIpsecSaIpcompInEntry ::= SEQUENCE {

    wgIpsecSaIpcompInAddress             IpAddress,
    wgIpsecSaIpcompInCpi                 IpsecDoiIpcompTransform,

    wgIpsecSaIpcompInDestId              OCTET STRING,
    wgIpsecSaIpcompInDestIdType          IpsecDoiIdentType,
    wgIpsecSaIpcompInSourceId            OCTET STRING,
    wgIpsecSaIpcompInSourceIdType        IpsecDoiIdentType,
    wgIpsecSaIpcompInProtocol            Integer32,
    wgIpsecSaIpcompInDestPort            Integer32,
    wgIpsecSaIpcompInSourcePort          Integer32,

    wgIpsecSaIpcompInCreator             IpsecSaCreatorIdent,

    wgIpsecSaIpcompInEncapsulation       IpsecDoiEncapsulationMode,
    wgIpsecSaIpcompInDecompAlg           IpsecDoiIpcompTransform,

    wgIpsecSaIpcompInSeconds             Counter32,
    wgIpsecSaIpcompInUserOctets          Counter32,
    wgIpsecSaIpcompInPackets             Counter32,

    wgIpsecSaIpcompInDecompErrors        Counter32,
    wgIpsecSaIpcompInOtherReceiveErrors  Counter32
    }

    wgIpsecSaIpcompInAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination address of the SA.

            For implementations that do not support IPv6, this address
            should appear as one of the IPv4-mapped IPv6 addresses as
            defined in Section 2.5.4 of [IPV6AA].
            Specifically, the prefix '0000:0000:0000:0000:0000:FFFF:' is
            used for IPv4 only nodes, while the prefix
            '0000:0000:0000:0000:0000:0000:' is used for bi-lingual
            nodes."
        ::= { wgIpsecSaIpcompInEntry 1 }

    wgIpsecSaIpcompInCpi OBJECT-TYPE
        SYNTAX      IpsecDoiIpcompTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The CPI of the SA. Since the lower values of CPIs are
            reserved to be the same as the algorithm, the syntax for
            this object is the same as the transform."
        REFERENCE   "RFC 2393 Section 3.3"
        ::= { wgIpsecSaIpcompInEntry 2 }

   wgIpsecSaIpcompInDestId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination identifier of the SA, or 0 if unknown or if
            the SA uses transport mode, or 0 if this SA is used with
            multiple SAs in protection suites.

            This value, if non-zero, is taken directly from the optional
            ID payloads that are exchange during SA creation
            negotiation."
        ::= { wgIpsecSaIpcompInEntry 3 }

   wgIpsecSaIpcompInDestIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by
            'wgIpsecSaIpcompInDestId', or 0 if unknown or if the SA uses
            transport mode, or 0 if this SA is used with multiple SAs in
            protection suites."
        ::= { wgIpsecSaIpcompInEntry 4 }

    wgIpsecSaIpcompInSourceId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (1..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source identifier of the SA, or 0 if unknown or if the
            SA uses transport mode encapsulation, or 0 if this SA is
            used with multiple SAs in protection suites.

            This value, if non-zero, is taken directly from the optional
            ID payloads that are exchange during SA creation
            negotiation."
        ::= { wgIpsecSaIpcompInEntry 5 }

    wgIpsecSaIpcompInSourceIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by
            'wgIpsecSaIpcompInSourceId', or 0 if unknown or if the SA uses
            transport mode encapsulation, or 0 if this SA is used with
            multiple SAs in protection suites."
        ::= { wgIpsecSaIpcompInEntry 6 }

   wgIpsecSaIpcompInProtocol OBJECT-TYPE
        SYNTAX      Integer32 (0..255)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The transport-layer protocol number that this SA carries,
            or 0 if it carries any protocol."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaIpcompInEntry 7 }

    wgIpsecSaIpcompInDestPort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaIpcompInEntry 8 }

    wgIpsecSaIpcompInSourcePort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaIpcompInEntry 9 }

   wgIpsecSaIpcompInCreator OBJECT-TYPE
        SYNTAX      IpsecSaCreatorIdent
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The creator of this SA.

            This MIB makes no assumptions about how the SAs are created.
            They may be created statically, or by a key exchange
            protocol such as IKE, or by some other method."
        ::= { wgIpsecSaIpcompInEntry 10 }

   wgIpsecSaIpcompInEncapsulation OBJECT-TYPE
        SYNTAX      IpsecDoiEncapsulationMode
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of encapsulation used by this SA."
        ::= { wgIpsecSaIpcompInEntry 11 }

   wgIpsecSaIpcompInDecompAlg OBJECT-TYPE
        SYNTAX      IpsecDoiIpcompTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the decompression algorithm
            applied to traffic."
        ::= { wgIpsecSaIpcompInEntry 12 }

   wgIpsecSaIpcompInSeconds OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of seconds that the SA has existed."
        ::= { wgIpsecSaIpcompInEntry 13 }

    wgIpsecSaIpcompInUserOctets OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "bytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of user level traffic measured in bytes handled
            by the SA."
        ::= { wgIpsecSaIpcompInEntry 14 }

    wgIpsecSaIpcompInPackets OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets handled by the SA."
        ::= { wgIpsecSaIpcompInEntry 15 }

    wgIpsecSaIpcompInDecompErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to
            decompression errors."
        ::= { wgIpsecSaIpcompInEntry 16 }

    wgIpsecSaIpcompInOtherReceiveErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to errors
            other than decompression errors. This may include packets
            dropped due to a lack of receive buffers, and packets
            dropped due to congestion at the decompression element."
        ::= { wgIpsecSaIpcompInEntry 17 }


    -- the IPSec Outbound ESP MIB-Group
    --
    -- a collection of objects providing information about
    -- IPSec Outbound ESP SAs

    wgIpsecSaEspOutTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF WGIpsecSaEspOutEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The (conceptual) table containing information on IPSec
            Outbound ESP SAs.

            There should be one row for every outbound ESP security
            association that exists in the entity. The maximum number of
            rows is implementation dependent."
        ::= { wgSaTables 4 }

   wgIpsecSaEspOutEntry OBJECT-TYPE
        SYNTAX      WGIpsecSaEspOutEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry (conceptual row) containing the information on a
            particular IPSec Outbound ESP SA.

            A row in this table cannot be created or deleted by SNMP
            operations on columns of the table."
        INDEX{ wgIpsecSaEspOutAddress, wgIpsecSaEspOutSpi }
        ::= { wgIpsecSaEspOutTable 1 }

   WGIpsecSaEspOutEntry ::= SEQUENCE {

    wgIpsecSaEspOutAddress         IpAddress,
    wgIpsecSaEspOutSpi             Integer32,

    wgIpsecSaEspOutSourceId        OCTET STRING,
    wgIpsecSaEspOutSourceIdType    IpsecDoiIdentType,
    wgIpsecSaEspOutDestId          OCTET STRING,
    wgIpsecSaEspOutDestIdType      IpsecDoiIdentType,
    wgIpsecSaEspOutProtocol        Integer32,
    wgIpsecSaEspOutSourcePort      Integer32,
    wgIpsecSaEspOutDestPort        Integer32,

    wgIpsecSaEspOutCreator         IpsecSaCreatorIdent,

    wgIpsecSaEspOutEncapsulation   IpsecDoiEncapsulationMode,
    wgIpsecSaEspOutEncAlg          IpsecDoiEspTransform,
    wgIpsecSaEspOutEncKeyLength    Integer32,
    wgIpsecSaEspOutAuthAlg         IpsecDoiAuthAlgorithm,

    wgIpsecSaEspOutLimitSeconds    Integer32,
    wgIpsecSaEspOutLimitKbytes     Integer32,

    wgIpsecSaEspOutAccSeconds      Counter32,
    wgIpsecSaEspOutAccKbytes       Counter32,
    wgIpsecSaEspOutUserOctets      Counter32,
    wgIpsecSaEspOutPackets         Counter32,

    wgIpsecSaEspOutSendErrors      Counter32
    }


   wgIpsecSaEspOutAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination address of the SA.

            For implementations that do not support IPv6, this address
            should appear as one of the IPv4-mapped IPv6 addresses as
            defined in Section 2.5.4 of [IPV6AA].

            Specifically, the prefix '0000:0000:0000:0000:0000:FFFF:' is
            used for IPv4 only nodes, while the prefix
            '0000:0000:0000:0000:0000:0000:' is used for bi-lingual
            nodes."
        ::= { wgIpsecSaEspOutEntry 1 }

    wgIpsecSaEspOutSpi OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The security parameters index of the SA."
        REFERENCE "RFC 2406 Section 2.1"
        ::= { wgIpsecSaEspOutEntry 2 }

    wgIpsecSaEspOutSourceId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (4..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source identifier of the SA, or 0 if unknown or if the
            SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchange during phase 2 negotiations."
        ::= { wgIpsecSaEspOutEntry 3 }

    wgIpsecSaEspOutSourceIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by
            'wgIpsecSaEspOutSourceId', or 0 if unknown or if the SA uses
            transport mode encapsulation."
        ::= { wgIpsecSaEspOutEntry 4 }

   wgIpsecSaEspOutDestId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (4..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination identifier of the SA, or 0 if unknown or if
            the SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchange during phase 2 negotiations."
        ::= { wgIpsecSaEspOutEntry 5 }

    wgIpsecSaEspOutDestIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by 'wgIpsecSaEspOutDestId',
            or 0 if unknown or if the SA uses transport mode
            encapsulation."
        ::= { wgIpsecSaEspOutEntry 6 }

    wgIpsecSaEspOutProtocol OBJECT-TYPE
        SYNTAX      Integer32 (0..255)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The transport-layer protocol number that this SA carries,
            or 0 if it carries any protocol."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaEspOutEntry 7 }

    wgIpsecSaEspOutSourcePort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaEspOutEntry 8 }

    wgIpsecSaEspOutDestPort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaEspOutEntry 9 }

    wgIpsecSaEspOutCreator OBJECT-TYPE
        SYNTAX      IpsecSaCreatorIdent
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The creator of this SA.

            This MIB makes no assumptions about how the SAs are created.
            They may be created statically, or by a key exchange
            protocol such as IKE, or by some other method."
        ::= { wgIpsecSaEspOutEntry 10 }

    wgIpsecSaEspOutEncapsulation OBJECT-TYPE
        SYNTAX      IpsecDoiEncapsulationMode
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of encapsulation used by this SA."
        ::= { wgIpsecSaEspOutEntry 11 }

   wgIpsecSaEspOutEncAlg OBJECT-TYPE
        SYNTAX      IpsecDoiEspTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the encryption algorithm
            applied to traffic or 0 if there is no encryption used."
        ::= { wgIpsecSaEspOutEntry 12 }

   wgIpsecSaEspOutEncKeyLength OBJECT-TYPE
        SYNTAX      Integer32 (0..65531)
        UNITS       "bits"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The length of the encryption key in bits used for the
            algorithm specified in the 'wgIpsecSaEspOutEncAlg' object, or
            0 if the key length is implicit in the specified algorithm
            or there is no encryption specified."
        ::= { wgIpsecSaEspOutEntry 13 }

    wgIpsecSaEspOutAuthAlg OBJECT-TYPE
        SYNTAX      IpsecDoiAuthAlgorithm
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the hash algorithm applied to
            traffic or 0 if there is no authentication used."
        ::= { wgIpsecSaEspOutEntry 14 }

    wgIpsecSaEspOutLimitSeconds OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum lifetime in seconds of the SA, or 0 if there is
            no time constraint on its expiration.

            The display value is limited to 4294967295 seconds (more
            than 136 years); values greater than that value will be
            truncated."
        ::= { wgIpsecSaEspOutEntry 15 }

   wgIpsecSaEspOutLimitKbytes OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum traffic in kbytes that the SA is allowed to
            support, or 0 if there is no traffic constraint on its
            expiration.

            The display value is limited to 4294967295 kilobytes; values
            greater than that value will be truncated."
        ::= { wgIpsecSaEspOutEntry 16 }

    wgIpsecSaEspOutAccSeconds OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of seconds accumulated against the SA's
            expiration by time.

            This is also the number of seconds that the SA has existed."
        ::= { wgIpsecSaEspOutEntry 17 }

    wgIpsecSaEspOutAccKbytes OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of traffic accumulated that counts against the
            SA's expiration by traffic limitation, measured in Kbytes.

            This value may be 0 if the SA does not expire based on
            traffic."
        ::= { wgIpsecSaEspOutEntry 18 }

    wgIpsecSaEspOutUserOctets OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "bytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of user level traffic measured in bytes handled
            by the SA.

            This is not necessarily the same as the amount of traffic
            applied against the traffic expiration limit."
        ::= { wgIpsecSaEspOutEntry 19 }

    wgIpsecSaEspOutPackets OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets handled by the SA."
        ::= { wgIpsecSaEspOutEntry 20 }

    wgIpsecSaEspOutSendErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to any error.
            This may include errors due to a lack of transmit buffers."
        ::= { wgIpsecSaEspOutEntry 21 }


    -- the IPSec Outbound AH MIB-Group
    --
    -- a collection of objects providing information about
    -- IPSec Outbound AH SAs

    wgIpsecSaAhOutTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF WGIpsecSaAhOutEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The (conceptual) table containing information on IPSec
            Outbound AH SAs.

            There should be one row for every outbound AH security
            association that exists in the entity. The maximum number of
            rows is implementation dependent."
        ::= { wgSaTables 5 }

    wgIpsecSaAhOutEntry OBJECT-TYPE
        SYNTAX      WGIpsecSaAhOutEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry (conceptual row) containing the information on a
            particular IPSec Outbound AH SA.

            A row in this table cannot be created or deleted by SNMP
            operations on columns of the table."
        INDEX{ wgIpsecSaAhOutAddress, wgIpsecSaAhOutSpi }
        ::= { wgIpsecSaAhOutTable 1 }

    WGIpsecSaAhOutEntry ::= SEQUENCE {

    wgIpsecSaAhOutAddress          IpAddress,
    wgIpsecSaAhOutSpi              Integer32,

    wgIpsecSaAhOutSourceId         OCTET STRING,
    wgIpsecSaAhOutSourceIdType     IpsecDoiIdentType,
    wgIpsecSaAhOutDestId           OCTET STRING,
    wgIpsecSaAhOutDestIdType       IpsecDoiIdentType,
    wgIpsecSaAhOutProtocol         Integer32,
    wgIpsecSaAhOutSourcePort       Integer32,
    wgIpsecSaAhOutDestPort         Integer32,

    wgIpsecSaAhOutCreator          IpsecSaCreatorIdent,

    wgIpsecSaAhOutEncapsulation    IpsecDoiEncapsulationMode,
    wgIpsecSaAhOutAuthAlg          IpsecDoiAhTransform,

    wgIpsecSaAhOutLimitSeconds     Integer32,
    wgIpsecSaAhOutLimitKbytes      Integer32,

    wgIpsecSaAhOutAccSeconds       Counter32,
    wgIpsecSaAhOutAccKbytes        Counter32,
    wgIpsecSaAhOutUserOctets       Counter32,
    wgIpsecSaAhOutPackets          Counter32,

    wgIpsecSaAhOutSendErrors       Counter32
    }


    wgIpsecSaAhOutAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination address of the SA.

            For implementations that do not support IPv6, this address
            should appear as one of the IPv4-mapped IPv6 addresses as
            defined in Section 2.5.4 of [IPV6AA].

            Specifically, the prefix '0000:0000:0000:0000:0000:FFFF:' is
            used for IPv4 only nodes, while the prefix
            '0000:0000:0000:0000:0000:0000:' is used for bi-lingual
            nodes."
        ::= { wgIpsecSaAhOutEntry 1 }

    wgIpsecSaAhOutSpi OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The security parameters index of the SA."
        REFERENCE "RFC 2402 Section 2.4"
        ::= { wgIpsecSaAhOutEntry 2 }

    wgIpsecSaAhOutSourceId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (4..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source identifier of the SA, or 0 if unknown or if the
            SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchange during phase 2 negotiations."
        ::= { wgIpsecSaAhOutEntry 3 }

    wgIpsecSaAhOutSourceIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by 'wgIpsecSaAhOutSourceId',
            or 0 if unknown or if the SA uses transport mode
            encapsulation."
        ::= { wgIpsecSaAhOutEntry 4 }

    wgIpsecSaAhOutDestId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (4..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination identifier of the SA, or 0 if unknown or if
            the SA uses transport mode encapsulation.

            This value is taken directly from the optional ID payloads
            that are exchange during phase 2 negotiations."
        ::= { wgIpsecSaAhOutEntry 5 }

    wgIpsecSaAhOutDestIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by 'wgIpsecSaAhOutDestId',
            or 0 if unknown or if the SA uses transport mode
            encapsulation."
        ::= { wgIpsecSaAhOutEntry 6 }

    wgIpsecSaAhOutProtocol OBJECT-TYPE
        SYNTAX      Integer32 (0..255)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The transport-layer protocol number that this SA carries,
            or 0 if it carries any protocol."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaAhOutEntry 7 }

    wgIpsecSaAhOutSourcePort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaAhOutEntry 8 }

    wgIpsecSaAhOutDestPort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaAhOutEntry 9 }

    wgIpsecSaAhOutCreator OBJECT-TYPE
        SYNTAX      IpsecSaCreatorIdent
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The creator of this SA.

            This MIB makes no assumptions about how the SAs are created.
            They may be created statically, or by a key exchange
            protocol such as IKE, or by some other method."
        ::= { wgIpsecSaAhOutEntry 10 }

    wgIpsecSaAhOutEncapsulation OBJECT-TYPE
        SYNTAX      IpsecDoiEncapsulationMode
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of encapsulation used by this SA."
        ::= { wgIpsecSaAhOutEntry 11 }

    wgIpsecSaAhOutAuthAlg OBJECT-TYPE
        SYNTAX      IpsecDoiAhTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the hash algorithm applied to
            traffic or 0 if there is no authentication used."
        ::= { wgIpsecSaAhOutEntry 12 }

    wgIpsecSaAhOutLimitSeconds OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum lifetime in seconds of the SA, or 0 if there is
            no time constraint on its expiration.

            The display value is limited to 4294967295 seconds (more
            than 136 years); values greater than that value will be
            truncated."
        ::= { wgIpsecSaAhOutEntry 13 }

    wgIpsecSaAhOutLimitKbytes OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The maximum traffic in Kbytes that the SA is allowed to
            support, or 0 if there is no traffic constraint on its
            expiration.

            The display value is limited to 4294967295 kilobytes; values
            greater than that value will be truncated."
        ::= { wgIpsecSaAhOutEntry 14 }

    wgIpsecSaAhOutAccSeconds OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of seconds accumulated against the SA's
            expiration by time.

            This is also the number of seconds that the SA has existed."
        ::= { wgIpsecSaAhOutEntry 15 }

    wgIpsecSaAhOutAccKbytes OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "kilobytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of traffic accumulated that counts against the
            SA's expiration by traffic limitation, measured in Kbytes.

            This value may be 0 if the SA does not expire based on
            traffic."
        ::= { wgIpsecSaAhOutEntry 16 }

    wgIpsecSaAhOutUserOctets OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "bytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of user level traffic measured in bytes handled
            by the SA.

            This is not necessarily the same as the amount of traffic
            applied against the traffic expiration limit."
        ::= { wgIpsecSaAhOutEntry 17 }

    wgIpsecSaAhOutPackets OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets handled by the SA."
        ::= { wgIpsecSaAhOutEntry 18 }

    wgIpsecSaAhOutSendErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets discarded by the SA due to any error.
            This may include errors due to a lack of transmit buffers."
        ::= { wgIpsecSaAhOutEntry 19 }


    -- the IPSec Outbound IPCOMP MIB-Group
    --
    -- a collection of objects providing information about
    -- IPSec Outbound IPCOMP SAs

    wgIpsecSaIpcompOutTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF WGIpsecSaIpcompOutEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The (conceptual) table containing information on IPSec
            Outbound IPCOMP SAs.

            There should be one row for every outbound IPCOMP (security)
            association that exists in the entity. The maximum number of
            rows is implementation dependent."
        ::= { wgSaTables 6 }

    wgIpsecSaIpcompOutEntry OBJECT-TYPE
        SYNTAX      WGIpsecSaIpcompOutEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry (conceptual row) containing the information on a
            particular IPSec Outbound IPCOMP SA.

            A row in this table cannot be created or deleted by SNMP
            operations on columns of the table."
        INDEX{ wgIpsecSaIpcompOutAddress, wgIpsecSaIpcompOutCpi }
        ::= { wgIpsecSaIpcompOutTable 1 }

    WGIpsecSaIpcompOutEntry ::= SEQUENCE {

    wgIpsecSaIpcompOutAddress         IpAddress,
    wgIpsecSaIpcompOutCpi             IpsecDoiIpcompTransform,

    wgIpsecSaIpcompOutSourceId        OCTET STRING,
    wgIpsecSaIpcompOutSourceIdType    IpsecDoiIdentType,
    wgIpsecSaIpcompOutDestId          OCTET STRING,
    wgIpsecSaIpcompOutDestIdType      IpsecDoiIdentType,
    wgIpsecSaIpcompOutProtocol        Integer32,
    wgIpsecSaIpcompOutSourcePort      Integer32,
    wgIpsecSaIpcompOutDestPort        Integer32,

    wgIpsecSaIpcompOutCreator         IpsecSaCreatorIdent,

    wgIpsecSaIpcompOutEncapsulation   IpsecDoiEncapsulationMode,
    wgIpsecSaIpcompOutCompAlg         IpsecDoiIpcompTransform,

    wgIpsecSaIpcompOutSeconds         Counter32,
    wgIpsecSaIpcompOutUserOctets      Counter32,
    wgIpsecSaIpcompOutPackets         Counter32
    }

    wgIpsecSaIpcompOutAddress OBJECT-TYPE
        SYNTAX      IpAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination address of the SA.

            If the IPCOMP SA is shared across multiple SAs in protection
            suites, this value may be 0.

            For implementations that do not support IPv6, this address
            should appear as one of the IPv4-mapped IPv6 addresses as
            defined in Section 2.5.4 of [IPV6AA].

            Specifically, the prefix '0000:0000:0000:0000:0000:FFFF:' is
            used for IPv4 only nodes, while the prefix
            '0000:0000:0000:0000:0000:0000:' is used for bi-lingual
            nodes."
        ::= { wgIpsecSaIpcompOutEntry 1 }

    wgIpsecSaIpcompOutCpi OBJECT-TYPE
        SYNTAX      IpsecDoiIpcompTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The CPI of the SA. Since the lower values of CPIs are
            reserved to be the same as the algorithm, the syntax for
            this object is the same as the transform."
        REFERENCE "RFC 2393 Section 3.3"
        ::= { wgIpsecSaIpcompOutEntry 2 }

    wgIpsecSaIpcompOutSourceId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (4..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source identifier of the SA, or 0 if unknown or if the
            SA uses transport mode encapsulation, or 0 if this SA is
            used with multiple SAs in protection suites.

            This value, if non-zero, is taken directly from the optional
            ID payloads that are exchange during phase 2 negotiations."
        ::= { wgIpsecSaIpcompOutEntry 3 }

    wgIpsecSaIpcompOutSourceIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by
            'wgIpsecSaIpcompOutSourceId', or 0 if unknown or if the SA
            uses transport mode encapsulation, or 0 if this SA is used
            with multiple SAs in protection suites."
        ::= { wgIpsecSaIpcompOutEntry 4 }

    wgIpsecSaIpcompOutDestId OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (4..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination identifier of the SA, or 0 if unknown or if
            the SA uses transport mode encapsulation, or 0 if this SA is
            used with multiple SAs in protection suites.

            This value, if non-zero, is taken directly from the optional
            ID payloads that are exchange during phase 2 negotiations."
        ::= { wgIpsecSaIpcompOutEntry 5 }

    wgIpsecSaIpcompOutDestIdType OBJECT-TYPE
        SYNTAX      IpsecDoiIdentType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of identifier presented by
            'wgIpsecSaIpcompOutDestId', or 0 if unknown or if the SA uses
            transport mode encapsulation, or 0 if this SA is used with
            multiple SAs in protection suites."
        ::= { wgIpsecSaIpcompOutEntry 6 }

    wgIpsecSaIpcompOutProtocol OBJECT-TYPE
        SYNTAX      Integer32 (0..255)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The transport-layer protocol number that this SA carries,
            or 0 if it carries any protocol."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaIpcompOutEntry 7 }

    wgIpsecSaIpcompOutSourcePort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The source port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaIpcompOutEntry 8 }

    wgIpsecSaIpcompOutDestPort OBJECT-TYPE
        SYNTAX      Integer32 (0.. 65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The destination port number of the protocol that this SA
            carries, or 0 if it carries any port number."
        REFERENCE   "RFC2401 section 4.4.2"
        ::= { wgIpsecSaIpcompOutEntry 9 }

    wgIpsecSaIpcompOutCreator OBJECT-TYPE
        SYNTAX      IpsecSaCreatorIdent
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The creator of this SA.

            This MIB makes no assumptions about how the SAs are created.
            They may be created statically, or by a key exchange
            protocol such as IKE, or by some other method."
        ::= { wgIpsecSaIpcompOutEntry 10 }

    wgIpsecSaIpcompOutEncapsulation OBJECT-TYPE
        SYNTAX      IpsecDoiEncapsulationMode
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The type of encapsulation used by this SA."
        ::= { wgIpsecSaIpcompOutEntry 11 }

    wgIpsecSaIpcompOutCompAlg OBJECT-TYPE
        SYNTAX      IpsecDoiIpcompTransform
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A unique value representing the compression algorithm
            applied to traffic."
        ::= { wgIpsecSaIpcompOutEntry 12 }

    wgIpsecSaIpcompOutSeconds OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "seconds"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of seconds that the SA has existed."
        ::= { wgIpsecSaIpcompOutEntry 13 }

    wgIpsecSaIpcompOutUserOctets OBJECT-TYPE
        SYNTAX      Counter32
        UNITS       "bytes"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The amount of user level traffic measured in bytes handled
            by the SA.

            This is not necessarily the same as the amount of traffic
            applied against the traffic expiration limit."
        ::= { wgIpsecSaIpcompOutEntry 14 }

    wgIpsecSaIpcompOutPackets OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The number of packets handled by the SA."
        ::= { wgIpsecSaIpcompOutEntry 15 }


    --
    -- entity IPSec statistics
    --
    wgIpsecEspCurrentInboundSAs OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of inbound ESP SAs in the entity."
        ::= { wgSaStatistics 1 }

    wgIpsecEspTotalInboundSAs OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of inbound ESP SAs created in the entity
            since boot time."
        ::= { wgSaStatistics 2 }

    wgIpsecEspCurrentOutboundSAs OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of outbound ESP SAs in the entity."
        ::= { wgSaStatistics 3 }

    wgIpsecEspTotalOutboundSAs OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of outbound ESP SAs created in the entity
            since boot time."
        ::= { wgSaStatistics 4 }

    wgIpsecAhCurrentInboundSAs OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of inbound AH SAs in the entity."
        ::= { wgSaStatistics 5 }

    wgIpsecAhTotalInboundSAs OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of inbound AH SAs created in the entity
            since boot time."
        ::= { wgSaStatistics 6 }

    wgIpsecAhCurrentOutboundSAs OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of outbound AH SAs in the entity."
        ::= { wgSaStatistics 7 }

    wgIpsecAhTotalOutboundSAs OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of outbound AH SAs created in the entity
            since boot time."
        ::= { wgSaStatistics 8 }

    wgIpsecIpcompCurrentInboundSAs OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of inbound IPCOMP SAs in the entity."
        ::= { wgSaStatistics 9 }

    wgIpsecIpcompTotalInboundSAs OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of inbound IPCOMP SAs created in the
            entity since boot time."
        ::= { wgSaStatistics 10 }

    wgIpsecIpcompCurrentOutboundSAs OBJECT-TYPE
        SYNTAX      Gauge32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The current number of outbound IPCOMP SAs in the entity."
        ::= { wgSaStatistics 11 }

    wgIpsecIpcompTotalOutboundSAs OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of outbound IPCOMP SAs created in the
            entity since boot time."
        ::= { wgSaStatistics 12 }


    --
    -- IPSec error counts
    --

    wgIpsecDecryptionErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of packets received by the entity in SAs
            since boot time with decryption errors."
        ::= { wgSaErrors 1 }

    wgIpsecAuthenticationErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of packets received by the entity in SAs
            since boot time with authentication errors.

            This includes all packets in which the hash value is
            determined to be invalid, for both ESP and AH SAs."
        ::= { wgSaErrors 2 }

    wgIpsecReplayErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of packets received by the entity in SAs
            since boot time with replay errors."
        ::= { wgSaErrors 3 }

    wgIpsecPolicyErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of packets received by the entity in SAs
            since boot time and discarded due to policy errors. This
            includes packets that had selectors that were invalid for
            the SA that carried them."
        ::= { wgSaErrors 4 }

    wgIpsecOtherReceiveErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of packets received by the entity in SAs
            since boot time and discarded due to errors not due to
            decryption, authentication, replay or policy."
        ::= { wgSaErrors 5 }

    wgIpsecSendErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of packets to be sent by the entity in SAs
            since boot time and discarded due to errors."
        ::= { wgSaErrors 6 }

    wgIpsecUnknownSpiErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The total number of packets received by the entity since
            boot time with SPIs or CPIs that were not valid."
        ::= { wgSaErrors 7 }

END

