VRRP-MIB DEFINITIONS ::= BEGIN  
     
    IMPORTS  
        MODULE-IDENTITY, OBJECT-TYPE,  
        NOTIFICATION-TYPE, Counter32,  
        Integer32, mib-2, Unsigned32, 
        IpAddress                           FROM SNMPv2-SMI  
     
        TEXTUAL-CONVENTION, RowStatus,  
        MacAddress, TruthValue, TimeStamp, 
        TimeInterval, StorageType           FROM SNMPv2-TC  
     
        MODULE-COMPLIANCE, OBJECT-GROUP,  
        NOTIFICATION-GROUP                  FROM SNMPv2-CONF  
        ifIndex                             FROM IF-MIB  
        InetAddressType, InetAddress        FROM INET-ADDRESS-MIB;  
     
   vrrpMIB  MODULE-IDENTITY  
        LAST-UPDATED "200612130000Z"  
        ORGANIZATION "IETF VRRP Working Group"  
        CONTACT-INFO  
               "Kalyan Tata   
                Nokia Inc.  
                313 Fairchild Dr.  
                Mountain View, CA 94043"  
 
        DESCRIPTION  
            "This MIB describes objects used for managing Virtual  
             Router Redundancy Protocol (VRRP) over IPv4 and IPv6 
             protocols. 
 
             This MIB supports VRRP for IPv4 and IPv6 protocols 
             simultaneously running on a given interface of a  
             router. 
     
             Copyright (C) The IETF Trust (2006)."  
 

        REVISION "200612130000Z"    -- 13 Dec 2006  
   -- 
   -- RFC Ed.: In the following text, please replace XXX 
   --          with actual RFC number and remove this note 
        DESCRIPTION 
         "Revised version, published as RFC XXXX. 
 
          This revision provides MIB support for the Virtual Router  
          Redundancy Protocol (VRRP) in both IPv4 and IPv6  
          environments. 
 
          Key revisions include : 
          o  Deprecating vrrpOperTable, vrrpRouterStatsTable and  
             vrrpAssoIpAddrTable in favor of IP version neutral  
             vrrpOperationsTable, vrrpRouterStatisticsTable and  
             vrrpAssociatedIpAddrTable. 
          o  vrrpNodeVersion scalar objects has been deprecated and 
             is replaced by the vrrpOperationsInetAddrType object  
             in the vrrpOperationsTable. 
          o  vrrpAuthFailureTrap has been deprecated. 
          o  vrrpNewMasterReason object has been added to  
             vrrpTrapNewMaster notification. 
          o  A new notification vrrpTrapProtoError has been added. 
          o  DEFVAL clause has been added." 
 
        REVISION "200003030000Z"    -- 03 Mar 2000 
        DESCRIPTION 
         "This MIB describes objects used for managing Virtual     
          Router Redundancy Protocol (VRRP) routers. Initial  
          version as published in RFC 2787." 
        ::= { mib-2 68 }  
 
   --  
   --  Textual Conventions  
   --  
     
   VrId ::= TEXTUAL-CONVENTION  
        DISPLAY-HINT "d" 
        STATUS       current  
        DESCRIPTION  
            "A number which, along with IP version and interface   
            index (IfIndex), serves to uniquely identify a virtual 
            router on a given VRRP router. There is no relationship 
            between VrId value used on a IPv4 interface and VrId  
            value used on IPv6 interface. It is legal to use same  
            VrId value on IPv4 and IPv6 interfaces"  
     
        SYNTAX      Integer32 (1..255)  
     
   --  
   --  VRRP MIB Groups  
   --  
     
   vrrpOperations      OBJECT IDENTIFIER ::= { vrrpMIB 1 }  
   vrrpStatistics      OBJECT IDENTIFIER ::= { vrrpMIB 2 }  
   vrrpConformance     OBJECT IDENTIFIER ::= { vrrpMIB 3 }  
     
   --  
   --  Start of MIB objects  
   --  
 
   vrrpNodeVersion  OBJECT-TYPE 
     SYNTAX       Integer32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
        "This value identifies the particular version of the VRRP 
         supported by this node. 
         This object is deprecated in the IP Version Independent 
         MIB." 
     ::= { vrrpOperations 1 }   
     
   vrrpNotificationCntl  OBJECT-TYPE  
        SYNTAX       INTEGER {  
            enabled     (1),  
            disabled    (2)  
        }  
        MAX-ACCESS   read-write  
        STATUS       current  
        DESCRIPTION  
           "Indicates whether the VRRP-enabled router will generate 
            SNMP notifications for events defined in this MIB.  
            'Enabled' results in SNMP notifications; 'disabled', no  
            notifications are sent."  
        DEFVAL { enabled }  
        ::= { vrrpOperations 2 }  
     
   --  
   --  VRRP Operations Table  
   --  
     
    vrrpOperationsTable OBJECT-TYPE  
        SYNTAX       SEQUENCE OF VrrpOperationsEntry  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "Unified Operations table for a VRRP router which   
             consists of a sequence (i.e., one or more conceptual 
             rows) of 'vrrpOperationsEntry' items which describe  
             the operational characteristics of a virtual router."  
        ::= { vrrpOperations 7 }  
     
    vrrpOperationsEntry OBJECT-TYPE  
        SYNTAX       VrrpOperationsEntry  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "An entry in the vrrpOperationsTable containing the   
             operational characteristics of a virtual router.  On a  
             VRRP router, a given virtual router is identified by a 
             combination of the IP version, VRID and ifIndex. 
             ifIndex represents a physical interface of the router. 
     
             Note that rows in this table can be distinguished on a 
             multi-stacked device running VRRP over IPv4 and  
             IPv6 on the same physical interface.  
     
             Rows in the table cannot be modified unless the value  
             of 'vrrpOperationsState' has transitioned to  
             'initialize'" 
     
        INDEX    { vrrpOperationsInetAddrType,  
                   vrrpOperationsVrId, ifIndex }  
        ::= { vrrpOperationsTable 1 }  
     
 
    VrrpOperationsEntry ::=  
 
        SEQUENCE {  
            vrrpOperationsInetAddrType  
                InetAddressType,  
            vrrpOperationsVrId  
                VrId,  
            vrrpOperationsVirtualMacAddr  
                MacAddress,  
            vrrpOperationsState  
                INTEGER,  
            vrrpOperationsPriority  
                Unsigned32, 
            vrrpOperationsAddrCount 
                Integer32,  
            vrrpOperationsMasterIpAddr  
                InetAddress,  
            vrrpOperationsPrimaryIpAddr  
                InetAddress,  
            vrrpOperationsAdvInterval  
                TimeInterval,  
            vrrpOperationsPreemptMode  
                TruthValue,  
            vrrpOperationsAcceptMode  
                TruthValue,  
            vrrpOperationsUpTime  
                TimeStamp,  
            vrrpOperationsStorageType 
                StorageType, 
            vrrpOperationsRowStatus  
                RowStatus  
    }  
 
    vrrpOperationsInetAddrType OBJECT-TYPE  
        SYNTAX       InetAddressType  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "The IP address type of VrrpOperationsEntry. This value  
             applies to both vrrpOperationsMasterIpAddr and  
             vrrpOperationsPrimaryIpAddr." 
        REFERENCE "RFC 4001" 
        ::= { vrrpOperationsEntry 1 }   
    
    vrrpOperationsVrId OBJECT-TYPE  
        SYNTAX       VrId  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "This object contains the Virtual Router Identifier  
             (VRID)."  
        REFERENCE "RFC 4001" 
        ::= { vrrpOperationsEntry 2 }  
     
    vrrpOperationsVirtualMacAddr OBJECT-TYPE  
        SYNTAX       MacAddress  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The virtual MAC address of the virtual router.  
            Although this object can be derived from the  
            'vrrpOperationsVrId' object, it is defined so that it  
            is easily obtainable by a management application and  
            can be included in VRRP-related SNMP notifications."  
        REFERENCE "STD 58 RFC 2578" 
        ::= { vrrpOperationsEntry 3 }  
     
    vrrpOperationsState OBJECT-TYPE  
        SYNTAX       INTEGER {  
            initialize(1),  
            backup(2),  
            master(3)  
        }  
        MAX-ACCESS   read-only  
        STATUS       current  
     
        DESCRIPTION  
            "The current state of the virtual router. This object   
            has three defined values:  
     
              - `initialize', which indicates that the  
                virtual router is waiting for a startup event.  
     
              - `backup', which indicates the virtual router is  
                monitoring the availability of the master router.  
     
              - `master', which indicates that the virtual router  
                is forwarding packets for IP addresses that are  
                associated with this router."  
        REFERENCE " RFC 3768" 
        ::= { vrrpOperationsEntry 4 }  
     
    vrrpOperationsPriority OBJECT-TYPE  
        SYNTAX       Unsigned32 (0..255)  
        MAX-ACCESS   read-create  
        STATUS       current  
        DESCRIPTION  
            "This object specifies the priority to be used for the  
            virtual router master election process.  Higher values  
            imply higher priority.  
     
            A priority of '0', although not settable, is sent by  
            the master router to indicate that this router has  
            ceased to participate in VRRP and a backup virtual  
            router should transition to become a new master.  
     
            A priority of 255 is used for the router that owns the  
            associated IP address(es) for VRRP over IPv4 and hence 
            not settable. 
 
            A 'badValue(3)' should be returned when a user tries to  
            set 0 or 255 for this object. " 
        DEFVAL       { 100 }  
        ::= { vrrpOperationsEntry 5 }  
     
    vrrpOperationsAddrCount OBJECT-TYPE  
        SYNTAX       Integer32 (0..255)  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The number of IP addresses that are associated with  
            this virtual router.  This number is equal to the  
            number of rows in the vrrpAssociatedAddrTable that  
            correspond to a given IP version/VRID/ifIndex."  
        REFERENCE "RFC 3768 section 5.3.5.  Count IP Addrs" 
        ::= { vrrpOperationsEntry 6 }   
     
    vrrpOperationsMasterIpAddr OBJECT-TYPE  
        SYNTAX       InetAddress  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The master router's real IP address. Master router  
            would set this address to vrrpOperationsPrimaryIpAddr  
            while transitioning to master state. For backup  
            routers, this is the IP address listed as the source in 
            VRRP advertisement last received by this virtual  
            router."  
        REFERENCE " RFC 3768" 
        ::= { vrrpOperationsEntry 7 }  
         
    vrrpOperationsPrimaryIpAddr OBJECT-TYPE  
        SYNTAX       InetAddress  
        MAX-ACCESS   read-create  
        STATUS       current  
        DESCRIPTION  
            "In the case where there are more than one IP  
            Address (associated IP addresses) for a given  
            `ifIndex', this object is used to specify the IP  
            address that will become the 
            vrrpOperationsMasterIpAddr', should the virtual router  
            transition from backup state to master."  
        ::= { vrrpOperationsEntry 8 }  
     
    vrrpOperationsAdvInterval OBJECT-TYPE  
        SYNTAX       TimeInterval (1..4096)  
        UNITS        "centiseconds"  
        MAX-ACCESS   read-create  
        STATUS       current  
        DESCRIPTION  
            "The time interval, in centiseconds, between sending  
            advertisement messages. Only the master router sends  
            VRRP advertisements."  
        REFERENCE " RFC 3768 section 5.3.7" 
        DEFVAL       { 100}  
        ::= { vrrpOperationsEntry 9 }  
     
    vrrpOperationsPreemptMode OBJECT-TYPE  
        SYNTAX       TruthValue  
        MAX-ACCESS   read-create  
        STATUS       current  
        DESCRIPTION  
            "Controls whether a higher priority virtual router will 
            preempt a lower priority master."  
        REFERENCE " RFC 3768 section 6.1" 
        DEFVAL       { true }  
        ::= { vrrpOperationsEntry 10 } 
 
    vrrpOperationsAcceptMode OBJECT-TYPE  
        SYNTAX       TruthValue  
        MAX-ACCESS   read-create  
        STATUS       current  
        DESCRIPTION  
            "Controls whether a virtual router in Master state  
            will accept packets addressed to the address owner's  
            IPv6 address as its own if it is not the IPv6 address  
            owner.  Default is False. 
            This object is not relevant for rows representing VRRP 
            over IPv4 and should be set to false."  
        DEFVAL       { false }  
        ::= { vrrpOperationsEntry 11 }   
     
    vrrpOperationsUpTime OBJECT-TYPE  
        SYNTAX       TimeStamp  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "This is the value of the `sysUpTime' object when this  
            virtual router (i.e., the `vrrpOperationsState')  
            transitioned out of `initialized'."  
        REFERENCE " RFC 3768 section 6.1" 
        ::= { vrrpOperationsEntry 12 }  
 
    vrrpOperationsStorageType OBJECT-TYPE 
       SYNTAX      StorageType 
       MAX-ACCESS  read-create 
       STATUS      current 
       DESCRIPTION 
           "The storage type for this conceptual row. Write access 
           is not required. It is optional to support nonVolatile  
           StorageType enumeration." 
       REFERENCE " RFC4181 section 4.6.4" 
       DEFVAL       { nonVolatile } 
       ::= { vrrpOperationsEntry 13 } 
     
    vrrpOperationsRowStatus OBJECT-TYPE  
        SYNTAX       RowStatus  
        MAX-ACCESS   read-create  
        STATUS       current  
        DESCRIPTION  
            "The RowStatus variable should be used in accordance to 
            installation and removal conventions for conceptual  
            rows. When `vrrpOperationsRowStatus' is set to  
            active(1), no other objects in the conceptual row can 
            be modified. 
     
            To create a row in this table, a manager sets this  
            object to either createAndGo(4) or createAndWait(5).  
            Until instances of all corresponding columns are  
            appropriately configured, the value of the  
            corresponding instance of the `vrrpOperationsRowStatus' 
            column will be read as notReady(3).   
            In particular, a newly created row cannot be made  
            active(1) until (minimally) the corresponding instance  
            of vrrpOperationsInetAddrType, vrrpOperationsVrId and  
            vrrpOperationsPrimaryIpAddr has been set and there is  
            at least one active row in the  
            `vrrpAssociatedIpAddrTable' defining an associated  
            IP address. 
 
            notInService(2) should be used to administratively  
            bring the row down. 
 
            A typical order of operation to add a row is: 
            1. Create a row in vrrpOperationsTable with  
            createAndWait(5). 
            2. Create one or more corresponding rows in 
            vrrpAssociatedIpAddrTable. 
            3. Populate the vrrpOperationsEntry. 
            4. set vrrpOperationsRowStatus to active(1). 
 
            A typical order of operation to delete an entry is: 
            1. Set vrrpOperationsRowStatus to notInService(2). 
            2. Set the corresponding rows in  
            vrrpAssociatedIpAddrTable to destroy(6) to delete the  
            entry.  
            3. set vrrpOperationsRowStatus to destroy(6) to delete  
            the entry."  
        ::= { vrrpOperationsEntry 14 }  
 
   --  
   --  VRRP Associated Address Table 
   --  
     
    vrrpAssociatedIpAddrTable OBJECT-TYPE  
        SYNTAX       SEQUENCE OF VrrpAssociatedIpAddrEntry  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "The table of addresses associated with this virtual  
             router."  
        ::= { vrrpOperations 8 }  
     
    vrrpAssociatedIpAddrEntry OBJECT-TYPE  
        SYNTAX       VrrpAssociatedIpAddrEntry  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "An entry in the table contains an IP address that is  
            associated with a virtual router.  The number of rows  
            for a given IP version, VrID and ifIndex will equal the  
            number of IP addresses associated (e.g., backed up) by  
            the virtual router (equivalent to  
            'vrrpOperationsIpAddrCount').  
     
            Rows in the table cannot be modified unless the value  
            of `vrrpOperationsState' has transitioned to  
            `initialize'." 
     
        INDEX    { vrrpOperationsInetAddrType, vrrpOperationsVrId, 
                   ifIndex, vrrpAssociatedIpAddr } 
 
 
        ::= { vrrpAssociatedIpAddrTable 1 }  
     
    VrrpAssociatedIpAddrEntry ::=  
        SEQUENCE {  
            vrrpAssociatedIpAddr  
                InetAddress,  
            vrrpAssociatedStorageType 
                StorageType, 
            vrrpAssociatedIpAddrRowStatus  
                RowStatus  
    }  
         
    vrrpAssociatedIpAddr OBJECT-TYPE  
        SYNTAX       InetAddress (SIZE(0|4|16)) 
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "The assigned IP addresses that a virtual router is  
            responsible for backing up. 
            The size of this object is either 4 or 16 depending on  
            vrrpOperationsInetAddrType."  
        REFERENCE "RFC 3768 Section 5.3.9" 
        ::= { vrrpAssociatedIpAddrEntry 1 }  
 
   vrrpAssociatedStorageType OBJECT-TYPE 
       SYNTAX      StorageType 
       MAX-ACCESS  read-create 
       STATUS      current 
       DESCRIPTION 
           "The storage type for this conceptual row. Write access  
           is not required. It is optional to support nonVolatile  
           StorageType enumeration." 
       REFERENCE " RFC4181 section 4.6.4" 
       DEFVAL       { nonVolatile } 
       ::= { vrrpAssociatedIpAddrEntry 2 } 
     
    vrrpAssociatedIpAddrRowStatus OBJECT-TYPE  
        SYNTAX       RowStatus  
        MAX-ACCESS   read-create  
        STATUS       current  
        DESCRIPTION  
            "The RowStatus variable, used according to  
            installation and removal conventions for conceptual  
            rows. To create a row in this table, a manager sets  
            this object to either createAndGo(4) or  
            createAndWait(5). Setting this object to active(1)  
            results in the addition of an associated address for a  
            virtual router. Setting this object to notInService(2)  
            results in administratively bringing down the row. 
 
            Destroying the entry or setting it to destroy(6)  
            removes the associated address from the virtual router. 
            The use of other values is implementation-dependent. 
 
            Only vrrpAssociatedStorageType can be modified when the  
            row is in active(1) state for Implementations  
            supporting write access to vrrpAssociatedStorageType 
 
            Implementations should not allow deletion of the last 
            row corresponding to an active row in  
            vrrpOperationsTable. 
 
            Refer to description of vrrpOperationsRowStatus for a  
            typical row creation and deletion scenarios."  
        ::= { vrrpAssociatedIpAddrEntry 3 }  
     
   --  
   --  VRRP Router Statistics  
   --  
     
    vrrpRouterChecksumErrors OBJECT-TYPE  
 
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of VRRP packets received with an 
            invalid VRRP checksum value."  
        REFERENCE "RFC3768 Section 5.3.8" 
        ::= { vrrpStatistics 1 }  
     
    vrrpRouterVersionErrors OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of VRRP packets received with an  
            unknown or unsupported version number."  
        REFERENCE "RFC3768 Section 5.3.1" 
        ::= { vrrpStatistics 2 }  
     
    vrrpRouterVrIdErrors OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
       STATUS       current  
        DESCRIPTION  
            "The total number of VRRP packets received with an  
            invalid VRID for this virtual router."  
        REFERENCE "RFC3768 Section 5.3.3" 
        ::= { vrrpStatistics 3 }  
 
   --  
   --  VRRP Router Statistics Table  
   --  
     
   vrrpRouterStatisticsTable OBJECT-TYPE  
        SYNTAX       SEQUENCE OF VrrpRouterStatisticsEntry  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "Table of virtual router statistics."  
        ::= { vrrpStatistics 5 }  
     
    vrrpRouterStatisticsEntry OBJECT-TYPE  
        SYNTAX       VrrpRouterStatisticsEntry  
        MAX-ACCESS   not-accessible  
        STATUS       current  
        DESCRIPTION  
            "An entry in the table, containing statistics  
            information about a given virtual router."  
        AUGMENTS    { vrrpOperationsEntry }  
        ::= { vrrpRouterStatisticsTable 1 }  
 
    VrrpRouterStatisticsEntry ::=  
        SEQUENCE {  
            vrrpStatisticsMasterTransitions   
                Counter32,  
            vrrpStatisticsRcvdAdvertisements  
                Counter32,  
            vrrpStatisticsAdvIntervalErrors  
                Counter32,  
            vrrpStatisticsIpTtlErrors  
                Counter32,  
            vrrpStatisticsRcvdPriZeroPackets  
                Counter32,  
            vrrpStatisticsSentPriZeroPackets  
                Counter32,  
            vrrpStatisticsRcvdInvalidTypePkts  
                Counter32,  
            vrrpStatisticsAddressListErrors  
                Counter32,  
            vrrpStatisticsPacketLengthErrors  
                Counter32,  
            vrrpStatisticsRcvdInvalidAuthentications 
                 Counter32, 
            vrrpStatisticsDiscontinuityTime  
                 TimeStamp,  
            vrrpStatisticsRefreshRate 
                 Unsigned32 
        }  
     
     
    vrrpStatisticsMasterTransitions OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of times that this virtual router's  
            state has transitioned to MASTER.   
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
     
        ::= { vrrpRouterStatisticsEntry 1 }  
 
    vrrpStatisticsRcvdAdvertisements OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of VRRP advertisements received by  
            this virtual router.   
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
     
        ::= { vrrpRouterStatisticsEntry 2 }  
     
    vrrpStatisticsAdvIntervalErrors OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of VRRP advertisement packets  
            received for which the advertisement interval is  
            different than the one configured for the local virtual 
            router. 
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
     
        ::= { vrrpRouterStatisticsEntry 3 }  
     
    vrrpStatisticsIpTtlErrors OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current   
        DESCRIPTION  
            "The total number of VRRP packets received by the  
            Virtual router with IPv4 TTL (for VRRP over IPv4) or  
            IPv6 Hop Limit (for VRRP over IPv6) not equal to 255. 
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
        REFERENCE "RFC3768 Section 5.2.3" 
        ::= { vrrpRouterStatisticsEntry 4 } 
 
    vrrpStatisticsRcvdPriZeroPackets OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of VRRP packets received by the  
            virtual router with a priority of '0'.   
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
        REFERENCE "RFC3768 Section 5.3.4" 
        ::= { vrrpRouterStatisticsEntry 5 }  
     
    vrrpStatisticsSentPriZeroPackets OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of VRRP packets sent by the virtual  
            router with a priority of '0'.   
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
        REFERENCE "RFC3768 Section 5.3.4" 
        ::= { vrrpRouterStatisticsEntry 6 }  
     
    vrrpStatisticsRcvdInvalidTypePkts OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
 
 
        STATUS       current  
        DESCRIPTION  
            "The number of VRRP packets received by the virtual  
            router with an invalid value in the 'type' field.   
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."   
        ::= { vrrpRouterStatisticsEntry 7 }  
     
    vrrpStatisticsAddressListErrors OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of packets received for which the  
            address list does not match the locally configured list 
            for the virtual router.   
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
        ::= { vrrpRouterStatisticsEntry 8 }  
     
    vrrpStatisticsPacketLengthErrors OBJECT-TYPE  
        SYNTAX       Counter32  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "The total number of packets received with a packet  
            length less than the length of the VRRP header.   
     
            Discontinuities in the value of this counter can occur  
            at re-initialization of the management system, and at  
            other times as indicated by the value of  
            vrrpStatisticsDiscontinuityTime."  
     
        ::= { vrrpRouterStatisticsEntry 9 }  
 
   vrrpStatisticsRcvdInvalidAuthentications OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       current 
     DESCRIPTION 
         "The total number of packets received with an unknown 
         authentication type." 
     REFERENCE "RFC3768 Section 5.3.6" 
     ::= { vrrpRouterStatisticsEntry 10 }    
 
     
   vrrpStatisticsDiscontinuityTime OBJECT-TYPE  
       SYNTAX     TimeStamp  
       MAX-ACCESS read-only  
       STATUS     current  
       DESCRIPTION  
           "The value of sysUpTime on the most recent occasion at  
            which any one or more of this entry's counters suffered 
            a discontinuity.  
     
            If no such discontinuities have occurred since the last 
            re-initialization of the local management subsystem,  
            then this object contains a zero value." 
     
       ::= { vrrpRouterStatisticsEntry 11 }  
     
   vrrpStatisticsRefreshRate OBJECT-TYPE  
       SYNTAX     Unsigned32  
       UNITS "milli-seconds"  
       MAX-ACCESS read-only 
       STATUS     current  
       DESCRIPTION  
           "The minimum reasonable polling interval for this entry. 
            This object provides an indication of the minimum  
            Amount of time required to update the counters in this  
            entry." 
 
       ::= { vrrpRouterStatisticsEntry 12 }  

   --  
   --   Notification Definitions  
   --  
   vrrpNotifications   OBJECT IDENTIFIER ::= { vrrpMIB 0 }  
     
   ---  
   --- Objects used in the notifications  
   ---  
 
   vrrpNewMasterReason OBJECT-TYPE  
        SYNTAX        INTEGER { 
            notmaster (0),  
            priority  (1),  
            preempted (2),  
            masterNoResponse (3)  
        }  
        MAX-ACCESS   read-only  
        STATUS       current  
        DESCRIPTION  
            "This indicates the reason for vrrpNewMaster trap.  
            Used by vrrpTrapNewMaster trap. The object can be  
            polled if the vrrpNewMaster trap is lost to identify  
            the reason for transmission. Backup router should  
            return notmaster(0) when pooled. "  
        ::= { vrrpOperations 9 }  
     
   vrrpTrapProtoErrReason OBJECT-TYPE  
        SYNTAX        INTEGER {  
            hopLimitError (0),  
            versionError  (1),  
            checksumError (2),  
            vridError(3)  
        }  
        MAX-ACCESS   accessible-for-notify  
        STATUS       current  
        DESCRIPTION  
            "This indicates the reason for protocol error trap.  
            Used by vrrpTrapProtoError trap."  
        ::= { vrrpOperations 10 }  
 
     
    vrrpTrapNewMaster NOTIFICATION-TYPE  
        OBJECTS      { vrrpOperationsMasterIpAddr,  
                       vrrpNewMasterReason  
                     }  
        STATUS       current  
        DESCRIPTION  
            "The newMaster trap indicates that the sending agent  
            has transitioned to 'Master' state."  
        ::= { vrrpNotifications 1 }  
    
    vrrpTrapProtoError NOTIFICATION-TYPE  
        OBJECTS      { vrrpTrapProtoErrReason  
                     }  
        STATUS       current  
        DESCRIPTION  
            "The error trap indicates that the sending agent has  
            encountered the protocol error indicated by  
            vrrpTrapProtoErrorReason."  
        ::= { vrrpNotifications 3 }  
 
 
   --    
   --  deprecated objects follow.  
   --    

   --  vrrpOperTable(3) & vrrpAssoIpAddrTable(4) have been   
   --  deprecated and should not be used.  
 
 
vrrpOperTable OBJECT-TYPE 
     SYNTAX       SEQUENCE OF VrrpOperEntry 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "Operations table for a VRRP router which consists of a 
          sequence (i.e., one or more conceptual rows) of 
          'vrrpOperEntry' items. 
 
          This table has been deprecated as a new IP version  
          neutral 'vrrpOperationsTable' has been added. " 
 
     ::= { vrrpOperations 3 } 
 
vrrpOperEntry OBJECT-TYPE 
     SYNTAX       VrrpOperEntry 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "An entry in the vrrpOperTable containing the operational 
          characteristics of a virtual router.  On a VRRP router, 
          a given virtual router is identified by a combination 
          of the IF index and VRID. 
 
          Rows in the table cannot be modified unless the value 
          of `vrrpOperAdminState' is `disabled' and the 
          `vrrpOperState' has transitioned to `initialize'. 
 
          This object is deprecated in favor of the IP Version  
          independent object, vrrpOperationsEntry" 
 
     INDEX    { ifIndex, vrrpOperVrId } 
     ::= { vrrpOperTable 1 } 
 
VrrpOperEntry ::= 
     SEQUENCE { 
         vrrpOperVrId 
             VrId, 
         vrrpOperVirtualMacAddr 
             MacAddress, 
         vrrpOperState 
             INTEGER, 
         vrrpOperAdminState 
             INTEGER, 
         vrrpOperPriority 
             Integer32, 
         vrrpOperIpAddrCount 
             Integer32, 
         vrrpOperMasterIpAddr 
             IpAddress, 
         vrrpOperPrimaryIpAddr 
             IpAddress, 
         vrrpOperAuthType 
             INTEGER, 
         vrrpOperAuthKey 
             OCTET STRING, 
         vrrpOperAdvertisementInterval 
             Integer32, 
         vrrpOperPreemptMode 
             TruthValue, 
         vrrpOperVirtualRouterUpTime 
             TimeStamp, 
         vrrpOperProtocol 
             INTEGER, 
         vrrpOperRowStatus 
             RowStatus 
 } 
 
 vrrpOperVrId OBJECT-TYPE 
     SYNTAX       VrId 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "This object contains the Virtual Router Identifier  
         (VRID). 
         This object is deprecated in favor of the IP Version  
         independent object, vrrpOperationsVrId " 
     ::= { vrrpOperEntry 1 } 
 
 vrrpOperVirtualMacAddr OBJECT-TYPE 
     SYNTAX       MacAddress 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The virtual MAC address of the virtual router.  Although  
         this object can be derived from the 'vrrpOperVrId' object, 
         it is defined so that it is easily obtainable by a  
         management application and can be included in VRRP-related  
         SNMP traps. 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsVirtualMacAddr." 
     ::= { vrrpOperEntry 2 } 
 
 vrrpOperState OBJECT-TYPE 
     SYNTAX       INTEGER { 
         initialize(1), 
         backup(2), 
         master(3) 
     } 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
 
     DESCRIPTION 
         "The current state of the virtual router. This object has 
         three defined values: 
 
           - `initialize', which indicates that all the 
             virtual router is waiting for a startup event. 
 
           - `backup', which indicates the virtual router is 
             monitoring the availability of the master router. 
 
           - `master', which indicates that the virtual router 
             is forwarding packets for IP addresses that are 
             associated with this router. 
 
         Setting the `vrrpOperAdminState' object (below) initiates 
         transitions in the value of this object. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsState." 
     ::= { vrrpOperEntry 3 } 
 
 vrrpOperAdminState OBJECT-TYPE 
     SYNTAX       INTEGER { 
         up(1), 
         down(2) 
     } 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
        "This object will enable/disable the virtual router 
        function. 
         
        Setting the value to `up', will transition the state of 
        the virtual router from `initialize' to `backup' or 
        `master', depending on the value of `vrrpOperPriority'. 
         
        Setting the value to `down', will transition the router 
        from `master' or `backup' to `initialize'.  State 
        transitions may not be immediate; they sometimes depend on 
        other factors, such as the interface (IF) state. 
         
        The `vrrpOperAdminState' object must be set to `down' prior 
        to modifying the other read-create objects in the 
        conceptual row.  The value of the `vrrpOperRowStatus' 
        object (below) must be `active', signifying that the 
        conceptual row is valid (i.e., the objects are correctly 
        set), in order for this object to be set to `up'. 
         
         This object is deprecated in favor of the IP Version  
        Independent object, vrrpOperationsState." 
     DEFVAL    { down } 
     ::= { vrrpOperEntry 4 } 
 
 vrrpOperPriority OBJECT-TYPE 
     SYNTAX       Integer32 (0..255) 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
         "This object specifies the priority to be used for the 
         virtual router master election process.  Higher values  
         imply higher priority. 
 
         A priority of '0', although not settable, is sent by 
         the master router to indicate that this router has ceased 
         to participate in VRRP and a backup virtual router should 
         transition to become a new master. 
 
         A priority of 255 is used for the router that owns the 
         associated IP address(es). 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsPriority." 
     DEFVAL       { 100 } 
     ::= { vrrpOperEntry 5 } 
 
 vrrpOperIpAddrCount OBJECT-TYPE 
     SYNTAX       Integer32 (0..255) 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The number of IP addresses that are associated with this 
         virtual router.  This number is equal to the number of  
         rows in the vrrpAssoIpAddrTable that correspond to a  
         given IF index/VRID pair. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsAddrCount." 
     ::= { vrrpOperEntry 6 } 
 
 vrrpOperMasterIpAddr OBJECT-TYPE 
     SYNTAX       IpAddress 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The master router's real (primary) IP address.  This is 
         the IP address listed as the source in VRRP advertisement 
         last received by this virtual router. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsMasterIpAddr." 
     ::= { vrrpOperEntry 7 } 
 
 vrrpOperPrimaryIpAddr OBJECT-TYPE 
     SYNTAX       IpAddress 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
         "In the case where there is more than one IP address for 
         a given `ifIndex', this object is used to specify the IP 
         address that will become the `vrrpOperMasterIpAddr',  
         should the virtual router transition from backup to  
         master. If this object is set to 0.0.0.0, the IP address  
         which is numerically lowest (of all the associated IP  
         address for the interface) will be selected. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsPrimaryIpAddr." 
     DEFVAL       { '00000000'H } -- 0.0.0.0 
     ::= { vrrpOperEntry 8 } 
 
 vrrpOperAuthType OBJECT-TYPE 
     SYNTAX       INTEGER { 
         noAuthentication(1),       -- VRRP protocol exchanges are 
                                    -- not authenticated. 
         simpleTextPassword(2),     -- Exchanges are authenticated 
                                    -- by a clear text password. 
         ipAuthenticationHeader(3)  -- Exchanges are authenticated 
                                    -- using the IP authentication 
                                    -- header. 
     } 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
 
         "Authentication type used for VRRP protocol exchanges  
         between virtual routers.  This value of this object is the  
         same for a given ifIndex. 
 
         New enumerations to this list can only be added via a new 
         RFC on the standards track. 
 
         This object is deprecated in the IP Version MIB." 
     DEFVAL       { noAuthentication } 
     ::= { vrrpOperEntry 9 } 
 
 vrrpOperAuthKey OBJECT-TYPE 
     SYNTAX       OCTET STRING (SIZE (0..16)) 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
         "The Authentication Key.  This object is set according to 
         the value of the 'vrrpOperAuthType' object 
         ('simpleTextPassword' or 'ipAuthenticationHeader').  If  
         the length of the value is less than 16 octets, the agent  
         will left adjust and zero fill to 16 octets. The value of  
         this object is the same for a given ifIndex. 
 
         When read, vrrpOperAuthKey always returns an Octet String 
         of length zero. 
 
         This object is deprecated in the IP Version MIB." 
     ::= { vrrpOperEntry 10 } 
 
 vrrpOperAdvertisementInterval OBJECT-TYPE 
     SYNTAX       Integer32 (1..255) 
     UNITS        "seconds" 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
         "The time interval, in seconds, between sending 
         advertisement messages.  Only the master router sends 
         VRRP advertisements. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsAdvInterval. " 
     DEFVAL       { 1 } 
     ::= { vrrpOperEntry 11 } 
 
 vrrpOperPreemptMode OBJECT-TYPE 
     SYNTAX       TruthValue 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
         "Controls whether a higher priority virtual router will 
         preempt a lower priority master. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsPreemptMode. " 
     DEFVAL       { true } 
     ::= { vrrpOperEntry 12 } 
 
 vrrpOperVirtualRouterUpTime OBJECT-TYPE 
 
     SYNTAX       TimeStamp 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "This is the value of the `sysUpTime' object when this 
         virtual router (i.e., the `vrrpOperState') transitioned 
         out of `initialized'.  
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsUpTime." 
     ::= { vrrpOperEntry 13 } 
 
 vrrpOperProtocol OBJECT-TYPE 
     SYNTAX   INTEGER { 
         ip (1), 
         bridge (2), 
         decnet (3), 
         other (4) 
     } 
     MAX-ACCESS read-create 
     STATUS     deprecated 
     DESCRIPTION 
         "The particular protocol being controlled by this Virtual 
         Router. 
 
         New enumerations to this list can only be added via a new 
         RFC on the standards track. 
 
         This object is deprecated in the IP Version Independent  
         MIB." 
     DEFVAL { ip } 
     ::= { vrrpOperEntry 14 } 
 
 vrrpOperRowStatus OBJECT-TYPE 
     SYNTAX       RowStatus 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
         "The RowStatus variable, used in accordance to  
         installation and removal conventions for conceptual rows.  
         The RowStatus of a currently active row in the  
         vrrpOperTable is constrained by the operational state of  
         the corresponding virtual router. 
         When `vrrpOperRowStatus' is set to active(1), no other 
         objects in the conceptual row, with the exception of 
         `vrrpOperAdminState', can be modified. Prior to setting  
         the `vrrpOperRowStatus' object from `active' to a  
         different value, the `vrrpOperAdminState' object must be  
         set to `down' and the `vrrpOperState' object be  
         transitioned to `initialize'. 
 
         To create a row in this table, a manager sets this object 
         to either createAndGo(4) or createAndWait(5).  Until  
         instances of all corresponding columns are appropriately  
         configured, the value of the corresponding instance of the  
         `vrrpOperRowStatus' column will be read as notReady(3). 
 
         In particular, a newly created row cannot be made  
         active(1) until (minimally) the corresponding instance of 
         `vrrpOperVrId' has been set and there is at least one  
         active row in the `vrrpAssoIpAddrTable' defining an  
         associated IP address for the virtual router. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpOperationsRowStatus. " 
 
     ::= { vrrpOperEntry 15 } 
 
--  
--  Deprecated VRRP Associated IP Address Table 
--  
 
 vrrpAssoIpAddrTable OBJECT-TYPE 
     SYNTAX       SEQUENCE OF VrrpAssoIpAddrEntry 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "The table of addresses associated with this virtual 
          router. 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpAssociatedIpAddrTable. " 
     ::= { vrrpOperations 4 } 
 
 vrrpAssoIpAddrEntry OBJECT-TYPE 
     SYNTAX       VrrpAssoIpAddrEntry 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "An entry in the table contains an IP address that is 
         associated with a virtual router.  The number of rows for 
         a given ifIndex and VrId will equal the number of IP 
         addresses associated (e.g., backed up) by the virtual 
         router (equivalent to 'vrrpOperIpAddrCount'). 
 
         Rows in the table cannot be modified unless the value 
         of `vrrpOperAdminState' is `disabled' and the 
         `vrrpOperState' has transitioned to `initialize'. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpAssociatedIpAddrEntry." 
 
     INDEX    { ifIndex, vrrpOperVrId, vrrpAssoIpAddr } 
     ::= { vrrpAssoIpAddrTable 1 } 
 
 VrrpAssoIpAddrEntry ::= 
     SEQUENCE { 
         vrrpAssoIpAddr 
             IpAddress, 
         vrrpAssoIpAddrRowStatus 
             RowStatus 
 } 
 
 vrrpAssoIpAddr OBJECT-TYPE 
     SYNTAX       IpAddress 
 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "The assigned IP addresses that a virtual router is 
         responsible for backing up. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpAssociatedIpAddr." 
     ::= { vrrpAssoIpAddrEntry 1 } 
 
 vrrpAssoIpAddrRowStatus OBJECT-TYPE 
     SYNTAX       RowStatus 
     MAX-ACCESS   read-create 
     STATUS       deprecated 
     DESCRIPTION 
         "The row status variable, used according to installation 
         and removal conventions for conceptual rows.  Setting this 
         object to active(1) or createAndGo(4) results in the 
         addition of an associated address for a virtual router. 
         Destroying the entry or setting it to notInService(2) 
         removes the associated address from the virtual router. 
         The use of other values is implementation-dependent. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpAssociatedIpAddrRowStatus." 
     ::= { vrrpAssoIpAddrEntry 2 } 
 
  
   -- 
   -- Deprecated vrrpRouterStatsTable. 
   -- 
 
vrrpRouterStatsTable OBJECT-TYPE 
     SYNTAX       SEQUENCE OF VrrpRouterStatsEntry 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "Table of virtual router statistics. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpRouterStatisticsTable." 
     ::= { vrrpStatistics 4 } 
 
 vrrpRouterStatsEntry OBJECT-TYPE 
     SYNTAX       VrrpRouterStatsEntry 
     MAX-ACCESS   not-accessible 
     STATUS       deprecated 
     DESCRIPTION 
         "An entry in the table, containing statistics information 
         about a given virtual router. 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpRouterStatisticsEntry." 
     AUGMENTS    { vrrpOperEntry } 
     ::= { vrrpRouterStatsTable 1 } 
 
 VrrpRouterStatsEntry ::= 
     SEQUENCE { 
         vrrpStatsBecomeMaster 
             Counter32, 
         vrrpStatsAdvertiseRcvd 
             Counter32, 
         vrrpStatsAdvertiseIntervalErrors 
             Counter32, 
         vrrpStatsAuthFailures 
             Counter32, 
         vrrpStatsIpTtlErrors 
             Counter32, 
         vrrpStatsPriorityZeroPktsRcvd 
             Counter32, 
         vrrpStatsPriorityZeroPktsSent 
             Counter32, 
         vrrpStatsInvalidTypePktsRcvd 
             Counter32, 
         vrrpStatsAddressListErrors 
             Counter32, 
         vrrpStatsInvalidAuthType 
             Counter32, 
         vrrpStatsAuthTypeMismatch 
             Counter32, 
         vrrpStatsPacketLengthErrors 
             Counter32 
     } 
 
 vrrpStatsBecomeMaster OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of times that this virtual router's  
         state has transitioned to MASTER. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsMasterTransitions." 
     ::= { vrrpRouterStatsEntry 1 } 
 
 vrrpStatsAdvertiseRcvd OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of VRRP advertisements received by this 
         virtual router. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsRcvdAdvertisements." 
     ::= { vrrpRouterStatsEntry 2 } 
 
 vrrpStatsAdvertiseIntervalErrors OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of VRRP advertisement packets received 
         for which the advertisement interval is different than the 
         one configured for the local virtual router. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsAdvIntervalErrors." 
     ::= { vrrpRouterStatsEntry 3 } 
 
 vrrpStatsAuthFailures OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of VRRP packets received that do not  
         pass the authentication check. 
 
         This object is deprecated in the IP Version MIB." 
     ::= { vrrpRouterStatsEntry 4 } 
 
 vrrpStatsIpTtlErrors OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
 
     DESCRIPTION 
         "The total number of VRRP packets received by the virtual 
         router with IP TTL (Time-To-Live) not equal to 255. 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsIpTtlErrors." 
 
     ::= { vrrpRouterStatsEntry 5 } 
 
 vrrpStatsPriorityZeroPktsRcvd OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of VRRP packets received by the virtual 
         router with a priority of '0'. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsRcvdPriZeroPackets." 
     ::= { vrrpRouterStatsEntry 6 } 
 
 vrrpStatsPriorityZeroPktsSent OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of VRRP packets sent by the virtual  
         router with a priority of '0'. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsSentPriZeroPackets. " 
     ::= { vrrpRouterStatsEntry 7 } 
 
 vrrpStatsInvalidTypePktsRcvd OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The number of VRRP packets received by the virtual router 
         with an invalid value in the 'type' field. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsRcvdInvalidTypePkts. " 
     ::= { vrrpRouterStatsEntry 8 } 
 
 vrrpStatsAddressListErrors OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of packets received for which the  
         address list does not match the locally configured list  
         for the virtual router. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsAddressListErrors." 
     ::= { vrrpRouterStatsEntry 9 } 
 
   vrrpStatsInvalidAuthType OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of packets received with an unknown 
         authentication type. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsPacketLengthErrors." 
     ::= { vrrpRouterStatsEntry 10 } 
 
   vrrpStatsAuthTypeMismatch OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of packets received with 'Auth Type' not 
         equal to the locally configured authentication method 
         (`vrrpOperAuthType'). 
 
         This object is deprecated in favor of the IP Version  
         Independent object,  
         vrrpStatisticsRcvdInvalidAuthentications." 
     ::= { vrrpRouterStatsEntry 11 } 
 
   vrrpStatsPacketLengthErrors OBJECT-TYPE 
     SYNTAX       Counter32 
     MAX-ACCESS   read-only 
     STATUS       deprecated 
     DESCRIPTION 
         "The total number of packets received with a packet length 
         less than the length of the VRRP header. 
 
         This object is deprecated in favor of the IP Version  
         Independent object, vrrpStatisticsPacketLengthErrors. " 
     ::= { vrrpRouterStatsEntry 12 } 
 
     
 
 vrrpTrapPacketSrc OBJECT-TYPE 
     SYNTAX       IpAddress 
     MAX-ACCESS   accessible-for-notify 
     STATUS       deprecated 
     DESCRIPTION 
         "The IP address of an inbound VRRP packet. Used by 
          vrrpTrapAuthFailure trap. 
 
          This object is deprecated in the IP Version MIB. " 
     ::= { vrrpOperations 5 } 
 
  vrrpTrapAuthErrorType OBJECT-TYPE 
     SYNTAX        INTEGER { 
         invalidAuthType (1), 
         authTypeMismatch (2), 
         authFailure (3) 
     } 
     MAX-ACCESS   accessible-for-notify 
     STATUS       deprecated 
     DESCRIPTION 
         "Potential types of configuration conflicts. 
         Used by vrrpAuthFailure trap. 
 
         This object is deprecated in the IP Version MIB. " 
 
     ::= { vrrpOperations 6 } 


   ---  
   --- vrrpAuthFailureTrap (2) has been deprecated.  
   --- 
 
   vrrpTrapAuthFailure NOTIFICATION-TYPE 
     OBJECTS      { vrrpTrapPacketSrc, 
                    vrrpTrapAuthErrorType 
                  } 
     STATUS       deprecated 
     DESCRIPTION 
         "A vrrpAuthFailure trap signifies that a packet has 
         been received from a router whose authentication key 
         or authentication type conflicts with this router's 
         authentication key or authentication type.  Implementation 
         of this trap is optional. 
 
         This object is deprecated in the IP Version MIB. " 
     ::= { vrrpNotifications 2 } 
     
     
     
   --  
   --  Conformance Information  
   --  
     
    vrrpMIBCompliances  OBJECT IDENTIFIER ::= { vrrpConformance 1 } 
    vrrpMIBGroups       OBJECT IDENTIFIER ::= { vrrpConformance 2 } 
     
   --   
   -- Compliance Statements  
   --  
     

   vrrpMIBCompliance MODULE-COMPLIANCE 
     STATUS deprecated 
     DESCRIPTION 
        "This compliance is deprecated in favour of   
           vrrpModuleFullCompliance." 
     MODULE -- this module  
     MANDATORY-GROUPS  { 
         vrrpOperGroup, 
         vrrpStatsGroup, 
         vrrpTrapGroup, 
         vrrpNotificationGroup 
     } 
     OBJECT        vrrpOperPriority 
     WRITE-SYNTAX  Integer32 (1..255) 
     DESCRIPTION  "Setable values are from 1 to 255." 
 
     ::= { vrrpMIBCompliances 1 } 
     
    vrrpModuleFullCompliance MODULE-COMPLIANCE  
        STATUS current  
        DESCRIPTION  
 
           "The compliance statement for both VRRP for IPv4 and  
           VRRP for IPv6 implementations."  
     
        MODULE -- this module  
        MANDATORY-GROUPS  {  
            vrrpOperationsGroup,  
            vrrpStatisticsGroup,  
            vrrpTrapInfoGroup,  
            vrrpNotificationsGroup  
        }  
        OBJECT        vrrpOperationsPriority 
        WRITE-SYNTAX  Unsigned32 (1..254) 
        DESCRIPTION  "Setable values are from 1 to 254." 

        ::= { vrrpMIBCompliances 2 }    
  
    vrrpModuleReadOnlyCompliance MODULE-COMPLIANCE  
        STATUS current  
        DESCRIPTION  
           "When this MIB is implemented without support for read- 
           create (i.e. in read-only mode), then such an  
           implementation can claim read-only compliance. Such a  
           device can then be monitored but can not be configured  
           with this MIB."  
     
        MODULE -- this module  
        MANDATORY-GROUPS  {  
            vrrpOperationsGroup,  
            vrrpStatisticsGroup,  
            vrrpTrapInfoGroup,  
            vrrpNotificationsGroup  
        }  
     
        OBJECT        vrrpOperationsPriority 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 

        OBJECT        vrrpOperationsPrimaryIpAddr 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        OBJECT        vrrpOperationsAdvInterval 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        OBJECT        vrrpOperationsPreemptMode 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        OBJECT        vrrpOperationsAcceptMode 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        OBJECT        vrrpOperationsStorageType 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        OBJECT        vrrpOperationsRowStatus 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 

 
        OBJECT        vrrpAssociatedStorageType 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        OBJECT        vrrpAssociatedIpAddrRowStatus 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        OBJECT        vrrpNotificationCntl 
        MIN-ACCESS    read-only 
        DESCRIPTION  "Write access is not required." 
 
        ::= { vrrpMIBCompliances 3 } 

   --  
   -- Conformance Groups  
   --  
 
vrrpOperGroup  OBJECT-GROUP 
     OBJECTS  { 
         vrrpNodeVersion, 
         vrrpNotificationCntl, 
         vrrpOperVirtualMacAddr, 
         vrrpOperState, 
         vrrpOperAdminState, 
         vrrpOperPriority, 
         vrrpOperIpAddrCount, 
         vrrpOperMasterIpAddr, 
         vrrpOperPrimaryIpAddr, 
         vrrpOperAuthType, 
         vrrpOperAuthKey, 
         vrrpOperAdvertisementInterval, 
         vrrpOperPreemptMode, 
         vrrpOperVirtualRouterUpTime, 
         vrrpOperProtocol, 
         vrrpOperRowStatus, 
         vrrpAssoIpAddrRowStatus 
         } 
     STATUS deprecated 
     DESCRIPTION 
        "Conformance group for VRRP operations." 
     ::= { vrrpMIBGroups 1 } 
 
 vrrpStatsGroup  OBJECT-GROUP 
     OBJECTS  { 
         vrrpRouterChecksumErrors, 
         vrrpRouterVersionErrors, 
         vrrpRouterVrIdErrors, 
         vrrpStatsBecomeMaster, 
         vrrpStatsAdvertiseRcvd, 
         vrrpStatsAdvertiseIntervalErrors, 
         vrrpStatsAuthFailures, 
         vrrpStatsIpTtlErrors, 
         vrrpStatsPriorityZeroPktsRcvd, 
         vrrpStatsPriorityZeroPktsSent, 
         vrrpStatsInvalidTypePktsRcvd, 
         vrrpStatsAddressListErrors, 
         vrrpStatsInvalidAuthType, 
         vrrpStatsAuthTypeMismatch, 
         vrrpStatsPacketLengthErrors 
 
         } 
     STATUS deprecated 
     DESCRIPTION 
        "Conformance group for VRRP statistics." 
     ::= { vrrpMIBGroups 2 } 
  
 vrrpTrapGroup  OBJECT-GROUP 
     OBJECTS  { 
         vrrpTrapPacketSrc, 
         vrrpTrapAuthErrorType 
         } 
     STATUS deprecated 
     DESCRIPTION 
        "Conformance group for objects contained in VRRP  
        notifications." 
     ::= { vrrpMIBGroups 3 } 
 
 vrrpNotificationGroup NOTIFICATION-GROUP 
     NOTIFICATIONS { 
         vrrpTrapNewMaster, 
         vrrpTrapAuthFailure 
         } 
     STATUS deprecated 
     DESCRIPTION 
        "The VRRP MIB Notification Group." 
     ::= { vrrpMIBGroups 4 } 
 
 
 vrrpOperationsGroup   OBJECT-GROUP  
        OBJECTS  {  
            vrrpNotificationCntl,  
            vrrpOperationsVirtualMacAddr,  
            vrrpOperationsState,  
            vrrpOperationsPriority,  
            vrrpOperationsMasterIpAddr, 
            vrrpOperationsAdvInterval,  
            vrrpOperationsPreemptMode,  
            vrrpOperationsAcceptMode, 
            vrrpOperationsUpTime, 
            vrrpOperationsStorageType, 
            vrrpOperationsRowStatus,  
            vrrpOperationsAddrCount,  
            vrrpOperationsPrimaryIpAddr, 
            vrrpAssociatedStorageType, 
            vrrpAssociatedIpAddrRowStatus  
            }  
        STATUS current  
        DESCRIPTION  
 
           "Conformance group for VRRP over IPv4 and IPv6  
           operations."  
        ::= { vrrpMIBGroups 5 }  
 
     
 vrrpStatisticsGroup  OBJECT-GROUP  
        OBJECTS  {  
            vrrpRouterChecksumErrors,  
            vrrpRouterVersionErrors,  
            vrrpRouterVrIdErrors,  
            vrrpStatisticsMasterTransitions,  
            vrrpStatisticsRcvdAdvertisements,  
            vrrpStatisticsAdvIntervalErrors,  
            vrrpStatisticsRcvdPriZeroPackets,  
            vrrpStatisticsSentPriZeroPackets,  
            vrrpStatisticsRcvdInvalidTypePkts,  
            vrrpStatisticsIpTtlErrors,  
            vrrpStatisticsAddressListErrors,   
            vrrpStatisticsPacketLengthErrors,  
            vrrpStatisticsRcvdInvalidAuthentications, 
            vrrpStatisticsDiscontinuityTime,  
            vrrpStatisticsRefreshRate 
            }  
        STATUS current  
        DESCRIPTION  
           "Conformance group for VRRP over IPv4 and IPv6  
           statistics."  
        ::= { vrrpMIBGroups 6 }  
  
  vrrpTrapInfoGroup  OBJECT-GROUP  
        OBJECTS  {  
            vrrpNewMasterReason,  
            vrrpTrapProtoErrReason  
            }  
        STATUS current  
        DESCRIPTION  
           "Conformance group for objects contained in VRRP   
            notifications."  
        ::= { vrrpMIBGroups 7 }  
     
 vrrpNotificationsGroup NOTIFICATION-GROUP  
        NOTIFICATIONS {  
            vrrpTrapNewMaster,  
            vrrpTrapProtoError  
            }  
        STATUS current  
        DESCRIPTION  
           "The VRRP MIB Notification Group."  
        ::= { vrrpMIBGroups 8 }  
     
END 
