--
-- Juniper Enterprise Specific MIB: Chassis MIB
-- 
-- Copyright (c) 1998-2008, Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--


JUNIPER-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
    Integer32, Gauge32, Counter32
        FROM SNMPv2-SMI
    DisplayString, TimeStamp, TimeInterval, TEXTUAL-CONVENTION, DateAndTime
        FROM SNMPv2-TC
    jnxMibs, jnxChassisTraps, jnxChassisOKTraps
        FROM JUNIPER-SMI;

jnxBoxAnatomy MODULE-IDENTITY

    LAST-UPDATED "201010220000Z" -- Fri Oct 22 00:00:00 2008 UTC
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
            "        Juniper Technical Assistance Center
		     Juniper Networks, Inc.
		     1194 N. Mathilda Avenue
		     Sunnyvale, CA 94089
		     E-mail: support@juniper.net"

    DESCRIPTION
            "The MIB modules representing Juniper Networks'
	    implementation of enterprise specific MIBs 
	    supported by a single SNMP agent."
    REVISION      "201010220000Z"
    DESCRIPTION
               "Added load average variables"
    REVISION      "200403230000Z"
    DESCRIPTION
               "Added chassis identification objects."
    REVISION     "200406300000Z"    -- July 30, 2004
    DESCRIPTION
               "Added following new traps for chassis
                alarm conditions: jnxFruFailed, jnxFruOffline
                and jnxFruOnline."
    REVISION     "200409170000Z"    -- Sep 17, 2004
    DESCRIPTION
               "Added new traps for chassis
                alarm condition jnxFruCheck."
    REVISION     "200507180000Z"    -- Jul 18, 2005
    DESCRIPTION
               "Added new fru type FEB in jnxFruType enumeration."
    REVISION     "200507190000Z"    -- Jul 19, 2005
    DESCRIPTION
               "Added new offline reason pfeVersionMismatch
                to jnxFruOfflineReason enumeration."
    REVISION     "200611200000Z"    -- Nov 20, 2006
    DESCRIPTION
               "Added new offline reason fruFebOffline
                to jnxFruOfflineReason enumeration."
    REVISION     "200807310000Z"    -- Jul 31, 2008
    DESCRIPTION
               "Added jnxBoxSystemDomainType object."
    REVISION     "200808010000Z"    -- Aug 01, 2008
    DESCRIPTION
               "Added new fru type PSD to jnxFruType enumeration and
                added jcsX chassis IDs to JnxChassisId enumeration."
    REVISION     "200812310000Z"    -- Dec 31, 2008
    DESCRIPTION "Added nodeX chassis IDs to JnxChassisId enumeration."
    REVISION     "200901090000Z"    -- Jan 09, 2009
    DESCRIPTION 
               "Added sfcX and lcc4-lcc15 chassis IDs to JnxChassisId
                enumeration."



    ::= { jnxMibs 1 }

--
-- Textual Conventions
--

JnxChassisId ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION  "Identifies a specific router chassis."
    SYNTAX       INTEGER {
                     unknown       (1),
                     singleChassis (2),
                     scc           (3),
                     lcc0          (4),
                     lcc1          (5),
                     lcc2          (6),
                     lcc3          (7),
                     jcs1          (8),
                     jcs2          (9),
                     jcs3          (10),
                     jcs4          (11),
                     node0         (12),
                     node1         (13),
                     sfc0          (14),
                     sfc1          (15),
                     sfc2          (16),
                     sfc3          (17),
                     sfc4          (18),
                     lcc4          (19),
                     lcc5          (20),
                     lcc6          (21),
                     lcc7          (22),
                     lcc8          (23),
                     lcc9          (24),
                     lcc10         (25),
                     lcc11         (26),
                     lcc12         (27),
                     lcc13         (28),
                     lcc14         (29),
                     lcc15         (30),
                     member0       (31),
                     member1       (32),
                     member2       (33),
                     member3       (34),
                     member4       (35),
                     member5       (36),
                     member6       (37),
                     member7       (38)
                 }



-- Juniper Box Anatomy MIB
--

-- Top level objects

    jnxBoxClass OBJECT-TYPE 
	SYNTAX		OBJECT IDENTIFIER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	        "The class of the box, indicating which product line
		the box is about, for example, 'Internet Router'."
	::= { jnxBoxAnatomy 1 }

    jnxBoxDescr OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The name, model, or detailed description of the box,
		indicating which product the box is about, for example
		'M40'."
	::= { jnxBoxAnatomy 2 }

    jnxBoxSerialNo OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The serial number of this subject, blank if unknown 
		or unavailable."
	::= { jnxBoxAnatomy 3 }

    jnxBoxRevision OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The revision of this subject, blank if unknown or
		unavailable."
	::= { jnxBoxAnatomy 4 }

    jnxBoxInstalled OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when the subject was last
		installed, up-and-running.  Zero if unknown or 
		already up-and-running when the agent was up."
	::= { jnxBoxAnatomy 5 }

--
-- Box Containers Table
--

    jnxContainersTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JnxContainersEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"A list of containers entries."
	::= { jnxBoxAnatomy 6 }

    jnxContainersEntry OBJECT-TYPE
	SYNTAX		JnxContainersEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"An entry of containers table."
	INDEX 	{ jnxContainersIndex }
	::= { jnxContainersTable 1 }

    JnxContainersEntry ::= SEQUENCE {
	    jnxContainersIndex		Integer32,
	    jnxContainersView		Integer32,
	    jnxContainersLevel		Integer32,
	    jnxContainersWithin		Integer32,
	    jnxContainersType		OBJECT IDENTIFIER,
	    jnxContainersDescr          DisplayString,
	    jnxContainersCount		Integer32
    }

    jnxContainersIndex OBJECT-TYPE
	SYNTAX		Integer32 (1..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The index for this entry."
	::= { jnxContainersEntry 1 }

    jnxContainersView OBJECT-TYPE
	SYNTAX		Integer32 (1..63)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The view(s) from which the specific container
		appears.

		This variable indicates that the specific container
		is embedded and accessible from the corresponding
		view(s).

		The value is a bit map represented as a sum.
		If multiple bits are set, the specified
		container(s) are located and accessible from 
		that set of views.

		The various values representing the bit positions
		and its corresponding views are:
		    1   front
		    2   rear
		    4   top
		    8   bottom
		   16   leftHandSide
		   32   rightHandSide

		Note 1: 
		LefHandSide and rightHandSide are referred
		to based on the view from the front.

		Note 2: 
		If the specified containers are scattered 
		around various views, the numbering is according
		to the following sequence:
		    front -> rear -> top -> bottom
			  -> leftHandSide -> rightHandSide
		For each view plane, the numbering sequence is
		first from left to right, and then from up to down.

		Note 3: 
		Even though the value in chassis hardware (e.g. 
		slot number) may be labelled from 0, 1, 2, and up,
		all the indices in MIB start with 1 (not 0) 
		according to network management convention."
	::= { jnxContainersEntry 2 }

    jnxContainersLevel OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The abstraction level of the box or chassis.
		It is enumerated from the outside to the inside, 
		from the outer layer to the inner layer.
		For example, top level (i.e. level 0) refers to 
		chassis frame, level 1 FPC slot within chassis 
		frame, level 2 PIC space within FPC slot."
	::= { jnxContainersEntry 3 }

    jnxContainersWithin OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The index of its next higher level container 
		housing	this entry.  The associated 
		jnxContainersIndex in the jnxContainersTable 
		represents its next higher level container."
	::= { jnxContainersEntry 4 }

    jnxContainersType OBJECT-TYPE
	SYNTAX		OBJECT IDENTIFIER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The type of this container."
	::= { jnxContainersEntry 5 }

    jnxContainersDescr OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The name or detailed description of this
		subject."
	::= { jnxContainersEntry 6 }

    jnxContainersCount OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The maximum number of containers of this level
		per container of the next higher level.  
		e.g. if there are six level 2 containers in 
		level 1 container, then jnxContainersCount for
		level 2 is six."
	::= { jnxContainersEntry 7 }

--
-- Box Contents Table
--

    jnxContentsLastChange OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when the box contents 
		table last changed.  Zero if unknown or already 
		existing when the agent was up."
	::= { jnxBoxAnatomy 7 }

    jnxContentsTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JnxContentsEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"A list of contents entries."
	::= { jnxBoxAnatomy 8 }

    jnxContentsEntry OBJECT-TYPE
	SYNTAX		JnxContentsEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"An entry of contents table."
	INDEX	{ jnxContentsContainerIndex, 
		  jnxContentsL1Index,
		  jnxContentsL2Index,
		  jnxContentsL3Index }
	::= { jnxContentsTable 1 }

    JnxContentsEntry ::= SEQUENCE {
	    jnxContentsContainerIndex	Integer32,
	    jnxContentsL1Index          Integer32,
	    jnxContentsL2Index          Integer32,
	    jnxContentsL3Index          Integer32,
	    jnxContentsType		OBJECT IDENTIFIER,
	    jnxContentsDescr		DisplayString,
	    jnxContentsSerialNo		DisplayString,
	    jnxContentsRevision		DisplayString,
	    jnxContentsInstalled	TimeStamp,
            jnxContentsPartNo           DisplayString,
            jnxContentsChassisId        JnxChassisId,
            jnxContentsChassisDescr     DisplayString,
            jnxContentsChassisCleiCode  DisplayString
    }

    jnxContentsContainerIndex OBJECT-TYPE
	SYNTAX		Integer32 (1..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The associated jnxContainersIndex in the 
		jnxContainersTable."
	::= { jnxContentsEntry 1 }
	
    jnxContentsL1Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level one index of the container
		housing this subject.  Zero if unavailable
		or inapplicable."
	::= { jnxContentsEntry 2 }

    jnxContentsL2Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level two index of the container
		housing this subject.  Zero if unavailable
		or inapplicable."
	::= { jnxContentsEntry 3 }

    jnxContentsL3Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level three index of the container
		housing this subject.  Zero if unavailable
		or inapplicable."
	::= { jnxContentsEntry 4 }

    jnxContentsType OBJECT-TYPE
	SYNTAX		OBJECT IDENTIFIER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The type of this subject.  zeroDotZero
		if unknown."
	::= { jnxContentsEntry 5 }

    jnxContentsDescr OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The name or detailed description of this
		subject."
	::= { jnxContentsEntry 6 }

    jnxContentsSerialNo OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The serial number of this subject, blank if 
		unknown or unavailable."
	::= { jnxContentsEntry 7 }

    jnxContentsRevision OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The revision of this subject, blank if unknown 
		or unavailable."
	::= { jnxContentsEntry 8 }

    jnxContentsInstalled OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when the subject was last 
		installed, up-and-running.  Zero if unknown
		or already up-and-running when the agent was up."
	::= { jnxContentsEntry 9 }

    jnxContentsPartNo OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The part number of this subject, blank if unknown 
		or unavailable."
	::= { jnxContentsEntry 10 }

    jnxContentsChassisId OBJECT-TYPE
        SYNTAX          JnxChassisId
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "Identifies the chassis on which the contents of this
                row exists."
        ::= { jnxContentsEntry 11 }

    jnxContentsChassisDescr OBJECT-TYPE
        SYNTAX          DisplayString (SIZE (0..255))
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "A textual description of the chassis on which the
                contents of this row exists."
        ::= { jnxContentsEntry 12 }

    jnxContentsChassisCleiCode OBJECT-TYPE
        SYNTAX          DisplayString (SIZE (0..255))
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The clei code of this subject, blank if unknown
                 or unavailable.

                 A CLEI code is an intelligent code that consists of 10
                 alphanumeric characters with 4 data elements.  The first data
                 element is considered the basic code with the first 2 characters
                 indicating the technology or equipment type, and the third and
                 fourth characters denoting the functional sub-category.  The
                 second data element represents the features, and its three
                 characters denote functional capabilities or changes.  The third
                 data element has one character and denotes a reference to a
                 manufacturer, system ID, specification, or drawing.  The fourth
                 data element consists of two characters and contains complementary
                 data.  These two characters provide a means of differentiating or
                 providing uniqueness between the eight character CLEI codes by
                 identifying the manufacturing vintage of the product.  Names are
                 assigned via procedures defined in [GR485].

                 The assigned maintenance agent for the CLEI code, Telcordia
                 Technologies, is responsible for assigning certain equipment and
                 other identifiers (e.g., location, manufacturer/supplier) for the
                 telecommunications industry."
        ::= { jnxContentsEntry 13 }

--
-- Box LED Indicators Table
--

    jnxLEDLastChange OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The value of sysUpTime when the box LED table 
		last changed.  Zero if unknown or already at 
		that state when the agent was up."
	::= { jnxBoxAnatomy 9 }

    jnxLEDTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JnxLEDEntry
	MAX-ACCESS	not-accessible
	STATUS		deprecated
	DESCRIPTION
		"A list of status entries."
	::= { jnxBoxAnatomy 10 }

    jnxLEDEntry OBJECT-TYPE
	SYNTAX		JnxLEDEntry
	MAX-ACCESS	not-accessible
	STATUS		deprecated
	DESCRIPTION
		"An entry of status table."
	INDEX 	{ jnxLEDAssociateTable,
		  jnxLEDAssociateIndex,
		  jnxLEDL1Index,
		  jnxLEDL2Index,
		  jnxLEDL3Index }
	::= { jnxLEDTable 1 }

    JnxLEDEntry ::= SEQUENCE {
	    jnxLEDAssociateTable	INTEGER,
	    jnxLEDAssociateIndex	Integer32,
	    jnxLEDL1Index		Integer32,
	    jnxLEDL2Index		Integer32,
	    jnxLEDL3Index		Integer32,
	    jnxLEDOriginator		OBJECT IDENTIFIER,
	    jnxLEDDescr			DisplayString,
	    jnxLEDState			INTEGER,
	    jnxLEDStateOrdered		INTEGER
    }

    jnxLEDAssociateTable OBJECT-TYPE
	SYNTAX		INTEGER {
		other(1),
		jnxContainersTable(2),
		jnxContentsTable(3)
	}
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The associated table that this entry is 
		related."
	::= { jnxLEDEntry 1 }

    jnxLEDAssociateIndex OBJECT-TYPE
	SYNTAX		Integer32 (1..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The index of the associated table that this
		entry is related."
	::= { jnxLEDEntry 2 }

    jnxLEDL1Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The level one index of the associated
		table that this entry is related.  Zero 
		if unavailable or inapplicable."
	::= { jnxLEDEntry 3 }

    jnxLEDL2Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The level two index of the associated
		table that this entry is related.  Zero 
		if unavailable or inapplicable."
	::= { jnxLEDEntry 4 }

    jnxLEDL3Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The level three index of the associated
		table that this entry is related.  Zero
		if unavailable or inapplicable."
	::= { jnxLEDEntry 5 }

    jnxLEDOriginator OBJECT-TYPE
	SYNTAX		OBJECT IDENTIFIER
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The originator of the this entry."
	::= { jnxLEDEntry 6 }

    jnxLEDDescr OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The name or detailed description of this subject."
	::= { jnxLEDEntry 7 }

    jnxLEDState OBJECT-TYPE
	SYNTAX		INTEGER {
		other(1),     -- unknown or unavailable
		green(2),     -- ok, good, normally working,
			      -- or on-line as a standby backup if
			      -- there is an active primary
		yellow(3),    -- alarm, warning, marginally working
		red(4),	      -- alert, failed, not working
		blue(5),      -- ok, on-line as an active primary
		amber(6)      -- alarm, off-line, not running
	}
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The state of the LED indicator."
	::= { jnxLEDEntry 8 }

    jnxLEDStateOrdered OBJECT-TYPE
	SYNTAX		INTEGER {
		blue(1),      -- ok, on-line as an active primary
		green(2),     -- ok, good, normally working,
			      -- or on-line as a standby backup if
			      -- there is an active primary
		amber(3),     -- alarm, off-line, not running
		yellow(4),    -- alarm, warning, marginally working
		red(5),	      -- alert, failed, not working
		other(6)      -- unknown or unavailable
	}
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The state of the LED indicator.  Identical to jnxLEDState, but
                with enums ordered from 'most operational' to 'least
                operational' states."
	::= { jnxLEDEntry 9 }
--
-- Box Filled Status Table
--
-- This table show the empty/filled status of the container in the 
-- box containers table.
--

    jnxFilledLastChange OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when the box filled 
		status table last changed.  Zero if unknown or
		already at that state when the agent was up."
	::= { jnxBoxAnatomy 11 }
	
    jnxFilledTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JnxFilledEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"A list of filled status entries."
	::= { jnxBoxAnatomy 12 }

    jnxFilledEntry OBJECT-TYPE
	SYNTAX		JnxFilledEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"An entry of filled status table."
	INDEX	{ jnxFilledContainerIndex,
		  jnxFilledL1Index,
		  jnxFilledL2Index,
		  jnxFilledL3Index }
	::= { jnxFilledTable 1 }

    JnxFilledEntry ::= SEQUENCE {
	    jnxFilledContainerIndex   	Integer32,
	    jnxFilledL1Index          	Integer32,
	    jnxFilledL2Index          	Integer32,
	    jnxFilledL3Index          	Integer32,
	    jnxFilledDescr              DisplayString,
            jnxFilledState              INTEGER,
            jnxFilledChassisId          JnxChassisId,
            jnxFilledChassisDescr       DisplayString
    }

    jnxFilledContainerIndex OBJECT-TYPE
	SYNTAX		Integer32 (1..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The associated jnxContainersIndex in the 
		jnxContainersTable."
	::= { jnxFilledEntry 1 }
	
    jnxFilledL1Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level one index of the container
		housing this subject.  Zero if unavailable
		or inapplicable."
	::= { jnxFilledEntry 2 }

    jnxFilledL2Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level two index of the container
		housing this subject.  Zero if unavailable
		or inapplicable."
	::= { jnxFilledEntry 3 }

    jnxFilledL3Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level three index of the container
		housing this subject.  Zero if unavailable
		or inapplicable."
	::= { jnxFilledEntry 4 }

    jnxFilledDescr OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The name or detailed description of this
		subject."
	::= { jnxFilledEntry 5 }

    jnxFilledState OBJECT-TYPE
	SYNTAX		INTEGER {
		unknown(1),
		empty(2),
		filled(3)
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The filled state of this subject."
	::= { jnxFilledEntry 6 }

    jnxFilledChassisId OBJECT-TYPE
        SYNTAX         JnxChassisId
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
                "Identifies the chassis on which the contents of this
                row exists."
        ::= { jnxFilledEntry 7 }

    jnxFilledChassisDescr OBJECT-TYPE
        SYNTAX         DisplayString (SIZE (0..255))
        MAX-ACCESS      read-only
        STATUS         current
        DESCRIPTION
                "A textual description of the chassis on which the
                contents of this row exists."
        ::= { jnxFilledEntry 8 }


--
-- Box Operating Status Table
--
-- This table reveals the operating status of some subjects 
-- of interest in the box contents table.
--

    jnxOperatingTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JnxOperatingEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"A list of operating status entries."
	::= { jnxBoxAnatomy 13 }

    jnxOperatingEntry OBJECT-TYPE
	SYNTAX		JnxOperatingEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"An entry of operating status table."
	INDEX	{ jnxOperatingContentsIndex,
		  jnxOperatingL1Index,
		  jnxOperatingL2Index,
		  jnxOperatingL3Index }
	::= { jnxOperatingTable 1 }

    JnxOperatingEntry ::= SEQUENCE {
	    jnxOperatingContentsIndex   Integer32,
	    jnxOperatingL1Index         Integer32,
	    jnxOperatingL2Index         Integer32,
	    jnxOperatingL3Index         Integer32,
	    jnxOperatingDescr           DisplayString,
	    jnxOperatingState	    	INTEGER,
	    jnxOperatingTemp            Gauge32,
	    jnxOperatingCPU		Gauge32,
	    jnxOperatingISR             Gauge32,
	    jnxOperatingDRAMSize        Integer32,
	    jnxOperatingBuffer          Gauge32,
	    jnxOperatingHeap            Gauge32,
	    jnxOperatingUpTime          TimeInterval,
	    jnxOperatingLastRestart     TimeStamp,
	    jnxOperatingMemory          Integer32,
            jnxOperatingStateOrdered    INTEGER,
            jnxOperatingChassisId       JnxChassisId,
            jnxOperatingChassisDescr    DisplayString,
            jnxOperatingRestartTime     DateAndTime,
            jnxOperating1MinLoadAvg     Gauge32,
            jnxOperating5MinLoadAvg     Gauge32,
            jnxOperating15MinLoadAvg     Gauge32
    }

    jnxOperatingContentsIndex OBJECT-TYPE
	SYNTAX		Integer32 (1..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The associated jnxContentsContainerIndex in the 
		jnxContentsTable."
	::= { jnxOperatingEntry 1 }
	
    jnxOperatingL1Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level one index associated with this
		subject.  Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 2 }

    jnxOperatingL2Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level two index associated with this 
		subject.  Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 3 }

    jnxOperatingL3Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level three index associated with this
		subject.  Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 4 }

    jnxOperatingDescr OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The name or detailed description of this subject."
	::= { jnxOperatingEntry 5 }

    jnxOperatingState OBJECT-TYPE
	SYNTAX		INTEGER {
		unknown(1),
		running(2),   -- up and running,
			      -- as a active primary
		ready(3),     -- ready to run, not running yet
		reset(4),     -- held in reset, not ready yet
	        runningAtFullSpeed(5),  
			      -- valid for fans only
	        down(6),      -- down or off, for power supply
		standby(7)    -- running as a standby backup
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The operating state of this subject."
	::= { jnxOperatingEntry 6 }

    jnxOperatingTemp OBJECT-TYPE
	SYNTAX		Gauge32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The temperature in Celsius (degrees C) of this 
		subject.  Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 7 }

    jnxOperatingCPU OBJECT-TYPE
	SYNTAX		Gauge32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The CPU utilization in percentage of this 
		subject.  Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 8 }
	
    jnxOperatingISR OBJECT-TYPE
	SYNTAX		Gauge32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The CPU utilization in percentage of this subject
		spending in interrupt service routine (ISR).
		Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 9 }
	
    jnxOperatingDRAMSize OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		deprecated
	DESCRIPTION
		"The DRAM size in bytes of this subject.
		Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 10 }
	
    jnxOperatingBuffer OBJECT-TYPE
	SYNTAX		Gauge32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The buffer pool utilization in percentage
		of this subject.  Zero if unavailable or 
		inapplicable."
	::= { jnxOperatingEntry 11 }
	
    jnxOperatingHeap OBJECT-TYPE
	SYNTAX		Gauge32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The heap utilization in percentage of 
		this subject.  Zero if unavailable or 
		inapplicable."
	::= { jnxOperatingEntry 12 }

    jnxOperatingUpTime OBJECT-TYPE
	SYNTAX		TimeInterval
	MAX-ACCESS	read-only
        STATUS          deprecated
	DESCRIPTION
		"The time interval in 10-millisecond period
		that this subject has been up and running.  
		Zero if unavailable or inapplicable."
	::= { jnxOperatingEntry 13 }

    jnxOperatingLastRestart OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when this subject 
		last restarted.  Zero if unavailable or 
		inapplicable."
	::= { jnxOperatingEntry 14 }

    jnxOperatingMemory OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The installed memory size in Megabytes 
		of this subject.  Zero if unavailable or
		inapplicable."
	::= { jnxOperatingEntry 15 }

    jnxOperatingStateOrdered OBJECT-TYPE
	SYNTAX		INTEGER {
		running(1),   -- up and running,
			      -- as a active primary
		standby(2),   -- running as a standby backup
		ready(3),     -- ready to run, not running yet
	        runningAtFullSpeed(4),  
			      -- valid for fans only
		reset(5),     -- held in reset, not ready yet
	        down(6),      -- down or off, for power supply
		unknown(7)
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The operating state of this subject.  Identical to
                 jnxOperatingState, but with enums ordered from 'most
                 operational' to 'least operational' states."
	::= { jnxOperatingEntry 16 }

    jnxOperatingChassisId OBJECT-TYPE
        SYNTAX         JnxChassisId
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
                "Identifies the chassis on which the contents of this
                row exists."
        ::= { jnxOperatingEntry 17 }

    jnxOperatingChassisDescr OBJECT-TYPE
        SYNTAX         DisplayString (SIZE (0..255))
        MAX-ACCESS      read-only
        STATUS         current
        DESCRIPTION
                "A textual description of the chassis on which the
                contents of this row exists."
        ::= { jnxOperatingEntry 18 }

    jnxOperatingRestartTime OBJECT-TYPE
        SYNTAX          DateAndTime
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The time at which this entity
                last restarted."
        ::= { jnxOperatingEntry 19 }

        jnxOperating1MinLoadAvg OBJECT-TYPE
            SYNTAX          Gauge32
            MAX-ACCESS      read-only
            STATUS          current
            DESCRIPTION
                    "The CPU Load Average over the last 1 minutes
                     Here it will be shown as percentage value
                     Zero if unavailable or inapplicable."
            ::= { jnxOperatingEntry 20 }

        jnxOperating5MinLoadAvg OBJECT-TYPE
            SYNTAX          Gauge32
            MAX-ACCESS      read-only
            STATUS          current
            DESCRIPTION
                    "The CPU Load Average over the last 5 minutes
                     Here it will be shown as percentage value
                     Zero if unavailable or inapplicable."
            ::= { jnxOperatingEntry 21 }

        jnxOperating15MinLoadAvg OBJECT-TYPE
            SYNTAX          Gauge32
            MAX-ACCESS      read-only
            STATUS          current
            DESCRIPTION
                    "The CPU Load Average over the last 15 minutes
                     Here it will be shown as percentage value
                     Zero if unavailable or inapplicable."
            ::= { jnxOperatingEntry 22 }

--
-- Box Redundancy Information Table
--
-- This table shows the internal configuration setting for the 
-- available redundant subsystems or components in the box.
--

    jnxRedundancyTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JnxRedundancyEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"A list of redundancy information entries."
	::= { jnxBoxAnatomy 14 }

    jnxRedundancyEntry OBJECT-TYPE
	SYNTAX		JnxRedundancyEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"An entry in the redundancy information table."
	INDEX	{ jnxRedundancyContentsIndex,
		  jnxRedundancyL1Index,
		  jnxRedundancyL2Index,
		  jnxRedundancyL3Index }
	::= { jnxRedundancyTable 1 }

    JnxRedundancyEntry ::= SEQUENCE {
	    jnxRedundancyContentsIndex       Integer32,
	    jnxRedundancyL1Index             Integer32,
	    jnxRedundancyL2Index             Integer32,
	    jnxRedundancyL3Index             Integer32,
	    jnxRedundancyDescr               DisplayString,
	    jnxRedundancyConfig	     	     INTEGER,
	    jnxRedundancyState	     	     INTEGER,
	    jnxRedundancySwitchoverCount     Counter32,
	    jnxRedundancySwitchoverTime      TimeStamp,
	    jnxRedundancySwitchoverReason    INTEGER,
	    jnxRedundancyKeepaliveHeartbeat  Integer32,
	    jnxRedundancyKeepaliveTimeout    Integer32,
	    jnxRedundancyKeepaliveElapsed    Integer32,
            jnxRedundancyKeepaliveLoss       Counter32,
            jnxRedundancyChassisId           JnxChassisId,
            jnxRedundancyChassisDescr        DisplayString
    }

    jnxRedundancyContentsIndex OBJECT-TYPE
	SYNTAX		Integer32 (1..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The associated jnxContentsContainerIndex in the 
		jnxContentsTable."
	::= { jnxRedundancyEntry 1 }
 	
    jnxRedundancyL1Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level one index associated with this
		subject.  Zero if unavailable or inapplicable."
	::= { jnxRedundancyEntry 2 }

    jnxRedundancyL2Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level two index associated with this 
		subject.  Zero if unavailable or inapplicable."
	::= { jnxRedundancyEntry 3 }

    jnxRedundancyL3Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level three index associated with this
		subject.  Zero if unavailable or inapplicable."
	::= { jnxRedundancyEntry 4 }

    jnxRedundancyDescr OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The name or detailed description of this subject."
	::= { jnxRedundancyEntry 5 }

    jnxRedundancyConfig OBJECT-TYPE
	SYNTAX		INTEGER {
		unknown(1),
		master(2),    -- election priority set as a master
		backup(3),    -- election priority set as a backup
		disabled(4),  -- election disabled
		notApplicable(5) -- any among the available can be master
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The election priority of redundancy configuration for
		this subject.  The value 'notApplicable' means no
		specific instance is configured to be master or
		backup; whichever component boots up first becomes a
		master."
	::= { jnxRedundancyEntry 6 }

    jnxRedundancyState OBJECT-TYPE
	SYNTAX		INTEGER {
		unknown(1),
		master(2),    -- master
		backup(3),    -- backup
		disabled(4)   -- disabled
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The current running state for this subject."
	::= { jnxRedundancyEntry 7 }

    jnxRedundancySwitchoverCount OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The total number of switchover as perceived by
		this subject since routing engine is up and running.
		The switchover is defined as a change in state of
		jnxRedundancyState from master to backup or vice
		versa.	Its value is reset when the routing engine
		is reset or rebooted."
	::= { jnxRedundancyEntry 8 }

    jnxRedundancySwitchoverTime OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when the jnxRedundancyState
		of this subject was last switched over from master
		to backup or vice versa.  Zero if unknown or never
		switched over since the routing engine is up and
		running."
	::= { jnxRedundancyEntry 9 }

    jnxRedundancySwitchoverReason OBJECT-TYPE
	SYNTAX		INTEGER {
		other(1),		-- others
		neverSwitched(2),	-- never switched
		userSwitched(3),	-- user-initiated switchover
		autoSwitched(4)		-- automatic switchover
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The reason of the last switchover for this subject."
	::= { jnxRedundancyEntry 10 }

    jnxRedundancyKeepaliveHeartbeat OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The period of sending keepalive messages between
		the master and backup subsystems.  It is a system-wide
		preset value in seconds used by internal mastership
		resolution.  Zero if unavailable or inapplicable."
	::= { jnxRedundancyEntry 11 }

    jnxRedundancyKeepaliveTimeout OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The timeout period in seconds, by the keepalive 
		watchdog timer, before initiating a switch over to 
		the backup subsystem.  Zero if unavailable or 
		inapplicable."
	::= { jnxRedundancyEntry 12 }

    jnxRedundancyKeepaliveElapsed OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The elapsed time in seconds by this subject since 
		receiving the last keepalive message from the other
		subsystems.  Zero if unavailable or inapplicable."
	::= { jnxRedundancyEntry 13 }

    jnxRedundancyKeepaliveLoss OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The total number of losses on keepalive messages 
		between the master and backup subsystems as perceived
		by this subject since the system is up and running.  
		Zero if unavailable or inapplicable."
	::= { jnxRedundancyEntry 14 }

    jnxRedundancyChassisId OBJECT-TYPE
        SYNTAX         JnxChassisId
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
                "Identifies the chassis on which the contents of this
                row exists."
        ::= { jnxRedundancyEntry 15 }

    jnxRedundancyChassisDescr OBJECT-TYPE
        SYNTAX         DisplayString (SIZE (0..255))
        MAX-ACCESS      read-only
        STATUS         current
        DESCRIPTION
                "A textual description of the chassis on which the
                contents of this row exists."
        ::= { jnxRedundancyEntry 16 }

	
--
-- FRU (Field Replaceable Unit) Status Table
--
-- This table shows the status of the FRUs in the chassis.
--

    jnxFruTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JnxFruEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"A list of FRU status entries."
	::= { jnxBoxAnatomy 15 }

    jnxFruEntry OBJECT-TYPE
	SYNTAX		JnxFruEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"An entry in the FRU status table."
	INDEX	{ jnxFruContentsIndex,
		  jnxFruL1Index,
		  jnxFruL2Index,
		  jnxFruL3Index }
	::= { jnxFruTable 1 }

    JnxFruEntry ::= SEQUENCE {
	    jnxFruContentsIndex       Integer32,
	    jnxFruL1Index             Integer32,
	    jnxFruL2Index             Integer32,
	    jnxFruL3Index             Integer32,
	    jnxFruName                DisplayString,
	    jnxFruType        	      INTEGER,
	    jnxFruSlot                Integer32,
	    jnxFruState	     	      INTEGER,
	    jnxFruTemp                Gauge32,
	    jnxFruOfflineReason       INTEGER,
	    jnxFruLastPowerOff        TimeStamp,
	    jnxFruLastPowerOn         TimeStamp,
            jnxFruPowerUpTime         TimeInterval,
            jnxFruChassisId           JnxChassisId,
            jnxFruChassisDescr        DisplayString,
            jnxFruPsdAssignment       Integer32
    }

    jnxFruContentsIndex OBJECT-TYPE
	SYNTAX		Integer32 (1..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The associated jnxContentsContainerIndex in the 
		jnxContentsTable."
	::= { jnxFruEntry 1 }
 	
    jnxFruL1Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level one index associated with this
		subject.  Zero if unavailable or inapplicable."
	::= { jnxFruEntry 2 }

    jnxFruL2Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level two index associated with this 
		subject.  Zero if unavailable or inapplicable."
	::= { jnxFruEntry 3 }

    jnxFruL3Index OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The level three index associated with this
		subject.  Zero if unavailable or inapplicable."
	::= { jnxFruEntry 4 }

    jnxFruName OBJECT-TYPE
	SYNTAX		DisplayString (SIZE (0..255))
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The name or detailed description of this subject."
	::= { jnxFruEntry 5 }

    jnxFruType OBJECT-TYPE
	SYNTAX		INTEGER {
		other(1),                               -- unknown or others
		clockGenerator(2),                      -- CG
		flexiblePicConcentrator(3),             -- FPC
		switchingAndForwardingModule(4),        -- SFM
		controlBoard(5),                        -- CBD, SCB
		routingEngine(6),                       -- RE
		powerEntryModule(7),                    -- PEM
		frontPanelModule(8),                    -- FPM
		switchInterfaceBoard(9),                -- SIB
		processorMezzanineBoardForSIB(10),      -- SPMB
		portInterfaceCard(11),                  -- PIC
		craftInterfacePanel(12),                -- CIP
		fan(13),                                -- fan
		lineCardChassis(14),                    -- LCC
                forwardingEngineBoard(15),              -- FEB
                protectedSystemDomain(16)               -- PSD
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The FRU type for this subject."
	::= { jnxFruEntry 6 }

    jnxFruSlot OBJECT-TYPE
	SYNTAX		Integer32 (0..'7fffffff'h)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The slot number of this subject.  This is equivalent
		to jnxFruL1Index in meaning.  Zero if unavailable or 
		inapplicable."
	::= { jnxFruEntry 7 }

    jnxFruState OBJECT-TYPE
	SYNTAX		INTEGER {
		unknown(1),
		empty(2),
		present(3),
		ready(4),
		announceOnline(5),
		online(6),
		anounceOffline(7),
		offline(8),
		diagnostic(9),
		standby(10)
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The current state for this subject."
	::= { jnxFruEntry 8 }

    jnxFruTemp OBJECT-TYPE
	SYNTAX		Gauge32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The temperature in Celsius (degrees C) of this 
		subject.  Zero if unavailable or inapplicable."
	::= { jnxFruEntry 9 }

    jnxFruOfflineReason OBJECT-TYPE
	SYNTAX		INTEGER {
		unknown(1),	                -- unknown or other
		none(2),	                -- none	
		error(3),      	                -- error 
		noPower(4),	                -- no power  
		configPowerOff(5),              -- configured to power off
		configHoldInReset(6),           -- configured to hold in reset
		cliCommand(7),                  -- offlined by cli command
		buttonPress(8),                 -- offlined by button press
		cliRestart(9),                  -- restarted by cli command
		overtempShutdown(10),           -- overtemperature shutdown
		masterClockDown(11),            -- master clock down
		singleSfmModeChange(12),        -- single SFM mode change
		packetSchedulingModeChange(13), -- packet scheduling mode change
		physicalRemoval(14),            -- physical removal
		unresponsiveRestart(15),        -- restarting unresponsive board
		sonetClockAbsent(16),           -- sonet out clock absent
                rddPowerOff(17),                -- RDD power off
                majorErrors(18),                -- major errors
                minorErrors(19),                -- minor errors
                lccHardRestart(20),             -- LCC hard restart
                lccVersionMismatch(21),         -- LCC version mismatch
                powerCycle(22),                 -- power cycle
                reconnect(23),                  -- reconnect
                overvoltage(24),                -- overvoltage
                pfeVersionMismatch(25),         -- PFE version mismatch
                febRddCfgChange(26),            -- FEB redundancy cfg changed
                fpcMisconfig(27),               -- FPC is misconfigured
                fruReconnectFail(28),           -- FRU did not reconnect
                fruFwddReset(29),               -- FWDD reset the fru
                fruFebSwitch(30),               -- FEB got switched
                fruFebOffline(31),              -- FEB was offlined
                fruInServSoftUpgradeError(32),  -- In Service Software Upgrade Error
                fruChasdPowerRatingExceed(33),  -- Chassis power rating exceeded
                fruConfigOffline(34),           -- Configured offline
                fruServiceRestartRequest(35),   -- restarting request from a service
                spuResetRequest(36),            -- SPU reset request
                spuFlowdDown(37),               -- SPU flowd down
                spuSpi4Down(38),                -- SPU SPI4 down
                spuWatchdogTimeout(39),         -- SPU Watchdog timeout
                spuCoreDump(40),                -- SPU kernel core dump
                fpgaSpi4LinkDown(41),           -- FPGA SPI4 link down
                i3Spi4LinkDown(42),             -- I3 SPI4 link down
                cppDisconnect(43),              -- CPP disconnect
                cpuNotBoot(44),                 -- CPU not boot
                spuCoreDumpComplete(45),        -- SPU kernel core dump complete
                rstOnSpcSpuFailure(46),         -- Rst on SPC SPU failure
                softRstOnSpcSpuFailure(47),     -- Soft Reset on SPC SPU failure
                hwAuthenticationFailure(48),    -- HW authentication failure
                reconnectFpcFail(49),           -- Reconnect FPC fail
                fpcAppFailed(50),               -- FPC app failed
                fpcKernelCrash(51),             -- FPC kernel crash
                spuFlowdDownNoCore(52),         -- SPU flowd down, no core dump
                spuFlowdCoreDumpIncomplete(53), -- SPU flowd crash with incomplete core dump
                spuFlowdCoreDumpComplete(54),   -- SPU flowd crash with complete core dump
                spuIdpdDownNoCore(55),          -- SPU idpd down, no core dump
                spuIdpdCoreDumpIncomplete(56),  -- SPU idpd crash with incomplete core dump
                spuIdpdCoreDumpComplete(57),    -- SPU idpd crash with complete core dump
                spuCoreDumpIncomplete(58),      -- SPU kernel crash with incomplete core dump
                spuIdpdDown(59),                -- SPU idpd down
                fruPfeReset(60),                -- PFE reset
                fruReconnectNotReady(61),       -- FPC not ready to reconnect
                fruSfLinkDown(62),              -- FE - Fabric links down
                fruFabricDown(63),              -- Fabric transitioned from up to down
                fruAntiCounterfeitRetry(64),    -- FPC offlined due to Anti Counterfeit Retry
                fruFPCChassisClusterDisable(65), -- FPC offlined due to Chassis Cluster Disable
                spuFipsError(66),                -- SPU fips error
                fruFPCFabricDownOffline(67),     -- FPC offlined due to Fabric down
                febCfgChange(68),                -- FEB config change
                routeLocalizationRoleChange(69), -- Route localization role change
                fruFpcUnsupported(70),           -- FPC unsupported
                psdVersionMismatch(71),          -- PSD version mismatch
                fruResetThresholdExceeded(72),   -- FRU Reset Threshold Exceeded
                picBounce(73),                   -- PIC Bounce
                badVoltage(74),                  -- bad voltage
                fruFPCReducedFabricBW(75),       -- FPC offlined due to Reduced Fabric Bandwidth
                fruAutoheal(76)                  -- FRU offlined due to software autoheal action
	}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The offline reason of this subject."
	::= { jnxFruEntry 10 }

    jnxFruLastPowerOff OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when this subject was last 
		powered off.  Zero if unavailable or inapplicable."
	::= { jnxFruEntry 11 }

    jnxFruLastPowerOn OBJECT-TYPE
	SYNTAX		TimeStamp
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when this subject was last 
		powered on.  Zero if unavailable or inapplicable."
	::= { jnxFruEntry 12 }

    jnxFruPowerUpTime OBJECT-TYPE
	SYNTAX		TimeInterval
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The time interval in 10-millisecond period
		that this subject has been up and running
		since the last power on time.  Zero if 
		unavailable or inapplicable."
	::= { jnxFruEntry 13 }

    jnxFruChassisId OBJECT-TYPE
        SYNTAX         JnxChassisId
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
                "Identifies the chassis on which the contents of this
                row exists."
        ::= { jnxFruEntry 14 }

    jnxFruChassisDescr OBJECT-TYPE
        SYNTAX         DisplayString (SIZE (0..255))
        MAX-ACCESS      read-only
        STATUS         current
        DESCRIPTION
                "A textual description of the chassis on which the
                contents of this row exists."
        ::= { jnxFruEntry 15 }

    jnxFruPsdAssignment OBJECT-TYPE
        SYNTAX         Integer32 (0..31)
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
                "The PSD assignment of this subject. Zero if unavailable or
                not applicable."
        ::= { jnxFruEntry 16 }

--
-- definition of Kernel Memory Used related stuff
--

    jnxBoxKernelMemoryUsedPercent OBJECT-TYPE
	SYNTAX		Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The percentage of kernel memory used
		of this subject.  0 if unavailable or
		inapplicable."
	::= { jnxBoxAnatomy 16 }

--
-- definition of system domain information
--

    jnxBoxSystemDomainType OBJECT-TYPE
	SYNTAX		INTEGER {
                     notApplicable(1),
                     rootSystemDomain(2),
                     protectedSystemDomain(3)
        }
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The system domain type of this subject, notApplicable will
		be returned if this feature is not supported."
	::= { jnxBoxAnatomy 17 }


--
-- definition of chassis related traps
--
    -- Traps for chassis alarm conditions   

    jnxPowerSupplyFailure NOTIFICATION-TYPE
	OBJECTS		{ jnxContentsContainerIndex,
			  jnxContentsL1Index,
			  jnxContentsL2Index,
			  jnxContentsL3Index,
			  jnxContentsDescr,
			  jnxOperatingState }
	STATUS		current
	DESCRIPTION
		"A jnxPowerSupplyFailure trap signifies that
		the SNMP entity, acting in an agent role, has
		detected that the specified power supply in the
		chassis has been in the failure (bad DC output) 
		condition."
	::= { jnxChassisTraps 1 }

    jnxFanFailure NOTIFICATION-TYPE
	OBJECTS		{ jnxContentsContainerIndex,
			  jnxContentsL1Index,
			  jnxContentsL2Index,
			  jnxContentsL3Index,
			  jnxContentsDescr,
			  jnxOperatingState }
	STATUS		current
	DESCRIPTION
		"A jnxFanFailure trap signifies that the SNMP
		entity, acting in an agent role, has detected
		that the specified cooling fan or impeller in 
		the chassis has been in the failure (not spinning) 
		condition."
	::= { jnxChassisTraps 2 }

    jnxOverTemperature NOTIFICATION-TYPE
	OBJECTS		{ jnxContentsContainerIndex,
			  jnxContentsL1Index,
			  jnxContentsL2Index,
			  jnxContentsL3Index,
			  jnxContentsDescr,
			  jnxOperatingTemp }
	STATUS		current
	DESCRIPTION
		"A jnxOverTemperature trap signifies that the 
		SNMP entity, acting in an agent role, has 
		detected that the specified hardware component
		in the chassis has experienced over temperature
		condition."
	::= { jnxChassisTraps 3 }

    jnxRedundancySwitchover NOTIFICATION-TYPE
	OBJECTS		{ jnxRedundancyContentsIndex,
			  jnxRedundancyL1Index,
			  jnxRedundancyL2Index,
			  jnxRedundancyL3Index,
			  jnxRedundancyDescr,
			  jnxRedundancyConfig,
			  jnxRedundancyState,
			  jnxRedundancySwitchoverCount,
			  jnxRedundancySwitchoverTime,
			  jnxRedundancySwitchoverReason }
	STATUS		current
	DESCRIPTION
		"A jnxRedundancySwitchover trap signifies that 
		the SNMP entity, acting in an agent role, has 
		detected that the specified hardware component
		in the chassis has experienced a redundancy 
		switchover event defined as a change in state
		of jnxRedundancyState from master to backup or
		vice versa."
	::= { jnxChassisTraps 4 }

    jnxFruRemoval NOTIFICATION-TYPE
	OBJECTS		{ jnxFruContentsIndex,
			  jnxFruL1Index,
			  jnxFruL2Index,
			  jnxFruL3Index,
			  jnxFruName,
			  jnxFruType,
			  jnxFruSlot }
	STATUS		current
	DESCRIPTION
		"A jnxFruRemoval trap signifies that the SNMP 
		entity, acting in an agent role, has detected 
		that the specified FRU (Field Replaceable Unit)
		has been removed from the chassis."
	::= { jnxChassisTraps 5 }

    jnxFruInsertion NOTIFICATION-TYPE
	OBJECTS		{ jnxFruContentsIndex,
			  jnxFruL1Index,
			  jnxFruL2Index,
			  jnxFruL3Index,
			  jnxFruName,
			  jnxFruType,
			  jnxFruSlot }
	STATUS		current
	DESCRIPTION
		"A jnxFruInsertion trap signifies that the SNMP 
		entity,	acting in an agent role, has detected that
		the specified FRU (Field Replaceable Unit) has been 
		inserted into the chassis."
	::= { jnxChassisTraps 6 }

    jnxFruPowerOff NOTIFICATION-TYPE
	OBJECTS		{ jnxFruContentsIndex,
			  jnxFruL1Index,
			  jnxFruL2Index,
			  jnxFruL3Index,
			  jnxFruName,
			  jnxFruType,
			  jnxFruSlot,
			  jnxFruOfflineReason,
			  jnxFruLastPowerOff,
			  jnxFruLastPowerOn }
	STATUS		current
	DESCRIPTION
		"A jnxFruPowerOff trap signifies that the SNMP 
		entity, acting in an agent role, has detected 
		that the specified FRU (Field Replaceable Unit)
		has been powered off in the chassis."
	::= { jnxChassisTraps 7 }

    jnxFruPowerOn NOTIFICATION-TYPE
	OBJECTS		{ jnxFruContentsIndex,
			  jnxFruL1Index,
			  jnxFruL2Index,
			  jnxFruL3Index,
			  jnxFruName,
			  jnxFruType,
			  jnxFruSlot,
			  jnxFruOfflineReason,
			  jnxFruLastPowerOff,
			  jnxFruLastPowerOn }
	STATUS		current
	DESCRIPTION
		"A jnxFruPowerOn trap signifies that the SNMP 
		entity,	acting in an agent role, has detected that
		the specified FRU (Field Replaceable Unit) has been 
		powered on in the chassis."
	::= { jnxChassisTraps 8 }

    jnxFruFailed NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
        STATUS          current
        DESCRIPTION
                "This indicates the specified FRU (Field Replaceable Unit)
                 has failed in the chassis. Most probably this is due toi
                 some hard error such as fru is not powering up or not
                 able to load ukernel. In these cases, fru is replaced."
        ::= { jnxChassisTraps 9 }

    jnxFruOffline NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot,
                          jnxFruOfflineReason,
                          jnxFruLastPowerOff,
                          jnxFruLastPowerOn }
        STATUS          current
        DESCRIPTION
                "A jnxFruOffline trap signifies that the SNMP
                entity, acting in an agent role, has detected
                that the specified FRU (Field Replaceable Unit)
                has gone offline in the chassis."
        ::= { jnxChassisTraps 10 }

    jnxFruOnline NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
        STATUS          current
        DESCRIPTION
                "A jnxFruOnline trap signifies that the SNMP
                entity, acting in an agent role, has detected that
                the specified FRU (Field Replaceable Unit) has
                gone online in the chassis."
        ::= { jnxChassisTraps 11 }

    jnxFruCheck NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
        STATUS          current
        DESCRIPTION
                "A jnxFruCheck trap signifies that the SNMP
                entity, acting in an agent role, has detected that
                the specified FRU (Field Replaceable Unit) has
                encountered some operational errors and gone into
                check state in the chassis."
        ::= { jnxChassisTraps 12 }   

    jnxFEBSwitchover NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
        STATUS          current
        DESCRIPTION
                "A jnxFEBSwitchover trap signifies that the SNMP
                entity, acting in an agent role, has detected that
                the specified FEB (Forwarding Engine Board) has
                switched over."
        ::= { jnxChassisTraps 13 }


    jnxHardDiskFailed NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
        STATUS          current
        DESCRIPTION
                "A jnxHardDiskFailed trap signifies that the SNMP
                entity, acting in an agent role, has detected that
                the Disk in the specified Routing Engine has
                encountered some operational errors and gone into
                failed state in the chassis."
        ::= { jnxChassisTraps 14 }

    jnxHardDiskMissing NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
        STATUS          current
        DESCRIPTION
                "A DiskMissing trap signifies that the SNMP
                entity, acting in an agent role, has detected that
                hard disk in the specified outing Engine is missing
                from boot device list."
        ::= { jnxChassisTraps 15 }

    jnxBootFromBackup NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
         STATUS         current
         DESCRIPTION
                 "A jnxBootFromBackup trap signifies that the SNMP
                 entity, acting in an agent role, has detected that
                 the specified  routing-engine/member has booted from
                 the back up root partition"
         ::= { jnxChassisTraps 16 }     


    -- Traps for chassis alarm cleared conditions

    jnxPowerSupplyOK NOTIFICATION-TYPE
	OBJECTS		{ jnxContentsContainerIndex,
			  jnxContentsL1Index,
			  jnxContentsL2Index,
			  jnxContentsL3Index,
			  jnxContentsDescr,
			  jnxOperatingState }
	STATUS		current
	DESCRIPTION
		"A jnxPowerSupplyOK trap signifies that the 
		SNMP entity, acting in an agent role, has
		detected that the specified power supply in the
		chassis has recovered from the failure (bad DC output) 
		condition."
	::= { jnxChassisOKTraps 1 }

    jnxFanOK NOTIFICATION-TYPE
	OBJECTS		{ jnxContentsContainerIndex,
			  jnxContentsL1Index,
			  jnxContentsL2Index,
			  jnxContentsL3Index,
			  jnxContentsDescr,
			  jnxOperatingState }
	STATUS		current
	DESCRIPTION
		"A jnxFanOK trap signifies that the SNMP
		entity, acting in an agent role, has detected that
		the specified cooling fan or impeller in the chassis
		has recovered from the failure (not spinning) condition."
	::= { jnxChassisOKTraps 2 }

    jnxTemperatureOK NOTIFICATION-TYPE
	OBJECTS		{ jnxContentsContainerIndex,
			  jnxContentsL1Index,
			  jnxContentsL2Index,
			  jnxContentsL3Index,
			  jnxContentsDescr,
			  jnxOperatingTemp }
	STATUS		current
	DESCRIPTION
		"A jnxTemperatureOK trap signifies that the 
		SNMP entity, acting in an agent role, has 
		detected that the specified hardware component
		in the chassis has recovered from over temperature
		condition." 
	::= { jnxChassisOKTraps 3 }

    jnxFruOK NOTIFICATION-TYPE
        OBJECTS         { jnxFruContentsIndex,
                          jnxFruL1Index,
                          jnxFruL2Index,
                          jnxFruL3Index,
                          jnxFruName,
                          jnxFruType,
                          jnxFruSlot }
        STATUS          current
        DESCRIPTION
                "A jnxFruOK trap signifies that the SNMP
                entity, acting in an agent role, has detected that
                the specified FRU (Field Replaceable Unit) has
                recovered from previous operational errors and it
                is in ok state in the chassis."
        ::= { jnxChassisOKTraps 4 }


END
