HP-ICF-BRIDGE DEFINITIONS ::= BEGIN

    IMPORTS
        OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE, Integer32
            FROM SNMPv2-SMI
        TruthValue, TimeStamp, TimeInterval
            FROM SNMPv2-TC
        MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
            FROM SNMPv2-CONF
        dot1dBasePortEntry
            FROM BRIDGE-MIB
        VlanIndex
            FROM Q-BRIDGE-MIB
        hpSwitch
            FROM HP-ICF-OID
        ConfigStatus
            FROM HP-ICF-TC
        hpSwitchStpPortEntry
            FROM CONFIG-MIB
        ifIndex
            FROM IF-MIB
        portCopyEntry
            FROM SMON-MIB;

    BridgeId ::= TEXTUAL-CONVENTION
        STATUS       current
        DESCRIPTION  "The Bridge Identifier as used in the Spanning Tree
                      Protocol to uniquely identify a bridge."
        SYNTAX OCTET STRING (SIZE (8))


    hpicfBridge MODULE-IDENTITY
        LAST-UPDATED "200609300000Z"  -- September 30, 2006
        ORGANIZATION "Hewlett-Packard Company
                      Network Infrastructure Solutions"
        CONTACT-INFO "Hewlett-Packard Company
                      8000 Foothills Blvd.
                      Roseville, CA 95747"
        DESCRIPTION  "This MIB module contains HP proprietary
                      extensions to the standard Bridge MIBs."

        REVISION     "200609300000Z"  -- September 30, 2006
        DESCRIPTION  "Added 'hpicfBridgeMirrorSessionID' MIB object."

        REVISION     "200609260000Z"  -- September 26, 2006
        DESCRIPTION  "Added 'hpicfBridgeRstpAutoEdgePort' MIB object."
       
        REVISION     "200608131738Z"  -- Aug 08, 2006
        DESCRIPTION  "Added hpicfLoopProtect MIB and 
                      updated conformance statements."  

        REVISION     "200302200000Z"  -- February 20, 2003
        DESCRIPTION
                     "Added 'mstpOperation' option to the
                     'hpicfBridgeRstpForceVersion' MIB object.
                      Added 'ieee8021s' option to the 
                      'hpicfBridgeRstpProtocolVersion' MIB object."


        REVISION     "200205231738Z"  -- May 23, 2002
        DESCRIPTION  "Added conformance information."

        REVISION     "200110032050Z"  -- October 3, 2001
        DESCRIPTION  "Modified hpicfBridgeRstp MIB to contain
                      ConfigStatus."

        REVISION     "200011030642Z"  -- November 3, 2000
        DESCRIPTION  "Initial revision."
        ::= { hpSwitch 12 }

    hpicfBridgeObjects 
        OBJECT IDENTIFIER ::= { hpicfBridge 1 }
    hpicfBridgeBase 
        OBJECT IDENTIFIER ::= { hpicfBridgeObjects 1 }
-- **********************************************************************
-- VLAN Objects
-- **********************************************************************

    hpicfBridgeMaxVlans OBJECT-TYPE
        SYNTAX      INTEGER (1..4094)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Defines the number of VLANs that the switch will
                    support for dynamic use without requiring a reboot."
        ::= { hpicfBridgeBase 1 }

    hpicfBridgeVlanEnable OBJECT-TYPE
        SYNTAX      INTEGER {
                        enable(1),
                        disable(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Administrative status of VLAN support on this
                    switch."
        ::= { hpicfBridgeBase 2 }

    hpicfBridgePrimaryVlan OBJECT-TYPE
        SYNTAX      VlanIndex
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The 802.1Q VLAN ID of the primary VLAN for this
                    switch."
        ::= { hpicfBridgeBase 3 }

    hpicfBridgeVlanConfigStatus OBJECT-TYPE
        SYNTAX      ConfigStatus
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "If one or more variables in this group has been
                    reconfigured since the last reboot in such a way
                    as to require a reboot to take effect, the value
                    of this variable will be set to 'notInService'."
        ::= { hpicfBridgeBase 4 }

-- **********************************************************************
-- GVRP Objects
-- **********************************************************************
    hpicfBridgeGvrp OBJECT IDENTIFIER ::= { hpicfBridgeObjects 2 }

    hpicfBridgeGvrpPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfBridgeGvrpPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table that contains information about the
                    GVRP port configurations on this switch."
        ::= { hpicfBridgeGvrp 1 }

    hpicfBridgeGvrpPortEntry OBJECT-TYPE
        SYNTAX      HpicfBridgeGvrpPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "GVRP information associated with a single port."
        AUGMENTS    { dot1dBasePortEntry }
        ::= { hpicfBridgeGvrpPortTable 1 }

    HpicfBridgeGvrpPortEntry ::= 
        SEQUENCE {
            hpicfBridgeGvrpRestrictedVlanReg TruthValue
        }

    hpicfBridgeGvrpRestrictedVlanReg OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Controls GVRP's ability to learn new VLANs on
                    this port.  When set to 'false', GVRP will accept
                    JOIN requests for new VLANs on this port.  When
                    set to 'true', GVRP will only process protocol
                    packets that concern themselves with known VLANs."
        ::= { hpicfBridgeGvrpPortEntry 1 }

-- **********************************************************************
-- Rapid Reconfiguration Spanning Tree Objects
-- **********************************************************************

    hpicfBridgeRstp OBJECT IDENTIFIER ::= { hpicfBridgeObjects 4 }

    hpicfBridgeRstpForceVersion OBJECT-TYPE
        SYNTAX      INTEGER {
                        stpCompatibility(0),
                        rstpOperation(2),
                        mstpOperation(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Operational mode of Spanning Tree protocol:
                     - stpCompatibility means protocol operates as STP protocol
                       on all ports.
                     - rstpOperation means protocol operates as Rapid 
                       Reconfiguration on all ports except on those ports where
                       legacy system has been detected.
                     - mstpOperation means protocol operates in native MSTP mode,
                       this option is available only if object
                       'hpicfBridgeRstpProtocolVersion' is set to 'ieee8021s'."
        ::= { hpicfBridgeRstp 1 }
        
    hpicfBridgeRstpConfigStatus OBJECT-TYPE
        SYNTAX      ConfigStatus
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The configuration status of this group of objects. If
                    one or more variables in this group were
                    reconfigured since last reboot and required reboot to
                    take effect, the value of this variable will be set to
                    notInService."
        ::= { hpicfBridgeRstp 2 }

    hpicfBridgeRstpProtocolVersion OBJECT-TYPE
        SYNTAX      INTEGER {
                        ieee8021d(0),
                        ieee8021w(2),
                        ieee8021s(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The protocol version currently running on switch
                     - ieee8021d version of STP protocol,
                     - ieee8021w Rapid Reconfiguration version of STP protocol,
                     - ieee8021s Multiple STP (MSTP) protocol"
        ::= { hpicfBridgeRstp 3 }

    hpicfBridgeRstpAdminStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                        enable(1),
                        disable(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The operational status of the spanning tree protocol"
        ::= { hpicfBridgeRstp 4 }

     hpicfBridgeRstpPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfBridgeRstpPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A table that contains port-specific information
                    for the Spanning Tree Protocol."
        ::= { hpicfBridgeRstp 5 }

    hpicfBridgeRstpPortEntry OBJECT-TYPE
        SYNTAX      HpicfBridgeRstpPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "A list of information maintained by every port
                    about the Spanning Tree Protocol state for that
                    port."
        INDEX       { hpicfBridgeRstpPortIndex }
        ::= { hpicfBridgeRstpPortTable 1 }

    HpicfBridgeRstpPortEntry ::=
        SEQUENCE {
            hpicfBridgeRstpPortIndex                    INTEGER,
            hpicfBridgeRstpAdminEdgePort                INTEGER,
            hpicfBridgeRstpOperEdgePort                 INTEGER,
            hpicfBridgeRstpAdminPointToPointMac         INTEGER,
            hpicfBridgeRstpOperPointToPointMac          TruthValue,
            hpicfBridgeRstpPortPathCost                 INTEGER,
            hpicfBridgeRstpForceBpduMigrationCheck      TruthValue,
            hpicfBridgeRstpAutoEdgePort	                TruthValue,
            hpicfBridgeRstpPortBpduFiltering            TruthValue
        }

    hpicfBridgeRstpPortIndex OBJECT-TYPE
        SYNTAX      INTEGER (1..65535)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The port number of the port for which this entry
                    contains Spanning Tree Protocol management
                    information."
        REFERENCE
             "IEEE 802.1w"
        ::= { hpicfBridgeRstpPortEntry 1 }

    hpicfBridgeRstpAdminEdgePort OBJECT-TYPE
        SYNTAX      INTEGER {
                        enable(1),
                        disable(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Indicate that port is connected to LAN segment that don't 
                     have any bridge connected to it"
        REFERENCE
             "IEEE P802.1w Clause 17.3; IEEE P802.1t Clause 18"
        ::= { hpicfBridgeRstpPortEntry 2 }

    hpicfBridgeRstpOperEdgePort OBJECT-TYPE
        SYNTAX      INTEGER {
                        enable(1),
                        disable(2)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Reflects the value of the operEdgePort parameter, as 
                     defined by the operation of the Bridge Detection state
                     machine (Clause 18 of P802.1t). The value of this parameter
                     is used by a Designated Port in order to determine how 
                     rapidly it may transition to the Forwarding Port State 
                     (see 17.23, Port Role Transitions state machine). 
                     The Bridge Detection state machine sets this parameter to 
                     the value of adminEdgePort (P802.1t 18.1.3) on 
                     initialization, and forces its value to FALSE if any BPDUs
                     are received on the Port."
        REFERENCE
             "IEEE P802.1w Clause 17.3; IEEE P802.1t Clause 18"
        ::= { hpicfBridgeRstpPortEntry 3 }

    hpicfBridgeRstpAdminPointToPointMac OBJECT-TYPE
        SYNTAX      INTEGER {
                        forceTrue(1),
                        forceFalse(2),
                        auto(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "
        forceTrue: This value indicates that the administrator requires the MAC
                   to be treated as if it is connected to a point-to-point LAN 
                   segment, regardless of any indications to the contrary that 
                   are generated by the MAC entity.
        forceFalse: This value indicates that the administrator requires the MAC
                    to be treated as if it is connected to a non-point-to-point
                    LAN segment, regardless of any indications to the contrary 
                    that are generated by the MAC entity.
        auto:   This value indicates that the administrator requires the 
                point-to-point status of the MAC to be determined in accordance
                with the specific MAC procedures defined in 6.5."
        REFERENCE
             "IEEE P802.1w; IEEE P802.1t"
        ::= { hpicfBridgeRstpPortEntry 4 }

    hpicfBridgeRstpOperPointToPointMac OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "
        true: This value indicates that the MAC is connected to a 
              point-to-point LAN segment; i.e., there is at most one other 
              system attached to the LAN segment.
        false: This value indicates that the MAC is connected to a 
               non-point-to-point LAN segment; i.e., there can be more than one
               other system attached to the LAN segment."
        REFERENCE
             "IEEE P802.1w; IEEE P802.1t"
        ::= { hpicfBridgeRstpPortEntry 5 }

    hpicfBridgeRstpPortPathCost OBJECT-TYPE
        SYNTAX      INTEGER (1..200000000)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Rapid Reconfiguration Port Path Cost - 32 bit values"
        REFERENCE
             "IEEE 802.1w"
        ::= { hpicfBridgeRstpPortEntry 6 }

    hpicfBridgeRstpForceBpduMigrationCheck OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "When operating in RST (version 2 or greater) mode
                    writing TRUE(1) to this object forces this port to 
                    transmit RST BPDUs. Any other operation on this object
                    has no effect and it always returns FALSE(2) when read."
        REFERENCE
             "IEEE P802.1w"
        ::= { hpicfBridgeRstpPortEntry 7 }

    hpicfBridgeRstpAutoEdgePort OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Represents the value of 'autoEdgePort' parameter. 
                    This parameter is optional. It is used by the Bridge 
                    Detection state machine for the automatic identification 
                    of edge ports. The default is false."
        REFERENCE
             "IEEE 802.1D-2004"
        ::= { hpicfBridgeRstpPortEntry 8 }

    hpicfBridgeRstpPortBpduFiltering OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This value indicates whether or not BPDUs need
                    to be filtered on this port. If the value is true the
                    received BPDUs will be dropped and no BPDUs will be
                    transmitted on the port. If the value is false the BPDUs
                    are being processed as usual. The default is false."
        REFERENCE
             "IEEE P802.1w"
        ::= { hpicfBridgeRstpPortEntry 9 }

-- **********************************************************************
-- Loop Protection Objects
-- **********************************************************************

-- Port Remediation Textual Convention
    LoopProtectReceiverAction::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            " This TC describes the actions a port that receives a loop
              protection protocol packet can take.
            
              The disableTx(1) enumeration indicates that the sender of
              the loop protect packet will be disabled. 

              The noDisable(2) enumeration indicates that no port is to
              be disabled." 
    SYNTAX   INTEGER  
             {
                disableTx(1),
                noDisable(2)    
             }


    hpicfBridgeLoopProtect   OBJECT IDENTIFIER ::= { hpicfBridgeObjects 5 }

    hpicfBridgeLoopProtectNotifications
                             OBJECT IDENTIFIER ::= { hpicfBridgeLoopProtect 0 }
    hpicfBridgeLoopProtectBase 
                             OBJECT IDENTIFIER ::= { hpicfBridgeLoopProtect 1 }
    hpicfBridgeLoopProtectPort 
                             OBJECT IDENTIFIER ::= { hpicfBridgeLoopProtect 2 }

    hpicfBridgeLoopProtectInterval OBJECT-TYPE
        SYNTAX      Integer32 (1..10) 
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The interval in seconds at which loop protection packets are
                     transmitted. The default value is 5 seconds."
        ::= { hpicfBridgeLoopProtectBase 1 }

    hpicfBridgeLoopProtectTrapLoopDetectEnable OBJECT-TYPE
        SYNTAX      TruthValue 
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Indicates whether notifications should be sent when a loop
                     is detected on a port.  By default this object will
                     have a value of false(2)."
        ::= { hpicfBridgeLoopProtectBase 2 }

    hpicfBridgeLoopProtectEnableTimer OBJECT-TYPE
        SYNTAX      Integer32 (0..2147483647) 
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The time in seconds to wait before reenabling a port
                     disabled by loop protection. When a port is disabled by 
                     loop protection a reenable timer for the port is initialized 
                     with the value of this period. If the period is not equal to 
                     zero the port will be reenabled after the period has 
                     elapsed. Otherwise the port will remain disabled."
        ::= { hpicfBridgeLoopProtectBase 3 }

    hpicfBridgeLoopProtectPortTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfBridgeLoopProtectPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Per-interface configuration for Loop Protection."
        ::= { hpicfBridgeLoopProtectPort 1 }

    hpicfBridgeLoopProtectPortEntry OBJECT-TYPE
        SYNTAX      HpicfBridgeLoopProtectPortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Loop Protection configuration information for
                     a single port."
        INDEX       { ifIndex }
        ::= { hpicfBridgeLoopProtectPortTable 1 }

    HpicfBridgeLoopProtectPortEntry ::=
        SEQUENCE {
            hpicfBridgeLoopProtectPortEnable          TruthValue,
            hpicfBridgeLoopProtectPortLoopDetected    TruthValue,
            hpicfBridgeLoopProtectPortLastLoopTime    TimeStamp,
            hpicfBridgeLoopProtectPortLoopCount       Counter32,    
            hpicfBridgeLoopProtectPortReceiverAction  LoopProtectReceiverAction 
        }

    hpicfBridgeLoopProtectPortEnable  OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This object indicates whether this port has
                     Loop protection enabled. The default value is FALSE"
        ::= { hpicfBridgeLoopProtectPortEntry 1 }

    hpicfBridgeLoopProtectPortLoopDetected OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This object will be set to TRUE when a loop is detected on 
                     the port. The value of this object will be reset to FALSE when 
                     the port's hpicfBridgeLoopProtectPortEnable is set to 
                     FALSE." 
        ::= { hpicfBridgeLoopProtectPortEntry 2 }
    
    hpicfBridgeLoopProtectPortLastLoopTime OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The value of sysUpTime when a loop was last detected
                     on this port. A value of 0 means that the timestamp has
                     not been set."
        ::= { hpicfBridgeLoopProtectPortEntry 3 }

    hpicfBridgeLoopProtectPortLoopCount OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "When the loop protect feature is enabled on the port this 
                     object counts the number of loops detected on the port. 
                     When the feature is disabled on the port the value of this
                     object is set to 0."
        ::= { hpicfBridgeLoopProtectPortEntry 4 } 
        
   hpicfBridgeLoopProtectPortReceiverAction OBJECT-TYPE
        SYNTAX      LoopProtectReceiverAction 
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Controls the action taken when a Loop protection packet is
                     received on this port. When set to 'disableTx' the port 
                     that transmitted the packet will be disabled. When set to 
                     'noDisable' the transmitting port will not be disabled." 
        ::= { hpicfBridgeLoopProtectPortEntry 5 } 
        
-- **********************************************************************
-- hpicfBridgeLoopProtect Notifications 
-- **********************************************************************

    hpicfBridgeLoopProtectLoopDetectedNotification NOTIFICATION-TYPE
        OBJECTS     { ifIndex,
                      hpicfBridgeLoopProtectPortLoopCount,       
                      hpicfBridgeLoopProtectPortReceiverAction}
        STATUS      current
        DESCRIPTION "A hpicfBridgeLoopProtectLoopDetectedNotification signifies
                     that a loop has been detected by the loop protection protocol.
                     Generation of this notification is controlled by 
                     hpicfBridgeLoopProtectTrapLoopDetectEnable. To prevent 
                     excessive notifications this trap is rate-limited to allow 
                     a maximum of 1 notifications every 30 seconds.
                     Notifications that are not sent due to rate-limiting are
                     dropped, and not queued up to be sent later."
        ::= { hpicfBridgeLoopProtectNotifications 1 }
                 


-- **********************************************************************
-- Local Mirror Session  Objects
-- **********************************************************************

    hpicfBridgeMirrorSession     OBJECT IDENTIFIER 
                                             ::= { hpicfBridgeObjects 6 } 
    hpicfBridgeMirrorSessionBase OBJECT IDENTIFIER 
                                             ::= { hpicfBridgeMirrorSession 1 } 
    hpicfBridgeMirrorSessionDestination OBJECT IDENTIFIER 
                                             ::= { hpicfBridgeMirrorSession 2 } 

    hpicfBridgeMirrorSessionTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfBridgeMirrorSessionEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This table contains mirror session information 
                     related to a given specified destination. A mirror 
                     session is a group of one or more portCopyEntries 
                     all having the same specified destination. A given
                     specified destination may be associated with more
                     then one mirror session."
        ::= { hpicfBridgeMirrorSessionDestination 1 }


    hpicfBridgeMirrorSessionEntry OBJECT-TYPE
        SYNTAX      HpicfBridgeMirrorSessionEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the hpicfBridgeMirrorSessionEntry contains
                     mirror session specific identification
                     information."
        AUGMENTS    { portCopyEntry }
        ::= { hpicfBridgeMirrorSessionTable 1 }


    HpicfBridgeMirrorSessionEntry ::=
        SEQUENCE {
            hpicfBridgeMirrorSessionID                Integer32
        }

    hpicfBridgeMirrorSessionID OBJECT-TYPE
        SYNTAX      Integer32 (0..2147483647)
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "This variable is valid only for mirroring
                     transfers. It allows mirroring destinations
                     to be grouped. A given hpicfBridgeMirrorSessionID
                     can only be used with 1 destination. However,
                     multiple sources may be related to the same
                     hpicfBridgeMirrorSessionID. To ensure that the
                     hpicfBridgeMirrorSessionID is properly assigned,
                     it can only be updated when the respective
                     portCopyEntry object is in the notReady state.
                     For non-mirroring transfers, the value should
                     be set to 0. "
        DEFVAL { 1 }
        ::= { hpicfBridgeMirrorSessionEntry 1 }

-- **********************************************************************
-- Conformance information
-- **********************************************************************

    hpicfBridgeConformance   OBJECT IDENTIFIER ::= { hpicfBridge 2 }
    hpicfBridgeGroups        OBJECT IDENTIFIER ::= { hpicfBridgeConformance 1 }
    hpicfBridgeCompliances   OBJECT IDENTIFIER ::= { hpicfBridgeConformance 2 }
    hpicfBridgeNotGroups     OBJECT IDENTIFIER ::= { hpicfBridgeConformance 3 }

    hpicfBridgeVlanBaseGroup OBJECT-GROUP
        OBJECTS     { hpicfBridgeMaxVlans,
                      hpicfBridgeVlanEnable,
                      hpicfBridgePrimaryVlan,
                      hpicfBridgeVlanConfigStatus }
        STATUS      current
        DESCRIPTION "Basic VLAN configuration information that is not
                    in the standard 802.1Q Bridge MIB."
        ::= { hpicfBridgeGroups 1 }

    hpicfBridgeGvrpPortGroup OBJECT-GROUP
        OBJECTS     { hpicfBridgeGvrpRestrictedVlanReg }
        STATUS      current
        DESCRIPTION "GVRP configuration information that is not (yet)
                    in the standard 802.1Q Bridge MIB.

                    Note that this information is very likely to be added
                    to a future update of the 802.1Q Bridge MIB, at which
                    time, support for objects in this group will most
                    likely be deprecated."
        ::= { hpicfBridgeGroups 2 }

    hpicfBridgeRstpBaseGroup OBJECT-GROUP
        OBJECTS     { hpicfBridgeRstpForceVersion,
                      hpicfBridgeRstpConfigStatus,
                      hpicfBridgeRstpProtocolVersion,
                      hpicfBridgeRstpAdminStatus,
                      hpicfBridgeRstpPortTable }
        STATUS      current
        DESCRIPTION "Rapid Spanning Tree Protocol (RSTP) configuration
                    information that is in neither the standard 802.1w
                    MIB, nor the standard 802.1d (STP) MIB.

                    Note that as RSTP improves compatibility, some 
                    objects in this MIB will likely be deprecated."
        ::= {hpicfBridgeGroups 3 }

    hpicfBridgeLoopProtectBaseGroup OBJECT-GROUP
        OBJECTS     { hpicfBridgeLoopProtectInterval,
                      hpicfBridgeLoopProtectEnableTimer,
                      hpicfBridgeLoopProtectTrapLoopDetectEnable, 
                      hpicfBridgeLoopProtectPortEnable,
                      hpicfBridgeLoopProtectPortLoopDetected,
                      hpicfBridgeLoopProtectPortLastLoopTime,
                      hpicfBridgeLoopProtectPortLoopCount,
                      hpicfBridgeLoopProtectPortReceiverAction  
                    }
        STATUS      current
        DESCRIPTION "A collection of objects providing basic instrumentation
                     and control of the HP Loop protection entity."

        ::= {hpicfBridgeGroups 4 }
       

-- **********************************************************************
-- Notification groups
-- **********************************************************************

       hpicfBridgeLoopProtectNotGrp NOTIFICATION-GROUP
           NOTIFICATIONS { hpicfBridgeLoopProtectLoopDetectedNotification }
           STATUS      current
           DESCRIPTION "Notifications for Loop protection."
           ::= { hpicfBridgeNotGroups 1 }
        
        
     hpicfBridgeMirrorSessionBaseGroup OBJECT-GROUP
        OBJECTS     { hpicfBridgeMirrorSessionID 
                    }
        STATUS      current
        DESCRIPTION "A collection of objects providing identification
                     of a mirroring session entity."

        ::= {hpicfBridgeGroups 5 }
       
        
-- **********************************************************************
-- Compliance statements
-- **********************************************************************

    hpicfBridgeCompliance MODULE-COMPLIANCE
        STATUS      deprecated
        DESCRIPTION "The compliance statement for HP Switches with IEEE
                    802.1Q VLAN support for bridging objects not found
                    in the standard Bridge MIBs."
        MODULE
            MANDATORY-GROUPS { hpicfBridgeVlanBaseGroup }

            GROUP       hpicfBridgeGvrpPortGroup
            DESCRIPTION "Support for this group is required for switches
                        that support GVRP until such time as support for
                        these objects is added to a standard MIB."

        ::= { hpicfBridgeCompliances 1 }

    hpicfBridgeComplianceRevTwo MODULE-COMPLIANCE
        STATUS      deprecated
        DESCRIPTION "The compliance statement for HP Switches with IEEE
                    802.1W Rapid Spanning Tree Protocol support for 
                    bridging objects not found in the standard Bridge 
                    MIBs."
        MODULE
            MANDATORY-GROUPS { hpicfBridgeVlanBaseGroup }

            GROUP       hpicfBridgeGvrpPortGroup
            DESCRIPTION "Support for this group is required for switches
                        that support GVRP until such time as support for
                        these objects is added to a standard MIB."
            GROUP       hpicfBridgeRstpBaseGroup
            DESCRIPTION "Support for this group is required for switches
                        that implement RSTP until such time as support for
                        these objects is added to a standard MIB."

        ::= { hpicfBridgeCompliances 2 }

    hpicfBridgeComplianceRevThree MODULE-COMPLIANCE
        STATUS      deprecated
        DESCRIPTION "The compliance statement for HP Switches with IEEE
                    802.1W Rapid Spanning Tree Protocol support for 
                    bridging objects not found in the standard Bridge 
                    MIBs."
        MODULE
            MANDATORY-GROUPS { hpicfBridgeVlanBaseGroup }

            GROUP       hpicfBridgeGvrpPortGroup
            DESCRIPTION "Support for this group is required for switches
                        that support GVRP until such time as support for
                        these objects is added to a standard MIB."
            GROUP       hpicfBridgeRstpBaseGroup
            DESCRIPTION "Support for this group is required for switches
                        that implement RSTP until such time as support for
                        these objects is added to a standard MIB."

        ::= { hpicfBridgeCompliances 3 }

    hpicfBridgeComplianceRevFour MODULE-COMPLIANCE
        STATUS      current
        DESCRIPTION "The compliance statement for HP Switches with IEEE
                    802.1W Rapid Spanning Tree Protocol support for 
                    bridging objects not found in the standard Bridge 
                    MIBs."
        MODULE
            MANDATORY-GROUPS { hpicfBridgeVlanBaseGroup }

            GROUP       hpicfBridgeGvrpPortGroup
            DESCRIPTION "Support for this group is required for switches
                        that support GVRP until such time as support for
                        these objects is added to a standard MIB."
            GROUP       hpicfBridgeRstpBaseGroup
            DESCRIPTION "Support for this group is required for switches
                        that implement RSTP until such time as support for
                        these objects is added to a standard MIB."
            GROUP       hpicfBridgeMirrorSessionBaseGroup
            DESCRIPTION "Support for this group is mandatory for switches
                        that implement the multi session mirroring
                        (intelligent mirroring) feature." 
        ::= { hpicfBridgeCompliances 4 }

    hpicfBridgeLoopProtectCompliance MODULE-COMPLIANCE
        STATUS      current
        DESCRIPTION "The compliance statement for HP Switches with 
                     support for hpicfBridge loop protection objects."
                      
        MODULE
            MANDATORY-GROUPS { hpicfBridgeLoopProtectBaseGroup, 
                               hpicfBridgeLoopProtectNotifications }
            GROUP       hpicfBridgeLoopProtectBaseGroup
            DESCRIPTION "Support for this group is mandatory for switches
                        that implement the loop protection feature." 

            GROUP       hpicfBridgeLoopProtectNotifications
            DESCRIPTION "Implementation of this group is mandatory
                         for switches that implement the loop protection
                         feature."
        ::= { hpicfBridgeCompliances 5 }
END
