-- *******************************************************************
-- CISCO-LWAPP-DOT11-CLIENT-CCX-TC-MIB.my
-- Sheeba Kamra  Jan 2007
--   
-- Copyright (c) 2006-2007 by Cisco Systems, Inc.
--   

-- All rights reserved.
-- *****************************************************************

CISCO-LWAPP-DOT11-CLIENT-CCX-TC-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    ciscoMgmt
        FROM CISCO-SMI;

-- ********************************************************************
-- *  MODULE IDENTITY
-- ********************************************************************

ciscoLwappDot11ClientCCXTextualConventions MODULE-IDENTITY
    LAST-UPDATED    "200703220000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            Email: cs-wnbu-snmp@cisco.com"
    DESCRIPTION
        "This module defines the textual conventions used
        throughout the Cisco enterprise MIBs designed for
        implementation on Central Controllers (CC) that
        terminate the Light Weight Access Point Protocol
        tunnel from Light-weight LWAPP Access Points, 
        specifically for the functions of the Cisco Client 
        Extensions (CCX) program.

        This MIB provides textual conventions used in the
        configuration and status information mibs
        about the CCX clients that the controller is aware of.


                 GLOSSARY

        Light Weight Access Point Protocol ( LWAPP )

        This is a generic protocol that defines the
        communication between the Access Points and the
        Central Controller.

        Mobile Node ( MN )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point. Mobile Node,
        Mobile Station(Ms) and client are used
        interchangeably.

        Cisco Client eXtentions (CCX)
        The Cisco Client Extensions (CCX) Program is a 
        program of working through silicon providers to 
        embed Cisco client technology in wireless client 
        reference designs, and to promote compliant and 
        interoperable third-party clients with Cisco's 
        infrastructure, thus further driving wireless adoption 
        in the market.  

        Extensible Authentication Protocol (EAP) 

        The Extensible Authentication Protocol (EAP) is an 
        Internet Engineering Task Force (IETF) standard that 
        provides an infrastructure for network access clients and 
        authentication servers to host plug-in modules for current
        and future authentication methods and technologies.

        Wired Equivalent Privacy (WEP) 

        A security method defined by 802.11. WEP uses a  
        symmetric key stream cipher called RC4 to encrypt the data
        packets. 



        REFERENCE

        [1] Part 11 Wireless LAN Medium Access Control ( MAC )
        and Physical Layer ( PHY ) Specifications.

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol. 

        [3] Cisco Compatible Extensions for WLAN Devices
        Version 5.0.11"
    REVISION        "200703220000Z"
    DESCRIPTION
        "Added 2 more radio types to CiscoLwappDot11ClientRadioType."
    REVISION        "200702220000Z"
    DESCRIPTION
        "Reverted some of the enum names to be in line with the CCXV5
        spec."
    REVISION        "200702190000Z"
    DESCRIPTION
        "Incorporated review comments."
    REVISION        "200701300000Z"
    DESCRIPTION
        "Initial version of this  mib module."
          ::= { ciscoMgmt 611 }



CiscoLwappDot11ClientReqStatus ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This field indicates the status of current request.The values
        used can be one of the following:

            initiate - this will be used to trigger a request to get 
            some parameters from a CCX client.

            inProgress - this indicates that the request to get the 
            details from the client is still in progress.

            success - indicates that the query was executed 
            successfully. 

            failed -  this indicates that the request to get some 
            parameters from a CCX client failed.

            requestNotProcessedByClient - indicates that the CCX client
            did not honour this request."
    SYNTAX          INTEGER  {
                        initiate(1),
                        inProgress(2),
                        success(3),
                        failure(4),
                        requestNotProcessedByClient(5)
                    }

CiscoLwappDot11ClientSSId ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This represents the Service Set Identifier assigned
        to WLAN."
    SYNTAX          OCTET STRING (SIZE (1..32))

CiscoLwappDot11ClientAuthMethod ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the authentication method used by the client.
        The possible values are:
           none - this indicates that no authentication method is
           used

           preSharedKey - this refers to the method of using pre
           shared key for authentication

           eap - this is Extensible Authentication Protocol 

           unknown - this indicates an authentication protocol other
           than the ones defined above"
    SYNTAX          INTEGER  {
                        none(0),
                        preSharedKey(1),
                        eap(2),
                        unknown(255)
                    }

CiscoLwappDot11ClientEAPMethod ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This identifies the Extensible Authentication Protocol(EAP)
        method used. The possible values are:

           leap - this is Lightweight Extensible Authentication 
           Protocol

           eapFast - this is Extensible Authentication 
           Protocol with Flexible Authentication via Secure Tunneling

           eapTls - this is Extensible Authentication
           Protocol with Transport Layer Security

           eapTtls - this is Extensible Authentication Protocol with
           Tunneled Transport Layer Security

           peap0EapMschap2 - this refers to Protected Extensible 
           Authentication Protocol Version 0 with Microsoft 
           Challenge Handshake Authentication Protocol version 2

           peap1EapGtc - this refers to Protected Extensible 
           Authentication Protocol Version 1 with Generic Token Card

           eapMd5 - this is Extensible Authentication Protocol with
           Message-Digest algorithm 5

           eapSim - this is Extensible Authentication Protocol using 
           the Global System for Mobile Communications (GSM) 
           Subscriber Identity Module (SIM)

           preSharedKey - this refers to the method of using pre
           shared key for authentication

           unknown - this indicates an EAP method other
           than the ones defined above"
    SYNTAX          INTEGER  {
                        leap(0),
                        eapFast(1),
                        eapTls(2),
                        eapTtls(3),
                        peap0EapMschap2(4),
                        peap1EapGtc(5),
                        eapMd5(6),
                        eapSim(7),
                        preSharedKey(8),
                        unknown(255)
                    }

CiscoLwappDot11ClientKeyMgmtMethod ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the key management method used by the client.
        The possible values are:

           staticWep - this is Wired Equivalent Privacy with a static
           key defined

           dynamicWep - this is Wired Equivalent Privacy with a 
           dynamic key

           wpa - this indicates wifi protected access

           wpaCckm - this is wifi protected access with 
           Cisco Centralized Key Management

           wpa2 - this indicates version 2 of wifi protected access

           wpa2Cckm - this is wifi protected access  
           version 2 with Cisco Centralized Key Management

           cckm - this indicates Cisco Centralized Key 
           Management

           unknown - this indicates a key management method other
           than the ones defined above"
    SYNTAX          INTEGER  {
                        none(0),
                        staticWep(1),
                        dynamicWep(2),
                        wpa(3),
                        wpaCckm(4),
                        wpa2(5),
                        wpa2Cckm(6),
                        cckm(7),
                        unknown(255)
                    }

CiscoLwappDot11ClientEncryptionMethod ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the encryption method used  by the client.
        The possible values are:

           none - no encryption is used

           wep40 - this is Wired Equivalent Privacy with a 40 bit 
           secret key

           wep104 - this is Wired Equivalent Privacy with a 104 bit
           secret key

           tkip - this indicates Temporal Key Integrity
           Protocol

           ckip - this is Cisco Key Integrity Protocol

           aesCcmp - this is Advanced Encryption Standard 
           - Counter Mode Cipher Block Chaining-Message Authentication 
           Code Protocol

           unknown - this indicates an encryption method other
           than the ones defined above"
    SYNTAX          INTEGER  {
                        none(0),
                        wep40(1),
                        wep104(2),
                        tkip(3),
                        ckip(4),
                        aesCcmp(5),
                        unknown(255)
                    }

CiscoLwappDot11ClientCredentialType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This indicates how the 802.11 credentials are configured for
        the client.
        The possible values are:

           localSaved - credentials are locally saved

           manuallyPrompted - client is prompted for the credentials

           hostOsLogin - this means the host operating system's login
           credentials will be used

           unknown - this indicates a credential method other
           than the ones defined above"
    SYNTAX          INTEGER  {
                        localSaved(0),
                        manuallyPrompted(1),
                        hostOsLogin(2),
                        unknown(255)
                    }

CiscoLwappDot11ClientPowerSaveMode ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the type of power save mode configured on the
        client. The possible values are:

           awake - this indicates that the client is constantly awake

           normal - this indicates normal power save mode

           maxPower - this indicates maximum power save mode

           uApsd - this indicates Unsolicited Automatic  
           Power Save Delivery

           sApsd - this indicates Solicited Automatic Power  
           Save Delivery

           unknown - this indicates a power save mode other
           than the ones defined above"
    SYNTAX          INTEGER  {
                        awake(0),
                        normal(1),
                        maxPower(2),
                        uApsd(3),
                        sApsd(4),
                        unknown(255)
                    }

CiscoLwappDot11ClientTxPowerMode ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This field identifies the transmit power mode of the
        client. The possible values are:

           fixed - this indicates that the client is operating at a
           fixed power mode

           automatic - this indicates that the client power will be
           determined automatically"
    SYNTAX          INTEGER  {
                        fixed(0),
                        automatic(1)
                    }

CiscoLwappDot11ClientRadioType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the radio type of the client. The possible values
        are:
            unused - this is currently a reserved radio type and is 
            not used

            fhss - this is Frequency-hopping spread spectrum based
            radio

            dsss - this is Direct Sequence spread spectrum based
            radio

            infraRedBaseband - this is infrared baseband based radio

            oFdm - this is orthogonal frequency division 
            multiplexing based radio

            highRateDsss - this is high rate direct sequence spread 
            spectrum based radio

            erp - this indicates effective radiated power based radio

            draft11n2point4Ghz - this indicates a 2.4 Ghz band radio
            as defined in draft 802.11n

            draft11n5Ghz - this indicates a 5 Ghz band radio
            as defined in draft 802.11n"
    SYNTAX          INTEGER  {
                        unused(0),
                        fhss(1),
                        dsss(2),
                        irBaseband(3),
                        oFdm(4),
                        highRateDsss(5),
                        erp(6),
                        draft11n2point4Ghz(7),
                        draft11n5Ghz(8)
                    }

CiscoLwappDot11ClientDataRates ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This field indicates the data rates supported by a
        client.  If a data rate is supported by a client, the 
        corresponding bit is set to 1 else it is 
        set to 0.  The different data rates (in Mhz) are 1, 2,
        5.5, 6, 9, 11, 12, 18, 24, 36, 48, 54."
    SYNTAX          BITS {
                        mhz1(0),
                        mhz2(1),
                        mhz5point5(2),
                        mhz6(3),
                        mhz9(4),
                        mhz11(5),
                        mhz12(6),
                        mhz18(7),
                        mhz24(8),
                        mhz36(9),
                        mhz48(10),
                        mhz54(11)
                    }

CLDot11ClientDiagAssocReason ::= TEXTUAL-CONVENTION
    STATUS        current
    DESCRIPTION
       "This field indicates the reason for which the client
       has to be associated to a diagnostic WLAN."
    SYNTAX         INTEGER {
                       reconnect(0),
                       unreliableLink(1),
                       dot11AuthFail(2),
                       dot11AssocFail(3),
                       rsnaFail(4),
                       dhcpFail(5),
                       dnsFail(6),
                       ipConnectivityFail(7),
                       dot1xAuthFail(8),
                       commonEapNegotiationFail(9),
                       userInitiatedReasonUnknown(10),
                       executingTest(11),
                       reserved(12)
                  }


END



