-- ArubaOS 3.2.0.0_16376
-- vim:set ts=4 sw=4:
WLSX-VOICE-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       TEXTUAL-CONVENTION,
       MODULE-IDENTITY,
       OBJECT-TYPE,
       snmpModules,
       Integer32,
       Unsigned32,
	   Counter32,
	   IpAddress,
	   NOTIFICATION-TYPE
           FROM SNMPv2-SMI

       TDomain,
       DisplayString,
       PhysAddress,
       TAddress,
       TimeInterval,
       RowStatus,
       StorageType,
       TestAndIncr,
       DateAndTime,
	   MacAddress,
	   TruthValue
           FROM SNMPv2-TC
           
       ArubaEnableValue,
	   ArubaVlanValidRange,
	   ArubaVoiceCacBit,
	   ArubaVoiceCdrDirection,
	   ArubaVoipRegState,
	   ArubaVoipProtocol,
	   ArubaCallStates
	   		FROM ARUBA-TC
	   wlanStaPhyAddress,
	   wlanAPMacAddress, 
	   wlanAPRadioNumber, 
	   wlanAPBSSID
           FROM WLSX-WLAN-MIB
       OBJECT-GROUP
           FROM SNMPv2-CONF
		wlsxEnterpriseMibModules
			FROM ARUBA-MIB;

   wlsxVoiceMIB MODULE-IDENTITY 
       LAST-UPDATED "0701102156Z"
       ORGANIZATION "Aruba Wireless Networks"
       CONTACT-INFO
            "Postal:    1322 Crossman Avenue
                        Sunnyvale, CA 94089	
            E-mail:     dl-support@arubanetworks.com
            Phone:      +1 408 227 4500"
       DESCRIPTION
           "This MIB module defines MIB objects which provide
            information about Voice call status and call detail reporting
		in the Aruba controller."
       REVISION        "0701102156Z"
       DESCRIPTION
           "The initial revision."
       ::= { wlsxEnterpriseMibModules 12 }

   wlsxVoiceStatsGroup          OBJECT IDENTIFIER ::= { wlsxVoiceMIB 1 }

   wlsxVoiceCdrInfoGroup     	OBJECT IDENTIFIER ::= { wlsxVoiceStatsGroup 1 }
   wlsxVoiceCallCtrsGroup		OBJECT IDENTIFIER ::= { wlsxVoiceStatsGroup 2 }
   wlsxVoiceClientInfoGroup     OBJECT IDENTIFIER ::= { wlsxVoiceStatsGroup 3 }
   wlsxVoiceAPBssidInfoGroup	OBJECT IDENTIFIER ::= { wlsxVoiceStatsGroup 4 }

   wlsxVoiceCdrTotal  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of CDR info in the controller.
            "
        ::= { wlsxVoiceCdrInfoGroup 1 }

   wlsxVoiceCdrTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF VoiceCdrEntry
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
	  	"
			This table lists Call Detail Record Info. 
		"
      ::= { wlsxVoiceCdrInfoGroup 2 } 
      
      
   wlsxVoiceCdrEntry OBJECT-TYPE
	  SYNTAX       VoiceCdrEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             ""
	  INDEX {voiceCdrId}
      ::= { wlsxVoiceCdrTable 1 } 
      

--- Based on voip_mgr.h:voip_sip_call_cdr_t
   VoiceCdrEntry ::=
     SEQUENCE {
	voiceCdrId				Unsigned32,
	voiceCdrIp				IpAddress,
	voiceCdrMac				MacAddress,
	voiceCdrName				DisplayString,
	voiceCdrDialNum			DisplayString,
	voiceCdrDir				ArubaVoiceCdrDirection,
	voiceCdrOrigTime			Unsigned32,
	voiceCdrSetupTime			Unsigned32,
	voiceCdrTeardownTime			Unsigned32,
	voiceCdrStatus			ArubaCallStates,
	voiceCdrReason			DisplayString,
	voiceCdrDuration			Integer32,
	voiceCdrRValue			Integer32,
	voiceCdrApSwitchDelay		Integer32,
	voiceCdrCodec			Integer32,
	voiceCdrApName			DisplayString,
	voiceCdrApMac			MacAddress,
	voiceCdrBssid			DisplayString,
	voiceCdrEssid			DisplayString,
	voiceCdrHandovers			Integer32,
	voiceCdrMOS				Integer32
    }
   	voiceCdrId OBJECT-TYPE
         SYNTAX       Unsigned32
  		 MAX-ACCESS   not-accessible		
         STATUS       current
         DESCRIPTION
            "
			Voice CDR id
            "
        ::= { wlsxVoiceCdrEntry 1 }
        
   	voiceCdrIp OBJECT-TYPE
         SYNTAX       IpAddress
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR IP
            "
        ::= { wlsxVoiceCdrEntry 2 }
        
   	voiceCdrMac OBJECT-TYPE
         SYNTAX       MacAddress
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR MAC
            "
        ::= { wlsxVoiceCdrEntry 3 }
        
   	voiceCdrName OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR Name
            "
        ::= { wlsxVoiceCdrEntry 4 }
        
   	voiceCdrDialNum OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR dialed number
            "
        ::= { wlsxVoiceCdrEntry 5 }
        
   	voiceCdrDir OBJECT-TYPE
         SYNTAX       ArubaVoiceCdrDirection
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR direction incoming or outgoing
            "
        ::= { wlsxVoiceCdrEntry 6 }
        
   	voiceCdrOrigTime OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR orig time
            "
        ::= { wlsxVoiceCdrEntry 7 }

   	voiceCdrSetupTime OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR setup time
            "
        ::= { wlsxVoiceCdrEntry 8 }

   	voiceCdrTeardownTime OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR teardown number
            "
        ::= { wlsxVoiceCdrEntry 9 }

   	voiceCdrStatus OBJECT-TYPE
         SYNTAX       ArubaCallStates
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR Status
            "
        ::= { wlsxVoiceCdrEntry 10 }

   	voiceCdrReason OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR Reason
            "
        ::= { wlsxVoiceCdrEntry 11 }

   	voiceCdrDuration OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR Duration
            "
        ::= { wlsxVoiceCdrEntry 12 }

   	voiceCdrRValue OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR R-Value
            "
        ::= { wlsxVoiceCdrEntry 13 }

   	voiceCdrApSwitchDelay OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR AP switch delay
            "
        ::= { wlsxVoiceCdrEntry 14 }

   	voiceCdrCodec OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR codec
            "
        ::= { wlsxVoiceCdrEntry 15 }

   	voiceCdrApName OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR AP Name
            "
        ::= { wlsxVoiceCdrEntry 16 }

   	voiceCdrApMac OBJECT-TYPE
         SYNTAX       MacAddress
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR AP MAC Address
            "
        ::= { wlsxVoiceCdrEntry 17 }

   	voiceCdrBssid OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR BSSID
            "
        ::= { wlsxVoiceCdrEntry 18 }

   	voiceCdrEssid OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR ESSID
            "
        ::= { wlsxVoiceCdrEntry 19 }

   	voiceCdrHandovers OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR client handovers AKA mobility rate
            "
        ::= { wlsxVoiceCdrEntry 20 }


   	voiceCdrMOS OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice CDR MOS
            "
        ::= { wlsxVoiceCdrEntry 21 }

--
-- end VoiceCdrEntry
--



--
-- begin scalar counters
--
   voiceCallCtrsTotal  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 1 }

   voiceCallCtrsSuccess  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of successful calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 2 }

   voiceCallCtrsFailed  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of failed calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 3 }

   voiceCallCtrsRejected  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of rejected calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 4 }

   voiceCallCtrsAborted  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of aborted calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 5 }

   voiceCallCtrsOrig  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of originated calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 6 }

   voiceCallCtrsRecvd  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of received calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 7 }

   voiceCallCtrsActive  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of active calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 8 }

   voiceCallCtrsNotFnd  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of not found calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 9 }

   voiceCallCtrsBusy  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of busy calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 10 }

   voiceCallCtrsSvc  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of service unavailable calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 11 }

   voiceCallCtrsReqTerm  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of request terminated calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 12 }

   voiceCallCtrsDecline  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of declined calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 13 }

   voiceCallCtrsUnauth  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of unauthorized calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 14 }

   voiceCallCtrsMisc  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total number of miscellaneous calls.
            "
        ::= { wlsxVoiceCallCtrsGroup 15 }
--
-- end scalar counters
--


--
-- begin voice client
--
   wlsxVoiceClientTotal  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of Active client sessions in the controller.
            "
        ::= { wlsxVoiceClientInfoGroup 1 }


   wlsxVoiceClientTable  OBJECT-TYPE
		SYNTAX       SEQUENCE OF VoiceClientEntry 
        MAX-ACCESS   not-accessible		
        STATUS       current 
        DESCRIPTION 
	  	"
			This table lists all voice client Info
		"
      ::= { wlsxVoiceClientInfoGroup 2 } 
      
   wlsxVoiceClientEntry OBJECT-TYPE 
	  SYNTAX       VoiceClientEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             ""
	  INDEX {wlanStaPhyAddress }
      ::= { wlsxVoiceClientTable 1 } 

      

--- Based on voip_cac.h:voip_client struct
   VoiceClientEntry ::=
	SEQUENCE {
		voiceClientIp			IpAddress,
		voiceClientProtocol			ArubaVoipProtocol,  
		voiceClientRegState			ArubaVoipRegState,
		voiceClientContactName		DisplayString,
		voiceClientServerName		DisplayString,
		voiceClientEssid			DisplayString,
		voiceClientVlanId			ArubaVlanValidRange,
		voiceClientTunnelId			Integer32
    }

   	voiceClientIp OBJECT-TYPE
         SYNTAX       IpAddress
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client IP Address 
            "
        ::= { wlsxVoiceClientEntry 1 }

   	voiceClientProtocol OBJECT-TYPE
         SYNTAX       ArubaVoipProtocol
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client protocol used
            "
        ::= { wlsxVoiceClientEntry 2 }

   	voiceClientRegState OBJECT-TYPE
         SYNTAX       ArubaVoipRegState
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client state
            "
        ::= { wlsxVoiceClientEntry 3 }

   	voiceClientContactName OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client contact name
            "
        ::= { wlsxVoiceClientEntry 4 }

   	voiceClientServerName OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client Server name
            "
        ::= { wlsxVoiceClientEntry 5 }

   	voiceClientEssid OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client ESSID
            "
        ::= { wlsxVoiceClientEntry 6 }

   	voiceClientVlanId OBJECT-TYPE
         SYNTAX       ArubaVlanValidRange
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client VLAN id 
            "
        ::= { wlsxVoiceClientEntry 7 }

   	voiceClientTunnelId OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice client tunnel ID
            "
        ::= { wlsxVoiceClientEntry 8 }

--
-- end voiceClientEntry
--

    
   wlsxVoiceAPBssidTotal  OBJECT-TYPE 
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total Number of active voip info in the controller.
            "
        ::= { wlsxVoiceAPBssidInfoGroup 1 }

   wlsxVoiceAPBssidTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF VoiceAPBssidEntry
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
	  	"
			This table lists Active Voip Info. 
		"
      ::= { wlsxVoiceAPBssidInfoGroup 2 } 

      
   wlsxVoiceAPBssidEntry OBJECT-TYPE 
	  SYNTAX       VoiceAPBssidEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             ""
	  INDEX {wlanAPMacAddress, wlanAPRadioNumber, wlanAPBSSID}
      ::= { wlsxVoiceAPBssidTable 1 } 
      

   VoiceAPBssidEntry ::=
     SEQUENCE {
	voiceAPBssidName				DisplayString,
	voiceAPBssidGroup				DisplayString,
	voiceAPBssidIp				IpAddress,
	voiceAPBssidTotCalls			Unsigned32,
	voiceAPBssidVoiceType			DisplayString,
	voiceAPBssidFlag				BITS,
	voiceAPBssidUpTime			TimeTicks,
	voiceAPBssid100Sent			Counter32,
	voiceAPBssid503Sent			Counter32,
	voiceAPBssidExtraCallDisc		Counter32,
	voiceAPBssidKickedOff			Counter32,
	voiceAPBssidTspecDenied		Counter32,
	voiceAPBssidCacFlag			ArubaVoiceCacBit,		
	voiceAPBssidTotVoiceClients   Unsigned32,
	voiceAPBssidCallsSCCP			Unsigned32,
	voiceAPBssidCallsSIP			Unsigned32,
	voiceAPBssidCallsSVP			Unsigned32,
	voiceAPBssidCallsVocera		Unsigned32,
	voiceAPBssidCallsNoe		    Unsigned32,
	voiceAPBssidEssid			DisplayString
    }
    
   	voiceAPBssidName OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Name
            "
        ::= { wlsxVoiceAPBssidEntry 1 }
        
   	voiceAPBssidGroup OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Group
            "
        ::= { wlsxVoiceAPBssidEntry 2 }
        
   	voiceAPBssidIp OBJECT-TYPE
         SYNTAX       IpAddress
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP IP addresss
            "
        ::= { wlsxVoiceAPBssidEntry 3 }

   	voiceAPBssidTotCalls OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP current calls
            "
        ::= { wlsxVoiceAPBssidEntry 4 }
        
   	voiceAPBssidVoiceType OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Type
            "
        ::= { wlsxVoiceAPBssidEntry 5 }
         
   	voiceAPBssidFlag OBJECT-TYPE
		SYNTAX 	BITS {
			apRemoteAP(0),
			apPPPOE(1),
			apWiredApEnabled(2),
			apEnet1Mode(3),
			apActiveLoadBalancing(4),
			apDisconnectExtraCalls(5),
			apBatteryBoost(6)
	    }
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP flag
            "
        ::= { wlsxVoiceAPBssidEntry 6 }
         
   	voiceAPBssidUpTime OBJECT-TYPE
         SYNTAX       TimeTicks
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP up time
            "
        ::= { wlsxVoiceAPBssidEntry 7 }
         
   	voiceAPBssid100Sent OBJECT-TYPE
         SYNTAX       Counter32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice 100 sent
            "
        ::= { wlsxVoiceAPBssidEntry 8 }
         
   	voiceAPBssid503Sent OBJECT-TYPE
         SYNTAX       Counter32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice 503 sent
            "
        ::= { wlsxVoiceAPBssidEntry 9 }
         
   	voiceAPBssidExtraCallDisc OBJECT-TYPE
         SYNTAX       Counter32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP extra call disconnect
            "
        ::= { wlsxVoiceAPBssidEntry 10 }
         
   	voiceAPBssidKickedOff OBJECT-TYPE
         SYNTAX       Counter32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP kicked off
            "
        ::= { wlsxVoiceAPBssidEntry 11 }
         
   	voiceAPBssidTspecDenied OBJECT-TYPE
         SYNTAX       Counter32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Tspec Denied
            "
        ::= { wlsxVoiceAPBssidEntry 12 }
         
   	voiceAPBssidCacFlag OBJECT-TYPE
		SYNTAX 	ArubaVoiceCacBit
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP CAC flag
            "
        ::= { wlsxVoiceAPBssidEntry 13 }

   	voiceAPBssidTotVoiceClients OBJECT-TYPE
		SYNTAX 	Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP total number of voice clients
            "
        ::= { wlsxVoiceAPBssidEntry 14 }

   	voiceAPBssidCallsSCCP OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Total SCCP calls
            "
        ::= { wlsxVoiceAPBssidEntry 15 }

   	voiceAPBssidCallsSIP OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Total SIP calls
            "
        ::= { wlsxVoiceAPBssidEntry 16 }

   	voiceAPBssidCallsSVP OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Total SVP calls
            "
        ::= { wlsxVoiceAPBssidEntry 17 }

   	voiceAPBssidCallsVocera OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Total Vocera calls
            "
        ::= { wlsxVoiceAPBssidEntry 18 }

   	voiceAPBssidCallsNoe OBJECT-TYPE
         SYNTAX       Unsigned32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP Total NOE calls
            "
        ::= { wlsxVoiceAPBssidEntry 19 }

   	voiceAPBssidEssid OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Voice AP ESSID
            "
        ::= { wlsxVoiceAPBssidEntry 20 }

--
-- end VoiceApEntry
--
        
END        
