  IANATn3270eTC-MIB DEFINITIONS ::= BEGIN

 IMPORTS
      MODULE-IDENTITY, mib-2
          FROM SNMPv2-SMI
      TEXTUAL-CONVENTION
          FROM SNMPv2-TC;

    ianaTn3270eTcMib MODULE-IDENTITY
        LAST-UPDATED "200005100000Z"  -- May 10, 2000
        ORGANIZATION "IANA"
        CONTACT-INFO
            "Internet Assigned Numbers Authority

             Postal: ICANN
                     4676 Admiralty Way, Suite 330
                     Marina del Rey, CA 90292

             Tel:    +1  310 823 9358 x20
             E-Mail: iana&iana.org"
        DESCRIPTION
            "This module defines a set of textual conventions
            for use by the TN3270E-MIB and the TN3270E-RT-MIB.

            Any additions or changes to the contents of this
            MIB module must first be discussed on the tn3270e
            working group list at: tn3270e&list.nih.gov
            and approved by one of the following TN3270E
            working group contacts:

                Ed Bailey (co-chair) - elbailey&us.ibm.com
                Michael Boe (co-chair) - mboe&cisco.com
                Ken White - kennethw&vnet.ibm.com
                Robert Moore - remoore&us.ibm.com

            The above list of contacts can be altered with
            the approval of the two co-chairs.

            The Textual Conventions defined within this MIB have
            no security issues associated with them unless
            explicitly stated in their corresponding
            DESCRIPTION clause."

     -- revision log, in reverse chronological order

        REVISION    "200005100000Z"  -- May 10, 2000
        DESCRIPTION "Fix to import mib-2 instead of experimental."

        REVISION    "199909011000Z"  -- September 1, 1999
        DESCRIPTION
            "Initial version transferred from the TN3270E
            working group to IANA."
        ::= { mib-2 61 }

  -- Textual Conventions

  IANATn3270eAddrType ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "The textual convention for defining the type of a
          client address.  The enumeration value unknown(0) is
          also used to indicate that no actual address is present."
      SYNTAX INTEGER {
                      unknown(0),
                      ipv4(1),
                      ipv6(2)
                     }

  IANATn3270eAddress ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "Denotes a client address.  The type of client address is
          determined by use of the IANATn3270eAddrType textual
convention.
          The length in octets of a IANATn3270eAddress object is:

            IANATn3270eAddrType   Address Length
            +++++++++++++++++++   ++++++++++++++
                     unknown(0)   not specified or unknown; the
                                  actual length of the
                                  IANATn3270eAddress octet string
                                  indicates if an address
                                  is present
                        ipv4(1)   4 OCTETS
                        ipv6(2)   16 OCTETS

          This textual convention is similar to the TAddress
          TC defined by RFC1903 except that it allows a
          zero-length octet string and is not a full transport
          layer address."
      SYNTAX OCTET STRING (SIZE (0..255))

  IANATn3270eClientType ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "The textual convention for defining the set of
           enumerations used by tn3270eTcpConnClientIdFormat
           in the TN3270E-MIB:

           ENUMERATION        OCTETs  DESCRIPTION

           none(1)              0     Not specified
           other(2)           1..512  Implementation specific
           ipv4(3)              6     4-octet IP Address plus
                                      2-octet TCP Port
           ipv6(4)              18    16-octet IPv6 Address
                                      plus 2-octet TCP Port
           domainName(5)      1..512  The DNS name of a
                                      client.
           truncDomainName(6) 1..512  The (truncated) DNS name
                                      of a client.
           string(7)          1..512  Unknown Utf8String
           certificate(8)     1..512  certificate
           userId(9)          1..8    Client's userid
           x509dn(10)         1..512  X.509 Distinguished Name

           Representation of a certificate(8) may be lead to
           a security exposure and is NOT RECOMMENDED without
           adequate security."
      SYNTAX INTEGER {
                      none(1),
                      other(2),
                      ipv4(3),
                      ipv6(4),
                      domainName(5),
                      truncDomainName(6),
                      string(7),
                      certificate(8),
                      userId(9),
                      x509dn(10)
                     }

  IANATn3270Functions ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "This textual convention reflects the current set of
          TN3270 and TN3270E functions that can be negotiated
          between a server and its client:

          RFC856
          transmitBinary  The sender of this command REQUESTS
                          permission to begin transmitting, or
                          confirms that it will now begin
                          transmitting characters which are to
                          be interpreted as 8 bits of binary
                          data by the receiver of the data.
          RFC860
          timingMark      The sender of this command REQUESTS
                          that the receiver of this command
                          return a WILL TIMING-MARK in the data
                          stream at the 'appropriate place'.
          RFC885
          endOfRecord     The sender of this command requests
                          permission to begin transmission of
                          the Telnet END-OF-RECORD (EOR) code
                          when transmitting data characters, or
                          the sender of this command confirms it
                          will now begin transmission of EORs
                          with transmitted data characters.
          RFC1091
          terminalType    Sender is willing to send terminal
                          type information in a subsequent
                          sub-negotiation.

          RFC1041
          tn3270Regime    Sender is willing to send list of
                          supported 3270 Regimes in a
                          subsequent sub-negotiation.
          RFC2355
          scsCtlCodes     (Printer sessions only).  Allows the
                          use of the SNA Character Stream (SCS)
                          and SCS control codes on the session.
                          SCS is used with LU type 1 SNA sessions.
          dataStreamCtl   (Printer sessions only).  Allows the use
                          of the standard 3270 data stream.  This
                          corresponds to LU type 3 SNA sessions.
          responses       Provides support for positive and
                          negative response handling.  Allows the
                          server to reflect to the client any and
                          all definite, exception, and no response
                          requests sent by the host application.
          bindImage       Allows the server to send the SNA Bind
                          image and Unbind notification to the
                          client.
          sysreq          Allows the client and server to emulate
                          some (or all, depending on the server) of
                          the functions of the SYSREQ key in an SNA
                          environment."
      SYNTAX BITS {
                   transmitBinary(0),-- rfc856
                   timemark(1),      -- rfc860
                   endOfRecord(2),   -- rfc885
                   terminalType(3),  -- rfc1091
                   tn3270Regime(4),  -- rfc1041
                   scsCtlCodes(5),   -- rfc2355
                   dataStreamCtl(6), -- rfc2355
                   responses(7),     -- rfc2355
                   bindImage(8),     -- rfc2355
                   sysreq(9)         -- rfc2355
                  }

  IANATn3270ResourceType ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "The type of resource defined by a resource pool.  Refer
          to tn3270eResPoolTable."
      SYNTAX INTEGER {
                      other(1),
                      terminal(2),
                      printer(3),
                      terminalOrPrinter(4)
                     }

  IANATn3270DeviceType ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "This textual convention defines the list of device
          types that can be set, as defined by RFC 2355."
      SYNTAX INTEGER {
                   -- terminals
                      ibm3278d2(1),    -- (24 row x 80 col display)
                      ibm3278d2E(2),   -- (24 row x 80 col display)
                      ibm3278d3(3),    -- (32 row x 80 col display)
                      ibm3278d3E(4),   -- (32 row x 80 col display)
                      ibm3278d4(5),    -- (43 row x 80 col display)
                      ibm3278d4E(6),   -- (43 row x 80 col display)
                      ibm3278d5(7),    -- (27 row x 132 col display)
                      ibm3278d5E(8),   -- (27 row x 132 col display)
                      ibmDynamic(9),   -- (no pre-defined display size)

                   -- printers
                      ibm3287d1(10),
                      unknown(100)
                     }

  IANATn3270eLogData ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
        "An octet string representing log data as pertaining to
        either a TN3270 or TN3270E Session as reported from a
        TN3270E Server. Log data is stored in an octet string
        in time order (from earliest to latest).

        Each log element has the following form:

        +------+----+---------+------------+
        !length!type!TimeStamp! data       !
        +------+----+---------+------------+

        where

        length    = one-octet length of the data portion of the
                    trace element, not including the length,
                    type, and TimeStamp fields
        type      = one-octet code point characterizing the data.
        TimeStamp = A 4-octet field representing the number of
                    TimeTicks since the TN3270E server was last
                    activated.  The server's last activation time
                    is available in the tn3270eSrvrConfLastActTime
                    object in the TN3270E MIB, which has the
                    syntax DateAndTime.
        data      = initial part of a PDU.

        length   type

          0-255  x'00' - unknown
          0      x'01' - inactivity timer expired
          0      x'02' - dynamic timer expired
          0      x'03' - actlu req
          0      x'04' - bind req
          0      x'05' - clear req
          0      x'06' - dactlu req
          0      x'07' - warm actpu req
          0      x'08' - sdt req
          0      x'09' - unbind req
          0      x'0A' - notify resp
          0      x'0B' - reply PSID neg rsp
          0      x'0C' - reply PSID pos rsp
          0      x'0D' - unbind rsp
          0      x'0E' - hierarchical reset
          0      x'0F' - client connect req
          0      x'10' - client disconnect req
          0      x'11' - timingmark received
          0      x'12' - flowControl timer expired
          0      x'13' - neg rsp to host
          0      x'14' - neg rsp from host
          0      x'15' - data contention
          0      x'16' - no buffer to send SNA data
          0      x'17' - receive response while inbound
          0      x'18' - client protocol error
          0      x'19' - badClientSequenceReceived
          1-255  x'1A' - utf8String
          2      x'1B' - hexCode, implementation dependent

          Log element entries have a minimum length of 6 octets.
          The zero-length string indicates that no log data is
          available."
      SYNTAX OCTET STRING (SIZE (0 | 6..2048))

  END
