
   SNMP-PROXY-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY,
       OBJECT-TYPE,
       snmpModules
           FROM SNMPv2-SMI

       RowStatus,
       StorageType
           FROM SNMPv2-TC

       SnmpEngineID,
       SnmpAdminString
           FROM SNMP-FRAMEWORK-MIB

       SnmpTagValue
           FROM SNMP-TARGET-MIB

       MODULE-COMPLIANCE,
       OBJECT-GROUP
           FROM SNMPv2-CONF;

   snmpProxyMIB MODULE-IDENTITY
       LAST-UPDATED "200210140000Z"
       ORGANIZATION "IETF SNMPv3 Working Group"
       CONTACT-INFO
           "WG-email:   snmpv3@lists.tislabs.com
            Subscribe:  majordomo@lists.tislabs.com
                        In message body:  subscribe snmpv3

            Co-Chair:   Russ Mundy
                        Network Associates Laboratories
            Postal:     15204 Omega Drive, Suite 300
                        Rockville, MD 20850-4601
                        USA
            EMail:      mundy@tislabs.com
            Phone:      +1 301-947-7107

            Co-Chair:   David Harrington
                        Enterasys Networks
            Postal:     35 Industrial Way
                        P. O. Box 5004
                        Rochester, New Hampshire 03866-5005
                        USA
            EMail:      dbh@enterasys.com
            Phone:      +1 603-337-2614
   
            Co-editor:  David B. Levi
                        Nortel Networks
            Postal:     3505 Kesterwood Drive
                        Knoxville, Tennessee 37918
            EMail:      dlevi@nortelnetworks.com
            Phone:      +1 865 686 0432
   
            Co-editor:  Paul Meyer
                        Secure Computing Corporation
            Postal:     2675 Long Lake Road
                        Roseville, Minnesota 55113
            EMail:      paul_meyer@securecomputing.com
            Phone:      +1 651 628 1592

            Co-editor:  Bob Stewart
                        Retired"
       DESCRIPTION
           "This MIB module defines MIB objects which provide
            mechanisms to remotely configure the parameters
            used by a proxy forwarding application.

            Copyright (C) The Internet Society (2002). This
            version of this MIB module is part of RFC 3413;
            see the RFC itself for full legal notices.
           "
       REVISION    "200210140000Z"             -- 14 October 2002
       DESCRIPTION "Clarifications, published as
                    RFC 3413."
       REVISION    "199808040000Z"             -- 4 August 1998
       DESCRIPTION "Clarifications, published as
                    RFC 2573."
       REVISION    "199707140000Z"             -- 14 July 1997
       DESCRIPTION "The initial revision, published as RFC2273."
       ::= { snmpModules 14 }

   snmpProxyObjects        OBJECT IDENTIFIER ::= { snmpProxyMIB 1 }
   snmpProxyConformance    OBJECT IDENTIFIER ::= { snmpProxyMIB 3 }

   --
   --
   -- The snmpProxyObjects group
   --
   --

   snmpProxyTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF SnmpProxyEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table of translation parameters used by proxy forwarder
            applications for forwarding SNMP messages."
       ::= { snmpProxyObjects 2 }

   snmpProxyEntry OBJECT-TYPE
       SYNTAX      SnmpProxyEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A set of translation parameters used by a proxy forwarder
            application for forwarding SNMP messages.

            Entries in the snmpProxyTable are created and deleted
            using the snmpProxyRowStatus object."
       INDEX { IMPLIED snmpProxyName }
       ::= { snmpProxyTable 1 }

   SnmpProxyEntry ::= SEQUENCE {
       snmpProxyName               SnmpAdminString,
       snmpProxyType               INTEGER,
       snmpProxyContextEngineID    SnmpEngineID,
       snmpProxyContextName        SnmpAdminString,
       snmpProxyTargetParamsIn     SnmpAdminString,
       snmpProxySingleTargetOut    SnmpAdminString,
       snmpProxyMultipleTargetOut  SnmpTagValue,
       snmpProxyStorageType        StorageType,
       snmpProxyRowStatus          RowStatus
   }

   snmpProxyName OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE(1..32))
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The locally arbitrary, but unique identifier associated
            with this snmpProxyEntry."
       ::= { snmpProxyEntry 1 }

   snmpProxyType OBJECT-TYPE
       SYNTAX      INTEGER {
                       read(1),
                       write(2),
                       trap(3),
                       inform(4)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The type of message that may be forwarded using
            the translation parameters defined by this entry."
       ::= { snmpProxyEntry 2 }

   snmpProxyContextEngineID OBJECT-TYPE
       SYNTAX      SnmpEngineID
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The contextEngineID contained in messages that
            may be forwarded using the translation parameters
            defined by this entry."
       ::= { snmpProxyEntry 3 }

   snmpProxyContextName OBJECT-TYPE
       SYNTAX      SnmpAdminString
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The contextName contained in messages that may be
            forwarded using the translation parameters defined
            by this entry.

            This object is optional, and if not supported, the
            contextName contained in a message is ignored when
            selecting an entry in the snmpProxyTable."
       ::= { snmpProxyEntry 4 }

   snmpProxyTargetParamsIn OBJECT-TYPE
       SYNTAX      SnmpAdminString
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object selects an entry in the snmpTargetParamsTable.
            The selected entry is used to determine which row of the
            snmpProxyTable to use for forwarding received messages."
       ::= { snmpProxyEntry 5 }

   snmpProxySingleTargetOut OBJECT-TYPE
       SYNTAX      SnmpAdminString
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object selects a management target defined in the
            snmpTargetAddrTable (in the SNMP-TARGET-MIB).  The
            selected target is defined by an entry in the
            snmpTargetAddrTable whose index value (snmpTargetAddrName)
            is equal to this object.

            This object is only used when selection of a single
            target is required (i.e. when forwarding an incoming
            read or write request)."
       ::= { snmpProxyEntry 6 }

   snmpProxyMultipleTargetOut OBJECT-TYPE
       SYNTAX      SnmpTagValue
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object selects a set of management targets defined
            in the snmpTargetAddrTable (in the SNMP-TARGET-MIB).

            This object is only used when selection of multiple
            targets is required (i.e. when forwarding an incoming
            notification)."
       ::= { snmpProxyEntry 7 }

   snmpProxyStorageType OBJECT-TYPE
       SYNTAX      StorageType
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The storage type of this conceptual row.
            Conceptual rows having the value 'permanent' need not
            allow write-access to any columnar objects in the row."
       DEFVAL { nonVolatile }
       ::= { snmpProxyEntry 8 }

   snmpProxyRowStatus OBJECT-TYPE
       SYNTAX      RowStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The status of this conceptual row.

            To create a row in this table, a manager must
            set this object to either createAndGo(4) or
            createAndWait(5).

            The following objects may not be modified while the
            value of this object is active(1):
                - snmpProxyType
                - snmpProxyContextEngineID
                - snmpProxyContextName
                - snmpProxyTargetParamsIn
                - snmpProxySingleTargetOut
                - snmpProxyMultipleTargetOut"
       ::= { snmpProxyEntry 9 }

   --
   --
   -- Conformance information
   --
   --

   snmpProxyCompliances OBJECT IDENTIFIER ::=
                                            { snmpProxyConformance 1 }
   snmpProxyGroups      OBJECT IDENTIFIER ::=
                                            { snmpProxyConformance 2 }

   --
   --
   -- Compliance statements
   --
   --

   snmpProxyCompliance MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for SNMP entities which include
            a proxy forwarding application."
       MODULE SNMP-TARGET-MIB
           MANDATORY-GROUPS { snmpTargetBasicGroup,
                              snmpTargetResponseGroup }
       MODULE -- This Module
           MANDATORY-GROUPS { snmpProxyGroup }
       ::= { snmpProxyCompliances 1 }

   snmpProxyGroup OBJECT-GROUP
       OBJECTS {
           snmpProxyType,
           snmpProxyContextEngineID,
           snmpProxyContextName,
           snmpProxyTargetParamsIn,
           snmpProxySingleTargetOut,
           snmpProxyMultipleTargetOut,
           snmpProxyStorageType,
           snmpProxyRowStatus
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing remote configuration of
            management target translation parameters for use by
            proxy forwarder applications."
       ::= { snmpProxyGroups 3 }

   END
