-- *******************************************************************
-- Juniper Networks IPSEC Generic Flow Monitoring object mibs 
--
-- Copyright (c) 2001-2007, Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
-- *******************************************************************

JUNIPER-IPSEC-FLOW-MON-MIB DEFINITIONS ::= BEGIN

    IMPORTS
         MODULE-IDENTITY, OBJECT-TYPE, Counter32, 
		 Counter64, Integer32, Unsigned32 
           FROM SNMPv2-SMI
         InetAddress, InetAddressType
           FROM INET-ADDRESS-MIB
        TEXTUAL-CONVENTION, DisplayString, TimeInterval
           FROM SNMPv2-TC
        jnxIpSecMibRoot  
           FROM JUNIPER-SMI;


    jnxIpSecFlowMonMIB  MODULE-IDENTITY
        LAST-UPDATED "200705112153Z"     -- May 16, 2007 
        ORGANIZATION "Juniper Networks, Inc."
        CONTACT-INFO
                     "Juniper Technical Assistance Center
                      Juniper Networks, Inc.
                      1194 N. Mathilda Avenue
                      Sunnyvale, CA 94089
                      E-mail: support@juniper.net"
        DESCRIPTION
            "This module defines the object used to monitor the
	         entries pertaining to IPSec objects and the management
	         of the IPSEC VPN functionalities.  
             tables:
                   - IKE tunnel table
                   - IPSec tunnel table
                   - IPSec security associations table.

	         This mib module is based on JNX-IPSEC-MONITOR-MIB. 
	         Building on the existing IKE infrastruature, the  
	         security IKE implementation integrates the value-added 
	         features for the security products"
        REVISION    "200705160000Z" -- May 16, 2007
        DESCRIPTION 
            "Revised the MIB to exlude platform/product specific attributes"
        ::= { jnxIpSecMibRoot 1 } 


    --
    -- Branch tree objects
    -- 
    jnxIpSecFlowMonNotifications OBJECT IDENTIFIER ::= { jnxIpSecFlowMonMIB 0 }
    jnxIpSecFlowMonPhaseOne      OBJECT IDENTIFIER ::= { jnxIpSecFlowMonMIB 1 }
    jnxIpSecFlowMonPhaseTwo      OBJECT IDENTIFIER ::= { jnxIpSecFlowMonMIB 2 }

   
    -- +++++++++++++++++++++++++++++++++++++++++++++++++++
    -- Local Textual Conventions
    -- +++++++++++++++++++++++++++++++++++++++++++++++++++

    JnxIkePeerType ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of IPsec Phase-1 IKE peer identity.  It is the 
             local IKE identify to send in the exchange. 
             The IKE peer may be identified by one of the ID types 
	         defined in IPSEC DOI.
                 idIpv4Addr - IPv4 Address.   
                 idUfqdn    - user fully qualified domain name (user@hostname).  
                 idFqdn     - full qualified domain name 
                 idDn       - distinquished name"
         SYNTAX INTEGER {
                   unknown              (0),    
                   idIpv4Addr           (1),   
                   idFqdn               (2),  
                   idDn                 (3),
                   idUfqdn              (4)  
         }

    JnxIkeNegoMode ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The IPsec Phase-1 IKE negotiation mode.
             Main Mode: A six-message Phase 1 exchange that provides identity
                        protection.
             Aggressive mode: a three-message phase 1 exchange that does 
             not provide identity protection"
         SYNTAX INTEGER {
                   main         (1),
                   aggressive   (2)
         }

    JnxIkeHashAlgo ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The hash algorithm used in IPsec Phase-1 IKE negotiations."
         SYNTAX INTEGER {
                   md5(1),
                   sha(2),
                   sha256(3)
         }

    JnxIkeAuthMethod ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The authentication method used in IPsec Phase-1 IKE
             negotiations."
         SYNTAX INTEGER {
                   preSharedKey           (1),
                   dssSignature           (2),
                   rsaSignature           (3),
                   rsaEncryption          (4),   
                   revRsaEncryption       (5),   
                   xauthPreSharedKey      (6),
                   xauthDssSignature      (7),
                   xauthRsaSignature      (8),
                   xauthRsaEncryption     (9),
                   xauthRevRsaEncryption  (10)
         }

    JnxIkePeerRole ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "Role of the local endpoint in negotiating the IPsec Phase-1 IKE
             security association. It can be either Initiator or Responder."
         SYNTAX INTEGER {
                   initiator            (1),
                   responder            (2)
         }

    JnxIkeTunStateType ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "State of the Phase-1 IKE negotiation."
         SYNTAX INTEGER {
                   up     (1),
                   down   (2)
         }


    JnxDiffHellmanGrp ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The Diffie Hellman Group used in negotiations.
                   modp768        -- 768-bit MODP
                   modp1024       -- 1024-bit MODP
                   modp1536       -- 1536-bit MODP; voyager only
            "
         SYNTAX INTEGER {
                   unknown	(0),
                   modp768	(1),
                   modp1024	(2),
                   modp1536     (5)
         }

    JnxKeyType    ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of key used by an IPsec Phase-2 Tunnel."
         SYNTAX INTEGER{
                  unknown               (0),
                  keyIke                (1),
                  keyManual             (2)
         }

    JnxEncapMode  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The encapsulation mode used by an IPsec Phase-2 Tunnel."
         SYNTAX INTEGER{
                  unknown               (0),
                  tunnel                (1),  
                  transport             (2)
         }

    JnxEncryptAlgo   ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The encryption algorithm used in negotiations."
         SYNTAX INTEGER {
                   espDes               (1),
                   esp3des              (2),
                   espNull              (3),
                   espAes128            (4),  
                   espAes192            (5),
                   espAes256            (6)
         }

    JnxAuthAlgo      ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The authentication algorithm used by a
             security association of an IPsec Phase-2 Tunnel."
         SYNTAX INTEGER{
                   unknown            (0),
                   hmacMd5            (1),
                   hmacSha            (2),
                   hmacSha256         (3)

         }

    JnxRemotePeerType  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of the remote peer gateway (endpoint). It can be one
             of the following two types:
               - static (Remote peer whose IP address is known beforehand)
               - dynamic (Remote peer whose IP address is not known
                 beforehand).
             "
         SYNTAX INTEGER {
                   unknown              (0),
                   static               (1),
                   dynamic              (2)
         }

    JnxSpiType  ::= TEXTUAL-CONVENTION
         STATUS     current
         DESCRIPTION
            "The type of the SPI associated with IPsec Phase-2 security
             associations."
         SYNTAX Unsigned32 (256..4294967295)


    JnxSAType   ::= TEXTUAL-CONVENTION
        STATUS     current
        DESCRIPTION
            "SA Type manual or dynamic"
        SYNTAX INTEGER {
                   unknown   (0),
                   manual    (1),
                   dynamic   (2)
        }


    -- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
	-- Number of IKE Tunnels currently active  
    -- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

    jnxIkeNumOfTunnels OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Number of IKE Tunnels (phase-1) actively negotiating between
             peers.  The SA can be in either the up or down state.  
             This attribute should detail the number of IKE tunnels 
             in jnxIkeTunnelMonTable."
        ::= {  jnxIpSecFlowMonPhaseOne 1 }


   -- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- The IPsec Phase-1 Internet Key Exchange Tunnel Table
   --
   -- Phase 1 is used to negotiate the parameter and key material required 
   -- to establish an ISAKMP AS. 
   -- 
   -- The phase 1 IKE gateway key exchange: tunnel peer device.  Phase 1 
   -- security association components include encryption algorithm, 
   -- authentication, Diffie-Hellman group values and anthentication method
   -- such as pre-shared keys or certificates.
   -- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

    jnxIkeTunnelMonTable  OBJECT-TYPE
         SYNTAX SEQUENCE OF JnxIkeTunnelMonEntry
         MAX-ACCESS 	    not-accessible
         STATUS 	    current
         DESCRIPTION
            "The IPsec Phase-1 Internet Key Exchange Tunnel Table.
             There is one entry in this table for each active IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIpSecFlowMonPhaseOne 2 }

    jnxIkeTunnelMonEntry OBJECT-TYPE
         SYNTAX     JnxIkeTunnelMonEntry
         MAX-ACCESS not-accessible
         STATUS     current
         DESCRIPTION
             "Each entry contains the attributes associated with
              an active IPsec Phase-1 IKE Tunnel."
         INDEX { jnxIkeTunMonRemoteGwAddrType,
                 jnxIkeTunMonRemoteGwAddr,
                 jnxIkeTunMonIndex }
         ::= { jnxIkeTunnelMonTable 1 }

    JnxIkeTunnelMonEntry ::= SEQUENCE {
         jnxIkeTunMonRemoteGwAddrType      InetAddressType,
         jnxIkeTunMonRemoteGwAddr          InetAddress,
         jnxIkeTunMonIndex                 Integer32,
         jnxIkeTunMonLocalGwAddrType       InetAddressType,
         jnxIkeTunMonLocalGwAddr           InetAddress,
         jnxIkeTunMonState                 JnxIkeTunStateType,   
         jnxIkeTunMonInitiatorCookie       DisplayString,
         jnxIkeTunMonResponderCookie       DisplayString,
         jnxIkeTunMonLocalRole             JnxIkePeerRole,  
         jnxIkeTunMonLocalIdType           JnxIkePeerType,
         jnxIkeTunMonLocalIdValue          DisplayString,
         jnxIkeTunMonLocalCertName         DisplayString,
         jnxIkeTunMonRemoteIdType          JnxIkePeerType,
         jnxIkeTunMonRemoteIdValue         DisplayString,
         jnxIkeTunMonNegoMode              JnxIkeNegoMode,
         jnxIkeTunMonDiffHellmanGrp        JnxDiffHellmanGrp,
         jnxIkeTunMonEncryptAlgo           JnxEncryptAlgo,
         jnxIkeTunMonHashAlgo              JnxIkeHashAlgo,
         jnxIkeTunMonAuthMethod            JnxIkeAuthMethod,
         jnxIkeTunMonLifeTime              Integer32,
         jnxIkeTunMonActiveTime            TimeInterval,
         jnxIkeTunMonInOctets              Counter64,
         jnxIkeTunMonInPkts                Counter32,
         jnxIkeTunMonOutOctets             Counter64,
         jnxIkeTunMonOutPkts               Counter32,
         jnxIkeTunMonXAuthUserId           DisplayString, 
         jnxIkeTunMonDPDDownCount          Counter32	
      }


      jnxIkeTunMonRemoteGwAddrType OBJECT-TYPE
         SYNTAX 	InetAddressType
         MAX-ACCESS     not-accessible
         STATUS 	current
         DESCRIPTION
            "The IP address type of the remote gateway (endpoint) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelMonEntry 1 }

      jnxIkeTunMonRemoteGwAddr OBJECT-TYPE
         SYNTAX 	InetAddress
         MAX-ACCESS     not-accessible
         STATUS 	current
         DESCRIPTION
            "The IP address of the remote gateway (endpoint) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelMonEntry 2 }

      jnxIkeTunMonIndex OBJECT-TYPE
         SYNTAX 	Integer32 (1..2147483647)
         MAX-ACCESS     not-accessible
         STATUS 	current
         DESCRIPTION
            "The index of the IPsec Phase-1 IKE Tunnel Table.
             The value of the index is a number which begins
             at one and is incremented with each tunnel that
             is created. The value of this object will
             wrap at 2,147,483,647."
         ::= { jnxIkeTunnelMonEntry 3 }

      jnxIkeTunMonLocalGwAddr OBJECT-TYPE
         SYNTAX         InetAddress
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The IP address of the local endpoint (gateway) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelMonEntry 4 }

      jnxIkeTunMonLocalGwAddrType OBJECT-TYPE
         SYNTAX 	InetAddressType
         MAX-ACCESS     read-only
         STATUS 	current
         DESCRIPTION
            "The IP address type of the local endpoint (gateway) for the IPsec
             Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelMonEntry 5 }

      jnxIkeTunMonState OBJECT-TYPE
         SYNTAX 	JnxIkeTunStateType
         MAX-ACCESS     read-only 
         STATUS 	current 
         DESCRIPTION
            "The state of the IKE tunnel, It can be: 
			1. up - negotiation completed
			2. down- being negotiated"
         ::= { jnxIkeTunnelMonEntry 6 }
		 
      jnxIkeTunMonInitiatorCookie OBJECT-TYPE
         SYNTAX 	DisplayString
         MAX-ACCESS     read-only 
         STATUS 	current 
         DESCRIPTION
            "Cookie as generated by the peer that initiated the IKE Phase-1
             negotiation. This cookie is carried in the ISAKMP header."
         ::= { jnxIkeTunnelMonEntry 7 }

      jnxIkeTunMonResponderCookie OBJECT-TYPE
         SYNTAX 	DisplayString
         MAX-ACCESS     read-only 
         STATUS		current 
         DESCRIPTION
            "Cookie as generated by the peer responding to the IKE Phase-1
             negotiation initiated by the remote peer. This cookie is carried
             in the ISAKMP header."
         ::= { jnxIkeTunnelMonEntry 8 }
		 
      jnxIkeTunMonLocalRole OBJECT-TYPE
         SYNTAX 	JnxIkePeerRole
         MAX-ACCESS     read-only 
         STATUS 	current 
         DESCRIPTION
            "The role of local peer identity.  The Role of the local peer can be:
             1. initiator.
             2. or responder."
         ::= { jnxIkeTunnelMonEntry 9 }

      jnxIkeTunMonLocalIdType OBJECT-TYPE
         SYNTAX 	JnxIkePeerType
         MAX-ACCESS     read-only
         STATUS 	current
         DESCRIPTION
            "The type of local peer identity.  The local
            peer may be identified by:
             1. an IP address, or
             2. or a fully qualified domain name string.
             3. or a distinguished name string."
         ::= { jnxIkeTunnelMonEntry 10 }

      jnxIkeTunMonLocalIdValue OBJECT-TYPE
         SYNTAX 	DisplayString
         MAX-ACCESS     read-only
         STATUS 	current
         DESCRIPTION
            "The value of the local peer identity.

             If the local peer type is an IP Address, then this
             is the IP Address used to identify the local peer.

             If the local peer type is id_fqdn, then this is
             the FQDN of the remote peer.

             If the local peer type is a id_dn, then this is
             the distinguished name string of the local peer."
         ::= { jnxIkeTunnelMonEntry 11 }

      jnxIkeTunMonLocalCertName OBJECT-TYPE
         SYNTAX         DisplayString
         MAX-ACCESS     read-only
         STATUS current
         DESCRIPTION
            "Name of the certificate used for authentication of the local
             tunnel endpoint. This object will have some valid value only
             if negotiated IKE authentication method is other than pre-saherd
             key. If the IKE negotiation do not use certificate based
             authentication method, then the value of this object will be a
             NULL string."  
         ::= { jnxIkeTunnelMonEntry 12 }

      jnxIkeTunMonRemoteIdType OBJECT-TYPE
         SYNTAX         JnxIkePeerType
         MAX-ACCESS     read-only
         STATUS current
         DESCRIPTION
            "The type of remote peer identity.
            The remote peer may be identified by:
             1. an IP address, or
             2. or a fully qualified domain name string.
             3. or a distinguished name string."
         ::= { jnxIkeTunnelMonEntry 13 }

      jnxIkeTunMonRemoteIdValue OBJECT-TYPE
         SYNTAX 	DisplayString
         MAX-ACCESS     read-only
         STATUS 	current
         DESCRIPTION
            "The value of the remote peer identity.

             If the remote peer type is an IP Address, then this
             is the IP Address used to identify the remote peer.

             If the remote peer type is id_fqdn, then this is
             the FQDN of the remote peer.

             If the remote peer type is a id_dn, then this is
             the distinguished named string of the remote peer."
         ::= { jnxIkeTunnelMonEntry 14 }

      jnxIkeTunMonNegoMode OBJECT-TYPE
         SYNTAX 	JnxIkeNegoMode
         MAX-ACCESS     read-only
         STATUS 	current
         DESCRIPTION
            "The negotiation mode of the IPsec Phase-1 IKE Tunnel."
         ::= { jnxIkeTunnelMonEntry 15 }

      jnxIkeTunMonDiffHellmanGrp OBJECT-TYPE
         SYNTAX 	JnxDiffHellmanGrp
         MAX-ACCESS     read-only
         STATUS 	current
         DESCRIPTION
            "The Diffie Hellman Group used in IPsec Phase-1 IKE
             negotiations."
         ::= { jnxIkeTunnelMonEntry 16 }

      jnxIkeTunMonEncryptAlgo OBJECT-TYPE
         SYNTAX 	JnxEncryptAlgo
         MAX-ACCESS     read-only
         STATUS 	current
         DESCRIPTION
            "The encryption algorithm used in IPsec Phase-1 IKE negotiations."
         ::= { jnxIkeTunnelMonEntry 17 }

      jnxIkeTunMonHashAlgo OBJECT-TYPE
         SYNTAX         JnxIkeHashAlgo
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The hash algorithm used in IPsec Phase-1 IKE negotiations."
         ::= { jnxIkeTunnelMonEntry 18 }

      jnxIkeTunMonAuthMethod OBJECT-TYPE
         SYNTAX         JnxIkeAuthMethod
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The authentication method used in IPsec Phase-1 IKE
             negotiations."
         ::= { jnxIkeTunnelMonEntry 19 }

      jnxIkeTunMonLifeTime OBJECT-TYPE
         SYNTAX         Integer32 (1..2147483647)
         UNITS          "seconds"
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The negotiated LifeTime of the IPsec Phase-1 IKE Tunnel
             in seconds."
         ::= { jnxIkeTunnelMonEntry 20 }

      jnxIkeTunMonActiveTime OBJECT-TYPE
         SYNTAX         TimeInterval
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The length of time the IPsec Phase-1 IKE tunnel has been
             active in hundredths of seconds."
         ::= { jnxIkeTunnelMonEntry 21 }

      jnxIkeTunMonInOctets OBJECT-TYPE
         SYNTAX         Counter64
         UNITS          "Octets"
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The total number of octets received by this IPsec Phase-1 
			 IKE security association."
         ::= { jnxIkeTunnelMonEntry 22 }

      jnxIkeTunMonInPkts OBJECT-TYPE
         SYNTAX         Counter32
         UNITS          "Packets"
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The total number of packets received by this IPsec Phase-1 
			 IKE security association."
         ::= { jnxIkeTunnelMonEntry 23 }

      jnxIkeTunMonOutOctets OBJECT-TYPE
         SYNTAX 	Counter64
         UNITS          "Octets"
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
            "The total number of octets sent by this IPsec Phase-1
             IKE security association."
         ::= { jnxIkeTunnelMonEntry 24 }

      jnxIkeTunMonOutPkts OBJECT-TYPE
         SYNTAX     Counter32
         UNITS      "Packets"
         MAX-ACCESS read-only
         STATUS     current
         DESCRIPTION
            "The total number of packets sent by this IPsec Phase-1
             IKE security association."
         ::= { jnxIkeTunnelMonEntry 25 }

      jnxIkeTunMonXAuthUserId OBJECT-TYPE
         SYNTAX         DisplayString 
         MAX-ACCESS 	read-only
         STATUS         current
         DESCRIPTION
            "The extended Authentication (XAuth) User Identifier, identifies the 
             user associated with this IPSec Phase negotiation." 
         ::= { jnxIkeTunnelMonEntry 26 }

      jnxIkeTunMonDPDDownCount OBJECT-TYPE
         SYNTAX         Counter32
         UNITS          "Packets"
         MAX-ACCESS     read-only
         STATUS         obsolete 
         DESCRIPTION
            "The number of times that the remote peer is detected 
             in a dead (or down) state. This attribute is obsolete"   
         ::= { jnxIkeTunnelMonEntry 27 }



   -- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- The IPsec Phase-2 Tunnel Table
   -- 
   -- During this phase, IKE negotiates IPSEC SA parameters and setup 
   -- matching IPSEC SA in the peers.
   -- 
   -- Phase 2 VPN: tunnel peer connection, associated with a specific policy
   -- or a tunnel interface.  Phase 2 security association components include
   -- encryption and authentication algorithms, proxy-IDs and optional DH 
   -- group values.
   -- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

    jnxIpSecNumOfTunnels  OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Number of IPSEC VPN Tunnels.   
             This attribute should detail the number of IPSEC VPN tunnel
             in jnxIpSecTunnelTable."
        ::= {  jnxIpSecFlowMonPhaseTwo 1 }


     jnxIpSecTunnelMonTable OBJECT-TYPE
         SYNTAX SEQUENCE OF JnxIpSecTunnelMonEntry
         MAX-ACCESS         not-accessible
         STATUS             current
         DESCRIPTION
            "The IPsec Phase-2 Tunnel Table.
            There is one entry in this table for each active IPsec Phase-2 
            Tunnel.  If the tunnel is terminated, then the entry is no longer 
            available after the table has been refreshed. "
         ::= { jnxIpSecFlowMonPhaseTwo 2 }

     jnxIpSecTunnelMonEntry OBJECT-TYPE
         SYNTAX     JnxIpSecTunnelMonEntry
         MAX-ACCESS not-accessible
         STATUS     current
         DESCRIPTION
            "Each entry contains the attributes
            associated with an active IPsec Phase-2 Tunnel."
         INDEX { jnxIpSecTunMonRemoteGwAddrType,
		 jnxIpSecTunMonRemoteGwAddr,
                 jnxIpSecTunMonIndex}
         ::= { jnxIpSecTunnelMonTable 1 }

      JnxIpSecTunnelMonEntry ::= SEQUENCE {
         jnxIpSecTunMonRemoteGwAddrType     InetAddressType,
         jnxIpSecTunMonRemoteGwAddr         InetAddress,
         jnxIpSecTunMonIndex                Integer32,
         jnxIpSecTunMonLocalGwAddrType      InetAddressType,
         jnxIpSecTunMonLocalGwAddr          InetAddress,
         jnxIpSecTunMonLocalProxyId         DisplayString,
         jnxIpSecTunMonRemoteProxyId        DisplayString,
         jnxIpSecTunMonKeyType              JnxKeyType,
         jnxIpSecTunMonRemotePeerType       JnxRemotePeerType,  
         jnxIpSecTunMonOutEncryptedBytes    Counter64,
         jnxIpSecTunMonOutEncryptedPkts     Counter64,
         jnxIpSecTunMonInDecryptedBytes     Counter64,
         jnxIpSecTunMonInDecryptedPkts      Counter64,
         jnxIpSecTunMonAHInBytes            Counter64,
         jnxIpSecTunMonAHInPkts             Counter64,
         jnxIpSecTunMonAHOutBytes           Counter64,
         jnxIpSecTunMonAHOutPkts            Counter64,
         jnxIpSecTunMonReplayDropPkts       Counter64,
         jnxIpSecTunMonAhAuthFails          Counter64,
         jnxIpSecTunMonEspAuthFails         Counter64,
         jnxIpSecTunMonDecryptFails         Counter64,
         jnxIpSecTunMonBadHeaders           Counter64,
         jnxIpSecTunMonBadTrailers          Counter64,
         jnxIpSecTunMonDroppedPkts          Counter64   -- obsolete        
      }											

      jnxIpSecTunMonRemoteGwAddrType OBJECT-TYPE
         SYNTAX        InetAddressType
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
            "The IP address type of the remote gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelMonEntry 1 }

      jnxIpSecTunMonRemoteGwAddr OBJECT-TYPE
         SYNTAX        InetAddress
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
            "The IP address of the remote gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelMonEntry 2 }

     jnxIpSecTunMonIndex OBJECT-TYPE
         SYNTAX 	Integer32 (1..2147483647)
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
            "The index of the IPsec Phase-2 Tunnel Table.
             The value of the index is a number which begins at one and 
	         is incremented with each tunnel that is created. The value of 
	         this object will wrap at 2,147,483,647."
         ::= { jnxIpSecTunnelMonEntry 3 }

    jnxIpSecTunMonLocalGwAddrType OBJECT-TYPE
         SYNTAX        InetAddressType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
            "The IP address type of the local gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelMonEntry 4 }

       jnxIpSecTunMonLocalGwAddr OBJECT-TYPE
         SYNTAX        InetAddress
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
            "The IP address of the local gateway (endpoint) for the IPsec
             Phase-2 Tunnel."
         ::= { jnxIpSecTunnelMonEntry 5 }

      jnxIpSecTunMonLocalProxyId OBJECT-TYPE
         SYNTAX        DisplayString
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Identifier for the local end."
         ::= { jnxIpSecTunnelMonEntry 6 }

      jnxIpSecTunMonRemoteProxyId OBJECT-TYPE
         SYNTAX        DisplayString
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Identifier for the remote end."
         ::= { jnxIpSecTunnelMonEntry 7 }
		 
      jnxIpSecTunMonKeyType OBJECT-TYPE
         SYNTAX        JnxKeyType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
            "The type of key used by the IPsec Phase-2 Tunnel. It can be
             one of the following two types:
               - IKE negotiated
               - Manually installed"
         ::= { jnxIpSecTunnelMonEntry 8 }

      jnxIpSecTunMonRemotePeerType OBJECT-TYPE
         SYNTAX        JnxRemotePeerType
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "The type of the remote peer gateway (endpoint). It can be one
             of the following two types:
               - static (Remote peer whose IP address is known beforehand)
               - dynamic (Remote peer whose IP address is not known
                          beforehand)"
         ::= { jnxIpSecTunnelMonEntry 9 }

      jnxIpSecTunMonOutEncryptedBytes OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of bytes encrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelMonEntry 10 }


      jnxIpSecTunMonOutEncryptedPkts OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets encrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelMonEntry 11 }
		 

      jnxIpSecTunMonInDecryptedBytes OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of bytes decrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelMonEntry 12 }
		 

      jnxIpSecTunMonInDecryptedPkts OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets decrypted by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelMonEntry 13 }
		 

      jnxIpSecTunMonAHInBytes OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of incoming bytes authenticated using AH by this Phase-2
             tunnel."
         ::= { jnxIpSecTunnelMonEntry 14 }
		 

      jnxIpSecTunMonAHInPkts OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of incoming packets authenticated using AH by this Phase-2
             tunnel."
         ::= { jnxIpSecTunnelMonEntry 15 }
		 

      jnxIpSecTunMonAHOutBytes OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of outgoing bytes applied AH by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelMonEntry 16 }
		 

      jnxIpSecTunMonAHOutPkts OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of outgoing packets applied AH by this Phase-2 tunnel."
         ::= { jnxIpSecTunnelMonEntry 17 }
		 
      jnxIpSecTunMonReplayDropPkts OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets dropped by this Phase-2 tunnel due to
             anti replay check failure."
         ::= { jnxIpSecTunnelMonEntry 18 }
		 

      jnxIpSecTunMonAhAuthFails OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed AH authentication."
         ::= { jnxIpSecTunnelMonEntry 19 }
		 

      jnxIpSecTunMonEspAuthFails OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed ESP authentication."
         ::= { jnxIpSecTunnelMonEntry 20 }
		 

      jnxIpSecTunMonDecryptFails OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed decryption."
         ::= { jnxIpSecTunnelMonEntry 21 }


      jnxIpSecTunMonBadHeaders OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed due to bad headers."
         ::= { jnxIpSecTunnelMonEntry 22 }
	
	 
      jnxIpSecTunMonBadTrailers OBJECT-TYPE
         SYNTAX        Counter64
         MAX-ACCESS    read-only 
         STATUS        current 
         DESCRIPTION
            "Number of packets received by this Phase-2 tunnel that
             failed due to bad ESP trailers."
         ::= { jnxIpSecTunnelMonEntry 23 }
	
	 
      jnxIpSecTunMonDroppedPkts  OBJECT-TYPE
         SYNTAX         Counter64
         MAX-ACCESS 	read-only 
         STATUS         obsolete
         DESCRIPTION
            "Total number of dropped packets for this Phase-2 tunnel. 
             This attribute is obsolete."
         ::= { jnxIpSecTunnelMonEntry 26 }


   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
   -- The IPsec Phase-2 Security Association (SA) Table
   -- +++++++++++++++++++++++++++++++++++++++++++++++++++++++

      jnxIpSecSaMonTable OBJECT-TYPE
         SYNTAX SEQUENCE OF JnxIpSecSaMonEntry
         MAX-ACCESS         not-accessible
         STATUS             current
         DESCRIPTION
            "The IPsec Phase-2 Security Association Table.
            This table identifies the structure (in terms of
            component SAs) of each active Phase-2 IPsec tunnel.
            This table contains an entry for each active and
            expiring security association and maps each entry
            in the active Phase-2 tunnel table (ipSecTunTable)
            into a number of entries in this table. 

            SA contains the information negotiated by IKE. The SA 
            is like a contract laying out the rules of the VPN 
            connection for the duration of the SA. An SA is assigned 
            a 32-bit number that, when used in conjunction with the 
            destination IP address, uniquely identifies the SA. This 
            number is called the Security Parameters Index or SPI.

            IPSec SAs area unidirectional and they are unique in 
            each security protocol. A set of SAs are needed for a 
            protected data pipe, one per direction per protocol.  
            "
         ::= { jnxIpSecFlowMonPhaseTwo 3 }

      jnxIpSecSaMonEntry OBJECT-TYPE
         SYNTAX     JnxIpSecSaMonEntry
         MAX-ACCESS not-accessible
         STATUS     current
         DESCRIPTION
            "Each entry contains the attributes associated with
             active and expiring IPsec Phase-2
             security associations."
         INDEX { jnxIpSecTunMonRemoteGwAddrType, -- From jnxIpSecTunnelTable 
                 jnxIpSecTunMonRemoteGwAddr,     -- From jnxIpSecTunnelTable
                 jnxIpSecTunMonIndex,            -- From jnxIpSecTunnelTable
                 jnxIpSecSaMonIndex  }
         ::= { jnxIpSecSaMonTable 1 }

      JnxIpSecSaMonEntry ::= SEQUENCE {
         jnxIpSecSaMonIndex                 Integer32,
         jnxIpSecSaMonProtocol              INTEGER,	  
         jnxIpSecSaMonInSpi                 JnxSpiType,		  
         jnxIpSecSaMonOutSpi                JnxSpiType,		  
         jnxIpSecSaMonType                  JnxSAType,
         jnxIpSecSaMonEncapMode             JnxEncapMode,
         jnxIpSecSaMonLifeSize              Integer32,
         jnxIpSecSaMonLifeTime              Integer32,
         jnxIpSecSaMonActiveTime            TimeInterval,
         jnxIpSecSaMonLifeSizeThreshold     Integer32,  
         jnxIpSecSaMonLifeTimeThreshold     Integer32, 
         jnxIpSecSaMonEncryptAlgo           JnxEncryptAlgo,
         jnxIpSecSaMonAuthAlgo              JnxAuthAlgo,	  
         jnxIpSecSaMonState                 INTEGER
      }

      jnxIpSecSaMonIndex OBJECT-TYPE
         SYNTAX      Integer32 (1..65535)
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
            "The index, in the context of the IPsec tunnel ipSecTunIndex,
            of the security association represented by this table entry.
            The value of this index is a number which begins at one and
            is incremented with each SPI associated with an IPsec Phase-2
            Tunnel.  The value of this object will wrap at 65535."
         ::= { jnxIpSecSaMonEntry 1 }

      jnxIpSecSaMonProtocol OBJECT-TYPE
         SYNTAX INTEGER{
                   ah(1),
                   esp(2)
                }
         MAX-ACCESS read-only 
         STATUS     current
         DESCRIPTION
            "The index, represents the security protocol (AH, ESP or
             IPComp) for which this security association was setup."
         ::= { jnxIpSecSaMonEntry 2 }

      jnxIpSecSaMonInSpi OBJECT-TYPE
         SYNTAX     JnxSpiType
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
             "The value of the incoming SPI."
         ::= { jnxIpSecSaMonEntry 3 }

      jnxIpSecSaMonOutSpi OBJECT-TYPE
         SYNTAX     JnxSpiType
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
             "The value of the outgoing SPI."
         ::= { jnxIpSecSaMonEntry 4 }

      jnxIpSecSaMonType OBJECT-TYPE
         SYNTAX     JnxSAType
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
             "This field represents the type of security associations 
			 which can be either manual or dynamic"
         ::= { jnxIpSecSaMonEntry 5 }

      jnxIpSecSaMonEncapMode OBJECT-TYPE
         SYNTAX     JnxEncapMode
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
            "The encapsulation mode used by an IPsec Phase-2 Tunnel. "
         ::= { jnxIpSecSaMonEntry 6 }

      jnxIpSecSaMonLifeSize OBJECT-TYPE
         SYNTAX     Integer32
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
            "The negotiated LifeSize of the IPsec Phase-2 Tunnel in kilobytes. "
         ::= { jnxIpSecSaMonEntry 7 }

      jnxIpSecSaMonLifeTime OBJECT-TYPE
         SYNTAX     Integer32
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
            "The negotiated LifeTime of the IPsec Phase-2 Tunnel in seconds. "
         ::= { jnxIpSecSaMonEntry 8 }

      jnxIpSecSaMonActiveTime OBJECT-TYPE
         SYNTAX     TimeInterval
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
            "The length of time the IPsec Phase-2 Tunnel has been active in 
             hundredths of seconds. "
         ::= { jnxIpSecSaMonEntry 9 }

      jnxIpSecSaMonLifeSizeThreshold OBJECT-TYPE
         SYNTAX     Integer32
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
            "The security association LifeSize refresh threshold in kilobytes. "
         ::= { jnxIpSecSaMonEntry 10 }

      jnxIpSecSaMonLifeTimeThreshold OBJECT-TYPE
         SYNTAX     Integer32
         MAX-ACCESS read-only 
         STATUS     current 
         DESCRIPTION
            "The security association LifeTime refresh threshold in seconds. "
         ::= { jnxIpSecSaMonEntry 11 }

      jnxIpSecSaMonEncryptAlgo OBJECT-TYPE
         SYNTAX     JnxEncryptAlgo
         MAX-ACCESS read-only 
         STATUS     current
         DESCRIPTION
            "The Encryption algorithm used to encrypt 
			 the packets which can be either es-cbc or 3des-cbc. "
         ::= { jnxIpSecSaMonEntry 12 }

      jnxIpSecSaMonAuthAlgo OBJECT-TYPE
         SYNTAX     JnxAuthAlgo
         MAX-ACCESS read-only 
         STATUS     current
         DESCRIPTION
            "The algorithm used for authentication of packets which
			 can be hmac-md5-96 or hmac-sha1-96 or hmac-sha-256-128"
         ::= { jnxIpSecSaMonEntry 13 }

      jnxIpSecSaMonState OBJECT-TYPE
         SYNTAX INTEGER{
                   unknown  (0),
                   active   (1),
                   expiring (2)
                }
         MAX-ACCESS read-only
         STATUS     current
         DESCRIPTION
            "This column represents the status of the security association
            represented by this table entry. If the status of the SA is
            'active', the SA is ready for active use. The status
            'expiring' represents any of the various states that the
            security association transitions through before being purged."
         ::= { jnxIpSecSaMonEntry 14 }

END

