NETLINK-SPECIFIC-MIB DEFINITIONS ::= BEGIN

-- **************************************************************************
-- *                                                                        *
-- *  CSI Netlink                                                           *   
-- *                                                                        *   
-- * File: netlink-mib.txt                                                  *
-- * Release: 4.0.0 (with some pre 4.0.2 Voice Additions                    *
-- * Release Date:  April 3, 1998                                           *
-- *                                                                        *
-- **************************************************************************
-- *                                                                        *
-- * Copyright (c) 1998 by CSI Netlink.  All rights reserved. No part of    *
-- * this work covered by copyrights herein may be reproduced or copied in  *
-- * any form or by any means - electronic, graphic, or mechanical,         *
-- * including photocopying, recording, taping, or using information and    *
-- * retrieval systems - without prior written permission from CSI Netlink. *
-- *                                                                        *
-- * This is proprietary information which is protected by copyright.       *
-- * Netlink, FRX4000 (TM), FRX6000 (TM), FRX7000 (TM), and FRX8000 (TM)    *
-- * are trademarks of Cabletron Systems, Inc. NetFRAD (TM) and OmniLinx    *
-- * Switch (TM) are trademarks of CSI Netlink. All other product           *
-- * designations are the property of their respective owners.              *
-- *                                                                        *
-- **************************************************************************

IMPORTS
    OBJECT-TYPE
        FROM RFC-1212
    RowStatus, MacAddress, TimeInterval
        FROM SNMPv2-TC
    mib-2, DisplayString, PhysAddress
        FROM RFC1213-MIB
    enterprises, mgmt, TimeTicks, Gauge, Counter, IpAddress, NetworkAddress
        FROM RFC1155-SMI;

--  This MIB module uses the extended OBJECT-TYPE macro as
--  defined in RFC 1212.

-- textual conventions

-- DisplayString ::= OCTET STRING
-- This data type is used to model textual information taken
-- from the NVT ASCII character set.  By convention, objects
-- with this syntax are declared as having
--
--      SIZE (0..255)

-- PhysAddress ::= OCTET STRING
-- This data type is used to model media addresses.  For many
-- types of media, this will be in a binary representation.
-- For example, an ethernet address would be represented as
-- a string of 6 octets.

NlSubscriberAddress ::= OCTET STRING (SIZE(1..15))
-- this should really be a X121Address, which is defined in RFC 1382 as
--           X121Address ::= OCTET STRING (SIZE(0..17))
             -- 0 to 17 bytes in length containing the ASCII
             -- characters [0-9], each octet contains one digit
             -- of the address.
-- Since we only support non-TOA/NPI type addresses (see X.25 Blue Book)
-- our addresses are upto 15 digits.
-- Since we cannot configure empty addresses, the minimum is 1 digit,
-- which suits us, since indices need at least one component.
-- NOTE: need to support wildcard characters '?' and '*'.
-- NOTE: the screen interface allows 'U' and 'G', which is a bug.
-- Also, since we use it as an index, we could use the binary equivalent
-- of decimal digits, rather than the ASCII equivalent. But, since digits
-- besides decimal digits are used (?, *) we prefer the ASCII representation.
-- This will make usage from most management applications (ie. browsers) a
-- little more complicated, but no funny mapping is done.
-- We use the SMI rules for variable-string indexing (first subid specifies
-- the length, the rest of the subids are big-endian).

-- the following RFC 1747 object type is used by the SDLC link station
-- tables defined in this mib.
snaDLC              OBJECT IDENTIFIER ::= {mib-2 41}
sdlc                OBJECT IDENTIFIER ::= {snaDLC 1}
sdlcLSGroup         OBJECT IDENTIFIER ::= {sdlc 2}
sdlcLSAdminTable    OBJECT IDENTIFIER ::= {sdlcLSGroup 1}
sdlcLSAdminEntry    OBJECT IDENTIFIER ::= {sdlcLSAdminTable 1}
sdlcLSAddress       OBJECT-TYPE
                    SYNTAX      INTEGER (1..255)
                    ACCESS      read-only
                    STATUS      mandatory
                    DESCRIPTION
                         "This value is the poll address of the
                         secondary link station for this SDLC link.  It
                         uniquely identifies the SDLC link station
                         within a single SDLC port."
                    ::= { sdlcLSAdminEntry 1 }

netlink OBJECT IDENTIFIER ::= { enterprises 173 }

-- ***********************
-- *  THE NETWORK GROUP  *
-- ***********************

network OBJECT IDENTIFIER ::= { netlink 6 }
netstat OBJECT IDENTIFIER ::=     { network 1 }

--
--  The netstat group is used to describe network status information for
--  a node. It only applies to the FRX8000 nodes since the FRX4000s and
--  FRX6000s have no knowledge of any other nodes.               
--

nsMaxNeigh OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Maximum number of neighbor nodes. This value is currently
        always 64 for FRX8000 and 20 for an N7400 or 7500. 
        A neighbor is the closest node in a path from the local node."
        ::= { netstat 1 }

nsThisNode OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "This nodes number. (1-250) "
        ::= { netstat 2 }

nsNodTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A table showing all nodes known to this node
        along with status and neighbor information."
        ::= { netstat 3 }

nsEntry OBJECT-TYPE
        SYNTAX NsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "Each entry of the node table is indexed by 
        node number."
        INDEX { nsNodNum }
        ::= { nsNodTable 1 }

NsEntry ::=
        SEQUENCE {
                nsNodNum
                        INTEGER,
                nsStatus
                        INTEGER,
                nsNumNeigh
                        INTEGER
        }

nsNodNum OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The node number of the desired node. This is the
        index into the node table."
        ::= { nsEntry 1 }

nsStatus OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The operational status of the node. The status is 
        given as:
            1 = Node is defined in the database;
            9 = Node is operational;"
        ::= { nsEntry 2 }

nsNumNeigh OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Current number of neighbor nodes to this node."
        ::= { nsEntry 3 }

nsNeighTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NsNeighEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "The neighbor table lists the status of a nodes
        neighbors."
        ::= { netstat 4 }

nsNeighEntry OBJECT-TYPE
        SYNTAX NsNeighEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "The table entries are indexed by the node number and 
        the neighbors node number."
        INDEX { nsNTNode, nsNTNeigh }
        ::= { nsNeighTable 1 }

NsNeighEntry ::=
        SEQUENCE {
                nsNTNode
                        INTEGER,
                nsNTNeigh
                        INTEGER,
                nsNTNeighStat
                        INTEGER
        }

nsNTNode OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The node number of the node whose neighbor's status
        is being sought."
        ::= { nsNeighEntry 1 }

nsNTNeigh OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The node number of the neighbor whose status is being
        sought."
        ::= { nsNeighEntry 2 }

nsNTNeighStat OBJECT-TYPE
        SYNTAX INTEGER { notConnected(1),
                         connected(2) }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The status of the neighbor node given as:
            1 = previously, but not currently, connected;
            2 = Currently connected; "
        ::= { nsNeighEntry 3 }

-- ********************
-- *  THE NODE GROUP  *
-- ********************

local OBJECT IDENTIFIER ::=   { netlink 7 }
node OBJECT IDENTIFIER ::=          { local 1 }
nodeCfgTable OBJECT IDENTIFIER ::=   { node 1 }
nodeAlmTable OBJECT IDENTIFIER ::=   { node 2 }
nodeSNMPGroup OBJECT IDENTIFIER ::=  { node 3 }

--
--  The NODE group is used to describe configuration of the node
--

nodeModel OBJECT-TYPE
        SYNTAX INTEGER { model1(1),
                                         model2(2),
                                         rackmount(3),
                                         highavail(4),
                                         netfrad(5),
                                         frx4000(6),
                                         ss1800(7)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Describes the unit model"
        ::= { nodeSNMPGroup 1 }

--
--  The Traps group provides information about Traps on the node
--

nodeTrapText OBJECT-TYPE
        SYNTAX DisplayString
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Text of the last alarm generated"
        ::= {  nodeSNMPGroup 2 }

nodeTrapAdrTable OBJECT-TYPE
        SYNTAX SEQUENCE OF TpAdrEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A table used to define the IP address of end-nodes
        to receive alarms generated by this node. Up to 16 addresses
        can be specified."
        ::= { nodeSNMPGroup 3 }

tpAdrEntry OBJECT-TYPE
        SYNTAX TpAdrEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Trap entry containing objects relating to SNMP traps."
        INDEX { tpAdrIdx }
        ::= { nodeTrapAdrTable 1 }

TpAdrEntry ::=
        SEQUENCE {
                tpAdrIdx
                        INTEGER,
                tpAddress
                        IpAddress,
                tpAdrFlag
                        INTEGER,
                tpAdrSLev
                        INTEGER
        }
tpAdrIdx OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The index into the trap configuration table"
        ::= { tpAdrEntry 1 }

tpAddress OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The IP Address of the end-station to send alarms"
        ::= { tpAdrEntry 2 }

tpAdrFlag OBJECT-TYPE
        SYNTAX INTEGER { disableTraps(1), 
                         enableTraps(2), 
                         delete(3) }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Defines the state of this entry as:
            0 = Do not send traps to the Address;
            1 = Send traps to the Address;
            2 = This Address entry is deleted from the table; "
        ::= { tpAdrEntry 3 }

tpAdrSLev OBJECT-TYPE
        SYNTAX INTEGER { critical(1),
                         major(2),
                         minor(3),
                         informational(4) }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Lowest severity level traps that will be sent to 
        this Address; 1 is the highest, 4 is the lowest."
        ::= { tpAdrEntry 4 }

nodeBagTable OBJECT IDENTIFIER ::=   { node 4 }

-- *****************************
-- *  THE HARDWARE CARD GROUP  *
-- *****************************

hwcard OBJECT IDENTIFIER ::=            { local 2 }

--
--  This item describes the Max number of Protocols allowed on each RLP
--

rlpMaxProtos OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Maximum number of protocols allowed on each RLP.
    This value is currently 11 for FRX4000s, 9 for FRX6000s, and
        5 for FRX7000s and FRX8000s."
        ::= { hwcard 1 }

--
--  The RLP Table used to describe each RLP on a node
--

rlpConfigTable OBJECT-TYPE
        SYNTAX SEQUENCE OF RlpEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe each RLP on the node"
        ::= { hwcard 2 }

rlpEntry OBJECT-TYPE
        SYNTAX RlpEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An RLP entry containing objects relating to RLPs."
        INDEX { rlpIndex }
        ::= { rlpConfigTable 1 }

RlpEntry ::=
        SEQUENCE {
                rlpIndex
                        INTEGER,
                rlpStatus
                        INTEGER,
                rlpMemorySize
                        INTEGER,
                rlpLIC1Type
                        INTEGER,
                rlpLIC2Type
                        INTEGER,
                rlpProtocol
                        OCTET STRING,
                rlpGroupNumber
                        INTEGER,
                rlpGroupResponsibility
                        INTEGER
        }

rlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP number on the node"
        ::= { rlpEntry 1 }

rlpStatus OBJECT-TYPE
        SYNTAX INTEGER { installed(1),
                         configured(2),
                         load-failed(3),
                         loading(4),
                         ipl-failed(5),
                         ipl-in-progress(6),
                         failed(7),
                         operational(8),
                         power-off(9),
                         power-on(10) }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The current state of this RLP"
        ::= { rlpEntry 2 }

rlpMemorySize OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The amount of memory installed on this RLP"
        ::= { rlpEntry 3 }

rlpLIC1Type OBJECT-TYPE
        SYNTAX INTEGER { none(1),
                                         rs232(2),
                                         rs422(3),
                                         v35(4) ,
                                         hs-rs232(5),
                                         x21(6),
                                         rs449(7),
                                         universal(8),
                                         t1(10),
                                         e1(11),
                                         voice(13) 
                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Type of Line Interface card in the first position"
        ::= { rlpEntry 4 }

rlpLIC2Type OBJECT-TYPE
        SYNTAX INTEGER { none(1),
                                         rs232(2),
                                         rs422(3),
                                         v35(4) ,
                                         hs-rs232(5),
                                         x21(6),
                                         rs449(7),
                                         universal(8),
                                         t1(10),
                                         e1(11),
                                         voice(13) 
        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Type of Line Interface card in the second position"
        ::= { rlpEntry 5 }

rlpProtocol OBJECT-TYPE
        SYNTAX OCTET STRING
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The protocols configured on this RLP. This is an OCTET 
        STRING where each octet represents a protocol type. The size of this
        is the maximum number of protocols allowed on an RLP (rlpMaxProtos).
        The protocol types are defined as:
                00 = none 
                01 = X.25
                02 = Frame Relay
                03 = Async
                04 = SDLC
                05 = BSC Interactive
                07 = IP
                08 = SNMP
                09 = RIP
                0A = LLC2
                0B = Trunk
                0C = IPX
                0D = Config
                0E = LLC2-R
                0F = IP-R
                10 = NVSP
                11 = Bridge
        "
        ::= { rlpEntry 6 }

rlpGroupNumber OBJECT-TYPE
        SYNTAX INTEGER (1..4)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The group to which this RLP belongs- always 1 if not
        FRX7000."
        ::= { rlpEntry 7 }

rlpGroupResponsibility OBJECT-TYPE
        SYNTAX INTEGER {
                primary (1),
                secondary (2)
        }       
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION "The responsibility of this RLP within its group, always
        primary if not FRX7000."
        ::= { rlpEntry 8 }

-- ********************
-- *  THE PORT GROUP  *
-- ********************

port OBJECT IDENTIFIER ::=              { local 3 }
portX25Group OBJECT IDENTIFIER ::=  { port 1 }

portPhyX25AdminTable  OBJECT-TYPE
       SYNTAX      SEQUENCE OF PortPhyX25AdminEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
               "This table contains Netlink Enterprise specific
               objects to manage an X25 port. Changing one of
               these parameters may take effect in the operating
               port immediately or may wait until the interface is
               restarted depending on the details of the
               implementation.

               Most of the objects in this read-write table have
               corresponding read-only objects in the
               portX25OperTable that return the current
               operating value.

               The operating values may be different from these
               configured values if a configured parameter was
               configured after the interface was started."
       ::= { portX25Group 1 }

portPhyX25AdminEntry  OBJECT-TYPE
       SYNTAX      PortPhyX25AdminEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
               "A list of configured values for an X25 port."
       INDEX   { nlIfRlp, nlIfPort }
                    ::= { portPhyX25AdminTable 1 }

PortPhyX25AdminEntry  ::= SEQUENCE
{
        portPhyX25AdminConnector        INTEGER,
        portPhyX25AdminSpeed            INTEGER,
        portPhyX25AdminGenerateClock    INTEGER,
        portPhyX25AdminRcvClockFromDTE INTEGER,
        portPhyX25AdminDialOut                  INTEGER,
        portPhyX25AdminInactivityTimer  INTEGER,
        portPhyX25AdminDisconnectTimer  INTEGER,
        portPhyX25AdminSetupTimer               INTEGER,
        portPhyX25AdminTrunkFlag                INTEGER,
        portPhyX25AdminTrunkGroup               OCTET STRING,
        portPhyX25AdminRowStatus        RowStatus
}

portPhyX25AdminConnector    OBJECT-TYPE
        SYNTAX      INTEGER{
                rs232 (3),
                v35 (5),
                rs449 (6),
                rs530 (7),
                x21 (8),
                t1 (10),
                e1 (11)
           }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "Physical port interface connector type."
        ::= { portPhyX25AdminEntry 1 }

portPhyX25AdminSpeed      OBJECT-TYPE
        SYNTAX      INTEGER 
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                "This object defines the speed of the X25 port.  The speed may
                only be set to one of a series of reasonable values, and if an attempt 
                is made to set the speed to a value which is within the valid range
                but not equal to one of these values, the speed will be rounded up. 
                If the connector type of the port is RS232, the port could be a
                standard port or a high speed port.  If the port is a high speed
                RS232 port, the maximum valid speed is 256000.  If the port is a 
                standard RS232 port, the maximum valid speed is 64000 on the 
                FRX4000/SS1840 and 19200 on all other products.  It may be possible
                to set the speed of a standard RS232 port to a speed which is valid
                for a high speed RS232 port but invalid for a standard RS232 port.
                In this case, the port may not end up having the invalid speed.  
                The default speed for a standard RS232 port on the FRX6000 is 19200."
        DEFVAL { 64000 }

        ::= { portPhyX25AdminEntry 2 }

portPhyX25AdminGenerateClock      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
         }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                "Specifies whether the port will generate the clock
            necessary to synchronize traffic over the link."
                DEFVAL { no }
        ::= { portPhyX25AdminEntry 3 }

portPhyX25AdminRcvClockFromDTE      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This object defines whether the receive clock
                        will be used from the DTE."
                DEFVAL { no }
        ::= { portPhyX25AdminEntry 4 }

portPhyX25AdminDialOut      OBJECT-TYPE
        SYNTAX  INTEGER {
               none(1),
               dialIn(2),
                           dialOut(3) 
               }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This flag indicates whether the port is connected to a dial
                        modem, and whethter connections will be initiated through
                        dial-in or dial-out calls." 
                DEFVAL { none }
        ::= { portPhyX25AdminEntry 5 }

portPhyX25AdminInactivityTimer      OBJECT-TYPE
        SYNTAX      INTEGER  (1..30)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This timer defines in minutes, the period of inactivity
                        allowed between calls. Once the timer expires, the port
                        is disabled untill the next call is placed, if a Dial out
                        port, or the Disconnect Timer expires, if a Dial in port.
                        This variable is only meaningful if the port is a Dial port."
                DEFVAL { 5 }
        ::= { portPhyX25AdminEntry 6 }

portPhyX25AdminDisconnectTimer      OBJECT-TYPE
        SYNTAX      INTEGER   (1..255)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This timer defines, in seconds, the length of time a
                        dial-in port will remain disabled after expiration of the
                        InActivity Timer."
                DEFVAL { 5 }
        ::= { portPhyX25AdminEntry 7 }

portPhyX25AdminSetupTimer      OBJECT-TYPE
        SYNTAX      INTEGER   (1..255)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This  timer determines the length of time, in seconds, that
                        a response must be received by the port, after entering the
                        Linkup state. If a response is not received, the port enters
                        a Failed state."
                DEFVAL { 5 }
        ::= { portPhyX25AdminEntry 8 }

portPhyX25AdminTrunkFlag      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This flag, when set, indicates the port is associated
                        with a network trunk group.  It will be disabled/enabled
                        if the network trunk is not operational."
                DEFVAL { no }
        ::= { portPhyX25AdminEntry 9 }

portPhyX25AdminTrunkGroup      OBJECT-TYPE
        SYNTAX      OCTET STRING
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This variable contains a string of 8 bytes, with each
                        byte indicating 8 ports on an RLP that may be a part of
                        a trunk group. Since a TurboFrad has only 1 RLP, only the
                        first byte is valid if the node is an FRX4000. Each
                        port is represented by a single bit within the RLP byte.
                        The bit position represents the port number...for example,
                        if port 2 on RLP 0 was in a trunk group, the first byte of
                        the string would contain x04 and all other bytes would be 0."
        ::= { portPhyX25AdminEntry 10 }

portPhyX25AdminRowStatus      OBJECT-TYPE
        SYNTAX      RowStatus
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portPhyX25AdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device, and which is
                supplied by a management station wishing to exercise an
                on-line update of the existing conceptual row.  For a
                management protocol set operation, a genErr response is
                returned when the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { portPhyX25AdminEntry 11 }

portPhyX25OperTable  OBJECT-TYPE
       SYNTAX      SEQUENCE OF PortPhyX25OperEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
               "This table contains Netlink Enterprise specific
               objects to manage an X25 port. Changing one of
               these parameters may take effect in the operating
               port immediately or may wait until the interface is
               restarted depending on the details of the
               implementation.

               All of the objects in this table are read-only.

               The operating values may be different from these
               configured values if a configured parameter was
               configured after the interface was started."
           ::= { portX25Group 2 }

portPhyX25OperEntry  OBJECT-TYPE
                    SYNTAX      PortPhyX25OperEntry
                    ACCESS      not-accessible
                    STATUS      mandatory
                    DESCRIPTION
                            "A list of configured values for an X25 port."
                    INDEX   { nlIfRlp, nlIfPort }
                    ::= { portPhyX25OperTable 1 }

PortPhyX25OperEntry  ::= SEQUENCE
{
        portPhyX25OperConnector                 INTEGER,
        portPhyX25OperSpeed                     INTEGER,
        portPhyX25OperGenerateClock     INTEGER,
        portPhyX25OperRcvClockFromDTE   INTEGER,
        portPhyX25OperDialOut                   INTEGER,
        portPhyX25OperInactivityTimer   INTEGER,
        portPhyX25OperDisconnectTimer   INTEGER,
        portPhyX25OperSetupTimer                INTEGER,
        portPhyX25OperTrunkFlag                 INTEGER,
        portPhyX25OperTrunkGroup                OCTET STRING
}

portPhyX25OperConnector    OBJECT-TYPE
        SYNTAX      INTEGER{
                rs232 (3),
                v35 (5),
                rs449 (6),
                rs530 (7),
                x21 (8),
                t1 (10),
                e1 (11)
           }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "Physical port interface connector type."
        ::= { portPhyX25OperEntry 1 }

portPhyX25OperSpeed      OBJECT-TYPE
        SYNTAX      INTEGER 
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                "This object defines the speed of the X25 port.  The speed may
                only be set to one of a series of reasonable values, and if an attempt 
                is made to set the speed to a value which is within the valid range
                but not equal to one of these values, the speed will be rounded up. 
                If the connector type of the port is RS232, the port could be a
                standard port or a high speed port.  If the port is a high speed
                RS232 port, the maximum valid speed is 256000.  If the port is a 
                standard RS232 port, the maximum valid speed is 64000 on the 
                FRX4000/SS1840 and 19200 on all other products.  It may be possible
                to set the speed of a standard RS232 port to a speed which is valid
                for a high speed RS232 port but invalid for a standard RS232 port.
                In this case, the port may not end up having the invalid speed.  
                The default speed for a standard RS232 port on the FRX6000 is 19200."
        ::= { portPhyX25OperEntry 2 }

portPhyX25OperGenerateClock      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
         }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                "Specifies whether the port will generate the clock
            necessary to synchronize traffic over the link."
        ::= { portPhyX25OperEntry 3 }

portPhyX25OperRcvClockFromDTE      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This object defines whether the receive clock will be
                        used from the DTE."
        ::= { portPhyX25OperEntry 4 }

portPhyX25OperDialOut      OBJECT-TYPE
        SYNTAX  INTEGER {
               none(1),
               dialIn(2),
               dialOut(3)
               }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This flag indicates whether the port is connected to a dial
                        modem, and whethter connections will be initiated through
                        dial-in or dial-out calls." 
        ::= { portPhyX25OperEntry 5 }

portPhyX25OperInactivityTimer      OBJECT-TYPE
        SYNTAX      INTEGER  (1..30)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This timer defines in minutes, the period of inactivity
                        allowed between calls. Once the timer expires, the port
                        is disabled untill the next call is placed, if a Dial out
                        port, or the Disconnect Timer expires, if a Dial in port.
                        This variable is only meaningful if the port is a Dial port."
        ::= { portPhyX25OperEntry 6 }

portPhyX25OperDisconnectTimer      OBJECT-TYPE
        SYNTAX      INTEGER   (1..255)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This timer defines, in seconds, the length of time a
                        dial-in port will remain disabled after expiration of the
                        InActivity Timer."
        ::= { portPhyX25OperEntry 7 }

portPhyX25OperSetupTimer      OBJECT-TYPE
        SYNTAX      INTEGER   (1..255)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This  timer determines the length of time, in seconds, that
                        a response must be received by the port, after entering the
                        Linkup state. If a response is not received, the port enters
                        a Failed state."
        ::= { portPhyX25OperEntry 8 }

portPhyX25OperTrunkFlag      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This flag, when set, indicates the port is associated
                        with a network trunk group.  It will be disabled/enabled
                        if the network trunk is not operational."
        ::= { portPhyX25OperEntry 9 }

portPhyX25OperTrunkGroup      OBJECT-TYPE
        SYNTAX      OCTET STRING
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This variable contains a string of 8 bytes, with each
                        byte indicating a port on this RLP that may be a part of
                        a trunk group."
        ::= { portPhyX25OperEntry 10 }

-- Admin Table for X25 logical ports

portLogicalX25AdminTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF PortLogicalX25AdminEntry
        ACCESS      not-accessible
        STATUS      mandatory
        DESCRIPTION
           "This table contains Netlink Enterprise specific
           objects to manage an X25 Logical port. Changing one of
           these parameters may take effect in the operating
           port immediately or may wait until the interface is
           restarted depending on the details of the
           implementation.

           The operating values may be different from these
           configured values if a configured parameter was
           configured after the interface was started."
           ::= { portX25Group 3 }

portLogicalX25AdminEntry  OBJECT-TYPE
       SYNTAX      PortLogicalX25AdminEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
           "A list of configured values for an X25 logical port."
       INDEX   { nlIfRlp, nlIfPhyPort, nlIfPort }
                    ::= { portLogicalX25AdminTable 1 }

PortLogicalX25AdminEntry  ::= SEQUENCE
{
        portLogicalX25AdminFrDlci       INTEGER,
        portLogicalX25AdminCxnPriority INTEGER,
        portLogicalX25AdminRfc1490      INTEGER,
        portLogicalX25AdminBAG          INTEGER,
        portLogicalX25AdminRowStatus    RowStatus 
}

portLogicalX25AdminFrDlci      OBJECT-TYPE
        SYNTAX      INTEGER   (16..991)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            " The DLCI number used to identify the entry in the table. The
            range is 16-991. "
                DEFVAL { 16 }
        ::= { portLogicalX25AdminEntry 1 }

portLogicalX25AdminCxnPriority      OBJECT-TYPE
        SYNTAX      INTEGER   (0..9)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            " This field sets the priority of the connection among others on the
            physical port. The range is 0 for lowest priority to 9 for
            the highest priority. "
                DEFVAL { 0 }
        ::= { portLogicalX25AdminEntry 2 }

portLogicalX25AdminRfc1490      OBJECT-TYPE
        SYNTAX      INTEGER  {
                                annexG (1),
                                rfc1490 (2)
                                }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        " This field indicates the encapsulation method used"
                DEFVAL { rfc1490 }
        ::= { portLogicalX25AdminEntry 3 }

portLogicalX25AdminBAG      OBJECT-TYPE
        SYNTAX      INTEGER   (0..16)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
          "Assigns this DLCI to one of sixteen groups whose parameters
          regulate bandwidth usage. A 0 value indicates the DLCI does
          not use BAGs"
                DEFVAL { 0 }
        ::= { portLogicalX25AdminEntry 4 }

portLogicalX25AdminRowStatus      OBJECT-TYPE
        SYNTAX      RowStatus
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portLogicalX25AdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device, and which is
                supplied by a management station wishing to exercise an
                on-line update of the existing conceptual row.  For a
                management protocol set operation, a genErr response is
                returned when the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { portLogicalX25AdminEntry 5 }

-- Oper Table for X25 logical ports

portLogicalX25OperTable  OBJECT-TYPE

        SYNTAX      SEQUENCE OF PortLogicalX25OperEntry
        ACCESS      not-accessible
        STATUS      mandatory
        DESCRIPTION
           "This table contains Netlink Enterprise specific
           objects to manage an X25 Logical port. Changing one of
           these parameters may take effect in the operating
           port immediately or may wait until the interface is
           restarted depending on the details of the
           implementation.

           The operating values may be different from these
           configured values if a configured parameter was
           configured after the interface was started."
           ::= { portX25Group 4 }

portLogicalX25OperEntry  OBJECT-TYPE
       SYNTAX      PortLogicalX25OperEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
           "A list of configured values for an X25 port."
       INDEX   { nlIfRlp, nlIfPhyPort, nlIfPort }
                    ::= { portLogicalX25OperTable 1 }

PortLogicalX25OperEntry  ::= SEQUENCE
{
        portLogicalX25OperFrDlci        INTEGER,
        portLogicalX25OperCxnPriority INTEGER,
        portLogicalX25OperRfc1490       INTEGER,
        portLogicalX25OperBAG           INTEGER
}

portLogicalX25OperFrDlci      OBJECT-TYPE
        SYNTAX      INTEGER   (1..255)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            " The DLCI number used to identify the entry in the table. The
            range is 16-991. "

        ::= { portLogicalX25OperEntry 1 }

portLogicalX25OperCxnPriority      OBJECT-TYPE
        SYNTAX      INTEGER   (0..9)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            " This field sets the priority of the connection among others on the
            physical port. The range is 0 for lowest priority to 9 for
            the highest priority. "
        ::= { portLogicalX25OperEntry 2 }

portLogicalX25OperRfc1490      OBJECT-TYPE
        SYNTAX      INTEGER  {
                                annexG (1),
                                rfc1490 (2)
                                }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        " This field indicates the encapsulation method used"
        ::= { portLogicalX25OperEntry 3 }

portLogicalX25OperBAG      OBJECT-TYPE
        SYNTAX      INTEGER   (1..16)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
          "Assigns this DLCI to one of sixteen groups whose parameters
          regulate bandwidth usage."
        ::= { portLogicalX25OperEntry 4 }

-- Admin Table for both logical and physical ports
--

portX25AdminTable  OBJECT-TYPE
       SYNTAX      SEQUENCE OF PortX25AdminEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
               "This table contains Netlink Enterprise specific
               objects to manage an X25 port. Changing one of
               these parameters may take effect in the operating
               port immediately or may wait until the interface is
               restarted depending on the details of the
               implementation.

               Most of the objects in this read-write table have
               corresponding read-only objects in the
               portX25OperTable that return the current
               operating value.

               The operating values may be different from these
               configured values if a configured parameter was
               configured after the interface was started."
         ::= { portX25Group 5 }

portX25AdminEntry  OBJECT-TYPE
       SYNTAX      PortX25AdminEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
             "A list of configured values for an X25 port."
          INDEX   { nlIfRlp, nlIfPort }

    ::= { portX25AdminTable 1 }

PortX25AdminEntry ::= SEQUENCE
{
        portX25AdminBlockedFlag         INTEGER,
        portX25AdminFlowCtrlNeg                 INTEGER,
        portX25AdminThruptClassNeg      INTEGER,
        portX25AdminLocChgPrev          INTEGER,
        portX25AdminRevChgAccpt         INTEGER,
        portX25AdminFastSelAccpt        INTEGER,
        portX25AdminInCallBar           INTEGER,
        portX25AdminOutCallBar          INTEGER,
        portX25AdminMaxPktSize          INTEGER,
        portX25AdminDefPktSize          INTEGER,
        portX25AdminMaxWinSize          INTEGER,
        portX25AdminDefWinSize          INTEGER,
        portX25AdminMaxThruptClass      INTEGER,
        portX25AdminCUGPref             INTEGER,
        portX25AdminCUGIndex            INTEGER,
        portX25AdminCUGIncAccess        INTEGER,
        portX25AdminCUGOutAccess        INTEGER
}

portX25AdminBlockedFlag OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION
            " A flag which when set, means the port should not be
            enabled after a boot-up of the node. "
                DEFVAL { no }
        ::= { portX25AdminEntry 1 }

portX25AdminFlowCtrlNeg      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
           "A flag which if set, permits negotiation of
           the flow control parameters on a per call basis.
           If N is selected, the default packet and window
           sizes will be used. If Y is selected, the packet
           or window size in a call packet (up to the
           configured Max Packet Size or Max Window Size) is
           used."
                DEFVAL { no }
        ::= { portX25AdminEntry 2 }

portX25AdminThruptClassNeg      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "A flag which ,if set, permists negotiation of
            the throughput class for either direction of
            data transmission on a per call basis. If N is
            selected, the configured Max Throughput Class
            value is used.  If Y, any throughput class in
            a call packet (up to the Max Thruput Class) is
            used."
                DEFVAL { no }
         ::= { portX25AdminEntry 3 }

portX25AdminLocChgPrev      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "If Y is selected, no calls can be charged to
            port.  Incoming calls from the network with
            reverse charge specified will be rejected. Outgoing
            calls will insert reverse charge in the call packet
            if not already included."
                DEFVAL { no }
         ::= { portX25AdminEntry 4 }

portX25AdminRevChgAccpt      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "A flag, if set, that authorizes transmission of
            incoming calls that request the reverse charge
            facility. If N is selected, and a call requests
            it, it will not be transmitted."
                DEFVAL { no }
         ::= { portX25AdminEntry 5 }

portX25AdminFastSelAccpt      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "A flag, if set, that authorizes transmission of
            incoming calls that request the Fast Select
            facility."
                DEFVAL { no }
         ::= { portX25AdminEntry 6 }

portX25AdminInCallBar      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "An X25 facility that prevents transmission of
            incoming calls to the local DTE."
                DEFVAL { no }
         ::= { portX25AdminEntry 7 }

portX25AdminOutCallBar      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
            "An X25 facility that prevents transmission of
             incoming calls to the local DTE."
                DEFVAL { no }
        ::= { portX25AdminEntry 8 }

portX25AdminMaxPktSize      OBJECT-TYPE
        SYNTAX      INTEGER  (128..4096)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        " The maximum data packet size that will be allowed to pass
            through this port."
                DEFVAL { 1024 }
        ::= { portX25AdminEntry 9 }

portX25AdminDefPktSize      OBJECT-TYPE
        SYNTAX      INTEGER             (16..4096)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This is the size that will be assigned to an incoming call
                        setup packet if the packet does not request a packet size."
                DEFVAL { 128 }
        ::= { portX25AdminEntry 10 }

portX25AdminMaxWinSize      OBJECT-TYPE
        SYNTAX      INTEGER  (2..7)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This is the maximum number of unacknowledged packets
                        per logical channel that can pass through this port."
                DEFVAL { 7 }
        ::= { portX25AdminEntry 11 }

portX25AdminDefWinSize      OBJECT-TYPE
        SYNTAX      INTEGER (1..7)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This size will be assigned to an incoming call
                        setup packet if the packet doesn't request a window size."
                DEFVAL { 2 }
        ::= { portX25AdminEntry 12 }

portX25AdminMaxThruptClass      OBJECT-TYPE
        SYNTAX      INTEGER  (3..13)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This specifies the default throughput class that will be
                        inserted into a Call Request packet if Thruput Class
                        negotiation is not enabled or if a thruput class is not
                        requested in the call request."
        ::= { portX25AdminEntry 13 }

portX25AdminCUGPref      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This flag, if set, indicates the port belongs to at least
                        one CUG."
                DEFVAL { no }
        ::= { portX25AdminEntry 14 }

portX25AdminCUGIndex      OBJECT-TYPE
        SYNTAX      INTEGER  (1..100)
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        "This number is an index into a Closed User Group table
                        which identifies the default Closed User Group for the
                        port."
                DEFVAL { 1 }
        ::= { portX25AdminEntry 15 }

portX25AdminCUGIncAccess      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        " This flag, when set, indicates whether this port will
                        be allowed to receive calls from outside its CUGs."
                DEFVAL { no }
        ::= { portX25AdminEntry 16 }

portX25AdminCUGOutAccess      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-write
        STATUS      mandatory
        DESCRIPTION
                        " This flag, when set, indicates whether this port will
                        be allowed to make calls outside its CUGs."
                DEFVAL { no }
        ::= { portX25AdminEntry 17 }

portX25OperTable  OBJECT-TYPE
       SYNTAX      SEQUENCE OF PortX25OperEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
               "This table contains Netlink Enterprise specific
               objects to manage an X25 port. Changing one of
               these parameters may take effect in the operating
               port immediately or may wait until the interface is
               restarted depending on the details of the
               implementation.

               The objects in this read-only table 
               corresponding read-only objects in the
               portX25OperTable that return the current
               operating value.

               The operating values may be different from these
               configured values if a configured parameter was
               configured after the interface was started."
         ::= { portX25Group 6 }

portX25OperEntry  OBJECT-TYPE
       SYNTAX      PortX25OperEntry
       ACCESS      not-accessible
       STATUS      mandatory
       DESCRIPTION
             "A list of configured values for an X25 port."
          INDEX   { nlIfRlp, nlIfPort }
    ::= { portX25OperTable 1 }

PortX25OperEntry ::= SEQUENCE {
        portX25OperBlockedFlag  INTEGER,
        portX25OperFlowCtrlNeg          INTEGER,
        portX25OperThruptClassNeg       INTEGER,
        portX25OperLocChgPrev           INTEGER,
        portX25OperRevChgAccpt          INTEGER,
        portX25OperFastSelAccpt         INTEGER,
        portX25OperInCallBar            INTEGER,
        portX25OperOutCallBar           INTEGER,
        portX25OperMaxPktSize           INTEGER,
        portX25OperDefPktSize           INTEGER,
        portX25OperMaxWinSize           INTEGER,
        portX25OperDefWinSize           INTEGER,
        portX25OperMaxThruptClass       INTEGER,
        portX25OperCUGPref              INTEGER,
        portX25OperCUGIndex             INTEGER,
        portX25OperCUGIncAccess         INTEGER,
        portX25OperCUGOutAccess         INTEGER
}

portX25OperBlockedFlag OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
            " A flag which when set, means the port should not be
            enabled after a boot-up of the node. "
        ::= { portX25OperEntry 1 }

portX25OperFlowCtrlNeg      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
           "A flag which if set, permits negotiation of
           the flow control parameters on a per call basis.
           If N is selected, the default packet and window
           sizes will be used. If Y is selected, the packet
           or window size in a call packet (up to the
           configured Max Packet Size or Max Window Size) is
           used."
        ::= { portX25OperEntry 2 }

portX25OperThruptClassNeg      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            "A flag which ,if set, permists negotiation of
            the throughput class for either direction of
            data transmission on a per call basis. If N is
            selected, the configured Max Throughput Class
            value is used.  If Y, any throughput class in
            a call packet (up to the Max Thruput Class) is
            used."
         ::= { portX25OperEntry 3 }

portX25OperLocChgPrev      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            "If Y is selected, no calls can be charged to
            port.  Incoming calls from the network with
            reverse charge specified will be rejected. Outgoing
            calls will insert reverse charge in the call packet
            if not already included."
         ::= { portX25OperEntry 4 }

portX25OperRevChgAccpt      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            "A flag, if set, that authorizes transmission of
            incoming calls that request the reverse charge
            facility. If N is selected, and a call requests
            it, it will not be transmitted."
         ::= { portX25OperEntry 5 }

portX25OperFastSelAccpt     OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            "A flag, if set, that authorizes transmission of
            incoming calls that request the Fast Select
            facility."
         ::= { portX25OperEntry 6 }

portX25OperInCallBar      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            "An X25 facility that prevents transmission of
            incoming calls to the local DTE."
         ::= { portX25OperEntry 7 }

portX25OperOutCallBar      OBJECT-TYPE
        SYNTAX      INTEGER {
            no (1),
            yes (2)
            }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
            "An X25 facility that prevents transmission of
             incoming calls to the local DTE."
        ::= { portX25OperEntry 8 }

portX25OperMaxPktSize      OBJECT-TYPE
        SYNTAX      INTEGER  (128..4096)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        " The maximum data packet size that will be allowed to pass
            through this port."
        ::= { portX25OperEntry 9 }

portX25OperDefPktSize      OBJECT-TYPE
        SYNTAX      INTEGER             (16..4096)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This is the size that will be assigned to an incoming call
                        setup packet if the packet does not request a packet size."
        ::= { portX25OperEntry 10 }

portX25OperMaxWinSize      OBJECT-TYPE
        SYNTAX      INTEGER  (2..7)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This is the maximum number of unacknowledged packets
                        per logical channel that can pass through this port."
        ::= { portX25OperEntry 11 }

portX25OperDefWinSize      OBJECT-TYPE
        SYNTAX      INTEGER (1..7)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This size will be assigned to an incoming call
                        setup packet if the packet doesn't request a window size."
        ::= { portX25OperEntry 12 }

portX25OperMaxThruptClass      OBJECT-TYPE
        SYNTAX      INTEGER  (3..13)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This specifies the default throughput class that will be
                        inserted into a Call Request packet if Thruput Class
                        negotiation is not enabled or if a thruput class is not
                        requested in the call request."
        ::= { portX25OperEntry 13 }

portX25OperCUGPref      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This flag, if set, indicates the port belongs to at least
                        one CUG."
        ::= { portX25OperEntry 14 }

portX25OperCUGIndex      OBJECT-TYPE
        SYNTAX      INTEGER  (1..100)
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        "This number is an index into a Closed User Group table
                        which identifies the default Closed User Group for the
                        port."
        ::= { portX25OperEntry 15 }

portX25OperCUGIncAccess      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        " This flag, when set, indicates whether this port will
                        be able to receive calls from outside its CUGs."
        ::= { portX25OperEntry 16 }

portX25OperCUGOutAccess      OBJECT-TYPE
        SYNTAX  INTEGER {
               no(1),
               yes(2)
               }
        ACCESS      read-only
        STATUS      mandatory
        DESCRIPTION
                        " This flag, when set, indicates whether this port will
                        be able to make calls outside its CUGs."
        ::= { portX25OperEntry 17 }

portFrGroup OBJECT IDENTIFIER ::=  { port 2 }

-- The Frame Relay Port Configuration table
-- contains information on the FR physical port.

portFrConfigTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortFrEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A list of Frame Relay ports .  The number of
            entries will be the number of Frame Relay ports on the node."
    ::= { portFrGroup 1 }

portFrEntry OBJECT-TYPE
    SYNTAX  PortFrEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "An Frame Relay Port entry containing objects
            relating to the port that are configurable
            by the user."
    INDEX   {  portFrRlpIndex , portFrPortIndex }
    ::= { portFrConfigTable 1 }

PortFrEntry ::=
    SEQUENCE {
        portFrRlpIndex
            INTEGER,
        portFrPortIndex
        INTEGER,
        portFrBlockedFlag
            INTEGER,
        portFrMaxBytesPerFrame
            INTEGER,
        portFrT392Timer
            INTEGER,
        portFrOutgoingRateControl
            INTEGER,
        portFrBandwidthAllocation
            INTEGER,
        portFrConnector
         INTEGER,
        portFrLogicalDCE
         INTEGER,
        portFrGenClock
            INTEGER,
        portFrRcvClkFrmDTE
            INTEGER,
        portFrLLM
            INTEGER,
        portFrRowStatus
            RowStatus,
        portFrSpeed
            INTEGER,
        portFrBackupUseOnly
            INTEGER
    }
portFrRlpIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " The RLP number of the Frame Relay port. It will be in the
            range 1-8."
    ::= { portFrEntry 1 }
portFrPortIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " The Port number of the Frame Relay port. It will
            be in the range 1-8 for a physical port. It will be in the range
            9-64 for a Frame Relay logical port."
    ::= { portFrEntry 2 }

portFrBlockedFlag OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " A flag which when set, means the port should not be
            enabled after a boot-up of the node. "
    DEFVAL { no }
    ::= { portFrEntry 3 }

portFrMaxBytesPerFrame OBJECT-TYPE
    SYNTAX  INTEGER (16..4096)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The maximum number of bytes allowed in an I Frame for this
            Frame Relay port."
    DEFVAL { 1600 }
    ::= { portFrEntry 4 }

portFrT392Timer OBJECT-TYPE
    SYNTAX  INTEGER (5..30)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This timer indicates how long the network will wait between
            Status Enquiry messages before recording an error.  It
            should be greater than or equal to the frDlcmiPollingInterval
            variable in the RFC1315 Mib."
    DEFVAL { 15 }
    ::= { portFrEntry 5 }

portFrOutgoingRateControl OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " This is a flag which, when set, enables the enforcement of
            the Outgoing Rate Control parameters."
    DEFVAL { no }
    ::= { portFrEntry 6 }

portFrBandwidthAllocation OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " This is a flag which, when set, enables whether the bandwidth
            allocation will be enforced. "
    DEFVAL { no }
    ::= { portFrEntry 7 }

portFrConnector OBJECT-TYPE
    SYNTAX  INTEGER {
                rs232 (3),
                v35 (5),
                rs449 (6),
                rs530 (7),
                x21 (8),
                t1 (10),
                e1 (11)
            }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This defines the connector type of the Frame Relay port."
    ::= { portFrEntry 8 }

portFrLogicalDCE OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
            }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This defines the port as logical DCE or DTE."
    DEFVAL { no }
    ::= { portFrEntry 9 }

portFrGenClock OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
            }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This specifies whether the port will generate the clock
             necessary to synchronize traffic over the link."
    DEFVAL { no }
    ::= { portFrEntry 10 }

portFrRcvClkFrmDTE OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
            }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This allows the clock to be looped back from the DTE using
             the TT (Terminal Timing) signal, which can be helpful on
             high-speed lines."
    DEFVAL { no }
    ::= { portFrEntry 11 }

portFrLLM OBJECT-TYPE
    SYNTAX  INTEGER {
                none(1),
                lmi(2),
                annexd(3)
            }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This determines whether, and what type of, configurable
             network management (status enquiries) will be allowed."
    DEFVAL { annexd }
    ::= { portFrEntry 12 }

portFrRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portFrConfigTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device, and which is
                supplied by a management station wishing to exercise an
                on-line update of the existing conceptual row.  For a
                management protocol set operation, a genErr response is
                returned when the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
    ::= { portFrEntry 13 }

portFrSpeed OBJECT-TYPE
    SYNTAX      INTEGER (75..2048000)
    ACCESS      read-write
    STATUS      mandatory
    DESCRIPTION
    "This object defines the speed of the Frame Relay port.  The speed may
     only be set to one of a series of reasonable values, and if an attempt is made
     to set the speed to a value which is within the valid range but not equal to one
     of these values, the speed will be rounded up.  If the connector type of the port
     is RS232, the port could be a standard port or a high speed port.  If the port is
     a high speed RS232 port, the maximum valid speed is 256000.  If the port is a standard
     RS232 port, the maximum valid speed is 64000 on the FRX4000/SS1840 and 19200
     on all other products.  It may be possible to set the speed of a standard RS232 port
     to a speed which is valid for a high speed RS232 port but invalid for a standard
     RS232 port. In this case, the port may not end up having the invalid speed.  The default
     speed for a standard RS232 port on the FRX6000 is 19200."
    DEFVAL { 64000 }
    ::= { portFrEntry 14 }

portFrBackupUseOnly OBJECT-TYPE
    SYNTAX      INTEGER {
                no(1),
                yes(2)
                }
    ACCESS      read-write
    STATUS      mandatory
    DESCRIPTION "This object determines whether all DLCIs on the port will
                be reserved exclusively as backups for other DLCIs in the
                same node. If yes is specified for this object, the port
                will remain disabled until needed for backup."
    DEFVAL { no }
    ::= { portFrEntry 15 }

-- The Frame Relay DLCI Configuration table
-- The DLCI contains information about the DCLI configured on a FR
-- port. Note that deleting of a DLCI entry does not affect the existence
-- of the DLCI for the running protocol. The DLCI record is removed from
-- the database file, but will remain known to the node until it is
-- rebooted. This is consistent with the way DLCI information is handled
-- when configuring through the user interface menu system.

portDLCIConfigTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortDLCIEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A list of DLCI's on Frame Relay ports .  The number of
            entries will be the number of DLCIs on all the Frame Relay
            ports on a node."
    ::= { portFrGroup 2 }

portDLCIEntry OBJECT-TYPE
    SYNTAX  PortDLCIEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "An Frame Relay Port DLCI entry
            relating to the Rate Control Information that is configurable
            by the user."
    INDEX   {  portDLCIRlpIndex , portDLCIPortIndex, portDLCIIndex }
    ::= { portDLCIConfigTable 1 }

PortDLCIEntry ::=
    SEQUENCE {
        portDLCIRlpIndex
            INTEGER,
        portDLCIPortIndex
            INTEGER,
        portDLCIIndex
            INTEGER,
        portDLCIIncomingCIR
            INTEGER,
        portDLCIOutgoingCIR
            INTEGER,
        portDLCIIncomingBc
            INTEGER,
        portDLCIOutgoingBc
            INTEGER,
        portDLCIIncomingBe
            INTEGER,
        portDLCIOutgoingBe
            INTEGER,
        portDLCIBecnRecoveryCnt
            INTEGER,
        portDLCIPriority
            INTEGER,
        portDLCIRowStatus
            RowStatus,
        portDLCIBackupGroup
            INTEGER,
        portDLCIBackupProtEnb
            INTEGER
    }
portDLCIRlpIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " The RLP number on which the DLCI is located. The range for
            this is 1-8. "
    ::= { portDLCIEntry 1 }
portDLCIPortIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " The port number on which the DLCI is located. The range for
            this is 1-8 for a physical FR port and 9-64 for a logical FR port. "
    ::= { portDLCIEntry 2 }
portDLCIIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " The DLCI number used to identify the entry in the table. The
            range is 16-991. "
    ::= { portDLCIEntry 3 }
portDLCIIncomingCIR OBJECT-TYPE
    SYNTAX  INTEGER (0..2000)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The committed information rate that is supported on the
            DLCI for incoming data. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 4 }
portDLCIOutgoingCIR OBJECT-TYPE
    SYNTAX  INTEGER (0..2000)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The committed information rate that is supported on the
            DLCI for outgoing data. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 5 }
portDLCIIncomingBc OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The committed burst size is the maximum amount of data
            to be transmitted under normal conditions within the time
            period defined by Bc/Cir that is supported on the
            DLCI for incoming data. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 6 }
portDLCIOutgoingBc OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The committed burst size is the maximum amount of data
            to be transmitted under normal conditions within the time
            period defined by Bc/Cir that is supported on the
            DLCI for Outgoing data. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 7 }
portDLCIIncomingBe OBJECT-TYPE
    SYNTAX  INTEGER (0..32767)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The excess burst size is the maximum amount of incoming data
            in excess of the committed burst size that the network will try to
            transfer during the time interval determined by Bc/Cir on this
            DLCI. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 8 }
portDLCIOutgoingBe OBJECT-TYPE
    SYNTAX  INTEGER (0..32767)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The excess burst size is the maximum amount of incoming data
            in excess of the committed burst size that the network will try to
            transfer during the time interval determined by Bc/Cir on this
            DLCI. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 9 }
portDLCIBecnRecoveryCnt OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " The BECN recovery Count is a method of controlling the rate
            of return to max traffic flow after it has been reduced due to
            congestion. The value determines the number of packets received
            sequentially without BECN set, before increasing the Excess Burst
            Size by 1/8 of it's configured value. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 10 }

portDLCIPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..4)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " This field sets the priority of the DLCI among others on the
            physical port. The range is 0 for lowest priority to 4 for
            the highest priority. "
    DEFVAL { 0 }
    ::= { portDLCIEntry 11 }

portDLCIRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portDLCIConfigTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned.

            Also note that deleting a DLCI entry will only remove it from
            the database file, and it's existence will still be known by
            the protocol until the node is rebooted."
    ::= { portDLCIEntry 12 }

portDLCIBackupGroup OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This object specifies (if configured as any number other than
            zero) that this is a primary DLCI, and identifies the backup
            DLCI(s) (in a Frame Relay backup group) that will take over if
            this DLCI fails. This is applicable only on an initiating node,
            which is the node that will initiate the switchover to a backup
            DLCI. At switchover, the initiating node notifies the remote
            node of the change."
    DEFVAL { 0 }
    ::= { portDLCIEntry 13 }

portDLCIBackupProtEnb OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
            }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This object specifies whether the DLCI will be used as a
            non-initiating backup DLCI. The DLCI will wait for a backup
            protocol message from the initiating end, telling the backup
            where to send the rest of the messages."
    DEFVAL { no }
    ::= { portDLCIEntry 14 }

-- The Frame Relay Backup Group Configuration table

-- A Frame Relay Backup Group is one or more DLCIs (on the same RLP)
-- that can act as a backup for one or more "primary" DLCIs (also on
-- the same RLP). If a node detects a failure in a primary DLCI
-- connection, the software will search any DLCI in the backup group
-- configured for the primary DLCI, and will select the first
-- available one as a backup. The backup will become operational and
-- will remain in that state until the primary becomes active again.
-- If the backup fails while in use, the software will check the
-- status of the primary, then (if necessary) search the primary's
-- backup group for another backup.

portFrBackupGroupTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF FrBackupEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "   A Table describes the Frame Relay Backup MIB . "
    ::= { portFrGroup 3 }

portFrBackupEntry OBJECT-TYPE
    SYNTAX  FrBackupEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "   This Entry contains the  SNMP objects that are used for
                configurating the Frame Relay Backup. "
    INDEX  { portFrBackupRLP, portFrBackupPort, portFrBackupDLCI, portFrBackupGroup }

 ::= { portFrBackupGroupTable 1 }

FrBackupEntry ::=
    SEQUENCE  {
        portFrBackupRLP
            INTEGER,
        portFrBackupPort
            INTEGER,
        portFrBackupDLCI
            INTEGER,
        portFrBackupGroup
            INTEGER,
        portFrBackupWaitTimer
            INTEGER,
        portFrBackupProtEnab
            INTEGER,
        portFrBackupRowStatus
            RowStatus
    }

portFrBackupRLP   OBJECT-TYPE
    SYNTAX  INTEGER (1..8)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " This RLP number identifies the RLP containing the
             primary and backup DLCIs. "
    ::= { portFrBackupEntry 1 }

portFrBackupPort  OBJECT-TYPE
    SYNTAX  INTEGER (1..8)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " This Port number is the physical port on which
             the backup DLCI is being configured. "
    ::= { portFrBackupEntry 2 }

portFrBackupDLCI  OBJECT-TYPE
    SYNTAX  INTEGER (16..991)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " This DLCI number is the backup being configured. "
    ::= { portFrBackupEntry 3 }

portFrBackupGroup OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            " This Group number is the backup being configured. "
    ::= { portFrBackupEntry 4 }

portFrBackupWaitTimer OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            " This is the time after a primary DLCI failure that the
             software will wait for this DLCI to become active before
             checking the next backup DLCI. If the backup does not
             become active before the timer expires, the software will
             search the backup group for the next available backup."
    DEFVAL { 120 }
    ::= { portFrBackupEntry 5 }

portFrBackupProtEnab  OBJECT-TYPE
    SYNTAX  INTEGER {
                no(1),
                yes(2)
            }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
        " This enables or disables the backup protocol on the specified
         DLCI. It should be set to yes if and only if the remote device
         is an FRX4000 or FRX6000 with the backup protocol enabled on the
         remote DLCI connected to this backup group entry. "
    DEFVAL { no }
    ::= { portFrBackupEntry 6 }

portFrBackupRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portFrBackupGroupTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
    ::= { portFrBackupEntry 7 }

portBsciGroup   OBJECT IDENTIFIER ::=   { port 4 }

--
--  BSC Interactive Port Administrative Table
--

portBsciAdminTable OBJECT-TYPE
        SYNTAX SEQUENCE OF PortBsciAdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A list of BSC Interactive ports . The number of
                        entries will be the number of BSC Interactive ports on the node."
        ::= { portBsciGroup 1 }

portBsciAdminEntry OBJECT-TYPE
        SYNTAX PortBsciAdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A BSCI Interactive Port entry containing objects
                        relating to the port that are configurable by the user."
        INDEX { nlIfRlp, nlIfPort }
        ::= { portBsciAdminTable 1 }

PortBsciAdminEntry ::=
        SEQUENCE {
                portBsciAdminBlockedFlag                                INTEGER,
                portBsciAdminConnector                                  INTEGER,
                portBsciAdminSpeed                                              INTEGER,
                portBsciAdminRetransmitInterval                 INTEGER,
                portBsciAdminMAXRetransmits                             INTEGER,
                portBsciAdminMaxBytesPerFrame                   INTEGER,
                portBsciAdminGenerateClock                              INTEGER,
                portBsciAdminRcvClockFromDTE                    INTEGER,
                portBsciAdminPadType                                    INTEGER,
                portBsciAdminUseEBCDIC                                  INTEGER,
                portBsciAdminCallInfoInRequestPacket    INTEGER,
                portBsciAdminClearVCOnLastDeviceDown    INTEGER,
                portBsciAdminTransTextSupported                 INTEGER,
                portBsciAdminEndToEndAck                                INTEGER,
                portBsciAdminFullDuplex                                 INTEGER,
                portBsciAdminMultidrop                                  INTEGER,
                portBsciAdminSlowPollRetryCount                 INTEGER,
                portBsciAdminSlowPollRetryFreq                  INTEGER,
                portBsciAdminStartSynchChars                    INTEGER,
                portBsciAdminEndPadChars                                INTEGER,
                portBsciAdminPollInterval                               INTEGER,
                portBsciAdminNoResponseTimer                    INTEGER,
                portBsciAdminNoResponseRetryCount               INTEGER,
                portBsciAdminErrorRetransmitCount               INTEGER,
                portBsciAdminNAKRetryCount                              INTEGER,
                portBsciAdminBlockCheck                                 INTEGER,
                portBsciAdminDataMode                                   INTEGER,
                portBsciAdminRowStatus                                  RowStatus,
                portBsciAdminAnswerNonConfigured                        INTEGER,
                portBsciAdminActivateConnectionWithoutPoll              INTEGER
        }

portBsciAdminBlockedFlag OBJECT-TYPE
        SYNTAX  INTEGER {
                                disabled(1),
                                enabled(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Causes the port to be enabled or disabled at node IPL."
        DEFVAL { disabled }
        ::= { portBsciAdminEntry 1 }

portBsciAdminConnector OBJECT-TYPE
        SYNTAX INTEGER {
                                rs232(3),
                                v35(5),
                                rs449(6),
                                rs530(7),
                                x21(8),
                                t1(10)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Physical port interface connector type."
        ::= { portBsciAdminEntry 2 }

portBsciAdminSpeed OBJECT-TYPE
        SYNTAX  INTEGER (75..19200)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Data transmission rate in bits per second."
        DEFVAL { 9600 }
        ::= { portBsciAdminEntry 3 }

portBsciAdminRetransmitInterval OBJECT-TYPE
        SYNTAX  INTEGER (1..9999)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Length of time before the node will transmit an I-frame
                                if the previous transmission is not acknowledged."
        DEFVAL { 2000}
        ::= { portBsciAdminEntry 4 }

portBsciAdminMAXRetransmits OBJECT-TYPE
        SYNTAX  INTEGER (1..99)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum number of times the node will attempt to send
                                an I-frame after a retransmission period expiration."
        DEFVAL { 5 }
        ::= { portBsciAdminEntry 5 }

portBsciAdminMaxBytesPerFrame OBJECT-TYPE
        SYNTAX  INTEGER (25..4105)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum frame size that will be transmitted on the port."
        DEFVAL { 4105 }
        ::= { portBsciAdminEntry 6 }

portBsciAdminGenerateClock OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies whether the port will generate the clock
                                necessary to synchronize traffic over the link."
        DEFVAL { yes }
        ::= { portBsciAdminEntry 7 }

portBsciAdminRcvClockFromDTE OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Allows the clock to be looped back from the DTE
                                using the TT (Terminal Timing) signal."
        DEFVAL { no }
        ::= { portBsciAdminEntry 8 }

portBsciAdminPadType OBJECT-TYPE
        SYNTAX  INTEGER {
                                tpad(1),
                                hpad(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "BSCI Pad Type"
        DEFVAL { tpad }
        ::= { portBsciAdminEntry 9 }

portBsciAdminUseEBCDIC OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies whether all devices on a line use the same
                                character set for successive session polls."
        DEFVAL { yes }
        ::= { portBsciAdminEntry 10 }

portBsciAdminCallInfoInRequestPacket OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies whether the user will have the option of
                                including call information in a call request packet."
        DEFVAL { yes }
        ::= { portBsciAdminEntry 11 }

portBsciAdminClearVCOnLastDeviceDown OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Causes the virtual circuit to be cleared when no
                                terminals are using it."
        DEFVAL { no }
        ::= { portBsciAdminEntry 12 }

portBsciAdminTransTextSupported OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Causes all characters transmitted to be treated as data."
        DEFVAL { no }
        ::= { portBsciAdminEntry 13 }

portBsciAdminEndToEndAck OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Allows management of acknowledgments end to end across
                                the network rather than locally at each end."
        DEFVAL { no }
        ::= { portBsciAdminEntry 14 }

portBsciAdminFullDuplex OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies full-duplex transmission."
        DEFVAL { yes }
        ::= { portBsciAdminEntry 15 }

portBsciAdminMultidrop OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies whether transmission will be multidrop."
        DEFVAL { no }
        ::= { portBsciAdminEntry 16 }

portBsciAdminSlowPollRetryCount OBJECT-TYPE
        SYNTAX  INTEGER (10..150)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies how many times the control unit will be polled
                                before it is put on the slow poll list."
        DEFVAL { 20 }
        ::= { portBsciAdminEntry 17 }

portBsciAdminSlowPollRetryFreq OBJECT-TYPE
        SYNTAX  INTEGER (1..200)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies the number of times active control units will
                                be polled between pollings on the slow poll list."
        DEFVAL { 20 }
        ::= { portBsciAdminEntry 18 }

portBsciAdminStartSynchChars OBJECT-TYPE
        SYNTAX  INTEGER (2..10)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies the number of synchronization characters
                                that will be added to the beginning of each frame."
        DEFVAL { 2 }
        ::= { portBsciAdminEntry 19 }

portBsciAdminEndPadChars OBJECT-TYPE
        SYNTAX  INTEGER (1..10)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies the number of padding characters that will
                                be added to the end of each frame."
        DEFVAL { 1 }
        ::= { portBsciAdminEntry 20 }

portBsciAdminPollInterval OBJECT-TYPE
        SYNTAX  INTEGER (100..1000)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies the time between passes through the polling list."
        DEFVAL { 500 }
        ::= { portBsciAdminEntry 21 }

portBsciAdminNoResponseTimer OBJECT-TYPE
        SYNTAX  INTEGER (2..10)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Activated after transmission of a general poll or a
                                data frame."
        DEFVAL { 2 }
        ::= { portBsciAdminEntry 22 }

portBsciAdminNoResponseRetryCount OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies how many times the user device will be polled
                                before control is passed on the next cluster."
        DEFVAL { 5 }
        ::= { portBsciAdminEntry 23 }

portBsciAdminErrorRetransmitCount OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies the number of times the Netlink device will
                                resend a block of data after the receiving device has
                                detected an error in that block."
        DEFVAL { 5 }
        ::= { portBsciAdminEntry 24 }

portBsciAdminNAKRetryCount OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies the number of times the Netlink device will
                                send a frame when the receiving device is unable to
                                acknowledge."
        DEFVAL { 5 }
        ::= { portBsciAdminEntry 25 }

portBsciAdminBlockCheck OBJECT-TYPE
        SYNTAX  INTEGER {
                                crc16(1),
                                even-lrc(2),
                                odd-lrc(3)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Sets the redundancy check parameter."
        DEFVAL { even-lrc }
        ::= { portBsciAdminEntry 26 }

portBsciAdminDataMode OBJECT-TYPE
        SYNTAX  INTEGER {
                                odd-7bit(1),
                                even-7bit(2),
                                none-8bit(3)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Sets the parity parameter."
        DEFVAL { none-8bit }
        ::= { portBsciAdminEntry 27 }

portBsciAdminRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portBsciAdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device, and which is
                supplied by a management station wishing to exercise an
                on-line update of the existing conceptual row.  For a
                management protocol set operation, a genErr response is
                returned when the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { portBsciAdminEntry 28 }

portBsciAdminAnswerNonConfigured OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Only valid if pad type is HPAD.  If yes, the HPAD will
                     respond to all devices on the line.  If no, the HPAD will
                     respond only to those devices that are configured on the
                     node."
        DEFVAL { yes }
        ::= { portBsciAdminEntry 29 }

portBsciAdminActivateConnectionWithoutPoll OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Only valid if pad type is TPAD.  If yes, will active the 
                     TPAD connection without a poll of the connected device."
        DEFVAL { no }
        ::= { portBsciAdminEntry 30 }

--
--  BSC Interactive Port Operational Table
--

portBsciOperTable OBJECT-TYPE
        SYNTAX SEQUENCE OF PortBsciOperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A list of BSC Interactive ports . The number of
                        entries will be the number of BSC Interactive ports on the node."
        ::= { portBsciGroup 2 }

portBsciOperEntry OBJECT-TYPE
        SYNTAX PortBsciOperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A BSCI Interactive Port entry containing objects
                        relating to the port that are configurable by the user."
        INDEX { nlIfRlp, nlIfPort }
        ::= { portBsciOperTable 1 }

PortBsciOperEntry ::=
        SEQUENCE {
                portBsciOperBlockedFlag                                 INTEGER,
                portBsciOperConnector                                   INTEGER,
                portBsciOperSpeed                                               INTEGER,
                portBsciOperRetransmitInterval                  INTEGER,
                portBsciOperMAXRetransmits                              INTEGER,
                portBsciOperMaxBytesPerFrame                    INTEGER,
                portBsciOperGenerateClock                               INTEGER,
                portBsciOperRcvClockFromDTE                             INTEGER,
                portBsciOperPadType                                             INTEGER,
                portBsciOperUseEBCDIC                                   INTEGER,
                portBsciOperCallInfoInRequestPacket             INTEGER,
                portBsciOperClearVCOnLastDeviceDown             INTEGER,
                portBsciOperTransTextSupported                  INTEGER,
                portBsciOperEndToEndAck                                 INTEGER,
                portBsciOperFullDuplex                                  INTEGER,
                portBsciOperMultidrop                                   INTEGER,
                portBsciOperSlowPollRetryCount                  INTEGER,
                portBsciOperSlowPollRetryFreq                   INTEGER,
                portBsciOperStartSynchChars                             INTEGER,
                portBsciOperEndPadChars                                 INTEGER,
                portBsciOperPollInterval                                INTEGER,
                portBsciOperNoResponseTimer                             INTEGER,
                portBsciOperNoResponseRetryCount                INTEGER,
                portBsciOperErrorRetransmitCount                INTEGER,
                portBsciOperNAKRetryCount                               INTEGER,
                portBsciOperBlockCheck                                  INTEGER,
                portBsciOperDataMode                                    INTEGER,
                portBsciOperAnswerNonConfigured                 INTEGER,
                portBsciOperActivateConnectionWithoutPoll               INTEGER
        }

portBsciOperBlockedFlag OBJECT-TYPE
        SYNTAX  INTEGER {
                                disabled(1),
                                enabled(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Causes the port to be enabled or disabled at node IPL."
        ::= { portBsciOperEntry 1 }

portBsciOperConnector OBJECT-TYPE
        SYNTAX INTEGER {
                                rs232(3),
                                v35(5),
                                rs449(6),
                                rs530(7),
                                x21(8),
                                t1(10)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Physical port interface connector type."
        ::= { portBsciOperEntry 2 }

portBsciOperSpeed OBJECT-TYPE
        SYNTAX  INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Data transmission rate in bits per second."
        ::= { portBsciOperEntry 3 }

portBsciOperRetransmitInterval OBJECT-TYPE
        SYNTAX  INTEGER (1..9999)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Length of time before the node will transmit an I-frame
                                if the previous transmission is not acknowledged."
        ::= { portBsciOperEntry 4 }

portBsciOperMAXRetransmits OBJECT-TYPE
        SYNTAX  INTEGER (1..99)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Maximum number of times the node will attempt to send
                                an I-frame after a retransmission period expiration."
        ::= { portBsciOperEntry 5 }

portBsciOperMaxBytesPerFrame OBJECT-TYPE
        SYNTAX  INTEGER (25..4105)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Maximum frame size that will be transmitted on the port."
        ::= { portBsciOperEntry 6 }

portBsciOperGenerateClock OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies whether the port will generate the clock
                                necessary to synchronize traffic over the link."
        ::= { portBsciOperEntry 7 }

portBsciOperRcvClockFromDTE OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Allows the clock to be looped back from the DTE
                                using the TT (Terminal Timing) signal."
        ::= { portBsciOperEntry 8 }

portBsciOperPadType OBJECT-TYPE
        SYNTAX  INTEGER {
                                tpad(1),
                                hpad(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "BSCI Pad Type"
        ::= { portBsciOperEntry 9 }

portBsciOperUseEBCDIC OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies whether all devices on a line use the same
                                character set for successive session polls."
        ::= { portBsciOperEntry 10 }

portBsciOperCallInfoInRequestPacket OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies whether the user will have the option of
                                including call information in a call request packet."
        ::= { portBsciOperEntry 11 }

portBsciOperClearVCOnLastDeviceDown OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Causes the virtual circuit to be cleared when no
                                terminals are using it."
        ::= { portBsciOperEntry 12 }

portBsciOperTransTextSupported OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Causes all characters transmitted to be treated as data."
        ::= { portBsciOperEntry 13 }

portBsciOperEndToEndAck OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Allows management of acknowledgments end to end across
                                the network rather than locally at each end."
        ::= { portBsciOperEntry 14 }

portBsciOperFullDuplex OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies full-duplex transmission."
        ::= { portBsciOperEntry 15 }

portBsciOperMultidrop OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies whether transmission will be multidrop."
        ::= { portBsciOperEntry 16 }

portBsciOperSlowPollRetryCount OBJECT-TYPE
        SYNTAX  INTEGER (10..150)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies how many times the control unit will be polled
                                before it is put on the slow poll list."
        ::= { portBsciOperEntry 17 }

portBsciOperSlowPollRetryFreq OBJECT-TYPE
        SYNTAX  INTEGER (1..200)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies the number of times active control units will
                                be polled between pollings on the slow poll list."
        ::= { portBsciOperEntry 18 }

portBsciOperStartSynchChars OBJECT-TYPE
        SYNTAX  INTEGER (2..10)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies the number of synchronization characters
                                that will be added to the beginning of each frame."
        ::= { portBsciOperEntry 19 }

portBsciOperEndPadChars OBJECT-TYPE
        SYNTAX  INTEGER (1..10)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies the number of padding characters that will
                                be added to the end of each frame."
        ::= { portBsciOperEntry 20 }

portBsciOperPollInterval OBJECT-TYPE
        SYNTAX  INTEGER (100..1000)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies the time between passes through the polling list."
        ::= { portBsciOperEntry 21 }

portBsciOperNoResponseTimer OBJECT-TYPE
        SYNTAX  INTEGER (2..10)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Activated after transmission of a general poll or a
                                data frame."
        ::= { portBsciOperEntry 22 }

portBsciOperNoResponseRetryCount OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies how many times the user device will be polled
                                before control is passed on the next cluster."
        ::= { portBsciOperEntry 23 }

portBsciOperErrorRetransmitCount OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies the number of times the Netlink device will
                                resend a block of data after the receiving device has
                                detected an error in that block."
        ::= { portBsciOperEntry 24 }

portBsciOperNAKRetryCount OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies the number of times the Netlink device will
                                send a frame when the receiving device is unable to
                                acknowledge."
        ::= { portBsciOperEntry 25 }

portBsciOperBlockCheck OBJECT-TYPE
        SYNTAX  INTEGER {
                                crc16(1),
                                even-lrc(2),
                                odd-lrc(3)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Sets the redundancy check parameter."
        ::= { portBsciOperEntry 26 }

portBsciOperDataMode OBJECT-TYPE
        SYNTAX  INTEGER {
                                odd-7bit(1),
                                even-7bit(2),
                                none-8bit(3)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Sets the parity parameter."
        ::= { portBsciOperEntry 27 }

portBsciOperAnswerNonConfigured OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Only valid if pad type is HPAD.  If yes, the HPAD will
                     respond to all devices on the line.  If no, the HPAD will
                     respond only to those devices that are configured on the
                     node."
        ::= { portBsciOperEntry 28 }

portBsciOperActivateConnectionWithoutPoll OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Only valid if pad type is TPAD.  If yes, will active the 
                     TPAD connection without a poll of the connected device."
        ::= { portBsciOperEntry 29 }

--
-- BSCI Port Subscriber Administrative Table
--

bsciSubscrAdminTable OBJECT-TYPE
        SYNTAX SEQUENCE OF BsciSubscrAdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A list of BSC Interactive port subscribers."
        ::= { portBsciGroup 3 }

bsciSubscrAdminEntry OBJECT-TYPE
        SYNTAX BsciSubscrAdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A BSCI Interactive Port Subscriber entry containing objects
                        relating to the port that are configurable by the user."
        INDEX { nlIfRlp, nlIfPort, bsciSubscrAdminSequence }
        ::= { bsciSubscrAdminTable 1 }

BsciSubscrAdminEntry ::=
        SEQUENCE {
                bsciSubscrAdminSequence                         INTEGER,
                bsciSubscrAdminLocalID                          NlSubscriberAddress,
                bsciSubscrAdminRemoteID                         NlSubscriberAddress,
                bsciSubscrAdminAutocall                         INTEGER,
                bsciSubscrAdminAutocallRtyTimer         INTEGER,
                bsciSubscrAdminAutocallMaxRtry          INTEGER,
                bsciSubscrAdminConnectionID                     INTEGER,
                bsciSubscrAdminRowStatus                        RowStatus
        }

bsciSubscrAdminSequence OBJECT-TYPE
        SYNTAX  INTEGER (1..16)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Subscriber index for a specific BSCI port subscriber."
        ::= { bsciSubscrAdminEntry 1 }

bsciSubscrAdminLocalID OBJECT-TYPE
        SYNTAX  NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Subscriber address of the local end of a BSCI connection."
        ::= { bsciSubscrAdminEntry 2 }

bsciSubscrAdminRemoteID OBJECT-TYPE
        SYNTAX  NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Subscriber address of the remote end of a BSCI connection."
        ::= { bsciSubscrAdminEntry 3 }

bsciSubscrAdminAutocall OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Causes a BSCI TPAD to automatically call its HPAD when
                                the controller becomes active."
        DEFVAL { no }
        ::= { bsciSubscrAdminEntry 4 }

bsciSubscrAdminAutocallRtyTimer OBJECT-TYPE
        SYNTAX  INTEGER (15..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Time between autocall retries."
        DEFVAL { 60 }
        ::= { bsciSubscrAdminEntry 5 }

bsciSubscrAdminAutocallMaxRtry OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum number of times an autocall will be sent."
        DEFVAL { 0 }
        ::= { bsciSubscrAdminEntry 6 }

bsciSubscrAdminConnectionID OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Identifier that will link the BSCI port with a device
                                configured in the BSCI Devices Table."
        DEFVAL { 0 }
        ::= { bsciSubscrAdminEntry 7 }

bsciSubscrAdminRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the bsciDevAdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { bsciSubscrAdminEntry 8 }

--
-- BSCI Port Subscriber Operational Table
--

bsciSubscrOperTable OBJECT-TYPE
        SYNTAX SEQUENCE OF BsciSubscrOperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A list of BSC Interactive port subscribers."
        ::= { portBsciGroup 4 }

bsciSubscrOperEntry OBJECT-TYPE
        SYNTAX BsciSubscrOperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A BSCI Interactive Port Subscriber entry containing objects
                        relating to the port that are configurable by the user."
        INDEX { nlIfRlp, nlIfPort, bsciSubscrOperSequence }
        ::= { bsciSubscrOperTable 1 }

BsciSubscrOperEntry ::=
        SEQUENCE {
                bsciSubscrOperSequence                          INTEGER,
                bsciSubscrOperLocalID                           NlSubscriberAddress,
                bsciSubscrOperRemoteID                          NlSubscriberAddress,
                bsciSubscrOperAutocall                          INTEGER,
                bsciSubscrOperAutocallRtyTimer          INTEGER,
                bsciSubscrOperAutocallMaxRtry           INTEGER,
                bsciSubscrOperConnectionID                      INTEGER
        }

bsciSubscrOperSequence OBJECT-TYPE
        SYNTAX  INTEGER (1..16)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Subscriber index for a specific BSCI port subscriber."
        ::= { bsciSubscrOperEntry 1 }

bsciSubscrOperLocalID OBJECT-TYPE
        SYNTAX  NlSubscriberAddress
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Subscriber address of the local end of a BSCI connection."
        ::= { bsciSubscrOperEntry 2 }

bsciSubscrOperRemoteID OBJECT-TYPE
        SYNTAX  NlSubscriberAddress
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Subscriber address of the remote end of a BSCI connection."
        ::= { bsciSubscrOperEntry 3 }

bsciSubscrOperAutocall OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Causes a BSCI TPAD to automatically call its HPAD when
                                the controller becomes active."
        ::= { bsciSubscrOperEntry 4 }

bsciSubscrOperAutocallRtyTimer OBJECT-TYPE
        SYNTAX  INTEGER (15..255)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Time between autocall retries."
        ::= { bsciSubscrOperEntry 5 }

bsciSubscrOperAutocallMaxRtry OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Maximum number of times an autocall will be sent."
        ::= { bsciSubscrOperEntry 6 }

bsciSubscrOperConnectionID OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Identifier that will link the BSCI port with a device
                                configured in the BSCI Devices Table."
        ::= { bsciSubscrOperEntry 7 }

--
-- BSC Interactive Device Administrative Table
--

bsciDevAdminTable OBJECT-TYPE
        SYNTAX SEQUENCE OF BsciDevAdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A list of BSC Interactive devices."
        ::= { portBsciGroup 5 }

bsciDevAdminEntry OBJECT-TYPE
        SYNTAX BsciDevAdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A BSCI Interactive Device entry containing objects
                        relating to the device that are configurable by the user."
        INDEX { nlIfRlp, nlIfPort, bsciDevAdminControlUnitID,
                        bsciDevAdminDeviceUnitID }
        ::= { bsciDevAdminTable 1 }

BsciDevAdminEntry ::=
        SEQUENCE {
                bsciDevAdminControlUnitID                       INTEGER,
                bsciDevAdminDeviceUnitID                        INTEGER,
                bsciDevAdminConnectionID                        INTEGER,
                bsciDevAdminSingleUserVC                        INTEGER,
                bsciDevAdminTransTextSupported          INTEGER,
                bsciDevAdminPrinterAttached                     INTEGER,
                bsciDevAdminRowStatus                           RowStatus,
                bsciDevAdminDisableStatusRequest                INTEGER
        }

bsciDevAdminControlUnitID OBJECT-TYPE
        SYNTAX  INTEGER (0..31)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Control Unit identifier."
        ::= { bsciDevAdminEntry 1 }

bsciDevAdminDeviceUnitID OBJECT-TYPE
        SYNTAX  INTEGER (0..31)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Device Unit identifier."
        ::= { bsciDevAdminEntry 2 }

bsciDevAdminConnectionID OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The BSCI port connection ID for the device."
        DEFVAL { 0 }
        ::= { bsciDevAdminEntry 3 }

bsciDevAdminSingleUserVC OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies whether each end of the connection is within
                                a same Control Unit/Device Type pair."
        DEFVAL { no }
        ::= { bsciDevAdminEntry 4 }

bsciDevAdminTransTextSupported OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Causes all characters transmitted to be treated as data."
        DEFVAL { no }
        ::= { bsciDevAdminEntry 5 }

bsciDevAdminPrinterAttached OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies whether the device has a printer attached."
        DEFVAL { no }
        ::= { bsciDevAdminEntry 6 }

bsciDevAdminRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the bsciDevAdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { bsciDevAdminEntry 7 }

bsciDevAdminDisableStatusRequest OBJECT-TYPE
        SYNTAX INTEGER {
                        normal (1),
                        none (2),
                        always-active (3)
                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines how the BSCI port will report the status
                     of the attached device.  Normal status- the port will
                     report what the device reports.  No status- the port will
                     report status only if the device is active.  Always active
                     status- the port will always report the device as active."
        DEFVAL { normal }
        ::= { bsciDevAdminEntry 8 }

--
-- BSC Interactive Device Operational Table
--

bsciDevOperTable OBJECT-TYPE
        SYNTAX SEQUENCE OF BsciDevOperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A list of BSC Interactive devices."
        ::= { portBsciGroup 6 }

bsciDevOperEntry OBJECT-TYPE
        SYNTAX BsciDevOperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION
                        "A BSCI Interactive Device entry containing objects
                        relating to the device that are configurable by the user."
        INDEX { nlIfRlp, nlIfPort, bsciDevOperControlUnitID,
                        bsciDevOperDeviceUnitID }
        ::= { bsciDevOperTable 1 }

BsciDevOperEntry ::=
        SEQUENCE {
                bsciDevOperControlUnitID                        INTEGER,
                bsciDevOperDeviceUnitID                         INTEGER,
                bsciDevOperConnectionID                         INTEGER,
                bsciDevOperSingleUserVC                         INTEGER,
                bsciDevOperTransTextSupported           INTEGER,
                bsciDevOperPrinterAttached                      INTEGER,
                bsciDevOperDisableStatusRequest                 INTEGER
        }

bsciDevOperControlUnitID OBJECT-TYPE
        SYNTAX  INTEGER (0..31)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Control Unit identifier."
        ::= { bsciDevOperEntry 1 }

bsciDevOperDeviceUnitID OBJECT-TYPE
        SYNTAX  INTEGER (0..31)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Device Unit identifier."
        ::= { bsciDevOperEntry 2 }

bsciDevOperConnectionID OBJECT-TYPE
        SYNTAX  INTEGER (0..255)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The BSCI port connection ID for the device."
        ::= { bsciDevOperEntry 3 }

bsciDevOperSingleUserVC OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies whether each end of the connection is within
                                a same Control Unit/Device Type pair."
        ::= { bsciDevOperEntry 4 }

bsciDevOperTransTextSupported OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Causes all characters transmitted to be treated as data."
        ::= { bsciDevOperEntry 5 }

bsciDevOperPrinterAttached OBJECT-TYPE
        SYNTAX  INTEGER {
                                no(1),
                                yes(2)
                                }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies whether the device has a printer attached."
        ::= { bsciDevOperEntry 6 }

bsciDevOperDisableStatusRequest OBJECT-TYPE
        SYNTAX INTEGER {
                        normal (1),
                        none (2),
                        always-active (3)
                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Determines how the BSCI port will report the status
                     of the attached device.  Normal status- the port will
                     report what the device reports.  No status- the port will
                     report status only if the device is active.  Always active
                     status- the port will always report the device as active."
        ::= { bsciDevOperEntry 7 }

portSdlcGroup OBJECT IDENTIFIER ::=  { port 5 }

portSdlcAdminTable  OBJECT-TYPE
                    SYNTAX      SEQUENCE OF PortSdlcAdminEntry
                    ACCESS      not-accessible
                    STATUS      mandatory
                    DESCRIPTION
                            "This table contains Netlink Enterprise specific
                            objects to manage SDLC port. Changing on of the
                            these parameters may take effect in the operating
                            port immediately or may wait until the interface is                             restarted depending on the details of the 
                            implementation.

                            Most of the objects in this read-write table have 
                            corresponding read-only objects in the 
                            portSdlcOperTable that return the current 
                            operating value.

                            The operating values may be different from these 
                            configured values if a configured parameter was 
                            configured afterthe interface was started."
                    ::= { portSdlcGroup 1 }

portSdlcAdminEntry  OBJECT-TYPE
                    SYNTAX      PortSdlcAdminEntry
                    ACCESS      not-accessible
                    STATUS      mandatory
                    DESCRIPTION
                            "A list of configured values for an SDLC port."
                    INDEX   { nlIfRlp, nlIfPort }
                    ::= { portSdlcAdminTable 1 }

PortSdlcAdminEntry  ::= SEQUENCE
{
        portSdlcAdminCommit         INTEGER,
        portSdlcAdminMAXRetries     INTEGER,
        portSdlcAdminMAXOut         INTEGER,
        portSdlcAdminPadType        INTEGER,
        portSdlcAdminGenerateClock INTEGER,
        portSdlcAdminRcvClockFromDTE INTEGER,
        portSdlcAdminNrz INTEGER,
        portSdlcAdminPacketSize INTEGER,
        portSdlcAdminDisableRequestDisconnect INTEGER,
        portSdlcAdminLPDASupport INTEGER,
        portSdlcAdminConnector   INTEGER,
        portSdlcAdminSpeed       INTEGER,
                portSdlcAdminRowStatus   RowStatus,
        portSdlcAdminIdleFillChar    INTEGER,
        portSdlcAdminInactivityTimer INTEGER,
        portSdlcAdminL1Duplex        INTEGER
}

portSdlcAdminCommit      OBJECT-TYPE
                         SYNTAX      INTEGER
                         ACCESS      read-write
                         STATUS      obsolete
                         DESCRIPTION
                             "Writing a value to this object commits the
                             the SDLC port related modified configuration
                             values to the database."
                         DEFVAL { 0 }
                         ::= { portSdlcAdminEntry 1 }

portSdlcAdminMAXRetries  OBJECT-TYPE
                         SYNTAX      INTEGER (0..99)
                         ACCESS      read-write
                         STATUS      mandatory
                         DESCRIPTION
                             "This object defines the max. number of retries
                             to a non-responding Link station, before putting
                             the Link station to slow-poll list if it is not
                             Normal response Mode OR disconnecting the link 
                             station if it is data txfr state." 

                         DEFVAL { 5 }
                         ::= { portSdlcAdminEntry 2 }

portSdlcAdminMAXOut      OBJECT-TYPE
                         SYNTAX      INTEGER  (1..7)
                         ACCESS      read-write
                         STATUS      mandatory
                         DESCRIPTION
                             "This object defines the number of outstanding 
                             frames for triggering window full condition."

                         DEFVAL { 7 }
                         ::= { portSdlcAdminEntry 3 }

portSdlcAdminPadType      OBJECT-TYPE
                                    SYNTAX      INTEGER
                                    {
                                        xpad (1),
                                        tpad (2),
                                        hpad (3),
                                        npad (4)
                                    }
                                    ACCESS      read-write
                                    STATUS      mandatory
                                    DESCRIPTION
                                        "This object defines the SNA
                                         PAD types."
                                    DEFVAL { tpad }
                                    ::= { portSdlcAdminEntry 4 }

portSdlcAdminGenerateClock      OBJECT-TYPE
                                SYNTAX      INTEGER
                                {
                                        no (1),
                                        yes (2)
                                }
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION
                                    "This object defines if the port would
                                     generate clock."

                                DEFVAL { yes }
                                ::= { portSdlcAdminEntry 5 }

portSdlcAdminRcvClockFromDTE    OBJECT-TYPE
                                SYNTAX      INTEGER
                                {
                                        no (1),
                                        yes (2)
                                }
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION
                                    "This object defines if the rcv clock will
                                     be used from DTE."

                                DEFVAL { no }
                                ::= { portSdlcAdminEntry 6 }

portSdlcAdminNrz                OBJECT-TYPE
                                SYNTAX      INTEGER
                                {
                                        no (1),
                                        yes (2)
                                }
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION
                                    "This object defines the data encoding
                                     at the physical layer"

                                DEFVAL { yes }
                                ::= { portSdlcAdminEntry 7 }

portSdlcAdminPacketSize         OBJECT-TYPE
                                SYNTAX      INTEGER (16..4096)
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION
                                    "This object defines the packet size of the
                                     X25 layer used by SNA PAD"

                                DEFVAL { 1024 }
                                ::= { portSdlcAdminEntry 8 }

portSdlcAdminDisableRequestDisconnect      OBJECT-TYPE
                                           SYNTAX      INTEGER
                                           {
                                                no (1),
                                                yes (2)
                                           }
                                           ACCESS      read-write
                                           STATUS      mandatory
                                           DESCRIPTION
                                    "This object defines if a Request To  
                                    Disconnect(RD) will be sent when remote
                                    PAD clear the connection"

                                           DEFVAL { no }
                                           ::= { portSdlcAdminEntry 9 }

portSdlcAdminLPDASupport     OBJECT-TYPE
                             SYNTAX      INTEGER
                             {  
                                        none (1),
                                        lpda-1 (2),
                                        lpda-2 (3)
                             }
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                    "This object defines the type LPDA support
                                     on SDLC port."

                             DEFVAL { none }
                             ::= { portSdlcAdminEntry 10 }

portSdlcAdminConnector     OBJECT-TYPE
                             SYNTAX      INTEGER
                             {  
                                        rs232 (3),
                                                                                v35 (5),
                                                                                rs449 (6),
                                                                                rs530 (7),
                                                                                x21 (8),
                                                                                t1 (10)
                             }
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                    "This object defines the connector type
                                     of the SDLC port."

                             ::= { portSdlcAdminEntry 11 }

portSdlcAdminSpeed     OBJECT-TYPE
                       SYNTAX      INTEGER (75..2048000)
                       ACCESS      read-write
                       STATUS      mandatory
                       DESCRIPTION
                        "This object defines the speed of the SDLC port.  The speed may
                         only be set to one of a series of reasonable values, and if an attempt is made 
                         to set the speed to a value which is within the valid range but not equal to one 
                         of these values, the speed will be rounded up.  If the connector type of the port 
                         is RS232, the port could be a standard port or a high speed port.  If the port is 
                         a high speed RS232 port, the maximum valid speed is 256000.  If the port is a standard 
                         RS232 port, the maximum valid speed is 64000 on the FRX4000/SS1840 and 19200
                         on all other products.  It may be possible to set the speed of a standard RS232 port 
                         to a speed which is valid for a high speed RS232 port but invalid for a standard 
                         RS232 port. In this case, the port may not end up having the invalid speed.  The default
                         speed for a standard RS232 port on the FRX6000 is 19200."
                         DEFVAL { 64000 }
                             ::= { portSdlcAdminEntry 12 }

portSdlcAdminRowStatus     OBJECT-TYPE
                             SYNTAX      RowStatus
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portSdlcAdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device, and which is
                supplied by a management station wishing to exercise an
                on-line update of the existing conceptual row.  For a
                management protocol set operation, a genErr response is
                returned when the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."

                             ::= { portSdlcAdminEntry 13 }

portSdlcAdminIdleFillChar     OBJECT-TYPE
                              SYNTAX      INTEGER
                              {
                                  hex-ff (1),
                                  hex-7e (2)
                              }
                              ACCESS      read-write
                              STATUS      mandatory
                              DESCRIPTION
                                  "This object specifies a character that
                                   wll be inserted into the stream when the
                                   SNA link is idle."
                              DEFVAL { hex-ff }
                              ::= { portSdlcAdminEntry 14 }

portSdlcAdminInactivityTimer  OBJECT-TYPE
                              SYNTAX      INTEGER (15..250)
                              ACCESS      read-write
                              STATUS      mandatory
                              DESCRIPTION
                                  "This object determines how long the node
                                   will wait with no activity on the port
                                   before it will declare the attached device
                                   down."
                              DEFVAL { 50 }
                              ::= { portSdlcAdminEntry 15 }

portSdlcAdminL1Duplex         OBJECT-TYPE
                              SYNTAX      INTEGER
                              {
                                  full-duplex (1),
                                  half-duplex (2)
                              }
                              ACCESS      read-write
                              STATUS      mandatory
                              DESCRIPTION
                                  "This object determines whether level-1
                                   (physical layer) transmission can be in
                                   one (half duplex) or both (full duplex)
                                   directions at once."
                              DEFVAL { full-duplex }
                              ::= { portSdlcAdminEntry 16 }

portSdlcOperTable  OBJECT-TYPE
                   SYNTAX      SEQUENCE OF PortSdlcOperEntry
                   ACCESS      not-accessible
                   STATUS      mandatory
                   DESCRIPTION
                       "This table contains current Netlink enterprise specific
                       port parameters"

                    ::= { portSdlcGroup 2 }

portSdlcOperEntry  OBJECT-TYPE
                   SYNTAX      PortSdlcOperEntry
                   ACCESS      not-accessible
                   STATUS      mandatory
                   DESCRIPTION
                            "A list of operational values for an SDLC port."

                   INDEX   { nlIfRlp, nlIfPort }
                   ::= { portSdlcOperTable 1 }

PortSdlcOperEntry  ::= SEQUENCE
{
        portSdlcOperCommit         INTEGER,
        portSdlcOperMAXRetries     INTEGER,
        portSdlcOperMAXOut         INTEGER,
        portSdlcOperPadType        INTEGER,
        portSdlcOperGenerateClock INTEGER,
        portSdlcOperRcvClockFromDTE INTEGER,
        portSdlcOperNrz INTEGER,
        portSdlcOperPacketSize INTEGER,
        portSdlcOperDisableRequestDisconnect INTEGER,
        portSdlcOperLPDASupport INTEGER,
        portSdlcOperConnector   INTEGER,
        portSdlcOperSpeed       INTEGER,
        portSdlcOperIdleFillChar    INTEGER,
        portSdlcOperInactivityTimer INTEGER,
        portSdlcOperL1Duplex        INTEGER
}

portSdlcOperCommit      OBJECT-TYPE
                        SYNTAX      INTEGER
                        ACCESS      read-only
                        STATUS      obsolete
                        DESCRIPTION
                             "This object is not used."
                        ::= { portSdlcOperEntry 1 }

portSdlcOperMAXRetries  OBJECT-TYPE
                        SYNTAX      INTEGER (0..99)
                        ACCESS      read-only
                        STATUS      mandatory
                        DESCRIPTION
                             "This object defines the max. number of retries
                             to a non-responding Link station, before putting
                             the Link station to slow-poll list if it is not
                             Normal response Mode OR disconnecting the link 
                             station if it is data txfr state." 
                        ::= { portSdlcOperEntry 2 }

portSdlcOperMAXOut      OBJECT-TYPE
                        SYNTAX      INTEGER (1..7)
                        ACCESS      read-only
                        STATUS      mandatory
                        DESCRIPTION
                             "This object defines the number of outstanding 
                             frames for triggering window full condition."

                        ::= { portSdlcOperEntry 3 }

portSdlcOperPadType      OBJECT-TYPE
                                   SYNTAX      INTEGER
                                   {
                                       xpad (1),
                                       tpad (2),
                                       hpad (3),
                                       npad (4)
                                   }
                                   ACCESS      read-only
                                   STATUS      mandatory
                                   DESCRIPTION
                                       "This object defines the SNA
                                       PAD type"

                                   ::= { portSdlcOperEntry 4 }

portSdlcOperGenerateClock      OBJECT-TYPE
                               SYNTAX      INTEGER
                               {
                                       no (1),
                                       yes (2)
                               }
                               ACCESS      read-only
                               STATUS      mandatory
                               DESCRIPTION
                                    "This object defines if the port would
                                     generate clock."
                               ::= { portSdlcOperEntry 5 }

portSdlcOperRcvClockFromDTE    OBJECT-TYPE
                               SYNTAX      INTEGER
                               {
                                       no (1),
                                       yes (2)
                               }
                               ACCESS      read-only
                               STATUS      mandatory
                               DESCRIPTION
                                    "This object defines if the rcv clock will
                                     be used from DTE."
                               ::= { portSdlcOperEntry 6 }

portSdlcOperNrz                OBJECT-TYPE
                               SYNTAX      INTEGER
                               {
                                       no (1),
                                       yes (2)
                               }
                               ACCESS      read-only
                               STATUS      mandatory
                               DESCRIPTION
                                    "This object defines the data encoding
                                    at the physical layer"
                               ::= { portSdlcOperEntry 7 }

portSdlcOperPacketSize         OBJECT-TYPE
                               SYNTAX      INTEGER (16..4096)
                               ACCESS      read-only
                               STATUS      mandatory
                               DESCRIPTION
                                    "This object defines the packet size of the
                                     X25 layer used by SNA PAD"

                               ::= { portSdlcOperEntry 8 }

portSdlcOperDisableRequestDisconnect      OBJECT-TYPE
                                          SYNTAX      INTEGER
                                          {
                                                 no (1),
                                                 yes (2)
                                          }
                                          ACCESS      read-only
                                          STATUS      mandatory
                                          DESCRIPTION
                                    "This object defines if a Request To  
                                    Disconnect(RD) will be sent when remote
                                    PAD clear the connection"
                                          ::= { portSdlcOperEntry 9 }

portSdlcOperLPDASupport     OBJECT-TYPE
                            SYNTAX      INTEGER
                            {  
                                       none (1),
                                       lpda-1 (2),
                                       lpda-2 (3)
                            }
                            ACCESS      read-only
                            STATUS      mandatory
                            DESCRIPTION
                                    "This object defines the type LPDA support
                                     on SDLC port."
                            ::= { portSdlcOperEntry 10 }

portSdlcOperConnector     OBJECT-TYPE
                             SYNTAX      INTEGER
                             {  
                                        rs232 (3),
                                        v35 (5),
                                        rs449 (6),
                                                                                rs530 (7),
                                                                                x21 (8),
                                                                                t1 (10)
                             }
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                    "This object defines the operational
                                                                        connector type of the SDLC port."

                             ::= { portSdlcOperEntry 11 }

portSdlcOperSpeed     OBJECT-TYPE
                             SYNTAX      INTEGER
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                    "This object defines the operational speed
                                     of the SDLC port."

                             ::= { portSdlcOperEntry 12 }

portSdlcOperIdleFillChar      OBJECT-TYPE
                              SYNTAX      INTEGER
                              {
                                  hex-ff (1),
                                  hex-7e (2)
                              }
                              ACCESS      read-only
                              STATUS      mandatory
                              DESCRIPTION
                                  "This object specifies a character that
                                   wll be inserted into the stream when the
                                   SNA link is idle."
                              ::= { portSdlcOperEntry 13 }

portSdlcOperInactivityTimer   OBJECT-TYPE
                              SYNTAX      INTEGER (15..250)
                              ACCESS      read-only
                              STATUS      mandatory
                              DESCRIPTION
                                  "This object determines how long the node
                                   will wait with no activity on the port
                                   before it will declare the attached device
                                   down."
                              ::= { portSdlcOperEntry 14 }

portSdlcOperL1Duplex          OBJECT-TYPE
                              SYNTAX      INTEGER
                              {
                                  full-duplex (1),
                                  half-duplex (2)
                              }
                              ACCESS      read-only
                              STATUS      mandatory
                              DESCRIPTION
                                  "This object determines whether level-1
                                   (physical layer) transmission can be in
                                   one (half duplex) or both (full duplex)
                                   directions at once."
                              ::= { portSdlcOperEntry 15 }

-- The lSSdlcAdminTable contains information about the PUs configured on
-- an SDLC port. Note that deleting of a PU entry does not affect the
-- existence of the PU for the running protocol. The PU record is removed
-- from the database file, but will remain known to the node until it is
-- rebooted or until an online update of the port is performed. This is
-- consistent with the way PU information is handled when configuring
-- through the user interface menu system. 

lSSdlcAdminTable  OBJECT-TYPE
                  SYNTAX      SEQUENCE OF LSSdlcAdminEntry
                  ACCESS      not-accessible
                  STATUS      mandatory
                  DESCRIPTION
                      "This table contains Enterprise specific Link station
                      configurable parameters to manage the link stations."

                  ::= { portSdlcGroup 3 }

lSSdlcAdminEntry  OBJECT-TYPE
                  SYNTAX      LSSdlcAdminEntry
                  ACCESS      not-accessible
                  STATUS      mandatory
                  DESCRIPTION
                      "A list of configured values for an SDLC port."

                  INDEX   { nlIfRlp, nlIfPort, sdlcLSAddress }
                  ::= { lSSdlcAdminTable 1 }

LSSdlcAdminEntry  ::= SEQUENCE
{
        lSSdlcAdminLocalSub         NlSubscriberAddress,
        lSSdlcAdminRemoteSub        NlSubscriberAddress,
        lSSdlcAdminAutoCall         INTEGER,
        lSSdlcAdminRetryTime        INTEGER,
        lSSdlcAdminRetryCount       INTEGER,
        lSSdlcAdminLlc2Conversion   INTEGER,
        lSSdlcAdminLPDAResourceID   INTEGER,
                lSSdlcAdminRowStatus            RowStatus,
        lSSdlcAdminL2DatMode        INTEGER
}

lSSdlcAdminLocalSub      OBJECT-TYPE
                         SYNTAX      NlSubscriberAddress
                         ACCESS      read-write
                         STATUS      mandatory
                         DESCRIPTION
                             "This object defines the local subscriber ID
                             of the Link Station"

                         ::= { lSSdlcAdminEntry 1 }

lSSdlcAdminRemoteSub      OBJECT-TYPE
                          SYNTAX      NlSubscriberAddress
                          ACCESS      read-write
                          STATUS      mandatory
                          DESCRIPTION
                             "This object defines the remote subscriber ID
                             used to connect to remote Link Station"
                          ::= { lSSdlcAdminEntry 2 }

lSSdlcAdminAutoCall       OBJECT-TYPE
                          SYNTAX      INTEGER
                          {
                                no (1),
                                yes (2)
                          }
                          ACCESS      read-write
                          STATUS      mandatory
                          DESCRIPTION
                              "This object defines if auto call is enabled for
                              the link station. If enabled, the link station
                              will initiate connection establishment, when
                              appropriate. Else, it will passively listen to
                              the connection request for establish a connection
                              with the remote PAD"

                          DEFVAL { no }
                          ::= { lSSdlcAdminEntry 3 }

lSSdlcAdminRetryTime      OBJECT-TYPE
                          SYNTAX      INTEGER (15..225)
                          ACCESS      read-write
                          STATUS      mandatory
                          DESCRIPTION
                              "This object is used, only when 
                              lSSdlcAdminAutoCall object is yes. This defines
                              the time interval measured in seconds in which
                              the connection request is retried"

                          DEFVAL { 60 }
                          ::= { lSSdlcAdminEntry 4 }

lSSdlcAdminRetryCount     OBJECT-TYPE
                          SYNTAX      INTEGER (0..255)
                          ACCESS      read-write
                          STATUS      mandatory
                          DESCRIPTION
                              "This object is used, only when 
                              lSSdlcAdminAutoCall object is yes. This defines
                              the number of times the connection initiation
                              is retried before given up. The value of Zero(0)
                              means to try indefinitely"

                          DEFVAL { 0 }
                          ::= { lSSdlcAdminEntry 5 }

lSSdlcAdminLlc2Conversion   OBJECT-TYPE
                            SYNTAX      INTEGER
                            {
                                no (1),
                                yes (2)
                            }
                            ACCESS      read-write
                            STATUS      mandatory
                            DESCRIPTION
                                "This object defines if this link station 
                                connects to a LLC2 device/host."

                            DEFVAL { no }
                            ::= { lSSdlcAdminEntry 6 }

lSSdlcAdminLPDAResourceID       OBJECT-TYPE
                                SYNTAX      INTEGER (0..255)
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION
                                    "This objects the resource ID used during
                                     LPDA command support"

                                DEFVAL { 0 }
                                ::= { lSSdlcAdminEntry 7 }

lSSdlcAdminRowStatus                    OBJECT-TYPE
                                                                SYNTAX      RowStatus
                                                                ACCESS      read-write
                                                                STATUS      mandatory
                                DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the lSSdlcAdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned.

            Also note that deleting a PU entry will only remove it from
            the database file, and it's existence will still be known by
            the protocol until the node is rebooted or until an online
            update of the port is performed."

                                                                ::= { lSSdlcAdminEntry 8 }

lSSdlcAdminL2DatMode      OBJECT-TYPE
                          SYNTAX      INTEGER
                          {
                                two-way-alternate (1),
                                two-way-simultaneous (2)
                          }
                          ACCESS      read-write
                          STATUS      mandatory
                          DESCRIPTION
                              "This object determines whether transmission
                               can be in one (alternate) or two (simultaneous)
                               directions at the same time."
                          DEFVAL { two-way-alternate }
                          ::= { lSSdlcAdminEntry 9 }

lSSdlcOperTable  OBJECT-TYPE
                 SYNTAX      SEQUENCE OF LSSdlcOperEntry
                 ACCESS      not-accessible
                 STATUS      mandatory
                 DESCRIPTION
                     "This table contains the operational parameters of the
                     SDLC port"
                 ::= { portSdlcGroup 4 }

lSSdlcOperEntry  OBJECT-TYPE
                 SYNTAX      LSSdlcOperEntry
                 ACCESS      not-accessible
                 STATUS      mandatory
                 DESCRIPTION
                      "A list of configured values for an SDLC port."
                 INDEX   { nlIfRlp, nlIfPort, sdlcLSAddress }
                 ::= { lSSdlcOperTable 1 }

LSSdlcOperEntry  ::= SEQUENCE
{
        lSSdlcOperLocalSub         NlSubscriberAddress,
        lSSdlcOperRemoteSub        NlSubscriberAddress,
        lSSdlcOperAutoCall         INTEGER,
        lSSdlcOperRetryTime        INTEGER,
        lSSdlcOperRetryCount       INTEGER,
        lSSdlcOperLlc2Conversion   INTEGER,
        lSSdlcOperLPDAResourceID   INTEGER,
        lSSdlcOperL2DatMode        INTEGER
}

lSSdlcOperLocalSub      OBJECT-TYPE
                        SYNTAX      NlSubscriberAddress
                        ACCESS      read-only
                        STATUS      mandatory
                        DESCRIPTION
                             "This object defines the local subscriber ID
                             of the Link Station"
                        ::= { lSSdlcOperEntry 1 }

lSSdlcOperRemoteSub      OBJECT-TYPE
                         SYNTAX      NlSubscriberAddress
                         ACCESS      read-only
                         STATUS      mandatory
                         DESCRIPTION
                             "This object defines the remote subscriber ID
                             used to connect to remote Link Station"
                         ::= { lSSdlcOperEntry 2 }

lSSdlcOperAutoCall       OBJECT-TYPE
                         SYNTAX      INTEGER
                         {
                               no (1),
                               yes (2)
                         }
                         ACCESS      read-only
                         STATUS      mandatory
                         DESCRIPTION
                              "This object defines if auto call is enabled for
                              the link station. If enabled, the link station
                              will initiate connection establishment, when
                              appropriate. Else, it will passively listen to
                              the connection request for establish a connection
                              with the remote PAD"
                         ::= { lSSdlcOperEntry 3 }

lSSdlcOperRetryTime      OBJECT-TYPE
                         SYNTAX      INTEGER (15..225)
                         ACCESS      read-only
                         STATUS      mandatory
                         DESCRIPTION
                              "This object is valid, only when 
                              lSSdlcAdminAutoCall object is yes. This defines
                              the time interval measured in seconds in which
                              the connection request is retried"
                         ::= { lSSdlcOperEntry 4 }

lSSdlcOperRetryCount     OBJECT-TYPE
                         SYNTAX      INTEGER (0..255)
                         ACCESS      read-only
                         STATUS      mandatory
                         DESCRIPTION
                              "This object is used, only when 
                              lSSdlcAdminAutoCall object is yes. This defines
                              the number of times the connection initiation
                              is retried before given up. The value of Zero(0)
                              means to try indefinitely"
                         ::= { lSSdlcOperEntry 5 }

lSSdlcOperLlc2Conversion   OBJECT-TYPE
                           SYNTAX      INTEGER
                           {
                               no (1),
                               yes (2)
                           }
                           ACCESS      read-only
                           STATUS      mandatory
                           DESCRIPTION
                                "This object defines if this link station 
                                connects to a LLC2 device/host."
                           ::= { lSSdlcOperEntry 6 }

lSSdlcOperLPDAResourceID       OBJECT-TYPE
                               SYNTAX      INTEGER (0..255)
                               ACCESS      read-only
                               STATUS      mandatory
                               DESCRIPTION
                                    "This objects the resource ID used during
                                     LPDA command support"
                               ::= { lSSdlcOperEntry 7 }

lSSdlcOperL2DatMode       OBJECT-TYPE
                          SYNTAX      INTEGER
                          {
                                two-way-alternate (1),
                                two-way-simultaneous (2)
                          }
                          ACCESS      read-only
                          STATUS      mandatory
                          DESCRIPTION
                              "This object determines whether transmission
                               can be in one (alternate) or two (simultaneous)
                               directions at the same time."
                          ::= { lSSdlcOperEntry 8 }

lSSdlcLlc2AdminTable  OBJECT-TYPE
                      SYNTAX      SEQUENCE OF LSSdlcLlc2AdminEntry
                      ACCESS      not-accessible
                      STATUS      mandatory
                      DESCRIPTION
                          "This table contains the LLC2 related parameters
                          used to configure LLC2 session, when the SDLC 
                          station is connected to a LLC2 device at the remote
                          end"
                     ::= { portSdlcGroup 5 }

lSSdlcLlc2AdminEntry  OBJECT-TYPE
                      SYNTAX      LSSdlcLlc2AdminEntry
                      ACCESS      not-accessible
                      STATUS      mandatory
                      DESCRIPTION
                          "A list of configured values for an SDLC port."
                      INDEX   { nlIfRlp, nlIfPort, sdlcLSAddress }
                      ::= { lSSdlcLlc2AdminTable 1 }

-- The lSSdlcLlc2AdminTable contains information about the PUs configured
-- on an SDLC port. Note that deleting of a PU entry does not affect the
-- existence of the PU for the running protocol. The PU record is removed
-- from the database file, but will remain known to the node until it is
-- rebooted or until an online update of the port is performed. This is
-- consistent with the way PU information is handled when configuring
-- through the user interface menu system. 

LSSdlcLlc2AdminEntry  ::= SEQUENCE
{
        lSSdlcLlc2AdminLocalSap    INTEGER,
        lSSdlcLlc2AdminLocalMac    PhysAddress,
        lSSdlcLlc2AdminIdblk       INTEGER,
        lSSdlcLlc2AdminIdnum       INTEGER,
        lSSdlcLlc2AdminLanTi       INTEGER,
        lSSdlcLlc2AdminLanT1       INTEGER,
        lSSdlcLlc2AdminLanT2       INTEGER,
        lSSdlcLlc2AdminLanN2       INTEGER,
        lSSdlcLlc2AdminLanN3       INTEGER,
        lSSdlcLlc2AdminLanTw       INTEGER,
        lSSdlcLlc2AdminBAG         INTEGER,
        lSSdlcLlc2AdminPriority    INTEGER,
                lSSdlcLlc2AdminRowStatus        RowStatus,
        lSSdlcLlc2AdminSuppressXID  INTEGER
}

lSSdlcLlc2AdminLocalSap      OBJECT-TYPE
                             SYNTAX      INTEGER (0..252)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Local SAP 
                                 address (multiple of 4)"
                             DEFVAL { 4 }
                             ::= { lSSdlcLlc2AdminEntry 1 }

lSSdlcLlc2AdminLocalMac      OBJECT-TYPE
                             SYNTAX      PhysAddress
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines the local MAC address"
                             DEFVAL { '000000000000'H }    -- 00:00:00:00:00:00
                             ::= { lSSdlcLlc2AdminEntry 2 }

lSSdlcLlc2AdminIdblk         OBJECT-TYPE
                             SYNTAX      INTEGER (0..4095)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines idblk used in XID"
                             DEFVAL { 0 }
                             ::= { lSSdlcLlc2AdminEntry 3 }

lSSdlcLlc2AdminIdnum         OBJECT-TYPE
                             SYNTAX      INTEGER (0..1048575)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines idnum used in XID"
                             DEFVAL { 0 }
                             ::= { lSSdlcLlc2AdminEntry 4 }

lSSdlcLlc2AdminLanTi         OBJECT-TYPE
                             SYNTAX      INTEGER (1..50)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines LLC2 inactivity timer
                                  measured in units of seconds"
                             DEFVAL { 30 }
                             ::= { lSSdlcLlc2AdminEntry 5 }

lSSdlcLlc2AdminLanT1         OBJECT-TYPE
                             SYNTAX      INTEGER (1..250)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines LLC2 reply timer
                                  measured in units of 100 milliseconds"
                             DEFVAL { 10 }
                             ::= { lSSdlcLlc2AdminEntry 6 }

lSSdlcLlc2AdminLanT2         OBJECT-TYPE
                             SYNTAX      INTEGER (100..5000)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Receiver Ack Timer
                                  measured in units of milliseconds"
                             DEFVAL { 100 }
                             ::= { lSSdlcLlc2AdminEntry 7 }

lSSdlcLlc2AdminLanN2         OBJECT-TYPE
                             SYNTAX      INTEGER (0..255)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Maximum Retransmissions"
                             DEFVAL { 8 }
                             ::= { lSSdlcLlc2AdminEntry 8 }

lSSdlcLlc2AdminLanN3         OBJECT-TYPE
                             SYNTAX      INTEGER (1..127)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines count of I-format LPDU's
                                 before sending Ack"

                             DEFVAL { 3 }
                             ::= { lSSdlcLlc2AdminEntry 9 }

lSSdlcLlc2AdminLanTw         OBJECT-TYPE
                             SYNTAX      INTEGER (1..127)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Outstanding Frames"
                             DEFVAL { 7 }
                             ::= { lSSdlcLlc2AdminEntry 10 }

lSSdlcLlc2AdminBAG           OBJECT-TYPE
                             SYNTAX      INTEGER (0..16)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines bandwidth allocation 
                                 group"
                             DEFVAL { 0 }
                             ::= { lSSdlcLlc2AdminEntry 11 }

lSSdlcLlc2AdminPriority      OBJECT-TYPE
                             SYNTAX      INTEGER (0..9)
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines priority for traffic 
                                 within the node"
                             DEFVAL { 0 }
                             ::= { lSSdlcLlc2AdminEntry 12 }

lSSdlcLlc2AdminRowStatus        OBJECT-TYPE
                                                        SYNTAX      RowStatus
                                                        ACCESS      read-write
                                                        STATUS      mandatory
                            DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the lSSdlcLlc2AdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned.

            Also note that deleting a PU entry will only remove it from
            the database file, and it's existence will still be known by
            the protocol until the node is rebooted or until an online
            update of the port is performed."
                                                        ::= { lSSdlcLlc2AdminEntry 13 }

lSSdlcLlc2AdminSuppressXID   OBJECT-TYPE
                             SYNTAX      INTEGER
                             {
                                 no (1),
                                 yes (2)
                             }
                             ACCESS      read-write
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object prevents (if yes) the returning
                                  of an XID in response to a null XID. This
                                  might be desirable if the remote TPAD is not
                                  running PU 2.1. It should be noted that even
                                  if an XID is sent, an SNRM (Set Normal
                                  Response Mode) immediately follows, so the
                                  connection will be established."
                             DEFVAL { no }
                             ::= { lSSdlcLlc2AdminEntry 14 }

lSSdlcLlc2OperTable  OBJECT-TYPE
                     SYNTAX      SEQUENCE OF LSSdlcLlc2OperEntry
                     ACCESS      not-accessible
                     STATUS      mandatory
                     DESCRIPTION
                         "This table contains operartional parameters related
                         to LLC2 session of this link station."
                     ::= { portSdlcGroup 6 }

lSSdlcLlc2OperEntry  OBJECT-TYPE
                     SYNTAX      LSSdlcLlc2OperEntry
                     ACCESS      not-accessible
                     STATUS      mandatory
                     DESCRIPTION
                          "A list of configured values for an SDLC port."
                     INDEX   { nlIfRlp, nlIfPort, sdlcLSAddress }
                     ::= { lSSdlcLlc2OperTable 1 }

LSSdlcLlc2OperEntry  ::= SEQUENCE
{
        lSSdlcLlc2OperLocalSap     INTEGER,
        lSSdlcLlc2OperLocalMac     PhysAddress,
        lSSdlcLlc2OperIdblk        INTEGER,
        lSSdlcLlc2OperIdnum        INTEGER,
        lSSdlcLlc2OperLanTi        INTEGER,
        lSSdlcLlc2OperLanT1        INTEGER,
        lSSdlcLlc2OperLanT2        INTEGER,
        lSSdlcLlc2OperLanN2        INTEGER,
        lSSdlcLlc2OperLanN3        INTEGER,
        lSSdlcLlc2OperLanTw        INTEGER,
        lSSdlcLlc2OperBAG          INTEGER,
        lSSdlcLlc2OperPriority     INTEGER,
        lSSdlcLlc2OperSuppressXID  INTEGER
}

lSSdlcLlc2OperLocalSap       OBJECT-TYPE
                             SYNTAX      INTEGER (0..252)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Local SAP 
                                 address (multiple of 4)"
                             ::= { lSSdlcLlc2OperEntry 1 }

lSSdlcLlc2OperLocalMac       OBJECT-TYPE
                             SYNTAX      PhysAddress
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines the local MAC address"
                             ::= { lSSdlcLlc2OperEntry 2 }

lSSdlcLlc2OperIdblk          OBJECT-TYPE
                             SYNTAX      INTEGER (0..4095)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines idblk used in XID"
                             ::= { lSSdlcLlc2OperEntry 3 }

lSSdlcLlc2OperIdnum          OBJECT-TYPE
                             SYNTAX      INTEGER (0..1048575)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines idnum used in XID"
                             ::= { lSSdlcLlc2OperEntry 4 }

lSSdlcLlc2OperLanTi          OBJECT-TYPE
                             SYNTAX      INTEGER (1..50)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines LLC2 inactivity timer
                                  measured in units of seconds"
                             ::= { lSSdlcLlc2OperEntry 5 }

lSSdlcLlc2OperLanT1          OBJECT-TYPE
                             SYNTAX      INTEGER (1..250)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines LLC2 reply timer
                                  measured in units of 100 milliseconds"
                             ::= { lSSdlcLlc2OperEntry 6 }

lSSdlcLlc2OperLanT2          OBJECT-TYPE
                             SYNTAX      INTEGER (100..5000)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Receiver Ack Timer
                                  measured in units of milliseconds"
                             ::= { lSSdlcLlc2OperEntry 7 }

lSSdlcLlc2OperLanN2          OBJECT-TYPE
                             SYNTAX      INTEGER (0..255)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Maximum Retransmissions"
                             ::= { lSSdlcLlc2OperEntry 8 }

lSSdlcLlc2OperLanN3          OBJECT-TYPE
                             SYNTAX      INTEGER (1..127)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines count of I-format LPDU's
                                 before sending Ack"
                             ::= { lSSdlcLlc2OperEntry 9 }

lSSdlcLlc2OperLanTw          OBJECT-TYPE
                             SYNTAX      INTEGER (1..127)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines Outstanding Frames"
                             ::= { lSSdlcLlc2OperEntry 10 }

lSSdlcLlc2OperBAG            OBJECT-TYPE
                             SYNTAX      INTEGER (0..16)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines bandwidth allocation 
                                 group"
                             ::= { lSSdlcLlc2OperEntry 11 }

lSSdlcLlc2OperPriority       OBJECT-TYPE
                             SYNTAX      INTEGER (0..9)
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object defines priority for traffic 
                                 within the node"
                             ::= { lSSdlcLlc2OperEntry 12 }

lSSdlcLlc2OperSuppressXID    OBJECT-TYPE
                             SYNTAX      INTEGER
                             {
                                 no (1),
                                 yes (2)
                             }
                             ACCESS      read-only
                             STATUS      mandatory
                             DESCRIPTION
                                 "This object prevents (if yes) the returning
                                  of an XID in response to a null XID. This
                                  might be desirable if the remote TPAD is not
                                  running PU 2.1. It should be noted that even
                                  if an XID is sent, an SNRM (Set Normal
                                  Response Mode) immediately follows, so the
                                  connection will be established."
                             ::= { lSSdlcLlc2OperEntry 13 }

portT1Group     OBJECT IDENTIFIER ::=   { port 7 }

portT1AdminTable OBJECT-TYPE
        SYNTAX SEQUENCE OF PortT1AdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "The configuration information pertaining to a T1 port.
        T1 ports can operate at full T1 bandwidth or DS0A channelized which provides
        24 separate channels."
        ::= { portT1Group 1 }

portT1AdminEntry OBJECT-TYPE
        SYNTAX PortT1AdminEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A T1 port entry containing objects relating to T1 ports."
        INDEX { nlIfRlp, nlIfPort }
        ::= { portT1AdminTable 1 }

PortT1AdminEntry ::=
        SEQUENCE {
                portT1AdminBlockedPortFlag      INTEGER,
                portT1AdminGenerateClock                INTEGER,
                portT1AdminFramingMode          INTEGER,
                portT1AdminFrameModelSelect     INTEGER,
                portT1AdminLineEncoding                 INTEGER,
                portT1AdminLineBuildOut                 INTEGER,
                portT1AdminRowStatus                    RowStatus,
                portT1AdminProtocolFraming      INTEGER,
                portT1AdminNRZI                         INTEGER
}

portT1AdminBlockedPortFlag OBJECT-TYPE
        SYNTAX INTEGER  {
                                                no(1),
                                                yes(2)
                                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 1 }

portT1AdminGenerateClock OBJECT-TYPE
        SYNTAX INTEGER  {
                                                no(1),
                                                yes(2)
                                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 2 }

portT1AdminFramingMode OBJECT-TYPE
        SYNTAX INTEGER  {
                                                fullT1(1),
                                                ds0aT1(2)
                                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies how this T1 port is to function. ds0AT1 specifies a
        24 channelized T1."
        ::= { portT1AdminEntry 3 }

portT1AdminFrameModelSelect OBJECT-TYPE
        SYNTAX INTEGER  {
                                                d4(1),
                                                esf(2)
                                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 4 }

portT1AdminLineEncoding OBJECT-TYPE
        SYNTAX INTEGER  {
                                                b8zs(1),
                                                ami(2)
                                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 5 }

portT1AdminLineBuildOut OBJECT-TYPE
        SYNTAX INTEGER  {
                                                zerodb(1),
                                                x133-266ft(2),
                                                x266-399ft(3),
                                                x399-533ft(4),
                                                x533-655ft(5),
                                                minus7p5db(6),
                                                minus15db(7),
                                                minus22p5db(8)
                                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 6 }

portT1AdminRowStatus OBJECT-TYPE
        SYNTAX RowStatus        
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 7 }

portT1AdminProtocolFraming OBJECT-TYPE
        SYNTAX INTEGER  {
                        sync(1),
                        bisync(2)
                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 8 }

portT1AdminNRZI OBJECT-TYPE
        SYNTAX INTEGER  {
                                                no(1),
                                                yes(2)
                                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1AdminEntry 9 }

portT1OperTable OBJECT-TYPE
        SYNTAX SEQUENCE OF PortT1OperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "The configuration information pertaining to a T1 port.
        T1 ports can operate at full T1 bandwidth or DS0A channelized which provides
        24 separate channels."
        ::= { portT1Group 2 }

portT1OperEntry OBJECT-TYPE
        SYNTAX PortT1OperEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A T1 port entry containing objects relating to T1 ports."
        INDEX { nlIfRlp, nlIfPort }
        ::= { portT1OperTable 1 }

PortT1OperEntry ::=
        SEQUENCE {
                portT1OperBlockedPortFlag       INTEGER,
                portT1OperGenerateClock         INTEGER,
                portT1OperFramingMode           INTEGER,
                portT1OperFrameModelSelect      INTEGER,
                portT1OperLineEncoding          INTEGER,
                portT1OperLineBuildOut          INTEGER,
                portT1OperProtocolFraming       INTEGER,
                portT1OperNRZI                          INTEGER
}

portT1OperBlockedPortFlag OBJECT-TYPE
        SYNTAX INTEGER  {
                                                no(1),
                                                yes(2)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1OperEntry 1 }

portT1OperGenerateClock OBJECT-TYPE
        SYNTAX INTEGER  {
                                                no(1),
                                                yes(2)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1OperEntry 2 }

portT1OperFramingMode OBJECT-TYPE
        SYNTAX INTEGER  {
                                                fullT1(1),
                                                ds0aT1(2)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies how this T1 port is to function. ds0AT1 specifies a
        24 channelized T1."
        ::= { portT1OperEntry 3 }

portT1OperFrameModelSelect OBJECT-TYPE
        SYNTAX INTEGER  {
                                                d4(1),
                                                esf(2)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1OperEntry 4 }

portT1OperLineEncoding OBJECT-TYPE
        SYNTAX INTEGER  {
                                                b8zs(1),
                                                ami(2)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1OperEntry 5 }

portT1OperLineBuildOut OBJECT-TYPE
        SYNTAX INTEGER  {
                                                zerodb(1),
                                                x133-266ft(2),
                                                x266-399ft(3),
                                                x399-533ft(4),
                                                x533-655ft(5),
                                                minus7p5db(6),
                                                minus15db(7),
                                                minus22p5db(8)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1OperEntry 6 }

portT1OperProtocolFraming OBJECT-TYPE
        SYNTAX INTEGER  {
                        sync(1),
                        bisync(2)
                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1OperEntry 7 }

portT1OperNRZI OBJECT-TYPE
        SYNTAX INTEGER  {
                                                no(1),
                                                yes(2)
                                        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION ""
        ::= { portT1OperEntry 8 }

portVoiceGroup OBJECT IDENTIFIER ::= { port 8 }

--
-- The Voice Port Administrative table
--

portVoiceAdminTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortVoiceAdminEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A list of Voice ports.  The number of entries
            will be the number of Voice ports on the node."
    ::= { portVoiceGroup 1 }

portVoiceAdminEntry OBJECT-TYPE
    SYNTAX  PortVoiceAdminEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A Voice Port entry containing objects relating
            to the port that are configurable by the user."
    INDEX   { portVoiceAdminRlpIndex, portVoiceAdminPortIndex }
    ::= { portVoiceAdminTable 1 }

PortVoiceAdminEntry ::=
    SEQUENCE {
        portVoiceAdminRlpIndex
            INTEGER,
        portVoiceAdminPortIndex
            INTEGER,
        portVoiceAdminBlockedFlag
            INTEGER,
        portVoiceAdminSpeed
            INTEGER,
        portVoiceAdminDTMF
            INTEGER,
        portVoiceAdminInterface
            INTEGER,
        portVoiceAdminTETimer
            INTEGER,
        portVoiceAdminLevelIn
            INTEGER,
        portVoiceAdminLevelOut
            INTEGER,
        portVoiceAdminCallTimer
            INTEGER,
        portVoiceAdminHuntGroup
            INTEGER,
        portVoiceAdminLongDialPrefix
            OCTET STRING,
        portVoiceAdminSLTTimeout
            INTEGER,
        portVoiceAdminLinkDownBusy
            INTEGER,
        portVoiceAdminFaxSupported
            INTEGER,
        portVoiceAdminTelephonyType
            INTEGER,
        portVoiceAdminJitter
            INTEGER,
        portVoiceAdminSampleDelay
            INTEGER,
        portVoiceAdminDialTimer
            INTEGER,
        portVoiceAdminAutoDial
            INTEGER,
        portVoiceAdminSuppression
            INTEGER,
        portVoiceAdminAutoDialNumber
            OCTET STRING,
        portVoiceAdminAutoPoll
            INTEGER,
        portVoiceAdminAutoPollTimer
            INTEGER,
        portVoiceAdminExtDigitsSource
            INTEGER,
        portVoiceAdminNumDigitsDelete
            INTEGER,
        portVoiceAdminForwardDelay
            INTEGER,
        portVoiceAdminForwardedType
            INTEGER,
        portVoiceAdminForwardedDigits
            INTEGER,
        portVoiceAdminMakeRatio
            INTEGER,
        portVoiceAdminBreakRatio
            INTEGER,
        portVoiceAdminDTMFOnDuration
            INTEGER,
        portVoiceAdminDTMFOffDuration
            INTEGER,
        portVoiceAdminToneType
            INTEGER,
        portVoiceAdminRowStatus
            RowStatus
    }

portVoiceAdminRlpIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The RLP number of the Voice port."
    ::= { portVoiceAdminEntry 1 }

portVoiceAdminPortIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The Port number of the Voice port."
    ::= { portVoiceAdminEntry 2 }

portVoiceAdminBlockedFlag OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The flag which causes the port to be enabled or disabled
            at node IPL. The port will remain in that state until this
            flag is changed and the node is rebooted, or until an on-
            line enable or disable is performed."
    DEFVAL { disabled }
    ::= { portVoiceAdminEntry 3 }

portVoiceAdminSpeed OBJECT-TYPE
    SYNTAX  INTEGER {
                bps-4800 (1),
                bps-8000 (2),
                bps-32000 (3),
                bps-64000 (4)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The speed of the port which is transmitted as part
            of a Call Setup frame. A Voice call will be established
            if there is enough bandwidth at each end to provide the
            minimum configured rate."
    DEFVAL { bps-8000 }
    ::= { portVoiceAdminEntry 4 }

portVoiceAdminDTMF OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The flag to enable, disable, or specify a time span
            over which DTMF (Dual Tone Multi Frequency) tones will
            be regenerated.
            0 =     pass tones transparently to the remote device.
            1 =     detect incoming tones and regenerate as received.
            2-255 = regenerate tones for the specified seconds."
    DEFVAL { 1 }
    ::= { portVoiceAdminEntry 5 }

portVoiceAdminInterface OBJECT-TYPE
    SYNTAX  INTEGER {
                em-4w (1),
                em-2w (2),
                loop-start (3),
                ac15-a (4),
                ac15-b (6),
                em-4w-te (10),
                em-2w-te (11)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The type of interface (in conjunction with the Telephony
            Interface Type) that will be used by the Voice channel.
            This requires rebooting for the change to take effect.
            Telephony Type     Interface Type
            --------------     --------------
            OPX (FXO)          Loop Start
            SLT (FXS)          Loop Start
            E&M                4W E&M, 4W E&M TE, 2W E&M, 2W E&M TE
            AC15               AC15A, AC15C"
    DEFVAL { loop-start }
    ::= { portVoiceAdminEntry 6 }

portVoiceAdminTETimer OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The delay at which the E&M 'E' lead follows the 'M' lead."
    DEFVAL { 3 }
    ::= { portVoiceAdminEntry 7 }

portVoiceAdminLevelIn OBJECT-TYPE
    SYNTAX  INTEGER (-22..7)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The local voice level into the voice port. This adjusts
            the sensitivity of the local voice channel to the signal
            from the attached device. The purpose of this is to match
            the voice channel dB level to the input signal. A more
            negative setting produces a higher input gain. If the level
            is reduced, the voice channel will be more sensitive to the
            input. This will also cause the voice output at the remote
            device to sound louder."
    DEFVAL { 0 }
    ::= { portVoiceAdminEntry 8 }

portVoiceAdminLevelOut OBJECT-TYPE
    SYNTAX  INTEGER (-22..7)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The local voice level out of the voice port. A more
            positive setting produces a higher volume."
    DEFVAL { -4 }
    ::= { portVoiceAdminEntry 9 }

portVoiceAdminCallTimer OBJECT-TYPE
    SYNTAX  INTEGER (1..30)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The amount of time the node will wait for a response to a
            Call Connect or Call Clear request. When the node issues a
            request, it will set a timer to the value configured here.
            If that timer expires with no response from the destination,
            the node will generate a busy tone."
    DEFVAL { 5 }
    ::= { portVoiceAdminEntry 10 }

portVoiceAdminHuntGroup OBJECT-TYPE
    SYNTAX  INTEGER {
                none (1),
                a (2),
                b (3)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The hunt group that includes the voice channel."
    DEFVAL { none }
    ::= { portVoiceAdminEntry 11 }

portVoiceAdminLongDialPrefix OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (1))
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The character that will be required preceeding calls using
            the long call format. When the user at an attached device
            dials a long form number, it must be preceeded by the prefix
            character specified here."
    DEFVAL { '2A'H }
    ::= { portVoiceAdminEntry 12 }

portVoiceAdminSLTTimeout OBJECT-TYPE
    SYNTAX  INTEGER (1..99)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The time the local port will wait before an actual fax
            transmission begins. If there is no fax tone when this
            timer expires, the connection will be terminated."
    DEFVAL { 30 }
    ::= { portVoiceAdminEntry 13 }

portVoiceAdminLinkDownBusy OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This flag enables or disables automatic busy-out of
            channels when the link is down. When enabled, the system
            will automatically busy-out channels when the composite
            link is down. When disabled, channels remain on-hook when
            the link is down. If your application is connected to a
            PBX that can route calls to another alternate source based
            on an all busy condition, enable this so the PBX will
            recognize this condition and reroute the calls while the
            composite link is down."
    DEFVAL { enabled }
    ::= { portVoiceAdminEntry 14 }

portVoiceAdminFaxSupported OBJECT-TYPE
    SYNTAX  INTEGER {
                no (1),
                yes (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The flag to indicate whether or not faxes will be
            transmitted on the port. If no, all calls will be treated
            as voice. If yes, both voice and fax will be transmitted."
    DEFVAL { yes }
    ::= { portVoiceAdminEntry 15 }

portVoiceAdminTelephonyType OBJECT-TYPE
    SYNTAX  INTEGER {
                opx (1),
                slt (2),
                em (3),
                ac15 (4)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The type of interface (in conjunction with the
            Interface Type) that will be used by the Voice channel.
            This requires rebooting for the change to take effect.
            Telephony Type     Interface Type
            --------------     --------------
            OPX (FXO)          Loop Start
            SLT (FXS)          Loop Start
            E&M                4W E&M, 4W E&M TE, 2W E&M, 2W E&M TE
            AC15               AC15A, AC15C"
    DEFVAL { opx }
    ::= { portVoiceAdminEntry 16 }

portVoiceAdminJitter OBJECT-TYPE
    SYNTAX  INTEGER (10..255)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The amount of jitter delay."
    DEFVAL { 80 }
    ::= { portVoiceAdminEntry 17 }

portVoiceAdminSampleDelay OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The amount of sample delay."
    DEFVAL { 10 }
    ::= { portVoiceAdminEntry 18 }

portVoiceAdminDialTimer OBJECT-TYPE
    SYNTAX  INTEGER (0..10)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The delay the node will use to determine when variable
            length dialing is complete. (Variable length dialing allows
            the user to place a call without entering the configured
            number of digits for the speed dial number.)"
    DEFVAL { 5 }
    ::= { portVoiceAdminEntry 19 }

portVoiceAdminAutoDial OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The flag to enable or disable the auto dial feature. Note
           that enabling this feature will disable the variable length
            dialing feature for this channel."
    DEFVAL { disabled }
    ::= { portVoiceAdminEntry 20 }

portVoiceAdminSuppression OBJECT-TYPE
    SYNTAX  INTEGER {
                very-low (1),
                low (2),
                medium (3),
                high (4),
                very-high (5)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The silence suppression level. A larger silence suppression
            level allows more data channels to operate simultaneously
            with the voice channels."
    DEFVAL { low }
    ::= { portVoiceAdminEntry 21 }

portVoiceAdminAutoDialNumber OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (0..4))
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The number to which the node will attempt to connect when
            the handset attached to this port is taken off-hook. This
            is applicable only when the Auto Dial feature is enabled."
    ::= { portVoiceAdminEntry 22 }

portVoiceAdminAutoPoll OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The flag to enable or disable auto polling. This is
            applicable only when the Auto Dial feature is enabled.
            When enabled, the node periodically polls the destination.
            If the poll is not acknowledged, the node will busy-out
            the channel. This can be useful in situations where the
            destination is an emergency number that must always be
            available. If the destination does not answer the automatic
            poll, the busy-out condition will notify an attached PBX
            that the emergency call should be routed to another call
            routing device."
    DEFVAL { disabled }
    ::= { portVoiceAdminEntry 23 }

portVoiceAdminAutoPollTimer OBJECT-TYPE
    SYNTAX  INTEGER (5..30)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The frequency with which an Auto Poll will be sent. This
            is applicable only when auto poll is enabled."
    DEFVAL { 10 }
    ::= { portVoiceAdminEntry 24 }

portVoiceAdminExtDigitsSource OBJECT-TYPE
    SYNTAX  INTEGER {
                map (1),
                user (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The source of the extended digits when the user of
            attached equipment dials a speed dial number. This is
            applicable only when the number of extended dial digits
            is greater than zero.  When map is specified, extended
            digits are taken from the extended digits field in the
            map table.  When user is specified, extended digits are
            taken from the user of attached equipment."
    DEFVAL { map }
    ::= { portVoiceAdminEntry 25 }

portVoiceAdminNumDigitsDelete OBJECT-TYPE
    SYNTAX  INTEGER (0..4)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The number of leading dial digits that will be deleted
            before a dial string is forwarded. This is primarily used
            to delete leading dial digits that may be inserted by an
            attached PBX."
    DEFVAL { 0 }
    ::= { portVoiceAdminEntry 26 }

portVoiceAdminForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (0..40)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The length of a pause that can be inserted in an extended
            dial string that is being forwarded. This is applicable only
            when forwarded output digits is all or extended. When a comma
            is encountered in an extended digits string, the node will
            pause for the length of time specified here before additional
            extended digits are forwarded."
    DEFVAL { 2 }
    ::= { portVoiceAdminEntry 27 }

portVoiceAdminForwardedType OBJECT-TYPE
    SYNTAX  INTEGER {
                dtmf (1),
                pulse (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The method how the dial digits will be forwarded. This
            is applicable only when forwarded output digits is all
            or extended."
    DEFVAL { dtmf }
    ::= { portVoiceAdminEntry 28 }

portVoiceAdminForwardedDigits OBJECT-TYPE
    SYNTAX  INTEGER {
                none (1),
                all (2),
                extended (3)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The flag indicating which dial digits, if any, to forward.
            If none, dial digits are not forwarded to the destination
            device when a call is initiated on this channel. If all,
            the dialed speed dial number and associated extended digits
            are forwarded to the destination device. If extended, only
            the extended digit string is forwarded."
    DEFVAL { none }
    ::= { portVoiceAdminEntry 29 }

portVoiceAdminMakeRatio OBJECT-TYPE
    SYNTAX  INTEGER (20..80)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The make ratio of each digit pulse that is forwarded.
            This is applicable only when forwarded output digits
            is all or extended and forwarded digit type is pulse."
    DEFVAL { 34 }
    ::= { portVoiceAdminEntry 30 }

portVoiceAdminBreakRatio OBJECT-TYPE
    SYNTAX  INTEGER (20..80)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The break ratio of each digit pulse that is forwarded.
            This is applicable only when forwarded output digits
            is all or extended and forwarded digit type is pulse."
    DEFVAL { 66 }
    ::= { portVoiceAdminEntry 31 }

portVoiceAdminDTMFOnDuration OBJECT-TYPE
    SYNTAX  INTEGER (30..1000)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The length of a tone that will be used to produce a
            single DTMF digit. This is applicable only when forwarded
            output digits is all or extended and forwarded digit type
            is DTMF."
    DEFVAL { 100 }
    ::= { portVoiceAdminEntry 32 }

portVoiceAdminDTMFOffDuration OBJECT-TYPE
    SYNTAX  INTEGER (30..1000)
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The length of silence between DTMF tones in a dial digit
            string. This is applicable only when forwarded output digits
            is all or extended and forwarded digit type is DTMF."
    DEFVAL { 100 }
    ::= { portVoiceAdminEntry 33 }

portVoiceAdminToneType OBJECT-TYPE
    SYNTAX  INTEGER {
                dtmf (1),
                mf (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The tone type to detect/regenerate for forwarding DTMF/MF."
    DEFVAL { dtmf }
    ::= { portVoiceAdminEntry 34 }

portVoiceAdminRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the portVoiceAdminTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device, and which is
                supplied by a management station wishing to exercise an
                on-line update of the existing conceptual row.  For a
                management protocol set operation, a genErr response is
                returned when the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
    ::= { portVoiceAdminEntry 35 }

--
-- The Voice Port Operational table
--

portVoiceOperTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortVoiceOperEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A list of Voice ports.  The number of entries
            will be the number of Voice ports on the node."
    ::= { portVoiceGroup 2 }

portVoiceOperEntry OBJECT-TYPE
    SYNTAX  PortVoiceOperEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A Voice Port entry containing objects relating
            to the port that are configurable by the user."
    INDEX   { portVoiceOperRlpIndex, portVoiceOperPortIndex }
    ::= { portVoiceOperTable 1 }

PortVoiceOperEntry ::=
    SEQUENCE {
        portVoiceOperRlpIndex
            INTEGER,
        portVoiceOperPortIndex
            INTEGER,
        portVoiceOperBlockedFlag
            INTEGER,
        portVoiceOperSpeed
            INTEGER,
        portVoiceOperDTMF
            INTEGER,
        portVoiceOperInterface
            INTEGER,
        portVoiceOperTETimer
            INTEGER,
        portVoiceOperLevelIn
            INTEGER,
        portVoiceOperLevelOut
            INTEGER,
        portVoiceOperCallTimer
            INTEGER,
        portVoiceOperHuntGroup
            INTEGER,
        portVoiceOperLongDialPrefix
            OCTET STRING,
        portVoiceOperSLTTimeout
            INTEGER,
        portVoiceOperLinkDownBusy
            INTEGER,
        portVoiceOperFaxSupported
            INTEGER,
        portVoiceOperTelephonyType
            INTEGER,
        portVoiceOperJitter
            INTEGER,
        portVoiceOperSampleDelay
            INTEGER,
        portVoiceOperDialTimer
            INTEGER,
        portVoiceOperAutoDial
            INTEGER,
        portVoiceOperSuppression
            INTEGER,
        portVoiceOperAutoDialNumber
            OCTET STRING,
        portVoiceOperAutoPoll
            INTEGER,
        portVoiceOperAutoPollTimer
            INTEGER,
        portVoiceOperExtDigitsSource
            INTEGER,
        portVoiceOperNumDigitsDelete
            INTEGER,
        portVoiceOperForwardDelay
            INTEGER,
        portVoiceOperForwardedType
            INTEGER,
        portVoiceOperForwardedDigits
            INTEGER,
        portVoiceOperMakeRatio
            INTEGER,
        portVoiceOperBreakRatio
            INTEGER,
        portVoiceOperDTMFOnDuration
            INTEGER,
        portVoiceOperDTMFOffDuration
            INTEGER,
        portVoiceOperToneType
            INTEGER
    }

portVoiceOperRlpIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The RLP number of the Voice port."
    ::= { portVoiceOperEntry 1 }

portVoiceOperPortIndex OBJECT-TYPE
    SYNTAX  INTEGER
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The Port number of the Voice port."
    ::= { portVoiceOperEntry 2 }

portVoiceOperBlockedFlag OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The flag which causes the port to be enabled or disabled
            at node IPL. The port will remain in that state until this
            flag is changed and the node is rebooted, or until an on-
            line enable or disable is performed."
    ::= { portVoiceOperEntry 3 }

portVoiceOperSpeed OBJECT-TYPE
    SYNTAX  INTEGER {
                bps-4800 (1),
                bps-8000 (2),
                bps-32000 (3),
                bps-64000 (4)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The speed of the port which is transmitted as part
            of a Call Setup frame. A Voice call will be established
            if there is enough bandwidth at each end to provide the
            minimum configured rate."
    ::= { portVoiceOperEntry 4 }

portVoiceOperDTMF OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The flag to enable, disable, or specify a time span
            over which DTMF (Dual Tone Multi Frequency) tones will
            be regenerated.
            0 =     pass tones transparently to the remote device.
            1 =     detect incoming tones and regenerate as received.
            2-255 = regenerate tones for the specified seconds."
    ::= { portVoiceOperEntry 5 }

portVoiceOperInterface OBJECT-TYPE
    SYNTAX  INTEGER {
                em-4w (1),
                em-2w (2),
                loop-start (3),
                ac15-a (4),
                ac15-b (6),
                em-4w-te (10),
                em-2w-te (11)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The type of interface (in conjunction with the Telephony
            Interface Type) that will be used by the Voice channel.
            This requires rebooting for the change to take effect.
            Telephony Type     Interface Type
            --------------     --------------
            OPX (FXO)          Loop Start
            SLT (FXS)          Loop Start
            E&M                4W E&M, 4W E&M TE, 2W E&M, 2W E&M TE
            AC15               AC15A, AC15C"
    ::= { portVoiceOperEntry 6 }

portVoiceOperTETimer OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The delay at which the E&M 'E' lead follows the 'M' lead."
    ::= { portVoiceOperEntry 7 }

portVoiceOperLevelIn OBJECT-TYPE
    SYNTAX  INTEGER (-22..7)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The local voice level into the voice port. This adjusts
            the sensitivity of the local voice channel to the signal
            from the attached device. The purpose of this is to match
            the voice channel dB level to the input signal. A more
            negative setting produces a higher input gain. If the level
            is reduced, the voice channel will be more sensitive to the
            input. This will also cause the voice output at the remote
            device to sound louder."
    ::= { portVoiceOperEntry 8 }

portVoiceOperLevelOut OBJECT-TYPE
    SYNTAX  INTEGER (-22..7)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The local voice level out of the voice port. A more
            positive setting produces a higher volume."
    ::= { portVoiceOperEntry 9 }

portVoiceOperCallTimer OBJECT-TYPE
    SYNTAX  INTEGER (1..30)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The amount of time the node will wait for a response to a
            Call Connect or Call Clear request. When the node issues a
            request, it will set a timer to the value configured here.
            If that timer expires with no response from the destination,
            the node will generate a busy tone."
    ::= { portVoiceOperEntry 10 }

portVoiceOperHuntGroup OBJECT-TYPE
    SYNTAX  INTEGER {
                none (1),
                a (2),
                b (3)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The hunt group that includes the voice channel."
    ::= { portVoiceOperEntry 11 }

portVoiceOperLongDialPrefix OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (1))
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The character that will be required preceeding calls using
            the long call format. When the user at an attached device
            dials a long form number, it must be preceeded by the prefix
            character specified here."
    ::= { portVoiceOperEntry 12 }

portVoiceOperSLTTimeout OBJECT-TYPE
    SYNTAX  INTEGER (1..99)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The time the local port will wait before an actual fax
            transmission begins. If there is no fax tone when this
            timer expires, the connection will be terminated."
    ::= { portVoiceOperEntry 13 }

portVoiceOperLinkDownBusy OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "This flag enables or disables automatic busy-out of
            channels when the link is down. When enabled, the system
            will automatically busy-out channels when the composite
            link is down. When disabled, channels remain on-hook when
            the link is down. If your application is connected to a
            PBX that can route calls to another alternate source based
            on an all busy condition, enable this so the PBX will
            recognize this condition and reroute the calls while the
            composite link is down."
    ::= { portVoiceOperEntry 14 }

portVoiceOperFaxSupported OBJECT-TYPE
    SYNTAX  INTEGER {
                no (1),
                yes (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The flag to indicate whether or not faxes will be
            transmitted on the port. If no, all calls will be treated
            as voice. If yes, both voice and fax will be transmitted."
    ::= { portVoiceOperEntry 15 }

portVoiceOperTelephonyType OBJECT-TYPE
    SYNTAX  INTEGER {
                opx (1),
                slt (2),
                em (3),
                ac15 (4)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The type of interface (in conjunction with the
            Interface Type) that will be used by the Voice channel.
            This requires rebooting for the change to take effect.
            Telephony Type     Interface Type
            --------------     --------------
            OPX (FXO)          Loop Start
            SLT (FXS)          Loop Start
            E&M                4W E&M, 4W E&M TE, 2W E&M, 2W E&M TE
            AC15               AC15A, AC15C"
    ::= { portVoiceOperEntry 16 }

portVoiceOperJitter OBJECT-TYPE
    SYNTAX  INTEGER (10..255)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The amount of jitter delay."
    ::= { portVoiceOperEntry 17 }

portVoiceOperSampleDelay OBJECT-TYPE
    SYNTAX  INTEGER (0..255)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The amount of sample delay."
    ::= { portVoiceOperEntry 18 }

portVoiceOperDialTimer OBJECT-TYPE
    SYNTAX  INTEGER (0..10)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The delay the node will use to determine when variable
            length dialing is complete. (Variable length dialing allows
            the user to place a call without entering the configured
            number of digits for the speed dial number.)"
    ::= { portVoiceOperEntry 19 }

portVoiceOperAutoDial OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The flag to enable or disable the auto dial feature. Note
            that enabling this feature will disable the variable length
            dialing feature for this channel."
    ::= { portVoiceOperEntry 20 }

portVoiceOperSuppression OBJECT-TYPE
    SYNTAX  INTEGER {
                very-low (1),
                low (2),
                medium (3),
                high (4),
                very-high (5)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The silence suppression level. A larger silence suppression
            level allows more data channels to operate simultaneously
            with the voice channels."
    ::= { portVoiceOperEntry 21 }

portVoiceOperAutoDialNumber OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (0..4))
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The number to which the node will attempt to connect when
            the handset attached to this port is taken off-hook. This
            is applicable only when the Auto Dial feature is enabled."
    ::= { portVoiceOperEntry 22 }

portVoiceOperAutoPoll OBJECT-TYPE
    SYNTAX  INTEGER {
                disabled (1),
                enabled (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The flag to enable or disable auto polling. This is
            applicable only when the Auto Dial feature is enabled.
            When enabled, the node periodically polls the destination.
            If the poll is not acknowledged, the node will busy-out
            the channel. This can be useful in situations where the
            destination is an emergency number that must always be
            available. If the destination does not answer the automatic
            poll, the busy-out condition will notify an attached PBX
            that the emergency call should be routed to another call
            routing device."
    ::= { portVoiceOperEntry 23 }

portVoiceOperAutoPollTimer OBJECT-TYPE
    SYNTAX  INTEGER (5..30)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The frequency with which an Auto Poll will be sent. This
            is applicable only when auto poll is enabled."
    ::= { portVoiceOperEntry 24 }

portVoiceOperExtDigitsSource OBJECT-TYPE
    SYNTAX  INTEGER {
                map (1),
                user (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The source of the extended digits when the user of
            attached equipment dials a speed dial number. This is
            applicable only when the number of extended dial digits
            is greater than zero.  When map is specified, extended
            digits are taken from the extended digits field in the
            map table.  When user is specified, extended digits are
            taken from the user of attached equipment."
    ::= { portVoiceOperEntry 25 }

portVoiceOperNumDigitsDelete OBJECT-TYPE
    SYNTAX  INTEGER (0..4)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The number of leading dial digits that will be deleted
            before a dial string is forwarded. This is primarily used
            to delete leading dial digits that may be inserted by an
            attached PBX."
    ::= { portVoiceOperEntry 26 }

portVoiceOperForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (0..40)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The length of a pause that can be inserted in an extended
            dial string that is being forwarded. This is applicable only
            when forwarded output digits is all or extended. When a comma
            is encountered in an extended digits string, the node will
            pause for the length of time specified here before additional
            extended digits are forwarded."
    ::= { portVoiceOperEntry 27 }

portVoiceOperForwardedType OBJECT-TYPE
    SYNTAX  INTEGER {
                dtmf (1),
                pulse (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The method how the dial digits will be forwarded. This
            is applicable only when forwarded output digits is all
            or extended."
    ::= { portVoiceOperEntry 28 }

portVoiceOperForwardedDigits OBJECT-TYPE
    SYNTAX  INTEGER {
                none (1),
                all (2),
                extended (3)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The flag indicating which dial digits, if any, to forward.
            If none, dial digits are not forwarded to the destination
            device when a call is initiated on this channel. If all,
            the dialed speed dial number and associated extended digits
            are forwarded to the destination device. If extended, only
            the extended digit string is forwarded."
    ::= { portVoiceOperEntry 29 }

portVoiceOperMakeRatio OBJECT-TYPE
    SYNTAX  INTEGER (20..80)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The make ratio of each digit pulse that is forwarded.
            This is applicable only when forwarded output digits
            is all or extended and forwarded digit type is pulse."
    ::= { portVoiceOperEntry 30 }

portVoiceOperBreakRatio OBJECT-TYPE
    SYNTAX  INTEGER (20..80)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The break ratio of each digit pulse that is forwarded.
            This is applicable only when forwarded output digits
            is all or extended and forwarded digit type is pulse."
    ::= { portVoiceOperEntry 31 }

portVoiceOperDTMFOnDuration OBJECT-TYPE
    SYNTAX  INTEGER (30..1000)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The length of a tone that will be used to produce a
            single DTMF digit. This is applicable only when forwarded
            output digits is all or extended and forwarded digit type
            is DTMF."
    ::= { portVoiceOperEntry 32 }

portVoiceOperDTMFOffDuration OBJECT-TYPE
    SYNTAX  INTEGER (30..1000)
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The length of silence between DTMF tones in a dial digit
            string. This is applicable only when forwarded output digits
            is all or extended and forwarded digit type is DTMF."
    ::= { portVoiceOperEntry 33 }

portVoiceOperToneType OBJECT-TYPE
    SYNTAX  INTEGER {
                dtmf (1),
                mf (2)
                }
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The tone type to detect/regenerate for forwarding DTMF/MF."
    ::= { portVoiceOperEntry 34 }

-- **********************************
-- *  THE NETLINK INTERFACES GROUP  *
-- **********************************

nlInterfaces OBJECT IDENTIFIER ::=  { local 4 }

--  The nlIinterfaces group is a netlink table which contains all interfaces
--  indexed by RLP and port

--
--  The Netlink If Table
--
-- This table is used to correlate an RLP and Port number to a MIB-II
-- Interface Table entry and a Netlink Interface Table entry. The table
-- is indexed by RLP and port number. 
-- The range of RLP numbers can be:
--     1-8 = RLP cards
--     250 = IP Interfaces
--     251 = IPX Interfaces
--     252 = LLC2 Interfaces
-- The range of port numbers can be:
-- For RLP cards (RLP 1-8) :
--     1-8 = Physical Port
--     9-64 = Logical Port
-- For IP Interfaces (RLP 250) :
--     1-257 = the interface number - FRX4000/FRX6000 version 3.4
--     1-129 = the interface number - other FRX4000/FRX6000 and FRX7000
-- For IPX Interfaces (RLP 251) :
--     1-64 = the interface number
-- For LLC2 Interfaces (RLP 252) :
--     1-96  = the interface number - FRX4000/FRX6000
--     1-251 = the interface number - FRX7000

nlIfTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlIfEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe each interface on a node.
        This table is indexed by RLP and Port number and can be used to 
        identify the corresponding MIB-II ifIndex of a Port as well as
        additional port information maintained by Netlink."
        ::= { nlInterfaces 1 }

nlIfEntry OBJECT-TYPE
        SYNTAX NlIfEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An Interface entry containing objects relating to interfaces."
        INDEX { nlIfRlp, nlIfPort }
        ::= { nlIfTable 1 }

NlIfEntry ::=
        SEQUENCE {
                nlIfRlp
                        INTEGER,
                nlIfPort
                        INTEGER,
                nlIfType
                        INTEGER,
                nlIfIndex
                        INTEGER,
                nlIfTableIndex
                        INTEGER,
                nlIfTableOid
                        OBJECT IDENTIFIER,
                nlIfConnectorType
                        INTEGER,
                nlIfPortStatus
                        INTEGER,
                nlIfPhyPort
                        INTEGER
        }

nlIfRlp OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP number on the node. RLP numbers 1-8 are Physical
        RLP cards, and RLP number 250, 251 and 252 define IP, IPX and LLC2
        interfaces respectively."
        ::= { nlIfEntry 1 }

nlIfPort OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port number on the RLP. Port numbers 1-8 are
        known to be physical ports, and 9-64 are logical ports. If the 
        RLP number identifies an IP, IPX or LLC2 interface, then the port 
        number can be 1-257 (IP), 1-64 (IPX), or 1-96 (LLC2)."
        ::= { nlIfEntry 2 }

nlIfType OBJECT-TYPE
   SYNTAX  INTEGER {
                           other(1),          -- none of the following
                           regular1822(2),
                           hdh1822(3),
                           ddnX25(4),
                           rfc877x25(5),
                           ethernetCsmacd(6),
                           iso88023Csmacd(7),
                           iso88024TokenBus(8),
                           iso88025TokenRing(9),
                           iso88026Man(10),
                           starLan(11),
                           proteon10Mbit(12),
                           proteon80Mbit(13),
                           hyperchannel(14),
                           fddi(15),
                           lapb(16),
                           sdlc(17),
                           ds1(18),           -- DS1/E1 (RFC 1406)
                           e1(19),            -- obsolete
                           basicISDN(20),
                           primaryISDN(21),
                           propPointToPointSerial(22), -- proprietary serial
                           ppp(23),
                           softwareLoopback(24),
                           eon(25),            -- CLNP over IP (RFC 1070)
                           ethernet3Mbit(26),
                           nsip(27),           -- XNS over IP
                           slip(28),           -- generic SLIP
                           ultra(29),          -- ULTRA technologies
                           ds3(30),            -- T-3
                           sip(31),            -- SMDS
                           frameRelay(32),    -- DTE only
                           rs232(33),
                           para(34),           -- parallel-port
                           arcnet(35),         -- arcnet
                           arcnetPlus(36),     -- arcnet plus
                           atm(37),            -- ATM cells
                           miox25(38),
                           sonet(39),          -- SONET or SDH
                           x25ple(40),
                           iso88022llc(41),
                           localTalk(42),
                           smdsDxi(43),
                           frameRelayService(44),  -- Frame relay DCE
                           v35(45),
                           hssi(46),
                           hippi(47),
                           modem(48),          -- Generic modem
                           aal5(49),           -- AAL5 over ATM
                           sonetPath(50),
                           sonetVT(51),
                           smdsIcip(52),       -- SMDS InterCarrier Interface
                           propVirtual(53),    -- proprietary virtual/internal
                           propMultiplexor(54), -- proprietary multiplexing
                           trunk(200),                  -- NETLINK: Trunk port
                           async(201),                  -- NETLINK: Async port
                           bsci(202),                   -- NETLINK: Bsci port
                           logicalPort(203),     -- NETLINK: Logical port
                           t1(204),                      -- NETLINK: T1 port
                           ip(205),             -- NETLINK: IP interface
                           ipx(206),             -- NETLINK: IPX interface
                           llc2(207),            -- NETLINK: LLC2 interface
                           voice(208) 
                   }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The type of interface"
        ::= { nlIfEntry 3 }

nlIfIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The associated index into the MIB-II ifTable for this
        port"
        ::= { nlIfEntry 4 }

nlIfTableIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The associated index into an enterprise table used to
        describe additional information for this port. See nlIfTableOid as the 
        pointer to the actual table."
        ::= { nlIfEntry 5 }

nlIfTableOid OBJECT-TYPE
        SYNTAX OBJECT IDENTIFIER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The OID of the table Entry that contains additional
        information about this port. The OID will point to a specific table
        depending on the type of port."
        ::= { nlIfEntry 6 }

nlIfConnectorType OBJECT-TYPE
        SYNTAX INTEGER { none(2),
                                         rs232(3),
                                         v25bis-dial(4),
                                         v35(5),
                                         rs449(6),
                                         rs530(7),
                                         x21(8),        
                                         csudsu(9),
                                         t1(10),
                                         e1(11),
                                         voice(13) 
                                        }

        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The physical connector type used for this port. Valid
        for ports 1-8 only."
        ::= { nlIfEntry 7 }

nlIfPortStatus OBJECT-TYPE
        SYNTAX INTEGER { linkUp(1),
                                         restarting(2),
                                         operational(3),
                                         disabled(4),
                                         disconnect(5),
                                         configured(6),
                                         dialReady(7),
                                         quiesced(8),
                                         failed(9),
                                         hardwareFault(10),
                                         other(11),
                                         ipl(12),
                                         na(13),
                                         remoteLoopback(14),
                                         blueAlarm(15),
                                         yellowAlarm(16),
                                         redAlarm(17),
                                         onHook(18),
                                         offHook(19),
                                         dialing(20),
                                         activeVoiceCall(21),
                                         onHookPending(22) 
                                   }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The status of this port state. Valid for ports 1-64 only."
        ::= { nlIfEntry 8 }

nlIfPhyPort OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Underlying Physical Port number on the RLP of this
        logical port. Port numbers 1-8 are valid, but this field is only
        applicable if the nlIfPort field is 9-64."
        ::= { nlIfEntry 9 }

nlIfLlc2Interfaces OBJECT IDENTIFIER ::= { nlInterfaces 2}

--
--  The Netlink LLC2 Interface Tables
--

nlIfLlc2LANTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlIfLlc2LANEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to define LLC2 interfaces over LAN."
        ::= { nlIfLlc2Interfaces 1 }

nlIfLlc2LANEntry OBJECT-TYPE
        SYNTAX NlIfLlc2LANEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An LLC2 LAN Interface entry containing objects relating
        to LLC2 LAN interfaces."
        INDEX { nlIfLlc2LANRlp, nlIfLlc2LANPort }
        ::= { nlIfLlc2LANTable 1 }

NlIfLlc2LANEntry ::=
        SEQUENCE {
                nlIfLlc2LANRlp                          INTEGER,
                nlIfLlc2LANPort                         INTEGER,
                nlIfLlc2LANType                         INTEGER,
                nlIfLlc2LANCard                         INTEGER,        
                nlIfLlc2LANID                           INTEGER,
                nlIfLlc2LANInterface                    INTEGER,
                nlIfLlc2LANRowStatus                    RowStatus,
                nlIfLlc2LANPriority                     INTEGER,
        nlIfLlc2LANBlockedPortFlag              INTEGER
        }

nlIfLlc2LANRlp   OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION "The RLP number on the node. For LLC2 LAN interfaces,
                this must be 252."
                ::= { nlIfLlc2LANEntry 1 }

nlIfLlc2LANPort OBJECT-TYPE
                SYNTAX INTEGER
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION "The Port number on the RLP. For LLC2 LAN interfaces,
                this corresponds to the LAN card number."
                ::= { nlIfLlc2LANEntry 2 }

nlIfLlc2LANType OBJECT-TYPE
                SYNTAX INTEGER {
                        ethernet (1),
                        token-ring (2)
                }
                ACCESS read-write
                STATUS mandatory
                DESCRIPTION "The type of the LLC2 interface- either ethernet or
                token ring."
                DEFVAL { ethernet }
                ::= { nlIfLlc2LANEntry 3 }

nlIfLlc2LANCard OBJECT-TYPE
                SYNTAX INTEGER (1..2)
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION "The LAN card that the LLC2 interface is running on."
                ::= { nlIfLlc2LANEntry 4 }

nlIfLlc2LANID   OBJECT-TYPE
                SYNTAX INTEGER (0..4095)
                ACCESS read-write
                STATUS mandatory
                DESCRIPTION "Valid only if the type of the LLC2 LAN interface is
                token ring.  Identifies the token ring adapter to the network."
                DEFVAL { 4095 }
                ::= { nlIfLlc2LANEntry 5 }

nlIfLlc2LANInterface OBJECT-TYPE
                     SYNTAX INTEGER (1..2)
                     ACCESS read-only
                     STATUS mandatory
                     DESCRIPTION "The LLC2 interface number."
                     ::= { nlIfLlc2LANEntry 6 }

nlIfLlc2LANRowStatus    OBJECT-TYPE
                        SYNTAX      RowStatus
                        ACCESS      read-write
                        STATUS      mandatory
                        DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlIfLlc2LANTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
                        ::= { nlIfLlc2LANEntry 7 }

nlIfLlc2LANPriority     OBJECT-TYPE
                        SYNTAX INTEGER (0..9)
                        ACCESS read-write
                        STATUS mandatory
                        DESCRIPTION "Interface priority- allows setting a priority for traffic
                        within the node.  The higher the number, the higher the priority relative
                        to other intra-nodal traffic."
                        DEFVAL { 0 }
                        ::= {nlIfLlc2LANEntry 8}

nlIfLlc2LANBlockedPortFlag      OBJECT-TYPE
                                SYNTAX  INTEGER {
                                                no(1),
                                                yes(2)
                                }
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION
                                        "The blocked port flag."
                                DEFVAL { no }
                                ::= { nlIfLlc2LANEntry 9 }

nlIfLlc2FrTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlIfLlc2FrEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to define LLC2 interfaces over Frame Relay."
        ::= { nlIfLlc2Interfaces 2 }

nlIfLlc2FrEntry OBJECT-TYPE
        SYNTAX NlIfLlc2FrEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An LLC2 FR Interface entry containing objects relating
        to LLC2 FR interfaces."
        INDEX { nlIfLlc2FrRlp, nlIfLlc2FrPort, nlIfLlc2FrDLCI, nlIfLlc2FrFormat }
        ::= { nlIfLlc2FrTable 1 }

NlIfLlc2FrEntry ::=
        SEQUENCE {
                nlIfLlc2FrRlp                           INTEGER,
                nlIfLlc2FrPort                          INTEGER,
                nlIfLlc2FrDLCI                          INTEGER,
                nlIfLlc2FrFormat                        INTEGER,        
                nlIfLlc2FrPriority                      INTEGER,
                nlIfLlc2FrBAG                           INTEGER,
                nlIfLlc2FrHostMACAddress                MacAddress,
                nlIfLlc2FrSessionType                   INTEGER,
                nlIfLlc2FrLANID                         INTEGER,
                nlIfLlc2FrInterface                     INTEGER,
                nlIfLlc2FrRowStatus                     RowStatus,
                nlIfLlc2FrBlockedPortFlag               INTEGER
        }

nlIfLlc2FrRlp   OBJECT-TYPE
                SYNTAX INTEGER (1..8)
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION "The RLP number on the node."
                ::= { nlIfLlc2FrEntry 1 }

nlIfLlc2FrPort  OBJECT-TYPE
                SYNTAX INTEGER (1..255)
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION "The Port number on the RLP. Port numbers 1-8 are
                known to be physical ports, and channels are 193-241."
                ::= { nlIfLlc2FrEntry 2 }

nlIfLlc2FrDLCI  OBJECT-TYPE
                SYNTAX INTEGER (16..991)
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION "The DLCI number used to identify the entry in the table. 
                The range is 16-991. "
                ::= { nlIfLlc2FrEntry 3 }

nlIfLlc2FrFormat OBJECT-TYPE
                 SYNTAX INTEGER {
                        native-llc2 (1),
                        tb-8023 (2),
                        srb-8025 (3)
                 }
                 ACCESS read-only
                 STATUS mandatory
                 DESCRIPTION "The RFC1490 encapsulation method used for LLC2 traffic."
                 ::= {nlIfLlc2FrEntry 4}

nlIfLlc2FrPriority OBJECT-TYPE
                   SYNTAX INTEGER (0..9)
                   ACCESS read-write
                   STATUS mandatory
                   DESCRIPTION "Interface priority- allows setting a priority for traffic
                   within the node.  The higher the number, the higher the priority relative
                   to other intra-nodal traffic."
                   DEFVAL { 0 }
                   ::= {nlIfLlc2FrEntry 5}

nlIfLlc2FrBAG OBJECT-TYPE
              SYNTAX INTEGER (1..16)
              ACCESS read-write
              STATUS mandatory
              DESCRIPTION "Assigns the interface to one of sixteen groups whose parameters
              regulate bandwidth usage."
              DEFVAL { 1 }
              ::= {nlIfLlc2FrEntry 6}

nlIfLlc2FrHostMACAddress OBJECT-TYPE
                         SYNTAX MacAddress
                         ACCESS read-write
                         STATUS mandatory
                         DESCRIPTION "The MAC address of the host or workstation to which 
                         the remote device needs to connect.  Valid only if the format is
                         native-llc2."
                         DEFVAL { '400000000001'H }    -- 40:00:00:00:00:01
                         ::= {nlIfLlc2FrEntry 7}

nlIfLlc2FrSessionType   OBJECT-TYPE
                        SYNTAX INTEGER {
                                terminated (1),
                                originated (2),
                                not-applicable (3)
                        }                               
                        ACCESS read-write
                        STATUS mandatory
                        DESCRIPTION "If originated, means that LLC2 connects from the configured
                        Host MAC address can use this interface.  If terminated, connections to
                        the configured address can use this interface.  Valid only if the
                        format is native-llc2."
                        DEFVAL { originated }
                        ::= {nlIfLlc2FrEntry 8}

nlIfLlc2FrLANID         OBJECT-TYPE
                        SYNTAX INTEGER (0..4095)
                        ACCESS read-write
                        STATUS mandatory
                        DESCRIPTION "Identifies the ring number used by a frame relay-compliant
                        source-route bridge at the other end of this PVC.  Valid only if the
                        format is srb-8025."
                        DEFVAL { 4095 }
                        ::= { nlIfLlc2FrEntry 9 }

nlIfLlc2FrInterface     OBJECT-TYPE
                        SYNTAX INTEGER 
                        ACCESS read-only
                        STATUS mandatory
                        DESCRIPTION "LLC2 interface number."
                        ::= { nlIfLlc2FrEntry 10 }

nlIfLlc2FrRowStatus     OBJECT-TYPE
                        SYNTAX      RowStatus
                        ACCESS      read-write
                        STATUS      mandatory
                        DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlIfLlc2FrTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
                        ::= { nlIfLlc2FrEntry 11 }

nlIfLlc2FrBlockedPortFlag       OBJECT-TYPE
                                SYNTAX  INTEGER {
                                                no(1),
                                                yes(2)
                                }
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION
                                        "The blocked port flag."
                                DEFVAL { no }
                                ::= { nlIfLlc2FrEntry 12 }      

ipxConfig OBJECT IDENTIFIER ::=    { nlInterfaces 3 }
ipxConfigRouting OBJECT IDENTIFIER ::= { ipxConfig 1 }

-- Routing Group

-- Static Route Config Table
--  The static route config table contains an entry for each static route entry
--  in the system 

ipxStaticRouteConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF IPXStaticRouteConfigEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION     "The IPX Static Route Configuration Table"
        ::= {ipxConfigRouting 1}

ipxStaticRouteConfigEntry OBJECT-TYPE
        SYNTAX  IPXStaticRouteConfigEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION     "Each entry corresponds to one instance of IPX Static Routing on the system"
        INDEX   {ipxStaticRouteConfigCircIndex,
                         ipxStaticRouteConfigNetNum
                        }

        ::= {ipxStaticRouteConfigTable 1}

IPXStaticRouteConfigEntry ::= SEQUENCE {
                        ipxStaticRouteConfigCircIndex
                                INTEGER,
                        ipxStaticRouteConfigNetNum
                                OCTET STRING,
                        ipxStaticRouteConfigRouter
                                OCTET STRING,
                        ipxStaticRouteConfigRowStatus
                                RowStatus
}

ipxStaticRouteConfigCircIndex OBJECT-TYPE 
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-only 
        STATUS  mandatory
        DESCRIPTION     "The unique identifier of the circuit used to reach the
                                first hop in the static route"
        ::= {ipxStaticRouteConfigEntry 1}

ipxStaticRouteConfigNetNum OBJECT-TYPE 
        SYNTAX  OCTET STRING (SIZE(4))    
        ACCESS  read-only 
        STATUS  mandatory
        DESCRIPTION     "The IPX network number of the route's destination"
        ::= {ipxStaticRouteConfigEntry 2}

ipxStaticRouteConfigRouter OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(6)) 
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION     "The hex value of the node address of the router that will forward a packet when this route is used. 
                                 If Novell's IPXWAN is used on the interface, this field will be ignored "
        ::= {ipxStaticRouteConfigEntry 3}

ipxStaticRouteConfigRowStatus OBJECT-TYPE 
        SYNTAX  RowStatus
        ACCESS  read-write
        STATUS  mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the ipxStaticRouteTable  and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= {ipxStaticRouteConfigEntry 4}

-- Static SAP Config Table
--  The static SAP config table contains an entry for each SAP route entry
--  in the system 

ipxServConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF IPXServConfigEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION     "The IPX Static Route Configuration Table"
        ::= {ipxConfigRouting 2}

ipxServConfigEntry OBJECT-TYPE
        SYNTAX  IPXServConfigEntry
        ACCESS  not-accessible
        STATUS  mandatory
        DESCRIPTION     "Each entry corresponds to one instance of IPX Static Routing on the system"
        INDEX   {ipxServConfigServiceType,
                         ipxServConfigServName
                        }

        ::= {ipxServConfigTable 1}

IPXServConfigEntry ::= SEQUENCE {
                        ipxServConfigServiceType
                                INTEGER,
                        ipxServConfigServName
                                OCTET STRING,
                        ipxServConfigServNetworkAddress
                                INTEGER, 
                        ipxServConfigServNodeAddress 
                                OCTET STRING, 
                        ipxServConfigServSocketNumber 
                                INTEGER, 
                        ipxServConfigInterveningNetworks 
                                INTEGER,
                        ipxServConfigGatewayAddress 
                                OCTET STRING, 
                        ipxServConfigInterface 
                                INTEGER,
                        ipxServConfigRowStatus
                                RowStatus
}

ipxServConfigServiceType  OBJECT-TYPE 
        SYNTAX  INTEGER (1..65535) 
        ACCESS  read-only 
        STATUS  mandatory
        DESCRIPTION     "The Service Type, a SAP service code "
        ::= {ipxServConfigEntry 1}

ipxServConfigServName  OBJECT-TYPE 
        SYNTAX  OCTET STRING (SIZE(1..48)) 
        ACCESS  read-only 
        STATUS  mandatory
        DESCRIPTION     "The Sercice Name, identifies a specific server in the IPX network. "
        ::= {ipxServConfigEntry 2}

ipxServConfigServNetworkAddress OBJECT-TYPE 
        SYNTAX  INTEGER  
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION     "The IPX network number portion of the IPX address of the server identified by ServName "
        DEFVAL { 1 } 
        ::= {ipxServConfigEntry 3}

ipxServConfigServNodeAddress OBJECT-TYPE 
        SYNTAX  OCTET STRING (SIZE(6))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION     "The  node portion of the IPX address of the service"
        ::= {ipxServConfigEntry 4}

ipxServConfigServSocketNumber OBJECT-TYPE 
        SYNTAX  INTEGER (0..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION     "The socket portion of the IPX address of the service"
        DEFVAL { 0 } 
        ::= {ipxServConfigEntry 5}

ipxServConfigInterveningNetworks OBJECT-TYPE 
        SYNTAX  INTEGER (1..65535)
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION     "The number of routers that a packet must pass through t reach the server"
        DEFVAL { 1 } 
        ::= {ipxServConfigEntry 6}

ipxServConfigGatewayAddress  OBJECT-TYPE 
        SYNTAX  OCTET STRING (SIZE(6))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION     "The node address of the router thar will forward a packet"
        ::= {ipxServConfigEntry 7}

ipxServConfigInterface  OBJECT-TYPE 
        SYNTAX  INTEGER (0..65535) 
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION     "The IPX network number assigned to the interface used to send packets that are destined for this server"
        DEFVAL { 0 } 
        ::= {ipxServConfigEntry 8}

ipxServConfigRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the ipxServTable  and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= {ipxServConfigEntry 9}

ipxConfigInterface OBJECT IDENTIFIER ::= { ipxConfig 2 }

-- Interface Group

-- Interface Table

ipxInterfaceTable OBJECT-TYPE
        SYNTAX SEQUENCE OF IPXInterfaceEntry 
        ACCESS  not-accessible
        STATUS  mandatory 
        DESCRIPTION "The IPX Interface Table"
        ::= {ipxConfigInterface 6} 

ipxInterfaceEntry OBJECT-TYPE
        SYNTAX  IPXInterfaceEntry 
        ACCESS  not-accessible 
        STATUS  mandatory 
        DESCRIPTION ""
        INDEX   {ipxInterfaceNumber 
                        } 

        ::= {ipxInterfaceTable 1} 

IPXInterfaceEntry ::= SEQUENCE {
        ipxInterfaceNumber INTEGER,
        ipxInterfaceBlockedPortFlag INTEGER,
        ipxInterfaceType INTEGER,
        ipxInterfaceFrameType INTEGER, 
        ipxInterfaceMaxTransUnit INTEGER, 
        ipxInterfaceNetworkAddress INTEGER, 
        ipxInterfaceBandwidthAllocGroup INTEGER, 
        ipxInterfacePortDiagEnabled INTEGER, 
        ipxInterfaceNetBIOSEnabled INTEGER, 
        ipxInterfaceNetBIOSHops INTEGER, 
        ipxInterfacePeriodicRIPEnabled INTEGER, 
        ipxInterfacePeriodicRIPTimer INTEGER, 
        ipxInterfacePeriodicSAPEnabled INTEGER, 
        ipxInterfacePeriodicSAPTimer INTEGER, 
        ipxInterfaceRIPEnabled INTEGER, 
        ipxInterfaceRIPAgeTimer INTEGER, 
        ipxInterfaceRIPMaxSize INTEGER, 
        ipxInterfaceSAPEnabled INTEGER, 
        ipxInterfaceSAPAgeTimer INTEGER, 
        ipxInterfaceTransportTime INTEGER, 
        ipxInterfaceSerializationEnabled INTEGER, 
        ipxInterfaceWatchdogSpoofingEnabled INTEGER, 
        ipxInterfaceLanCardNumber INTEGER, 
        ipxInterfaceWanEnabled INTEGER,
        ipxInterfaceSourceSubscriber OCTET STRING,
        ipxInterfaceDestinationSubscriber OCTET STRING,
        ipxInterfaceSVCRetryTimer INTEGER,
        ipxInterfaceSVCIdleTimer  INTEGER,
        ipxInterfaceMaxVC INTEGER,
        ipxInterfacePVCConnection INTEGER,
        ipxInterfaceSourceCard INTEGER,
        ipxInterfaceSourcePort INTEGER,
        ipxInterfaceSourceDLCI INTEGER, 
        ipxInterfaceRowStatus RowStatus 
}

ipxInterfaceNumber OBJECT-TYPE 
        SYNTAX INTEGER (1..64) 
        ACCESS read-only 
        STATUS mandatory
        DESCRIPTION "The Interface Number, a sequential number to identify the interface"
        ::= {ipxInterfaceEntry 1}

ipxInterfaceBlockedPortFlag OBJECT-TYPE 
        SYNTAX INTEGER 
                        { no(1),
                          yes(2)
                        }

        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "This flag causes the IPX interface to be enabled (N) or disabled (Y) at node IPL. The port
                                 will remain in that state until this parameter is changed"
        ::= {ipxInterfaceEntry 2}

ipxInterfaceType OBJECT-TYPE 
        SYNTAX INTEGER
                        { ethernet(1),
                          eight025(2),
                          x25(3),
                          frl(4)
                        }

        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The interface type. 802.5 is not valid on FRX4000"
        ::= {ipxInterfaceEntry 3}

ipxInterfaceFrameType OBJECT-TYPE 
        SYNTAX INTEGER
                        { typeII(1),
                          raw(2),
                          llc(3),
                          snap(4)
                        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The frame type - depends on the interfece type. Valid combinations are: 
                                 Ethernet, 802.5  - typeII, raw, llc, snap
                                 Frame relay, X25 - typeII"
        DEFVAL { typeII }
        ::= {ipxInterfaceEntry 4}

ipxInterfaceMaxTransUnit OBJECT-TYPE 
        SYNTAX INTEGER 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum frame size that can be transmitted or received over the IPX interface.: Valid ranges are:
                                 Ethernet                 - (45-1518)
                                 802.5                    - (48-4096)
                                 Frame relay, X25 - (31-4096) "
        DEFVAL { 4096 }
        ::= {ipxInterfaceEntry 5}

ipxInterfaceNetworkAddress OBJECT-TYPE 
        SYNTAX INTEGER 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Identifies the local interface to the Novell Network"
        DEFVAL { 0 }
        ::= {ipxInterfaceEntry 6}

ipxInterfaceBandwidthAllocGroup OBJECT-TYPE 
        SYNTAX INTEGER (1..16)  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Assigns the IPX interface to one of sixteen groups whose parameters regulate bandwidth usage"
        DEFVAL { 1 }
        ::= {ipxInterfaceEntry 7}

ipxInterfacePortDiagEnabled OBJECT-TYPE 
        SYNTAX INTEGER
                        { no(1),
                          yes(2)
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Enables/Disables the IPX interface's ability to handle Novell diagonistics packets"
        DEFVAL { no }
        ::= {ipxInterfaceEntry 8}

ipxInterfaceNetBIOSEnabled OBJECT-TYPE 
        SYNTAX INTEGER
                        { no(1),
                          yes(2)
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines whether Novell-encapsulated NetBIOS 
                                 frames received on the interface will be processed"
        DEFVAL { no }
        ::= {ipxInterfaceEntry 9}

ipxInterfaceNetBIOSHops OBJECT-TYPE 
        SYNTAX INTEGER (0..255)  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum number of hops allowed for routing a Novell-encapsulated NetBIOS frame"
        DEFVAL { 8 }
        ::= {ipxInterfaceEntry 10}

ipxInterfacePeriodicRIPEnabled OBJECT-TYPE 
        SYNTAX INTEGER  
                        { no(1),
                          yes(2)
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines whether the node will originate periodic IPX Routing Information Protocol messages
                                 from this interface to inform the network that the route through this interface is viable"
        DEFVAL { no }
        ::= {ipxInterfaceEntry 11}

ipxInterfacePeriodicRIPTimer OBJECT-TYPE 
        SYNTAX INTEGER (1..65535)  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "This is the interval between the periodic IPX RIP broadcasts from this interface"
        DEFVAL { 60 }
        ::= {ipxInterfaceEntry 12}

ipxInterfacePeriodicSAPEnabled OBJECT-TYPE 
        SYNTAX INTEGER  {
                                                no(1),
                                                yes(2)
                                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines whether the node will originate periodic IPX SAP messages
                                 from this interface to inform the network which SAP entries in the routing table are viable"
        DEFVAL { no }
        ::= {ipxInterfaceEntry 13}

ipxInterfacePeriodicSAPTimer OBJECT-TYPE 
        SYNTAX INTEGER (1..65535)  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The interval between the periodic SAP broadcasts from this interface"
        DEFVAL { 60 }
        ::= {ipxInterfaceEntry 14}

ipxInterfaceRIPEnabled OBJECT-TYPE 
        SYNTAX INTEGER  
                        { no(1),
                          yes(2)
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Datermines whether this interface will support RIP proceswsing "
        DEFVAL { no }
        ::= {ipxInterfaceEntry 15}

ipxInterfaceRIPAgeTimer OBJECT-TYPE 
        SYNTAX INTEGER (0..65535) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "This is used to delete route entries in the routing information table. The timer starts/restarts
                                 each time an entry is created/updated. If the timer expires, the router will assume that the entry is no
                                 longer valid and the entry will be deleteda from the table "
        DEFVAL { 180 }
        ::= {ipxInterfaceEntry 16}

ipxInterfaceRIPMaxSize OBJECT-TYPE 
        SYNTAX INTEGER  (54..446) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum possible RIP packet size "
        DEFVAL { 446 }
        ::= {ipxInterfaceEntry 17}

ipxInterfaceSAPEnabled OBJECT-TYPE 
        SYNTAX INTEGER 
                        { no(1),
                          yes(2)
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines whether the interface will support SAP or not "
        DEFVAL { no }
        ::= {ipxInterfaceEntry 18}

ipxInterfaceSAPAgeTimer OBJECT-TYPE 
        SYNTAX INTEGER (0..65535) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "This is used to delete route entries from the router information table. The timer starts/restars
                                 each time an entry is created/updated. If the timer expires, the router will assume that the entry is no
                                 longer valid and the entry will be deleted from the table "
        DEFVAL { 180 }
        ::= {ipxInterfaceEntry 19}

ipxInterfaceTransportTime OBJECT-TYPE 
        SYNTAX INTEGER (1..255) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "is the time (in 55 milliseconds unit) that will normally take to forward frames out of interface.
                                 Recommmended values are 1 for LAN interfaces and 30 for WAN interfaces. A value of 0 indicates that the
                                 back to back frame forwarding is acceptable. This time is used to calculate the least cost path during
                                 routing. If IPXWAMN is (Y), Transport time will be overridden by the value calculated by IPXWAN "
        DEFVAL { 1 }
        ::= {ipxInterfaceEntry 20}

ipxInterfaceSerializationEnabled OBJECT-TYPE 
        SYNTAX INTEGER 
                        { no(1),
                          yes(2)
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines whether NetWare file server serialization security frames will be 
                                 forwarded on the interface. These broadcasts frames are used by Novell to hold informations regarding the
                                 licensing of the file server executables "
        DEFVAL { no }
        ::= {ipxInterfaceEntry 21}

ipxInterfaceWatchdogSpoofingEnabled OBJECT-TYPE 
        SYNTAX INTEGER 
                        { no(1),
                          yes(2)
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines whether this interface will be used by the local node to respond to (keep alive) messages on
                                 behalf of the client workstations. Novell servers periodically issue these messages to all clients
                                 to determine whether each client is still alive "
        DEFVAL { no }
        ::= {ipxInterfaceEntry 22}

ipxInterfaceLanCardNumber OBJECT-TYPE
        SYNTAX INTEGER (0..1)  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The card number installed in an FRX6000. The first or only LAN card installed is always 0,
                                 and the second is card 1" 
        DEFVAL { 0 }
        ::= {ipxInterfaceEntry 23}

ipxInterfaceWanEnabled OBJECT-TYPE
        SYNTAX INTEGER
                        { no(1),
                          yes(2),
                          not-applicable(3) 
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Determines whether Novell's IPXWAN protocol will be used on the interface. IPXWAN specifies a method 
                                 for IPX routers to communicate across WAN links. FRX6000 and FRX4000 implement IPXWAN running over RFC 
                                 1490-complaint frame relay and RFC1356-complaint X.25" 
        DEFVAL { no }
        ::= {ipxInterfaceEntry 24}

ipxInterfaceSourceSubscriber OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(0..15)) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Subscruber id that defines an IPX interface in the node, by associating itself with port 66 (a
                                 number reserved for the IPXinterface) on the RLP that has an IPX installed on it. 
                                 .. Valid only for type X.25 " 
        ::= {ipxInterfaceEntry 25}

ipxInterfaceDestinationSubscriber OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(0..15)) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Subscriber ID associated with the physical X.25 port that will be used for the IPX interface .
                                 .. Valid only for type X.25 " 
        ::= {ipxInterfaceEntry 26}

ipxInterfaceSVCRetryTimer OBJECT-TYPE
        SYNTAX INTEGER (5..60) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The frequency with which calls will be placed to try to establish a connection 
                                 .. Valid only for type X.25 " 
        DEFVAL { 20 }
        ::= {ipxInterfaceEntry 27}

ipxInterfaceSVCIdleTimer OBJECT-TYPE
        SYNTAX INTEGER (0..5) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "is a period that an IPX connection can remain active with no traffic before the connection is cleared.
                                 .. Valid only for type X.25 " 
        DEFVAL { 1 }
        ::= {ipxInterfaceEntry 28}

ipxInterfaceMaxVC OBJECT-TYPE
        SYNTAX INTEGER (1..8) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "This specifies a number of virtual circuits over which IPX traffic will be transmitted in parallel.  
                                 .. Valid only for type X.25 " 
        DEFVAL { 1 }
        ::= {ipxInterfaceEntry 29 }

ipxInterfacePVCConnection OBJECT-TYPE
        SYNTAX INTEGER 
                        { no(1),
                          yes(2), 
                          not-applicable(3) 
                        } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Identifies this interface as one of a PVC.  
                                 .. Valid only for type X.25 " 
        DEFVAL { no }
        ::= {ipxInterfaceEntry 30}

ipxInterfaceSourceCard OBJECT-TYPE
        SYNTAX INTEGER (0..7) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Identifies the location of this end of the frame relay IPX interface.
                                 .. Valid only for frame relay " 
        DEFVAL { 0 }
        ::= {ipxInterfaceEntry 31}

ipxInterfaceSourcePort OBJECT-TYPE
        SYNTAX INTEGER (0..7) 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Identifies the location of this end of the frame relay IPX interface.
                                 .. Valid only for frame relay " 
        DEFVAL { 0 }
        ::= {ipxInterfaceEntry 32}

ipxInterfaceSourceDLCI OBJECT-TYPE
        SYNTAX INTEGER (16..991)  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Identifies the location of this end of the frame relay IPX interface.
                                 .. Valid only for frame relay " 
        DEFVAL { 16 }
        ::= {ipxInterfaceEntry 33}

ipxInterfaceRowStatus OBJECT-TYPE 
        SYNTAX RowStatus  
        ACCESS read-write
        STATUS mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the ipxInterfaceTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= {ipxInterfaceEntry 34}

-- The Node Default Group 

ipxConfigNodeDefault OBJECT IDENTIFIER ::= {ipxConfig 3}

ipxNodeDefaultConfigNetworkAddress OBJECT-TYPE 
    SYNTAX      INTEGER  
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION "Identifies the node to the IPX network" 
        ::= {ipxConfigNodeDefault 1}

ipxNodeDefaultConfigRIPSAPGap OBJECT-TYPE
    SYNTAX      INTEGER (0..100) 
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION "The minimum delay between consecutive RIP and SAP transmissions"
        ::= {ipxConfigNodeDefault 2}

ipxNodeDefaultConfigRouterName OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1..48))
        ACCESS  read-write
        STATUS  mandatory
        DESCRIPTION "An unique identifier within the IPX network" 
        ::= {ipxConfigNodeDefault 3}

--
--  The Netlink IP Interface Table
--

nlIfIpInterfaces OBJECT IDENTIFIER ::= { nlInterfaces 4}

nlIfIpTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlIfIpEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to define IP interfaces over frame relay,
                                X.25, or LAN (ethernet, 802.3, 802.5)."
        ::= { nlIfIpInterfaces 1 }

nlIfIpEntry OBJECT-TYPE
        SYNTAX NlIfIpEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An IP Interface entry containing objects relating
        to IP interfaces."
        INDEX { nlIfIpInterface }
        ::= { nlIfIpTable 1 }

NlIfIpEntry ::=
        SEQUENCE {
                nlIfIpInterface                 INTEGER,
                nlIfIpMtu                               INTEGER,
                nlIfIpNetworkMask               IpAddress,
                nlIfIpRouteMetric               INTEGER,
                nlIfIpICMPAddRoutes             INTEGER,
                nlIfIpRIPDeltaUpdates   INTEGER,
                nlIfIpRIPFullUpdates    INTEGER,
                nlIfIpPriority                  INTEGER,
                nlIfIpBAG                               INTEGER,
                nlIfIpType                              INTEGER,
                nlIfIpSourceAddress             IpAddress,
                nlIfIpDestAddress               IpAddress,
                nlIfIpBroadcastAddress  IpAddress,
                nlIfIpLANCard                   INTEGER,
                nlIfIpSourceSub                 NlSubscriberAddress,
                nlIfIpDestSub                   NlSubscriberAddress,
                nlIfIpSVCRetryTimer             INTEGER,
                nlIfIpSVCIdleTimer              INTEGER,
                nlIfIpMaxSVC                    INTEGER,
                nlIfIpPVCConnection             INTEGER,
                nlIfIpSourceRlp                 INTEGER,
                nlIfIpSourcePort                INTEGER,
                nlIfIpSourceDLCI                INTEGER,
                nlIfIpRIPSupport                INTEGER,
                nlIfIpInverseARP                INTEGER,
                nlIfIpProxyARP                  INTEGER,
                nlIfIpUnnumberedIf              INTEGER,
                nlIfIpRowStatus                 RowStatus
        }

nlIfIpInterface OBJECT-TYPE
        SYNTAX INTEGER (1..257)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The interface number which uniquely identifies the
                                interface to which this entry is applicable. The
                                interface identified by a particular value of this
                                number is NOT the same interface as defined by the
                                same value of ifIndex."
        ::= { nlIfIpEntry 1 }

nlIfIpMtu OBJECT-TYPE
        SYNTAX INTEGER (1..4096)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The maximum size (in bytes) of the data field that can
                                be used to encapsulate an IP datagram for transmission
                                over the interface. If the interface type is LAN based,
                                then the maximum size value cannot exceed 1500."
        DEFVAL { 4096 }
        ::= { nlIfIpEntry 2 }

nlIfIpNetworkMask OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The mask used during routing to determine the portion
                                of the address associated with the network."
        DEFVAL { 'FF000000'H }    -- 255.0.0.0
        ::= { nlIfIpEntry 3 }

nlIfIpRouteMetric OBJECT-TYPE
        SYNTAX INTEGER (0..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The number of network hops (network gateways in the
                                overall path over the internet) associated with this
                                interface."
        DEFVAL { 0 }
        ::= { nlIfIpEntry 4 }

nlIfIpICMPAddRoutes OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The flag which indicates whether IP may add routes
                                obtained by ICMP, whose error and control function
                                is used to send re-direction options back to the
                                source if problems are discovered."
        DEFVAL { yes }
        ::= { nlIfIpEntry 5 }

nlIfIpRIPDeltaUpdates OBJECT-TYPE
        SYNTAX INTEGER (10..300)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The frequency with which RIP messages will be sent to
                                every neighbor node, containing any changes to the
                                routing table that occurred since the last full update."
        DEFVAL { 30 }
        ::= { nlIfIpEntry 6 }

nlIfIpRIPFullUpdates OBJECT-TYPE
        SYNTAX INTEGER (10..300)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The frequency with which updates of the entire routing
                                table will be sent to every neighbor node, via one or
                                more RIP messages."
        DEFVAL { 60 }
        ::= { nlIfIpEntry 7 }

nlIfIpPriority OBJECT-TYPE
        SYNTAX INTEGER (0..9)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The priority setting for traffic within the node. The
                                higher the number, the higher the priority relative to
                                other intra-nodal traffic."
        DEFVAL { 5 }
        ::= { nlIfIpEntry 8 }

nlIfIpBAG OBJECT-TYPE
        SYNTAX INTEGER (1..16)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The bandwidth allocation group to which this interface
                                is assigned to. This object is only valid when the
                                interface type is frame relay or proprietary virtual."
        DEFVAL { 1 }
        ::= { nlIfIpEntry 9 }

nlIfIpType OBJECT-TYPE
        SYNTAX INTEGER {
                other(1),               -- none of the following
                rfc877x25(5),
                ethernetCsmacd(6),
                iso88023Csmacd(7),
                iso88025TokenRing(9),
                frameRelay(32),         -- DTE only
                propVirtual(53)         -- proprietary virtual/internal
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The type of IP interface."
        DEFVAL { rfc877x25 }
        ::= { nlIfIpEntry 10 }

nlIfIpSourceAddress OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The IP address of the end-to-end sender."
        DEFVAL { '00000000'H }    -- 0.0.0.0
        ::= { nlIfIpEntry 11 }

nlIfIpDestAddress OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The IP address of the end-to-end receiver. This object
                                is only valid when the interface type is X.25 or proprietary
                                virtual, or when the interface type is frame relay and the
                                inverse ARP flag indicates disabled."
        DEFVAL { '00000000'H }    -- 0.0.0.0
        ::= { nlIfIpEntry 12 }

nlIfIpBroadcastAddress OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The IP address that is used to send to all LAN hosts
                                on the network. This object is only valid when the
                                interface type is LAN based."
        DEFVAL { '00000000'H }    -- 0.0.0.0
        ::= { nlIfIpEntry 13 }

nlIfIpLANCard OBJECT-TYPE
        SYNTAX INTEGER (0..1)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The LAN card that contains the interface. This object
                                is only valid when the interface type is LAN based."
        DEFVAL { 0 }
        ::= { nlIfIpEntry 14 }

nlIfIpSourceSub OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The subscriber ID associated with the source IP
                                interface port. This object is only valid when the
                                interface type is X.25."
        ::= { nlIfIpEntry 15 }

nlIfIpDestSub OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The subscriber ID associated with the destination IP
                                interface port. This object is only valid when the
                                interface type is X.25."
        ::= { nlIfIpEntry 16 }

nlIfIpSVCRetryTimer OBJECT-TYPE
        SYNTAX INTEGER (5..60)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The frequency with which calls will be placed to try
                                to establish a connection. This object is only valid
                                when the interface type is X.25."
        DEFVAL { 20 }
        ::= { nlIfIpEntry 17 }

nlIfIpSVCIdleTimer OBJECT-TYPE
        SYNTAX INTEGER (0..5)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The period that an IP connection remains active with
                                no traffic before the connection is cleared. This object
                                is only valid when the interface type is X.25."
        DEFVAL { 1 }
        ::= { nlIfIpEntry 18 }

nlIfIpMaxSVC OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The number of virtual circuits over which IP traffic
                                will be transmitted in parallel. This object is only
                                valid when the interface type is X.25."
        DEFVAL { 1 }
        ::= { nlIfIpEntry 19 }

nlIfIpPVCConnection OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The flag which indicates whether this interface is a
                                PVC. This object is only valid when the interface type
                                is X.25."
        DEFVAL { no }
        ::= { nlIfIpEntry 20 }

nlIfIpSourceRlp OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The RLP of the logical interface of this end of the frame
                                relay link. This object is only valid when the interface
                                type is frame relay."
        DEFVAL { 1 }
        ::= { nlIfIpEntry 21 }

nlIfIpSourcePort OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The port of the logical interface of this end of the frame
                                relay link. This object is only valid when the interface
                                type is frame relay."
        DEFVAL { 1 }
        ::= { nlIfIpEntry 22 }

nlIfIpSourceDLCI OBJECT-TYPE
        SYNTAX INTEGER (16..991)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The DLCI of the logical interface of this end of the frame
                                relay link. This object is only valid when the interface
                                type is frame relay."
        DEFVAL { 16 }
        ::= { nlIfIpEntry 23 }

nlIfIpRIPSupport OBJECT-TYPE
        SYNTAX INTEGER {
                disabled(1),
                enabled(2),
                receive-only(3)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The RIP support that is being run on the interface."
        DEFVAL { enabled }
        ::= { nlIfIpEntry 24 }

nlIfIpInverseARP OBJECT-TYPE
        SYNTAX INTEGER {
                disabled(1),
                enabled(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The flag which indicates whether inverse ARP is enabled
                                or disabled. This object is only valid when the interface
                                type is frame relay."
        DEFVAL { disabled }
        ::= { nlIfIpEntry 25 }

nlIfIpProxyARP OBJECT-TYPE
        SYNTAX INTEGER {
                disabled(1),
                enabled(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The flag which indicates whether proxy ARP is enabled
                                or disabled. This object is only valid when the interface
                                type is LAN based."
        DEFVAL { disabled }
        ::= { nlIfIpEntry 26 }

nlIfIpUnnumberedIf OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The flag which indicates whether this interface is an
                                unnumbered interface (i.e., does not require a specific
                                source IP address). This object is only valid when the
                                interface type is frame relay or X.25."
        DEFVAL { yes }
        ::= { nlIfIpEntry 27 }

nlIfIpRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlIfIpTable and follows the SNMPv2
            RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { nlIfIpEntry 28 }

--
--  The Netlink IP Interface Secondary Addresses Table
--

nlIfIpSecondaryAddrTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlIfIpSecondaryAddrEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to define secondary IP interfaces on a
                                LAN (ethernet, 802.3, 802.5) interface."
        ::= { nlIfIpInterfaces 2 }

nlIfIpSecondaryAddrEntry OBJECT-TYPE
        SYNTAX NlIfIpSecondaryAddrEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An IP Secondary Address entry containing objects relating
        to IP secondary addresses."
        INDEX { nlIfIpInterface, nlIfIpSecondaryAddrSequence }
        ::= { nlIfIpSecondaryAddrTable 1 }

NlIfIpSecondaryAddrEntry ::=
        SEQUENCE {
                nlIfIpSecondaryAddrSequence                             INTEGER,
                nlIfIpSecondaryAddrNetworkMask                  IpAddress,
                nlIfIpSecondaryAddrRouteMetric                  INTEGER,
                nlIfIpSecondaryAddrSourceAddress                IpAddress,
                nlIfIpSecondaryAddrBroadcastAddress             IpAddress,
                nlIfIpSecondaryAddrRIPSupport                   INTEGER,
                nlIfIpSecondaryAddrRowStatus                    RowStatus
        }

nlIfIpSecondaryAddrSequence OBJECT-TYPE
        SYNTAX INTEGER (1..15)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The maximum number of secondary IP addresses that may
                                be configured on an interface."
        ::= { nlIfIpSecondaryAddrEntry 1 }

nlIfIpSecondaryAddrNetworkMask OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The mask used during routing to determine the portion
                                of the address associated with the network."
        DEFVAL { '00000000'H }    -- 0.0.0.0
        ::= { nlIfIpSecondaryAddrEntry 2 }

nlIfIpSecondaryAddrRouteMetric OBJECT-TYPE
        SYNTAX INTEGER (0..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The number of network hops (network gateways in the
                                overall path over the internet) associated with this
                                interface."
        DEFVAL { 0 }
        ::= { nlIfIpSecondaryAddrEntry 3 }

nlIfIpSecondaryAddrSourceAddress OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The IP address of the end-to-end sender."
        DEFVAL { '00000000'H }    -- 0.0.0.0
        ::= { nlIfIpSecondaryAddrEntry 4 }

nlIfIpSecondaryAddrBroadcastAddress OBJECT-TYPE
        SYNTAX IpAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The IP address that is used to send to all LAN hosts
                                on the network."
        DEFVAL { '00000000'H }    -- 0.0.0.0
        ::= { nlIfIpSecondaryAddrEntry 5 }

nlIfIpSecondaryAddrRIPSupport OBJECT-TYPE
        SYNTAX INTEGER {
                disabled(1),
                enabled(2),
                receive-only(3)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The RIP support that is being run on the interface."
        DEFVAL { enabled }
        ::= { nlIfIpSecondaryAddrEntry 6 }

nlIfIpSecondaryAddrRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion of
            conceptual rows in the nlIfIpSecondaryAddrTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { nlIfIpSecondaryAddrEntry 7 }

nlIfVoiceInterfaces OBJECT IDENTIFIER ::= { nlInterfaces 5}

--
--  The Netlink Voice Interface Table
--

nlIfVoiceTable OBJECT-TYPE
    SYNTAX SEQUENCE OF NlIfVoiceEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION "A Table to define Voice interfaces over frame relay."
    ::= { nlIfVoiceInterfaces 1 }

nlIfVoiceEntry OBJECT-TYPE
    SYNTAX NlIfVoiceEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
            "A Voice Interface entry containing objects relating
            to the interface that are configurable by the user."
    INDEX { nlIfVoiceInterface }
    ::= { nlIfVoiceTable 1 }

NlIfVoiceEntry ::=
    SEQUENCE {
        nlIfVoiceInterface          INTEGER,
        nlIfVoicePeerNodeType       INTEGER,
        nlIfVoicePeerNodeNumber     INTEGER,
        nlIfVoicePeerNodePort       INTEGER,
        nlIfVoiceLocalNodeNumber    INTEGER,
        nlIfVoiceLocalNodePort      INTEGER,
        nlIfVoiceFrameRelayRlp      INTEGER,
        nlIfVoiceFrameRelayPort     INTEGER,
        nlIfVoiceFrameRelayDLCI     INTEGER,
        nlIfVoiceEnableFragment     INTEGER,
        nlIfVoiceRowStatus          RowStatus
    }

nlIfVoiceInterface OBJECT-TYPE
    SYNTAX INTEGER (1..129)
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The interface number which uniquely identifies the
                interface to which this entry is applicable. The
                interface identified by a particular value of this
                number is NOT the same interface as defined by the
                same value of ifIndex."
    ::= { nlIfVoiceEntry 1 }

nlIfVoicePeerNodeType OBJECT-TYPE
    SYNTAX INTEGER {
                netlink (1),
                act (2)
                }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The node type for the node at the remote end of the
                frame relay connection."
    DEFVAL { act }
    ::= { nlIfVoiceEntry 2 }

nlIfVoicePeerNodeNumber OBJECT-TYPE
    SYNTAX INTEGER (1..61)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The node number of the remote device."
    DEFVAL { 1 }
    ::= { nlIfVoiceEntry 3 }

nlIfVoicePeerNodePort OBJECT-TYPE
    SYNTAX INTEGER (1..17)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The voice port on the remote device."
    DEFVAL { 1 }
    ::= { nlIfVoiceEntry 4 }

nlIfVoiceLocalNodeNumber OBJECT-TYPE
    SYNTAX INTEGER (1..61)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The node number of the local device."
    DEFVAL { 1 }
    ::= { nlIfVoiceEntry 5 }

nlIfVoiceLocalNodePort OBJECT-TYPE
    SYNTAX INTEGER (1..17)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The voice port on the local device."
    DEFVAL { 1 }
    ::= { nlIfVoiceEntry 6 }

nlIfVoiceFrameRelayRlp OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The RLP of the logical interface of this end of the frame
                relay link."
    DEFVAL { 1 }
    ::= { nlIfVoiceEntry 7 }

nlIfVoiceFrameRelayPort OBJECT-TYPE
    SYNTAX INTEGER (1..8)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The port of the logical interface of this end of the frame
                relay link."
    DEFVAL { 1 }
    ::= { nlIfVoiceEntry 8 }

nlIfVoiceFrameRelayDLCI OBJECT-TYPE
    SYNTAX INTEGER (16..991)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The DLCI of the logical interface of this end of the frame
                relay link."
    DEFVAL { 16 }
    ::= { nlIfVoiceEntry 9 }

nlIfVoiceEnableFragment OBJECT-TYPE
    SYNTAX  INTEGER {
                no (1),
                yes (2)
                }
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION ""
    DEFVAL { no }
    ::= { nlIfVoiceEntry 10 }

nlIfVoiceRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the noIfVoiceTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
    ::= { nlIfVoiceEntry 11 }

-- **************************
-- *  THE SUBSCRIBER GROUP  *
-- **************************

subscriber OBJECT IDENTIFIER ::=    { local 5 }

--
--  The Netlink Local Subscriber Table
--

nlLocalSubscriberTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlLocalSubscriberEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to define each local subscriber."
        ::= { subscriber 1 }

nlLocalSubscriberEntry OBJECT-TYPE
        SYNTAX NlLocalSubscriberEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Local Subscriber entry containing objects relating
        to local subscribers."
        INDEX { nlLocalSubscriberId }
        ::= { nlLocalSubscriberTable 1 }

NlLocalSubscriberEntry ::=
        SEQUENCE {
                nlLocalSubscriberId                                     NlSubscriberAddress,
                nlLocalSubscriberName                           DisplayString,
                nlLocalSubscriberAlgorithm                      INTEGER,
                nlLocalSubscriberSystematicRedirect     INTEGER,
                nlLocalSubscriberRedirectBusy           INTEGER,
                nlLocalSubscriberRedirectOO                     INTEGER,
                nlLocalSubscriberPriority                       INTEGER,
                nlLocalSubscriberRowStatus                      RowStatus
        }

nlLocalSubscriberId OBJECT-TYPE
        SYNTAX  NlSubscriberAddress
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Subscriber ID.  A valid subscriber ID is a string of
                numeric digits represented by their ASCII equivalents.  The
                ASCII equivalents of the wildcard characters '*' and '?' are 
                also allowed.  A '*' is a wildcard that matches any number of 
                digits, including zero. A '?' is a wildcard that matches any single digit."
        ::= { nlLocalSubscriberEntry 1 }

nlLocalSubscriberName OBJECT-TYPE
        SYNTAX DisplayString (SIZE (0..31))
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Subscriber name.  The subscriber name is not accessible from 
                     SNMP, and a blank string is always returned."
        ::= { nlLocalSubscriberEntry 2 }

nlLocalSubscriberAlgorithm OBJECT-TYPE
        SYNTAX INTEGER {
                round-robin(1),
                line-failed(2),
                line-busy(3),
                least-lcn(4)
                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The Subscriber routing algorithm.
                        The following 4 types of routing algorithms are supported.
                        1 - round robin selects ports specified cyclicly in numerical
                        order according to the list of Redirection addresses. If the port
                        is unreachable or congested, the call request is sent to the next
                        port.
                        2. Alternate Route on Line Failure - selects the first port
                         not in a failed state. If a connection is not made, the call
                        will be cleared even if other ports are available.
                        3. Alternate Route on Line Busy - selects the first port
                        that has LCN's available (not busy). If a port has failed,
                        the next available port is selected.
                        4. Least LCN with throughput selects the line with the minumum
                        loading, calculated by weight and number of LCN's in use.

                        If use of a routing algorithm is not desired, accept the default
                        and specify only one routing path."
        DEFVAL { round-robin }
        ::= { nlLocalSubscriberEntry 3 }

nlLocalSubscriberSystematicRedirect OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Systematic Redirection."
    DEFVAL { no }       
        ::= { nlLocalSubscriberEntry 4 }

nlLocalSubscriberRedirectBusy OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Redirect calls according to Redirection Addresses if the
                primary subscriber device is busy."
    DEFVAL { no }       
        ::= { nlLocalSubscriberEntry 5 }

nlLocalSubscriberRedirectOO OBJECT-TYPE
        SYNTAX INTEGER {
                no(1),
                yes(2)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Redirect calls according to Redirection Addresses if the
                primary subscriber device is out of order."
    DEFVAL { no }       
        ::= { nlLocalSubscriberEntry 6 }

nlLocalSubscriberPriority OBJECT-TYPE
        SYNTAX INTEGER (0..9)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Allows setting a priority for traffic within the node."
    DEFVAL { 0 }        
        ::= { nlLocalSubscriberEntry 7 }

nlLocalSubscriberRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlLocalSubscriberTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."

        ::= { nlLocalSubscriberEntry 8 }

-- Routing Paths Table.

nlLocalSubscriberRouteTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlLocalSubscriberRouteEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to define local subscriber route paths."
        ::= { subscriber 2 }

nlLocalSubscriberRouteEntry OBJECT-TYPE
        SYNTAX NlLocalSubscriberRouteEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Local Subscriber Route entry containing objects relating
        to local subscriber routes."
        INDEX { nlLocalSubscriberId, nlLocalSubscriberRouteIndex}
        ::= { nlLocalSubscriberRouteTable 1 }

NlLocalSubscriberRouteEntry ::=
        SEQUENCE {
                nlLocalSubscriberRouteIndex             INTEGER,
                nlLocalSubscriberRouteConf              INTEGER,
                nlLocalSubscriberRouteLP                INTEGER,
                nlLocalSubscriberRoutePort              INTEGER,
                nlLocalSubscriberRouteRowStatus RowStatus
        }

nlLocalSubscriberRouteIndex OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Route path index for a specific subscriber route path."
        ::= { nlLocalSubscriberRouteEntry 1 }

nlLocalSubscriberRouteConf OBJECT-TYPE
        SYNTAX INTEGER  {
                no(1),
                yes(2)
        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Flag to indicate if the LP/port routing path to the
                subscriber device is configured or not. This object is read-
                only. The route is always configured for an entry in the table."
        ::= { nlLocalSubscriberRouteEntry 2 }

nlLocalSubscriberRouteLP OBJECT-TYPE
        SYNTAX INTEGER  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Instance of the LP that makes up the routing path"
        ::= { nlLocalSubscriberRouteEntry 3 }

nlLocalSubscriberRoutePort OBJECT-TYPE
        SYNTAX INTEGER  
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Instance of the port that makes up the routing path"
        ::= { nlLocalSubscriberRouteEntry 4 }

nlLocalSubscriberRouteRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlLocalSubscriberRouteTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."

        ::= { nlLocalSubscriberRouteEntry 5 }

--- Redirection Address table.

nlLocalSubscriberRedirTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlLocalSubscriberRedirEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to list local subscriber redirection addresses."
        ::= { subscriber 3 }

nlLocalSubscriberRedirEntry OBJECT-TYPE
        SYNTAX NlLocalSubscriberRedirEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Local Subscriber Redirection Address entry containing
        objects relating to local subscriber redirection addresses."
        INDEX { nlLocalSubscriberId, nlLocalSubscriberRedirIndex }
        ::= { nlLocalSubscriberRedirTable 1 }

NlLocalSubscriberRedirEntry ::=
        SEQUENCE {
                nlLocalSubscriberRedirIndex             INTEGER,
                nlLocalSubscriberRedirAddr              NlSubscriberAddress,
                nlLocalSubscriberRedirRowStatus RowStatus
        }

nlLocalSubscriberRedirIndex OBJECT-TYPE
        SYNTAX INTEGER (1..5)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Redirection entry index for a local subscriber."
        ::= { nlLocalSubscriberRedirEntry 1 }

nlLocalSubscriberRedirAddr OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Subscriber redirection address."
        ::= { nlLocalSubscriberRedirEntry 2 }

nlLocalSubscriberRedirRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlLocalSubscriberRedirTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { nlLocalSubscriberRedirEntry 3 }

-- ********************
-- *  THE LLC2 GROUP  *
-- ********************

llc2 OBJECT IDENTIFIER ::=    { local 6 }

--
--  The Netlink LLC2 Host Table
--

nlLlc2HostTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlLlc2HostEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to define LLC2 host entries."
        ::= { llc2 1 }

nlLlc2HostEntry OBJECT-TYPE
        SYNTAX NlLlc2HostEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An LLC2 Host entry containing objects relating to
        LLC2 hosts."
        INDEX { nlLlc2HostGroup, nlLlc2HostIndex }
        ::= { nlLlc2HostTable 1 }

NlLlc2HostEntry ::=
        SEQUENCE {
                nlLlc2HostIndex                                 INTEGER,
                nlLlc2HostMACAddress                    MacAddress,
                nlLlc2HostSessionType                   INTEGER,
                nlLlc2HostT1ReplyTimer                  TimeInterval,
                nlLlc2HostT2RecvAckTimer                TimeInterval,
                nlLlc2HostTiInactivityTimer             TimeInterval,
                nlLlc2HostN3NumberLPDUs                 INTEGER,
                nlLlc2HostTwNumberOutstanding   INTEGER,
                nlLlc2HostN2ExpiredT1LPDUCount  INTEGER,
                nlLlc2HostPriority                              INTEGER,
                nlLlc2HostBAG                                   INTEGER,
                nlLlc2HostRoutingSubscriberId   NlSubscriberAddress,
                nlLlc2HostSrcMACAddressMask             MacAddress,
                nlLlc2HostAccess                                INTEGER,
                nlLlc2HostRowStatus                             RowStatus,
                nlLlc2HostInterface                             INTEGER,
                nlLlc2HostGroup                         INTEGER
        }

nlLlc2HostIndex OBJECT-TYPE
        SYNTAX INTEGER  (1..251)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "LLC2 Host Index"
        ::= { nlLlc2HostEntry 1 }

nlLlc2HostMACAddress OBJECT-TYPE
        SYNTAX MacAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The LLC2 Host MAC Address."
        DEFVAL { '400000000001'H }    -- 40:00:00:00:00:01
        ::= { nlLlc2HostEntry 2 }

nlLlc2HostSessionType OBJECT-TYPE
        SYNTAX INTEGER {
                originated(1),
                terminated(2)
                }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The mode in which the Host is operating"
        DEFVAL { terminated }
        ::= { nlLlc2HostEntry 3 }

nlLlc2HostT1ReplyTimer OBJECT-TYPE
        SYNTAX TimeInterval (1..250)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Reply Timer used to detect a failure of the Remote node."
        DEFVAL { 10 }
        ::= { nlLlc2HostEntry 4 }

nlLlc2HostT2RecvAckTimer OBJECT-TYPE
        SYNTAX TimeInterval (100..5000)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Receive Ack Timer used to delay sending an
                acknowledgement of a received information LPDU."
        DEFVAL { 100 }
        ::= { nlLlc2HostEntry 5 }

nlLlc2HostTiInactivityTimer OBJECT-TYPE
        SYNTAX TimeInterval (1..50)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Timer used to detect inoperative condition of the
                remote link station or transmission medium."
        DEFVAL { 30 }
        ::= { nlLlc2HostEntry 6 }

nlLlc2HostN3NumberLPDUs OBJECT-TYPE
        SYNTAX INTEGER (1..127)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The number of Information LPDUs that need to be received
                before an acknowledgement is sent."
        DEFVAL { 3 }
        ::= { nlLlc2HostEntry 7 }

nlLlc2HostTwNumberOutstanding OBJECT-TYPE
        SYNTAX INTEGER (1..127)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum number of sequentially numbered information
                LPDUs that can be outstanding at any time."
        DEFVAL { 7 }
        ::= { nlLlc2HostEntry 8 }

nlLlc2HostN2ExpiredT1LPDUCount OBJECT-TYPE
        SYNTAX INTEGER (0..255)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Maximum number of LPDU retransmissions occur following
                the expiration of Timer T1."
        DEFVAL { 8 }
        ::= { nlLlc2HostEntry 9 }

nlLlc2HostPriority OBJECT-TYPE
        SYNTAX INTEGER (0..9)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Traffic priorities within the node."
        DEFVAL { 0 }
        ::= { nlLlc2HostEntry 10 }

nlLlc2HostBAG OBJECT-TYPE
        SYNTAX INTEGER (1..16)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Bandwidth Allocation group to which the LLC2 Host belongs.
                This object is read-only. Bandwidth allocation groups do not apply
                to LLC2 hosts."
        DEFVAL { 1 }
        ::= { nlLlc2HostEntry 11 }

nlLlc2HostRoutingSubscriberId OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "LLC2 hosts Routing Subscriber Id"
        ::= { nlLlc2HostEntry 12 }

nlLlc2HostSrcMACAddressMask OBJECT-TYPE
        SYNTAX MacAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "LLC2 Host's Source MAC Address Mask"
        DEFVAL { '000000000000'H }    -- 00:00:00:00:00:00
        ::= { nlLlc2HostEntry 13 }

nlLlc2HostAccess OBJECT-TYPE
        SYNTAX INTEGER {
         lan(1),
         frameRelay(2),
         tokenRing(3),
         ethernet(4),
         all(5),
         not-applicable(6)
        }
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Specifies different type(s) of interface(s) that can be
                used for connections to a terminated host session."
        DEFVAL { not-applicable }
        ::= { nlLlc2HostEntry 14 }

nlLlc2HostRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Row status convention for LLC2 Host entry."
        ::= { nlLlc2HostEntry 15 }

nlLlc2HostInterface OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "LLC2 interface number associated with this host entry, always
        300 for non-FRX7000."
        DEFVAL { 300 }
        ::= { nlLlc2HostEntry 16 }

nlLlc2HostGroup OBJECT-TYPE
        SYNTAX INTEGER (1..4)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Traffic group associated with LLC2 interface, always 1 for
        non-FRX7000."
        ::= { nlLlc2HostEntry 17 }

-- LLC2 Terminated Host Connection Table.
--
nlLlc2TermConnectionTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlLlc2TermConnectionEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe LLC2 Terminated Host Connections."
        ::= { llc2 2 }

nlLlc2TermConnectionEntry OBJECT-TYPE
        SYNTAX NlLlc2TermConnectionEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An LLC2 Terminated Host Connection entry containing
        objects relating to LLC2 terminated host connections."
        INDEX { nlLlc2HostGroup, nlLlc2HostIndex, nlLlc2TermConnectionSequence }
        ::= { nlLlc2TermConnectionTable 1 }

NlLlc2TermConnectionEntry ::=
        SEQUENCE {
                nlLlc2TermConnectionSequence                    INTEGER,
                nlLlc2TermConnectionHSAP                                INTEGER,
                nlLlc2TermConnectionLocalSubscriberId   NlSubscriberAddress,
                nlLlc2TermConnectionRemoteSubscriberId  NlSubscriberAddress,
                nlLlc2TermConnectionRowStatus                   RowStatus
        }

nlLlc2TermConnectionSequence OBJECT-TYPE
        SYNTAX INTEGER (1..16)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "LLC2 Host connection Sequence number"
        ::= { nlLlc2TermConnectionEntry 1 }

nlLlc2TermConnectionHSAP OBJECT-TYPE
        SYNTAX INTEGER (4..254)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Service Access point used to connect to the Host"
        DEFVAL { 4 }
        ::= { nlLlc2TermConnectionEntry 2 }

nlLlc2TermConnectionLocalSubscriberId OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "LLC2 Host Connection's Local Subscriber Id"
        ::= { nlLlc2TermConnectionEntry 3 }

nlLlc2TermConnectionRemoteSubscriberId OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "LLC2 Host Connection's Remote Subscriber Id"
        ::= { nlLlc2TermConnectionEntry 4 }

nlLlc2TermConnectionRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlLlc2TermConnectionTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { nlLlc2TermConnectionEntry 5 }

-- LLC2 Originated Host Connection Table.
--
nlLlc2OrigConnectionTable OBJECT-TYPE
        SYNTAX SEQUENCE OF NlLlc2OrigConnectionEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe LLC2 Originated Host Connections."
        ::= { llc2 3 }

nlLlc2OrigConnectionEntry OBJECT-TYPE
        SYNTAX NlLlc2OrigConnectionEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An LLC2 Originated Host Connection entry containing
        objects relating to LLC2 originated host connections."
        INDEX { nlLlc2HostGroup, nlLlc2HostIndex, nlLlc2OrigConnectionSequence }
        ::= { nlLlc2OrigConnectionTable 1 }

NlLlc2OrigConnectionEntry ::=
        SEQUENCE {
                nlLlc2OrigConnectionSequence                    INTEGER,
                nlLlc2OrigConnectionHSAP                                INTEGER,
                nlLlc2OrigConnectionType                                INTEGER,
                nlLlc2OrigConnectionLocalSubscriberId   NlSubscriberAddress,
                nlLlc2OrigConnectionRemoteSubscriberId  NlSubscriberAddress,
                nlLlc2OrigConnectionIDBLK                               INTEGER,
                nlLlc2OrigConnectionIDNUM                               INTEGER,
                nlLlc2OrigConnectionMAXDATA                             INTEGER,
                nlLlc2OrigConnectionMAXIN                               INTEGER,
                nlLlc2OrigConnectionRowStatus                   RowStatus
        }

nlLlc2OrigConnectionSequence OBJECT-TYPE
        SYNTAX INTEGER (1..16)
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "LLC2 Host connection Sequence number"
        ::= { nlLlc2OrigConnectionEntry 1 }

nlLlc2OrigConnectionHSAP OBJECT-TYPE
        SYNTAX INTEGER (4..254)
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Service Access point used to connect to the Host"
        DEFVAL { 4 }
        ::= { nlLlc2OrigConnectionEntry 2 }

nlLlc2OrigConnectionType OBJECT-TYPE
        SYNTAX INTEGER {
                sdlc(1),
                llc2(2)
                } 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "Specifies Remote subscriber device type"
        DEFVAL { llc2 }
        ::= { nlLlc2OrigConnectionEntry 3 }

nlLlc2OrigConnectionLocalSubscriberId OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "LLC2 Host Connection's Local Subscriber Id"
        ::= { nlLlc2OrigConnectionEntry 4 }

nlLlc2OrigConnectionRemoteSubscriberId OBJECT-TYPE
        SYNTAX NlSubscriberAddress
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "LLC2 Host Connection's Remote Subscriber Id"
        ::= { nlLlc2OrigConnectionEntry 5 }

nlLlc2OrigConnectionIDBLK OBJECT-TYPE
        SYNTAX INTEGER 
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "This field is obsolete"
        DEFVAL { 0 }
        ::= { nlLlc2OrigConnectionEntry 6 }

nlLlc2OrigConnectionIDNUM OBJECT-TYPE
        SYNTAX INTEGER 
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "This field is obsolete"
        DEFVAL { 0 }
        ::= { nlLlc2OrigConnectionEntry 7 }

nlLlc2OrigConnectionMAXDATA OBJECT-TYPE
        SYNTAX INTEGER 
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "This field is obsolete"
        DEFVAL { 0 }
        ::= { nlLlc2OrigConnectionEntry 8 }

nlLlc2OrigConnectionMAXIN OBJECT-TYPE
        SYNTAX INTEGER 
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "This field is obsolete"
        DEFVAL { 0 }
        ::= { nlLlc2OrigConnectionEntry 9 }

nlLlc2OrigConnectionRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION 
            "This variable is used to manage the creation and deletion
            of conceptual rows in the nlLlc2OrigConnectionTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
        ::= { nlLlc2OrigConnectionEntry 10 }

nlLlc2NextHostNumber OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The host number to be used for the next created
        host record, always 1 on non-FRX7000."
            DEFVAL { 1 }
        ::= { llc2 4 }

-- **********************
-- *  THE STATUS GROUP  *
-- **********************

status  OBJECT IDENTIFIER ::=   { local 7 }

--
--  The Port Pin Status Table
--

pinStatusTable OBJECT-TYPE
        SYNTAX SEQUENCE OF PortPinEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe the status of each pin on a 
        physical port. This table is indexed by RLP and Port"
        ::= { status 4 }

portPinEntry OBJECT-TYPE
        SYNTAX PortPinEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A port pin entry containing objects relating to ports."
        INDEX { portPinRlp,portPinPort }
        ::= { pinStatusTable 1 }

PortPinEntry ::=
        SEQUENCE {
                portPinRlp
                        INTEGER,
                portPinPort
                        INTEGER,
                portPinStatus
                        OCTET STRING
        }

portPinRlp OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP number on the node"
        ::= { portPinEntry 1 }

portPinPort OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port number on the RLP. Port numbers 0-7 are
        known to be physical ports."
        ::= { portPinEntry 2 }

portPinStatus OBJECT-TYPE
        SYNTAX OCTET STRING
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The status of all pins for this physical port. There
        is one octet value for each of the pins. Each octet value is defined
        as follows:
                00 = unknown
                01 = active
                02 = inactive
                03 = unused "
        ::= { portPinEntry 3 }

-- **************************
-- *  THE STATISTICS GROUP  *
-- **************************

statistics OBJECT IDENTIFIER ::=        { local 8 }
statGroup OBJECT IDENTIFIER ::=         { statistics 1 }

--
-- The RLP Statistics group define the RLPStats Table
--

rlpStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF RlpStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe Statistics on each RLP"
        ::= { statGroup 2 }

rlpStatsEntry OBJECT-TYPE
        SYNTAX RlpStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An RLP statistics entry containing objects relating
        to RLP statistics."
        INDEX { rlpStatsIndex }
        ::= { rlpStatsTable 1 }

RlpStatsEntry ::=
        SEQUENCE {
                rlpStatsIndex
                        INTEGER,
                rlpStatsUsedBuffers
                        Counter,
                rlpStatsQMessages
                        Counter,
                rlpStatsInFrames
                        Counter,
                rlpStatsOutFrames
                        Counter,
                rlpStatsFrameRejects
                        Counter,
                rlpStatsFrameRetransmits
                        Counter
        }
rlpStatsIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP number"
        ::= { rlpStatsEntry 1 }

rlpStatsQMessages OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames queued on the RLP"
        ::= { rlpStatsEntry 2 }

rlpStatsUsedBuffers OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The percentage of total buffers available being used at
        the moment of inquiry"
        ::= { rlpStatsEntry 3 }

rlpStatsInFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames received."
        ::= { rlpStatsEntry 4 }

rlpStatsOutFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames transmitted."
        ::= { rlpStatsEntry 5 }

rlpStatsFrameRejects OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames rejected."
        ::= { rlpStatsEntry 6 }

rlpStatsFrameRetransmits OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames retransmitted . If
        this value is consistently greater than zero and there are no other
        problems, then increase the retransmission parameter."
        ::= { rlpStatsEntry 7 }

--
-- The Port Statistics group define the portStats Table
--

portStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF PortStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe Statistics on each RLP"
        ::= { statGroup 3 }

portStatsEntry OBJECT-TYPE
        SYNTAX PortStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A port statistics entry containing objects relating
        to port statistics."
        INDEX { portStatsRlpIndex, portStatsIndex }
        ::= { portStatsTable 1 }

PortStatsEntry ::=
        SEQUENCE {
                portStatsRlpIndex
                        INTEGER,
                portStatsIndex
                        INTEGER,
                portStatsInFrames
                        Counter,
                portStatsOutFrames
                        Counter,
                portStatsFrameRetrans
                        Counter,
                portStatsFCSErrors
                        Counter,
                portStatsLogicalRejects
                        Counter,
                portStatsInPercentUtils
                        Counter,
                portStatsOutPercentUtils
                        Counter
        }

portStatsRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP number"
        ::= { portStatsEntry 1 }

portStatsIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port number"
        ::= { portStatsEntry 2 }

portStatsInFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames received."
        ::= { portStatsEntry 3 }

portStatsOutFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames transmitted."
        ::= { portStatsEntry 4 }

portStatsFrameRetrans OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames retransmitted."
        ::= { portStatsEntry 5 }

portStatsFCSErrors OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of Frame Check Sequence (FCS) errors.
        A value consistently greater than zero indicates line probelms."
        ::= { portStatsEntry 6 }

portStatsLogicalRejects OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The sum of Rejects and Frame Rejects. 
        A value consistently greater than zero indicates line probelms."
        ::= { portStatsEntry 7 }

portStatsInPercentUtils OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The ratio of non-flag characters to total characters
        being received by the port."
        ::= { portStatsEntry 8 }

portStatsOutPercentUtils OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The ration of non-flag characters to total characters
        being transmitted by the port."
        ::= { portStatsEntry 9 }

statFrame OBJECT IDENTIFIER ::=                 { statGroup 4 }

--
-- The Frame Relay Frame Level Statistics group defines the FlvFRStats Table
--

frStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF FrStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe Frame Relay Frame Level Statistics on each Port"
        ::= { statFrame 1}

frStatsEntry OBJECT-TYPE
        SYNTAX FrStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A frame relay port statistics entry containing objects
        relating to frame relay port statistics."
        INDEX { frStatsRlpIndex, frStatsPortIndex }
        ::= { frStatsTable 1 }

FrStatsEntry ::=
        SEQUENCE {
                frStatsRlpIndex
                        INTEGER,
                frStatsPortIndex
                        INTEGER,
                frStatsRxDEFrames
                        Counter,
                frStatsTxDEFrames
                        Counter,
                frStatsTxFECNFrames
                        Counter,
                frStatsRxFECNFrames
                        Counter,
                frStatsTxBECNFrames
                        Counter,
                frStatsRxBECNFrames
                        Counter,
                frStatsTxLMIFrames
                        Counter,
                frStatsRxLMIFrames
                        Counter,
                frStatsTxANXDFrames
                        Counter,
                frStatsRxANXDFrames
                        Counter,
                frStatsTotDiscFrames
                        Counter
-- For the current time, we don't separate Discarded Frames
--              frStatsTxDiscFrames
--                      Counter,
--              frStatsRxDiscFrames
--                      Counter
}
frStatsRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP Number."
        ::= { frStatsEntry 1 }

frStatsPortIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port number."
        ::= { frStatsEntry 2 }

frStatsTxDEFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames transmitted on the port with the
                 Discard Eligibility bit set."
        ::= { frStatsEntry 3 }

frStatsRxDEFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames received on the port with the discard
                                 eligibility bit set."
        ::= { frStatsEntry 4 }

frStatsTxFECNFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The of number of frames transmitted on the port with FECN."
        ::= { frStatsEntry 5 }

frStatsRxFECNFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames received on the port with FECN."
        ::= { frStatsEntry 6 }

frStatsTxBECNFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames transmitted on the port with BECN."
        ::= { frStatsEntry 7 }

frStatsRxBECNFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of frames received on the port with BECN."
        ::= { frStatsEntry 8 }

frStatsTxLMIFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of LMI frames transmitted on the port."
        ::= { frStatsEntry 9 }

frStatsRxLMIFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of LMI frames received on the port."
        ::= { frStatsEntry 10 }

frStatsTxANXDFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of AnnexD frames transmitted on the port"
        ::= { frStatsEntry 11 }
--
frStatsRxANXDFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of AnnexD frames received on the port"
        ::= { frStatsEntry 12 }
--
frStatsTotDiscFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The total number of discarded frames on the port."
        ::= { frStatsEntry 13 }
--
-- frStatsRxDiscFrames OBJECT-TYPE
--      SYNTAX Counter
--      ACCESS read-only
--      STATUS mandatory
--      DESCRIPTION "The number of INFO Frames transmitted on the port"
--      ::= { frStatsEntry 14 }
--
-- The X25 Frame Level Tx Statistics group define the FlvX25TxStats Table
--

x25TxStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF X25TxStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe X25 Frame Level Txmit Statistics on each Port"
        ::= { statFrame 2 }

x25TxStatsEntry OBJECT-TYPE
        SYNTAX X25TxStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An X25 frame level transmit statistics entry containing
        objects relating to x25 frame level transmit statistics."
        INDEX { x25TxRlpIndex, x25TxPortIndex }
        ::= { x25TxStatsTable 1 }

X25TxStatsEntry ::=
        SEQUENCE {
                x25TxRlpIndex
                        INTEGER,
                x25TxPortIndex
                        INTEGER,
                x25TxSABMFrames
                        Counter,
                x25TxUAFrames
                        Counter,
                x25TxDISCFrames
                        Counter,
                x25TxDMFrames
                        Counter,
                x25TxFRMRFrames
                        Counter,
                x25TxREJFrames
                        Counter,
                x25TxRRFrames
                        Counter,
                x25TxRNRFrames
                        Counter,
                x25TxINFOFrames
                        Counter
}
x25TxRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP Number."
        ::= { x25TxStatsEntry 1 }

x25TxPortIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port number."
        ::= { x25TxStatsEntry 2 }

x25TxSABMFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of SABM's transmitted on the port."
        ::= { x25TxStatsEntry 3 }

x25TxUAFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of UA Frames transmitted on the port."
        ::= { x25TxStatsEntry 4 }

x25TxDISCFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of DISC Frames transmitted on the port."
        ::= { x25TxStatsEntry 5 }

x25TxDMFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of DM frames transmitted on the port."
        ::= { x25TxStatsEntry 6 }

x25TxFRMRFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The of Number of FRMR frames transmitted on the port."
        ::= { x25TxStatsEntry 7 }

x25TxREJFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of Reject Frames transmitted on the port."
        ::= { x25TxStatsEntry 8 }

x25TxRRFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of RR frames transmitted on the port."
        ::= { x25TxStatsEntry 9 }

x25TxRNRFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of RNR Frames transmitted on the port."
        ::= { x25TxStatsEntry 10 }

x25TxINFOFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of INFO Frames transmitted on the port"
        ::= { x25TxStatsEntry 11 }
--
-- The X25 Frame Level Rx Statistics group define the FlvX25RxStats Table
--

x25RxStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF X25RxStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe X25 Frame Level Rxmit Statistics on each Port"
        ::= { statFrame 3 }

x25RxStatsEntry OBJECT-TYPE
        SYNTAX X25RxStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An X25 frame level receive statistics entry containing
        objects relating to x25 frame level receive statistics."
        INDEX { x25RxRlpIndex, x25RxPortIndex }
        ::= { x25RxStatsTable 1 }

X25RxStatsEntry ::=
        SEQUENCE {
                x25RxRlpIndex
                        INTEGER,
                x25RxPortIndex
                        INTEGER,
                x25RxSABMFrames
                        Counter,
                x25RxUAFrames
                        Counter,
                x25RxDISCFrames
                        Counter,
                x25RxDMFrames
                        Counter,
                x25RxFRMRFrames
                        Counter,
                x25RxREJFrames
                        Counter,
                x25RxRRFrames
                        Counter,
                x25RxRNRFrames
                        Counter,
                x25RxINFOFrames
                        Counter
}
x25RxRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP Number."
        ::= { x25RxStatsEntry 1 }

x25RxPortIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port number."
        ::= { x25RxStatsEntry 2 }

x25RxSABMFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of SABM's received on the port."
        ::= { x25RxStatsEntry 3 }

x25RxUAFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of UA Frames received on the port."
        ::= { x25RxStatsEntry 4 }

x25RxDISCFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of DISC Frames received on the port."
        ::= { x25RxStatsEntry 5 }

x25RxDMFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of DM frames received on the port."
        ::= { x25RxStatsEntry 6 }

x25RxFRMRFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The of Number of FRMR frames received on the port."
        ::= { x25RxStatsEntry 7 }

x25RxREJFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of Reject Frames received on the port."
        ::= { x25RxStatsEntry 8 }

x25RxRRFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of RR frames received on the port."
        ::= { x25RxStatsEntry 9 }

x25RxRNRFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of RNR Frames received on the port."
        ::= { x25RxStatsEntry 10 }

x25RxINFOFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The number of INFO Frames received on the port"
        ::= { x25RxStatsEntry 11 }

statBag OBJECT IDENTIFIER ::=           { statGroup 5 }
statIp OBJECT IDENTIFIER ::=                    { statGroup 6 }
statT1  OBJECT IDENTIFIER ::=                   { statGroup 7 }

-- The statistics group for T1 Channels.

t1StatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF T1StatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe T1 Statistics."
        ::= { statT1 1}

t1StatsEntry OBJECT-TYPE
        SYNTAX T1StatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A T1 port statistics entry containing objects relating
        to T1 port statistics."
        INDEX { t1StatsRlpIndex, t1StatsPortIndex }
        ::= { t1StatsTable 1 }

T1StatsEntry ::=
        SEQUENCE {
                t1StatsRlpIndex
                        INTEGER,
                t1StatsPortIndex
                        INTEGER,
                t1StatsRcvFrames
                        Counter,
                t1StatsXmitFrames
                        Counter,
                t1StatsLCVCnt
                        Counter,
                t1StatsPCVRErrs
                        Counter,
                t1StatsOOSCnt
                        Counter,
                t1StatsBlueAlarms
                        Counter,
                t1StatsYellowAlarms
                        Counter,
                t1StatsRedAlarms
                        Counter,
                t1StatsRcvUsage
                        Counter,
                t1StatsXmitUsage
                        Counter,
                t1StatsXmitAbortFrames
                        Counter,
                t1StatsRcvAbortFrames
                        Counter,
                t1StatsRcvOverruns
                        Counter,
                t1StatsRcvErrors
                        Counter,
                t1StatsRcvChannelErrors
                        Counter
}

t1StatsRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP Number."
        ::= { t1StatsEntry 1 }

t1StatsPortIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port Number."
        ::= { t1StatsEntry 2 }

t1StatsRcvFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total received frames."
        ::= { t1StatsEntry 3 }

t1StatsXmitFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total transmitted frames."
        ::= { t1StatsEntry 4 }

t1StatsLCVCnt OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Line code violation count."
        ::= { t1StatsEntry 5 }

t1StatsPCVRErrs OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "PCVR Bit error count."
        ::= { t1StatsEntry 6 }

t1StatsOOSCnt OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Multiframe out of sync count."
        ::= { t1StatsEntry 7 }

t1StatsBlueAlarms OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Blue alarm count."
        ::= { t1StatsEntry 8 }

t1StatsYellowAlarms OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Yellow alarm count."
        ::= { t1StatsEntry 9 }

t1StatsRedAlarms OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Red alarm count."
        ::= { t1StatsEntry 10 }

t1StatsRcvUsage OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Receive port utilization."
        ::= { t1StatsEntry 11 }

t1StatsXmitUsage OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Transmit port utilization."
        ::= { t1StatsEntry 12 }

t1StatsXmitAbortFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total aborted transmit frames."
        ::= { t1StatsEntry 13 }

t1StatsRcvAbortFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total aborted receive frames."
        ::= { t1StatsEntry 14 }

t1StatsRcvOverruns OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total receive overruns."
        ::= { t1StatsEntry 15 }

t1StatsRcvErrors OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total bad receives."
        ::= { t1StatsEntry 16 }

t1StatsRcvChannelErrors OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total bad receives."
        ::= { t1StatsEntry 17 }

-- The statistics group for DS0A.

statDS0A  OBJECT IDENTIFIER ::=                 { statGroup 8 }

ds0aStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF DS0AStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe DS0A Statistics."
        ::= { statDS0A 1}

ds0aStatsEntry OBJECT-TYPE
        SYNTAX DS0AStatsEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A DS0A port statistics entry containing objects relating
        to DS0A port statistics."
        INDEX { ds0aStatsRlpIndex, ds0aStatsPortIndex, ds0aStatsChannelIndex }
        ::= { ds0aStatsTable 1 }

DS0AStatsEntry ::=
        SEQUENCE {
                ds0aStatsRlpIndex
                        INTEGER,
                ds0aStatsPortIndex
                        INTEGER,
                ds0aStatsChannelIndex
                        INTEGER,
                ds0aStatsXmitFrames
                        Counter,
                ds0aStatsRcvFrames
                        Counter,
                ds0aStatsRcvAbortFrames
                        Counter,
                ds0aStatsRcvOverruns
                        Counter,
                ds0aStatsRcvErrors
                        Counter
}

ds0aStatsRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP Number."
        ::= { ds0aStatsEntry 1 }

ds0aStatsPortIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port Number."
        ::= { ds0aStatsEntry 2 }

ds0aStatsChannelIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Channel Number."
        ::= { ds0aStatsEntry 3 }

ds0aStatsXmitFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total transmitted frames."
        ::= { ds0aStatsEntry 4 }

ds0aStatsRcvFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total received frames."
        ::= { ds0aStatsEntry 5 }

ds0aStatsRcvAbortFrames OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total receive aborted frames."
        ::= { ds0aStatsEntry 6 }

ds0aStatsRcvOverruns OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total receive overruns."
        ::= { ds0aStatsEntry 7 }

ds0aStatsRcvErrors OBJECT-TYPE
        SYNTAX Counter
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "Total receive errors."
        ::= { ds0aStatsEntry 8 }

-- The statistics group for Voice.
statVoice  OBJECT IDENTIFIER ::={ statGroup 9 }

--
-- The Voice Statistics Table
--

voiceStatsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF VoiceStatsEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION "A Table to describe Voice over Frame Relay Statistics."
    ::= { statVoice 1}

voiceStatsEntry OBJECT-TYPE
    SYNTAX VoiceStatsEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION "A voice port statistics entry containing objects relating
    to voice port statistics."
    INDEX {voiceStatsRlpIndex, voiceStatsPortIndex }

    ::= { voiceStatsTable 1 }

VoiceStatsEntry ::=
    SEQUENCE {
        voiceStatsRlpIndex
            INTEGER,
        voiceStatsPortIndex
            INTEGER,
        voiceStatsRxCalls
            Counter,
        voiceStatsTxCalls
            Counter,
        voiceStatsRxCallsAccepts
            Counter,
        voiceStatsTxCallsAccepts
            Counter,
        voiceStatsRxClears
            Counter,
        voiceStatsTxClears
            Counter,
        voiceStatsBusyCalls
            Counter,
        voiceStatsCallTimeouts
            Counter,
        voiceStatsRxCongestions
            Counter,
        voiceStatsTxCongestions
            Counter
}

voiceStatsRlpIndex OBJECT-TYPE
    SYNTAX INTEGER
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The RLP Number."
    ::= { voiceStatsEntry 1 }

voiceStatsPortIndex OBJECT-TYPE
    SYNTAX INTEGER
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Port Number."
    ::= { voiceStatsEntry 2 }

voiceStatsRxCalls OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of Calls Received from the Network."
    ::= { voiceStatsEntry 3 }

voiceStatsTxCalls OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of Calls Transmitted to the Network."
    ::= { voiceStatsEntry 4 }

voiceStatsRxCallsAccepts OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of Call Accepts Received from the Network."
    ::= { voiceStatsEntry 5 }

voiceStatsTxCallsAccepts OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of Call Accepts Transmitted to the Network."
    ::= { voiceStatsEntry 6 }

voiceStatsRxClears OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of Call Receives cleared."
    ::= { voiceStatsEntry 7 }

voiceStatsTxClears OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of Call Transmitts cleared."
    ::= { voiceStatsEntry 8 }

voiceStatsBusyCalls OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of calls which received Busy indication."
    ::= { voiceStatsEntry 9 }

voiceStatsCallTimeouts OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The Number of calls which transmitted time-out to the network."
    ::= { voiceStatsEntry 10 }

voiceStatsRxCongestions OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The number of congestion management frames Received."
    ::= { voiceStatsEntry 11 }

voiceStatsTxCongestions OBJECT-TYPE
    SYNTAX Counter
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION "The number of congestion management frames Transmitted."
    ::= { voiceStatsEntry 12 }

statThresh OBJECT IDENTIFIER ::=        { statistics 2 }

--
-- The Statistic Threshold group for RLPs defines the RlpThresh Table
--

rlpThreshTable OBJECT-TYPE
        SYNTAX SEQUENCE OF RlpThreshEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe Statistic thresholds on each RLP"
        ::= { statThresh 1 }

rlpThreshEntry OBJECT-TYPE
        SYNTAX RlpThreshEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "An RLP statistics threshold entry containing objects
        relating to RLP statistics thresholds."
        INDEX { rlpThreshRlpIndex }
        ::= { rlpThreshTable 1 }

RlpThreshEntry ::=
        SEQUENCE {
                rlpThreshRlpIndex
                        INTEGER,
                rlpThreshPercntBufInUse
                        INTEGER,
                rlpThreshMsgQueueLen
                        INTEGER,
                rlpThreshRxFramesPerSec
                        INTEGER,
                rlpThreshTxFramesPerSec
                        INTEGER,
                rlpThreshRejFramesPerSec
                        INTEGER,
                rlpThreshRtxFramesPerSec
                        INTEGER
}
rlpThreshRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP Number."
        ::= { rlpThreshEntry 1 }

rlpThreshPercntBufInUse OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Percent of Buffers in use on the RLP"
        ::= { rlpThreshEntry 2 }

rlpThreshMsgQueueLen OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Percent of Buffers in use on the RLP"
        ::= { rlpThreshEntry 3 }

rlpThreshRxFramesPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Rcvd frames per second on the RLP"
        ::= { rlpThreshEntry 4 }

rlpThreshTxFramesPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Txmitted frames per second on the RLP"
        ::= { rlpThreshEntry 5 }

rlpThreshRejFramesPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Rejected Frames per second on the RLP"
        ::= { rlpThreshEntry 6 }

rlpThreshRtxFramesPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Retransmitted frames per second on the RLP"
        ::= { rlpThreshEntry 7 }

--
-- The Statistic Threshold group for Ports defines the PortThresh Table
--

portThreshTable OBJECT-TYPE
        SYNTAX SEQUENCE OF PortThreshEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A Table to describe Statistic thresholds on each port"
        ::= { statThresh 2  }

portThreshEntry OBJECT-TYPE
        SYNTAX PortThreshEntry
        ACCESS not-accessible
        STATUS mandatory
        DESCRIPTION "A port statistics threshold entry containing objects
        relating to port statistics thresholds."
        INDEX { portThreshRlpIndex, portThreshIndex }
        ::= { portThreshTable 1 }

PortThreshEntry ::=
        SEQUENCE {
                portThreshRlpIndex
                        INTEGER,
                portThreshIndex
                        INTEGER,
                portThreshRxFramesPerSec
                        INTEGER,
                portThreshTxFramesPerSec
                        INTEGER,
                portThreshRtxFramesPerSec
                        INTEGER,
                portThreshFCSErrPerSec  
                        INTEGER,
                portThreshLogRejPerSec
                        INTEGER,
                portThreshTxErrorRatio
                        INTEGER,
                portThreshRxErrorRatio
                        INTEGER,
                portThreshTxPercentUtl
                        INTEGER,
                portThreshRxPercentUtl
                        INTEGER
}
portThreshRlpIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The RLP Number."
        ::= { portThreshEntry 1 }

portThreshIndex OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The Port Number."
        ::= { portThreshEntry 2 }

portThreshRxFramesPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Rcvd frames per second on the port."
        ::= { portThreshEntry 3 }

portThreshTxFramesPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Txmitted frames per second on the port."
        ::= { portThreshEntry 4 }

portThreshRtxFramesPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Retransmitted frames per second on the port."
        ::= { portThreshEntry 5 }

portThreshFCSErrPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for FCS errors per second on the port."
        ::= { portThreshEntry 6 }

portThreshLogRejPerSec OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Logical Rejects per second on the port."
        ::= { portThreshEntry 7 }

portThreshTxErrorRatio OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Txmit error ratio on the port."
        ::= { portThreshEntry 8 }

portThreshRxErrorRatio OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Rcv error ratio on the port."
        ::= { portThreshEntry 9 }

portThreshTxPercentUtl OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Txmit percent utilization on the port."
        ::= { portThreshEntry 10 }

portThreshRxPercentUtl OBJECT-TYPE
        SYNTAX INTEGER
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION "The threshold for Rcv percent utilization on the port."
        ::= { portThreshEntry 11 }

-- **********************
-- *  THE BRIDGE GROUP  *
-- **********************

bridge OBJECT IDENTIFIER ::= { local 9 }

bridgeAdminVirtualLANID         OBJECT-TYPE
                                SYNTAX INTEGER (0..4095)
                                ACCESS read-write
                                STATUS mandatory
                                DESCRIPTION 
                                        "LAN id inserted into token ring RIF field representing
                                         internal virtual ring, for LLC2 or bridged traffic"
                                ::= { bridge 1 }

bridgeOperVirtualLANID  OBJECT-TYPE
                        SYNTAX INTEGER (0..4095)
                        ACCESS read-only
                        STATUS mandatory
                        DESCRIPTION 
                                        "LAN id inserted into token ring RIF field representing
                                         internal virtual ring, for LLC2 or bridged traffic"
                        ::= { bridge 2 }

bridgeEnabled   OBJECT-TYPE
                SYNTAX INTEGER {
                        no (1),
                        yes (2)
                }
                ACCESS read-write
                STATUS mandatory
                DESCRIPTION 
                        "When yes the spanning tree algorithm is in effect and all
                         traffic types may be bridged. When no only llc/2 terminated
                         traffic is allowed on bridge interfaces."
                DEFVAL { yes }
                ::= { bridge 3 }

bridgeMaxSizeForwardingTable    OBJECT-TYPE
                                SYNTAX INTEGER (128..65535)
                                ACCESS read-write
                                STATUS mandatory
                                DESCRIPTION 
                                        "Number of entries allowed in the bridge forwarding
                                         table"
                                DEFVAL { 65535 }
                                ::= { bridge 4 }

bridgeIPEnabled OBJECT-TYPE
                SYNTAX INTEGER {
                                no (1),
                                yes (2)
                }
                ACCESS read-write
                STATUS mandatory
                DESCRIPTION 
                                "When yes, and BRIDGING ENABLED, IP traffic will be bridged,
                                 otherwise IP traffic will be routed."
                DEFVAL { no }
                ::= { bridge 5 }

bridgeIPXEnabled        OBJECT-TYPE
                        SYNTAX INTEGER {
                                        no (1),
                                        yes (2)
                        }
                        ACCESS read-write
                        STATUS mandatory
                        DESCRIPTION 
                                "When yes, and BRIDGING ENABLED, IPX traffic will be bridged,
                                 otherwise IPX traffic will be routed."
                        DEFVAL { no }
                        ::= { bridge 6 }

bridgeAdminSRBID        OBJECT-TYPE
                        SYNTAX INTEGER (0..15)
                        ACCESS read-write
                        STATUS mandatory
                        DESCRIPTION 
                                "bridge ID to be inserted into token ring RIF field, 
                                this bridge"
                        DEFVAL { 0 } 
                        ::= { bridge 7 }

bridgeOperSRBID OBJECT-TYPE
                SYNTAX INTEGER (0..15)
                ACCESS read-only
                STATUS mandatory
                DESCRIPTION 
                                "bridge ID to be inserted into token ring RIF field, 
                                this bridge"
                ::= { bridge 8 }

bridgeDefaultEthernetFrameType  OBJECT-TYPE
                                SYNTAX INTEGER {
                                                type-II (1),
                                                ieee8023 (2)
                                }
                                ACCESS      read-write
                                STATUS      mandatory
                                DESCRIPTION 
                                                                "default frame type to be used when 
                                                                 forwarding traffic on ethernet interfaces."
                                DEFVAL { type-II }
                                ::= { bridge 9 }

-- **************************
-- *  THE NETLINK IP GROUP  *
-- **************************

ipNl OBJECT IDENTIFIER ::= { local 11}

--
--  The Netlink IP Node Defaults Objects
--

nlIpDefaultRIPVersion OBJECT-TYPE
        SYNTAX INTEGER {
                ripVersion1(1),
                rip1Compatible(2),
                ripVersion2(3)
        }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION "The version of RIP that will be used by IP."
        DEFVAL { ripVersion1 }
        ::= { ipNl 1 }

-- *****************************
-- *  THE NETLINK VOICE GROUP  *
-- *****************************

voice OBJECT IDENTIFIER ::= { local 12 }

--
--  The Netlink Voice System Level Objects
--

voiceSystemVoiceNodeNum OBJECT-TYPE
    SYNTAX INTEGER (1..9999)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The number that identifies this node."
    DEFVAL { 1 }
    ::= { voice 1 }

voiceSystemRingVolFreq OBJECT-TYPE
    SYNTAX INTEGER {
                v75-hz-16-66 (1),
                v80-hz-20-00 (2),
                v75-hz-25-00 (3),
                v60-hz-50-00 (4),
                v75-hz-50-00 (5)
                }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The frequency and voltage of the telephone ring circuit.
                In two wire OPX mode, the node provides ring voltage to
                the telephone when it is called by a remote unit."
    DEFVAL { v80-hz-20-00 }
    ::= { voice 2 }

voiceSystemCountryCode OBJECT-TYPE
    SYNTAX INTEGER (1..999)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The telephone dialing prefix code that identifies
                the country in which the node is installed."
    DEFVAL { 1 }
    ::= { voice 3 }

voiceSystemDialDigits OBJECT-TYPE
    SYNTAX INTEGER (2..4)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The number of digits that will be used in the speed
                dialing scheme, as well as the number of digits one
                can specify for the Auto Dial feature. This requires
                rebooting for the change to take effect."
    DEFVAL { 3 }
    ::= { voice 4 }

voiceSystemVoiceRatesMin OBJECT-TYPE
    SYNTAX INTEGER {
                bps-4800 (1),
                bps-8000 (2),
                bps-32000 (3),
                bps-64000 (4)
                }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The minimum operating rate of all voice channels when
                congestion occurs."
    DEFVAL { bps-4800 }
    ::= { voice 5 }

voiceSystemVoiceRatesMax OBJECT-TYPE
    SYNTAX INTEGER {
                bps-4800 (1),
                bps-8000 (2),
                bps-32000 (3),
                bps-64000 (4)
                }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The maximum operating digitization rate of all voice
                channels when there is no congestion."
    DEFVAL { bps-64000 }
    ::= { voice 6 }

voiceSystemExtDialDigits OBJECT-TYPE
    SYNTAX INTEGER (0..16)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION "The number of extended dial digits that can be defined
                in the speed map table and/or entered by the user of
                attached equipment as part of a dial string. This requires
                rebooting for the change to take effect."
    DEFVAL { 0 }
    ::= { voice 7 }

--
-- The Netlink Voice Speed Dial Map table
--

voiceSpeedDialTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VoiceSpeedDialEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A list of speed-dial numbers."
    ::= { voice 8 }

voiceSpeedDialEntry OBJECT-TYPE
    SYNTAX  VoiceSpeedDialEntry
    ACCESS  not-accessible
    STATUS  mandatory
    DESCRIPTION
            "A Voice Speed Dial entry containing objects relating to
            the speed-dial number that are configurable by the user."
    INDEX   { voiceSpeedDialDigits }
    ::= { voiceSpeedDialTable 1 }

VoiceSpeedDialEntry ::=
    SEQUENCE {
        voiceSpeedDialDigits
            OCTET STRING,
        voiceSpeedDialLongDialMap
            OCTET STRING,
        voiceSpeedDialExtDialStr
            OCTET STRING,
        voiceSpeedDialRowStatus
            RowStatus
    }

voiceSpeedDialDigits OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1..4))
    ACCESS  read-only
    STATUS  mandatory
    DESCRIPTION
            "The speed-dial number. A question mark wildcard can be used
            for any digit, and an asterisk wildcard can be used for any
            number of digits."
    ::= { voiceSpeedDialEntry 1 }

voiceSpeedDialLongDialMap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(6))
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The number for which the speed-dial number is a shortcut."
    ::= { voiceSpeedDialEntry 2 }

voiceSpeedDialExtDialStr OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(1..16))
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "The extended set of digits that will be forwarded with the
            call if portVoiceOperExtDigitsSource in the physical port
            record is set to Map."
    ::= { voiceSpeedDialEntry 3 }

voiceSpeedDialRowStatus OBJECT-TYPE
    SYNTAX  RowStatus
    ACCESS  read-write
    STATUS  mandatory
    DESCRIPTION
            "This variable is used to manage the creation and deletion
            of conceptual rows in the voiceSpeedDialTable and follows the
            SNMPv2 RowStatus conventions by supporting the following values:

                 - `active', which indicates that the conceptual row is
                available for use by the managed device.  For a management
                protocol set operation, a genErr response is returned when
                the row does not exist.

                 - `createAndGo', which is supplied by a management
                 station wishing to create a new instance of a
                 conceptual row and to have its status automatically set
                 to active, making it available for use by the managed
                 device.  For a management protocol set operation, a
                 genErr response is returned when the row already exists.

                 - `destroy', which is supplied by a management station
                 wishing to delete all of the instances associated with
                 an existing conceptual row.

            Note that all of the above values may be specified in a
            management protocol set operation, and only the 'active'
            value will be returned in response to a management protocol
            retrieval operation.  For a management protocol set operation,
            if other variable bindings are included in the same PDU, then
            a genErr response is returned."
    ::= { voiceSpeedDialEntry 4 }

END
