   IANA-PWE3-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY
          FROM SNMPv2-SMI -- [RFC2578]
       pwe3
          FROM FOUNDRY-SN-ROOT-MIB
       TEXTUAL-CONVENTION
          FROM SNMPv2-TC; -- [RFC2579]

   ianaPwe3MIB  MODULE-IDENTITY
       LAST-UPDATED "200702041200Z"  -- 4 February 2006 12:00:00 GMT
       ORGANIZATION "IANA"
       CONTACT-INFO
            "Internet Assigned Numbers Authority
            Internet Corporation for Assigned Names and Numbers
            4676 Admiralty Way, Suite 330
            Marina del Rey, CA 90292-6601

            Phone: +1 310 823 9358
            EMail: iana@iana.org"
       DESCRIPTION
           "This MIB module defines the IANAPwTypeTC and
           IANAPwPsnTypeTC textual conventions for use in PWE3
           MIB modules.

           Any additions or changes to the contents of this MIB
           module require either publication of an RFC, Designated
           Expert Review as defined in RFC 2434, Guidelines for
           Writing an IANA Considerations Section in RFCs, and should
           be based on the procedures defined in [RFC4446]. The
           Designated Expert will be selected by the IESG Area
           Director(s) of the internet Area.

           Copyright (C) The IETF Trust (2007).  The initial
           version of this MIB module was published in RFC yyyy;
           for full legal notices see the RFC itself.  Supplementary
           information may be available at:
           http://www.ietf.org/copyrights/ianamib.html."
      -- RFC Ed.: replace yyyy with actual RFC number & remove this note

       REVISION     "200702041200Z"  -- 4 February 2006 12:00:00 GMT
       DESCRIPTION  "Original version, published as part of RFC yyyy."
   -- RFC Editor: please fill the yyyy and remove this note.

       ::= { pwe3 3 }
       -- ::= { transmission XXXX }
   -- RFC Editor: please fill the XXXX based on the IANA allocation
   -- and remove this note.

   IANAPwTypeTC ::= TEXTUAL-CONVENTION
      STATUS     current
      DESCRIPTION
         "Indicates the PW type (i.e. the carried service). "
    SYNTAX   INTEGER {
       other(0),
       frameRelayDlciMartiniMode(1),
       atmAal5SduVcc(2),
       atmTransparent(3),
       ethernetTagged(4),
       ethernet(5),
       hdlc(6),
       ppp(7),
       cem(8),  -- Historic type
       atmCellNto1Vcc(9),
       atmCellNto1Vpc(10),
       ipLayer2Transport(11),
       atmCell1to1Vcc(12),
       atmCell1to1Vpc(13),
       atmAal5PduVcc(14),
       frameRelayPortMode(15),
       cep(16),
       e1Satop(17),
       t1Satop(18),
       e3Satop(19),
       t3Satop(20),
       basicCesPsn(21),
       basicTdmIp(22),
       tdmCasCesPsn(23),
       tdmCasTdmIp(24),
       frDlci(25),
       wildcard (32767)
        }

   IANAPwPsnTypeTC ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Identifies the PSN type which the PW will use over the
          network."
      SYNTAX   INTEGER {
         mpls        (1),
         l2tp        (2),
         udpOverIp   (3),
         mplsOverIp  (4),
         mplsOverGre (5),
         other       (6)
         }

   IANAPwCapabilities ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "This TC describes a collection of cabailities related to
          a specific PW.
          Values may be added in the future based on new capabilities
          introduced in IETF documents.
         "
     SYNTAX   BITS {
       pwStatusIndication (0), -- Applicable only if maintenence
                               -- protocol is in use.
       pwVCCV             (1)
     }

   END


