   TCPIPX-MIB DEFINITIONS ::= BEGIN

   IMPORTS
	   enterprises
		   FROM RFC1155-SMI
           OBJECT-TYPE
                   FROM RFC-1212;

-- IPX address type.
-- First 4 octests are the network numbers and the last 6
-- octests are the node numbers.  In ascii, it is represented

-- as hex digits, as in:  nnnnnnnn:mmmmmmmmmmmm

IpxAddress ::= OCTET STRING (SIZE (10))

   -- TCP/IPX MIB object idenfifiers

novell        OBJECT IDENTIFIER ::= { enterprises 23 }
mibDoc        OBJECT IDENTIFIER ::= { novell 2 }
tcpx          OBJECT IDENTIFIER ::= { mibDoc 29 }
tcpxTcp       OBJECT IDENTIFIER ::= { tcpx 1 }
tcpxUdp       OBJECT IDENTIFIER ::= { tcpx 2 }

  -- the TCP/IPX Connection table

   -- The TCP/IPX connection table contains information
   -- about this entity's existing TCP connections over
   -- IPX.

   tcpIpxConnTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF TcpIpxConnEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
               "A table containing information specific on
               TCP connection over IPX network layer."
       ::= { tcpxTcp 1 }

   tcpIpxConnEntry OBJECT-TYPE
       SYNTAX  TcpIpxConnEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
               "Information about a particular current TCP
               connection over IPX  An object of this type is
               transient, in that it ceases to exist when (or
               soon after) the connection makes the transition
               to the CLOSED state."
       INDEX   { tcpIpxConnLocalAddress,
                 tcpIpxConnLocalPort,
                 tcpIpxConnRemAddress,
                 tcpIpxConnRemPort }
      ::= { tcpIpxConnTable 1 }

   TcpIpxConnEntry ::=
       SEQUENCE {

           tcpIpxConnState
               INTEGER,
           tcpIpxConnLocalAddress
               IpxAddress
           tcpIpxConnLocalPort
               INTEGER (0..65535),
           tcpIpxConnRemAddress
               IpxAddress,
           tcpIpxConnRemPort
               INTEGER (0..65535)
       }

   tcpIpxConnState OBJECT-TYPE
       SYNTAX  INTEGER {
                   closed(1),
                   listen(2),
                   synSent(3),
                   synReceived(4),
                   established(5),
                   finWait1(6),
                   finWait2(7),
                   closeWait(8),
                   lastAck(9),
                   closing(10),
                   timeWait(11),
                   deleteTCB(12)
               }
       ACCESS  read-write
       STATUS  mandatory
       DESCRIPTION
               "The state of this TCP connection.

               The only value which may be set by a management
               station is deleteTCB(12).  Accordingly, it is
               appropriate for an agent to return a `badValue'
               response if a management station attempts to set
               this object to any other value.

               If a management station sets this object to the
               value deleteTCB(12), then this has the effect of
               deleting the TCB (as defined in RFC 793) of the
               corresponding connection on the managed node,
               resulting in immediate termination of the
               connection.

               As an implementation-specific option, a RST
               segment may be sent from the managed node to the
               other TCP endpoint (note however that RST

               segments are not sent reliably)."
       ::= { tcpIpxConnEntry 1 }

   tcpIpxConnLocalAddress OBJECT-TYPE
       SYNTAX  IpxAddress
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The local IPX address for this TCP connection.
               In the case of a connection in the listen state
               which is willing to accept connections for any
               interface, the value 00000000:000000000000 is
               used.  See tcpUnspecConnTable for connections in
               the listen  state which is willing to accept
               connects for any IP interface associated with
               the node."
       ::= { tcpIpxConnEntry 2 }

   -- NetworkAddress defined in SMI only include IP currently,
   -- so we can't use it to represent both IP and IPX address.

   tcpIpxConnLocalPort OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The local port number for this TCP connection."
       ::= { tcpIpxConnEntry 3 }

   tcpIpxConnRemAddress OBJECT-TYPE
       SYNTAX  IpxAddress
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The remote IPX address for this TCP connection."
       ::= { tcpIpxConnEntry 4 }

   tcpIpxConnRemPort OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The remote port number for this TCP connection."
       ::= { tcpIpxConnEntry 5 }

   -- the UDP Listener table

   -- The UDP listener table contains information about this
   -- entity's UDP end-points on which a local application is
   -- currently accepting datagrams.

   udpIpxTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF UdpIpxEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
               "A table containing UDP listener information."
       ::= { tcpxUdp 1 }

   udpIpxEntry OBJECT-TYPE
       SYNTAX  UdpIpxEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
               "Information about a particular current UDP
               listener."
       INDEX   { udpIpxLocalAddress, udpIpxLocalPort }
       ::= { udpIpxTable 1 }

   UdpIpxEntry ::=
       SEQUENCE {
           udpIpxLocalAddress
    IpxAddress
           udpIpxLocalPort
               INTEGER (0..65535)
       }

   udpIpxLocalAddress OBJECT-TYPE
       SYNTAX  IpxAddress
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The local IPX address for this UDP listener.  In
               the case of a UDP listener which is willing to
               accept datagrams for any interface, the value
               00000000:000000000000 is used.  See
               udpUnspecTable for UDP listener which is
               willing to accept datagrams from any network
               layer."
       ::= { udpIpxEntry 1 }

   udpIpxLocalPort OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The local port number for this UDP listener."
       ::= { udpIpxEntry 2 }

   -- the TCP/UNSPEC Connection table

   -- The TCP/UPSPEC connection table contains information
   -- about this entity's existing TCP connections over
   -- unspecified network.
   -- Since the network is unspecified, the network
   -- address is also unspecified.  Hence, this
   -- connection table does not include any network
   -- address.

   tcpUnspecConnTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF TcpIpxConnEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
               "A table containing information specific on
               TCP connection over unspecified network layer."
       ::= { tcpxTcp 2 }

   tcpUnspecConnEntry OBJECT-TYPE
       SYNTAX  TcpUnspecConnEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
               "Information about a particular current TCP
               connection over unspecified network layer.  An
               object of this type is transient, in that it
               ceases to exist when the connection makes
               transition beyond LISTEN state, or when (or
               soon after) the connection makes transition
               to the CLOSED state,"
       INDEX   { tcpUnspecConnLocalPort }
       ::= { tcpUnspecConnTable 1 }

   TcpUnspecConnEntry ::=
       SEQUENCE {
           tcpUnspecConnState
               INTEGER,
           tcpUnspecConnLocalPort

               INTEGER (0..65535),
       }

   tcpUnspecConnState OBJECT-TYPE
       SYNTAX  INTEGER {
                   closed(1),
                   listen(2),
                   deleteTCB(12)
               }
       ACCESS  read-write
       STATUS  mandatory
       DESCRIPTION
               "The state of this TCP connection.

               Since the TCP connection can belong to this table
               only when its state is less than SYN_SENT, only
               closed and listen state apply.

               The only value which may be set by a management
               station is deleteTCB(12).  Accordingly, it is
               appropriate for an agent to return a `badValue'
               response if a management station attempts to set
               this object to any other value.

               If a management station sets this object to the
               value deleteTCB(12), then this has the effect of
               deleting the TCB (as defined in RFC 793) of the
               corresponding connection on the managed node,
               resulting in immediate termination of the
               connection.

               As an implementation-specific option, a RST
               segment may be sent from the managed node to the
               other TCP endpoint (note however that RST
               segments are not sent reliably)."
       ::= { tcpUnspecConnEntry 1 }

   tcpUnspecConnLocalPort OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The local port number for this TCP connection."
       ::= { tcpUnspecConnEntry 2 }

   -- the UDP Listener table

   -- The UDP listener table contains information about this
   -- entity's UDP end-points over unspecified network layer,
   -- on which a local application is currently accepting
   -- datagrams.  If network layer is unspecified, the network
   -- address is also unspecified.  Hence, this table does not
   -- include any network address.

   udpUnspecTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF UdpUnspecEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
                "A table containing UDP listener information."
       ::= { tcpxUdp 2 }

   udpUnspecEntry OBJECT-TYPE
       SYNTAX  UdpUnspecEntry
       ACCESS  not-accessible
       STATUS  mandatory
       DESCRIPTION
               "Information about a particular current UDP
               listener."
       INDEX   { udpUnspecLocalPort }
       ::= { udpUnspecTable 1 }

   UdpUnspecEntry ::=
       SEQUENCE {
           udpUnspecLocalPort
               INTEGER (0..65535)
       }

   udpUnspecLocalPort OBJECT-TYPE
       SYNTAX  INTEGER (0..65535)
       ACCESS  read-only
       STATUS  mandatory
       DESCRIPTION
               "The local port number for this UDP listener."
       ::= { udpUnspecEntry 1 }

    END
