DIFFSERV-DSCP-TC DEFINITIONS ::= BEGIN

    IMPORTS
    Integer32, MODULE-IDENTITY, mib-2
         FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
         FROM SNMPv2-TC;

diffServDSCPTC MODULE-IDENTITY
    LAST-UPDATED "200205090000Z"
    ORGANIZATION "IETF Differentiated Services WG"
    CONTACT-INFO
       "       Fred Baker
               Cisco Systems
               1121 Via Del Rey
               Santa Barbara, CA 93117, USA
               E-mail: fred@cisco.com

               Kwok Ho Chan
               Nortel Networks
               600 Technology Park Drive
               Billerica, MA 01821, USA
               E-mail: khchan@nortelnetworks.com

               Andrew Smith
               Harbour Networks
               Jiuling Building
               21 North Xisanhuan Ave.
               Beijing, 100089, PRC
               E-mail: ah_smith@acm.org

                 Differentiated Services Working Group:
                 diffserv@ietf.org"
    DESCRIPTION
       "The Textual Conventions defined in this module should be used
       whenever a Differentiated Services Code Point is used in a MIB."
    REVISION "200205090000Z"
    DESCRIPTION
       "Initial version, published as RFC 3289."
    ::= { mib-2 96 }

Dscp ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS   current
    DESCRIPTION
       "A Differentiated Services Code-Point that may be used for
       marking a traffic stream."
    REFERENCE
        "RFC 2474, RFC 2780"
    SYNTAX   Integer32 (0..63)

DscpOrAny ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS   current
    DESCRIPTION
       "The IP header Differentiated Services Code-Point that may be
       used for discriminating among traffic streams. The value -1 is
       used to indicate a wild card i.e. any value."
    REFERENCE
        "RFC 2474, RFC 2780"
    SYNTAX   Integer32 (-1 | 0..63)

END

