-- ==================================================================
-- Copyright (c) 2004-2011 Hangzhou H3C Tech. Co., Ltd.  All rights reserved.
--
-- Description: Lan Switch Device Physical Information MIB
-- Reference:
-- Version: V3.58
-- History:
--    v1.0 (1) Created by Hou Qiang, 2001.5.15
--         (2) Revised by Qi Zhenglin, 2002.01.08 ----r003 revision
--    v1.1 2004-7-12 add some card type define(hwLswSlotType 119-138)
--    v1.2 add enum value from 42 to 49 in hwLswPortType.
--    v1.3 2004-7-29 add some port type define(hwLswPortType 50-58)
--    v1.4 2004-8-11 add some slot type define
--                    (hwLswSlotType    type_LSA1FP8U(139))
--                    (hwLswSubslotType type_LSA1FP8U(139))
--    v1.5 2004-08-25 change emunation name
--                     from type_LS81SFCA(120) to type_LS81SRPG0(120),
--                     from type_LS81SFCB(121) to type_LS81SRPG1(121),
--                     from type_LS81SFCC(122) to type_LS81SRPG2(122),
--                     from type_LS81SFCD(123) to type_LS81SRPG3(123).
--                    modify comments for these emunations as well.
--    v1.6 2004-8-26 add some port types define(h2LswPortType 59-71)
--    v1.7 2004-09-08 add enum value from 140 to 148 in hwLswSlotType and hwLswSubSlotType by kangyinan
--    v1.8 2004-09-14 add enum value from 149 to 157 in hwLswSlotType and hwLswSubSlotType by wangyahui
--                    add enum value from 158 to 159 in hwLswSlotType and hwLswSubSlotType by kangyinan
--                    add enum value from 72 to 93 in hwLswPortType by wangyahui
--                    add enum value from 94 to 96 in hwLswPortType by kangyinan
--                    add type description for type_SP4, type_UP1, type_XP4 by kangyinan
--    v1.9 2004-10-12 updated by gaolong
--         Change all underscore('_') characters to hyphen characters('-') because underscore character is not allowed in MIB module.
--         The change refers to the value of hwLswSlotType, hwLswSlotAdminStatus, hwLswSubslotType, hwLswPortType, hwLswSubslotAdminStatus
--         Change MAX-ACCESS clause value of hwLswPortLoopbackOperate from write-only to read-write, and
--         update its DESCRIPTION.
--    v2.0 2004-10-19 add enum value from 160 to 162 in hwLswSlotType and hwLswSubSlotType by kangyinan
--                    add enum value 97 in hwLswPortType by kangyinan
--    v2.1  2004-11-23 add enum value from 163 to 166 in hwLswSlotType and hwLswSubSlotType by zhangchengmei
--    V2.2  2004-12-23 add enum value from 167 to 169 in hwLswSlotType and hwLswSubSlotType by zhangjianfeng
--    V2.3  2004-12-26 add enum value 170 in hwLswSlotType and hwLswSubSlotType by wangyahui
--    V2.4  2004-12-23 add enum value from 171 to 172 in hwLswSlotType and hwLswSubSlotType
--                     add enum value from 98 to 99 hwLswPortType by liyue
--    V2.5  2004-12-29 add enum value 173 in hwLswSlotType and hwLswSubSlotType by zhangjianfeng
--                     add enum value from 100 in hwLswPortType by zhangjianfeng
--    V2.6  2005-01-07 add enum value 174 and 175 in hwLswSlotType and hwLswSubSlotType by wangyahui
--    V2.7  2005-01-31 add enum value 176 in hwLswSlotType and hwLswSubSlotType by wangyahui
--    V2.8  2005-02-03 define HwLswTypeOfSlot
--                     change the SYNTAX of hwLswSlotType and hwLswSubSlotType to HwLswTypeOfSlot,add new enum vlaue to HwLswTypeOfSlot
--                     add enum value from 101 to 137 in hwLswPortType by zhangchengmei
--                     add enum value 178 in HwLswTypeOfSlot by zhouqiang
--                     add enum value 138 in hwLswPortType by zhouqiang
--                     add enum value from 179 to 180 in hwLswSubSlotType by wangyahui
--    V2.9  2005-03-22 add enum value from 181 to 187 in HwLswTypeOfSlot by zhangchengmei
--    V3.0  2005-05-10 add enum value from 188 to 216 in HwLswTypeOfSlot by zhangchengmei
--    V3.1  2005-07-18 add enum value from 217 to 219 in HwLswTypeOfSlot by yangliming
--          2005-06-25 add enum value from 139 to 142 in hwLswPortType by wangyahui
--    V3.11  2005-07-29 add enum value from 220 to 225 in HwLswTypeOfSlot by wangyahui
--    V3.12  2005-07-21 change the name of subidentifier 183 in HwLswTypeOfSlot by zhangchengmei
--                     add enum value 226 to 227 in HwLswTypeOfSlot by zhangchengmei
--           2005-08-29 add enum value 143 in hwLswPortType by qianxiaoyu
--    V3.13  2005-09-13 add enum value 228 to 253 in HwLswTypeOfSlot by zhangchengmei
--           2005-09-13 add enum value 257 to 268 in HwLswTypeOfSlot by zhangchengmei
--    V3.14  2005-11-04 add enum value 144 to 149 in hwLswPortType by zhangchengmei
--                      add enum value 150 in hwLswPortType by huangyuetao
--                      add enum value 269 to 271 in hwLswSlotType by yangxiaopeng
--                      add enum value 272 in HwLswTypeOfSlot by qianxiaoyu
--    V3.15  2005-11-24 add enum value 500 to 501 in hwLswSlotType by wangyahui
--    V3.16  2005-11-28 add enum value 300 to 316 in HwLswTypeOfSlot by zhangchengmei
--    V3.17  2005-12-30 add enum value 151 to 170 in hwLswPortType by zhangchengmei
--    V3.18  2006-01-04 add enum value 701 in HwLswTypeOfSlot by qianxiaoyu
--    V3.19  2006-02-12 add enum value 702 in HwLswTypeOfSlot by chenxiaohui
--                      add enum value 317 in HwLswTypeOfSlot by zhangchengmei
--    V3.20  2006-02-20 add enum value 703 in HwLswTypeOfSlot by chijuntao
--    V3.21  2006-02-28 add enum value 171 to 174 in hwLswPortType by wangshunli
--                      add enum value 318 to 336 in HwLswTypeOfSlot by zhaiyingying
--                      Modify description of hwLswSysIpAddr, hwLswSlotCpuRatio, hwLswSysCpuRatio
--                      and some wrong format of the description by wangyong
--    V3.22  2006-03-14 add enum value 175 in hwLswPortType by wangyahui
--                      add enum value 502 to 504 in HwLswTypeOfSlot by wangyahui
--    V3.23  2006-04-03 add enum value 176 in hwLswPortType by wangyahui
--    V3.24  2006-04-21 add enum value 337 to 340 in HwLswTypeOfSlot by zhaiyingying
--    V3.25  2006-04-21 add enum value 704 to 705 under HwLswTypeOfSlot by zhangxianguo
--                      add enum value 505 to 506 under HwLswTypeOfSlot by zhangjianfeng
--                      add enum value 341 to 349 under HwLswTypeOfSlot by zhaiyingying
--                      add enum value 177 to 178 under hwLswPortType by zhangjianfeng
--                      add enum value 179 to 180 under hwLswPortType by zhangxianguo
--    V3.26  2006-07-12 add enum value 507 to 509 in HwLswTypeOfSlot by wangyahui
--                      modify enum name 502 and 503 of HwLswTypeOfSlot by wangyahui
--                      add enum value 350 to 357 under HwLswTypeOfSlot by zhaiyingying
--                      Modify description of enum element(3) in HwLswTypeOfSlot by zhangxianguo
--    V3.27  2006-08-31 add enum value 510 to 514 in HwLswTypeOfSlot by wangyahui
--                      add enum value 800 to 801 in HwLswTypeOfSlot by luoguixing
--    V3.28  2006-10-26 add enum value 358 to 370 under HwLswTypeOfSlot by zhaiyingying
--                      add enum value 183 under hwLswPortType by zhaiyingying
--                      add enum value 515 to 526 in HwLswTypeOfSlot by wangyahui
--                      modify enum 505 and 506 of HwLswTypeOfSlot by wangyahui
--                      add enum value 181 to 182 in hwLswPortType by wangyahui
--    V3.29  2006-11-02 add enum value 527 to 536 in HwLswTypeOfSlot by wangyahui
--                      modify description of 511 to 513 in HwLswTypeOfSlot by wangyahui
--           2006-11-10 add enum value 371 to 378 under HwLswTypeOfSlot by shuxiongtao
--           2006-11-08 add enum value 184 to 185 under hwLswPortType by zhaiyingying
--    V3.30  2007-03-19 add enum value 537 in HwLswTypeOfSlot by wangyahui
--    V3.31  2007-04-25 add enum value 538 to 542 in HwLswTypeOfSlot by wangyahui
--                      add enum value 379 to 380 under HwLswTypeOfSlot by zhaiyingying
--                      add enum value 706 in HwLswTypeOfSlot by zhangzongyi
--    V3.32  2007-05-28 add enum value 707 in HwLswTypeOfSlot by ligaoxu
--                      add enum value 381 to 392 in HwLswTypeOfSlot by shuxiongtao
--                      modify name of enum value 371 and 374 in HwLswTypeOfSlot by shuxiongtao
--                      add enum value 186 in hwLswPortType by jinzhaoqiong
--    V3.33  2007-07-09 add enum value 543 to 551 in HwLswTypeOfSlot by Zhangjianfeng
--                      add enum value 552 to 554 in HwLswTypeOfSlot by wangyahui
--    V3.34  2007-07-26 add enum value 708 in HwLswTypeOfSlot by Xiuyihong
--    V3.35  2007-08-27 add enum value 187 to 188 in hwLswPortType by ruanhan
--                      add enum value 802 to 804 in HwLswTypeOfSlot by luoguixing
--                      add enum value 393 to 397 under HwLswTypeOfSlot by shuxiongtao
--    V3.36  2007-09-25 add enum value 555 to 559 in HwLswTypeOfSlot by wangyahui
--                      add enum value 805 in HwLswTypeOfSlot by luoguixing
--                      add enum value 398 to 399 in HwLswTypeOfSlot by hexuefei
--    V3.37  2007-10-16 add enum value 189 in hwLswPortType by liaoxin
--    V3.38  2007-11-20 add enum value 400 to 407 in HwLswTypeOfSlot by shuxiongtao
--    V3.39  2007-12-27 add enum value 560 to 568 in HwLswTypeOfSlot by wangyahui
--    V3.40  2008-01-30 add enum value 408 in HwLswTypeOfSlot by hexuefei
--                      add enum value 569 to 572 in HwLswTypeOfSlot by wangyahui
--    V3.41  2008-02-20 add enum value 573 to 574 in HwLswTypeOfSlot by zhangjianfeng
--                      modify name and comments of enum value 546 in HwLswTypeOfSlot by zhangjianfeng
--                      add enum value 575 to 576 in HwLswTypeOfSlot by wangyahui
--    V3.42  2008-03-31 add enum value 806 to 808 in HwLswTypeOfSlot by luoguixing
--                      add enum value 709 to 715 under HwLswTypeOfSlot by wangcong
--                      add enum value 191 to 196 under hwLswPortType by wangcong
--                      add enum value 409 to 431 in HwLswTypeOfSlot by zhaiyingying
--                      add enum value 432 in HwLswTypeOfSlot by shuxiongtao
--    V3.43  2008-04-29 add enum value 577 to 589 in HwLswTypeOfSlot by wangyahui
--    V3.44  2008-07-28 add enum value 590 to 592 in HwLswTypeOfSlot by wangyahui
--                      add enum value 809 to 810 in HwLswTypeOfSlot by luoguixing
--    V3.45  2008-08-26 modify name of enum value 379 and 399 in HwLswTypeOfSlot by wangwei
--                      modify description of 408 in HwLswTypeOfSlot by wangwei
--                      modify name and description of enum value 804 in HwLswTypeOfSlot by wangwei
--                      add enum value 433 to 434 in HwLswTypeOfSlot by wangwei
--                      add enum value 593 to 595 in HwLswTypeOfSlot by wangyahui
--    V3.46  2008-10-13 add enum vlaue 197 in hwLswPortType by ruanhan
--                      add enum value 811 in HwLswTypeOfSlot by luoguixing
--                      add enum value 596 and 601 in HwLswTypeOfSlot by wangyahui
--    V3.47  2008-12-01 add enum vlaue 725 in HwLswTypeOfSlot by ruanhan
--                      add enum value 602 to 619 in HwLswTypeOfSlot by wangyahui
--                      add enum value 435 to 442 in HwLswTypeOfSlot by zhaiyingying
--                      modify name of enum value 546 in HwLswTypeOfSlot by zhangjianfeng
--                      add enum value 443 in HwLswTypeOfSlot by shuxiongtao
--    V3.48  2008-12-25 add enum value 620 to 622 in HwLswTypeOfSlot by wangyahui
--                      add enum value 716 to 718 in HwLswTypeOfSlot by zhangshilin
--                      add enum value 444 to 445 in HwLswTypeOfSlot by wangchang
--    V3.49  2009-01-05 add enum value 446 to 452 in HwLswTypeOfSlot by wangchang
--                      add enum value 719 in HwLswTypeOfSlot by zhangshilin
--                      add enum value 623 to 633 in HwLswTypeOfSlot by wangyahui
--    V3.50  2009-03-19 add enum value 453 to 464 in HwLswTypeOfSlot by huyinxing
--    V3.51  2009-07-02 add enum value 634 to 637 in HwLswTypeOfSlot by wangyahui
--                      add enum value 465 to 468 in HwLswTypeOfSlot by zhaiyingying
--                      add enum value 469 to 472 in HwLswTypeOfSlot by huyinxing
--                      add enum value 198 in hwLswPortType by huyinxing
--                      add enum vlaue 199 in hwLswPortType by zhangjianfeng
--    V3.52  2009-08-28 add enum value 638 to 640 in HwLswTypeOfSlot by wangyahui
--    V3.53  2009-11-09 add enum value 726 in HwLswTypeOfSlot by ruanhan
--                      add enum value 641 in HwLswTypeOfSlot by wangyahui
--                      add enum value 473 to 477 in HwLswTypeOfSlot by yudongyang
--                      add enum value 478 to 485 in HwLswTypeOfSlot by heweibin
--    V3.54  2009-12-31 add enum value 200 to 201 in hwLswPortType by zhanghaiyang
--                      add enum value 642 to 651 in HwLswTypeOfSlot by wangyahui
--                      add enum value 486 in HwLswTypeOfSlot by yudongyang
--                      add enum value 727 to 728 in HwLswTypeOfSlot by xiaobing
--                      add enum value 652 to 659 in HwLswTypeOfSlot by wangyahui
--                      add enum value 487 to 488 in HwLswTypeOfSlot by huyinxing
--                      add enum value 660 to 662 in HwLswTypeOfSlot by wangyahui
--                      add enum value 202 to 203 in hwLswPortType by yangdonghong
--    V3.55  2010-03-03 Added hwLswSysPhyMemory, hwLswSysMemory,
--                      hwLswSysMemoryUsed, hwLswSysMemoryRatio by songhao
--                      add enum value 812 in HwLswTypeOfSlot by mashuhang
--                      add enum value 489 to 497 in HwLswTypeOfSlot by liubuxiang
--                      add enum value 498 to 499 in HwLswTypeOfSlot by shikejun
--                      add enum value 900 in HwLswTypeOfSlot by yangqiulin
--                      add enum value 901 to 902 in HwLswTypeOfSlot by huyinxing
--    V3.56  2010-08-29 add enum value 903 to 904 in HwLswTypeOfSlot by huyinxing
--                      add enum value 905 to 907 in HwLswTypeOfSlot by shikejun
--                      add enum value 663 to 685 in HwLswTypeOfSlot by wangyahui
--                      add enum value 813 in HwLswTypeOfSlot by mashuhang
--                      add enum value 729 in HwLswTypeOfSlot by zhangshilin
--                      add enum value 908 to 913 in HwLswTypeOfSlot by yangbin
--                      add enum value 914 to 918 in HwLswTypeOfSlot by huyinxing
--                      add enum value 919 to 927 in HwLswTypeOfSlot by langgaoyi
--                      add hwLswFabricTable by songhao
--    V3.57  2011-01-31 add enum value 686 to 691 in HwLswTypeOfSlot by wangyahui
--                      add enum value 928 to 929 in HwLswTypeOfSlot by langgaoyi
--                      add hwLswSysTemperature, hwLswSlotPhyMemory,
--                      hwLswSlotMemory, hwLswSlotMemoryUsed,
--                      hwLswSlotMemoryRatio and hwLswSlotTemperature by songhao
--    V3.58  2011-04-23 Add enum value 930 in HwLswTypeOfSlot by liuhui
--                      Add enum value 814 to 815 in HwLswTypeOfSlot by mashuhang
--                      Add enum value 692 to 694 in HwLswTypeOfSlot by wangyahui
--                      Add enum value 204 in hwLswPortType by yangliming
-- ==================================================================
HUAWEI-LSW-DEV-ADM-MIB DEFINITIONS ::= BEGIN
IMPORTS
    DisplayString, DateAndTime, TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    MODULE-IDENTITY, OBJECT-TYPE, IpAddress, Unsigned32, Integer32
        FROM SNMPv2-SMI
    lswCommon
        FROM HUAWEI-3COM-OID-MIB;

-- ==================================================================
--
-- ======================= definition begin =========================
--
-- ==================================================================

-- system information: hwLswDeviceAdmin
-- ==================================================================
    hwLswDeviceAdmin MODULE-IDENTITY
        LAST-UPDATED "200903190000Z"
        ORGANIZATION
            "Hangzhou H3C Technologies Co., Ltd."
        CONTACT-INFO
            "Platform Team H3C Technologies Co., Ltd.
             Hai-Dian District Beijing P.R. China
             http://www.h3c.com
             Zip: 100085"
        DESCRIPTION
        "The latest baseline."
        REVISION "200104040000Z"
        DESCRIPTION
        "The first baseline."
        ::= { lswCommon  18 }

    HwLswTypeOfSlot ::= TEXTUAL-CONVENTION
        STATUS      current
        DESCRIPTION "The type of slots for lan switch devices."
        SYNTAX INTEGER {
            type-NULL(0),           -- NULL
            type-10OR100M(1),           -- 10M/100M Ethernet Copper Interface Module
            type-1000BASE-LX-SM(2),     -- 1000BASE-X Module (SMF, LC)
            type-1000BASE-SX-MM(3),     -- 1000BASE-X Module (MMF, SC)
            type-1000BASE-TX(4),        --
            type-100M-SINGLEMODE-FX(5),     -- 100M Ethernet Single Mode Optical Interface Module
            type-100M-MULTIMODE-FX(6),      -- 100M Ethernet Multi-mode Optical Interface Module
            type-100M-100BASE-TX(7),        -- 100M Ethernet copper Interface Module(RJ45)
            type-100M-HUB(8),           -- 100M Base-TX transportation Interface Module
            type-VDSL(9),           -- VDSL
            type-STACK(10),         -- GigaStack Module
            type-1000BASE-ZENITH-FX(11),    -- 1000M Ethernet Single Mode Optical Interface Module(1550nm,70km,LC)
            type-1000BASE-LONG-FX(12),      -- 1000M Ethernet Single Mode Optical Interface Module(1550nm,40km,LC)
            type-ADSL(13),          -- ADSL
            type-4T10OR100-4FX100SM(14),    -- 4-Port Single Mode Optical Interface and 4-Port 10M/100M Ethernet Interface Module
            type-4T10OR100-4FX100MM(15),    -- 4-Port Multi-mode Optical Interface and 4-Port 10M/100M Ethernet Interface Module
            type-VSPL(16),          -- VDSL Board
            type-ASPL(17),          -- ADSL Board
            type-1000M-SFP(18),         -- 1000BASE-X SFP Module
            type-LS82O2CM(19),          -- ATM OC-3c/STM-1 Daughter Card (SFP)
            type-LS82P2CM(20),          -- POS OC-3c/STM-1 Daughter Card (SFP)
            type-LS82O4GM(21),          -- MPLS 1000BASE-X Daughter Card (GBIC)
            type-LS82GB4C(22),          -- 1000BASE-X Daughter Card (GBIC)
            type-LS82GT4C(23),          -- 1000BASE-T Daughter Card (RJ-45)
            type-LS82ST4C(24),          -- GigaStack Daughter Card
            bOARD-TYPE-LS82DSPU(25),        -- Dual Service Processing Module
            bOARD-TYPE-LS81GP8U(26),        -- Gigabit Ethernet Interface Process Module
            bOARD-TYPE-LS82GT20(27),        -- 1000BASE-T Module (RJ-45)
            bOARD-TYPE-LS82FE48(28),        -- 10/100BASE-TX Module (RJ-45)
            type-LS82T24B(29),          -- 24-Port 10/100BASE-TX (RJ-45) and 2 Port 1000BASE-X (GBIC) Module
            type-LSB1SRPA(30),          --
            type-LSB1FT48A(31),         -- 48-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet Board A
            type-LSB1FT48B(32),         -- 48-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet Board B
            type-LSB1F48GA(33),         -- 32-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet and 4-Port 1000Base-X (SFP) GE Board A
            type-LSB1F48GB(34),         -- 32-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet and 4-Port 1000Base-X (SFP) GE Board B
            type-LSB1FP20A(35),         -- 20-Port 100Base-FX (SFP) Fast Ethernet Board A
            type-LSB1FP20B(36),         -- 20-Port 100Base-FX (SFP) Fast Ethernet Board B
            type-FT48A(37),         -- 48-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet Interface Module
            type-GP4U(38),          -- 1000Base-X (SFP)  GE Interface Module
            type-GP2U(39),          -- 1000Base-X (SFP)  GE Interface Module
            type-TGX1A(40),         -- 10GBASE-R  (XENPAK) Interface Module
            type-1000BASE-LX-SM-IR-SC(41),  -- 1000M Ethernet Single Mode Optical Interface Module(1310nm,10km,SC)
            type-1000BASE-SX-MM-SR-SC(42),  -- 1000M Ethernet Multi-mode Optical Interface Module(850nm,500m,SC)
            type-1000BASE-T-RJ45(43),       -- 1000M Ethernet Copper Interface Module(RJ45)
            type-100BASE-FX-SM-IR-SC(44),   -- 100M Ethernet Single Mode Optical SubCard
            type-100BASE-FX-MM-SR-SC(45),   -- 100M Ethernet Multi-mode Optical SubCard
            type-GIGA-STACK-1M-PC(46),      -- GigaStack Daughter SubCard
            type-1000BASE-LX-SM-VLR-LC(47), -- 1000M Ethernet Single Mode Optical SubCard(1550nm,70km,LC)
            type-1000BASE-LX-SM-LR-LC(48),  -- 1000M Ethernet Single Mode Optical SubCard(1550nm,40km,LC)
            type-100BASE-FX-SM-LR-SC(49),   -- 100M Ethernet Single Mode Optical SubCard(1310nm,15km,SC)
            type-1000BASE-X-GBIC(50),       --
            type-100M-SINGLEMODE-FX-LC(51), -- 100M Ethernet Single-mode Optical SubCard(1310nm,2km,SC)
            type-100M-MULTIMODE-FX-LC(52),  -- 100M Ethernet Multi-mode Optical SubCard(1310nm,2km,SC)
            type-1000BASE-4SFP(53),     -- 4-Port 1000BASE-FX Single Mode Fiber Optic Transceivers LR with SC Connector
            type-1000BASE-4GBIC(54),        -- 4-Port 1000BASE-X Module(GBIC)
            type-1000BASE-FIXED-4SFP(55),   -- 4-Port 1000BASE-FX Single Mode Fiber Optic Transceivers LR with SC Connector
            type-1000BASE-FIXED-4GBIC(56),  -- 4-Port 1000BASE-X Module(GBIC)
            type-LSB1GP12A(57),         -- 12-Port 1000Base-X (SFP) GE Board A
            type-LSB1GP12B(58),         -- 12-Port 1000Base-X (SFP) GE Board B
            type-LSB1TGX1A(59),         -- 1-Port 10GBASE-R (XENPAK) Board A
            type-LSB1TGX1B(60),         -- 1-Port 10GBASE-R (XENPAK) Board B
            type-LSB1P4G8A(61),         -- 4*155M POS Optical Interface Module 8-Port 1000Base-X (SFP) GE and 4-Port 155M POS Board A
            type-LSB1P4G8B(62),         -- 4*155M POS Optical Interface Module 8-Port 1000Base-X (SFP) GE and 4-Port 155M POS Board B
            type-LSB1A4G8A(63),         -- 4*155M ATM Optical Interface Module 8-Port 1000Base-X (SFP) GE and 4-Port 155M ATM Board A
            type-LSB1A4G8B(64),         -- 4*155M ATM Optical Interface Module 8-Port 1000Base-X (SFP) GE and 4-Port 155M ATM Board B
            type-FT48C(65),         -- 48-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet Board C
            type-FP20(66),                  -- 20-port 100BASE-TX Module
            bOARD-TYPE-LS81FT48(67),        -- 48-Port 10/100BASE-TX Module (RJ-45)
            bOARD-TYPE-LS81GB8U(68),        -- 8-Port 1000BASE-X Module (GBIC)
            bOARD-TYPE-LS81GT8U(69),        -- 8-Port 1000BASE-T Module (RJ-45)
            bOARD-TYPE-LS81FS24(70),        -- 24-Port 100BASE-FX Module (SMF,MT-RJ)
            bOARD-TYPE-LS81FM24(71),        -- 24-Port 100BASE-FX Module (MMF,MT-RJ)
            bOARD-TYPE-LS82GP20(72),        -- Switching and Route Processing Board B (main board)
            type-LSB1SRPB(73),          --
            type-LSB1F32GA(74),         -- 32-Port Fast Ethernet + 4-Port Gigabit Ethernet module A
            type-LSB1F32GB(75),         -- 32-Port Fast Ethernet + 4-Port Gigabit Ethernet module B
            type-LSB2FT48A(76),         -- 48-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet Board A (ver 2)
            type-LSB2FT48B(77),         -- 48-Port 10Base-T/100Base-TX Auto-sensing Fast Ethernet Board B (ver 2)
            type-LSB1GT12A(78),         -- 12 Port 10/100/1000 Base-T  Interface Module
            type-LSB1GT12B(79),         -- 12 Port 10/100/1000 Base-T  Interface Module
            type-PC4U(80),          -- 4 Port155M POS(SFP) Interface Module
            type-FT32A(81),         -- 32 Port 10/100 Base-T FE Interface Module
            type-GT4U(82),          -- 4 Port 10/100/1000 Base-T  Interface Module
            bOARD-TYPE-LS83FP20A(83),       --
            bOARD-TYPE-LS82HGMU(84),        --
            type-LSB1GP8TB(85),         --
            type-LSB1GP8TC(86),         --
            type-LSB1GT8PB(87),         --
            type-LSB1GT8PC(88),         --
            type-LSB1FT48C(89),         -- 48-Port 100Base-TX Ethernet Interface module C
            type-LSB1FP20C(90),         -- 20-Port 100Base-FX(SFP) Fast Ethernet Interface Module C
            type-LSB1F32GC(91),         -- 32-Port Fast Ethernet + 4-Port Gigabit Ethernet interface module C
            type-LSB1GT12C(92),         -- 12-Port 10/100/1000 Base-T  Interface Module C
            type-LSB1GP12C(93),         -- 12-Port 1000Base-X(SFP) GE Interface Module C
            type-LSB1P4G8C(94),         -- 8-Port 1000Base-X(SFP) GE + 4-Port 155M POS Interface Module C
            type-LSB1TGX1C(95),         -- 1-Port 10GBase-R/X  Ethernet XENPAK Optical Interface Module C
            type-LSB1GT24B(96),         -- 24-Ports 10/100/1000Base-T Ethernet Interface Module B
            type-LSB1GT24C(97),         -- 24-Ports 10/100/1000Base-T Ethernet Interface Module C
            type-LSB1GP24B(98),         -- 24-Ports 1000Base-X Ethernet Interface Module B
            type-LSB1GP24C(99),         -- 24-Ports 1000Base-X Ethernet Interface Module C
            type-LSB1XP2B(100),         -- 2-Port 10GBase-R/W Ethernet XFP Optical Interface Module B
            type-LSB1XP2C(101),         -- 2-Port 10GBase-R/W Ethernet XFP Optical Interface Module C
            type-LSB1GV48B(102),        -- 48-Ports 10/100/1000Base-T Ethernet Interface Module B
            type-LSB1GV48C(103),        -- 48-Ports 10/100/1000Base-T Ethernet Interface Module C
            type-LSB1SRPC(104),         -- Switching and Route Processing Board C
            type-LSB1SRP1N0(105),       -- Switching and Route Processing Board 1N0
            type-LSB1SRP1N1(106),       -- Switching and Route Processing Board 1N1
            type-LSB1SRP1N2(107),       -- Switching and Route Processing Board 1N2
            type-GT24(108),         --
            type-GP24(109),         --
            type-XP2(110),          --
            type-GV48(111),         --
            type-LSG1GP8U(112),         -- 8 Port 1000BASE Module (SFP)
            type-LSG1GT8U(113),         -- 8 Port 1000BASE-T Module (RJ45)
            type-LSG1TG1U(114),         -- 1 Port 10GBASE Module(XENPAK)
            type-LSG1TD1U(115),         -- 1 Port 10GBASE-CX4 Module(IB4X)
            type-LSB2FT48C(116),        -- 48-Ports 100Base-TX Ethernet Interface module C
            type-LSB1GT48B(117),        -- 48-Ports 10/100/1000Base-T Ethernet Interface Module B
            type-LSB1GT48C(118),        -- 48-Ports 10/100/1000Base-T Ethernet Interface Module C
            type-LS81GT48(119),             -- 48 Port Gigabit Ethernet Electric Interface Unit

            type-LS81SRPG0(120),        -- Salience III, Switch and Route Processing Board
            type-LS81SRPG1(121),        -- Salience III Plus
            type-LS81SRPG2(122),        -- Salience III Lite
            type-LS81SRPG3(123),        -- Salience III Edge

--          type-LS81SRPG(124),              Switch And Route Processing Unit, Salience III. not used. not used.

            type-SR01SRPUB(125),                -- SR8812 Switching and Route Processing Unit
            type-SR01SRPUA(126),                -- SR8805 Switching and Route Processing Unit
            type-SR01GP12L(127),                -- 12-Port 1000Base-X Ethernet SFP Optical Interface Line Card(L)
            type-SR01GP12W(128),                -- 12-Port 1000Base-X Ethernet SFP Optical Interface Line Card(W)
            type-SR01FT48L(129),                -- 48-Port 10/100Base-TX Ethernet RJ45 Electrical Interface Line Card (L)
            type-SR01FT48W(130),                -- 48-Port 10/100Base-TX Ethernet RJ45 Electrical Interface Line Card (W)
            type-SR01XK1W(131),                 -- 1-Port 10GBase-R Ethernet XENPAK Optical Interface Line Card (W)
            type-SR01FP20W(132),                -- 20-Port 100Base-FX Ethernet SFP Optical Interface Line Card (W)
            type-SR01GT12W(133),                -- 12-Port 10/100/1000Base-T Ethernet RJ45 Electrical Interface Line Card (W)
            type-SR01F32GL(134),                -- 32-Port 10/100Base-TX Ethernet RJ45 Electrical Interface + 4-Port 1000Base-X Ethernet SFP Optical interface Line Card (L)
            type-SR01F32GW(135),                -- 32-Port 10/100Base-TX Ethernet RJ45 Electrical Interface  + 4-Port 1000Base-X  Ethernet SFP Optical interface Line Card (W)
            type-SR01GT8PL(136),                -- 8-Port 10/100/1000Base-T Ethernet RJ45 Electrical Interface + 4-Port 1000Base-X Ethernet SFP Optical Line Card (L)
            type-SR01GT8PW(137),                -- 8-Port 10/100/1000Base-T Ethernet RJ45 Electrical Interface + 4-Port 1000Base-X Ethernet SFP Optical Line Card (W)
            type-SR01P4G8W(138),                -- 4-Port 155M POS Optical Interface + 8-Port 1000Base-X Ethernet SFP Optical Interface Line Card (W)
            type-LSA1FP8U(139),                 -- 8 Ports 100Base-FX Ethernet SFP Card

            type-LSB1SP4B(140),                 -- 4-Port OC-48 POS SFP Optical Interface Board B
            type-LSB1SP4C(141),                 -- 4-Port OC-48 POS SFP Optical Interface Board C
            type-LSB1UP1B(142),                 -- 1-Port OC-192 POS XFP Optical Interface Board B
            type-LSB1UP1C(143),                 -- 1-Port OC-192 POS XFP Optical Interface Board C
            type-LSB1XP4B(144),                 -- 4-Port 10GBase Ethernet XFP Optical Interface Board B
            type-LSB1XP4C(145),                 -- 4-Port 10GBase Ethernet XFP Optical Interface Board C
            type-SP4(146),                      -- 4-Port OC-48 POS SFP Optical Interface Module
            type-UP1(147),                      -- 1-Port OC-192 POS XFP Optical Interface Module
            type-XP4(148),                      -- 4-Port 10GBase Ethernet XFP Optical Interface Module

            type-LS81VSNP(149),                 -- VerSatile Network Processing Board
            type-LS81T12P(150),                 -- 12-Port 1000Base-T Gigabit Ethernet Interface(RJ45)+4-Port 1000BASE-X  Gigabit Ethernet Optical Interface Board(SFP,LC)
            type-LS81P12T(151),                 -- 12-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC)+4-Port 1000BASE-T Gigabit Ethernet Interface Board(RJ45)
            type-LS81GP8UB(152),                -- 8-Port 1000M Ethernet Optical Interface Board(SFP,LC),LC Connector
            type-LS81FT48E(153),                -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45)
            type-LS81GP4UB(154),                -- 4-Port 1000M Ethernet Optical Interface Board(SFP,LC)
            type-LS81GT8UE(155),                -- 8-Port 1000M Ethernet Electrical Interface Switch Unit (RJ45)
            type-LS81GT48A(156),                -- 48 Port Gigabit Ethernet Electric Interface Unit
            type-LS81FP48(157),                 -- 48 Port 100M Ethernet Optical Interface Board(SFP,LC)

            type-LSB1XK1B(158),                 -- 1-Port 10GBase-R Ethernet XENPAK Optical Interface Board B
            type-LSB1XK1C(159),                 -- 1-Port 10GBase-R Ethernet XENPAK Optical Interface Board C

            type-SR01SRPUC(160),                -- Switching and Route Processing Unit C
            type-SR01SRPUD(161),                -- Switching and Route Processing Unit D
            type-SR01SRPUE(162),                -- Switching and Route Processing Unit E

            type-LSB1SRP1N3(163),               -- Switching and Route Process Unit, Clock Module
            type-LSB1VP2B(164),                 -- 2*10G Resilient Packet Ring Interface Line Card (B)
            type-LSB1NATB(165),                 -- NAT Service Processing Card (B)
            type-LSB1VPNB(166),                 -- VPN Service Processing Card (B)

            type-LSGP8P(167),                   -- 8-Port 1000M SFP Module
            type-LSXK1P(168),                   -- 1-Port 10G Xenpak Module
            type-LSXP2P(169),                   -- 2-Port 10G XFP Module

            type-LS81FT48F(170),                -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45)

            type-LS81PT8G(171),                 -- 8 Port 1000BASE-X Gigabit Passive Optical Line Interface Board
            type-LS81PT4G(172),                 -- 4 Port 1000BASE-X Gigabit Passive Optical Line Interface Board

            type-LSSTK24G(173),                 -- 2-Port 24G Cascade Port Module

            type-LS82GT20A(174),                -- 20-Port 1000Base-T Gigabit Ethernet Electrical Interface Board(RJ45), BCM5697
            type-LS82GP20A(175),                -- 20-Port 1000BASE-X Gigabit Ethernet Optical Interface Board(SFP,LC), BCM5697
            type-LS81TGX1C(176),                -- 1-Port 10G Base-R Ethernet Board

            type-VP2(177),                      -- 2*10G Resilient Packet Ring Interface Module
            type-LSA1FB8U(178),                 -- 8-Port 100Base-Fx BIDI Ethernet Board

            type-LS81T12PE(179),                -- 12-Port 1000Base-T GE Interface+4-Port 1000BASE-X GE Optical Interface Board(SFP,LC)
            type-LS81P12TE(180),                -- 12-Port 1000BASE-X GE Optical Interface(SFP,LC)+4-Port 1000 BASE-T GE Interface Board(RJ45)

            type-LSB1SRP2N0(181),               -- Switching and Route Process Unit,12*LPU
            type-LSB1SRP2N3(182),               -- Switching and Route Process Unit, Clock Module
            type-LSB1GV48DB(183),               -- 48 Ports 1000Base-T Ethernet Interface Line Card with POE(DB)
            type-LSB1FW8B(184),                 -- Firewall Service Processing Board with 8GE (B)
            type-LSB1IPSEC8B(185),              -- VPN Service Processing Board with 8GE (B)
            type-LSB1IDSB(186),                 -- IDS Service Processing Board (B)
            type-LSB1IPSB(187),                 -- IPS Service Processing Board (B)
            type-LSB2FT48CA(188),               -- 48 Ports 100Base-TX Ethernet Line Card (CA)
            type-LSB1FP20CA(189),               -- 20 Ports 100Base-FX Ethernet Interface Service Card (CA)
            type-LSB1F32GCA(190),               -- 32 Ports FE and 4 Ports GE Line Card(CA)
            type-LSB1P4G8CA(191),               -- 4 Ports OC-3c POS and 8 Ports GE Line Card(CA)
            type-LSB1GT12CA(192),               -- 12 Ports 1000Base-T Ethernet Interface Line Card(CA)
            type-LSB1GT24CA(193),               -- 24 Ports 1000Base-T Ethernet Interface Line Card(CA)
            type-LSB1GP12CA(194),               -- 12 Ports 1000Base Ethernet Optical Interface Service Card(CA)
            type-LSB1GP24CA(195),               -- 24 Ports 1000Base-X Ethernet Interface Line Card (CA)
            type-LSB1GT8PCA(196),               -- 8 Ports 1000Base-T Ethernet Interface & 4 Ports 1000Base-X Ethernet SFP Interface Line Card(CA)
            type-LSB1XP2CA(197),                -- 2-Port 10GBase-R/W Ethernet XFP Optical Interface Card(CA)
            type-LSB1XK1CA(198),                -- 10GBase-R Ethernet XENPAK Optical Interface Line Card(CA)
            type-LSB1XP4CA(199),                -- 4-Port 10GBase-R/X Ethernet Optical Interface Line Card(CA)
            type-LSB1UP1CA(200),                -- Single Port OC-192c POS XFP Optical Interface Card(CA)
            type-LSB1SP4CA(201),                -- 4-Port OC-48c POS SFP Optical Interface Card(CA)
            type-LSB1VP2CA(202),                -- 2*10G RPR Process Unit(CA)
            type-SR01FT48WA(203),               -- 48 Ports 100Base-TX Ethernet Line Card (WA)
            type-SR01FP20WA(204),               -- 20 Ports 100Base-FX Ethernet Interface Service Card (WA)
            type-SR01F32GWA(205),               -- 32 Ports FE and 4 Ports GE Line Card(WA)
            type-SR01P4G8WA(206),               -- 4 Ports OC-3c POS and 8 Ports GE Line Card(WA)
            type-SR01GT12WA(207),               -- 12 Ports 1000Base-T Ethernet Interface Line Card(WA)
            type-SR01GT24WA(208),               -- 24 Ports 1000Base-T Ethernet Interface Line Card(WA)
            type-SR01GP12WA(209),               -- 12 Ports 1000Base Ethernet Optical Interface Service Card(WA)
            type-SR01GP24WA(210),               -- 24 Ports 1000Base-X Ethernet Interface Line Card (WA)
            type-SR01GT8PWA(211),               -- 8 Ports 1000Base-T Ethernet Interface & 4 Ports 1000Base-X Ethernet SFP Interface Line Card(WA)
            type-SR01XP2WA(212),                -- 2-Port 10GBase-R/W Ethernet XFP Optical Interface Card(WA)
            type-SR01XK1WA(213),                -- 10GBase-R Ethernet XENPAK Optical Interface Line Card(WA)
            type-SR01UP1WA(214),                -- Single Port OC-192c POS XFP Optical Interface Card(WA)
            type-SR01SP4WA(215),                -- 4-Port OC-48c POS SFP Optical Interface Card(WA)
            type-GP8U(216),                     -- 8-Port 1000Base-X SFP Optical Interface Module
            type-LSEXP1P(217),                  -- Single 10G SFP Optical Interface Module
            type-LSEXK1P(218),                  -- Single 10G XENPAK Interface Module
            type-LSEXS1P(219),                  -- Single 10G STACK Interface Module

            type-LS81GP48(220),                 -- 48-Port 1000M Ethernet Optical Interface Board(SFP,LC),LC Connector
            type-LS81GT48B(221),                -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45)
            type-LS81T16P(222),                 -- 16-Port 1000Base-T Gigabit Ethernet Interface(RJ45) + 8-Port 1000BASE-X Gigabit Ethernet Optical Interface Board(SFP,LC)
            type-LS81T32P(223),                 -- 32-Port 1000Base-T Gigabit Ethernet Interface(RJ45) + 16-Port 1000BASE-X Gigabit Ethernet Optical Interface Board(SFP,LC)
            type-LS81TGX2(224),                 -- 2-Port 10GBASE Ethernet Interface Board(XFP,LC)
            type-LS81TGX4(225),                 -- 4-Port 10GBASE Ethernet Interface Module(XFP,LC),XG

            type-LSB1GV48DA(226),               -- 48 Ports 1000Base-T Ethernet Interface Line Card with POE(DA)
            type-SR01GV48VB(227),               -- 48 Ports 1000Base-T Ethernet Interface Line Card with POE(VB)

            type-LSB1GT24DB(228),               -- 24 Ports 1000Base-T Ethernet Interface Line Card(DB)
            type-LSB1GP24DB(229),               -- 24 Ports 1000Base-X Ethernet Interface Line Card(DB)
            type-LSB1GP24DC(230),               -- 24 Ports 1000Base-X Ethernet Interface Line Card(DC)
            type-LSB1FW8DB(231),                -- 8-port 1000BASE-X (SFP) Firewall Service Card(DB)
            type-LSB1IPSEC8DB(232),             -- 8-port 1000BASE-X (SFP) IPSEC Service Card(DB)
            type-SR01GT24VB(233),               -- 24 Ports 1000Base-T Ethernet Interface Line Card(VB)
            type-SR01GP24VC(234),               -- 24 Ports 1000Base-X Ethernet Interface Line Card(VC)
            type-SR01VP2WA(235),                -- 2*10G RPR Process Unit(WA)
            type-SR01FW8VB(236),                -- 8-port 1000BASE-X (SFP) Firewall Service Card(VB)
            type-SR01IPSEC8VB(237),             -- 8-port 1000BASE-X (SFP) IPSEC Service Card(VB)
            type-SR01NATL(238),                 -- NAT Service Processing Card (L)
            type-SR01VPNL(239),                 -- VPN Service Processing Card (L)

            type-LSB1GP24CB(240),               -- 24 Ports 1000Base-X Ethernet Interface Line Card(CB)
            type-LSB1GP48DB(241),               -- 48-Port Gigabit Ethernet Optical Interface Line Card(DB)
            type-LSB1XP2CB(242),                -- 2-Port 10Gigabit Ethernet Optical Interface Card(CB)
            type-XP4L(243),                     -- 4 Port 1000BASE Optic Interface Module (XFP)
            type-LSB1XP4LDB(244),               -- 4-Port 10GBase-R/W Ethernet XFP Optical Interface Line Speed Card(DB)
            type-LSB1XP4LDC(245),               -- 4-Port 10GBase-R/W Ethernet XFP Optical Interface Line Speed Card(DC)
            type-AHP4(246),                     -- 2-Port OC-3 ATM and 2-Port OC-3/12 ATM Interface Module (SFP)
            type-LSB1AHP4GCA(247),              -- 2-Port OC-3 ATM and 2-Port OC-3/12 ATM and 8-Port 1000Base-X Ethernet Optical Interface Line Card(CA)
            type-CLP4(248),                     -- 4 Ports OC-3/STM-1 CPOS Optical Interface Module(SFP)
            type-LSB1CLP4GCA(249),              -- 4 Ports OC-3/STM-1 CPOS Optical Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(CA)
            type-ET32(250),                     -- 32-Port Channelized E1/T1 Interface Module
            type-LSB1ET32GCA(251),              -- 32-Port Channelized E1/T1 Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(CA)
            type-LSB1IDSDB(252),                -- Intrusion Detection Service Card(DB)
            type-LSB1SRP2N1(253),               -- Switching and Route Processing Board,8*LPU

            bOARD-TYPE-LS82SRPB(254),           --
            bORAD-TYPE-LS83SRPC(255),           --
            type-Main(256),                     --

            type-LSB1SRP2N2(257),               -- Switching and Route Processing Board,5*LPU
            type-LSB1NAMB(258),                 -- NAM Service Processing Card (B)
            type-RSP2(259),                     -- 2*2.5G Resilient Packet Ring Interface
            type-LSB1RSP2CA(260),               -- 2*2.5G Resilient Packet Ring Interface Line Card(CA)
            type-SR01XP4LVC(261),               -- 4-Port 10GBase-R/W Ethernet XFP Optical Interface Line Speed Card(VC)
            type-SR01AHP4GWA(262),              -- 2-Port OC-3 ATM and 2-Port OC-3/12 ATM and 8-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01CLP4GWA(263),              -- 4 Ports OC-3/STM-1 CPOS Optical Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01ET32GWA(264),              -- 32-Port Channelized E1/T1 Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01IDSVB(265),                -- Intrusion Detection Service Card(VB)
            type-SR01SRPUF(266),                -- Switching and Route Processing Board,12*LPU
            type-SR01NAML(267),                 -- NAM Service Processing Card (L)
            type-SR01RSP2WA(268),                -- 2*2.5G Resilient Packet Ring Interface Line Card(WA)
            type-LSPM1XP1P(269),                -- 1-Port 10G XFP Module
            type-LSPM1XP2P(270),                -- 2-Port 10G XFP Module
            type-LSPM1CX2P(271),                -- 2-Port 10G CX4 Module
            type-STK-1000BASE-T(272),           -- Single Port 1000BASE-T Stack Ethernet Interface Card
--
-- 273 to 299 reserved for other product
--


--
-- 300 to 499 reserved for advanced switchs part I
--
            type-LSB1SRP1M0(300),               -- Switching and Route Process Unit,2*LPU or 3*LPU
            type-LSB1SRP1M1(301),               -- Switching and Route Process Unit
            type-LSB1GP12DB(302),               -- 12 Ports 1000Base Ethernet Optical Interface Service Card(DB)
            type-LSB1GT12DB(303),               -- 12 Ports 1000Base-T Ethernet Interface Line Card(DB)
            type-LSB1XK1DB (304),               -- 10GBase-R Ethernet XENPAK Optical Interface Line Card(DB)
            type-LSB1XP2DB (305),               -- 2-Port 10GBase-R/W Ethernet XFP Optical Interface Card(DB)
            type-LSB1XP2DC (306),               -- 2-Port 10GBase-R/W Ethernet XFP Optical Interface Card(DC)
            type-LSB1GT48LDB(307),              -- 48-Port Gigabit Ethernet RJ45 Electrical Interface Card (DB)
            type-LSB1XP4TDB(308),               -- 4-Port 10GBase-R/W Ethernet XFP Optical Interface Line Speed Test Card(DB)
            type-LSB1XP4TDC(309),               -- 4-Port 10GBase-R/W Ethernet XFP Optical Interface Line Speed Test Card(DC)
            type-LSB1RSP2DC(310),               -- 2*2.5G Resilient Packet Ring Interface Line Card(DC)
            type-LSB1VP2DC (311),               -- 2*10G Resilient Packet Ring Process Unit(DC)
            type-LSB1XP4DB (312),               -- 4-Port 10GBase-R/X Ethernet Optical Interface Line Card(DB)
            type-LSB1SRP2E0(313),               -- Switching and Route Process Unit,12*LPU
            type-LSB1SRP2E1(314),               -- Switching and Route Process Unit,8*LPU
            type-LSB1SRP2E2(315),               -- Switching and Route Process Unit,5*LPU
            type-LSB1SRP2E3(316),               -- Switching and Route Process Unit, Clock module
            type-SR01SRPUQ(317),                -- Switching and Route Processing Unit Q
            type-AHP1(318),                     -- 1-Port OC-12c(3c)/STM-4(1) ATM Optical Interface Module(SFP)
            type-AHP2(319),                     -- 2-Port OC-12c(3c)/STM-4(1) ATM Optical Interface Module(SFP)
            type-CLP1(320),                     -- 1-Port OC-3/STM-1 CPOS Optical Interface Module(SFP)
            type-CLP2(321),                     -- 2-Port OC-3/STM-1 CPOS Optical Interface Module(SFP)
            type-ET16(322),                     -- 16-Port Channelized E1/T1 Interface Module
            type-LSB1SRP1NA0(323),              -- Switching and Route Process Unit,12*LPU
            type-LSB1SRP1NA1(324),              -- Switching and Route Process Unit,8*LPU
            type-LSB1SRP1NA2(325),              -- Switching and Route Process Unit,5*LPU
            type-LSB1SRP1NA3(326),              -- Switching and Route Process Unit, Clock module
            type-SR01AHP1GWA(327),              -- 1-Port OC-12c(3c)/STM-4(1) ATM Optical Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01AHP2GWA(328),              -- 2-Port OC-12c(3c)/STM-4(1) ATM Optical Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01CLP1GWA(329),              -- 1-Port OC-3/STM-1 CPOS Optical Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01CLP2GWA(330),              -- 2-Port OC-3/STM-1 CPOS Optical Interface and 4-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01ET16GWA(331),              -- 16-Port Channelized E1/T1 Interface and  4-Port 1000Base-X Ethernet Optical Interface Line Card(WA)
            type-SR01GP12VB (332),              -- 12-Port Gigabit Ethernet Optical Interface Card(VB)
            type-SR01XK1VB(333),                -- 1-Port 10Gigabit Ethernet Optical Interface Card(VB)
            type-SR01XP2VC(334),                -- 2-Port 10GBase-RW Ethernet XFP Optical Interface Line Card(VC)
            type-SR01XP4LVB(335),               -- 4-Port 10GBase-R/W Ethernet XFP Optical Interface Line Speed Card(VB)
            type-SR01SRPUEA(336),               -- Switching and Route Process UnitŁ¬Clock Module
            type-LSB1SRP1N4(337),               -- Switching and Route Process Unit, 12*LPU
            type-LSB1SRP1N5(338),               -- Switching and Route Process Unit, 8*LPU
            type-LSB1SRP1N6(339),               -- Switching and Route Process Unit, 5*LPU
            type-LSB1SRP1N7(340),               -- Switching and Route Process Unit, Clock Module
            type-LSB1SRP2N4(341),               -- Switching and Route Process Unit, 12*LPU
            type-LSB1SRP2N5(342),               -- Switching and Route Process Unit, 8*LPU
            type-LSB1SRP2N6(343),               -- Switching and Route Process Unit, 5*LPU
            type-LSB1SRP2N7(344),               -- Switching and Route Process Unit, Clock Module
            type-LSB1SRP1NA4(345),              -- Switching and Route Process Unit, 12*LPU
            type-LSB1SRP1NA5(346),              -- Switching and Route Process Unit, 8*LPU
            type-LSB1SRP1NA6(347),              -- Switching and Route Process Unit, 5*LPU
            type-LSB1SRP1NA7(348),              -- Switching and Route Process Unit, Clock Module
            type-LSB2GV48DA(349),               -- 48-Ports 1000Base-T Ethernet Interface Line Card with POE(DA)
            type-LSB1RGP2GDB(350),              -- 2-Port GE RPR and 8-Port GE Optical Interface Service Card(DB)
            type-LSB1RGP4GDB(351),              -- 4-Port GE RPR and 8-Port GE Optical Interface Service Card(DB)
            type-LSB2GP24DB(352),               -- 24-Port 1000BASE-X  Interface Module(DB),(SFP,LC)
            type-LSB2GP24DC(353),               -- 24-Port 1000BASE-X  Interface Module(DC),(SFP,LC)
            type-LSB2GT24DB(354),               -- 24-Port 10/100/1000BASE-T Interface Module(DB),(RJ45)
            type-LSB2FW8DB (355),               -- 8-Port 1000BASE-X Interface Firewall Service Module(DB),(SFP,LC)
            type-LSB2IPSEC8DB(356),             -- 8-Port 1000BASE-X Interface IPSEC Service Module(DB),(SFP,LC)
            type-LSB2GV48DB(357),               -- 48-Port 10/100/1000BASE-T Interface Module(DB),(PoE,RJ45)
            type-RGP2(358),                     -- 2-Port GE Resilient Packet Ring Interface Module
            type-RGP4(359),                     -- 4-Port GE Resilient Packet Ring Interface Module
            type-SR02FW8VB(360),                -- 8-Port 1000BASE-X Interface Firewall Service Module(VB),(SFP,LC)
            type-SR02IPSEC8VB(361),             -- 8-Port 1000BASE-X Interface IPSEC Service Module(VB),(SFP,LC)
            type-LSB2SRP1N0(362),               -- Switching and Route Process Unit, 12*LPU
            type-LSB2SRP1N1(363),               -- Switching and Route Process Unit, 8*LPU
            type-LSB2SRP1N2(364),               -- Switching and Route Process Unit, 5*LPU
            type-LSB2SRP1N3(365),               -- Switching and Route Process Unit, Clock module
            type-LSB2SRP1N4(366),               -- Switching and Route Process Unit, 12*LPU
            type-LSB2SRP1N5(367),               -- Switching and Route Process Unit, 8*LPU
            type-LSB2SRP1N6(368),               -- Switching and Route Process Unit, 5*LPU
            type-LSB2SRP1N7(369),               -- Switching and Route Process Unit, Clock module
            type-SR02SRPUE (370),               -- Switching and Route Process Unit, Clock module
            type-SR01LN1BQH0(371),              -- Single XG Service Board(BQH)
            type-SR01DXP1L (372),               -- 1-Port 10GBASE-R/W Ethernet Optical Interface Card,(XFP,LC)
            type-SR01DGP10L(373),               -- 10-Port 1000BASE-X Optical Interface Card,(SFP,LC)
            type-SR01DRSP2L(374),               -- 2-Port 2.5G RPR Optical Interface Card,(SFP,LC)
            type-SR01DRUP1L(375),               -- 1-Port 10G RPR Optical Interface Card,(XFP,LC)
            type-SR01DGP20R(376),               -- 20-Port 1000BASE-X Optical Interface Card,(SFP,LC)
            type-SR01DPLP8L(377),               -- 8-Port 155M POS Optical Interface Card,(SFP,LC)
            type-SR01DXP2R (378),               -- 2-Port 10GBASE-R/W Ethernet Optical Interface Card,(XFP,LC)
            type-LSB1FW2A0(379),                -- Gigabit Firewall Card, 4 Gigabit Port for Management
            type-LSB1GP48LDB(380),              -- 48-Port Line Rate Gigabit Ethernet Optical Interface Card(DB)
            type-SR01LN1BNA0(381),              -- Single XG Service Board(BNA)
            type-SR01LN2BQH0(382),              -- Dual XG Service Board(BQH)
            type-SR01LN2BNA0(383),              -- Dual XG Service Board(BNA)
            type-SR01DGT20R(384),               -- 20-Port 10/100/1000BASE-T Electrical Interface Card,(RJ45)
            type-SR01DPSP4L(385),               -- 4-Port 2.5G POS Optical Interface Card(SFP,LC)
            type-SR01DPUP1L(386),               -- 1-Port 10G POS Optical Interface Card,(XFP,LC)
            type-SR01DPL2G6L(387),              -- 2-Port 155M POS Optical Interface(SFP,LC)+6-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-SR01DPH2G6L(388),              -- 2-Port 622M POS Optical Interface(SFP,LC)+6-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-SR01DPS2G4L(389),              -- 2-Port 2.5G POS Optical Interface(SFP,LC)+4-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-SR01DCL1G8L(390),              -- 1-Port 155M CPOS Optical Interface(SFP,LC)+8-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-SR01DCL2G8L(391),              -- 2-Port 155M CPOS Optical Interface(SFP,LC)+8-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-SR01DET8G8L(392),              -- 8-Port E1/T1 Electrical Interface(RJ45)+8-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-SR02SRP2E3(393),               -- Switching and Route Process Unit, Clock Module
            type-SR02SRP1E3(394),               -- Switching and Route Process Unit, Clock Module
            type-SR02SRP1M3(395),               -- Switching and Route Process Unit, Clock Module
            type-SR01DQCP4L(396),               -- 4-Port OC-3c/OC-12c/OC-48c POS/GE Optical Interface Card,(SFP,LC)
            type-SR01DTCP8L(397),               -- 8-Port OC-3c/OC-12c POS/GE Optical Interface Card,(SFP,LC)
            type-LSB1AFC1A0(398),               -- Anomaly Flow Cleaner Board
            type-LSB1SSL1A0(399),               -- SSL VPN High-end Board
            type-IMNAM(400),                    -- Net Analysis Service Processing Board
            type-IMNAT(401),                    -- Network Address Translation Service Processing Board
            type-PICAHP1L(402),                 -- 1-Port OC-12c/STM-4c ATM Optical Interface Card,(SFP,LC)
            type-PICALP4L(403),                 -- 4-Port OC-3c/STM-1c ATM Optical Interface Card,(SFP,LC)
            type-PICCHP4L(404),                 -- 4-Port 622M CPOS Optical Interface Card(SFP,LC)
            type-PICCHS1G4L(405),               -- 1-Port 622M CPOS Optical Interface(Channelized to E3/T3)+4-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-PICCLS4G4L(406),               -- 4-Port 155M CPOS Optical Interface(Channelized to E3/T3)+4-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-PICCSP1L(407),                 -- 1-Port 2.5G CPOS Optical Interface Card(SFP,LC)
            type-LSB1ACG1A0(408),               -- Application Control Gateway Board
            type-LST1MRPNC1(409),               -- Management and Route Process Unit
            type-LST1SF18B1(410),               -- S12518 Switch Fabric Card
            type-LST1SF08B1(411),               -- S12508 Switch Fabric Card
            type-LST1GT48LEC1(412),             -- 48-Port 10/100/1000BASE-T Interface Module(LEC),(RJ45)
            type-LST1GP48LEC1(413),             -- 48-Port 1000BASE-X Interface Module (LEC),(SFP,LC)
            type-LST1XP4LEC1(414),              -- 4-Port 10GBASE-R/W Interface Module (LEC),(XFP,LC)
            type-LST1XP8LEC1(415),              -- 8-Port 10GBASE-R/W Interface Module (LEC),(XFP,LC)
            type-LSR1SRP2B1(416),               -- Switching and Route Process Unit
            type-LSR1SRP2C1(417),               -- Switching and Route Process Unit
            type-LSR1SRP2B2(418),               -- Switching and Route Process Unit
            type-LSR1SRP2C2(419),               -- Switching and Route Process Unit
            type-LSR1GT24LEC1(420),             -- 16-Port 10/100/1000BASE-T Interface and 8-port 1000BASE-T/1000BASE-X Combo Interface Service Card(LEC)
            type-LSR1GP24LEB1(421),             -- 16-Port 1000BASE-X Interface and 8-port 1000BASE-T/1000BASE-X Combo Interface Service Card(LEB)
            type-LSR1GP24LEC1(422),             -- 16-Port 1000BASE-X Interface and 8-port 1000BASE-T/1000BASE-X Combo Interface Service Card(LEC)
            type-LSR1GT48LEB1(423),             -- 48-Port 10/100/1000BASE-T Interface Module(LEB),(RJ45)
            type-LSR1GT48LEC1(424),             -- 48-Port 10/100/1000BASE-T Interface Module(LEC),(RJ45)
            type-LSR1GP48LEB1(425),             -- 48-Port 1000BASE-X Interface Module(LEB),(SFP,LC)
            type-LSR1GP48LEC1(426),             -- 48-Port 1000BASE-X Interface Module(LEC),(SFP,LC)
            type-LSR2GV48REB1(427),             -- 48-Port 10/100/1000BASE-T Interface Module(REB),(PoE,RJ45)
            type-LSR1XP2LEB1(428),              -- 2-Port 10GBase-R/W Interface Module (LEB),(XFP,LC)
            type-LSR1XP2LEC1(429),              -- 2-Port 10GBase-R/W Interface Module (LEC),(XFP,LC)
            type-LSR1XP4LEB1(430),              -- 4-Port 10GBase-R/W Interface Module (LEB),(XFP,LC)
            type-LSR1XP4LEC1(431),              -- 4-Port 10GBase-R/W Interface Module (LEC),(XFP,LC)
            type-IMFW(432),                     -- Firewall Service Processing Board
            type-LSB1LB1A0(433),                -- Load Balance Board
            type-LSB1IPS1A0(434),               -- Gigabit IPS Card
            type-LST1GT48LEB1(435),             -- 48-Port 10/100/1000BASE-T Interface Module(LEB),(RJ45)
            type-LST1GP48LEB1(436),             -- 48-Port 1000BASE-X Interface Module (LEB),(SFP,LC)
            type-LST1XP4LEB1(437),              -- 4-Port 10GBASE-R/W Interface Module (LEB),(XFP,LC)
            type-LST1XP8LEB1(438),              -- 8-Port 10GBASE-R/W Interface Module (LEB),(XFP,LC)
            type-LST1XP32REB1(439),             -- 32-Port 10GBASE-R Interface Module (REB),(SFP+,LC)
            type-LST1XP32REC1(440),             -- 32-Port 10GBASE-R Interface Module (REC),(SFP+,LC)
            type-LSR1FW2A1(441),                -- Firewall Service Module
            type-LSR1SSL1A1(442),               -- SSL VPN Service Module
            type-SR01DET32G2L(443),             -- 32-Port E1/T1 75ohm Electrical Interface(DB56 Female Socket)+2-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-LSR1GP24LEF1(444),             -- 16-Port 1000BASE-X Interface and 8-port 1000BASE-T/1000BASE-X Combo Interface Service Card(LEF)
            type-LSR1XP4LEF1(445),              -- 4-Port 10GBASE-R/W Interface Module (LEF),(XFP,LC)
            type-LSR1LB1A1(446),                -- Load Balance Module
            type-LSR1NSM1A1(447),               -- NetStream Module
            type-LSR1ACG1A1(448),               -- Application Control Gateway Service Module
            type-LSR1IPS1A1(449),               -- Intrusion Protection System Service Module
            type-LSR2GP24LEB1(450),             -- 16-Port 1000BASE-X Interface and 8-port 1000BASE-T/1000BASE-X Combo Interface Service Card(LEB)
            type-LSR2GT24LEB1(451),             -- 16-Port 10/100/1000BASE-T Interface and 8-port 1000BASE-T/1000BASE-X Combo Interface Service Card(LEB)
            type-LSR2GT48LEB1(452),             -- 48-Port 10/100/1000BASE-T Interface Module(LEB),(RJ45)
            type-SPC-GP24L(453),                -- 24-Port 1000BASE-X Interface Service Card,(SFP,LC)
            type-SPC-GT48L(454),                -- 48-Port 10/100/1000BASE-T Interface Module,(RJ45)
            type-SPC-GP48L(455),                -- 48-Port 1000BASE-X Interface Module,(SFP,LC)
            type-SPC-XP2L(456),                 -- 2-Port 10GBASE-R/W Interface Service Card,(XFP,LC)
            type-SPC-XP4L(457),                 -- 4-Port 10GBase-R/W Interface Module,(XFP,LC)
            type-SR06SRP2E3(458),               -- SDI,Routing Switch Processing Board
            type-SPE-2010-E(459),               -- SDI,Single XG Service Board
            type-SPE-2020-E(460),               -- SDI,Dual XG Service Board
            type-SPC-XP4L-S-SDI(461),           -- SDI 4-Port 10GBase-R/W Interface Module,(XFP,LC)
            type-SPC-GT48L-SDI(462),            -- SDI 48-Port 10/100/1000BASE-T Interface Module,(RJ45)
            type-SPC-GP48L-S-SDI(463),          -- SDI 48-Port 1000BASE-X Interface Module,(SFP,LC)
            type-SR02OPMA0(464),                -- Single Mode 1310&1550nm Optical Protect Board(LC)
            type-LSR1XP16REB1(465),             -- 16-Port 10GBASE-R Interface Module (REB),(SFP+,LC)
            type-LSR1GP48LEF1(466),             -- 48-Port 1000BASE-X Interface Module (LEF),(SFP,LC)
            type-LST1GP48LEF1(467),             -- 48-Port 1000BASE-X Interface Module (LEF),(SFP,LC)
            type-LST1XP8LEF1(468),              -- 8-Port 10GBASE-R/W Interface Module (LEF),(XFP,LC)
            type-SPE-1010-II(469),              -- Single XG Service Board-II
            type-SPE-1010-E-II(470),            -- Enhanced Single XG Service Board-II
            type-SPE-1020-II(471),              -- Double XG Service Board-II
            type-SPE-1020-E-II(472),            -- Enhanced Double XG Service Board-II
            type-LST1FW2A1(473),                -- Firewall Board (LEC)
            type-LST1NSM1A1(474),               -- NetStream Service Board (LEC)
            type-LST1LB1A1(475),                -- Load Balancing Board (LEC)
            type-LST1ACG1A1(476),               -- Application Control Gateway Board Module (LEC)
            type-LST1IPS1A1(477),               -- Gigabit Intrusion Prevention System Module
            type-LSR1DRUP1L1(478),              -- 1-Port OC-192c/STM-64c RPR Optical Interface Card,(XFP,LC)
            type-LSR1DPUP1L1(479),              -- 1-Port OC-192c/STM-64c POS Optical Interface Card,(XFP,LC)
            type-LSR1DPSP4L1(480),              -- 4-Port OC-48c/STM-16c POS Optical Interface Card,(SFP,LC)
            type-LSR1DTCP8L1(481),              -- 8-Port OC-3c/OC-12c POS/GE Optical Interface Card,(SFP,LC)
            type-LSR1DXP1L1(482),               -- 1-Port 10GBASE-R/W Ethernet Optical Interface Card,(XPF,LC)
            type-LSR1DGP10L1(483),              -- 10-Port 1000BASE-X Optical Interface Card,(SFP,LC)
            type-LSR1LN1BNL1(484),              -- Single Service Processing Board
            type-LSR1LN2BL1(485),               -- Dual Serivice Processing Board
            type-LSR1SRP2D1(486),               -- Switching and Route Process Unit With Clock
            type-IM-NAT-II(487),                -- Network Address Translation Service Processing Board,II
            type-IM-NAM-II(488),                -- Net Analysis Service Processing Board,II
            type-CR-MRP-I(489),                 -- Management and Route Unit With OAM Module and Clock Module
            type-CR-SF18C(490),                 -- Switch Fabric Card for CR16018
            type-CR-SF08C(491),                 -- Switch Fabric Card for CR16008/CR16004
            type-CR-SPC-XP8LEF(492),            -- 8-Port 10GBASE-R/W Interface Module,(XFP,LC)
            type-CR-SPC-XP4LEF(493),            -- 4-Port 10GBASE-R/W Interface Module,(XFP,LC)
            type-CR-SPC-GP48LEF(494),           -- 48-Port 1000BASE-X Interface Module,(SFP,LC)
            type-CR-SPC-GT48LEF(495),           -- 48-Port 10/100/1000BASE-T Interface Module
            type-CR-SPE-3020-E(496),            -- Double XG Service Board (Enhanced)
            type-CR-SPC-PUP4L-E(497),           -- 4-Port 10G POS Optical Interface Module,(XFP,LC)
            type-LST1SF08C1(498),               -- Switch Fabric Card
            type-LST1SF18C1(499),               -- Switch Fabric Card

--
-- 500 to 699 reserved for secondary switchs
--
            type-LS81GP16TM(500),               -- 12-port 1000BASE-X SFP Interface and 4-port 1000BASE-T/1000BASE-X Combo Interface Metro Switch and Route Processing Board
            type-LS81VP4C(501),                 -- 4-port 1000BASE-X SFP Interface Virtual Daughter Card
            type-LS8M1PT8P0(502),               -- 8-Port 1000BASE-PX Optical Line Interface Board, SFP Req
            type-LS8M1PT8GB0(503),              -- 8-Port 1000BASE-PX20 Gigabit Passive Optical Line Interface Board B(20km, SFF), SC Connector
            type-LS8M1PT4GB0(504),              -- 4-Port 1000BASE-PX20 Gigabit Passive Optical Line Interface Board B(20km, SFF), SC Connector
            type-LS81GP2R(505),                 -- 2-Port 1000M Ethernet Optical Interface RPR Board
            type-LS81GP4R(506),                 -- 4-Port 1000M Ethernet Optical Interface RPR Board
            type-LS81IPSECA(507),               -- IPSec Service Board
            type-LS81FWA(508),                  -- Firewall Service Board
            type-LS82VSNP(509),                 -- Versatile Network Processing Service Module (PBR/NAT/NetStream) with 12-port 1000BASE-X SFP, XGBUS Uplink
            type-LSQ1GV48SA(510),               -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45)
            type-LSQ1SRPB(511),                 -- Salience VI
            type-LSQ1SRP2XB(512),               -- Salience VI-10GE
            type-LSQ1SRP1CB(513),               -- Salience VI-Turbo
            type-LSQ1FV48SA(514),               -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45)
            type-LSD1MPUA(515),                 -- Main Control Unit
            type-LSD1GP20A0(516),               -- 16-port 1000BASE-X SFP Interface and 4-port 1000BASE-T/1000BASE-X Combo Interface Line Card
            type-LSD1GP20TA0(517),              -- 16-port 1000BASE-X SFP Interface and 4-port 1000BASE-T/1000BASE-X Combo Interface and 16 1000BASE-T Interface Line Card
            type-LSD1GP36A0(518),               -- 32-port 1000BASE-X SFP Interface and 4-port 1000BASE-T/1000BASE-X Combo Interface Line Card
            type-LSD1GP20XA0(519),              -- 16-port 1000BASE-X SFP Interface and 4-port 1000BASE-T/1000BASE-X Combo Interface and 2-port 10GBASE-X XFP Interface Line Card
            type-LSD1GP20EA0(520),              -- 16-port 1000BASE-X SFP Interface and 4-port 1000BASE-T/1000BASE-X Combo Interface and 2-port GE RPR Interface Line Card
            type-LSD1GP20RA0(521),              -- 16-port 1000BASE-X SFP Interface and 4-port 1000BASE-T/1000BASE-X Combo Interface and 2-port OC48 RPR Interface Line Card
            type-LSD1GP16A0(522),               -- 16-port 1000BASE-X SFP Ethernet Interface SubCard
            type-LSD1GT16A0(523),               -- 16-port 1000BASE-T Ethernet Interface SubCard
            type-LSD1XP2A0(524),                -- 2-port 10GBASE-X XFP Ethernet Interface SubCard
            type-LSD1EP2A0(525),                -- 2-port 1000BASE-T Ethernet RPR Interface SubCard
            type-LSD1RP2A0(526),                -- 2-port OC48 RPR Interface SubCard
            type-LSQ1GV48SC(527),               -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45)-POE
            type-LSQ1FP48SA(528),               -- 48 Port 100M Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1GP24SC(529),               -- 24 Port 1000BASE-X Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1GT24SC(530),               -- 24-Port 1000BASE-T Ethernet Interface Board (RJ45)
            type-LSQ1TGX2SC(531),               -- 2-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1GP12EA(532),               -- 12-Port 1000BASE-X Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1TGX1EA(533),               -- 1-Port 10GBASE Ethernet Optical Interface Module(XFP,LC)
            type-LSQ1P24XGSC(534),              -- 24-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC)+2-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1T24XGSC(535),              -- 24-Port 1000BASE-T Gigabit Ethernet Interface(RJ45)+2-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LS81TGX1B(536),                -- 1 Port 10GBase-R Ethernet Interface Board(XENPAK,SC)
            type-LSQ1PT4PSC0(537),              -- 4-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LS81SRPG13(538),               -- Salience V, Switch and Route Processing Board
            type-LS81SRPG14(539),               -- Salience V Edge
            type-LS81SRPG15(540),               -- Salience V Plus
            type-LSQ1GP48SC0(541),              -- 48-Port 1000BASE Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1GP12SC0(542),              -- 12-Port 1000BASE-X Ethernet Optical Interface Board(SFP,LC)
            type-LSD1SRPA0(543),                -- Salience VIII 160
            type-LSD1SRPB0(544),                -- Salience VIII 480
            type-LSD1SRPC0(545),                -- Salience VIII 800
            type-LSD1GT16PES0(546),             -- 16-Port 10/100/1000BASE-T and 8-Port 100/1000BASE-X SFP Interface Card
            type-LSD1GP24ES0(547),              -- 24-Port 1000BASE-X Ethernet SFP Interface Card
            type-LSD1GT24XES0(548),             -- 24-Port 10/100/1000BASE-T and 2-port 10GBASE-X Ethernet XFP Optical Interface Card
            type-LSD1GP24XES0(549),             -- 24-Port 1000BASE-X Ethernet SFP interface and 2-port 10GBASE-X Ethernet XFP Optical Interface Card
            type-LSD1XP2ES0(550),               -- 2-Port 10GBASE-X Ethernet XFP Optical Interface Card
            type-LSD1GP48ES0(551),              -- 48-Port 1000BASE-X Ethernet SFP Interface Card
            type-LSQ1MPUA0(552),                -- Master Process Board
            type-LSQ1MPUA1(553),                -- Master Process Unit
            type-LSQ1FWBSC0(554),               -- Gigabit Firewall CardŁ¬4 Gigabit Port for Management
            type-LSQ1PT8PSC0(555),              -- 8-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LSQ1PT16PSC0(556),             -- 16-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-SA11MPUA0(557),                -- SmartEngine I-Lite
            type-SA11MPUB0(558),                -- SmartEngine I
            type-LSQ1AFCBSC0(559),              -- Anomaly Flow Cleaner Board
            type-LSQ1MPUB0(560),                -- Salience VI-Lite
            type-LSQ1MPUB1(561),                -- Salience VI-Lite
            type-LSQ1PT4PSC1(562),              -- 4-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LSQ1PT8PSC1(563),              -- 8-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LSQ1PT16PSC1(564),             -- 16-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LSQ1FP48USA0(565),             -- 48-Port 100M Ethernet Optical Interface Switch Unit(SFP,LC)
            type-LSQ1FP48USA1(566),             -- 48-Port 100M Ethernet Optical Interface Switch Unit(SFP,LC)
            type-LSQ1FV48USA0(567),             -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45),PoE
            type-LSQ1FV48USA1(568),             -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45),PoE
            type-LSQ1SRPD0(569),                -- Switch and Route Processing Unit, Salience VI-Plus
            type-LSQ1CGP24TSC0(570),            -- Switching and Routing Processing Unit with 24 1000BASE-X Gigabit Ethernet Optical Ports,including 8 Combo Ports,SFP Req.
            type-LSQ1GP24TSC0(571),             -- 16-Port 1000BASE-X Gigabit Ethernet Optical(SFP,LC) And 8-Port 10/100/1000BASE-T RJ45/1000BASE-X SFP Combo Interface Board
            type-LSQ1ACGASC0(572),              -- Application Control Gateway Board
            type-LSD1XP1ES0(573),               -- 1-Port 10GBASE-X Ethernet XFP Optical Interface Card
            type-LSD1GP12ES0(574),              -- 12-Port 1000BASE-X Ethernet SFP Interface Card
            type-LSQ1SRP12GB0(575),             -- Switch And Route Processing Unit with 12 1000BASE Ethernet Optical Interfaces(SFP,LC),Salience VI-GE
            type-LSQ1GV40PSC0(576),             -- 40-Port 10/100/1000BASE-T Electrical(RJ45) And 8-Port 1000BASE-X Optical Ethernet Interface Board(SFP,LC),PoE
            type-LSQ1FWBSC1(577),               -- Firewall Board
            type-LSQ1NSMSC0(578),               -- NetStream Board
            type-LSQ1NSMSC1(579),               -- NetStream Board
            type-LSQ1AFDBSC0(580),              -- Anomaly Flow Detector Board
            type-LS81MPUB(581),                 -- Salience IV
            type-LS81FP48XL(582),               -- 48-Port 100M Ethernet Optical Interface Module,(SFP,LC)
            type-LS81FT48XL(583),               -- 48-Port 10/100M Ethernet Electrical Interface Module(RJ45)
            type-LS81GP12XL(584),               -- 12-Port 1000/100M Ethernet Optical Interface Module(SFP,LC)
            type-LS81GP24XL(585),               -- 24-Port 1000/100M Ethernet Optical Interface Module(SFP,LC)
            type-LS81GP48XL(586),               -- 48-Port 1000/100M Ethernet Optical Interface Module(SFP,LC)
            type-LS81GT24XL(587),               -- 24-Port 10/100/1000M Ethernet Electrical Interface Module(RJ45)
            type-LS81GT48XL(588),               -- 48-Port 10/100/1000M Ethernet Electrical Interface Module(RJ45)
            type-LS81TGX2XL(589),               -- 2-Port 10GBASE Ethernet Optical Interface Module(XFP,LC)
            type-LSQ1GV48SD0(590),              -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45),PoE
            type-LSQ1GP48EB0(591),              -- 48-Port Enhanced 1000BASE-X Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1IPSSC0(592),               -- Gigabit IPS Card
            type-LSQ1GV48SD1(593),              -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45),PoE
            type-LSQ1GP48SD0(594),              -- 48-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC) Interface Board
            type-LSQ1GP48SD1(595),              -- 48-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC) Interface Board
            type-LSQ1SRPA0(596),                -- Salience VI-Smart
            type-LSQ1SRPA1(597),                -- Salience VI-Smart
            type-LSQ2FP48SA0(598),              -- 48 Port 100M Ethernet Optical Interface Board(SFP,LC)
            type-LSQ2FP48SA1(599),              -- 48 Port 100M Ethernet Optical Interface Board(SFP,LC)
            type-LSQ2FT48SA0(600),              -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45)
            type-LSQ2FT48SA1(601),              -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45)
            type-LSQ1GV24PSC0(602),             -- 24-Port 10/100/1000BASE-T Electrical(RJ45) Interface Board,including 4 Combo Ports,SFP Req,PoE,No Spell
            type-LSQ1GV24PSC1(603),             -- 24-Port 10/100/1000BASE-T Electrical(RJ45) Interface Board,including 4 Combo Ports,SFP Req,PoE,No Spell
            type-LSQ1CGV24PSC0(604),            -- Switching and Routing Processing Unit with 24 10/100/1000BASE-T Electrical Ports(RJ45),including 4 Combo Ports,SFP Req,PoE,No Spell
            type-LSQ1CGV24PSC1(605),            -- Switching and Routing Processing Unit with 24 10/100/1000BASE-T Electrical Ports(RJ45),including 4 Combo Ports,SFP Req,PoE,No Spell
            type-LSQ1GP24TEB0(606),             -- 16-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC)+8-Port Combo Interface Board
            type-LSQ1GP24TEB1(607),             -- 16-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC)+8-Port Combo Interface Board
            type-LSQ1GP24TSD0(608),             -- 16-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC)+8-Port Combo Interface Board
            type-LSQ1GP24TSD1(609),             -- 16-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC)+8-Port Combo Interface Board
            type-LSQ1GP24TXSD0(610),            -- 16-Port GE Optical Interface(SFP,LC)+8-Port Combo Interface+2-Port 10GE Optical Interface Board(XFP,LC)
            type-LSQ1GP24TXSD1(611),            -- 16-Port GE Optical Interface(SFP,LC)+8-Port Combo Interface+2-Port 10GE Optical Interface Board(XFP,LC)
            type-LSQ1TGX2EB0(612),              -- 2-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX2EB1(613),              -- 2-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX2SD0(614),              -- 2-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX2SD1(615),              -- 2-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX4SD0(616),              -- 4-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX4SD1(617),              -- 4-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX8SD0(618),              -- 8-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX8SD1(619),              -- 8-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1GP48EB1(620),              -- 48-Port Enhanced 1000BASE-X Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1TGX4EB0(621),              -- 4-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1TGX4EB1(622),              -- 4-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)
            type-LSQ1GP12SC3(623),              -- 12-Port 1000BASE-X Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1GP24TSC3(624),             -- 16-Port 1000BASE-X Gigabit Ethernet Optical(SFP,LC) And 8-Port 10/100/1000BASE-T RJ45/1000BASE-X SFP Combo Interface Board
            type-LSQ1GP48SC3(625),              -- 48-Port 1000BASE Ethernet Optical Interface Board(SFP,LC)
            type-LSQ1GV48SC3(626),              -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45),PoE
            type-LSQ1MPUA3(627),                -- Master Process Board
            type-LSQ1SRP1CB3(628),              -- Salience VI-Turbo
            type-LSQ1SRPA3(629),                -- Salience VI-Smart
            type-LSQ2FP48SA3(630),              -- 48 Port 100M Ethernet Optical Interface Board(SFP,LC)
            type-LSQ2FT48SA3(631),              -- 48-Port 100M Ethernet Electrical Interface Switch Unit(RJ45)
            type-LSQ1MPUB3(632),                -- Salience VI-Lite
            type-LSQ1CGP24TSC3(633),            -- Switching and Routing Processing Unit with 24 1000BASE-X Gigabit Ethernet Optical Ports,including 8 Combo Ports,SFP Req.
            type-LSQ1MPUB4(634),                -- Salience VI-Lite
            type-LSQ1SRPD4(635),                -- Salience VI-Plus
            type-LSQ1SSLSC0(636),               -- SSL VPN Service Board(B)
            type-LSQ1LBSC0(637),                -- Gigabit Load Balancing Card
            type-LSQ1NAT24SC0(638),             -- NAT/NetStream-Supported Line Processing Unit with 24 10/100/1000BASE-T Electrical Ports(RJ45),including Combo Ports,Upgradeable to PoE
            type-LSQ1SRP12GB4(639),             -- Salience VI-GE
            type-LSQ1TGS8SC0(640),              -- 8-Port 10GBASE Ethernet SFP+ Optical Interface Board
            type-LSQ3PT4PSC0(641),              -- 4-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-EWPXM2MPUB0(642),              -- Salience VI-Lite
            type-EWPXM2SRP12GB0(643),           -- Salience VI-GE
            type-EWPXM2SRPD0(644),              -- Salience VI-Plus
            type-EWPXM2GP24TSD0(645),           -- 16-Port 1000BASE-X Ethernet Optical Interface(SFP Req.)+8-Port Combo Interface Module
            type-EWPXM2GP24TXSD0(646),          -- 16-Port 1000BASE-X Ethernet Optical Interface(SFP Req.)+8-Port Combo Interface+2-Port 10GE Optical Interface(XFP Req.) Module
            type-EWPXM2TGX4SD0(647),            -- 4-Port 10GBASE Ethernet Optical Interface Module,XFP Req
            type-EWPXM2GP48SD0(648),            -- 48-Port 1000BASE-X Gigabit Ethernet Optical Interface Module,SFP Req
            type-EWPXM2GP24TSC0(649),           -- 24-Port 1000BASE-X/100BASE-FX Optical  Interface Module,including 8 Combo Ports,SFP Req
            type-EWPXM2TGX2SC0(650),            -- 2-Port 10GBASE Ethernet Optical Interface Module,XFP Req
            type-EWPXM2GP48SC0(651),            -- 48-Port 1000BASE-X/100BASE-FX Ethernet Optical Interface Module,SFP Req
            type-LS7500-GP48-SC(652),           -- 48-Port 1000BASE-X/100BASE-FX Ethernet Optical Interface Module(SFP,LC)
            type-LS7500-GP48-SD(653),           -- 48-Port 1000BASE-X Gigabit Ethernet Optical Interface Module(SFP,LC)
            type-LS7500-GT48-SC(654),           -- 48-Port 10/100/1000BASE-TX Ethernet Interface Module(RJ45)
            type-LS7500-GT48-SD(655),           -- 48-Port 10/100/1000BASE-T Ethernet Interface Module(RJ45)
            type-LS7500-SRPG1(656),             -- Main Control Unit
            type-LS7500-SRPG2(657),             -- Salience VI-Lite
            type-LS7500-XP4-SD(658),            -- 4-Port 10GBASE Ethernet Optical Interface Module(XFP,LC)
            type-LS7500-XP8-SD(659),            -- 8-Port 10GBASE Ethernet Optical Interface Module(XFP,LC)
            type-LSQ4PT4PSC0(660),              -- 4-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LSQ4PT8PSC0(661),              -- 8-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LSQ4PT16PSC0(662),             -- 16-Port 1000Base-PX Optical Line Terminal(EPON OLT SFP,SC)+8-Port 1000BASE-X Optical Interface Board(SFP,LC)
            type-LSQ1GP24TSA0(663),             -- 16-Port 1000BASE-X Gigabit Ethernet Optical(SFP,LC) And 8-Port 10/100/1000BASE-T RJ45/1000BASE-X SFP Combo Interface Board
            type-LSQ1GV24PSA0(664),             -- 24-Port 10/100/1000BASE-T Electrical(RJ45) Interface Board,including 4 Combo Ports,SFP Req,Upgradeable to PoE
            type-LSQ1SRPD3(665),                -- Salience VI-Plus
            type-LSQ1SUPA0(666),                -- Supervisor Engine Board
            type-LSU1FAB04A0(667),              -- Switch Fabric Board
            type-LSU1FAB08A0(668),              -- Switch Fabric Board
            type-LSU1TGS8EA0(669),              -- 8-Port 10GBASE Ethernet SFP+ Optical Interface Board(EA)
            type-LSU1TGS8EB0(670),              -- 8-Port 10GBASE Ethernet SFP+ Optical Interface Board
            type-LSU1TGS8SE0(671),              -- 8-Port 10GBASE Ethernet SFP+ Optical Interface Board(SE)
            type-LSUTGS16SC0(672),              -- 16-Port 10GBASE Ethernet SFP+ Optical Interface Board
            type-LUS1SUPA0(673),                -- Supervisor Engine Board
            type-LSU1GP24TXEA0(674),            -- 16-Port 1000BASE-X Optical Interface(SFP,LC)+8-Port Combo Interface+2-Port 10GE Optical Interface Board(XFP,LC)(EA)
            type-LSU1GP24TXEB0(675),            -- 16-Port 1000BASE-X Optical Interface(SFP,LC)+8-Port Combo Interface+2-Port 10GE Optical Interface Board(XFP,LC)(EB)
            type-LSU1GP24TXSE0(676),            -- 16-Port 1000BASE-X Optical Interface(SFP,LC)+8-Port Combo Interface+2-Port 10GE Optical Interface Board(XFP,LC)(SE)
            type-LSU1GP48EA0(677),              -- 48-Port 1000BASE-X Gigabit Ethernet Optical Interface(SFP,LC) Interface Board(EA)
            type-LSU1GP48EB0(678),              -- 48-Port Enhanced 1000BASE-X Ethernet Optical Interface Board(SFP,LC)(EB)
            type-LSU1GP48SE0(679),              -- 48-Port 1000BASE Ethernet Optical Interface Board(SFP,LC)(SE)
            type-LSU1GT48EA0(680),              -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45)(EA)
            type-LSU1GT48SE0(681),              -- 48-Port 1000Base-T Gigabit Ethernet Interface Board(RJ45)(SE)
            type-LSU1TGX4EA0(682),              -- 4-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)(EA)
            type-LSU1TGX4EB0(683),              -- 4-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)(EB)
            type-LSU1TGX4SE0(684),              -- 4-Port 10GBASE Ethernet Optical Interface Board(XFP,LC)(SE)
            type-LSQ1FAB08A0(685),              -- Switching Fabric Board
            type-EWPX2WCMD0(686),               -- Access Controller Card
            type-LSQ1WCMD0(687),                -- Access Controller Card
            type-LSQ1IAGSC0(688),               -- Wireless&IAG Service Card
            type-LSU1GP24TSE0(689),             -- 16-Port 1000BASE-X Optical Interface(SFP,LC)+8-Port Combo Interface Board(SE)
            type-LSQ1TGS16SC0(690),             -- 16-Port 10GBASE Ethernet SFP+ Optical Interface Board
            type-EWPX2TGS16SC0(691),            -- 16-Port 10GBASE Ethernet SFP+ Optical Interface Board
            type-LSQ1SUPA3(692),                -- Supervisor Engine Board
            type-LSQ1FAB04A3(693),              -- 320G Switch Fabric Board
            type-LSQ1FAB08A3(694),              -- 640G Switch Fabric Board,For S7608-X & S7608-XV

--
-- 700 to 799 reserved for primary switchs
--
            type-1000BASE-X-COMBO(701),         -- Single port 10/100/1000BASE-T/1000BASE-X Combo Interface Board
            type-EPON-1000M(702),               -- Optical Network Unit Interface Board
            type-1000BASE-FIXED-2SFP-T-2RJ45(703),         -- 2 port 10/100/1000BASE-T and 2 port 1000BASE-X Interface Board
            type-100M-1550-BIDI(704),           -- 100BASE-X BIDI Interface Board,Tx 1550nm, Rx 1310nm
            type-100M-1310-BIDI(705),           -- 100BASE-X BIDI reverse Interface Board,Tx 1310nm, Rx 1550nm
            type-1000BASE-FIXED-4RJ45-4SFP-COMBO(706),     -- 4 port 10/100/1000BASE-T and 4 port 1000BASE-X COMBO Interface Board
            type-LSH1PK2T(707),                 -- OSM Interface Board
            type-LSPM2GP2P(708),                -- 2-Port 1000BASE-X SFP Module
            type-LSWM1GT16P(709),               -- 16-Port 10/100/1000BASE-T Ethernet Electrical Interface Module
            type-LSWM1GP16P(710),               -- 16-Port 100/1000BASE-X Ethernet Optical Interface Module
            type-LSWM1XP2P(711),                -- 2-Port 10G Ethernet XFP Optical Interface Module
            type-LSWM1XP4P(712),                -- 4-Port 10G Ethernet XFP Optical Interface Module
            type-LSWM1SP2P(713),                -- 2-Port 10G Ethernet SFP PLUS Optical Interface Module
            type-LSWM1SP4P(714),                -- 4-Port 10G Ethernet SFP PLUS Optical Interface Module
            type-LSWM148POEM(715),              -- 48 Port Mid Power PoE Module
            type-LSWM1FW10(716),                -- RMI CPU XLR 732, with Firewall software
            type-LSWM1WCM10(717),               -- RMI CPU XLR 732, with Wireless Access Controller software
            type-LSWM1IPS10(718),               -- RMI CPU XLR 732, with IPS/AV software
            type-LSWM1WCM20(719),               -- RMI CPU XLR 408, with Wireless Access Controller software
            type-LSPM2SP2P(725),                -- 2-Port 10G Ethernet SFP PLUS Optical Interface Module
            type-LSPM2SP2PA(726),               -- 2-Port Second Version SFP+ Module
            type-LSP5GP8P(727),                 -- 8-Port 1G Ethernet SFP Optical Interface Module
            type-LSP5GT8P(728),                 -- 8-Port 10/100/1000BASE-T Ethernet Electrical Interface Module
            type-LSWM1FC4P(729),                -- 4-Port 8G Fibre Channel Interface Module

--
-- 800 to 899 reserved for WLAN products
--
            type-WX5002MPU(800),                -- Wireless Lan Control Board with 2-port 1000BASE-T/1000BASE-X Combo Interface
            type-LS8M1WCMA(801),                -- Wireless Lan Service Board
            type-EWPX1G24XA0(802),              -- 24-Port 1000BASE-T Gigabit Ethernet Interface(RJ45) and 4-port 1000BASE-T/1000BASE-X Combo Interface and 2-port 10GBASE Interface Line Card
            type-LSQ1WCMB0(803),                -- 1 Port 10GBASE Interface Board
            type-LSB1WCM2A0(804),               -- Wireless Controller Module Board
            type-EWPX1WCMB0(805),               -- 1 Port 10GBASE Interface Board
            type-EWPX1G24XC0(806),              -- 24-Port 1000BASE-T Gigabit Ethernet Interface(RJ45) and 4-port 1000BASE-T/1000BASE-X Combo Interface Line Card
            type-EWPX1WCMC0(807),               -- 1-Port 1000BASE-T Gigabit Ethernet of wireless Lan Service Board
            type-EWPX1FWA0(808),                -- Firewall Service Board
            type-EWPX1G10XC0(809),              -- 8-Port 1000BASE-T Gigabit Ethernet Interface(RJ45) and 2-port 1000BASE-X SFP Interface Line Card
            type-EWPX1WCM10C0(810),             -- 1-Port 1000BASE-T Gigabit Ethernet of wireless Lan Service Board
            type-LSR1WCM2A1(811),               -- 1-Port 1000BASE-T Gigabit Ethernet of wireless Lan Service Board
            type-EWPX1WAP0(812),                -- WAPI Encryption Card
            type-EWPX1WCMD0(813),               -- 2 Port 10GBASE Interface Board
            type-EWPX1G24XCE0(814),             -- 24-Port 1000BASE-T Gigabit Ethernet Interface(RJ45) and 4-port 1000BASE-T/1000BASE-X Combo Interface Line Card
            type-EWPX1WCMCE0(815),              -- 2-Port 1000BASE-T Gigabit Ethernet of wireless Lan Service Board

--
-- 900 to 1099 reserved for advanced switchs part II
--
            type-LSR1DRSP2L1(900),              -- 2-Port OC-48c/STM-16c RPR Optical Interface Card(SFP,LC)
            type-PIC-CLF2G8L(901),              -- 2-Port 155M CPOS Optical Interface(SFP,LC)+8-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-PIC-CLF4G8L(902),              -- 4-Port 155M CPOS Optical Interface(SFP,LC)+8-Port 1000BASE-X Optical Interface Card(SFP,LC)
            type-SR02SRP2F3(903),               -- Routing Switch Processing Board(2F)
            type-SR02SRP1F3(904),               -- Routing Switch Processing Board(1F)
            type-LST1GT48LEA1(905),             -- 48-Port 10/100/1000BASE-T Interface Module(LEA),(RJ45)
            type-LST1GP48LEA1(906),             -- 48-Port 1000BASE-X Interface Module(LEA),(SFP,LC)
            type-LST2XP8LEA1(907),              -- 8-Port 10GBASE-R Interface Module(LEA),(SFP+,LC)
            type-LST1GT48LEY1(908),             -- 48-Port 10/100/1000BASE-T Interface Module(LEY),(RJ45)
            type-LST1GP48LEY1(909),             -- 48-Port 1000BASE-X Interface Module(LEY),(SFP,LC)
            type-LST1XP32REY1(910),             -- 32-Port 10GBASE-R Interface Module(REY),(SFP+,LC)
            type-LST1XP8LEY1(911),              -- 8-Port 10GBASE-R/W Interface Module(LEY),(XFP,LC)
            type-LST1GP48LEZ1(912),             -- 48-Port 1000BASE-X Interface Module(LEZ),(SFP,LC)
            type-LST1XP8LEZ1(913),              -- 8-Port 10GBASE-R/W Interface Module(LEZ),(XFP,LC)
            type-IM-FW-II(914),                 -- Firewall Service Processing Board-II
            type-IM-IPS(915),                   -- Intrusion Prevention System Service Processing Board
            type-IM-SSL(916),                   -- SSL VPN Service Processing Board
            type-IM-LB(917),                    -- Load Balance Service Processing Board
            type-IM-ACG(918),                   -- Application Control Gateway Service Processing Board
            type-LSR1XP16REC1(919),             -- 16-Port 10GBASE-R Interface Module(REC),(SFP+,LC)
            type-LST2XP8LEB1(920),              -- 8-Port 10GBASE-R Interface Module(LEB),(SFP+,LC)
            type-LST2XP8LEC1(921),              -- 8-Port 10GBASE-R Interface Module(LEC),(SFP+,LC)
            type-LST2XP8LEF1(922),              -- 8-Port 10GBASE-R Interface Module(LEF),(SFP+,LC)
            type-LST2XP4LEB1(923),              -- 4-Port 10GBase-R Interface Module(LEB),(SFP+,LC)
            type-LST2XP4LEC1(924),              -- 4-Port 10GBase-R Interface Module(LEC),(SFP+,LC)
            type-LST2XP32REB1(925),             -- 32-Port 10GBASE-R Interface Module(REB),(SFP+,LC)
            type-LST2XP32REC1(926),             -- 32-Port 10GBASE-R Interface Module(REC),(SFP+,LC)
            type-LSR1WCM3A1(927),               -- Access Controller Module
            type-LST1XP16LEB1(928),             -- 16-Port 10GBASE-R Interface Module (LEB),(SFP+,LC)
            type-LST1XP16LEC1(929),             -- 16-Port 10GBASE-R Interface Module (LEC),(SFP+,LC)
            type-CR-SPC-XP4L-E-I(930)           -- 4-Port 10GBASE-R/W Optical Interface Module,(XFP,LC)
        }

    hwLswSystemPara OBJECT IDENTIFIER ::= {  hwLswDeviceAdmin 1  }

-- ==================================================================

    hwLswSysIpAddr OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "System IP address, which is the primary IP address of the VLAN
         interface that has smallest VLAN ID and is configured IP address."
        ::= { hwLswSystemPara 1 }

    hwLswSysIpMask OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Mask of the system IP address."
        ::= { hwLswSystemPara 2 }

    hwLswSysCpuRatio OBJECT-TYPE
        SYNTAX Integer32 (0..100)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "CPU usage of the system in accuracy of 1%, and the range of value is
        1 to 100."
        ::= { hwLswSystemPara 3 }

    hwLswSysVersion OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..64))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Information of the system version."
        ::= { hwLswSystemPara 4 }

     hwLswSysTime OBJECT-TYPE
        SYNTAX DateAndTime
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "System time."
        ::= { hwLswSystemPara 5 }

     hwLswSysUNMCastDropEnable OBJECT-TYPE
        SYNTAX INTEGER
        {
            disable (0),
            enable  (1)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Enable or disable discarding of unknown multicast packet."
        ::= { hwLswSystemPara 6 }

     hwLswSysManagementVlan OBJECT-TYPE
        SYNTAX Integer32 (1..4094)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "System management VLAN."
        ::= { hwLswSystemPara 7 }

     hwLswSysVlanRange OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..10))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "System VLAN range, if set VLAN range, must bind mangement IP/Mask."
        ::= { hwLswSystemPara 8 }

     hwLswSysManagementIpAddr OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "System IP address."
        ::= { hwLswSystemPara 9 }

    hwLswSysManagementIpMask OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Mask of the system IP address."
        ::= { hwLswSystemPara 10 }

    hwMacAddressCountPort OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Supportted MAC address number on port."
        ::= { hwLswSystemPara 11 }

    hwMacAddressCountMachine OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Supportted MAC address number on machine."
        ::= { hwLswSystemPara 12 }

    hwLswSysPhyMemory OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "byte"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The memory of physical.
        For the distributed device, it represents the memory size on the master
        slot.

        If the amount of physical memory exceeds 4,294,967,295 bytes,
        the value remains 4,294,967,295 bytes."
        ::= { hwLswSystemPara 13 }

    hwLswSysMemory OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "byte"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The memory of system.
        Note that the system memory means the memory can be used by the software
        platform.

        For the distributed device, it represents the memory size on the master
        slot.

        If the amount of system memory exceeds 4,294,967,295 bytes,
        the value remains 4,294,967,295 bytes."
        ::= { hwLswSystemPara 14 }

    hwLswSysMemoryUsed OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "byte"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The system memory in use.
        Note that the system memory means the memory can be used by the software
        platform.

        For the distributed device, it represents the memory size on the master
        slot.

        If the amount of used memory exceeds 4,294,967,295 bytes,
        the value remains 4,294,967,295 bytes."
        ::= { hwLswSystemPara 15 }

    hwLswSysMemoryRatio OBJECT-TYPE
        SYNTAX Unsigned32 (0..100)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The percentage of system memory in use.
        Note that the system memory means the memory can be used by the software
        platform.

                                hwLswSysMemoryUsed
        hwLswSysMemoryRatio = --------------------
                                 hwLswSysMemory

        For the distributed device, it represents the memory used ratio on the
        master slot."
        ::= { hwLswSystemPara 16 }

    hwLswSysTemperature OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The temperature of system.

        For the distributed device, it represents the temperature on the
        master slot."
        ::= { hwLswSystemPara 17 }

-- ==================================================================
--
-- slot and port management group
--
-- ==================================================================

    hwLswSlotConf OBJECT IDENTIFIER ::= { hwLswDeviceAdmin 4 }

-- ==================================================================
--
-- Frame information table
--
-- ==================================================================

    hwLswFrameTable    OBJECT-TYPE
        SYNTAX     SEQUENCE OF HwLswFrameEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Frame information table."
        ::= {hwLswSlotConf 2}

    hwLswFrameEntry    OBJECT-TYPE
        SYNTAX     HwLswFrameEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Frame description table entry."
        INDEX { hwLswFrameIndex }
        ::= {hwLswFrameTable 1}

   HwLswFrameEntry ::= SEQUENCE
    {
        hwLswFrameIndex        Integer32,
        hwLswFrameType         Integer32,
        hwLswFrameDesc         DisplayString,
        hwLswSlotNumber        Integer32,
        hwLswFrameAdminStatus  INTEGER
    }

    hwLswFrameIndex    OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "The unique index of frame."
        ::= {hwLswFrameEntry 1}

    hwLswFrameType    OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Frame type."
        ::= {hwLswFrameEntry 2}

    hwLswFrameDesc    OBJECT-TYPE
        SYNTAX       DisplayString (SIZE(0..64))
        MAX-ACCESS     read-write
        STATUS     current
        DESCRIPTION
        "Frame description."
        ::= {hwLswFrameEntry 3}

    hwLswSlotNumber    OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Number of slots of the current frame."
        ::= {hwLswFrameEntry 4}

    hwLswFrameAdminStatus    OBJECT-TYPE
        SYNTAX     INTEGER
        {
              normal (1),
              fault  (2),
              other  (3)
        }
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "The Status of frame."
        ::= {hwLswFrameEntry 5}


-- ==================================================================
--
-- slot information table
--
-- ==================================================================

    hwLswSlotTable    OBJECT-TYPE
        SYNTAX     SEQUENCE OF HwLswSlotEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Slot description table."
        ::= {hwLswSlotConf 3}

    hwLswSlotEntry    OBJECT-TYPE
        SYNTAX     HwLswSlotEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Slot description table entry."
        INDEX { hwLswFrameIndex, hwLswSlotIndex }
        ::= {hwLswSlotTable 1}

   HwLswSlotEntry ::= SEQUENCE
    {
        hwLswSlotIndex                Integer32,
        hwLswSlotType                 HwLswTypeOfSlot,
        hwLswSlotDesc                 DisplayString,
        hwLswSlotCpuRatio             Integer32,
        hwLswSlotPcbVersion           DisplayString,
        hwLswSlotSoftwareVersion      DisplayString,
        hwLswSubslotNumber            Integer32,
        hwLswSlotAdminStatus          INTEGER,
        hwLswSlotOperStatus           INTEGER,
        hwLswSlotPhyMemory            Unsigned32,
        hwLswSlotMemory               Unsigned32,
        hwLswSlotMemoryUsed           Unsigned32,
        hwLswSlotMemoryRatio          Unsigned32,
        hwLswSlotTemperature          Integer32
   }

    hwLswSlotIndex    OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Slot index. When the slot is empty, listed as vacant slot."
        ::= {hwLswSlotEntry 1}

    hwLswSlotType    OBJECT-TYPE
        SYNTAX     HwLswTypeOfSlot
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Slot type. BOM number is recommended."
        ::= {hwLswSlotEntry 2}

    hwLswSlotDesc    OBJECT-TYPE
        SYNTAX     DisplayString(SIZE(0..64))
        MAX-ACCESS     read-write
        STATUS     current
        DESCRIPTION
        "Slot description."
        ::= {hwLswSlotEntry 3}

    hwLswSlotCpuRatio     OBJECT-TYPE
        SYNTAX         Integer32
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
        "CPU usage of the slot in accuracy of 1%, and the range of value is 1 to
         100."
        ::= {hwLswSlotEntry 4}

    hwLswSlotPcbVersion    OBJECT-TYPE
        SYNTAX       DisplayString (SIZE(0..64))
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "Hardware version of the board."
        ::= {hwLswSlotEntry 5}

    hwLswSlotSoftwareVersion    OBJECT-TYPE
        SYNTAX               DisplayString (SIZE(0..64))
        MAX-ACCESS           read-only
        STATUS               current
        DESCRIPTION
        "Software version of the board."
        ::= {hwLswSlotEntry 6}

    hwLswSubslotNumber    OBJECT-TYPE
        SYNTAX         Integer32
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Number of the cards of the board."
        ::= {hwLswSlotEntry 7}

    hwLswSlotAdminStatus    OBJECT-TYPE
        SYNTAX           INTEGER
        {
            not-install (1),
            normal      (2),
            fault       (3),
            forbidden   (4)
        }
        MAX-ACCESS       read-only
        STATUS           current
        DESCRIPTION
        "Slot status."
        ::= {hwLswSlotEntry 8}

    hwLswSlotOperStatus    OBJECT-TYPE
        SYNTAX          INTEGER
        {
            disable (1),
            enable  (2),
            reset   (3),
            test    (4)
        }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
        "Slot operation status."
        ::= {hwLswSlotEntry 9}

    hwLswSlotPhyMemory    OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "byte"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The memory of physical on the board.

        If the amount of physical memory exceeds 4,294,967,295 bytes,
        the value remains 4,294,967,295 bytes."
        ::= {hwLswSlotEntry 10}

    hwLswSlotMemory    OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "byte"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The memory of system on the board.

        Note that the system memory means the memory can be used by
        the software platform.

        If the amount of system memory exceeds 4,294,967,295 bytes,
        the value remains 4,294,967,295 bytes."
        ::= {hwLswSlotEntry 11}

    hwLswSlotMemoryUsed    OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "byte"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The system memory in use on the board.

        Note that the system memory means the memory can be used by
        the software platform.

        If the amount of used memory exceeds 4,294,967,295 bytes,
        the value remains 4,294,967,295 bytes."
        ::= {hwLswSlotEntry 12}

    hwLswSlotMemoryRatio    OBJECT-TYPE
        SYNTAX Unsigned32 (0..100)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The percentage of system memory in use on the board.

        Note that the system memory means the memory can be used by
        the software platform."
        ::= {hwLswSlotEntry 13}

    hwLswSlotTemperature    OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "The temperature of system on the board."
        ::= {hwLswSlotEntry 14}

-- ==================================================================
--
-- sub slot information table
--
-- ==================================================================

    hwLswSubslotTable    OBJECT-TYPE
        SYNTAX     SEQUENCE OF HwLswSubslotEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Subslot description table."
        ::= {hwLswSlotConf 4}

    hwLswSubslotEntry    OBJECT-TYPE
        SYNTAX     HwLswSubslotEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Subslot description table entry."
        INDEX {
            hwLswFrameIndex,
            hwLswSlotIndex,
            hwLswSubslotIndex
        }
        ::= {hwLswSubslotTable 1}

   HwLswSubslotEntry ::= SEQUENCE
    {
        hwLswSubslotIndex       Integer32,
        hwLswSubslotType        HwLswTypeOfSlot,
        hwLswSubslotPortNum     Integer32,
        hwLswSubslotAdminStatus INTEGER,
        hwLswSubslotFirstIfIndex Integer32
   }

   hwLswSubslotIndex      OBJECT-TYPE
        SYNTAX         Integer32
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
        "Subslot index."
        ::= {hwLswSubslotEntry 1}

-- value list of hwLswSubslotType are identical with the value list of hwLswSlotType.
    hwLswSubslotType      OBJECT-TYPE
        SYNTAX         HwLswTypeOfSlot
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
        "Type of the pinch board in the subslot."
        ::= {hwLswSubslotEntry 2}

    hwLswSubslotPortNum   OBJECT-TYPE
        SYNTAX         Integer32
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
        "Number of physical ports in the pinch board."
        ::= {hwLswSubslotEntry 3}


    hwLswSubslotAdminStatus    OBJECT-TYPE
        SYNTAX              INTEGER
        {
            not-install (1),
            normal      (2),
            fault       (3),
            forbidden   (4)
        }
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
        "Status of the pinch board in the subslot."
        ::= {hwLswSubslotEntry 4}

    hwLswSubslotFirstIfIndex   OBJECT-TYPE
        SYNTAX         Integer32
        MAX-ACCESS     read-only
        STATUS         current
        DESCRIPTION
        "The value of ifIndex of the first physical port in the pinch board."
        ::= {hwLswSubslotEntry 5}
-- ==================================================================
--
-- port information table
--
-- ==================================================================

    hwLswPortTable    OBJECT-TYPE
        SYNTAX     SEQUENCE OF HwLswPortEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Port configuration table."
        ::= {hwLswSlotConf 5}

    hwLswPortEntry    OBJECT-TYPE
        SYNTAX     HwLswPortEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Port configuration table entry."
        INDEX {
            hwLswFrameIndex,
            hwLswSlotIndex,
            hwLswSubslotIndex,
            hwLswPortIndex
        }
        ::= {hwLswPortTable 1}

    HwLswPortEntry ::= SEQUENCE
    {
        hwLswPortIndex             Integer32,
        hwLswPortType              INTEGER,
        hwLswPortIfindex           Integer32,
        hwLswPortIsPlugged         INTEGER
     }

    hwLswPortIndex    OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "The port number on the device. The first port number is 1, which is
         reserved if the port does not exist."
        ::= {hwLswPortEntry 1}

    hwLswPortType   OBJECT-TYPE
        SYNTAX     INTEGER
        {
            type-NULL(0),           -- NULL
            type-10OR100M(1),           -- 10BASE-T or 100BASE-TX  Electrical Interface
            type-1000BASE-LX-SM(2),     -- 1000BASE-LX Single Mode Fiber Optic Transceivers IR
            type-1000BASE-SX-MM(3),     -- 1000BASE-SX Multi Mode Fiber Optic Transceivers SR
            type-1000BASE-TX(4),        -- 1000BASE-T Electrical Interface
            type-100M-SINGLEMODE-FX(5),     -- 100BASE-FX Single Mode Fiber Optic Transceivers
            type-100M-MULTIMODE-FX(6),      -- 100BASE-FX Multi Mode Fiber Optic Transceivers
            type-100M-100BASE-TX(7),        -- 100BASE-TX Electrical Interface
            type-100M-HUB(8),           -- 100M HUB
            type-VDSL(9),           -- Very High Speed DSL
            type-STACK(10),         -- Gigabit STACK
            type-1000BASE-ZENITH-FX(11),    -- 1000BASE-LX Single Mode Fiber Optic Transceivers VLR
            type-1000BASE-LONG-FX(12),      -- 1000BASE-LX Single Mode Fiber Optic Transceivers LR
            type-ADSL(13),          -- Asymmetric Digital Subscriber Line
            type-10OR100M-db(14),       -- 10/100M ethernet electric port,each RJ-45 has 2 ethernet ports
            type-10GBASE-LR-SM(15),     -- 10GBASE-LR  Single Mode Fiber Optic Transceivers
            type-10GBASE-LX4-MM(16),        -- 10GBASE-LX4 Multi Mode Fiber Optic Transceivers
            type-10GBASE-LX4-SM(17),        -- 10GBASE-LX4 Single Mode Fiber Optic Transceivers
            type-100M-LONG-FX(18),      -- 100BASE-FX Single Mode Fiber Optic Transceivers LR SC
            type-1000BASE-CX(19),       -- 1000BASE-CX
            type-1000BASE-ZENITH-FX-LC(20), -- 1000BASE-LX Single Mode Fiber Optic Transceivers VLR with LC Connector
            type-1000BASE-LONG-FX-LC(21),   -- 1000BASE-LX Single Mode Fiber Optic Transceivers LR with LC Connector
            type-100M-SM-FX-SC(22),     -- 100BASE-FX Single Mode Fiber Optic Transceivers with SC Connector
            type-100M-MM-FX-SC(23),     -- 100BASE-FX Multi Mode Fiber Optic Transceivers with SC Connector
            type-100M-SM-FX-LC(24),     -- 100BASE-FX Single Mode Fiber Optic Transceivers with LC Connector
            type-100M-MM-FX-LC(25),     -- 100BASE-FX Multi Mode Fiber Optic Transceivers with LC Connector
            type-GBIC-NO-CONNECTOR(26),     --
            type-GBIC-1000-BASE-T(27),      --
            type-GBIC-1000-BASE-LX(28),     --
            type-GBIC-1000-BASE-SX(29),     --
            type-GBIC-1000-BASE-ZX(30),     --
            type-COMBO-NO-CONNECTOR(31),    --
            type-COMBO-1000-BASE-LX(32),    --
            type-COMBO-1000-BASE-LX-FIBER(33),  --
            type-COMBO-1000-BASE-LX-COPPER(34), --
            type-COMBO-1000-BASE-SX(35),    --
            type-COMBO-1000-BASE-SX-FIBER(36),  --
            type-COMBO-1000-BASE-SX-COPPER(37), --
            type-COMBO-1000-BASE-ZX(38),    --
            type-COMBO-1000-BASE-ZX-FIBER(39),  --
            type-COMBO-1000-BASE-ZX-COPPER(40), --
            type-155-POS-SX-MMF(41),        --
            type-155-POS-LX-SMF(42),        --
            type-1000BASE-T(43),        -- 1000 Base-T Port
            type-1000BASE-SX-SFP(44),       -- 1000 Base-SX SFP Port
            type-1000BASE-LX-SFP(45),       -- 1000 Base-SX SFP Port
            type-1000BASE-T-AN-SFP(46),     -- 1000 Base-T AN SFP Port
            type-10GBASE-LX4-XENPAK(47),    -- 10G Base-LX4 XENPAK Port
            type-10GBASE-LR-XENPAK(48),     -- 10G Base-LR XENPAK Port
            type-10GBASE-CX4(49),       -- 10G Base-CX4 Port
            type-1000BASE-ZX-SFP(50),           -- 1000 Base-ZX SFP Port
            type-1000BASE-MM-SFP(51),           -- 1000 Base-MM SFP Port
            type-100BASE-SX-SFP(52),            -- 100 Base-SX SFP Port
            type-100BASE-LX-SFP(53),            -- 100 Base-LX SFP Port
            type-100BASE-T-AN-SFP(54),          -- 100 Base-T SFP Port
            type-100BASE-ZX-SFP(55),            -- 100 Base-ZX SFP Port
            type-100BASE-MM-SFP(56),            -- 100 Base-MM SFP Port
            type-SFP-NO-CONNECTOR(57),          -- No Connector SFP Port
            type-SFP-UNKNOWN-CONNECTOR(58),     --  Unknown SFP Port
            type-POS-NO-CONNECTOR(59),          -- POS no connector
            type-10G-BASE-SR(60),               -- 10GBASE-SR Fiber Optic Transceivers with SC Connector
            type-10G-BASE-ER(61),               -- 10GBASE-ER Fiber Optic Transceivers with SC Connector
            type-10G-BASE-LX4(62),              -- 10GBASE-LX4 Fiber Optic Transceivers with SC Connector
            type-10G-BASE-SW(63),               -- 10GBASE-SW Fiber Optic Transceivers with SC Connector
            type-10G-BASE-LW(64),               -- 10GBASE-LW Fiber Optic Transceivers with SC Connector
            type-10G-BASE-EW(65),               -- 10GBASE-EW Fiber Optic Transceivers with SC Connector
            type-10G-LR-SM-LC(66),              -- 10GBASE-LR Single Mode Fiber Optic Transceivers with LC Connector
            type-10G-SR-MM-LC(67),              -- 10GBASE-SR Multi Mode Fiber Optic Transceivers with LC Connector
            type-10G-ER-SM-LC(68),              -- 10GBASE-ER Single Mode Fiber Optic Transceivers with LC Connector
            type-10G-LW-SM-LC(69),              -- 10GBASE-LW Single Mode Fiber Optic Transceivers with LC Connector
            type-10G-SW-MM-LC(70),              -- 10GBASE-SW Multi Mode Fiber Optic Transceivers with LC Connector
            type-10G-EW-SM-LC(71),              -- 10GBASE-EW Single Mode Fiber Optic Transceivers with LC Connector

            type-100BASE-SM-MTRJ(72),           -- 100 Base-SM MTRJ Port
            type-100BASE-MM-MTRJ(73),           -- 100 Base-MM MTRJ Port

            type-XFP-NO-CONNECTOR(74),          -- XFP without Transceiver
            type-XFP-10GBASE-SR(75),            -- 10GBASE-SR XFP Transceiver
            type-XFP-10GBASE-LR(76),            -- 10GBASE-LR XFP Transceiver
            type-XFP-10GBASE-ER(77),            -- 10GBASE-ER XFP Transceiver
            type-XFP-10GBASE-SW(78),            -- 10GBASE-SW XFP Transceiver
            type-XFP-10GBASE-LW(79),            -- 10GBASE-LW XFP Transceiver
            type-XFP-10GBASE-EW(80),            -- 10GBASE-EW XFP Transceiver
            type-XFP-10GBASE-CX4(81),           -- 10GBASE-CX4 XFP Transceiver
            type-XFP-10GBASE-LX4(82),           -- 10GBASE-LX4 XFP Transceiver
            type-XFP-UNKNOWN(83),               -- Unknown  XFP Transceiver

            type-XPK-NOCONNECTOR(84),           -- Xenpak without Transceiver
            type-XPK-10GBASE-SR(85),            -- 10GBASE-SR Xenpak Transceiver
            type-XPK-10GBASE-LR(86),            -- 10GBASE-LR Xenpak Transceiver
            type-XPK-10GBASE-ER(87),            -- 10GBASE-ER Xenpak Transceiver
            type-XPK-10GBASE-SW(88),            -- 10GBASE-SW Xenpak Transceiver
            type-XPK-10GBASE-LW(89),            -- 10GBASE-LW Xenpak Transceiver
            type-XPK-10GBASE-EW(90),            -- 10GBASE-EW Xenpak Transceiver
            type-XPK-10GBASE-CX4(91),           -- 10GBASE-CX4 Xenpak Transceiver
            type-XPK-10GBASE-LX4(92),           -- 10GBASE-LX4 Xenpak Transceiver
            type-XPK-UNKNOWN(93),               -- Unknown Xenpak Transceiver

            type-POS-OC48-SR-SM-LC(94),         -- OC48-SR Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC48-IR-SM-LC(95),         -- OC48-IR Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC48-LR-SM-LC(96),         -- OC48-LR Single Mode Fiber Optic Transceivers with LC Connector

            type-10G-BASE-CX4(97),              -- 10G BASE-CX4 Electrical Interface

            type-OLT-1000BASE-BX-SFF-SC(98),    -- 1000 BASE-BX SFF SC OLT Port
            type-ONU-1000BASE-BX-SFF-SC(99),    -- 1000 BASE-BX SFF SC ONU Port

            type-24G-CASCADE(100),              -- 24G Cascade port

            type-POS-OC3-SR-MM(101),            -- STM1/OC3 Short Reach Multi Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC3-IR-SM(102),            -- STM1/OC3 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC3-IR-1-SM(103),          -- STM1/OC3 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 1)
            type-POS-OC3-IR-2-SM(104),          -- STM1/OC3 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 2)
            type-POS-OC3-LR-SM(105),            -- STM1/OC3 Long Reach Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC3-LR-1-SM(106),          -- STM1/OC3 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 1)
            type-POS-OC3-LR-2-SM(107),          -- STM1/OC3 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 2)
            type-POS-OC3-LR-3-SM(108),          -- STM1/OC3 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 3)
            type-POS-OC12-SR-MM(109),           -- STM4/OC12 Short Reach Multi Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC12-IR-SM(110),           -- STM4/OC12 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC12-IR-1-SM(111),         -- STM4/OC12 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 1)
            type-POS-OC12-IR-2-SM(112),         -- STM4/OC12 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 2)
            type-POS-OC12-LR-SM(113),           -- STM4/OC12 Long Reach Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC12-LR-1-SM(114),         -- STM4/OC12 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 1)
            type-POS-OC12-LR-2-SM(115),         -- STM4/OC12 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 2)
            type-POS-OC12-LR-3-SM(116),         -- STM4/OC12 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 3)
            type-POS-OC48-SR-SM(117),           -- STM16/OC48 Short Reach Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC48-IR-SM(118),           -- STM16/OC48 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC48-IR-1-SM(119),         -- STM16/OC48 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 1)
            type-POS-OC48-IR-2-SM(120),         -- STM16/OC48 Intermediate Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 2)
            type-POS-OC48-LR-SM(121),           -- STM16/OC48 Long Reach Single Mode Fiber Optic Transceivers with LC Connector
            type-POS-OC48-LR-1-SM(122),         -- STM16/OC48 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 1)
            type-POS-OC48-LR-2-SM(123),         -- STM16/OC48 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 2)
            type-POS-OC48-LR-3-SM(124),         -- STM16/OC48 Long Reach Single Mode Fiber Optic Transceivers with LC Connector(variation 3)
            type-POS-I-64-1(125),               -- STM64/OC192 Interconnect Fiber Optic Transceivers with LC Connector(wavelength 1310nm G.652 fiber)
            type-POS-I-64-2(126),               -- STM64/OC192 Interconnect Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.652 fiber)
            type-POS-I-64-3(127),               -- STM64/OC192 Interconnect Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.653 fiber)
            type-POS-I-64-5(128),               -- STM64/OC192 Interconnect Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.655 fiber)
            type-POS-S-64-1(129),               -- STM64/OC192 Short Haul Fiber Optic Transceivers with LC Connector(wavelength 1310nm G.652 fiber)
            type-POS-S-64-2(130),               -- STM64/OC192 Short Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.652 fiber)
            type-POS-S-64-3(131),               -- STM64/OC192 Short Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.653 fiber)
            type-POS-S-64-5(132),               -- STM64/OC192 Short Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.655 fiber)
            type-POS-L-64-1(133),               -- STM64/OC192 Long Haul Fiber Optic Transceivers with LC Connector(wavelength 1310nm G.652 fiber)
            type-POS-L-64-2(134),               -- STM64/OC192 Long Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.652 fiber)
            type-POS-L-64-3(135),               -- STM64/OC192 Long Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.653 fiber)
            type-POS-V-64-2(136),               -- STM64/OC192 Very Long Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.652 fiber)
            type-POS-V-64-3(137),               -- STM64/OC192 Very Long Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.653 fiber)
            type-100BASE-FX-BIDI(138),          -- 100 BASE-FX BIDI Port
            type-100BASE-BX10-U-SFP(139),       -- 100 BASE-BX10-U-SFP Port
            type-100BASE-BX10-D-SFP(140),       -- 100 BASE-BX10-D-SFP Port
            type-1000BASE-BX10-U-SFP(141),      -- 1000 BASE-BX10-U-SFP Port
            type-1000BASE-BX10-D-SFP(142),      -- 1000 BASE-BX10-D-SFP Port
            type-STK-1000BASE-T(143),           -- 1000 BASE-T Stack Port
            type-RPR-PHYPOS-CONNECTOR(144),     -- Resilient Packet Ring POS physical port
            type-RPR-PHY10GE-CONNECTOR(145),    -- 10G Resilient Packet Ring physical port
            type-RPR-LOGICPOS-CONNECTOR(146),   -- Resilient Packet Ring POS logical port
            type-RPR-LOGIC10GE-CONNECTOR(147),  -- 10G Resilient Packet Ring logical port
            type-10GBASE-ZR(148),               -- Fiber Optic Transceivers with SC Connector, XENPAK
            type-TYPE-ERROR-CONNECTOR(149),     -- Error Optic Transceivers type
            type-10G-STACK(150),                -- 10G Stack Port
            type-155-ATM-SX-MMF(151),           -- ATM OC-3 Multi-mode Short Reach Optical Transceiver
            type-155-ATM-LX-SMF(152),           -- ATM OC-3 single mode long reach optical transceiver
            type-622-ATM-SX-MMF(153),           -- ATM OC-12 Multi-mode Short Reach Optical Transceiver
            type-622-ATM-LX-SMF(154),           -- ATM OC-12 Single Mode Long Reach Optical Transceiver
            type-155-ATM-NO-CONNECTOR(155),     -- ATM OC-3 No Connector
            type-622-ATM-NO-CONNECTOR(156),     -- ATM OC-12 No Connector
            type-155-CPOS-E1-NO-CONNECTOR(157), -- CPOS(E1) OC-3 No Connector
            type-155-CPOS-T1-NO-CONNECTOR(158), -- CPOS(T1) OC-3 No Connector
            type-622-CPOS-E1-NO-CONNECTOR(159), -- CPOS(E1) OC-12 No Connector
            type-622-CPOS-T1-NO-CONNECTOR(160), -- CPOS(T1) OC-12 No Connector
            type-155-CPOS-E1-SX-MMF(161),       -- CPOS(E1) OC-3 Multi-mode Short Reach Optical Transceiver
            type-155-CPOS-T1-SX-MMF(162),       -- CPOS(T1) OC-3 Multi-mode Short Reach Optical Transceiver
            type-155-CPOS-E1-LX-SMF(163),       -- CPOS(E1) OC-3 Single Mode Long Reach Optical Transceiver
            type-155-CPOS-T1-LX-SMF(164),       -- CPOS(T1) OC-3 Single Mode Long Reach Optical Transceiver
            type-622-CPOS-E1-SX-MMF(165),       -- CPOS(E1) OC-12 Multi-mode Short Reach Optical Transceiver
            type-622-CPOS-T1-SX-MMF(166),       -- CPOS(T1) OC-12 Multi-mode Short Reach Optical Transceiver
            type-622-CPOS-E1-LX-SMF(167),       -- CPOS(E1) OC-12 Single Mode Long Reach Optical Transceiver
            type-622-CPOS-T1-LX-SMF(168),       -- CPOS(T1) OC-12 Single Mode Long Reach Optical Transceiver
            type-E1-CONNECTOR(169),             -- E1 RJ45 Transceiver
            type-T1-CONNECTOR(170),             -- T1 RJ45 Transceiver
            type-1000BASE-STK-SFP(171),         -- 1-port 1000 Base-STK SFP Module
            type-1000BASE-BIDI-SFP(172),        -- 1-port 1000 Base-BIDI SFP Module
            type-1000BASE-CWDM-SFP(173),        -- 1-port 1000 Base-CWDM SFP Module
            type-100BASE-BIDI-SFP(174),         -- 1-port 100 Base-BIDI SFP Module
            type-OLT-1000BASE-PX-SFP(175),      -- 1000BASE-PX SFP OLT Interface
            type-OLT-1000BASE-NO-CONNECTOR(176), -- 1000BASE OLT No Connector
            type-RPR-PHYGE-CONNECTOR(177),      -- Resilient Packet Ring GE physical port
            type-RPR-LOGICGE-CONNECTOR(178),    -- Resilient Packet Ring GE logical port
            type-100M-1550-BIDI(179),           -- Single Port 100M Ethernet Bi-direction Optical Interface Module(TX1550nm, RX1310nm, 15km, SC)
            type-100M-1310-BIDI(180),           -- Single Port 100M Ethernet Bi-direction Optical reverse Interface Module(TX1310nm, RX1550nm, 15km, SC)
            type-RPR-PHYOC48-CONNECTOR(181),    -- Resilient Packet Ring OC48 physical port
            type-RPR-LOGICOC48-CONNECTOR(182),  -- Resilient Packet Ring OC48 logical port
            type-100-1000-BASE-LX-SMF(183),     -- 100BASE-LX/1000BASE-LX Single Mode Fiber Optic Transceivers
            type-10G-ZW-SM-LC(184),             -- 10GBASE-ZW Single Mode Fiber Optic Transceivers with LC Connector
            type-10G-ZR-SM-LC(185),             -- 10GBASE-ZR Single Mode Fiber Optic Transceivers with LC Connector
            type-XPK-10GBASE-ZR(186),           -- 10GBASE-ZR Xenpak Transceiver:LH80,SM1550
            type-SGMII-100-BASE-LX-SFP(187),    -- SGMII-100-BASE-LX-SFP Port
            type-SGMII-100-BASE-FX-SFP(188),    -- SGMII-100-BASE-FX-SFP Port
            type-WLAN-RADIO(189),               -- WLAN-RADIO Port
            type-SFP-PLUS-NO-CONNECTOR(191),    -- SFP+ without Transceiver
            type-SFP-PLUS-10GBASE-SR(192),      -- 10GBASE-SR SFP+ Transceiver
            type-SFP-PLUS-10GBASE-LR(193),      -- 10GBASE-LR SFP+ Transceiver
            type-SFP-PLUS-10GBASE-LRM(194),     -- 10GBASE-LRM SFP+ Transceiver
            type-SFP-PLUS-10GBASE-Cu(195),      -- 10GBASE-Cu SFP+ Transceiver
            type-SFP-PLUS-UNKNOWN(196),         -- Unknown SFP+ Transceiver
            type-SFP-PLUS-STACK-CONNECTOR(197), -- SFP+ STACK Transceiver
            type-POS-L-64-4(198),               -- STM64/OC192 Long Haul Fiber Optic Transceivers with LC Connector(wavelength 1550nm G.653 fiber)
            type-MINISAS-HD-STACK-CONNECTOR(199), -- MiniSAS HD STACK Transceiver
            type-ONU-1000BASE-PX-SFF(200),      -- 1000BASE-PX SFF ONU Interface
            type-RS485(201),                    -- RS485 Interface
            type-SFP-PLUS-10GBASE-ER(202),      -- 10GBASE-ER SFP+ Transceiver
            type-SFP-PLUS-10GBASE-ZR(203),      -- 10GBASE-ZR SFP+ Transceiver
            type-XFP-10GBASE-ZR(204)            -- 10GBASE-ZR XFP Transceiver
        }

        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Normally the port type is the same as its card type. When there are
         different types of ports in one card, use the actual port type."
        ::= {hwLswPortEntry 2}


     hwLswPortIfindex OBJECT-TYPE
        SYNTAX     Integer32
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "The value of ifIndex of the port."
        ::= {hwLswPortEntry 3}


     hwLswPortIsPlugged   OBJECT-TYPE
        SYNTAX     INTEGER
        {
            unplugged(0),
            plugged(1)
        }

        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Port is plugged or not."
        ::= {hwLswPortEntry 4}


-- ==================================================================
--
-- port loopback test table
--
-- ==================================================================

    hwLswPortLoopbackTable    OBJECT-TYPE
        SYNTAX     SEQUENCE OF HwLswPortLoopbackEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Port loopback test table."
        ::= {hwLswSlotConf 6}

    hwLswPortLoopbackEntry  OBJECT-TYPE
        SYNTAX     HwLswPortLoopbackEntry
        MAX-ACCESS     not-accessible
        STATUS     current
        DESCRIPTION
        "Port loopback test table entry."
      AUGMENTS    {hwLswPortEntry }
      ::= {hwLswPortLoopbackTable 1}

    HwLswPortLoopbackEntry ::= SEQUENCE
    {
        hwLswPortLoopbackIsSupport        INTEGER,
        hwLswPortLoopbackOperate          INTEGER,
        hwLswPortLoopbackResult           INTEGER,
        hwLswPortLoopbackAutoStopSupport  INTEGER,
        hwLswPortLoopbackRemoteResult     INTEGER,
        hwLswPortLoopbackLocalResult      INTEGER,
        hwLswPortLoopbackInternalResult   INTEGER,
        hwLswPortLoopbackExternalResult   INTEGER
     }

      hwLswPortLoopbackIsSupport  OBJECT-TYPE
        SYNTAX     INTEGER
        {
            neither(1),
            both(2),
            internalOnly(3),
            externalOnly(4)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "The loopback type can be supported by current port."
        ::= {hwLswPortLoopbackEntry 1}

    hwLswPortLoopbackOperate OBJECT-TYPE
        SYNTAX     INTEGER
        {
            stopRemoteOrLocalLoopBack(0),
            internalLoopback(1),
            externalLoopback(2),
            remoteLoopback(3),
            localLoopback(4)
        }
        MAX-ACCESS     read-write
        STATUS     current
        DESCRIPTION
        "Port loopback operate type. Read operation not supported."
        ::= {hwLswPortLoopbackEntry 2}

     hwLswPortLoopbackResult OBJECT-TYPE
        SYNTAX     INTEGER
        {
            testing (0),
            testok (1),
            testfailed (2)
        }
        MAX-ACCESS     read-only
        STATUS     current
        DESCRIPTION
        "Loopback test result of the port, used for checking if the test is successful.
         Only after the testing will the query value on the node make sense."
        ::= {hwLswPortLoopbackEntry 3}

      hwLswPortLoopbackAutoStopSupport  OBJECT-TYPE
        SYNTAX     INTEGER
        {
            support(1),
            notSupport(2)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "Whether this port support NEED-MANNUL-NOLOOP mode or not."
        ::= {hwLswPortLoopbackEntry 4}

     hwLswPortLoopbackRemoteResult OBJECT-TYPE
        SYNTAX     INTEGER
        {
            loopbackTestInit(0),
            loopbackTesting(1),
            loopbackTestSuccessed (2),
            loopbackTestFailed (3),
            loopbackTestTestAndFailed (4)
        }
        MAX-ACCESS     read-write
        STATUS     current
        DESCRIPTION
        "The remote loopback test result of the port, used for checking if the
         test is successful. Only after the testing will the query value on
         the node make sense."
        ::= {hwLswPortLoopbackEntry 5}

     hwLswPortLoopbackLocalResult OBJECT-TYPE
        SYNTAX     INTEGER
        {
            loopbackTestInit(0),
            loopbackTesting(1),
            loopbackTestSuccessed (2),
            loopbackTestFailed (3),
            loopbackTestTestAndFailed (4)
        }
        MAX-ACCESS     read-write
        STATUS     current
        DESCRIPTION
        "The local loopback test result of the port, used for checking if the
         test is successful. Only after the testing will the query value on the
         node make sense."
        ::= {hwLswPortLoopbackEntry 6}

     hwLswPortLoopbackInternalResult OBJECT-TYPE
        SYNTAX     INTEGER
        {
            loopbackTestInit(0),
            loopbackTesting(1),
            loopbackTestSuccessed (2),
            loopbackTestFailed (3),
            loopbackTestTestAndFailed (4)
        }
        MAX-ACCESS     read-write
        STATUS     current
        DESCRIPTION
        "The internal loopback test result of the port, used for checking if
         the test is successful. Only after the testing will the query value
         on the node make sense."
        ::= {hwLswPortLoopbackEntry 7}

     hwLswPortLoopbackExternalResult OBJECT-TYPE
        SYNTAX     INTEGER
        {
            loopbackTestInit(0),
            loopbackTesting(1),
            loopbackTestSuccessed (2),
            loopbackTestFailed (3),
            loopbackTestTestAndFailed (4)
        }
        MAX-ACCESS     read-write
        STATUS     current
        DESCRIPTION
        "The external loopback test result of the port, used for checking if the
         test is successful. Only after the testing will the query value on the
         node make sense."
        ::= {hwLswPortLoopbackEntry 8}

-- ==================================================================
-- Fabric table
-- ==================================================================
    hwLswFabricTable  OBJECT-TYPE
        SYNTAX          SEQUENCE OF HwLswFabricEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "This table contains the information of fabric."
        ::= {hwLswSlotConf 7}

    hwLswFabricEntry  OBJECT-TYPE
        SYNTAX          HwLswFabricEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "An entry in hwLswFabricTable."
        INDEX           {
                            hwLswFrameIndex,
                            hwLswSlotIndex,
                            hwLswSubslotIndex,
                            hwLswFabricChannelIndex
                        }
        ::= {hwLswFabricTable 1}

    HwLswFabricEntry ::= SEQUENCE {
        hwLswFabricChannelIndex   Integer32,
        hwLswFabricUtilIn         Integer32,
        hwLswFabricUtilOut        Integer32,
        hwLswFabricPeakIn         Integer32,
        hwLswFabricPeakInTime     DateAndTime,
        hwLswFabricPeakOut        Integer32,
        hwLswFabricPeakOutTime    DateAndTime
     }

    hwLswFabricChannelIndex   OBJECT-TYPE
        SYNTAX          Integer32
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
        "The channel number of fabric."
        ::= {hwLswFabricEntry 1}

    hwLswFabricUtilIn    OBJECT-TYPE
        SYNTAX          Integer32 (0..100)
        UNITS           "one percent"
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "Ingress utilization of fabric."
        ::= {hwLswFabricEntry 2}

    hwLswFabricUtilOut    OBJECT-TYPE
        SYNTAX          Integer32 (0..100)
        UNITS           "one percent"
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "Egress utilization of fabric."
        ::= {hwLswFabricEntry 3}

    hwLswFabricPeakIn     OBJECT-TYPE
        SYNTAX          Integer32 (0..100)
        UNITS           "one percent"
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "Ingress peak of utilization for fabric."
        ::= {hwLswFabricEntry 4}

    hwLswFabricPeakInTime OBJECT-TYPE
        SYNTAX          DateAndTime
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "Ingress peak time of utilization for fabric."
        ::= {hwLswFabricEntry 5}

    hwLswFabricPeakOut    OBJECT-TYPE
        SYNTAX          Integer32 (0..100)
        UNITS           "one percent"
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "Egress peak of utilization for fabric."
        ::= {hwLswFabricEntry 6}

    hwLswFabricPeakOutTime    OBJECT-TYPE
        SYNTAX          DateAndTime
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "Egress peak time of utilization for fabric."
        ::= {hwLswFabricEntry 7}

END
