-- *****************************************************************
-- CISCO-DHCP-SNOOPING-MIB
--   
-- March 2004, Edward Pham
--   
-- Copyright (c) 2004-2007, 2009-2010 by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-DHCP-SNOOPING-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    Counter32,
    Counter64,
    NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TruthValue,
    MacAddress,
    RowStatus
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    ifIndex,
    ifName,
    InterfaceIndex
        FROM IF-MIB
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    VlanIndex
        FROM Q-BRIDGE-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoDhcpSnoopingMIB MODULE-IDENTITY
    LAST-UPDATED    "200908260000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA 95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The MIB module is for configuration of DHCP Snooping
        feature. DHCP Snooping is a security mechanism which
        uses information gleaned from DHCP packets to provide
        per-interface security capabilities."
    REVISION        "200908260000Z"
    DESCRIPTION
        "Add cdsVlanOperStatusGroup."
    REVISION        "200908100000Z"
    DESCRIPTION
        "Add new enum 'strictIpMac' to cdsIfSrcGuardFilterType
         object."
    REVISION        "200904120000Z"
    DESCRIPTION
        "Add cdsIfVlanRelayInfoOptCircuitIdDirect."
    REVISION        "200711130000Z"
    DESCRIPTION
        "Add cdsNotifControlGroup and cdsBindingsNotificationGroup."
    REVISION        "200707120000Z"
    DESCRIPTION
        "Add cdsIfVlanRelayInfoOptCircuitIdGroup,
        cdsStatisticsExtGroup 
        and deprecate cdsRelayAgentRemoteIdGroup with 
        cdsRelayAgentInfoOptRemoteIdSubGroup."
    REVISION        "200705300000Z"
    DESCRIPTION
        "Add cdsBindingsHostnameGroup"
    REVISION        "200603161600Z"
    DESCRIPTION
        "Add cdsBindingsLimitGroup,
        cdsStaticBindingsGroup,
        cdsIfSrcGuardIpFilterGroup,
        cdsIfSrcGuardTrafficFilterGroup,
        cdsIfSrcGuardExtGroup 
        and deprecate cdsIfSrcGuardGroup with cdsIfSrcGuardGroupRev1."
    REVISION        "200510260000Z"
    DESCRIPTION
        "Add cdsIfFeatureConfigGroup."
    REVISION        "200403040000Z"
    DESCRIPTION
        "Initial revision of this MIB module."
    ::= { ciscoMgmt 380 }


ciscoDhcpSnoopingMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIB 0 }

ciscoDhcpSnoopingMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIB 1 }

ciscoDhcpSnoopingMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIB 2 }

cdsGlobal  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBObjects 1 }

cdsVlan  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBObjects 2 }

cdsInterface  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBObjects 3 }

cdsBindings  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBObjects 4 }

cdsStatistics  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBObjects 5 }

cdsSrcGuard  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBObjects 6 }


-- The Global group

cdsFeatureEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates whether the DHCP Snooping feature is
        enabled at the device level.

        Setting this object to 'false' disables the DHCP Snooping 
        feature globally thus disabling the feature at each VLAN.

        Setting this object to 'true' will start the DHCP Snooping 
        feature running in the device. Once the DHCP Snooping is 
        enabled, whether the feature is running at each VLAN is 
        controlled by the cdsVlanConfigTable." 
    ::= { cdsGlobal 1 }

cdsDatabaseFile OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the name of the database file used
        to store DHCP bindings information." 
    ::= { cdsGlobal 2 }

cdsDatabaseUpdateInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the time interval at which DHCP
        bindings information will be written to the database file
        denoted by cdsDatabaseFile object. Setting this object
        to zero will disable the storage of DHCP bindings." 
    ::= { cdsGlobal 3 }

cdsRelayAgentInfoOptEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates if the DHCP relay agent information
        option (option 82) will be inserted to DHCP packets by
        DHCP Snooping feature.

        If this object is set to 'true', DHCP option 82 data will
        be inserted to DHCP packets.

        If this object is set to 'false', DHCP option 82 data
        will not be inserted."
    REFERENCE       "RFC 3046, DHCP Relay Agent Information Option." 
    ::= { cdsGlobal 4 }

cdsRelayAgentInfoOptRemoteId OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "This object indicates the Remote ID used as part of the
        DHCP relay information option (option 82) data inserted
        to DHCP packets by DHCP Snooping feature. 

        The value of this object is ignored whenever the value
        of cdsRelayAgentInfoOptEnable object is 'false'.
        This object is deprecated and superceded by
        cdsRelayAgentInfoOptRemoteIdSub object."
    REFERENCE       "RFC 3046, DHCP Relay Agent Information Option." 
    ::= { cdsGlobal 5 }

cdsMatchMacAddressEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates if DHCP Snooping Mac address
        matching is enabled. 

        If this object is set to 'true', DHCP Snooping Mac
        address matching is enabled.

        If this object is set to 'false', DHCP Snooping Mac
        address matching is disabled." 
    ::= { cdsGlobal 6 }

cdsGlobalMaxBindingsLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum number of DHCP
        bindings allowed in the device." 
    ::= { cdsGlobal 7 }

cdsRelayAgentInfoOptRemoteIdSub OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the Remote ID used in Agent Remote ID
        sub-option of the DHCP relay information option (option 82) 
        data inserted to DHCP packets by DHCP Snooping feature. 

        The value of this object is in a format of a user-defined 
        string. Its default value is the device's MAC address.

        The value of this object is ignored whenever the value
        of cdsRelayAgentInfoOptEnable object is 'false'."
    REFERENCE       "RFC 3046, DHCP Relay Agent Information Option." 
    ::= { cdsGlobal 8 }

cdsBindingsNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether cdsBindingsNotification
        is generated by the system.

        Setting this object value to 'true' will enable
        generation of cdsBindingsNotification.

        Seting this object value to 'false' will disable
        generation of cdsBindingsNotification." 
    ::= { cdsGlobal 9 }
-- The DHCP Snooping Vlan Group
--   

--   
-- The DHCP Snooping VLAN Config Table

cdsVlanConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsVlanConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the mechanism to control DHCP Snooping
        per VLAN. When a VLAN is created in a device supporting this
        table, a corresponding entry of this table will be added."
    ::= { cdsVlan 1 }

cdsVlanConfigEntry OBJECT-TYPE
    SYNTAX          CdsVlanConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the configuration to enable
        or disable DHCP Snooping at each existing VLAN."
    INDEX           { cdsVlanIndex } 
    ::= { cdsVlanConfigTable 1 }

CdsVlanConfigEntry ::= SEQUENCE {
        cdsVlanIndex                  VlanIndex,
        cdsVlanDhcpSnoopingEnable     TruthValue,
        cdsVlanDhcpSnoopingOperStatus INTEGER 
}

cdsVlanIndex OBJECT-TYPE
    SYNTAX          VlanIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the VLAN number on which DHCP Snooping
        feature is configured." 
    ::= { cdsVlanConfigEntry 1 }

cdsVlanDhcpSnoopingEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates whether DHCP Snooping is enabled in
        this VLAN. 

        If this object is set to 'true', DHCP Snooping is enabled. 

        If this object is set to 'false', DHCP Snooping is disabled." 
    ::= { cdsVlanConfigEntry 2 }
 
cdsVlanDhcpSnoopingOperStatus OBJECT-TYPE
    SYNTAX          INTEGER { operational(1), notOperational(2) } 
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates whether DHCP Snooping is operational in
        this VLAN. 

        If this object is 'operational', DHCP Snooping is running. 

        If this object is 'notOperational', DHCP Snooping is not running." 
    ::= { cdsVlanConfigEntry 3 }
 

-- The DHCP Snooping Interface Group
--   

--   
-- The DHCP Snooping Interface Config Table

cdsIfConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsIfConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the mechanism to configure the trust
        state for DHCP Snooping purpose at each interface
        capable of this feature. Some of the interfaces
        (but not limited to) for which this feature might be
        applicable are: ifType = ethernetCsmacd(6)."
    ::= { cdsInterface 1 }

cdsIfConfigEntry OBJECT-TYPE
    SYNTAX          CdsIfConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the configuration to enable
        or disable trust state for DHCP Snooping at each 
        interface capable of this feature."
    INDEX           { ifIndex } 
    ::= { cdsIfConfigTable 1 }

CdsIfConfigEntry ::= SEQUENCE {
        cdsIfTrustEnable TruthValue
}

cdsIfTrustEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates whether the interface is trusted for
        DHCP Snooping purpose. 

        If this object is set to 'true', the interface is trusted.
        DHCP packets coming to this interface will be forwarded
        without checking.

        If this object is set to 'false', the interface is not
        trusted. DHCP packets coming to this interface will be
        subjected to DHCP checks." 
    ::= { cdsIfConfigEntry 1 }
 

-- The DHCP Snooping Rate Limit Interface Config Table

cdsIfRateLimitTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsIfRateLimitEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the mechanism to configure the rate limit
        for DHCP Snooping purpose at each interface capable
        of this feature. Some of the interfaces (but not limited to)
        for which this feature might be applicable are:
        ifType = ethernetCsmacd(6)."
    ::= { cdsInterface 2 }

cdsIfRateLimitEntry OBJECT-TYPE
    SYNTAX          CdsIfRateLimitEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the configuration of rate limit
        DHCP Snooping at each interface capable of this
        feature."
    INDEX           { ifIndex } 
    ::= { cdsIfRateLimitTable 1 }

CdsIfRateLimitEntry ::= SEQUENCE {
        cdsIfRateLimit Unsigned32
}

cdsIfRateLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "packets per second"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates rate limit value for DHCP Snooping
        purpose. If the value of this object is 0, no rate limit is
        applied for DHCP traffic at this interface." 
    ::= { cdsIfRateLimitEntry 1 }
 

-- The DHCP Snooping Interface Feature Enable Table

cdsIfFeatureConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsIfFeatureConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the mechanism to enable or disable
        DHCP Snooping feature at each interface capable of this
        feature. Some of the interfaces (but not limited to) for
        which this configuration might be applicable are: 
        ifType = ethernetCsmacd(6)."
    ::= { cdsInterface 3 }

cdsIfFeatureConfigEntry OBJECT-TYPE
    SYNTAX          CdsIfFeatureConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the configuration to enable
        or disable DHCP Snooping at each interface capable of this
        feature."
    INDEX           { ifIndex } 
    ::= { cdsIfFeatureConfigTable 1 }

CdsIfFeatureConfigEntry ::= SEQUENCE {
        cdsIfFeatureEnable TruthValue
}

cdsIfFeatureEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates whether the  DHCP Snooping feature
        is enabled at this interface. 

        If this object is set to 'true', DHCP Snooping is enabled. 

        If this object is set to 'false', DHCP Snooping is disabled." 
    ::= { cdsIfFeatureConfigEntry 1 }
 

-- The DHCP Bindings limit table

cdsIfBindingsLimitTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsIfBindingsLimitEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the mechanism to configure the binding limit
        for DHCP Snooping purpose at each interface capable of
        this feature. Some of the interfaces (but not limited to)
        for which this feature might be applicable are:
        ifType = ethernetCsmacd(6)."
    ::= { cdsInterface 4 }

cdsIfBindingsLimitEntry OBJECT-TYPE
    SYNTAX          CdsIfBindingsLimitEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the configuration of binding limit at
        each interface capable of this feature."
    INDEX           { ifIndex } 
    ::= { cdsIfBindingsLimitTable 1 }

CdsIfBindingsLimitEntry ::= SEQUENCE {
        cdsIfBindingsLimit Unsigned32
}

cdsIfBindingsLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum number of DHCP bindings
        allowed on this interface. This objects value will limit
        the number of entries in cdsBindingsTable and 
        cdsStaticBindingsTable. The sum of all instances' value of
        cdsIfBindingsLimit in this table should be less than or equal
        to the object value of cdsGlobalMaxBindingsLimit." 
    ::= { cdsIfBindingsLimitEntry 1 }
 

-- DHCP Snooping Option 82 circuit-id table

cdsIfVlanRelayInfoOptCircuitIdTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsIfVlanRelayInfoOptCircuitIdEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represent circuit-id information,
        configured on per port per vlan."
    ::= { cdsInterface 5 }

cdsIfVlanRelayInfoOptCircuitIdEntry OBJECT-TYPE
    SYNTAX          CdsIfVlanRelayInfoOptCircuitIdEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Entry contains circuit-id information for a particular interface
        and VLAN."
    INDEX           {
                        ifIndex,
                        cdsIfVlan
                    } 
    ::= { cdsIfVlanRelayInfoOptCircuitIdTable 1 }

CdsIfVlanRelayInfoOptCircuitIdEntry ::= SEQUENCE {
        cdsIfVlan                            VlanIndex,
        cdsIfVlanRelayInfoOptCircuitId       OCTET STRING,
        cdsIfVlanRelayInfoOptCircuitIdStatus RowStatus,
        cdsIfVlanRelayInfoOptCircuitIdDirect TruthValue
}

cdsIfVlan OBJECT-TYPE
    SYNTAX          VlanIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the VLAN on which circuit-id is
        configured." 
    ::= { cdsIfVlanRelayInfoOptCircuitIdEntry 1 }

cdsIfVlanRelayInfoOptCircuitId OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..64))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies circuit-id used in Agent Circuit ID
        sub-option of the DHCP relay information option (option 82) 
        data inserted to DHCP packets by DHCP Snooping feature. 

        The value of this object is in a format of a user-defined
        string. 

        The value of this object is ignored whenever the value
        of cdsRelayAgentInfoOptEnable object is 'false'."
    REFERENCE       "RFC 3046, DHCP Relay Agent Information Option." 
    ::= { cdsIfVlanRelayInfoOptCircuitIdEntry 2 }

cdsIfVlanRelayInfoOptCircuitIdStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to manage the creation and deletion
        of rows in this table. It only supports 'active(1)', 
        'destroy(6)' and 'createAndGo(4)' value. 

        Entry in this table gets created by setting
        cdsIfVlanRelayInfoOptCircuitIdStatus object to 'createAndGo'.
        Entry in this table gets deleted by setting 
        cdsIfVlanRelayInfoOptCircuitIdStatus object to 'destroy' 

        Value of cdsIfRelayInfoOptCircuitId object can be
        modified when the value of this RowStatus object is
        'active'." 
    ::= { cdsIfVlanRelayInfoOptCircuitIdEntry 3 }

cdsIfVlanRelayInfoOptCircuitIdDirect OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies to ignore the length and type in
        Agent Circuit ID sub-option of the DHCP relay information 
        option (option 82) data inserted to DHCP packets by 
        DHCP Snooping feature.

        The value of this object is ignored whenever the value
        of cdsRelayAgentInfoOptEnable object is 'false'." 
    ::= { cdsIfVlanRelayInfoOptCircuitIdEntry 4 }
 

-- The DHCP Bindings group

cdsBindingsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsBindingsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the DHCP bindings information learnt by
        the device."
    ::= { cdsBindings 1 }

cdsBindingsEntry OBJECT-TYPE
    SYNTAX          CdsBindingsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the Mac address, IP address type,
        IP address, VLAN number, interface number, leased time, and
        status of this instance."
    INDEX           {
                        cdsBindingsVlan,
                        cdsBindingsMacAddress
                    } 
    ::= { cdsBindingsTable 1 }

CdsBindingsEntry ::= SEQUENCE {
        cdsBindingsVlan       VlanIndex,
        cdsBindingsMacAddress MacAddress,
        cdsBindingsAddrType   InetAddressType,
        cdsBindingsIpAddress  InetAddress,
        cdsBindingsInterface  InterfaceIndex,
        cdsBindingsLeasedTime Unsigned32,
        cdsBindingsStatus     RowStatus,
        cdsBindingsHostname   SnmpAdminString
}

cdsBindingsVlan OBJECT-TYPE
    SYNTAX          VlanIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the VLAN to which a DHCP client host
        belongs." 
    ::= { cdsBindingsEntry 1 }

cdsBindingsMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the MAC address of a DHCP client
        host." 
    ::= { cdsBindingsEntry 2 }

cdsBindingsAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of IP address denoted
        in cdsBindingsIpAddress object." 
    ::= { cdsBindingsEntry 3 }

cdsBindingsIpAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the allocated IP address of
        a DHCP client host." 
    ::= { cdsBindingsEntry 4 }

cdsBindingsInterface OBJECT-TYPE
    SYNTAX          InterfaceIndex
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the interface where a DHCP client
        host connects to." 
    ::= { cdsBindingsEntry 5 }

cdsBindingsLeasedTime OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the leased time of this DHCP
        bindings." 
    ::= { cdsBindingsEntry 6 }

cdsBindingsStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to manage the deletion of rows
        in this table. This object only supports active(1) and
        destroy(6) value. 

        Whenever a DHCP binding is learnt by the device, an
        entry will be created by the device in this table with
        its RowStatus object set to active(1). Setting this
        object value to destroy(6) will clear the DHCP bindings
        information represented by this row instance." 
    ::= { cdsBindingsEntry 7 }

cdsBindingsHostname OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the host name of the DHCP client
        as denoted by DHCP option 12 field. An empty string
        indicates absence of option 12 in DHCP packet." 
    ::= { cdsBindingsEntry 8 }
 

-- The static bindings table

cdsStaticBindingsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsStaticBindingsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the DHCP bindings information configured
        by (local or network) management."
    ::= { cdsBindings 2 }

cdsStaticBindingsEntry OBJECT-TYPE
    SYNTAX          CdsStaticBindingsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the Mac address, IP address type,
        IP address, VLAN number, interface number, and status of
        this instance."
    INDEX           {
                        cdsStaticBindingsVlan,
                        cdsStaticBindingsMacAddress
                    } 
    ::= { cdsStaticBindingsTable 1 }

CdsStaticBindingsEntry ::= SEQUENCE {
        cdsStaticBindingsVlan       VlanIndex,
        cdsStaticBindingsMacAddress MacAddress,
        cdsStaticBindingsAddrType   InetAddressType,
        cdsStaticBindingsIpAddress  InetAddress,
        cdsStaticBindingsInterface  InterfaceIndex,
        cdsStaticBindingsStatus     RowStatus
}

cdsStaticBindingsVlan OBJECT-TYPE
    SYNTAX          VlanIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the VLAN to which a DHCP client host
        belongs." 
    ::= { cdsStaticBindingsEntry 1 }

cdsStaticBindingsMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the MAC address of a DHCP client
        host." 
    ::= { cdsStaticBindingsEntry 2 }

cdsStaticBindingsAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the type of IP address denoted
        in cdsStaticBindingsIpAddress object." 
    ::= { cdsStaticBindingsEntry 3 }

cdsStaticBindingsIpAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the allocated IP address of
        a DHCP client host." 
    ::= { cdsStaticBindingsEntry 4 }

cdsStaticBindingsInterface OBJECT-TYPE
    SYNTAX          InterfaceIndex
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the ifIndex value of the interface
        where a DHCP client host connects to." 
    ::= { cdsStaticBindingsEntry 5 }

cdsStaticBindingsStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to manage the creation and deletion
        of rows in this table. An entry can be created by setting
        the instance value of this object to 'createAndGo', and
        deleted by setting the instance value of this object to
        'destroy'. The value of cdsStaticBindingsAddrType,
        cdsStaticBindingsIpAddress, cdsStaticBindingsInterface 
        object can be modified when the value of this RowStatus
        object is 'active'." 
    ::= { cdsStaticBindingsEntry 6 }
 


-- The DHCP Snooping Statistics group

cdsTotalForwardedPkts OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the total number of packets subjected to
        DHCP Snooping is forwarded." 
    ::= { cdsStatistics 1 }

cdsTotalDroppedPkts OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the total number of packets subjected to
        DHCP Snooping is dropped." 
    ::= { cdsStatistics 2 }

cdsUntrustedPortDroppedPkts OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the number of packets subjected to DHCP Snooping
        is dropped because they come from untrusted interface." 
    ::= { cdsStatistics 3 }

cdsForwardedWithoutOption82Pkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the number of packets subjected to DHCP Snooping
        is forwarded without insertion of DHCP relay agent information
        option (option 82) data." 
    ::= { cdsStatistics 4 }
-- The IP Source Guard Group

cdsIfSrcGuardConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsIfSrcGuardConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the mechanism to enable or disable
        IP Source Guard at each physical interface capable of
        this feature. Some of the interfaces (but not limited to)
        for which this feature might be applicable are:
        ifType = ethernetCsmacd(6).

        When DHCP Snooping is enabled at an interface, a list of
        IP addresses is obtained through DHCP Snooping for this
        particular interface. If IP Source Guard is enabled, only
        traffic from these IP addresses is allowed to pass through
        the interface."
    ::= { cdsSrcGuard 1 }

cdsIfSrcGuardConfigEntry OBJECT-TYPE
    SYNTAX          CdsIfSrcGuardConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the configuration to enable
        or disable IP Source Guard as well as the configuration
        of the filter type at each physical interface capable
        of IP Source Guard feature."
    INDEX           { ifIndex } 
    ::= { cdsIfSrcGuardConfigTable 1 }

CdsIfSrcGuardConfigEntry ::= SEQUENCE {
        cdsIfSrcGuardEnable     TruthValue,
        cdsIfSrcGuardFilterType INTEGER
}

cdsIfSrcGuardEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object indicates whether IP Source Guard is enabled
        at this interface. 

        If this object is set to 'true', IP Source Guard is
        enabled. Traffic coming to this interface will be forwarded
        if it is from the list of IP addresses obtained through
        DHCP Snooping. Otherwise, it is denied.

        If this object is set to 'false', IP Source Guard is
        disabled.

        This object is deprecated and superceded by
        cdsIfSrcGuardFilterType object." 
    ::= { cdsIfSrcGuardConfigEntry 1 }

cdsIfSrcGuardFilterType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        ip(2),
                        ipMac(3),
                        strictIpMac(4)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the traffic filter type applied
        at this interface.

        'disable' indicates that Source Guard feature is disabled.

        'ip' indicates that Source Guard feature is enabled and 
        only applied to IP traffic.

        'ipMac' indicates that Source Guard feature is enabled and
        applied to both IP and MAC traffic.

        'strictIpMac' indicates that Source Guard feature is
        enabled and applied to IP traffic. IP traffic originating
        from a DHCP client will subject to validation of
        client IP address, MAC address, VLAN and interface where
        the DHCP client is connected."
    ::= { cdsIfSrcGuardConfigEntry 2 }
 

-- cdsIfSrcGuardAddrTable

cdsIfSrcGuardAddrTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CdsIfSrcGuardAddrEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides the information on IP addresses used
        for IP Source Guard purpose at each physical interface
        capable of this feature. Some of the interfaces
        (but not limited to) for which this feature might be
        applicable are: ifType = ethernetCsmacd(6)."
    ::= { cdsSrcGuard 2 }

cdsIfSrcGuardAddrEntry OBJECT-TYPE
    SYNTAX          CdsIfSrcGuardAddrEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A row instance contains the IP address type and IP
        address used for IP Source Guard purpose at each
        physical interface capable of this feature."
    INDEX           {
                        ifIndex,
                        cdsIfSrcGuardIndex
                    } 
    ::= { cdsIfSrcGuardAddrTable 1 }

CdsIfSrcGuardAddrEntry ::= SEQUENCE {
        cdsIfSrcGuardIndex           Unsigned32,
        cdsIfSrcGuardAddrType        InetAddressType,
        cdsIfSrcGuardAddress         InetAddress,
        cdsIfSrcGuardIpFilterAction  INTEGER,
        cdsIfSrcGuardFilterMode      INTEGER,
        cdsIfSrcGuardMacAddress      MacAddress,
        cdsIfSrcGuardMacFilterAction INTEGER,
        cdsIfSrcGuardVlansLow        OCTET STRING,
        cdsIfSrcGuardVlansHigh       OCTET STRING
}

cdsIfSrcGuardIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the index of this entry." 
    ::= { cdsIfSrcGuardAddrEntry 1 }

cdsIfSrcGuardAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of IP address denoted
        in cdsIfSrcGuardAddress object." 
    ::= { cdsIfSrcGuardAddrEntry 2 }

cdsIfSrcGuardAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the IP address obtained at
        this interface through DHCP Snooping or statically
        configured." 
    ::= { cdsIfSrcGuardAddrEntry 3 }

cdsIfSrcGuardIpFilterAction OBJECT-TYPE
    SYNTAX          INTEGER  {
                        permitIpAddress(1),
                        denyAllIpAddress(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the IP Source Guard action
        applied at this interface with respect to IP traffic.

        permitIpAddress(1) indicates that IP traffic coming
        from the IP address denoted by cdsIfSrcGuardAddress
        object will be allowed to go through.

        denyAllIpAdress(2) indicates that all IP traffic
        coming to this interface will be dropped. The value
        of cdsIfSrcGuardAddress object will be ignored in
        this case." 
    ::= { cdsIfSrcGuardAddrEntry 4 }

cdsIfSrcGuardFilterMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        active(1),
                        inactiveTrustPort(2),
                        inactiveNoSnoopingVlan(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the Source Guard filter mode at
        this interface.

        active(1) indicates that the Source Guard feature is
        active at this interface.

        inactiveTrustPort(2) indicates that the Source Guard
        feature is inactive because this interface is a DHCP
        Snooping trust interface.

        inactiveNoSnoopingVlan(3) indicates that the Source
        Guard feature is inactive because this interface
        does not have a VLAN which has DHCP Snooping enabled." 
    ::= { cdsIfSrcGuardAddrEntry 5 }

cdsIfSrcGuardMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MAC address for Source Guard
        purpose." 
    ::= { cdsIfSrcGuardAddrEntry 6 }

cdsIfSrcGuardMacFilterAction OBJECT-TYPE
    SYNTAX          INTEGER  {
                        allowMacAddress(1),
                        denyAllMacAddresses(2),
                        permitAllMacAddresses(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the Source Guard action
        applied at this interface with respect to MAC traffic.

        allowMacAddress(1) indicates that MAC traffic coming
        from the MAC address denoted by cdsIfSrcGuardMacAddress
        object will be allowed to go through.

        denyAllMacAddresses(2) indicates that all MAC traffic
        coming to this interface will be dropped. The value
        of cdsIfSrcGuardMacAddress object will be ignored in
        this case.

        permitAllMacAddresses(3) indicates that all MAC traffic
        coming to this interface will be allowed. The value
        of cdsIfSrcGuardMacAddress object will be ignored in
        this case." 
    ::= { cdsIfSrcGuardAddrEntry 7 }

cdsIfSrcGuardVlansLow OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (0..256))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A string of octets containing one bit per VLAN for
        VLANs with VlanIndex value of 0 to 2047. The first
        octet corresponds to VLANs with VlanIndex values
        of 0 through 7; the second octet to VLANs 8 through
        15; etc.  The most significant bit of each octet
        corresponds to the lowest value VlanIndex in that octet.

        For each VLAN, if Source Guard feature is enabled then
        the bit corresponding to that VLAN is set to '1'.

        Note that if the length of this string is less than
        256 octets, any 'missing' octets are assumed to contain
        the value zero. A NMS may omit any zero-valued octets
        from the end of this string in order to reduce SetPDU size,
        and the agent may also omit zero-valued trailing octets,
        to reduce the size of GetResponse PDUs." 
    ::= { cdsIfSrcGuardAddrEntry 8 }

cdsIfSrcGuardVlansHigh OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (0..256))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A string of octets containing one bit per VLAN for
        VLANs with VlanIndex value of 2048 to 4095. The first
        octet corresponds to VLANs with VlanIndex values
        of 2048 through 2055; the second octet to VLANs 2056
        through 2063; etc.  The most significant bit of each
        octet corresponds to the lowest value VlanIndex in that
        octet.

        For each VLAN, if Source Guard feature is enabled then
        the bit corresponding to that VLAN is set to '1'.

        Note that if the length of this string is less than
        256 octets, any 'missing' octets are assumed to contain
        the value zero. A NMS may omit any zero-valued octets
        from the end of this string in order to reduce SetPDU size,
        and the agent may also omit zero-valued trailing octets,
        to reduce the size of GetResponse PDUs." 
    ::= { cdsIfSrcGuardAddrEntry 9 }
 


-- Notifications

cdsBindingsNotification NOTIFICATION-TYPE
    OBJECTS         {
                        cdsBindingsAddrType,
                        cdsBindingsIpAddress,
                        ifName
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated when a DHCP binding
        is learnt dynamically by the device. cdsBindingsAddrType
        and cdsBindingsIpAddress provides the IP address 
        allocated for the DHCP client by the DHCP server. 
        ifName identifies the interface where the DHCP client
        connects to."
   ::= { ciscoDhcpSnoopingMIBNotifs 1 }
-- Conformance

cdsMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBConformance 1 }

cdsMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoDhcpSnoopingMIBConformance 2 }


cdsMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the CISCO-DHCP-SNOOPING-MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cdsIfConfigGroup,
                        cdsBindingsGroup
                    }

    GROUP           cdsGlobalEnableGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsDatabaseGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        storage of DHCP bindings information."

    GROUP           cdsVlanConfigGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        controlling DHCP Snooping per VLAN."

    GROUP           cdsIfRateLimitGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping rate limit per interface."

    GROUP           cdsStatisticsGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping statistics information."

    GROUP           cdsRelayAgentInfoOptGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping option 82 insertion information."

    GROUP           cdsIfSrcGuardGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        IP Source Guard."

    GROUP           cdsMatchMacAddressGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping Mac address matching."
    ::= { cdsMIBCompliances 1 }

cdsMIBCompliance2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the CISCO-DHCP-SNOOPING-MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cdsIfConfigGroup,
                        cdsBindingsGroup
                    }

    GROUP           cdsGlobalEnableGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsDatabaseGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        storage of DHCP bindings information."

    GROUP           cdsVlanConfigGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        controlling DHCP Snooping per VLAN."

    GROUP           cdsIfRateLimitGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping rate limit per interface."

    GROUP           cdsStatisticsGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping statistics information."

    GROUP           cdsRelayAgentInfoOptGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping option 82 insertion information."

    GROUP           cdsIfSrcGuardGroupRev1
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        IP Source Guard."

    GROUP           cdsMatchMacAddressGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping Mac address matching."

    GROUP           cdsRelayAgentRemoteIdGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        DHCP Option 82 remote ID relay agent."

    GROUP           cdsIfFeatureConfigGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        enable or disable of DHCP Snooping feature at the interface."

    GROUP           cdsBindingsLimitGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        binding limit for DHCP Snooping feature."

    GROUP           cdsStaticBindingsGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the DHCP bindings data statically configured by (local
        or network) management."

    GROUP           cdsIfSrcGuardIpFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsIfSrcGuardExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP and MAC source guard feature."

    GROUP           cdsIfSrcGuardTrafficFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    OBJECT          cdsStaticBindingsStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Support for 'createAndWait' is not required."
    ::= { cdsMIBCompliances 2 }

cdsMIBCompliance3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the CISCO-DHCP-SNOOPING-MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cdsIfConfigGroup,
                        cdsBindingsGroup
                    }

    GROUP           cdsGlobalEnableGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsDatabaseGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        storage of DHCP bindings information."

    GROUP           cdsVlanConfigGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        controlling DHCP Snooping per VLAN."

    GROUP           cdsIfRateLimitGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping rate limit per interface."

    GROUP           cdsStatisticsGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping statistics information."

    GROUP           cdsRelayAgentInfoOptGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping option 82 insertion information."

    GROUP           cdsIfSrcGuardGroupRev1
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        IP Source Guard."

    GROUP           cdsMatchMacAddressGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping Mac address matching."

    GROUP           cdsRelayAgentRemoteIdGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        DHCP Option 82 remote ID relay agent."

    GROUP           cdsIfFeatureConfigGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        enable or disable of DHCP Snooping feature at the interface."

    GROUP           cdsBindingsLimitGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        binding limit for DHCP Snooping feature."

    GROUP           cdsStaticBindingsGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the DHCP bindings data statically configured by (local
        or network) management."

    GROUP           cdsIfSrcGuardIpFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsIfSrcGuardExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP and MAC source guard feature."

    GROUP           cdsIfSrcGuardTrafficFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsBindingsHostnameGroup
    DESCRIPTION
        "This group is mandatory only for platforms where the host
        name of DHCP client in DHCP bindings data is available."

    OBJECT          cdsStaticBindingsStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Support for 'createAndWait' is not required."
    ::= { cdsMIBCompliances 3 }

cdsMIBCompliance4 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the CISCO-DHCP-SNOOPING-MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cdsIfConfigGroup,
                        cdsBindingsGroup
                    }

    GROUP           cdsGlobalEnableGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsDatabaseGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        storage of DHCP bindings information."

    GROUP           cdsVlanConfigGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        controlling DHCP Snooping per VLAN."

    GROUP           cdsIfRateLimitGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping rate limit per interface."

    GROUP           cdsStatisticsGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping statistics information."

    GROUP           cdsRelayAgentInfoOptGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping option 82 insertion information."

    GROUP           cdsIfSrcGuardGroupRev1
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        IP Source Guard."

    GROUP           cdsMatchMacAddressGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping Mac address matching."

    GROUP           cdsIfFeatureConfigGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        enable or disable of DHCP Snooping feature at the interface."

    GROUP           cdsBindingsLimitGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        binding limit for DHCP Snooping feature."

    GROUP           cdsStaticBindingsGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the DHCP bindings data statically configured by (local
        or network) management."

    GROUP           cdsIfSrcGuardIpFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsIfSrcGuardExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP and MAC source guard feature."

    GROUP           cdsIfSrcGuardTrafficFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsBindingsHostnameGroup
    DESCRIPTION
        "This group is mandatory only for platforms where the host
        name of DHCP client in DHCP bindings data is available."

    GROUP           cdsRelayAgentInfoOptRemoteIdSubGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of remote-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsIfVlanRelayInfoOptCircuitIdGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of circuit-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsStatisticsExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the counter indicating the number of packets forwarded
        without insertion of option 82 data."

    OBJECT          cdsStaticBindingsStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Support for 'createAndWait' is not required."
    ::= { cdsMIBCompliances 4 }

cdsMIBCompliance5 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the CISCO-DHCP-SNOOPING-MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cdsIfConfigGroup,
                        cdsBindingsGroup
                    }

    GROUP           cdsGlobalEnableGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsDatabaseGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        storage of DHCP bindings information."

    GROUP           cdsVlanConfigGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        controlling DHCP Snooping per VLAN."

    GROUP           cdsIfRateLimitGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping rate limit per interface."

    GROUP           cdsStatisticsGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping statistics information."

    GROUP           cdsRelayAgentInfoOptGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping option 82 insertion information."

    GROUP           cdsIfSrcGuardGroupRev1
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        IP Source Guard."

    GROUP           cdsMatchMacAddressGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping Mac address matching."

    GROUP           cdsIfFeatureConfigGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        enable or disable of DHCP Snooping feature at the interface."

    GROUP           cdsBindingsLimitGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        binding limit for DHCP Snooping feature."

    GROUP           cdsStaticBindingsGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the DHCP bindings data statically configured by (local
        or network) management."

    GROUP           cdsIfSrcGuardIpFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsIfSrcGuardExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP and MAC source guard feature."

    GROUP           cdsIfSrcGuardTrafficFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsBindingsHostnameGroup
    DESCRIPTION
        "This group is mandatory only for platforms where the host
        name of DHCP client in DHCP bindings data is available."

    GROUP           cdsRelayAgentInfoOptRemoteIdSubGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of remote-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsIfVlanRelayInfoOptCircuitIdGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of circuit-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsStatisticsExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the counter indicating the number of packets forwarded
        without insertion of option 82 data."

    GROUP           cdsNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification control for DHCP Snooping feature."

    GROUP           cdsBindingsNotificationGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification for DHCP Snooping feature."

    OBJECT          cdsStaticBindingsStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Support for 'createAndWait' is not required."
    ::= { cdsMIBCompliances 5 }

cdsMIBCompliance6 MODULE-COMPLIANCE
    STATUS          deprecated 
    DESCRIPTION
        "The compliance statement for the CISCO-DHCP-SNOOPING-MIB.
         This statement is deprecated and superceded by
         cdsMIBCompliance7."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cdsIfConfigGroup,
                        cdsBindingsGroup
                    }

    GROUP           cdsGlobalEnableGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsDatabaseGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsVlanConfigGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsIfRateLimitGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsStatisticsGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsRelayAgentInfoOptGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsIfSrcGuardGroupRev1
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        IP Source Guard."

    GROUP           cdsMatchMacAddressGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping Mac address matching."

    GROUP           cdsIfFeatureConfigGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        enable or disable of DHCP Snooping feature at the interface."

    GROUP           cdsBindingsLimitGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        binding limit for DHCP Snooping feature."

    GROUP           cdsStaticBindingsGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the DHCP bindings data statically configured by (local
        or network) management."

    GROUP           cdsIfSrcGuardIpFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsIfSrcGuardExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP and MAC source guard feature."

    GROUP           cdsIfSrcGuardTrafficFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsBindingsHostnameGroup
    DESCRIPTION
        "This group is mandatory only for platforms where the host
        name of DHCP client in DHCP bindings data is available."

    GROUP           cdsRelayAgentInfoOptRemoteIdSubGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of remote-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsIfVlanRelayInfoOptCircuitIdGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of circuit-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsStatisticsExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the counter indicating the number of packets forwarded
        without insertion of option 82 data."

    GROUP           cdsNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification control for DHCP Snooping feature."

    GROUP           cdsBindingsNotificationGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification for DHCP Snooping feature."

    GROUP           cdsIfVlanRelayInfoOptCircuitIdGroupSup1
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification control for DHCP Snooping feature."

    OBJECT          cdsStaticBindingsStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Support for 'createAndWait' is not required."
    ::= { cdsMIBCompliances 6 }


cdsMIBCompliance7 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the CISCO-DHCP-SNOOPING-MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cdsIfConfigGroup,
                        cdsBindingsGroup
                    }

    GROUP           cdsGlobalEnableGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsDatabaseGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsVlanConfigGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsIfRateLimitGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsStatisticsGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsRelayAgentInfoOptGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        enabling the DHCP Snooping feature at device level."

    GROUP           cdsIfSrcGuardGroupRev1
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        IP Source Guard."

    GROUP           cdsMatchMacAddressGroup
    DESCRIPTION
        "This group is mandatory only for the platform which supports
        DHCP Snooping Mac address matching."

    GROUP           cdsIfFeatureConfigGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        enable or disable of DHCP Snooping feature at the interface."

    GROUP           cdsBindingsLimitGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        binding limit for DHCP Snooping feature."

    GROUP           cdsStaticBindingsGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the DHCP bindings data statically configured by (local
        or network) management."

    GROUP           cdsIfSrcGuardIpFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsIfSrcGuardExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP and MAC source guard feature."

    GROUP           cdsIfSrcGuardTrafficFilterGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        interface IP source guard feature."

    GROUP           cdsBindingsHostnameGroup
    DESCRIPTION
        "This group is mandatory only for platforms where the host
        name of DHCP client in DHCP bindings data is available."

    GROUP           cdsRelayAgentInfoOptRemoteIdSubGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of remote-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsIfVlanRelayInfoOptCircuitIdGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        configuration of circuit-id sub-option for Option 82 DHCP 
        Snooping feature."

    GROUP           cdsStatisticsExtGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the counter indicating the number of packets forwarded
        without insertion of option 82 data."

    GROUP           cdsNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification control for DHCP Snooping feature."

    GROUP           cdsBindingsNotificationGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification for DHCP Snooping feature."

    GROUP           cdsIfVlanRelayInfoOptCircuitIdGroupSup1
    DESCRIPTION
        "This group is mandatory only for platforms which support
        bindings notification control for DHCP Snooping feature."

    GROUP           cdsVlanOperStatusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
         operational status of DHCP Snooping feature in VLAN."

    OBJECT          cdsStaticBindingsStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Support for 'createAndWait' is not required."
    ::= { cdsMIBCompliances 7 }

-- Units of Conformance
--   
-- cdsGlobalGroup

cdsGlobalEnableGroup OBJECT-GROUP
    OBJECTS         { cdsFeatureEnable }
    STATUS          current
    DESCRIPTION
        "A collection of object which are used to configure as
        well as show information regarding the feature enabling."
    ::= { cdsMIBGroups 1 }

cdsDatabaseGroup OBJECT-GROUP
    OBJECTS         {
                        cdsDatabaseFile,
                        cdsDatabaseUpdateInterval
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which are used to configure as
        well as show information regarding the DHCP Snooping 
        database filename and update interval."
    ::= { cdsMIBGroups 2 }

cdsVlanConfigGroup OBJECT-GROUP
    OBJECTS         { cdsVlanDhcpSnoopingEnable }
    STATUS          current
    DESCRIPTION
        "A collection of object which are used to configure as
        well as show information regarding the DHCP Snooping 
        feature per VLAN."
    ::= { cdsMIBGroups 3 }

cdsIfConfigGroup OBJECT-GROUP
    OBJECTS         { cdsIfTrustEnable }
    STATUS          current
    DESCRIPTION
        "A collection of object which are used to configure as
        well as show information regarding the interface trust
        state for DHCP Snooping purpose."
    ::= { cdsMIBGroups 4 }

cdsIfRateLimitGroup OBJECT-GROUP
    OBJECTS         { cdsIfRateLimit }
    STATUS          current
    DESCRIPTION
        "A collection of object which are used to configure as
        well as show information regarding the rate limit per 
        interface for DHCP Snooping purpose."
    ::= { cdsMIBGroups 5 }

cdsBindingsGroup OBJECT-GROUP
    OBJECTS         {
                        cdsBindingsAddrType,
                        cdsBindingsIpAddress,
                        cdsBindingsInterface,
                        cdsBindingsLeasedTime,
                        cdsBindingsStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object which are used to configure as
        well as show information regarding the DHCP bindings
        data."
    ::= { cdsMIBGroups 6 }

cdsStatisticsGroup OBJECT-GROUP
    OBJECTS         {
                        cdsTotalForwardedPkts,
                        cdsTotalDroppedPkts,
                        cdsUntrustedPortDroppedPkts
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object which are used to show statistics
        information regarding DHCP Snooping feature."
    ::= { cdsMIBGroups 7 }

cdsRelayAgentInfoOptGroup OBJECT-GROUP
    OBJECTS         { cdsRelayAgentInfoOptEnable }
    STATUS          current
    DESCRIPTION
        "A collection of objects which are used to configure as
        well as show information regarding DHCP Option 82
        insertion."
    ::= { cdsMIBGroups 8 }

cdsIfSrcGuardGroup OBJECT-GROUP
    OBJECTS         {
                        cdsIfSrcGuardEnable,
                        cdsIfSrcGuardAddrType,
                        cdsIfSrcGuardAddress
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects which are used to configure as
        well as show information regarding IP Source Guard 
        purpose."
    ::= { cdsMIBGroups 9 }

cdsRelayAgentRemoteIdGroup OBJECT-GROUP
    OBJECTS         { cdsRelayAgentInfoOptRemoteId }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects which are used to indicate information
        regarding DHCP Option 82 remote ID relay agent."
    ::= { cdsMIBGroups 10 }

cdsMatchMacAddressGroup OBJECT-GROUP
    OBJECTS         { cdsMatchMacAddressEnable }
    STATUS          current
    DESCRIPTION
        "A collection of objects which are used to configure as
        well as show information regarding DHCP Snooping Mac
        address matching."
    ::= { cdsMIBGroups 11 }

cdsIfFeatureConfigGroup OBJECT-GROUP
    OBJECTS         { cdsIfFeatureEnable }
    STATUS          current
    DESCRIPTION
        "A collection of object which are used to configure as
        well as show information regarding enable or disable of
        DHCP Snooping feature at the interface."
    ::= { cdsMIBGroups 12 }

cdsBindingsLimitGroup OBJECT-GROUP
    OBJECTS         {
                        cdsGlobalMaxBindingsLimit,
                        cdsIfBindingsLimit
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which provides information regarding
        binding limit for DHCP Snooping purpose."
    ::= { cdsMIBGroups 13 }

cdsStaticBindingsGroup OBJECT-GROUP
    OBJECTS         {
                        cdsStaticBindingsAddrType,
                        cdsStaticBindingsIpAddress,
                        cdsStaticBindingsInterface,
                        cdsStaticBindingsStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which is used to configure
        as well as show information regarding the DHCP bindings data
        configured by users."
    ::= { cdsMIBGroups 14 }

cdsIfSrcGuardIpFilterGroup OBJECT-GROUP
    OBJECTS         {
                        cdsIfSrcGuardIpFilterAction,
                        cdsIfSrcGuardFilterMode
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which is used to show information
        regarding interface IP source guard purpose."
    ::= { cdsMIBGroups 15 }

cdsIfSrcGuardExtGroup OBJECT-GROUP
    OBJECTS         {
                        cdsIfSrcGuardMacAddress,
                        cdsIfSrcGuardMacFilterAction,
                        cdsIfSrcGuardVlansLow,
                        cdsIfSrcGuardVlansHigh
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which is used to show additional
        information regarding the IP source guard feature."
    ::= { cdsMIBGroups 16 }

cdsIfSrcGuardTrafficFilterGroup OBJECT-GROUP
    OBJECTS         { cdsIfSrcGuardFilterType }
    STATUS          current
    DESCRIPTION
        "A collection of objects which is used to configure the
        type of traffic to be filtered by IP source guard feature."
    ::= { cdsMIBGroups 17 }

cdsIfSrcGuardGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cdsIfSrcGuardAddrType,
                        cdsIfSrcGuardAddress
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which are used to configure as
        well as show information regarding IP Source Guard 
        purpose."
    ::= { cdsMIBGroups 18 }

cdsBindingsHostnameGroup OBJECT-GROUP
    OBJECTS         { cdsBindingsHostname }
    STATUS          current
    DESCRIPTION
        "A collection of objects which indicates the host name
        of DHCP client in DHCP bindings data."
    ::= { cdsMIBGroups 19 }

cdsRelayAgentInfoOptRemoteIdSubGroup OBJECT-GROUP
    OBJECTS         { cdsRelayAgentInfoOptRemoteIdSub }
    STATUS          current
    DESCRIPTION
        "A collection of objects which are used to configure
        as well as show remote-id of option 82 DHCP Snooping."
    ::= { cdsMIBGroups 20 }

cdsIfVlanRelayInfoOptCircuitIdGroup OBJECT-GROUP
    OBJECTS         {
                        cdsIfVlanRelayInfoOptCircuitId,
                        cdsIfVlanRelayInfoOptCircuitIdStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which are used to configure
        as well as show circuit-id of option 82 DHCP Snooping."
    ::= { cdsMIBGroups 21 }

cdsStatisticsExtGroup OBJECT-GROUP
    OBJECTS         { cdsForwardedWithoutOption82Pkts }
    STATUS          current
    DESCRIPTION
        "A collection of objects which are used to show
        additional DHCP snooping statistics information."
    ::= { cdsMIBGroups 22 }

cdsNotifControlGroup OBJECT-GROUP
    OBJECTS         { cdsBindingsNotifEnabled }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) which provides information
        on bindings notifications control for DHCP Snooping feature."
    ::= { cdsMIBGroups 23 }

cdsBindingsNotificationGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { cdsBindingsNotification }
    STATUS          current
    DESCRIPTION
        "A collection of notification(s) which provides bindings
        notifications support for DHCP Snooping feature."
    ::= { cdsMIBGroups 24 }

cdsIfVlanRelayInfoOptCircuitIdGroupSup1 OBJECT-GROUP
    OBJECTS         { cdsIfVlanRelayInfoOptCircuitIdDirect }
    STATUS          current
    DESCRIPTION
        "A collection of objects which indicates to ignore the length
        and type in Agent Circuit ID sub-option of the DHCP relay
        information option (option 82) data inserted to DHCP packets by 
        DHCP Snooping feature."
    ::= { cdsMIBGroups 25 }

cdsVlanOperStatusGroup OBJECT-GROUP
    OBJECTS         { cdsVlanDhcpSnoopingOperStatus }
    STATUS          current
    DESCRIPTION
        "A collection of objects which provides information on
        operation status of DHCP Snooping feature in VLAN." 
    ::= { cdsMIBGroups 26 }

END



